{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Cenník"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Cenník","index":0,"n_rows":27550,"n_cols":15,"rows_kept":4500,"cut":true,"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["REF SAP","POPIS","MIN. OBJ. MNOŽSTVO","MJ","PC bez DPH","EAN KÓD ","DĹŽKA [cm]","VÝŠKA [cm]","ŠÍRKA [cm]","HMOTNOSŤ [g]","ZEM PÔVODU","COLNÉ ČÍSLO","WEB LINK","POPIS DLHÝ","RECYKLAČNÝ POPLATOK"]
["ZENL1121","SPÍNACIA JEDNOTKA PRE XAL",5,"ks",{"v":4.34660625,"d":"4.347"},"3389110115086",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZENL1121","dotykový blok s vratnou pružinou – 1 NC – montáž na zadnej skrinke",0]
["ZENL1111","SPÍNACIA JEDNOTKA PRE XAL",5,"ks",{"v":4.34660625,"d":"4.347"},"3389110115079",{"v":3.5,"d":"3.50"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZENL1111","dotykový blok s vratnou pružinou – 1 NO – montáž na zadnej skrinke",0]
["ZD5PA24","POLOZOSTAVA SPOJ.DIEL + OVL. PÁKA",1,"ks",{"v":53.53188749999999,"d":"53.532"},"3389110165630",{"v":8.8,"d":"8.80"},{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":35,"d":"35.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZD5PA24","hlavica 4-smerového pákového ovládača – Ø 22 – vratná pružina",0]
["ZD5PA22","POLOZOSTAVA SPOJ.DIEL + OVL. PÁKA",1,"ks",{"v":38.43315,"d":"38.433"},"3389110165609",{"v":5.3,"d":"5.30"},{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":22,"d":"22.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZD5PA22","hlavica 2-smerového pákového ovládača – Ø 22 – vratná pružina",0]
["ZD5PA203","TELO KRÍŽ. OVLÁDAČA",1,"ks",{"v":28.367324999999997,"d":"28.367"},"3389110286397",{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":47.5,"d":"47.50"},"FR","8536508090","https://www.se.com/sk/sk/product/ZD5PA203","teleso 4-smerového pákového ovládača – Ø 22 – 1 NO na jeden smer",0]
["ZD5PA14","POLOZOSTAVA KRÍŽOVÉHO OVLÁDAČA",1,"ks",{"v":40.2633,"d":"40.263"},"3389110165623",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZD5PA14","hlavica 4-smerového pákového ovládača – Ø 22 – usadený",0]
["ZD4PA24","HLAVICA PRE KRÍŽ. OVL.22MM",1,"ks",{"v":64.51278749999999,"d":"64.513"},"3389110120042",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZD4PA24","hlavica 4-smerového pákového ovládača – Ø 22 – vratná pružina",0]
["ZD4PA22","HLAVICA PRE KRÍŽ. OVL.22MM",1,"ks",{"v":55.81957499999999,"d":"55.820"},"3389110119886",{"v":5.4,"d":"5.40"},{"v":9.4,"d":"9.40"},{"v":3.6,"d":"3.60"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZD4PA22","hlava krížového ovládača Ø22 2 - smerová s návratom",0]
["ZD4PA203","TELO KRÍŽ. OVLÁDAČA",1,"ks",{"v":28.367324999999997,"d":"28.367"},"3389110286083",{"v":5.4,"d":"5.40"},{"v":8.6,"d":"8.60"},{"v":3.4,"d":"3.40"},{"v":58,"d":"58.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZD4PA203","teleso 4-smerového pákového ovládača – Ø 22 – 1 NO na jeden smer",0]
["ZD4PA103","BLIK KONTAKTOV",1,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110285918",{"v":8.7,"d":"8.70"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":61,"d":"61.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZD4PA103","telo s kontaktným blokom pre 2 - smerový joystic ovládač",0]
["ZBZM156","230V TEST KONTROLKA",1,"ks",{"v":21.046725,"d":"21.047"},"3389118030114",{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8536619090","https://www.se.com/sk/sk/product/ZBZM156","dvojitý svetelný blok pre test funkcie svetla 48...230V",0]
["ZBZG156","120V TEST KONTROLKA",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389118030107",{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":8.8,"d":"8.80"},{"v":10,"d":"10.00"},"FR","8536619090","https://www.se.com/sk/sk/product/ZBZG156","blok pre test funkcií 12V. 24V. 24...120V",0]
["ZBZ60","PROTECTIVE BOOT FOR CONTACT BLOCK",1,"ks",{"v":53.53188749999999,"d":"53.532"},"3389111000091",{"v":11,"d":"11.00"},{"v":7.7,"d":"7.70"},{"v":7,"d":"7.00"},{"v":90,"d":"90.00"},"FR","4016999790","https://www.se.com/sk/sk/product/ZBZ60","OCHRANNÝ KRYT PRE KONT. BLOK HARMONY",0]
["ZBZ58","EPDM PÚZDRO HLAVY STOP TLAČIDLA",2,"ks",{"v":5.3989425,"d":"5.399"},"3389119027786",{"v":3.4,"d":"3.40"},{"v":3.3,"d":"3.30"},{"v":3.4,"d":"3.40"},{"v":9,"d":"9.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBZ58","žlté tesnenie pre Ø40 & Ø60 hríbovú hlavu tlačítka",0]
["ZBZ4005","OCHRANNÝ KRYT, VÝŠKA 37 mm",1,"ks",{"v":8.418689999999998,"d":"8.419"},"3389119042765",{"v":11.3,"d":"11.30"},{"v":5,"d":"5.00"},{"v":10.7,"d":"10.70"},{"v":92,"d":"92.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBZ4005","Guard, Harmony XB4, Harmony XB5, isolation accessory, plastic, yellow, 37mm, for selector switch",0]
["ZBZ4","REDUKCIA 30/22MM",10,"ks",{"v":1.4183662499999998,"d":"1.418"},"3389110414677",{"v":7.5,"d":"7.50"},{"v":1.2,"d":"1.20"},{"v":5.5,"d":"5.50"},{"v":8.1,"d":"8.10"},"CZ","85389099","https://www.se.com/sk/sk/product/ZBZ4","PLASTIC DIAM 30-22 ADAPTA TOR",0]
["ZBZ3605","OCHRANNÝ KRYT PRE HRÍBOVÚ HLAVICU",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3389119020480",{"v":5.7,"d":"5.70"},{"v":3.4,"d":"3.40"},{"v":5.2,"d":"5.20"},{"v":45,"d":"45.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBZ3605","teleskopický ochranný kryt pre Ø40 núdzové tlačítko",0]
["ZBZ35","NOSIČ ŠTÍTKOV 30 X 50 MM VYSOKÝ",10,"ks",{"v":0.9608287499999999,"d":"0.961"},"3389110095913",{"v":12,"d":"12.00"},{"v":3,"d":"3.00"},{"v":10,"d":"10.00"},{"v":3,"d":"3.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBZ35","držiak štítkov 30 x 50 mm bez štítku – pre jednotky Ø 22 s guľatou hlavicou",0]
["ZBZ34","NOSIČ ŠTÍTKOV 30 X 40 MM VYSOKÝ",10,"ks",{"v":1.1895974999999999,"d":"1.190"},"3389110095883",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":13,"d":"13.00"},{"v":3,"d":"3.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBZ34","držiak štítkov 30 x 40 mm bez štítku – pre jednotky Ø 22 s guľatou hlavicou",0]
["ZBZ33","NOSIČ ŠTÍTKOV",10,"ks",{"v":0.8235675,"d":"0.824"},"3389110095852",{"v":5,"d":"5.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBZ33","držiak štítkov 30 x 50 mm bez štítku – pre jednotky Ø 22 s guľatou hlavicou",0]
["ZBZ32","NOSIČ ŠTÍTKOV",10,"ks",{"v":0.7320599999999999,"d":"0.732"},"3389110092592",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBZ32","držiak štítkov 30 x 40 mm bez štítku – pre jednotky Ø 22",0]
["ZBZ28","TESNENIE IP69K NA HRÍBOVÉ TLAČIDLO",1,"ks",{"v":8.601705,"d":"8.602"},"3389119022255",{"v":3.4,"d":"3.40"},{"v":3.3,"d":"3.30"},{"v":3.4,"d":"3.40"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBZ28","čierne tesn.-vlonovec – pre tlačidlo núdz. vyp. – Ø 22",0]
["ZBZ2102","PRÍSLUŠENSTVO",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110651850",{"v":5.4,"d":"5.40"},{"v":4.2,"d":"4.20"},{"v":5.2,"d":"5.20"},{"v":12,"d":"12.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBZ2102","čierny ochranný kryt pre Ø22 štandard. hlava alebo prepínač s kľúčom",0]
["ZBZ1902RA","OCHRANNÝ KRYT PLAST",1,"ks",{"v":8.876227499999999,"d":"8.876"},"3606480444883",{"v":8.5,"d":"8.50"},{"v":2.4,"d":"2.40"},{"v":5.5,"d":"5.50"},{"v":8,"d":"8.00"},"FR","39269097","https://www.se.com/sk/sk/product/ZBZ1902RA","kryt tlačítka pre náročné prostredie - mont. otoč. o 90°",0]
["ZBZ1902","OCHRANNÝ KRYT, PLAST",1,"ks",{"v":8.876227499999999,"d":"8.876"},"3606480444876",{"v":8,"d":"8.00"},{"v":2.5,"d":"2.50"},{"v":5.5,"d":"5.50"},{"v":8,"d":"8.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBZ1902","kryt tlačítka pre náročné prostredie",0]
["ZBZ1605","KOVOVÝ KRYT HLAVICE",1,"ks",{"v":40.2633,"d":"40.263"},"3389110099492",{"v":5.2,"d":"5.20"},{"v":5.7,"d":"5.70"},{"v":4.4,"d":"4.40"},{"v":46,"d":"46.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBZ1605","ochranný krýt pre Ø 40 hríbovú hlavicu a jednotky Ø 22 mm – žltý",0]
["ZBZ1604","KOVOVÝ KRYT HLAVICE",1,"ks",{"v":39.80576249999999,"d":"39.806"},"3389110099485",{"v":5.6,"d":"5.60"},{"v":4.5,"d":"4.50"},{"v":5,"d":"5.00"},{"v":46,"d":"46.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBZ1604","ochranný krýt pre Ø 40 hríbovú hlavicu a jednotky Ø 22 mm – červený",0]
["ZBZ1602","KOVOVÝ KRYT HLAVICE",1,"ks",{"v":39.80576249999999,"d":"39.806"},"3389110099478",{"v":4.5,"d":"4.50"},{"v":5.7,"d":"5.70"},{"v":5.3,"d":"5.30"},{"v":59,"d":"59.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBZ1602","ochranný krýt pre Ø 40 hríbovú hlavicu a jednotky Ø 22 mm – čierny",0]
["ZBZ1600","OCHRANNÝ KRYT PRE HRÍBOVÚ HLAVICU",1,"ks",{"v":43.46606249999999,"d":"43.466"},"3389110842500",{"v":5.3,"d":"5.30"},{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":60,"d":"60.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBZ1600","ochranný krýt pre Ø 40 hríbovú hlavicu a jednotky Ø 22 mm – pochrómovaný",0]
["ZBZ010","ADAPTÉR",10,"ks",{"v":5.44469625,"d":"5.445"},"3389110090505",{"v":15.5,"d":"15.50"},{"v":4.5,"d":"4.50"},{"v":5.2,"d":"5.20"},{"v":8,"d":"8.00"},"FR","8536699099","https://www.se.com/sk/sk/product/ZBZ010","adaptér pre 1,6 mm dosku s plošnými spojmi pre jednotku Ø 22 mm – súprava 10 ks",0]
["ZBZ007","Spona pre spínaciu jednotku",10,"ks",{"v":1.1895974999999999,"d":"1.190"},"3389110516838",{"v":2.8,"d":"2.80"},{"v":0.8,"d":"0.80"},{"v":2.6,"d":"2.60"},{"v":0.8,"d":"0.80"},"FR","7326909890","https://www.se.com/sk/sk/product/ZBZ007","spinka pre kontaktný blok",0]
["ZBZ006","UPEVŇOVACIA SKRUTKA DO PLOŠNÉHO SPOJA",10,"ks",{"v":1.60138125,"d":"1.601"},"3389110090543",{"v":2.4,"d":"2.40"},{"v":0.5,"d":"0.50"},{"v":0.5,"d":"0.50"},{"v":0.9,"d":"0.90"},"FR","7318159589","https://www.se.com/sk/sk/product/ZBZ006","upevň. skrutka – pre montáž s adaptérom dosky s ploš. spojmi na nosný pilier",0]
["ZBZ001","IDENTIFIKÁCIA EL. BLOKOV",10,"ks",{"v":1.1895974999999999,"d":"1.190"},"3389110090567",{"v":3.5,"d":"3.50"},{"v":1,"d":"1.00"},{"v":2,"d":"2.00"},{"v":1.1,"d":"1.10"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBZ001","držiak štítkov – Ø 22 – zaklapávací typ, bez štítku",0]
["ZBYP6101C0","Štítok 30 x 50 mm",1,"ks",{"v":6.222509999999999,"d":"6.223"},"3606489756291",{"v":15,"d":"15.00"},{"v":11,"d":"11.00"},{"v":0.1,"d":"0.10"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYP6101C0","Legend plate, Harmony XB5, 30 x 50mm, grey bezel, unmarked",0]
["ZBYP2367","Štítok s popisom",1,"ks",{"v":2.3334412499999995,"d":"2.333"},"3606489756253",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":2.5,"d":"2.50"},{"v":0.7,"d":"0.70"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYP2367","legend plate with off-on marking",0]
["ZBYP2178","Štítok s popisom",10,"ks",{"v":2.4707025,"d":"2.471"},"3606489756130",{"v":15,"d":"15.00"},{"v":11,"d":"11.00"},{"v":0.1,"d":"0.10"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYP2178","legend plate with o-i marking",0]
["ZBYP2101","Štítok 30 x 40 mm -BLNK LABEL(BLK/RED)",1,"ks",{"v":1.8759037499999995,"d":"1.876"},"3606489756017",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYP2101","Legend plate, Harmony XB5, 30 x 40mm, plastic, dark grey, unmarked",0]
["ZBYM2101","Štítok 30 x 40 mm",1,"ks",{"v":2.4249487499999995,"d":"2.425"},"3606489755911",{"v":3,"d":"3.00"},{"v":0.5,"d":"0.50"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},"FR","7616991099","https://www.se.com/sk/sk/product/ZBYM2101","Legend plate, Harmony XB5, 30 x 40mm, metal, unmarked",0]
["ZBYLEG502000","Samolepiaca fólia bez symbolov",1,"ks",{"v":200.401425,"d":"200.401"},"3606489755850",{"v":53,"d":"53.00"},{"v":0.5,"d":"0.50"},{"v":43,"d":"43.00"},{"v":282,"d":"282.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYLEG502000","Harmony XB5, Antimikrobiálna samolepiaca fólia 500 x 200, bez symbolu",""]
["ZBYLEG501000","Samolepiaca fólia bez symbolov",1,"ks",{"v":98.82809999999999,"d":"98.828"},"3606489755836",{"v":53,"d":"53.00"},{"v":0.5,"d":"0.50"},{"v":43,"d":"43.00"},{"v":235,"d":"235.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYLEG501000","Harmony XB5, Antimikrobiálna samolepiaca fólia 500 x 100, bez symbolu",""]
["ZBYLEG304000","Samolepiaca fólia bez symbolov",1,"ks",{"v":237.9195,"d":"237.920"},"3606489755775",{"v":44,"d":"44.00"},{"v":0.5,"d":"0.50"},{"v":32,"d":"32.00"},{"v":222,"d":"222.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYLEG304000","Harmony XB5, Antimikrobiálna samolepiaca fólia 300 x 400 mm, bez symbolu",""]
["ZBYLEG303000","Samolepiaca fólia bez symbolov",1,"ks",{"v":177.52455,"d":"177.525"},"3606489755751",{"v":44,"d":"44.00"},{"v":0.5,"d":"0.50"},{"v":32,"d":"32.00"},{"v":198,"d":"198.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYLEG303000","Harmony XB5, Antimikrobiálna samolepiaca fólia 300 x 300, bez symbolu",""]
["ZBYLEG302000","Samolepiaca fólia bez symbolov",1,"ks",{"v":100.65825,"d":"100.658"},"3606489755737",{"v":36,"d":"36.00"},{"v":0.5,"d":"0.50"},{"v":25,"d":"25.00"},{"v":135,"d":"135.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYLEG302000","Harmony XB5, Antimikrobiálna samolepiaca fólia 300 x 200, bez symbolu",0]
["ZBYLEG201000","Samolepiaca fólia bez symbolov",1,"ks",{"v":39.65019974999999,"d":"39.650"},"3606489755690",{"v":22,"d":"22.00"},{"v":0.5,"d":"0.50"},{"v":22,"d":"22.00"},{"v":60,"d":"60.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYLEG201000","Harmony XB5, Antimikrobiálna samolepiaca fólia 200 x 100, bez symbolu",""]
["ZBYLEG101000","Samolepiaca fólia bez symbolov",1,"ks",{"v":76.8663,"d":"76.866"},"3606489755676",{"v":22,"d":"22.00"},{"v":0.5,"d":"0.50"},{"v":22,"d":"22.00"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBYLEG101000","Harmony XB5, Antimikrobiálna samolepiaca fólia 100 x 100 mm, bez symbolu",0]
["ZBYD06102","POPISNÝ ŠTÍTOK 19X27MM PRE XALG",10,"ks",{"v":5.673464999999999,"d":"5.673"},"3389110974379",{"v":6,"d":"6.00"},{"v":1.5,"d":"1.50"},{"v":4.5,"d":"4.50"},{"v":0.8,"d":"0.80"},"DE","3919908099","https://www.se.com/sk/sk/product/ZBYD06102","self-adhesive blank legend - 19 x 27 mm - grey background - set of 10",0]
["ZBY9W3B501","Okrúhly štítok, podsvietený, 24 V, B/Č",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3606481919632",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":20,"d":"20.00"},"ID","8538909999","https://www.se.com/sk/sk/product/ZBY9W3B501","Okrúhly štítok, podsvietený, 24 V, dvojfarebný biela/červená, LED, neoznačený",0]
["ZBY9W3B330","KRUH. ŠTÍTOK ŽLTÝ \"S POPISOM\" 24V",1,"ks",{"v":24.707024999999998,"d":"24.707"},"3606489745387",{"v":6,"d":"6.00"},{"v":0.7,"d":"0.70"},{"v":6,"d":"6.00"},{"v":21,"d":"21.00"},"ID","8538909999","https://www.se.com/sk/sk/product/ZBY9W3B330","Illuminated ring 60mm, Harmony, plastic, yellow, white or red integral LED, marked EMERGENCY STOP, 24V AC DC",0]
["ZBY9W3B140","KRUH. ŠTÍTOK ŽLTÝ \"S POPISOM\" 24V",1,"ks",{"v":24.707024999999998,"d":"24.707"},"3606489745400",{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":16,"d":"16.00"},"ID","8538909999","https://www.se.com/sk/sk/product/ZBY9W3B140","Illuminated ring 60mm, Harmony, plastic, yellow, white or red integral LED, unmarked, 24V AC DC",0]
["ZBY9W3B101","KRUH. ŠTÍTOK ŽLTÝ \"S POPISOM\" 24V",1,"ks",{"v":24.707024999999998,"d":"24.707"},"3606489745370",{"v":8.5,"d":"8.50"},{"v":2.5,"d":"2.50"},{"v":6.5,"d":"6.50"},{"v":210,"d":"210.00"},"ID","8538909999","https://www.se.com/sk/sk/product/ZBY9W3B101","Podsvietený kruhový štítok núdzového zastavenia, bez popisu, 24V AC/DC",0]
["ZBY9W2B330","KRUH. ŠTÍTOK ŽLTÝ \"S POPISOM\" 24V",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3606489745141",{"v":8.5,"d":"8.50"},{"v":2.2,"d":"2.20"},{"v":6.5,"d":"6.50"},{"v":16,"d":"16.00"},"ID","85389099","https://www.se.com/sk/sk/product/ZBY9W2B330","Illuminated ring 60mm, Harmony, plastic, yellow, red fixed integral LED, marked EMERGENCY STOP, 24V AC DC",0]
["ZBY9W2B140","KRUH. ŠTÍTOK ŽLTÝ \"S POPISOM\" 24V",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3606489745165",{"v":8.5,"d":"8.50"},{"v":2.2,"d":"2.20"},{"v":6.5,"d":"6.50"},{"v":16,"d":"16.00"},"ID","8538909999","https://www.se.com/sk/sk/product/ZBY9W2B140","Illuminated ring 60mm, Harmony, plastic, yellow, red fixed integral LED, unmarked, 24V AC DC",0]
["ZBY9T30","KRUH. ŠTÍTOK ŽLTÝ NOUZOVÉ ZASTAVENÍ",1,"ks",{"v":4.3008525,"d":"4.301"},"3389119055178",{"v":6,"d":"6.00"},{"v":0.1,"d":"0.10"},{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},"FR","39269097","https://www.se.com/sk/sk/product/ZBY9T30","štítok - NOUZOVÉ ZASTAVENÍ - 60 mm",0]
["ZBY9PL30","Kruhový štítok \"AWARYJNY\"",1,"ks",{"v":2.69947125,"d":"2.699"},"3389119607469",{"v":6,"d":"6.00"},{"v":0.1,"d":"0.10"},{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},"DE","39269097","https://www.se.com/sk/sk/product/ZBY9PL30","Marked legend, Harmony XB5, Harmony XB4, yellow, 60mm, for emergency stop, marked STOP AWARYJNY/logo ISO13850",0]
["ZBY9530","Kruhový štítok na núdzové zastavenie",1,"ks",{"v":5.44469625,"d":"5.445"},"3389119023252",{"v":9,"d":"9.00"},{"v":0.5,"d":"0.50"},{"v":9,"d":"9.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY9530","kruhový štítok na núdzové zastavenie",0]
["ZBY9420","3D ŠTÍTOK PRE NÚDZOVÉ ZASTAVENIE",5,"ks",{"v":3.1112549999999994,"d":"3.111"},"3606480687488",{"v":6,"d":"6.00"},{"v":0.4,"d":"0.40"},{"v":6,"d":"6.00"},{"v":4,"d":"4.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZBY9420","3D kruhový štítok na núdzové zastavenie, PARADA DE EMERGENCIA",0]
["ZBY9360","KRUH. ŠTÍTOK \"EMERGENCY Switching OFF\"",10,"ks",{"v":2.15042625,"d":"2.150"},"3389119041065",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},"FR","4911990000","https://www.se.com/sk/sk/product/ZBY9360","štítok s popisom Ø60 pre núdzové zastav.-EMERGENCY SWITCHING OFF/logo ISO13850",0]
["ZBY9330T","KRUH. ŠTÍTOK \"EMERGENCY STOP\"",1,"ks",{"v":11.4384375,"d":"11.438"},"3389119020510",{"v":6.5,"d":"6.50"},{"v":0.1,"d":"0.10"},{"v":6.5,"d":"6.50"},{"v":0.9,"d":"0.90"},"FR","4911990000","https://www.se.com/sk/sk/product/ZBY9330T","štít. s popisom Ø60 pre núdz. zastav.- EMERGENCY STOP/logo ISO13850",0]
["ZBY9330M","KRUH. ŠTÍTOK \"EMERGENCY STOP\"",10,"ks",{"v":10.980899999999998,"d":"10.981"},"3606481202109",{"v":6,"d":"6.00"},{"v":1,"d":"1.00"},{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY9330M","Marked legend, Harmony XB4, Harmony XB5, yellow, 60mm, for emergency stop, marked EMERGENCY STOP/logo ISO13850",0]
["ZBY9320","3D štítok pre núdz.zastav.EMERGENCY STOP",1,"ks",{"v":3.1112549999999994,"d":"3.111"},"3606480561276",{"v":6,"d":"6.00"},{"v":0.5,"d":"0.50"},{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZBY9320","3D kruhový štítok na núdzové zastavenie, EMERGENCY STOP",0]
["ZBY9260","YELLOW CIRCULAR LEGEND NOT AUS DIA60MM",1,"ks",{"v":1.9674112499999996,"d":"1.967"},"3389119041058",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY9260","štítok s popisom Ø60 pre núdzové zastavenie- NOT - AUS/logo ISO13850",0]
["ZBY9230T","Štítok NOT HALT, 60 mm",1,"ks",{"v":8.18992125,"d":"8.190"},"3389119020527",{"v":12,"d":"12.00"},{"v":0.1,"d":"0.10"},{"v":8,"d":"8.00"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY9230T","štítok s popisom Ø60 pre núdzové zastavenie-NOT-HALT/logo ISO13850",0]
["ZBY9220","3D ŠTÍTOK PRE NÚDZOVÉ ZASTAVENIE",5,"ks",{"v":3.1112549999999994,"d":"3.111"},"3606480561269",{"v":6,"d":"6.00"},0.56,{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZBY9220","3D kruhový štítok na núdzové zastavenie, NOT-HALT",0]
["ZBY91SK","KRUH. ŠTÍTOK ŽLTÝ NÚDZOVÉ ZASTAVENIE",1,"ks",{"v":3.7060537499999993,"d":"3.706"},"3606481976321",{"v":6,"d":"6.00"},{"v":0.1,"d":"0.10"},{"v":6,"d":"6.00"},{"v":2.2,"d":"2.20"},"FR","39269097","https://www.se.com/sk/sk/product/ZBY91SK","Engraving NÃƒÅ¡DZOVÃƒâ€° ZASTAVENIE",0]
["ZBY9140T","KRUHOVÝ ŠTÍTOK NÚDZOVÉHO ZASTAVENIE 60MM",10,"ks",{"v":5.71921875,"d":"5.719"},"3389119041027",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY9140T","neoznačený štítok Ø60 pre tlačítko núdzového zastavenia",0]
["ZBY9140M","KRUHOVÝ ŠTÍTOK NÚDZOVÉHO ZASTAVENIE 60MM",10,"ks",{"v":3.8433149999999996,"d":"3.843"},"3606481202079",{"v":6,"d":"6.00"},{"v":1,"d":"1.00"},{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},"FR","39269097","https://www.se.com/sk/sk/product/ZBY9140M","Blank legend, Harmony XB4, Harmony XB5, unmarked Ø 60 for emergency stop pushbutton/logo ISO13850",0]
["ZBY9130T","KRUH. ŠTÍTOK ŽlTÝ ARRET D URGENCE",1,"ks",{"v":3.1112549999999994,"d":"3.111"},"3389119020503",{"v":12,"d":"12.00"},{"v":0.1,"d":"0.10"},{"v":8,"d":"8.00"},{"v":0.9,"d":"0.90"},"FR","4911990000","https://www.se.com/sk/sk/product/ZBY9130T","štít. s popisom Ø60 pre núdz. zastav.- ARRET D'URGENCE/logo ISO13850",0]
["ZBY9121","3D ŠTÍTOK PRE NÚDZOVÉ ZAST., BEZ POPISU",5,"ks",{"v":2.4707025,"d":"2.471"},"3606480561245",{"v":6,"d":"6.00"},0.56,{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZBY9121","okrúhly štítok Ø 60 – pre tlačidlo núdz. vyp.",0]
["ZBY9120","3D ŠTÍTOK PRE NÚDZOVÉ ZASTAVENIE",5,"ks",{"v":3.1112549999999994,"d":"3.111"},"3606480561252",{"v":6,"d":"6.00"},0.56,{"v":6,"d":"6.00"},{"v":4,"d":"4.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZBY9120","3D kruhový štítok na núdzové zastavenie, ARRET D'URGENCE",0]
["ZBY9101","KRUH.ŠTÍTOK ŽLTÝ BEZ POPISU",1,"ks",{"v":2.15042625,"d":"2.150"},"3389110099256",{"v":7,"d":"7.00"},{"v":1.4,"d":"1.40"},{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY9101","Blank legend, Harmony XB4, Harmony XB5, unmarked, 60mm, for emergency switching off pushbutton",0]
["ZBY8L330","Štítok - núdzové zastavenie, 90mm",10,"ks",{"v":3.9348224999999992,"d":"3.935"},"3606489745004",{"v":9,"d":"9.00"},{"v":0.1,"d":"0.10"},{"v":9,"d":"9.00"},{"v":0.9,"d":"0.90"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZBY8L330","Štítok, Harmony XB4, Harmony XB5, Ø 90 pre podsvietený ovládač núdzového zastavenia, s textom EMERGENCY STOP a s logom",0]
["ZBY8530","okrúhly štítok Ø 90, pre tlač. núdz. zas",1,"ks",{"v":2.8824862499999995,"d":"2.882"},"3389119023245",{"v":11,"d":"11.00"},{"v":0.5,"d":"0.50"},{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY8530","okrúhly štítok Ø 90 – pre tlačidlo núdz. zast. – žltý – NOODSTOP",0]
["ZBY8430","KRUH. ŠTÍTOK EMERGENCY STOP",10,"ks",{"v":2.5622099999999994,"d":"2.562"},"3389110099454",{"v":9,"d":"9.00"},{"v":1,"d":"1.00"},{"v":9,"d":"9.00"},{"v":5,"d":"5.00"},"FR","4911990000","https://www.se.com/sk/sk/product/ZBY8430","okrúhly štítok Ø 90 – pre tlačidlo núdz. vyp. – žltý – PARADA DE EMERGENCIA",0]
["ZBY8330","KRUH. ŠTÍTOK \"EMERGENCY STOP\"",1,"ks",{"v":2.60796375,"d":"2.608"},"3389110099379",{"v":9,"d":"9.00"},{"v":0.1,"d":"0.10"},{"v":9,"d":"9.00"},{"v":5.1,"d":"5.10"},"FR","4911990000","https://www.se.com/sk/sk/product/ZBY8330","okrúhly štítok Ø 90 – pre tlačidlo núdz. vyp. – žltý – EMERGENCY STOP",0]
["ZBY8230","ŠTÍTOK NOT HALT",10,"ks",{"v":2.60796375,"d":"2.608"},"3389110099416",{"v":9,"d":"9.00"},{"v":0.1,"d":"0.10"},{"v":9,"d":"9.00"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY8230","okrúhly štítok Ø 90 – pre tlačidlo núdz. vyp. – žltý – NOT-AUS",0]
["ZBY8130","ŠTÍTOK E STOP",1,"ks",{"v":2.5622099999999994,"d":"2.562"},"3389110099355",{"v":9,"d":"9.00"},{"v":0.1,"d":"0.10"},{"v":9,"d":"9.00"},{"v":4.8,"d":"4.80"},"FR","4911990000","https://www.se.com/sk/sk/product/ZBY8130","okrúhly štítok Ø 90 – pre tlačidlo núdz. vyp. – žltý – ARRET D'URGENCE",0]
["ZBY8101","KRUH.ŠTÍTOK ŽLTÝ BEZ POPISU",10,"ks",{"v":2.1961799999999996,"d":"2.196"},"3389110099348",{"v":9,"d":"9.00"},{"v":0.1,"d":"0.10"},{"v":9,"d":"9.00"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY8101","okrúhly štítok Ø 90 – pre tlačidlo núdz. vyp. – žltý – bez označenia",0]
["ZBY6H102","NOSIČ + ŠTÍTOK BEZ POPISU",10,"ks",{"v":2.1961799999999996,"d":"2.196"},"3389110095937",{"v":16,"d":"16.00"},{"v":3,"d":"3.00"},{"v":11,"d":"11.00"},{"v":4,"d":"4.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY6H102","držiak štítkov 30 x 50 mm s prázd. štítk. – pre jednotky Ø 22 s guľ. hlavicou",0]
["ZBY6H101","NOSIČ + ŠTÍTOK BEZ POPISU",10,"ks",{"v":2.1961799999999996,"d":"2.196"},"3389110095920",{"v":15,"d":"15.00"},{"v":3,"d":"3.00"},{"v":12,"d":"12.00"},{"v":3.7,"d":"3.70"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY6H101","držiak štítkov 30 x 50 mm s prázd. štítk. – pre jednotky Ø 22 s guľ. hlavicou",0]
["ZBY6102","NOSIČ ŠTÍTKOV",10,"ks",{"v":1.5556274999999997,"d":"1.556"},"3389110095876",{"v":12,"d":"12.00"},{"v":2,"d":"2.00"},{"v":10,"d":"10.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY6102","držiak štítkov 30 x 50 mm s prázd. štítk. – pre jednotky Ø 22 s guľ. hlavicou",0]
["ZBY6101","NOSIČ ŠTÍTKOV",10,"ks",{"v":2.013165,"d":"2.013"},"3389110095869",{"v":5,"d":"5.00"},{"v":0.5,"d":"0.50"},{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY6101","držiak štítkov 30 x 50 mm s prázd. štítk. – pre jednotky Ø 22 s guľ. hlavicou",0]
["ZBY5102","ŠTÍTKY NA GRAVÍROVANIE",10,"ks",{"v":0.7320599999999999,"d":"0.732"},"3389110098587",{"v":2.5,"d":"2.50"},{"v":0.1,"d":"0.10"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY5102","prázd. štítok 18 x 27mm – pre drž.štítk. 30 x 50mm – biely + žltý – bez označ.",0]
["ZBY5101","ŠTÍTKY NA GRAVÍROVANIE",10,"ks",{"v":0.7320599999999999,"d":"0.732"},"3389110098570",{"v":3,"d":"3.00"},{"v":0.1,"d":"0.10"},{"v":1.5,"d":"1.50"},{"v":1,"d":"1.00"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY5101","prázd.štítok 18 x 27 mm – pre drž.štítk. 30 x 50 mm – čier.+červ. – bez označ.",0]
["ZBY5100","HÁROK SAMOLEP. ŠTÍTKOV",10,"ks",{"v":7.4121074999999985,"d":"7.412"},"3389110098631",{"v":30,"d":"30.00"},{"v":0.2,"d":"0.20"},{"v":21.5,"d":"21.50"},{"v":41.7,"d":"41.70"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY5100","hárok so 40 štítkami 18 x 27 mm – pre držiak štítkov 30 x 50 mm – bez označenia",0]
["ZBY4H101","NOSIČ ŠTÍTKOV + PRÁZDNY ŠTÍTOK",10,"ks",{"v":2.1961799999999996,"d":"2.196"},"3389110095906",{"v":12,"d":"12.00"},{"v":4,"d":"4.00"},{"v":10,"d":"10.00"},{"v":3,"d":"3.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY4H101","držiak štítkov 30 x 40 mm s prázd. štítk. – pre jednotky Ø 22 s guľ. hlavicou",0]
["ZBY41101","NOSIČ ŠTÍTKOV, PLAST",1,"ks",{"v":1.3268587499999998,"d":"1.327"},"3389119043205",{"v":5,"d":"5.00"},{"v":1,"d":"1.00"},{"v":4.5,"d":"4.50"},{"v":0.7,"d":"0.70"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY41101","štítok 30 X 40 žltá - čierne značky",0]
["ZBY4101","NOSIČ ŠTÍTKOV",10,"ks",{"v":2.0589187499999997,"d":"2.059"},"3389110092639",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":1.2,"d":"1.20"},"FR","39269097","https://www.se.com/sk/sk/product/ZBY4101","držiak štítk. 30 x 40 mm s priesvit. štítk. na vygravírovanie – pre jedn. Ø 22",0]
["ZBY4100","HÁROK SAMOLEP. ŠTÍTKOV",10,"ks",{"v":7.686629999999999,"d":"7.687"},"3389110098594",{"v":29.7,"d":"29.70"},{"v":0.2,"d":"0.20"},{"v":21,"d":"21.00"},{"v":39,"d":"39.00"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY4100","hárok so 76 sťah. štítkami 8 x 27 mm – pre držiak štítk. 30 x 40 mm – bez označ.",0]
["ZBY2H101","NOSIČ ŠTÍTKOV VYSOKÝ S PRÁZDNYM ŠTÍTKOM",10,"ks",{"v":2.013165,"d":"2.013"},"3389110095890",{"v":3,"d":"3.00"},{"v":0.8,"d":"0.80"},{"v":4,"d":"4.00"},{"v":3,"d":"3.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2H101","držiak štítkov 30 x 40 mm s prázd. štítk. – pre jednotky Ø 22 s guľ. hlavicou",0]
["ZBY2387","ŠTÍTOK S POPISOM HAND-OFF-AUTO",10,"ks",{"v":2.0589187499999997,"d":"2.059"},"3389110094169",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2387","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom HAND-OFF-AUTO",0]
["ZBY2385","ŠTÍTOK S POPISOM AUTO-O-HAND",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110094619",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2385","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom AUTO - O - HAND",0]
["ZBY2367","ŠTANDARDNÝ NOSIČ ŠTÍTKOV OFF-ON",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110094176",{"v":4,"d":"4.00"},{"v":0.2,"d":"0.20"},{"v":3,"d":"3.00"},{"v":1.2,"d":"1.20"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2367","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom OFF-ON",0]
["ZBY2366","ŠTÍTOK S NÁPISOM STOP ŠTART",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110124927",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2366","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom STOP-START",0]
["ZBY2364","NOSIČ ŠTÍTKOV, AUTO-HAND",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110094541",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2364","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom AUTO-HAND",0]
["ZBY2334","NOSIČ ŠTÍTKU S NÁPISOM RUN",1,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110094398",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2334","držiak štítkov 30x40 mm so štítkom 8x27 mm s označením RUN",0]
["ZBY2330","NOSIČ ŠTÍTKOV EMERGENCY STOP",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110094053",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2330","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom EMERGENCY STOP",0]
["ZBY2326","ŠTÍTOK S POPISOM POWER ON",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110840933",{"v":4.2,"d":"4.20"},{"v":0.4,"d":"0.40"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2326","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom POWER ON",0]
["ZBY2323","ŠTÍTOK S POPISOM RESET",10,"ks",{"v":2.0589187499999997,"d":"2.059"},"3389110840957",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2323","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom RESET",0]
["ZBY2322","ŠTANDARDNÝ NOSIČ ŠTÍTKOV RESET",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110124910",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2322","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom RESET",0]
["ZBY2314","NOSIČ ŠTÍTKOV, CLOSE",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110093988",{"v":8,"d":"8.00"},{"v":1,"d":"1.00"},{"v":0.4,"d":"0.40"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2314","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom CLOSE",0]
["ZBY2313","NOSIČ ŠTÍTKOV, OPEN",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110094237",{"v":8,"d":"8.00"},{"v":1.5,"d":"1.50"},{"v":0.4,"d":"0.40"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2313","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom OPEN",0]
["ZBY2312","ŠTÍTOK S POPISOM OFF",1,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110840179",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2312","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom OFF",0]
["ZBY2311","ŠTÍTOK S POPISOM OFF",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110840841",{"v":4,"d":"4.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2311","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom ON",0]
["ZBY2308","ŠTÍTOK S POPISOM DOWN",1,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110839982",{"v":4,"d":"4.00"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2308","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom DOWN",0]
["ZBY2307","ŠTÍTOK S POPISOM UP",1,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110842098",{"v":4,"d":"4.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2307","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom UP",0]
["ZBY2306","ŠTÍTOK S POPISOM REVERSE",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110840988",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2306","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom REVERSE",0]
["ZBY2305","ŠTÍTOK S POPISOM FORWARD",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110839999",{"v":4,"d":"4.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2305","legend holder 30 x 40 mm with legend 8 x 27 mm with marking FORWARD",0]
["ZBY2304","ŠTÍTOK STOP",10,"ks",{"v":2.013165,"d":"2.013"},"3389110841305",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2304","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom STOP",0]
["ZBY2303","ŠTÍTOK S POPISOM START",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110841268",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1.1,"d":"1.10"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2303","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom START",0]
["ZBY2186","NOSIČ ŠTÍTKOV",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110092875",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1.1,"d":"1.10"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2186","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom I-O-II",0]
["ZBY2185","Štítok s nápismi AUTO 0 MAIN",1,"ks",{"v":2.3791949999999997,"d":"2.379"},"3389110093797",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2185","Štítok s nápismi AUTO 0 MAIN",0]
["ZBY2179","NOSIČ ŠTÍTKOV SO SYMBOLOM",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110092790",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2179","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom I-II",0]
["ZBY2178","NOSIČ ŠTÍTKOV",1,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110840247",{"v":4,"d":"4.00"},{"v":0.4,"d":"0.40"},{"v":3,"d":"3.00"},0.99,"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2178","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom O-I",0]
["ZBY2147","NOSIČ ŠTÍTKOV",10,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110840568",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2147","držiak štítkov 30 x 40 mm – pre jednotky Ø 22 – so štítkom I",0]
["ZBY2130","PORTAETIQUETA FR. EMERGENCIA",1,"ks",{"v":2.8367324999999997,"d":"2.837"},"3389110093018",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2130","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom ARRET D'URGENCE",0]
["ZBY2126","ŠTANDARDNÝ NOSIČ ŠTÍTKOV SOUS TENSION",1,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110093667",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2126","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom SOUS TENSION",0]
["ZBY2107","ŠTÍTOK S POPISOM MONTEE",1,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110093414",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2107","Legend holder, Harmony XB4, 30 x 40mm, plastic, 8 x 27mm legend, white marked MONTEE",0]
["ZBY2103","ŠTANDARDNÝ NOSIČ ŠTÍTKOV MARCHE",1,"ks",{"v":2.1046724999999995,"d":"2.105"},"3389110093384",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2103","držiak štítkov 30x40 mm so štítkom 8x27 mm s popisom MARCHE",0]
["ZBY2101","NOSIČ ŠTÍTKOV",10,"ks",{"v":2.0589187499999997,"d":"2.059"},"3389110839968",{"v":4,"d":"4.00"},{"v":0.3,"d":"0.30"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBY2101","držiak štítk. 30 x 40 mm s priesvit. štítk. na vygravírovanie – pre jedn. Ø 22",0]
["ZBY1147","HÁROK SAMOLEP. ŠTÍTKOV",10,"ks",{"v":4.483867500000001,"d":"4.484"},"3389110098815",{"v":15,"d":"15.00"},{"v":0.1,"d":"0.10"},{"v":11,"d":"11.00"},{"v":10,"d":"10.00"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY1147","hárok so 66 sťahovacími priesvitnými samolepiacimi štítkami – okrúhle – I",0]
["ZBY1101","HÁROK SAMOLEP. ŠTÍTKOV",10,"ks",{"v":4.07208375,"d":"4.072"},"3389110098792",{"v":30,"d":"30.00"},{"v":0.1,"d":"0.10"},{"v":22,"d":"22.00"},{"v":16,"d":"16.00"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY1101","strana 66 neoznačených štítkov",0]
["ZBY02304","ŠTÍTKY SO SYMBOLMI 8X27 MM",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110096224",{"v":10,"d":"10.00"},{"v":7,"d":"7.00"},{"v":0.1,"d":"0.10"},{"v":0.3,"d":"0.30"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY02304","označený štítok 8 x 27 mm – pre držiak štítkov 30 x 40 mm – STOP",0]
["ZBY02178","ŠTÍTKY SO SYMBOLMI 8X27 MM",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110096163",{"v":1,"d":"1.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.3,"d":"0.30"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY02178","označený štítok 8 x 27 mm – pre držiak štítkov 30 x 40 mm – O-I",0]
["ZBY0102","ŠTÍTKY NA GRAVÍROVANIE 8x27mm",10,"ks",{"v":1.5098737499999997,"d":"1.510"},"3389110096040",{"v":2.7,"d":"2.70"},{"v":0.1,"d":"0.10"},{"v":0.9,"d":"0.90"},{"v":0.2,"d":"0.20"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY0102","prázd. štítok 8 x 27 mm – pre drž.štítk. 30 x 40mm – biely + žltý – bez označ.",0]
["ZBY0101","ŠTÍTKY NA GRAVÍROVANIE 8x27mm",10,"ks",{"v":1.5098737499999997,"d":"1.510"},"3389110096026",{"v":2.5,"d":"2.50"},{"v":1,"d":"1.00"},{"v":4.6,"d":"4.60"},{"v":0.3,"d":"0.30"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY0101","prázd. štítok 8 x 27 mm – pre drž.štítk. 30 x 40 mm – čier. + červ. – bez ozn.",0]
["ZBY001","HÁROK ŠTÍTKOV PRE ZBZ001",10,"ks",{"v":4.98715875,"d":"4.987"},"3389110090574",{"v":30,"d":"30.00"},{"v":0.2,"d":"0.20"},{"v":21,"d":"21.00"},{"v":13,"d":"13.00"},"FR","3919908099","https://www.se.com/sk/sk/product/ZBY001","hárok s 50 prázdnymi štítkami – pre držiak štítkov – bez označenia",0]
["ZBW9143","HMATNÍK PRE PRESV. HLAVICU CERVENY",10,"ks",{"v":1.8301499999999997,"d":"1.830"},"3389110100884",{"v":10,"d":"10.00"},{"v":12,"d":"12.00"},{"v":1.5,"d":"1.50"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBW9143","červená hladká šošovka – pre okrúhle osvetlené tlačidlo Ø 22",0]
["ZBW9133","HMATNÍK PRE PRESV. STLÁČ. HLAVICU ZELENY",1,"ks",{"v":1.8301499999999997,"d":"1.830"},"3389110100754",{"v":6.5,"d":"6.50"},{"v":2,"d":"2.00"},{"v":4.5,"d":"4.50"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBW9133","zelená hladká šošovka – pre okrúhle osvetlené tlačidlo Ø 22",0]
["ZBW911","HMATNÍK PRE PRESV. STLÁČ. HLAVICU BIELY",10,"ks",{"v":1.5098737499999997,"d":"1.510"},"3389110100570",{"v":10,"d":"10.00"},{"v":12,"d":"12.00"},{"v":1.5,"d":"1.50"},{"v":15,"d":"15.00"},"CZ","85389099","https://www.se.com/sk/sk/product/ZBW911","biela hladká šošovka – pre okrúhle osvetlené tlačidlo Ø 22",0]
["ZBW008A","OCHRANNÁ KRYTKA PRE DVOJTLAČÍTKO",10,"ks",{"v":3.6602999999999994,"d":"3.660"},"3389110102000",{"v":15,"d":"15.00"},{"v":6,"d":"6.00"},{"v":9,"d":"9.00"},{"v":5,"d":"5.00"},"FR","4016999790","https://www.se.com/sk/sk/product/ZBW008A","ochranná krytka pre dvojité tlačidlo Ø 22 mm – číra – súprava 10 ks",0]
["ZBVM15","OBJÍMKA LED BIELA PRUŽNÁ 230 240V",4,"ks",{"v":12.353512499999999,"d":"12.354"},"3389119037594",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":4,"d":"4.00"},{"v":9,"d":"9.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVM15","objímka – Ø 22 – zabud. biela LED – 230 - 240 V",0]
["ZBVM14","OBJÍMKA LED PRE KONEKTOR BIELA",5,"ks",{"v":13.2685875,"d":"13.269"},"3389110090284",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":3.5,"d":"3.50"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVM14","objímka – Ø 22 – zabud. biela LED – 230 - 240 V",0]
["ZBVM1","OBJÍMKA LED BIELA",5,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110090031",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVM1","objímka – Ø 22 – zabud. biela LED – 230 - 240 V",0]
["ZBVJ15","OBJÍMKA LED BIELA PRUŽNÁ 12V AC/DC",1,"ks",{"v":8.876227499999999,"d":"8.876"},"3389119037440",{"v":4.4,"d":"4.40"},{"v":1,"d":"1.00"},{"v":3.8,"d":"3.80"},{"v":10,"d":"10.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVJ15","Light block, Harmony XB4, Harmony XB5, for head 22mm, universal LED, spring clamp terminals, 12V",0]
["ZBVJ1","OBJÍMKA LED BIELA",5,"ks",{"v":7.549368749999999,"d":"7.549"},"3389110069907",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":9,"d":"9.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVJ1","objímka – Ø 22 – zabud. biela LED – 12 V",0]
["ZBVGM1T","Objímka LED",1,"ks",{"v":10.5233625,"d":"10.523"},"3606481856326",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":3.3,"d":"3.30"},{"v":9,"d":"9.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVGM1T","Objímka LED",0]
["ZBVG15","OBJÍMKA LED BIELA PRUŽNÁ 110 120V",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389119037549",{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":4,"d":"4.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVG15","Light block, Harmony XB4, Harmony XB5, for head 22mm, universal LED, spring clamp terminals, 110...120V",0]
["ZBVG1","OBJÍMKA LED BIELA",5,"ks",{"v":11.4384375,"d":"11.438"},"3389110089660",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":9,"d":"9.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVG1","objímka – Ø 22 – zabud. biela LED – 48 - 120 V",0]
["ZBVBG1","OBJÍMKA LED 24-120V AC/DC BIELA",5,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110070422",{"v":5.6,"d":"5.60"},{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":9,"d":"9.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVBG1","objímka – Ø 22 – zabud. biela LED – 24 - 120 V",0]
["ZBVB57","OBJÍMKA LED DO PLOŠNÉHO SPOJA ŽLTÁ",5,"ks",{"v":10.5233625,"d":"10.523"},"3389110090420",{"v":6.6,"d":"6.60"},{"v":2.2,"d":"2.20"},{"v":3.3,"d":"3.30"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVB57","Light block, Harmony XB4, Harmony XB5, orange, for head 22mm integral LED, pins for printed circuit board, 24V",0]
["ZBVB47","OBJÍMKA LED DO PLOŠNÉHO SPOJA ČERVENÁ",5,"ks",{"v":10.5233625,"d":"10.523"},"3389110090390",{"v":6.5,"d":"6.50"},{"v":2.1,"d":"2.10"},{"v":3.3,"d":"3.30"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVB47","Light block, Harmony XB4, Harmony XB5, red, for head 22mm integral LED, pins for printed circuit board, 24V",0]
["ZBVB37","OBJÍMKA LED DO PLOŠNÉHO SPOJA ZELENÁ",5,"ks",{"v":10.5233625,"d":"10.523"},"3389110090376",{"v":6.6,"d":"6.60"},{"v":2.2,"d":"2.20"},{"v":3.3,"d":"3.30"},{"v":2,"d":"2.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVB37","objímka – Ø 22 – zabud. zelená LED – 24 V",0]
["ZBVB19","OBJÍMKA LED BIELA",5,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110177619",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":2,"d":"2.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVB19","biela objímka pre hlavu Ø22 integrovaná LED 24V šróbové svorky",0]
["ZBVB17","OBJÍMKA LED DO PLOŠNÉHO SPOJA BIELA",5,"ks",{"v":10.5233625,"d":"10.523"},"3389110090369",{"v":5,"d":"5.00"},{"v":0.5,"d":"0.50"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVB17","biela objímka pre hlavu Ø22 integrovaná LED 24V piny",0]
["ZBVB15","OBJÍMKA LED BIELA-PRUŽNÁ-24V AC/DC",4,"ks",{"v":10.065825,"d":"10.066"},"3389119037495",{"v":5.2,"d":"5.20"},{"v":5.6,"d":"5.60"},{"v":4.2,"d":"4.20"},{"v":10,"d":"10.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVB15","biela objímka pre hlavu Ø22 integrovaná LED 24V bezskrut. svorky",0]
["ZBVB14","OBJÍMKA LED PRE KONEKTOR BIELA",5,"ks",{"v":8.784719999999998,"d":"8.785"},"3389110090147",{"v":5.2,"d":"5.20"},{"v":5.4,"d":"5.40"},{"v":4.3,"d":"4.30"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVB14","biela objímka pre hlavu Ø22 integrovaná LED 24V zásuvný konektor",0]
["ZBVB1","OBJÍMKA LED BIELA",5,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110089615",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":3.3,"d":"3.30"},{"v":8.8,"d":"8.80"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBVB1","objímka – Ø 22 – zabud. biela LED – 24 V",0]
["ZBV6","OBJÍMKA PRE ŽIAROVKU BA9s",5,"ks",{"v":3.61454625,"d":"3.615"},"3389110089608",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":8.4,"d":"8.40"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBV6","objímka – Ø 22 – základňa BA 9s – 250 V",0]
["ZBV5B","Transformátor 400 / 24 V",1,"ks",{"v":27.45225,"d":"27.452"},"3389119039789",{"v":5.2,"d":"5.20"},{"v":5.7,"d":"5.70"},{"v":4.4,"d":"4.40"},{"v":90,"d":"90.00"},"ID","8504318090","https://www.se.com/sk/sk/product/ZBV5B","blok transf. pre svetelný blok s integrovanou LED - 400V",0.01]
["ZBV18M1","Objímka LED, blik, 230V",1,"ks",{"v":26.537175,"d":"26.537"},"3389110861235",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":3.5,"d":"3.50"},{"v":9,"d":"9.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBV18M1","biela blikajúca objímka Ø22 integrovaná LED 230V skrut. svorky",0]
["ZBV18B1","Obja LED 24 V blikaj",1,"ks",{"v":26.537175,"d":"26.537"},"3389110861136",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":3.5,"d":"3.50"},{"v":9,"d":"9.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZBV18B1","biela blikajúca objímka Ø22 integrovaná LED 24V skrut. svorky",0]
["ZBV017","KRUHOVÁ ŠOŠ. PRE SIGNÁLKY ČÍRA",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110099867",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":5,"d":"5.00"},{"v":2,"d":"2.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBV017","číra hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV0163","ŠTVORC. ŠOŠ. PRE SIGNÁLKY - LED MODRÁ",1,"ks",{"v":1.4183662499999998,"d":"1.418"},"3389110100006",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBV0163","modrá hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV016","KRUHOVÁ ŠOŠ. PRE SIGNÁLKY MODRÁ",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110099843",{"v":10,"d":"10.00"},{"v":3,"d":"3.00"},{"v":1.5,"d":"1.50"},{"v":20,"d":"20.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBV016","modrá hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV0153","ŠTVORC. ŠOŠ. PRE SIGNÁLKY - LED ŽLTÁ",10,"ks",{"v":1.4183662499999998,"d":"1.418"},"3389110099959",{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBV0153","žltá hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV015","KRUHOVÁ ŠOŠ. PRE SIGNÁLKY ŽLTÁ",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110099836",{"v":8,"d":"8.00"},{"v":3.5,"d":"3.50"},{"v":5,"d":"5.00"},{"v":2,"d":"2.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBV015","žltá hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV0143","ŠTVORC. ŠOŠ. PRE SIGNÁLKY - LED ČERVENÁ",1,"ks",{"v":1.3726124999999998,"d":"1.373"},"3389110099898",{"v":2.9,"d":"2.90"},{"v":0.9,"d":"0.90"},{"v":2.9,"d":"2.90"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBV0143","červená hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV014","KRUHOVÁ ŠOŠ. PRE SIGNÁLKY ČERVENÁ",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110099829",{"v":10,"d":"10.00"},{"v":12,"d":"12.00"},{"v":1.5,"d":"1.50"},{"v":2,"d":"2.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBV014","červená hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV0133","ŠTVORC. ŠOŠ. PRE SIGNÁLKY - LED ZELENÁ",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110099881",{"v":5.7,"d":"5.70"},{"v":5.7,"d":"5.70"},{"v":4.4,"d":"4.40"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBV0133","zelená hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV013","KRUHOVÁ ŠOŠ. PRE SIGNÁLKY ZELENÁ",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110099812",{"v":2.8,"d":"2.80"},{"v":1,"d":"1.00"},{"v":2.8,"d":"2.80"},{"v":2,"d":"2.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBV013","zelená hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV0113","ŠTVORC. ŠOŠ. PRE SIGNÁLKY - LED BIELA",10,"ks",{"v":2.9282399999999997,"d":"2.928"},"3389110099874",{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBV0113","biela hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBV011","KRUHOVÁ ŠOŠ. PRE SIGNÁLKY BIELA",10,"ks",{"v":1.1438437499999998,"d":"1.144"},"3389110099799",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},{"v":2,"d":"2.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBV011","biela hladká šošovka – pre okrúhlu kontrolku Ø 22",0]
["ZBSP3","USB/RJ45 ochranný kryt IP65/IP67/IP 69K",1,"ks",{"v":81.89921249999999,"d":"81.899"},"3606481194244",{"v":6,"d":"6.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":13,"d":"13.00"},"DE","7326909890","https://www.se.com/sk/sk/product/ZBSP3","USB/RJ45 ochranný kryt IP65/IP67/IP 69K,",0]
["ZBSP2","USB / RJ45 Ochranný kryt IP65 / IP67, tv",1,"ks",{"v":17.386425,"d":"17.386"},"3606481194237",{"v":8,"d":"8.00"},{"v":1.5,"d":"1.50"},{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},"DE","3926909790","https://www.se.com/sk/sk/product/ZBSP2","USB/RJ45 ochranný kryt IP65/IP67, tvrdený plast, transparentný",0]
["ZBSP1","USB / RJ45 Ochranný kryt IP65 / IP67, mä",10,"ks",{"v":5.3989425,"d":"5.399"},"3606481194220",{"v":13,"d":"13.00"},{"v":1.5,"d":"1.50"},{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},"DE","3926909790","https://www.se.com/sk/sk/product/ZBSP1","USB/RJ45 ochranný kryt IP65/IP67, mäkčený plast, čierny",0]
["ZBRV1","Bezdrôtová kontrolka pre ZBRT vysielače",1,"ks",{"v":37.518074999999996,"d":"37.518"},"3606482035065",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.3,"d":"4.30"},{"v":17,"d":"17.00"},"FR","8536501990","https://www.se.com/sk/sk/product/ZBRV1","Bezdrôtová kontrolka, Harmony XB5R, pre použitie s vysielačmi ZBRT , pre bezdrôtové a bezbatériové ovládače",0]
["ZBRTT1","Čidlo pre meranie teploty a vhkosti",1,"ks",{"v":224.193375,"d":"224.193"},"3606481808073",{"v":9,"d":"9.00"},{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"v":34,"d":"34.00"},"ID","8526920090","https://www.se.com/sk/sk/product/ZBRTT1","Wireless transmitter, Harmony XB5R, Transmitter components for wireless temperature sensors, green, 2400MHz",0]
["ZBRT2","VYSIELAČ BEZ OVL HLAVICE A SPOJ DIELU",1,"ks",{"v":75.951225,"d":"75.951"},"3606480659928",{"v":6.2,"d":"6.20"},{"v":4.7,"d":"4.70"},{"v":5.4,"d":"5.40"},{"v":34,"d":"34.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZBRT2","bezbatériový vysielač XB5R, hore-dole",0]
["ZBRT1","VYSIELAČ BEZ OVL. HLAVICE A SPOJ. DIELU",1,"ks",{"v":74.57861249999999,"d":"74.579"},"3606480334726",{"v":5.3,"d":"5.30"},{"v":3.2,"d":"3.20"},{"v":4.5,"d":"4.50"},{"v":18,"d":"18.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZBRT1","XB5 vysielač pre bezdrátové a bezbatériové tlačítko",0]
["ZBRRH","PROG PRIJÍMAČ PRE HARMONY HUB",1,"ks",{"v":118.95975,"d":"118.960"},"3606481477071",{"v":10.2,"d":"10.20"},{"v":9.2,"d":"9.20"},{"v":10.8,"d":"10.80"},{"v":118,"d":"118.00"},"ID","8537109899","https://www.se.com/sk/sk/product/ZBRRH","Wireless Receiver, Harmony XB5R, 4 PNP, 2 pusbuttons, LED, 200mA, 24V DC",0.01]
["ZBRRC","PROG. PRIJÍMAČ 4 PNP VÝST. 24VDC",1,"ks",{"v":169.288875,"d":"169.289"},"3606480334719",{"v":9.6,"d":"9.60"},{"v":4.6,"d":"4.60"},{"v":7.9,"d":"7.90"},{"v":122,"d":"122.00"},"ID","8537109899","https://www.se.com/sk/sk/product/ZBRRC","programovací prijímač - 4 PNP - 200 mA - 24 V DC - 2 tlačítka - 6 LED",0.01]
["ZBRRA","PROG. PRIJÍMAČ 2 RELÉ VÝST 24-240V AC/DC",1,"ks",{"v":164.71349999999998,"d":"164.714"},"3606480334702",{"v":9.6,"d":"9.60"},{"v":4.6,"d":"4.60"},{"v":8,"d":"8.00"},{"v":138,"d":"138.00"},"ID","8537109899","https://www.se.com/sk/sk/product/ZBRRA","programovací prijímač - 2 relé - 24..240 V AC/DC - 2 tlačítka - 6 LED",0.02]
["ZBRP1","LANKOVÝ VYPÍNAČ, BEZ BATERIE",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3606480571732",{"v":16.5,"d":"16.50"},{"v":6.7,"d":"6.70"},{"v":6.5,"d":"6.50"},{"v":150,"d":"150.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZBRP1","BEZDROTOVÝ LANK. VYPÍNAČ",0.02]
["ZBRM22A0","HANDYBOX Plastový pre XB5R",1,"ks",183.015,"3606480891083",{"v":16.3,"d":"16.30"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":200,"d":"200.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZBRM22A0","Wireless and batteryless transmitter, Harmony XB5R, plastic, black, 2 simples action",0]
["ZBRM22","MOBILNÝ BOX, 2 TLAČIDLÁ",1,"ks",{"v":64.51278749999999,"d":"64.513"},"3606480673542",{"v":16.8,"d":"16.80"},{"v":6.4,"d":"6.40"},{"v":6.8,"d":"6.80"},{"v":143,"d":"143.00"},"HU","8538909999","https://www.se.com/sk/sk/product/ZBRM22","Harmony XB5R - prázdna handy box pre mobile use - 2 funkcie - plastiová - zelená",0]
["ZBRCETH","KOMUNIKAČNÝ MODUL Modbus TCP",1,"ks",{"v":137.26125,"d":"137.261"},"3595864172248",{"v":14.2,"d":"14.20"},{"v":0.6,"d":"0.60"},{"v":12.1,"d":"12.10"},{"v":30,"d":"30.00"},"IN","8517620000","https://www.se.com/sk/sk/product/ZBRCETH","Modbus TCP communication module for ZBRN1, Harmony XB5R, 2 Ethernet RJ45 connectors",0]
["ZBRA2","PASÍVNA ANTENA",1,"ks",{"v":80.5266,"d":"80.527"},"3606480528514",{"v":22,"d":"22.00"},{"v":4,"d":"4.00"},{"v":10,"d":"10.00"},{"v":54,"d":"54.00"},"CN","8517710000","https://www.se.com/sk/sk/product/ZBRA2","External antenna for harmony Hub ZBRN1 and ZBRN2, Harmony XB5R, 2m cable, 1 radio frequency connector",0.01]
["ZBRA1","ANTÉNA XB5R, 24-240VAC/DC, 5m",1,"ks",{"v":87.84719999999999,"d":"87.847"},"3606480334689",{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":267,"d":"267.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZBRA1","relé anténa - 24…240 V AC/DC - kábel 5m - 1 výkonová LED - 2 com LEDs",0.03]
["ZBPA","OCHRANNÁ KRYTKA",10,"ks",{"v":1.23535125,"d":"1.235"},"3389110355505",{"v":3,"d":"3.00"},{"v":1.4,"d":"1.40"},{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},"FR","4016999790","https://www.se.com/sk/sk/product/ZBPA","priehľadný kryt pre kruhové zapustené tlačítko Ø22",0]
["ZBP0A","OCHRANNÁ KRYTKA",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110101973",{"v":9.3,"d":"9.30"},{"v":7,"d":"7.00"},{"v":7.1,"d":"7.10"},{"v":6,"d":"6.00"},"FR","4016999790","https://www.se.com/sk/sk/product/ZBP0A","ochranná krytka pre tlačidlo Ø 22 mm – číra – súprava 10 ks",0]
["ZBP017","OCHRANNÁ KRYTKA",1,"ks",{"v":0.9608287499999999,"d":"0.961"},"3389119061629",{"v":4,"d":"4.00"},{"v":1.5,"d":"1.50"},{"v":4,"d":"4.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBP017","ochranná krytka",0]
["ZBP0","OCHRANNÁ KRYTKA",10,"ks",{"v":1.23535125,"d":"1.235"},"3389110101935",{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":2.7,"d":"2.70"},"FR","4016999790","https://www.se.com/sk/sk/product/ZBP0","ochranná krytka pre vystupujúce okrúhle tlač. jedn. Ø 22 mm – číra – súpr. 10 ks",0]
["ZBGP","OCHRANNÁ KRYTKA",1,"ks",{"v":7.778137499999999,"d":"7.778"},"3389119034616",{"v":11,"d":"11.00"},{"v":3.5,"d":"3.50"},{"v":9,"d":"9.00"},{"v":5,"d":"5.00"},"FR","8301700000","https://www.se.com/sk/sk/product/ZBGP","čierny ochranný kryt pre Ø22 ovl. hlavica stis.",0]
["ZBG520E","SADA KĽÚČOV 520E",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110288841",{"v":8.2,"d":"8.20"},{"v":1.1,"d":"1.10"},{"v":6.2,"d":"6.20"},{"v":14,"d":"14.00"},"FR","8301700000","https://www.se.com/sk/sk/product/ZBG520E","sada 2 kľúčov 520E",0]
["ZBG458A","SADA KĽÚČOV 458A",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110288834",{"v":7.5,"d":"7.50"},{"v":1.4,"d":"1.40"},{"v":5.1,"d":"5.10"},{"v":14,"d":"14.00"},"FR","8301700000","https://www.se.com/sk/sk/product/ZBG458A","sada 2 kľúčov 458A",0]
["ZBG455","SADA DVOCH KĽÚČOV 455",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110091847",{"v":9.1,"d":"9.10"},{"v":1,"d":"1.00"},{"v":6.2,"d":"6.20"},{"v":12,"d":"12.00"},"FR","8301700000","https://www.se.com/sk/sk/product/ZBG455","kľúč pre blokovací kláves – 455 – súprava 2 ks",0]
["ZBG421E","SADA KĽÚČOV 421E",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110288827",{"v":7.5,"d":"7.50"},{"v":0.4,"d":"0.40"},{"v":4.6,"d":"4.60"},{"v":14,"d":"14.00"},"FR","8301700000","https://www.se.com/sk/sk/product/ZBG421E","kľúč pre blokovací kláves – 421E – súprava 2 ks",0]
["ZBG3131A","SADA KĽÚČOV 3131A",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110288865",{"v":10,"d":"10.00"},{"v":0.8,"d":"0.80"},{"v":5.1,"d":"5.10"},{"v":14,"d":"14.00"},"FR","8301700000","https://www.se.com/sk/sk/product/ZBG3131A","sada 2 kľúčov 3131A",0]
["ZBE702","Spínacia jednotka, 1 V",1,"ks",{"v":12.81105,"d":"12.811"},"3389110089523",{"v":3,"d":"3.00"},{"v":0.7,"d":"0.70"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE702","jednoduchý kontaktný blok pre hlavu Ø22 1V piny pre PCB",0]
["ZBE701","SPÍNACIA JEDNOTKA NO DO PLOŠNÉHO SPOJA",1,"ks",{"v":12.81105,"d":"12.811"},"3389110089516",{"v":3,"d":"3.00"},{"v":0.5,"d":"0.50"},{"v":2,"d":"2.00"},{"v":1.7,"d":"1.70"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE701","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NO",0]
["ZBE505","SPÍNACIA JEDNOTKA VYSOKÝ PRÚD",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389119042253",{"v":4.2,"d":"4.20"},{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":40,"d":"40.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE505","dvojitý kontaktný blok pre hlavu Ø22 1Z+1V skrutková svorka",0]
["ZBE504","Dvojitý kontaktný blok pre spínanie vyso",1,"ks",{"v":24.707024999999998,"d":"24.707"},"3389119042246",{"v":5,"d":"5.00"},{"v":4.2,"d":"4.20"},{"v":4.4,"d":"4.40"},{"v":41,"d":"41.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE504","Dvojitý kontaktný blok pre spínanie vysokých prúdov, Harmony XB4, zliatina striebra, skrutkové svorky, 2NC",0]
["ZBE503","SPÍNACIA JEDNOTKA 2NO VYSOKÝ PRÚD",1,"ks",{"v":11.4384375,"d":"11.438"},"3389119042239",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":4.4,"d":"4.40"},{"v":40,"d":"40.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE503","dvojitý kontaktný blok pre hlavu Ø22 2Z šróbová svorka",0]
["ZBE502","SPÍNACIA JEDNOTKA 1NC",1,"ks",{"v":10.065825,"d":"10.066"},"3389119042222",{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":5.2,"d":"5.20"},{"v":20,"d":"20.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE502","jednoduchý kontaktný blok pre hlavu Ø22 1V skrutková svorka",0]
["ZBE501","SPÍNACIA JEDNOTKA 1NO",1,"ks",{"v":10.065825,"d":"10.066"},"3389119042215",{"v":5.4,"d":"5.40"},{"v":3.8,"d":"3.80"},{"v":4.8,"d":"4.80"},{"v":22,"d":"22.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE501","jednoduchý kontaktný blok pre hlavu Ø22 1Z skrutková svorka",0]
["ZBE302","SPÍNACIA JEDNOTKA V S MONIT.PRIP. K HLAV",5,"ks",{"v":10.065825,"d":"10.066"},"3606482035027",{"v":4.2,"d":"4.20"},{"v":1.4,"d":"1.40"},{"v":3.3,"d":"3.30"},{"v":13,"d":"13.00"},"ID","8536508090","https://www.se.com/sk/sk/product/ZBE302","Monitorovací kontakt, 1V",0]
["ZBE205","SPÍNACIA JEDNOTKA V+Z",5,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110119251",{"v":5.7,"d":"5.70"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":17,"d":"17.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE205","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NO + 1 NC",0]
["ZBE204","SPÍNACIA JEDNOTKA 2V",5,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110119206",{"v":5.2,"d":"5.20"},{"v":1,"d":"1.00"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE204","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 2 NC",0]
["ZBE203","SPÍNACIA JEDNOTKA 2Z",5,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110119169",{"v":5.2,"d":"5.20"},{"v":5.8,"d":"5.80"},{"v":4.4,"d":"4.40"},{"v":17,"d":"17.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE203","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 2 NO",0]
["ZBE202","SPÍNACIA JEDNOTKA Z -ONESKORENÝ KONTAKT",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110177459",{"v":3.4,"d":"3.40"},{"v":1.1,"d":"1.10"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE202","dotyk. blok ovládac. tlač. – ZBE Ø 22 – 1 NC – IP20 – samostatná pružin. svorka",0]
["ZBE201","SPÍNACIA JEDNOTKA Z",5,"ks",{"v":11.4384375,"d":"11.438"},"3389110177442",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":4.3,"d":"4.30"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE201","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NO",0]
["ZBE102GEX","Spínacia jednotka V do výbušného prostr.",1,"ks",{"v":44.3811375,"d":"44.381"},"3606489486129",3.81,4.32,1.27,{"v":40,"d":"40.00"},"FR","9030337000","https://www.se.com/sk/sk/product/ZBE102GEX","Spínacia jednotka V do výbušného prostredia",0]
["ZBE1029","SPÍNACIA JEDNOTKA",5,"ks",{"v":5.124419999999999,"d":"5.124"},"3389110177473",{"v":3.3,"d":"3.30"},{"v":1,"d":"1.00"},{"v":2.8,"d":"2.80"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1029","Single contact block, Harmony XB4, silver alloy, screw terminals for lug, 1NC",0]
["ZBE1026P","SPÍN. JEDNOTKA V POZLÁTENÁ PRACHOTESNÁ",1,"ks",{"v":28.367324999999997,"d":"28.367"},"3389110862843",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":10,"d":"10.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1026P","dotyk. blok ovládac. tlač. – ZBE Ø 22 – 1 NC pozlátený a odolný voči prachu",0]
["ZBE1026","Spínacia jednotka V ( malé výkony)",5,"ks",{"v":9.6082875,"d":"9.608"},"3389110089547",{"v":5.4,"d":"5.40"},{"v":5.8,"d":"5.80"},{"v":4.4,"d":"4.40"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1026","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NC pozlátený",0]
["ZBE1025","SPÍNACIA JEDNOTKA-V-PRUŽNÁ",1,"ks",{"v":3.8433149999999996,"d":"3.843"},"3389119037433",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},{"v":10,"d":"10.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1025","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NC – pružin.svorky",0]
["ZBE1024","Spínacia jednotka V pre konektor",5,"ks",{"v":10.065825,"d":"10.066"},"3389110089509",{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":8,"d":"8.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1024","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NC",0]
["ZBE1023","SPÍNACIA JEDNOTKA V FASTON",5,"ks",{"v":4.52962125,"d":"4.530"},"3389110816365",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":10,"d":"10.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1023","jednoduchý kontaktný blok pre hlavu Ø22 1V konektor faston",0]
["ZBE102","SPÍNACIA JEDNOTKA V",5,"ks",{"v":3.2027625,"d":"3.203"},"3389110089486",{"v":5.4,"d":"5.40"},{"v":5.5,"d":"5.50"},{"v":3.4,"d":"3.40"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE102","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NC",0]
["ZBE101GEX","Spínacia jednotka Z do výbušného prostr.",1,"ks",{"v":44.3811375,"d":"44.381"},"3606489486112",{"v":15,"d":"15.00"},{"v":1,"d":"1.00"},{"v":11.5,"d":"11.50"},{"v":44,"d":"44.00"},"FR","9030337000","https://www.se.com/sk/sk/product/ZBE101GEX","Spínacia jednotka Z do výbušného prostredia",0]
["ZBE1019","SPÍNACIA JEDNOTKA",5,"ks",{"v":4.849897499999999,"d":"4.850"},"3389110177466",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1019","jednoduchý kontaktný blok pre hlavu Ø22 1Z šróbová svorka pre oka",0]
["ZBE1016P","SPÍN. JEDNOTKA Z POZLÁTENÁ PRACHOTESNÁ",5,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110862836",{"v":5.4,"d":"5.40"},{"v":6,"d":"6.00"},{"v":4.4,"d":"4.40"},{"v":10,"d":"10.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1016P","dotyk. blok ovládac. tlač. – ZBE Ø 22 – 1 NO pozlátený a odolný voči prachu",0]
["ZBE1016","Spínacia jednotka Z ( malé výkony)",5,"ks",{"v":9.6082875,"d":"9.608"},"3389110089530",{"v":5.8,"d":"5.80"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1016","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NO pozlátený",0]
["ZBE1015","SPÍNACIA JEDNOTKA-Z-PRUŽNÁ",4,"ks",{"v":3.8433149999999996,"d":"3.843"},"3389119037426",{"v":5.6,"d":"5.60"},{"v":4.2,"d":"4.20"},{"v":5.4,"d":"5.40"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1015","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NO – pružin.svorky",0]
["ZBE1014","Spínacia jednotka Z pre konektor",5,"ks",{"v":10.065825,"d":"10.066"},"3389110089493",{"v":5.4,"d":"5.40"},{"v":5.7,"d":"5.70"},{"v":4.5,"d":"4.50"},{"v":7,"d":"7.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1014","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NO",0]
["ZBE1013","SPÍNACIA JEDNOTKA FAST ON",5,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110816358",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":10,"d":"10.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE1013","jednoduchý kontaktný blok pre hlavu Ø22 1Z konektor faston",0]
["ZBE101","SPÍNACIA JEDNOTKA Z",5,"ks",{"v":3.2027625,"d":"3.203"},"3389110089479",{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},{"v":2.5,"d":"2.50"},{"v":9,"d":"9.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZBE101","dotykový blok ovládacieho tlačidla – ZBE Ø 22 – 1 NO",0]
["ZBDD2","Ochranná krytka pre otoč.ovládač XB4/XB5",1,"ks",{"v":12.81105,"d":"12.811"},"3389118342972",7.85,{"v":0.4,"d":"0.40"},7.85,{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBDD2","ochranná krytka pre otočné ovládače Ø22",0]
["ZBDA185","SADA KĽÚČOV N 4A185",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110091946",{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},{"v":0.4,"d":"0.40"},{"v":13,"d":"13.00"},"FR","8301700000","https://www.se.com/sk/sk/product/ZBDA185","sada 2 kľúčov 4A185",0]
["ZBD8D1","SADA KĽÚČOV 8D1",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110092554",{"v":10,"d":"10.00"},{"v":1,"d":"1.00"},{"v":5.3,"d":"5.30"},{"v":12,"d":"12.00"},"FR","8301700000","https://www.se.com/sk/sk/product/ZBD8D1","kľúč pre blokovací kláves – 8D1 – súprava 2 ks",0]
["ZBAF9","6 farieb",1,"ks",{"v":5.0329125,"d":"5.033"},"3606481340603",{"v":1,"d":"1.00"},{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},{"v":13,"d":"13.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBAF9","Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, bez symbolu, súprava 6 farebných hmatníkov",0]
["ZBAF639","Hmatník so symbolom",10,"ks",{"v":2.5622099999999994,"d":"2.562"},"3606481362094",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.3,"d":"5.30"},{"v":2,"d":"2.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBAF639","blue plain cap R for flush mounted push button, Harmony XB4, Harmony XB5",0]
["ZBAF6","Hmatník MO",1,"ks",{"v":1.69288875,"d":"1.693"},"3606481340726",{"v":2.5,"d":"2.50"},{"v":2,"d":"2.00"},{"v":2.5,"d":"2.50"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBAF6","Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, bez symbolu, modrá",0]
["ZBAF5","Hmatník ŽL",1,"ks",{"v":1.69288875,"d":"1.693"},"3606481340719",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":11,"d":"11.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBAF5","Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, bez symbolu, žltá",0]
["ZBAF4","Hmatník RU",1,"ks",{"v":1.69288875,"d":"1.693"},"3606481340702",{"v":2.5,"d":"2.50"},{"v":1.5,"d":"1.50"},{"v":2.5,"d":"2.50"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBAF4","Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, bez symbolu, červená",0]
["ZBAF335","Hmatník so symbolom",1,"ks",{"v":2.3883457499999996,"d":"2.388"},"3606481361981",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.3,"d":"5.30"},{"v":2,"d":"2.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBAF335","Harmony XB4, Harmony XB5, Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, symbol šípka nahor, čierna",""]
["ZBAF333","Hmatník so symbolom",1,"ks",{"v":2.9648429999999997,"d":"2.965"},"3606481361882",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.3,"d":"5.30"},{"v":2,"d":"2.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBAF333","Harmony XB4, Harmony XB5, Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, symbol START, zelená",""]
["ZBAF331","Hmatník so symbolom",1,"ks",{"v":2.3883457499999996,"d":"2.388"},"3606481361806",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.3,"d":"5.30"},{"v":2,"d":"2.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBAF331","Harmony XB4, Harmony XB5, Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, symbol I, zelená",""]
["ZBAF3","Hmatník ZE",1,"ks",{"v":1.69288875,"d":"1.693"},"3606481340696",{"v":2.5,"d":"2.50"},{"v":1.5,"d":"1.50"},{"v":2.5,"d":"2.50"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBAF3","Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, bez symbolu, zelená",0]
["ZBAF2","Hmatník ČE",10,"ks",{"v":1.69288875,"d":"1.693"},"3606481340689",{"v":2.5,"d":"2.50"},{"v":2,"d":"2.00"},{"v":2.5,"d":"2.50"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBAF2","Harmony XB4, Harmony XB5,  Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, bez symbolu, čierna",0]
["ZBAF1","Hmatník BI",1,"ks",{"v":1.69288875,"d":"1.693"},"3606481340672",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":11,"d":"11.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBAF1","Antimikrobiálny hmatník pre stláčací ovládač, zapustené prevedenie, bez symbolu, biela",0]
["ZBA79","SADA 10 HMAT. RÔZNE FARBY RÔZNE ZNAKY",1,"ks",{"v":18.301499999999997,"d":"18.302"},"3606480334665",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA79","SADA 10 HMAT ROZNE FARBY ROZNE ZNAKY",0]
["ZBA76","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":4.16359125,"d":"4.164"},"3389119044288",{"v":2,"d":"2.00"},{"v":0.3,"d":"0.30"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA76","modrý hmatník neoznačený pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA75","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":4.16359125,"d":"4.164"},"3389119044295",{"v":12,"d":"12.00"},{"v":0.1,"d":"0.10"},{"v":10,"d":"10.00"},{"v":0.5,"d":"0.50"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA75","žltý hmatník neoznačený pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA7432","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044189",{"v":12,"d":"12.00"},{"v":0.1,"d":"0.10"},{"v":10,"d":"10.00"},{"v":0.6,"d":"0.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7432","červený hmatník označený O pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA7335","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044721",{"v":1.5,"d":"1.50"},{"v":0.1,"d":"0.10"},{"v":1.5,"d":"1.50"},{"v":0.6,"d":"0.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7335","zelený hmatník s označením \"šipka\" pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA7331","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044141",{"v":12,"d":"12.00"},{"v":0.1,"d":"0.10"},{"v":10,"d":"10.00"},{"v":0.5,"d":"0.50"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7331","zelený hmatník s označením I pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA73","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":4.02633,"d":"4.026"},"3389119044134",{"v":12,"d":"12.00"},{"v":0.1,"d":"0.10"},{"v":10,"d":"10.00"},{"v":0.6,"d":"0.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA73","zelený hmatník neoznačený pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA7237","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044219",{"v":1.8,"d":"1.80"},{"v":0.5,"d":"0.50"},{"v":1.8,"d":"1.80"},{"v":0.6,"d":"0.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7237","čierny hmatník tlač. ovládače so symb. I pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA7235","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044196",{"v":1.6,"d":"1.60"},{"v":0.2,"d":"0.20"},{"v":1.6,"d":"1.60"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7235","čierny hmatník tlač.ovládače so symbolom \"šipka\" pre obdĺ. viachlavové tlač.Ø22",0]
["ZBA7232","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044226",{"v":6,"d":"6.00"},{"v":1,"d":"1.00"},{"v":2.5,"d":"2.50"},{"v":0.6,"d":"0.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7232","čierny hmatník tlač. ovládače so symb. O pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA72","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":4.02633,"d":"4.026"},"3389119044233",{"v":12,"d":"12.00"},{"v":0.1,"d":"0.10"},{"v":10,"d":"10.00"},{"v":0.5,"d":"0.50"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA72","čierny hmatník neoznačený pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA7138","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044264",{"v":12,"d":"12.00"},{"v":0.1,"d":"0.10"},{"v":10,"d":"10.00"},{"v":0.6,"d":"0.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7138","biely hmatník označený + pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA7134","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044257",{"v":1.5,"d":"1.50"},{"v":0.5,"d":"0.50"},{"v":1.5,"d":"1.50"},{"v":0.4,"d":"0.40"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7134","biely hmatník označený \"šipka\" pre obdĺžnikové tlač. Ø22",0]
["ZBA7131","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":6.039494999999999,"d":"6.039"},"3389119044271",{"v":1.8,"d":"1.80"},{"v":0.5,"d":"0.50"},{"v":1.8,"d":"1.80"},{"v":0.6,"d":"0.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA7131","biely hmatník označený I pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA710","SILIKÓNOVÁ KRYTKA PRE DVOJTL. OVLÁDAČE",10,"ks",{"v":5.26168125,"d":"5.262"},"3389119044325",{"v":5.5,"d":"5.50"},{"v":2,"d":"2.00"},{"v":3.5,"d":"3.50"},{"v":5,"d":"5.00"},"FR","39269097","https://www.se.com/sk/sk/product/ZBA710","ochranná krytka pre obdĺžnikové viachlavové tlačítko Ø22",0]
["ZBA71","HMATNÍKY PRE DVOJTLAČ. OVLÁDAČE",10,"ks",{"v":4.02633,"d":"4.026"},"3389119044240",{"v":2,"d":"2.00"},{"v":0.2,"d":"0.20"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA71","biely hmatník neoznačený pre obdĺžnikové viachlavové tlač. Ø22",0]
["ZBA709","SILIKÓNOVÁ KRYTKA PRE DVOJTL. OVLÁDAČE",10,"ks",{"v":5.26168125,"d":"5.262"},"3389119044318",{"v":17,"d":"17.00"},{"v":3,"d":"3.00"},{"v":14.5,"d":"14.50"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA709","ochranná krytka pre obdĺžnikové viachlavové tlačítko Ø22",0]
["ZBA708","SILIKÓNOVÁ KRYTKA PRE DVOJTL. OVLÁDAČE",10,"ks",{"v":5.26168125,"d":"5.262"},"3389119044301",{"v":5.1,"d":"5.10"},{"v":1.8,"d":"1.80"},{"v":3.5,"d":"3.50"},{"v":4,"d":"4.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA708","ochranná krytka pre obdĺžnikové viachlavové tlačítko Ø22",0]
["ZBA639","HMATNÍK",10,"ks",{"v":3.1570087499999997,"d":"3.157"},"3389110091625",{"v":10,"d":"10.00"},{"v":12,"d":"12.00"},{"v":1.5,"d":"1.50"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA639","modrý kryt – označ. R – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA6","HMATNÍK",10,"ks",{"v":0.5490449999999999,"d":"0.549"},"3389110090680",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":0.9,"d":"0.90"},"FR","85389099","https://www.se.com/sk/sk/product/ZBA6","modrý kryt – bez označenia – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA5","HMATNÍK",10,"ks",{"v":0.5490449999999999,"d":"0.549"},"3389110090666",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA5","žltý kryt – bez označenia – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA434","HMATNÍK",10,"ks",{"v":1.8301499999999997,"d":"1.830"},"3389110090925",{"v":2.5,"d":"2.50"},{"v":1.5,"d":"1.50"},{"v":2.5,"d":"2.50"},{"v":1,"d":"1.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBA434","červený kryt – označ. STOP – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA4","HMATNÍK",10,"ks",{"v":0.5490449999999999,"d":"0.549"},"3389110090659",{"v":2.5,"d":"2.50"},{"v":1,"d":"1.00"},{"v":2.5,"d":"2.50"},{"v":1.2,"d":"1.20"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA4","červený kryt – bez označenia – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA346","HMATNÍK",10,"ks",{"v":2.15042625,"d":"2.150"},"3389110861358",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBA346","zelená krytka s označením pre kruhové tlačítko Ø22",0]
["ZBA344","HMATNÍK DOWN",10,"ks",{"v":3.29427,"d":"3.294"},"3389110091502",5.08,2.54,2.54,{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBA344","čierny kryt – označ. dole – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA335","HMATNÍK",10,"ks",{"v":2.15042625,"d":"2.150"},"3389110091588",{"v":2.5,"d":"2.50"},{"v":1.5,"d":"1.50"},{"v":2.5,"d":"2.50"},{"v":1.2,"d":"1.20"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA335","čierny kryt – označ. šípkou – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA334","HMATNÍK",10,"ks",{"v":2.15042625,"d":"2.150"},"3389110091236",{"v":2.5,"d":"2.50"},{"v":1,"d":"1.00"},{"v":2.5,"d":"2.50"},{"v":1.3,"d":"1.30"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA334","biely kryt – označ. šípkou – čierne – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA333","HMATNÍK",10,"ks",{"v":2.15042625,"d":"2.150"},"3389110090826",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":0.9,"d":"0.90"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBA333","zelený kryt – označ. START – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA331","HMATNÍK",10,"ks",{"v":2.15042625,"d":"2.150"},"3389110090758",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":0.9,"d":"0.90"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBA331","zelený kryt – označ. I – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA3","HMATNÍK",10,"ks",{"v":0.5490449999999999,"d":"0.549"},"3389110090642",{"v":2.5,"d":"2.50"},{"v":1.2,"d":"1.20"},{"v":2.5,"d":"2.50"},{"v":1.3,"d":"1.30"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA3","zelený kryt – bez označenia – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA2935","HMATNÍK S POPISOM -",1,"ks",{"v":2.7452249999999996,"d":"2.745"},"3389110109306",{"v":2.4,"d":"2.40"},{"v":1.4,"d":"1.40"},{"v":2.4,"d":"2.40"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA2935","čierny kryt – označ. „-“ – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA2934","HMATNÍK S POPISOM +",1,"ks",{"v":2.7452249999999996,"d":"2.745"},"3389110105803",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":9,"d":"9.00"},{"v":1.2,"d":"1.20"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA2934","čierny kryt – označ. „+“ – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA245","HMATNÍK S OZNAČENÍM T",1,"ks",{"v":5.62771125,"d":"5.628"},"3389110861341",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":9,"d":"9.00"},{"v":5,"d":"5.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBA245","čierny kryt – označ. T – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA234","HMATNÍK",10,"ks",{"v":2.15042625,"d":"2.150"},"3389110091380",{"v":2.5,"d":"2.50"},{"v":2,"d":"2.00"},{"v":2.5,"d":"2.50"},{"v":1,"d":"1.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA234","čierny kryt – označ. STOP – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA232","HMATNÍK",10,"ks",{"v":2.15042625,"d":"2.150"},"3389110091274",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":4,"d":"4.00"},{"v":5,"d":"5.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZBA232","čierny kryt – označ. N/C – biele – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA2","HMATNÍK",10,"ks",{"v":0.5490449999999999,"d":"0.549"},"3389110090611",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA2","čierny kryt – bez označenia – pre guľatú hlavicu zapusteného tlačidla",0]
["ZBA145","HMATNÍK",10,"ks",{"v":1.8759037499999995,"d":"1.876"},"3389110841404",{"v":6.5,"d":"6.50"},{"v":3,"d":"3.00"},{"v":4.5,"d":"4.50"},{"v":5,"d":"5.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBA145","biely hmatník označený T pre kruhové tlačítko Ø22",0]
["ZBA131","HMATNÍK",10,"ks",{"v":2.0589187499999997,"d":"2.059"},"3389110090963",{"v":5.4,"d":"5.40"},{"v":4.3,"d":"4.30"},{"v":3.4,"d":"3.40"},{"v":0.9,"d":"0.90"},"FR","8538909999","https://www.se.com/sk/sk/product/ZBA131","biely kryt – označ. I – čierne – preguľatú hlavicu zapusteného tlačidla",0]
["ZBA1","HMATNÍK",10,"ks",{"v":0.5490449999999999,"d":"0.549"},"3389110090604",{"v":2.5,"d":"2.50"},{"v":1.2,"d":"1.20"},{"v":2.5,"d":"2.50"},{"v":1.3,"d":"1.30"},"FR","3926909790","https://www.se.com/sk/sk/product/ZBA1","biely kryt – bez označenia – pre guľatú hlavicu zapusteného tlačidla",0]
["ZB6ZB65B","Polozostava LED+sp. jednotky",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3389110205817",{"v":5.5,"d":"5.50"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB6ZB65B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – modrá zabud. LED 1 NO + 1 NC",0]
["ZB6ZB55B","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":22.876875,"d":"22.877"},"3389110784497",{"v":11,"d":"11.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":12,"d":"12.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB6ZB55B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – žltá zabud. LED 1 NO + 1 NC",0]
["ZB6ZB51B","KONTAKT Z + ŽIAR. ŽLTÁ, FASTON",1,"ks",{"v":19.216575,"d":"19.217"},"3389110784473",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB6ZB51B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – žltá zabud. LED 1 NO",0]
["ZB6ZB45B","Polozostava LED+sp. jednotky",1,"ks",{"v":22.876875,"d":"22.877"},"3389110784466",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":9,"d":"9.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB6ZB45B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – červená zabud. LED 1 NO + 1 NC",0]
["ZB6ZB42B","KONTAKT NC+ ŽIAR. ČERV., FASTON",1,"ks",{"v":21.046725,"d":"21.047"},"3389110784459",{"v":4.5,"d":"4.50"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB6ZB42B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – červená zabud. LED 1 NC",0]
["ZB6ZB35B","Polozostava LED+sp. jednotky",1,"ks",{"v":22.876875,"d":"22.877"},"3389110784442",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB6ZB35B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – zelená zabud. LED 1 NO + 1 NC",0]
["ZB6ZB31B","KONTAKT Z + ŽIAR. ZELENÁ, FASTON",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110784435",{"v":9,"d":"9.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":8,"d":"8.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB6ZB31B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – zelená zabud. LED 1 NO",0]
["ZB6ZB15B","Polozostava LED+sp. jednotky",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110784404",{"v":7,"d":"7.00"},{"v":2.5,"d":"2.50"},{"v":7,"d":"7.00"},{"v":11,"d":"11.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6ZB15B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – biela zabud. LED 1 NO + 1 NC",0]
["ZB6ZB11B","KONTAKT Z + ŽIAR. BIELA, FASTON",1,"ks",{"v":20.13165,"d":"20.132"},"3389110784398",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB6ZB11B","teleso pre osvetlené ovládacie tlačidlo – Ø 16 – biela zabud. LED 1 NO",0]
["ZB6Z5B","KONTAKT 1ZAP/1VYP",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110775372",{"v":4,"d":"4.00"},{"v":2.5,"d":"2.50"},{"v":2.5,"d":"2.50"},{"v":10,"d":"10.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6Z5B","teleso pre ovládacie tlačidlo – Ø 16 – 1 NO+1 NC",0]
["ZB6Z4B","KONTAKT 2VYP",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110775365",{"v":7.7,"d":"7.70"},{"v":3.8,"d":"3.80"},{"v":4.4,"d":"4.40"},{"v":6,"d":"6.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6Z4B","teleso pre ovládacie tlačidlo – Ø 16 – 2 NC",0]
["ZB6Z3B","KONTAKT 2ZAP",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110775358",{"v":4,"d":"4.00"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB6Z3B","teleso pre ovládacie tlačidlo – Ø 16 – 2 NO",0]
["ZB6Z2B","KONTAKT VYP",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3389110775341",{"v":7,"d":"7.00"},{"v":2.5,"d":"2.50"},{"v":7,"d":"7.00"},{"v":4,"d":"4.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6Z2B","teleso pre ovládacie tlačidlo – Ø 16 – 1 NC",0]
["ZB6Z1B","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3389110775334",{"v":16,"d":"16.00"},{"v":0.2,"d":"0.20"},{"v":11,"d":"11.00"},{"v":4,"d":"4.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6Z1B","teleso pre ovládacie tlačidlo – Ø 16 – 1 NO",0]
["ZB6YG095","TLEJIVKA",5,"ks",{"v":3.3857775,"d":"3.386"},"3389110864175",{"v":2.2,"d":"2.20"},{"v":0.8,"d":"0.80"},{"v":0.8,"d":"0.80"},{"v":0.6,"d":"0.60"},"FR","8539398090","https://www.se.com/sk/sk/product/ZB6YG095","číra neónová žiarovka pre signalizáciu – bayonet T1 1/4 – 110 - 230 V",0]
["ZB6YD22","ŠTÍTOK 4 X 28 MM ARRET ČIERNY",10,"ks",{"v":2.4249487499999995,"d":"2.425"},"3389110948974",{"v":0.4,"d":"0.40"},{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},{"v":30,"d":"30.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB6YD22","STÍTOK 4 X 28 MM \"ARRET\" ČIERNY",0]
["ZB6YD21","NOSIČ ŠTÍTKU 24X28MM BEZ POPISU",10,"ks",{"v":3.0197474999999994,"d":"3.020"},"3389110948981",{"v":7.5,"d":"7.50"},{"v":1.5,"d":"1.50"},{"v":3.5,"d":"3.50"},{"v":0.9,"d":"0.90"},"FR","4911990000","https://www.se.com/sk/sk/product/ZB6YD21","držiak štítku 24x48 mm pre štítok 8x21 mm neoznačený",0]
["ZB6YD20","NOSIČ ŠTÍTKU 24X28MM BEZ POPISU",10,"ks",{"v":1.8301499999999997,"d":"1.830"},"3389110948950",{"v":2.9,"d":"2.90"},{"v":0.4,"d":"0.40"},{"v":2.5,"d":"2.50"},{"v":0.3,"d":"0.30"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB6YD20","držiak štítku 24x48 mm pre štítok 8x21 mm neoznačený",0]
["ZB6YD001","OCHRAN. KRYT OBDĹŽNIKOVÝ",1,"ks",{"v":6.8630625,"d":"6.863"},"3389110784701",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB6YD001","ochranný uzáver pre obdĺžnikové tlačidlo Ø 16 mm",0]
["ZB6YA001","OCHRANNÝ KRYT",1,"ks",{"v":7.183338749999999,"d":"7.183"},"3389110784688",{"v":5.2,"d":"5.20"},{"v":2.8,"d":"2.80"},{"v":3.9,"d":"3.90"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB6YA001","ochranný uzáver pre okrúhle alebo štvorcové tlačidlo Ø 16 mm",0]
["ZB6Y7330","ŠTÍTOK EMERGENCY STOP",10,"ks",{"v":6.1767562499999995,"d":"6.177"},"3389110071597",{"v":4.5,"d":"4.50"},{"v":0.5,"d":"0.50"},{"v":4.5,"d":"4.50"},{"v":0.9,"d":"0.90"},"FR","4911990000","https://www.se.com/sk/sk/product/ZB6Y7330","okrúhly štítok Ø 45 – pre tlačidlo núdz. vyp. – žltý – EMERGENCY STOP",0]
["ZB6Y7130","ŠTÍTOK ARRET D URGENCE",1,"ks",{"v":6.039494999999999,"d":"6.039"},"3389110071580",{"v":5,"d":"5.00"},{"v":1,"d":"1.00"},{"v":4.5,"d":"4.50"},{"v":0.9,"d":"0.90"},"FR","4911990000","https://www.se.com/sk/sk/product/ZB6Y7130","štítok s popisom Ø45 pre ovl. tlač. núdzového zastavenia - ARRET D'URGENCE",0]
["ZB6Y7001","ŠTÍTOK 16MM A 45MM NEPOPÍSANÝ",1,"ks",{"v":4.34660625,"d":"4.347"},"3389110071573",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":4.5,"d":"4.50"},{"v":0.9,"d":"0.90"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB6Y7001","okrúhly štítok Ø 45 – pre tlačidlo núdz. vyp. – žltý – bez označenia",0]
["ZB6Y1001","ŠTÍTOK 8x21MM BEZ POPISU",20,"ks",{"v":1.4641199999999999,"d":"1.464"},"3389110949025",{"v":12.5,"d":"12.50"},{"v":0.4,"d":"0.40"},{"v":10,"d":"10.00"},{"v":30,"d":"30.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB6Y1001","neoznačený štítok 8x21 mm pre držiak štítkov 24x48 mm",0]
["ZB6Y011","KONZOLA PRE MONTÁŽ NA DOSKU PLOŠ. SPOJOV",4,"ks",{"v":3.9805762499999995,"d":"3.981"},"3389110767933",{"v":8,"d":"8.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":4,"d":"4.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6Y011","konzola telesa pre montáž dosky s ploš. spojmi a jednotky Ø 16 mm – súpr. 4 ks",0]
["ZB6Y010","ADAPTÉR NA DOSKU PLOŠ. SPOJOV",10,"ks",{"v":3.3857775,"d":"3.386"},"3389110767636",{"v":1.9,"d":"1.90"},{"v":1.9,"d":"1.90"},{"v":1.9,"d":"1.90"},{"v":4,"d":"4.00"},"FR","8536699099","https://www.se.com/sk/sk/product/ZB6Y010","Plug in socket adaptor, Harmony XB6, printed circuit board accessory, 16mm push button, set of 10",0]
["ZB6Y009","SPOJOVACÍ DIEL",10,"ks",{"v":3.34002375,"d":"3.340"},"3389110768121",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1.3,"d":"1.30"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6Y009","upevň. príruba telesa pre montáž dotyk. blokov na jednotky Ø 16 mm – súpr. 10 ks",0]
["ZB6Y005","KRYTKA MONT. OTVORU",10,"ks",{"v":2.2876874999999997,"d":"2.288"},"3389110784725",{"v":1.7,"d":"1.70"},{"v":0.8,"d":"0.80"},{"v":1.7,"d":"1.70"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB6Y005","okrúhla zaslepovacia krytka pre jednotky Ø 16 mm – súprava 10 ks",0]
["ZB6Y004","KONEKTOR FASTON",100,"ks",{"v":0.5490449999999999,"d":"0.549"},"3389110784718",{"v":15.5,"d":"15.50"},{"v":0.5,"d":"0.50"},{"v":11.5,"d":"11.50"},{"v":0.2,"d":"0.20"},"FR","8536699099","https://www.se.com/sk/sk/product/ZB6Y004","samičí konektorfaston jednotky Ø 16 mm – súprava 100 ks",0]
["ZB6Y003","PROTIROTAČNÝ PRÍPRAVOK",10,"ks",{"v":1.647135,"d":"1.647"},"3389110784664",{"v":1.9,"d":"1.90"},{"v":0.2,"d":"0.20"},{"v":1.9,"d":"1.90"},{"v":0.7,"d":"0.70"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6Y003","poistná podložka pre jednotku Ø 16 mm – súprava 10 ks",0]
["ZB6Y002","UPEVŇOVACIA MATICA",10,"ks",{"v":3.6602999999999994,"d":"3.660"},"3389110784640",{"v":14.5,"d":"14.50"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":30,"d":"30.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB6Y002","upínacia matica pre jednotku Ø 16 mm – súprava 10 ks",0]
["ZB6EM8B","LED OBJÍMKA PRE ZB6 ORANŽOVÁ",1,"ks",{"v":23.334412499999996,"d":"23.334"},"3389110274868",{"v":6.5,"d":"6.50"},{"v":2.2,"d":"2.20"},{"v":3.2,"d":"3.20"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EM8B","oranžová polozostava objímky s integ. LED 230...240V",0]
["ZB6EM5B","OBJÍMKA",1,"ks",{"v":23.334412499999996,"d":"23.334"},"3389110274844",{"v":6.5,"d":"6.50"},{"v":2.2,"d":"2.20"},{"v":3.2,"d":"3.20"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EM5B","teleso pre kontrolku – ZB6 – žltá zabud. LED – 230 - 240 V",0]
["ZB6EM4B","ČERVENÁ LED OBJÍMKA- 230V",1,"ks",{"v":22.876875,"d":"22.877"},"3389110274837",{"v":5,"d":"5.00"},{"v":0.7,"d":"0.70"},{"v":1.5,"d":"1.50"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EM4B","teleso pre kontrolku – ZB6 – červená zabud. LED – 230 - 240 V",0]
["ZB6EM3B","ZELENÁ LED 230 V",1,"ks",{"v":23.334412499999996,"d":"23.334"},"3389110274820",{"v":5,"d":"5.00"},{"v":0.8,"d":"0.80"},{"v":1.5,"d":"1.50"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EM3B","teleso pre kontrolku – ZB6 – zelená zabud. LED – 230 - 240 V",0]
["ZB6EM1B","LED MODUL 230V BIELA",5,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110274813",{"v":6.5,"d":"6.50"},{"v":3.2,"d":"3.20"},{"v":2.2,"d":"2.20"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EM1B","teleso pre kontrolku – ZB6 – biela zabud. LED – 230 - 240 V",0]
["ZB6EM0B","OBJÍMKA",5,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110784367",{"v":6.5,"d":"6.50"},{"v":2,"d":"2.00"},{"v":3.2,"d":"3.20"},{"v":3,"d":"3.00"},"FR","9030337000","https://www.se.com/sk/sk/product/ZB6EM0B","teleso pre kontrolku – ZB6 – základňa T1 1/4 – 230 V",0]
["ZB6EG3B","TELO SIGNÁLKY, ZB6, ZEL, INTEGRAL",1,"ks",{"v":37.518074999999996,"d":"37.518"},"3389110274769",{"v":6.6,"d":"6.60"},{"v":2.2,"d":"2.20"},{"v":3.3,"d":"3.30"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EG3B","zelená polozostava objímky s integ. LED 48...120V",0]
["ZB6EB6B","OBJÍMKA 6-24V MOD., FASTON",5,"ks",{"v":13.726125,"d":"13.726"},"3389110784329",{"v":6.5,"d":"6.50"},{"v":2.1,"d":"2.10"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EB6B","teleso pre kontrolku – ZB6 – modrá zabud. LED – 12 - 24 V",0]
["ZB6EB5B","OBJÍMKA 6-24V ŽL., FASTON",5,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110784305",{"v":6.5,"d":"6.50"},{"v":2.2,"d":"2.20"},{"v":3.2,"d":"3.20"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EB5B","teleso pre kontrolku – ZB6 – žltá zabud. LED – 12 - 24 V",0]
["ZB6EB4B","OBJÍMKA 6-24V FASTON",5,"ks",{"v":11.4384375,"d":"11.438"},"3389110784282",{"v":3.2,"d":"3.20"},{"v":2.2,"d":"2.20"},{"v":6.5,"d":"6.50"},{"v":2,"d":"2.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EB4B","teleso pre kontrolku – ZB6 – červená zabud. LED – 12 - 24 V",0]
["ZB6EB3B","OBJÍMKA 6-24V ZEL., FASTON",5,"ks",{"v":11.4384375,"d":"11.438"},"3389110784268",{"v":3.2,"d":"3.20"},{"v":2,"d":"2.00"},{"v":6.5,"d":"6.50"},{"v":2,"d":"2.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EB3B","teleso pre kontrolku – ZB6 – zelená zabud. LED – 12 - 24 V",0]
["ZB6EB3A","OBJÍMKA 6-24V ZEL., PLOŠ. SPOJE",5,"ks",{"v":13.2685875,"d":"13.269"},"3389110784251",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":4,"d":"4.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EB3A","teleso pre kontrolku – ZB6 – zelená zabud. LED – 12 - 24 V",0]
["ZB6EB1B","OBJÍMKA 6-24V BIE., FASTON",5,"ks",{"v":13.726125,"d":"13.726"},"3389110784244",{"v":5,"d":"5.00"},{"v":0.5,"d":"0.50"},{"v":1.8,"d":"1.80"},{"v":2,"d":"2.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EB1B","teleso pre kontrolku – ZB6 – biela zabud. LED – 12 - 24 V",0]
["ZB6EB1A","OBJÍMKA 6-24V BIE., PLOŠ. SPOJE",5,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110784237",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":4,"d":"4.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB6EB1A","teleso pre kontrolku – ZB6 – biela zabud. LED – 12 - 24 V",0]
["ZB6E2B","KONTAKT VYP FASTON",10,"ks",{"v":4.849897499999999,"d":"4.850"},"3389110775303",{"v":3.2,"d":"3.20"},{"v":2.2,"d":"2.20"},{"v":6.5,"d":"6.50"},{"v":2,"d":"2.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6E2B","dotykový blok ovládacieho tlačidla – ZB6 Ø 16 – 1 NC strieborná zliat.",0]
["ZB6E2A","KONTAKT VYP PRE DOSKU PLOŠ. SPOJOV",10,"ks",{"v":6.314017499999999,"d":"6.314"},"3389110775297",{"v":6.6,"d":"6.60"},{"v":2.2,"d":"2.20"},{"v":3.3,"d":"3.30"},{"v":2,"d":"2.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6E2A","dotykový blok ovládacieho tlačidla – ZB6 Ø 16 – 1 NC strieborná zliat.",0]
["ZB6E1B","SPÍNACIA JEDNOTKA",10,"ks",{"v":4.849897499999999,"d":"4.850"},"3389110775266",{"v":3.2,"d":"3.20"},{"v":2.2,"d":"2.20"},{"v":6.7,"d":"6.70"},{"v":2,"d":"2.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6E1B","dotykový blok ovládacieho tlačidla – ZB6 Ø 16 – 1 NO strieborná zliat.",0]
["ZB6E1A","SPÍNACIA JEDNOTKA",10,"ks",{"v":6.314017499999999,"d":"6.314"},"3389110775259",{"v":6.8,"d":"6.80"},{"v":2.5,"d":"2.50"},{"v":3.3,"d":"3.30"},{"v":2,"d":"2.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6E1A","dotykový blok ovládacieho tlačidla – ZB6 Ø 16 – 1 NO strieborná zliat.",0]
["ZB6DW6","OBDĹŽ. ZAPUS. PRESV. TLAČIDLO MODRÉ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110849028",{"v":7,"d":"7.00"},{"v":3,"d":"3.00"},{"v":7,"d":"7.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DW6","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – modrá",0]
["ZB6DW5","OVL. HLAVICA STLÁČ. PRESVETL.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110776041",{"v":7,"d":"7.00"},{"v":3,"d":"3.00"},{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DW5","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – žltá",0]
["ZB6DW4","OVL. HLAVICA STLÁČ. PRESVETL.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110776034",{"v":8.3,"d":"8.30"},{"v":2.7,"d":"2.70"},{"v":4.3,"d":"4.30"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DW4","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – červená",0]
["ZB6DW3","OBDĹŽ. ZAPUS. PRESV. TLAČIDLO ZELENÉ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110784206",{"v":13.1,"d":"13.10"},{"v":2.5,"d":"2.50"},{"v":4.1,"d":"4.10"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DW3","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – zelená",0]
["ZB6DW1","OBDĹŽ. ZAPUS. PRESV. TLAČIDLO BIELE",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110776027",{"v":8,"d":"8.00"},{"v":2.5,"d":"2.50"},{"v":8,"d":"8.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DW1","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – biela",0]
["ZB6DV5","OBDĹŽ. SIGNÁLKA ŽLTÁ",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110775679",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DV5","kryt kontrolky – Ø 16 – obdĺžnikový – žltá hladká šošovka",0]
["ZB6DV4","OBDĹŽ. SIGNÁLKA ČERVENÁ",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110775662",{"v":13.6,"d":"13.60"},{"v":3.3,"d":"3.30"},{"v":3.5,"d":"3.50"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DV4","krytkontrolky – Ø 16 – obdĺžnikový – červená hladká šošovka",0]
["ZB6DV3","OBDĹŽ. SIGNÁLKA ZELENÁ",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110775655",{"v":7.3,"d":"7.30"},{"v":4.4,"d":"4.40"},{"v":4.8,"d":"4.80"},{"v":9,"d":"9.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB6DV3","kryt kontrolky – Ø 16 – obdĺžnikový – zelená hladká šošovka",0]
["ZB6DV1","OBDĹŽ. SIGNÁLKA BIELA",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110775648",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DV1","kryt kontrolky – Ø 16 – obdĺžnikový – biela hladká šošovka",0]
["ZB6DGL","OVL. HLAVA OBDĹŽNIKOVÁ S KĽÚČOM",1,"ks",{"v":40.720837499999995,"d":"40.721"},"3389110785418",{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},{"v":3.5,"d":"3.50"},{"v":28.2,"d":"28.20"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DGL","obdĺžniková ovládateľná otočná hlavica Ø16 2-polohy s návratom Ronis 200",0]
["ZB6DGC","OVL. HLAVA OBDĹŽNIKOVÁ S KĽÚČOM",1,"ks",{"v":37.0605375,"d":"37.061"},"3389110785333",{"v":7,"d":"7.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DGC","obdĺžniková ovládateľná otočná hlavica Ø16 2-polohy pevné Ronis 200",0]
["ZB6DGB","OVL. HLAVA OBDĹŽNIKOVÁ S KĽÚČOM",1,"ks",{"v":37.0605375,"d":"37.061"},"3389110785326",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DGB","obdĺžniková ovládateľná otočná hlavica Ø16 2-polohy pevné Ronis 200",0]
["ZB6DF4","TLAČIDLO OBDĹŽ. PRESV. ČERVENÉ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110776270",{"v":5,"d":"5.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DF4","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – červená",0]
["ZB6DF1","TLAČIDLO OBDĹŽ. PRESV. BIELE",1,"ks",{"v":10.065825,"d":"10.066"},"3389110776256",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DF1","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – biela",0]
["ZB6DE3","TLAČIDLO OBDĹŽ. PRESV. ZELENÉ",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110776386",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DE3","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – zelená",0]
["ZB6DE1","TLAČIDLO OBDĹŽ. PRESV. BIELE",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110776379",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DE1","obdĺžniková hlavica osvetleného tlačidla – Ø 16 – biela",0]
["ZB6DD28","OBDĹŽNIK. OTOČ. OVLÁDAČ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110070859",{"v":5.5,"d":"5.50"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DD28","obdĺžniková hlavica voliaceho spínača – 2 polohy Ø 16 – čierna",0]
["ZB6DD25","OBDĹŽNIK. OTOČ. OVLÁDAČ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110776898",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DD25","obdĺžniková hlavica voliaceho spínača – 3 polohy Ø 16 – čierna",0]
["ZB6DD23","OBDĹŽNIK. OTOČ. OVLÁDAČ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110776874",{"v":16,"d":"16.00"},{"v":3,"d":"3.00"},{"v":11,"d":"11.00"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DD23","obdĺžniková hlavica voliaceho spínača – 3 polohy Ø 16 – čierna",0]
["ZB6DD22","OBDĹŽNIK. OTOČ. OVLÁDAČ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110776867",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":10,"d":"10.00"},{"v":11,"d":"11.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DD22","obdĺžniková hlavica voliaceho spínača – 2 polohy Ø 16 – čierna",0]
["ZB6DA6","Hlava tlačítkového spínača, modrá",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110288186",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DA6","modrá obd. zapuš. hlava tlačítka Ø16 s návratom neoznačená",0]
["ZB6DA5","OVL. HLAV. STLÁČACIA ŽLTÁ OBDĹŽ.",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110775525",{"v":4,"d":"4.00"},{"v":2,"d":"2.00"},{"v":3.5,"d":"3.50"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DA5","obdĺžniková hlavica tlačidla – Ø 16 – žltá",0]
["ZB6DA4","OVL. HLAV. STLÁČACIA ČERVENÁ OBDĹŽ.",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110775518",{"v":16,"d":"16.00"},{"v":2.5,"d":"2.50"},{"v":11,"d":"11.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DA4","obdĺžniková hlavica tlačidla – Ø 16 – červená",0]
["ZB6DA3","OVL. HLAV. STLÁČACIA ZELENÁ OBDĹŽ.",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110775501",{"v":13.7,"d":"13.70"},{"v":3,"d":"3.00"},{"v":3.6,"d":"3.60"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DA3","obdĺžniková hlavica tlačidla – Ø 16 – zelená",0]
["ZB6DA2","OVL. HLAV. STLÁČACIA ČIERNA OBDĹŽ.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110775495",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DA2","obdĺžniková hlavica tlačidla – Ø 16 – čierna",0]
["ZB6DA1","OVL. HLAV. STLÁČACIA BIELA OBDĹŽ.",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110775488",{"v":5.4,"d":"5.40"},{"v":2.3,"d":"2.30"},{"v":7.5,"d":"7.50"},{"v":12,"d":"12.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6DA1","obdĺžniková hlavica tlačidla – Ø 16 – biela",0]
["ZB6CW6","ŠTVORC. ZAPUS. PRESV. TLAČIDLO MODRÉ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110849011",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CW6","štvorcová hlavica osvetleného tlačidla – Ø 16 – modrá",0]
["ZB6CW5","ŠTVORC. ZAPUS. PRESV. TLAČIDLO ŽLTÉ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110776010",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CW5","štvorcová hlavica osvetleného tlačidla – Ø 16 – žltá",0]
["ZB6CW4","ŠTVORC. ZAPUS. PRESV. TLAČIDLO ČERV.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110776003",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB6CW4","štvorcová hlavica osvetleného tlačidla – Ø 16 – červená",0]
["ZB6CW3","ŠTVORC. ZAPUS. PRESV. TLAČIDLO ZELENÉ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110775990",{"v":8,"d":"8.00"},{"v":2.5,"d":"2.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CW3","štvorcová hlavica osvetleného tlačidla – Ø 16 – zelená",0]
["ZB6CW1","ŠTVORC. ZAPUS. PRESV. TLAČIDLO BIELE",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110775983",{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CW1","štvorcová hlavica osvetleného tlačidla – Ø 16 – biela",0]
["ZB6CV4","ŠTVORC. SIGNÁLKA ČERVENÁ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110775624",{"v":10,"d":"10.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CV4","kryt kontrolky – Ø 16 – štvorcový – červená hladká šošovka",0]
["ZB6CV3","ŠTVORC. SIGNÁLKA ZELENÁ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110775617",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":7,"d":"7.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CV3","kryt kontrolky – Ø 16 – štvorcový – zelená hladká šošovka",0]
["ZB6CGT","OVL. HLAVA ŠTVORCOVÁ S KĽÚČOM",1,"ks",{"v":41.635912499999996,"d":"41.636"},"3389110785302",{"v":0.2,"d":"0.20"},0.12,{"v":0.1,"d":"0.10"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CGT","štvorcová ovládateľná otočná hlavica Ø16 3-polohy s návratom Ronis 200",0]
["ZB6CGQ","OVL. HLAVA ŠTVORCOVÁ S KĽÚČOM",1,"ks",{"v":41.635912499999996,"d":"41.636"},"3389110785272",{"v":0.2,"d":"0.20"},0.12,{"v":0.1,"d":"0.10"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CGQ","Head for key selector switch, Harmony XB6, square Ø 16 3 position spring return 200",0]
["ZB6CGH","OVL. HLAVA ŠTVORCOVÁ S KĽÚČOM",1,"ks",{"v":37.9756125,"d":"37.976"},"3389110785203",{"v":0.2,"d":"0.20"},0.12,{"v":0.1,"d":"0.10"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CGH","štvorcová ovládateľná otočná hlavica Ø16 3-polohy pevné Ronis 200",0]
["ZB6CGF","OVL. HLAVA ŠTVORCOVÁ S KĽÚČOM",1,"ks",{"v":37.9756125,"d":"37.976"},"3389110785180",{"v":0.2,"d":"0.20"},0.12,{"v":0.1,"d":"0.10"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CGF","Head for key selector switch, Harmony XB6, square Ø 16 3 position stay put 200",0]
["ZB6CGC","OVL. HLAVA ŠTVORCOVÁ S KĽÚČOM",1,"ks",{"v":37.0605375,"d":"37.061"},"3389110785159",{"v":7,"d":"7.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CGC","štvorcová ovládateľná otočná hlavica Ø16 2-polohy pevné Ronis 200",0]
["ZB6CGB","OVL. HLAVA ŠTVORCOVÁ S KĽÚČOM",1,"ks",{"v":37.0605375,"d":"37.061"},"3389110785142",{"v":6,"d":"6.00"},{"v":1.8,"d":"1.80"},{"v":1.8,"d":"1.80"},{"v":27.5,"d":"27.50"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CGB","štvorcová ovládateľná otočná hlavica Ø16 2-polohy pevné Ronis 200",0]
["ZB6CF3","OVL.HL.STLÁČACIA PRESV.S ARETÁCIOU",1,"ks",{"v":10.065825,"d":"10.066"},"3389110776225",{"v":4.5,"d":"4.50"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CF3","štvorcová hlavica osvetleného tlačidla – Ø 16 – zelená",0]
["ZB6CF1","OVL.HL.STLÁČACIA PRESV.S ARETÁCIOU",1,"ks",{"v":10.065825,"d":"10.066"},"3389110776218",{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":2.5,"d":"2.50"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CF1","štvorcová hlavica osvetleného tlačidla – Ø 16 – biela",0]
["ZB6CE3","TLAČIDLO ŠTVORC. PRESV. ZELENÉ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110776348",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CE3","štvorcová hlavica osvetleného tlačidla – Ø 16 – zelená",0]
["ZB6CD28","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110070804",{"v":6,"d":"6.00"},{"v":4,"d":"4.00"},{"v":5.8,"d":"5.80"},{"v":11,"d":"11.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CD28","štvorcová hlavica voliaceho spínača – 2 polohy Ø 16 – čierna",0]
["ZB6CD25","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110776836",{"v":5,"d":"5.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CD25","štvorcová hlavica voliaceho spínača – 3 polohyØ 16 – čierna",0]
["ZB6CD23","OTOČ. OVLÁDAČ ŠTVORCOVÝ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110776812",{"v":7,"d":"7.00"},{"v":2.5,"d":"2.50"},{"v":6,"d":"6.00"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CD23","štvorcová hlavica voliaceho spínača – 3 polohy Ø 16 – čierna",0]
["ZB6CD22","OTOČ. OVLÁDAČ ŠTVORCOVÝ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110776805",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CD22","štvorcová hlavica voliaceho spínača – 2 polohy Ø 16 – čierna",0]
["ZB6CD02","OTOČ. OVL. ŠTVORC. BEZ RUKOVÄTE",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110777161",{"v":13,"d":"13.00"},{"v":6,"d":"6.00"},{"v":7,"d":"7.00"},{"v":6,"d":"6.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CD02","štvorcová hlavica osvetleného voliaceho spínača – 2 polohy Ø 16 – čierna",0]
["ZB6CA3","OVL. HLAV. STLÁČACIA ZELENÁ ŠTVOR.",1,"ks",{"v":10.065825,"d":"10.066"},"3389110775457",{"v":4.5,"d":"4.50"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CA3","štvorcová hlavica tlačidla – Ø 16 – zelená",0]
["ZB6CA2","OVL. HLAV. STLÁČACIA ČIERNA ŠTVOR.",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110775440",{"v":3.5,"d":"3.50"},{"v":2.5,"d":"2.50"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6CA2","štvorcová hlavica tlačidla – Ø 16 – čierna",0]
["ZB6AW6","OKR. ZAPUS. PRESV. TLAČIDLO MODRÉ",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110849004",{"v":4,"d":"4.00"},{"v":2.5,"d":"2.50"},{"v":2.5,"d":"2.50"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AW6","hlavica osvetleného tlačidla – Ø 16 – modrá",0]
["ZB6AW5","OKR. ZAPUS. PRESV. TLAČIDLO ŽLTÉ",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110775976",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":7,"d":"7.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AW5","hlavica osvetleného tlačidla – Ø 16 – žltá",0]
["ZB6AW4","OKR. ZAPUS. PRESV. TLAČIDLO ČERVENÉ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110775969",{"v":9.8,"d":"9.80"},{"v":2.6,"d":"2.60"},{"v":4.9,"d":"4.90"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AW4","hlavica osvetleného tlačidla – Ø 16 – červená",0]
["ZB6AW3","OKR. ZAPUS. PRESV. TLAČIDLO ZELENÉ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110784190",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AW3","hlavica osvetleného tlačidla – Ø 16 – zelená",0]
["ZB6AV6","OKRÚHLA SIGNÁLKA MODRÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110849103",{"v":13.3,"d":"13.30"},{"v":2.9,"d":"2.90"},{"v":4.1,"d":"4.10"},{"v":8,"d":"8.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB6AV6","kryt kontrolky – Ø 16 – okrúhly – modrá hladká šošovka",0]
["ZB6AV5","OVL. HLAVICA SIGNALIZAČNÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110775594",{"v":7,"d":"7.00"},{"v":2.5,"d":"2.50"},{"v":7,"d":"7.00"},{"v":8,"d":"8.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB6AV5","kryt kontrolky – Ø 16 – okrúhly – žltá hladká šošovka",0]
["ZB6AV4","OVL. HLAVICA SIGNALIZAČNÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110775587",{"v":8.6,"d":"8.60"},{"v":3.2,"d":"3.20"},{"v":5.1,"d":"5.10"},{"v":8,"d":"8.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB6AV4","kryt kontrolky – Ø 16 – okrúhly – červená hladká šošovka",0]
["ZB6AV3","OVL. HLAVICA SIGNALIZAČNÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110775570",{"v":8.6,"d":"8.60"},{"v":3.2,"d":"3.20"},{"v":5.1,"d":"5.10"},{"v":8,"d":"8.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB6AV3","kryt kontrolky – Ø 16 – okrúhly – zelená hladká šošovka",0]
["ZB6AV1","OVL. HLAVICA SIGNALIZAČNÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110775563",{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB6AV1","kryt kontrolky – Ø 16 – okrúhly – biela hladká šošovka",0]
["ZB6AS934","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":52.159274999999994,"d":"52.159"},"3389110071566",{"v":4.2,"d":"4.20"},{"v":5.8,"d":"5.80"},{"v":5,"d":"5.00"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AS934","Head for emergency stop push button, Harmony XB6, red mushroom 30mm, 16mm, trigger/latching key to release, unmarked",0]
["ZB6AS834","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":25.1645625,"d":"25.165"},"3389110071559",{"v":4.5,"d":"4.50"},{"v":6.2,"d":"6.20"},{"v":5.6,"d":"5.60"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AS834","okrúhla hlavica pre tlačidlo núdz. vyp. – Ø 16 – uvoľ. otočením – červená",0]
["ZB6AGS","OKRÚH. OVL. HLAVA S KĽÚČOM",1,"ks",{"v":41.635912499999996,"d":"41.636"},"3389110785111",{"v":5.842,"d":"5.84"},{"v":1.778,"d":"1.78"},{"v":1.778,"d":"1.78"},{"v":27.216,"d":"27.22"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AGS","ovládateľná hlavica otočná Ø16 3-polohy s návratom Ronis 200",0]
["ZB6AGQ","OKRÚH. OVL. HLAVA S KĽÚČOM",1,"ks",{"v":41.635912499999996,"d":"41.636"},"3389110785098",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AGQ","Head for key selector switch, Harmony XB6, Ø 16 3 position spring return 200",0]
["ZB6AGL","OKRÚH. OVL. HLAVA S KĽÚČOM",1,"ks",{"v":40.720837499999995,"d":"40.721"},"3389110785050",{"v":6.5,"d":"6.50"},{"v":2.5,"d":"2.50"},{"v":2.5,"d":"2.50"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AGL","ovládateľná hlavica otočná Ø16 2-polohy s návratom Ronis 200",0]
["ZB6AGH","OKRÚH. OVL. HLAVA S KĽÚČOM",1,"ks",{"v":37.9756125,"d":"37.976"},"3389110785029",{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":25,"d":"25.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AGH","ovládateľná hlavica otočná Ø16 3-polohy pevné Ronis 200",0]
["ZB6AGD","OKRÚH. OVL. HLAVA S KĽÚČOM",1,"ks",{"v":37.9756125,"d":"37.976"},"3389110784985",{"v":0.2,"d":"0.20"},0.12,{"v":0.1,"d":"0.10"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AGD","Head for key selector switch, Harmony XB6, Ø 16 3 position stay put 200",0]
["ZB6AGC","OKRÚH. OVL. HLAVA S KĽÚČOM",1,"ks",{"v":37.0605375,"d":"37.061"},"3389110784978",{"v":6,"d":"6.00"},{"v":1.8,"d":"1.80"},{"v":1.8,"d":"1.80"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AGC","ovládateľná hlavica otočná Ø16 2-polohy pevné Ronis 200",0]
["ZB6AGB","OKRÚH. OVL. HLAVA S KĽÚČOM",1,"ks",{"v":38.43315,"d":"38.433"},"3389110784961",{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AGB","ovládateľná hlavica otočná Ø16 2-polohy pevné Ronis 200",0]
["ZB6AGA","OKRÚH. OVL. HLAVA S KĽÚČOM",1,"ks",{"v":37.0605375,"d":"37.061"},"3389110784954",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AGA","ovládateľná hlavica otočná Ø16 2-polohy pevné Ronis 200",0]
["ZB6AF6","OVLÁDAČ STLÁČACÍ PRESV. MODRÝ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110849035",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AF6","modrá ovl. hlavica stláčacia presvetlená-lícujúca Ø16 s aretáciou pre integ. LED",0]
["ZB6AF4","OVLÁDAČ STLÁČACÍ PRESV. ČERVENÝ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110776171",{"v":6,"d":"6.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AF4","červená ovl. hlavica stláčacia presvet.-lícujúca Ø16 s aretáciou pre integ. LED",0]
["ZB6AF3","OVLÁDAČ STLÁČACÍ PRESV. ZELENÝ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110776164",{"v":5,"d":"5.00"},{"v":2,"d":"2.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AF3","zelená ovl. hlavica stláčacia presvet.-lícujúca Ø16 s aretáciou pre integ. LED",0]
["ZB6AE4","OTOČ. OVLÁDAČ PRESV. ČERVENÝ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110776317",{"v":4,"d":"4.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AE4","červená ovladateľná hlavica presvet.stískacia s presahom Ø16 s návratom 12...24V",0]
["ZB6AE3","OVL. HLAVICA STLÁČ. PRESVETL.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110776300",{"v":4,"d":"4.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AE3","zelená ovl. hlavica stláčacia s presahom Ø16 s návratom 12...24V",0]
["ZB6AD28","OVL. HLAVICA OTOČNÁ PRIEMER 16MM",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110070781",{"v":9.6,"d":"9.60"},{"v":3.4,"d":"3.40"},{"v":4.6,"d":"4.60"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AD28","hlavica voliaceho spínača – 2 polohy Ø 16 – čierna",0]
["ZB6AD27","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110776799",{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":6.4,"d":"6.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AD27","hlavica voliaceho spínača – 3 polohy Ø 16 – čierna",0]
["ZB6AD26","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110776782",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":17,"d":"17.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB6AD26","Head for selector switch, Harmony XB6, black Ø 16 3 position spring return",0]
["ZB6AD25","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110776775",{"v":13.2,"d":"13.20"},{"v":2.6,"d":"2.60"},{"v":4.7,"d":"4.70"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AD25","hlavica voliaceho spínača – 3 polohy Ø 16 – čierna",0]
["ZB6AD23","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110776751",{"v":5,"d":"5.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AD23","hlavica voliaceho spínača – 3 polohy Ø 16 – čierna",0]
["ZB6AD22","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110776744",{"v":7,"d":"7.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AD22","hlavica voliaceho spínača – 2 polohy Ø 16 – čierna",0]
["ZB6AC2","OVLÁDACIA HLAVICA S HRÍBOM",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110070903",{"v":6.4,"d":"6.40"},{"v":8,"d":"8.00"},{"v":2.1,"d":"2.10"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AC2","hlavica tlačidla – Ø 24 – Ø 16 – čierna",0]
["ZB6AA6","OVL. HLAV. STLÁČACIA MODRÁ OKR.",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110288209",{"v":4,"d":"4.00"},{"v":2.1,"d":"2.10"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AA6","hlavica tlačidla – Ø 16 – modrá",0]
["ZB6AA4","OVL. HLAV. STLÁČACIA ČERVENÁ OKR.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110775402",{"v":5,"d":"5.00"},{"v":2.3,"d":"2.30"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AA4","hlavica tlačidla – Ø 16 – červená",0]
["ZB6AA3","OVL. HLAV. STLÁČACIA ZELENÁ OKR.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110775419",{"v":4.5,"d":"4.50"},{"v":2,"d":"2.00"},{"v":3.5,"d":"3.50"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AA3","hlavica tlačidla – Ø 16 – zelená",0]
["ZB6AA2","OVL. HLAV. STLÁČACIA ČIERNA OKR.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110775396",{"v":8.1,"d":"8.10"},{"v":4,"d":"4.00"},{"v":5.2,"d":"5.20"},{"v":8,"d":"8.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB6AA2","hlavica tlačidla – Ø 16 – čierna",0]
["ZB5SZ70","OCHRANNÝ KRYT PRE BIOMETR. SNÍMAČ",1,"ks",{"v":8.784719999999998,"d":"8.785"},"3389119044974",{"v":18,"d":"18.00"},{"v":2,"d":"2.00"},{"v":12,"d":"12.00"},{"v":6,"d":"6.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5SZ70","samolepiaci ochranný kryt - pre biometrický spínač",0]
["ZB5SZ5","ZASLEPOVACIA KRYTKA",10,"ks",{"v":2.4249487499999995,"d":"2.425"},"3389110099539",{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5SZ5","čierna štvorcová záslepka pre Ø22 otvor",0]
["ZB5SZ3C0","DIA 22 Záslepka",1,"ks",{"v":1.9674112499999996,"d":"1.967"},"3606489754792",{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5SZ3C0","Harmony XB5, Blanking plug, plastic, grey, for Ø22 hole",0]
["ZB5SZ3","ZASLEPOVACIA KRYTKA",10,"ks",{"v":1.8759037499999995,"d":"1.876"},"3389110099522",{"v":2.8,"d":"2.80"},{"v":2.3,"d":"2.30"},{"v":2.8,"d":"2.80"},{"v":8,"d":"8.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5SZ3","čierna kruhová záslepka pre Ø22 otvor",0]
["ZB5RTC2","Zostava ovládacie hlavice s hríb. 40 mm",1,"ks",{"v":119.87482499999999,"d":"119.875"},"3606480571763",{"v":12.4,"d":"12.40"},{"v":4,"d":"4.00"},{"v":5.2,"d":"5.20"},{"v":68,"d":"68.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTC2","VYSIELAČ - 40MM HUBOVÁ HLAVICA S PRUŽ NÁVRATOM",""]
["ZB5RTA6","NEZÁVISLÉ TLAČ. VYSIELAČ, PLAST, MODRÁ",1,"ks",{"v":91.5075,"d":"91.508"},"3606480334641",{"v":8.4,"d":"8.40"},{"v":3,"d":"3.00"},{"v":5.4,"d":"5.40"},{"v":54,"d":"54.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTA6","XB5 vysielač - Ø22 mm plastová hlava - modrá",0]
["ZB5RTA5","NEZÁVISLÉ TLAČ. VYSIELAČ, PLAST, ŽLTÁ",1,"ks",{"v":91.5075,"d":"91.508"},"3606480334634",{"v":9.2,"d":"9.20"},{"v":3.6,"d":"3.60"},{"v":5.4,"d":"5.40"},{"v":54,"d":"54.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTA5","XB5 vysielač - Ø22 mm plastová hlava - žltá",0]
["ZB5RTA432","NEZÁVISLÉ TLAČ. VYSIELAČ, PLAST, ZN \"O\"",1,"ks",{"v":91.5075,"d":"91.508"},"3606480334627",{"v":8.6,"d":"8.60"},{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":39,"d":"39.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTA432","XB5 vysielač - Ø22 mm plastová hlava - biela O na červenom podklade",0]
["ZB5RTA4","NEZÁVISLÉ TLAČ. VYSIELAČ, PLAST, ČERVENÁ",1,"ks",{"v":91.5075,"d":"91.508"},"3606480334610",{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":5.3,"d":"5.30"},{"v":38,"d":"38.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTA4","XB5 vysielač - Ø22 mm plastová hlava - červená",0]
["ZB5RTA331","NEZÁVISLÉ TLAČ. VYSIELAČ, PLAST, ZN \"I\"",1,"ks",{"v":91.5075,"d":"91.508"},"3606480334603",{"v":8.7,"d":"8.70"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":50.9,"d":"50.90"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTA331","XB5 vysielač - Ø22 mm plastová hlava - biela I na zelenom podklade",0]
["ZB5RTA3","NEZÁVISLÉ TLAČ. VYSIELAČ, PLAST, ZELENÁ",1,"ks",{"v":91.5075,"d":"91.508"},"3606480334597",{"v":8.7,"d":"8.70"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":50.9,"d":"50.90"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTA3","XB5 vysielač - Ø22 mm plastová hlava - zelená",0]
["ZB5RTA2","NEZÁVISLÉ TLAČ. VYSIELAČ, PLAST, ČIERNA",1,"ks",{"v":91.5075,"d":"91.508"},"3606480334580",{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":5.3,"d":"5.30"},{"v":38,"d":"38.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTA2","XB5 vysielač - Ø22 mm plastová hlava - čierna",0]
["ZB5RTA1","NEZÁVISLÉ TLAČ. VYSIELAČ, PLAST, BIELA",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3606480334573",{"v":8.4,"d":"8.40"},{"v":3.2,"d":"3.20"},{"v":5.4,"d":"5.40"},{"v":52,"d":"52.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB5RTA1","XB5 vysielač - Ø22 mm plastová hlava - biela",0]
["ZB5CH313","CABEZA PULS.LUM.SAL.CUAD. BLANCO",1,"ks",{"v":21.046725,"d":"21.047"},"3389110177343",{"v":4.5,"d":"4.50"},{"v":3.1,"d":"3.10"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5CH313","bielá štvorc.ovl.hlav.stláčacia presvet.,lícujúca Ø22\"stiskni-stiskni\",integ.LED",0]
["ZB5FW933","Zapustené prevedenie, Ovl. hlavica stisk",1,"ks",{"v":19.674112499999996,"d":"19.674"},"3606481339713",5.33,5.59,4.32,{"v":20,"d":"20.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FW933","Head for illuminated push button, Harmony XB5, plastic, green flush mounted, 30mm, universal LED, illuminated ring",0]
["ZB5FW383","Zapustené prevedenie, Ovl. hlavica stisk",1,"ks",{"v":7.631725499999999,"d":"7.632"},"3606481339751",{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FW383","Harmony XB5, Antimikrobiálna hlavica podsvieteného stláčacieho ovládača, zapustené prevedenie, plast, žltá, Ø30, s návratom, bez symbolu",""]
["ZB5FW363","Zapustené prevedenie, Ovl. hlavica stisk",1,"ks",{"v":7.640876249999998,"d":"7.641"},"3606481339706",{"v":5.2,"d":"5.20"},{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FW363","Harmony XB5, Antimikrobiálna hlavica podsvieteného stláčacieho ovládača, zapustené prevedenie, plast, modrá, Ø30, s návratom, bez symbolu",0]
["ZB5FW343","Zapustené prevedenie, Ovl. hlavica stisk",1,"ks",{"v":7.631725499999999,"d":"7.632"},"3606481339683",{"v":5.2,"d":"5.20"},{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FW343","Harmony XB5, Antimikrobiálna hlavica podsvieteného stláčacieho ovládača, zapustené prevedenie, plast, červená, Ø30, s návratom, bez symbolu",""]
["ZB5FW333","Zapustené prevedenie, Ovl. hlavica stisk",1,"ks",{"v":8.784719999999998,"d":"8.785"},"3606481339676",{"v":5.2,"d":"5.20"},{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FW333","Harmony XB5, Antimikrobiálna hlavica podsvieteného stláčacieho ovládača, zapustené prevedenie, plast, zelená, Ø30, s návratom, bez symbolu",0]
["ZB5FW313","Zapustené prevedenie, Ovl. hlavica stlač",1,"ks",{"v":8.05266,"d":"8.053"},"3606481339669",{"v":5.3,"d":"5.30"},{"v":5.7,"d":"5.70"},{"v":4.5,"d":"4.50"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FW313","Harmony XB5, Antimikrobiálna hlavica podsvieteného stláčacieho ovládača, zapustené prevedenie, plast, biela, Ø30, s návratom, bez symbolu",0]
["ZB5FV083","Zapustené prevedenie, Signálna hlavica",1,"ks",{"v":4.721787,"d":"4.722"},"3606481340788",{"v":5.7,"d":"5.70"},{"v":4.5,"d":"4.50"},{"v":5.3,"d":"5.30"},{"v":22,"d":"22.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5FV083","Harmony XB5, Antimikrobiálna hlavica signálky , zapustené prevedenie, plast, žltá, Ø30, priesvitná šošovka pre integral led",""]
["ZB5FV053","Zapustené prevedenie, Signálna hlavica",1,"ks",{"v":4.98715875,"d":"4.987"},"3606481340764",{"v":5.3,"d":"5.30"},{"v":5.7,"d":"5.70"},{"v":4.5,"d":"4.50"},{"v":22,"d":"22.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5FV053","Harmony XB5, Antimikrobiálna hlavica signálky , zapustené prevedenie, plast, oranžová, Ø30, priesvitná šošovka pre integral led",0]
["ZB5FV043","Zapustené prevedenie, Signálna hlavica",1,"ks",{"v":4.98715875,"d":"4.987"},"3606481340757",{"v":5.2,"d":"5.20"},{"v":5.4,"d":"5.40"},{"v":4.3,"d":"4.30"},{"v":15,"d":"15.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5FV043","Harmony XB5, Antimikrobiálna hlavica signálky , zapustené prevedenie, plast, červená, Ø30, priesvitná šošovka pre integral led",0]
["ZB5FV013","Zapustené prevedenie, Signálna hlavica",1,"ks",{"v":4.98715875,"d":"4.987"},"3606481340733",{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":15,"d":"15.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5FV013","Harmony XB5, Antimikrobiálna hlavica signálky , zapustené prevedenie, plast, biela, Ø30, priesvitná šošovka pre integral led",0]
["ZB5FL432","Ovl. Hlavica stláčacia, zapustené, so sy",1,"ks",{"v":6.524484749999999,"d":"6.524"},"3606481361653",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.3,"d":"5.30"},{"v":25,"d":"25.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5FL432","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, červená, Ø30, s návratom, symbol O",""]
["ZB5FL4","Zapustené prevedenie, Ovládacia hlavica",1,"ks",{"v":6.81730875,"d":"6.817"},"3606481339638",5.59,4.57,5.59,{"v":20,"d":"20.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FL4","Harmony XB5, Antimicrobial Flush mounted push button head, plastic, projecting, red, Ø30, spring return, unmarked, dark grey bezel",0]
["ZB5FK1583","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606481339744",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FK1583","Head for illuminated selector switch, Harmony XB5, plastic, yellow handle, universal LED, 3 positions, to center",0]
["ZB5FK1563","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606481340368",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FK1563","Head for illuminated selector switch, Harmony XB5, plastic, blue handle, universal LED, 3 positions, to center",0]
["ZB5FK1543","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606481340351",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FK1543","Head for illuminated selector switch, Harmony XB5, plastic, red handle, universal LED, 3 positions, to center",0]
["ZB5FK1533","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606481339584",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FK1533","Head for illuminated selector switch, Harmony XB5, plastic, green handle, universal LED, 3 positions, to center",0]
["ZB5FK1463","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":36.145462499999994,"d":"36.145"},"3606481340344",5.59,5.33,4.57,{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FK1463","Head for illuminated selector switch, Harmony XB5, plastic, blue handle, universal LED, 2 positions, spring return",0]
["ZB5FK1433","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3606481340313",5.33,5.59,4.57,{"v":30,"d":"30.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FK1433","Head for illuminated selector switch, Harmony XB5, plastic, green handle, flush mounted, universal LED, 2 positions",0]
["ZB5FK1363","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606481340290",{"v":6.1,"d":"6.10"},5.08,4.32,{"v":30,"d":"30.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FK1363","Head for illuminated selector switch, Harmony XB5, plastic, blue handle, flush mounted, universal LED, 3 positions",0]
["ZB5FK1353","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606481339560",{"v":5.588,"d":"5.59"},{"v":5.334,"d":"5.33"},{"v":4.318,"d":"4.32"},{"v":27.216,"d":"27.22"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FK1353","Head for illuminated selector switch, Harmony XB5, plastic, orange handle, flush mounted, universal LED, 3 positions",0]
["ZB5FK1283","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3606481339720",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FK1283","Head for illuminated selector switch, Harmony XB5, plastic, yellow handle, universal LED, 2 positions, stay put",0]
["ZB5FK1263","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3606481339522",5.33,5.84,4.57,{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FK1263","Head for illuminated selector switch, Harmony XB5, plastic, blue handle, universal LED, 2 positions, stay put",0]
["ZB5FK1243","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3606481339508",{"v":5.334,"d":"5.33"},{"v":5.588,"d":"5.59"},{"v":4.572,"d":"4.57"},{"v":27.216,"d":"27.22"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FK1243","Head for illuminated selector switch, Harmony XB5, plastic, red handle, universal LED, 2 positions, stay put",0]
["ZB5FK1233","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3606481339492",5.59,5.59,4.57,{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FK1233","Head for illuminated selector switch, Harmony XB5, universal LED,  green handle, flush, 22mm, 2 positions, stay put",0]
["ZB5FK1213","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3606481339485",5.33,5.59,4.57,{"v":30,"d":"30.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FK1213","Head for illuminated selector switch, Harmony XB5, plastic, white handle, universal LED, 2 positions, stay put",0]
["ZB5FJ5","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":10.5233625,"d":"10.523"},"3606481339478",5.33,5.59,4.57,{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FJ5","Head for selector switch, Harmony XB5, flush mounted black long handle 3 pos return center",0]
["ZB5FJ3C0","Ovládacia hlavica otočná, zapustené, ČI,",1,"ks",{"v":9.928563749999999,"d":"9.929"},"3606489773380",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FJ3C0","Harmony XB5, Flush mounted selector switch head, plastic, black, Ø30, long handle, 3 positions, stay put, grey bezel",""]
["ZB5FJ3","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3606481339461",5.33,5.59,4.57,{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FJ3","Head for selector switch, Harmony XB5, flush mounted black long handle 3 pos stay put",0]
["ZB5FJ2","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":7.640876249999998,"d":"7.641"},"3606481339454",{"v":5.334,"d":"5.33"},{"v":5.588,"d":"5.59"},{"v":4.572,"d":"4.57"},{"v":27.216,"d":"27.22"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FJ2","Head for selector switch, Harmony XB5, flush mounted black long handle 2 pos stay put",0]
["ZB5FH43C0","Ovládacia hlavica stláčacia presvetlená,",1,"ks",{"v":19.216575,"d":"19.217"},"3606489773229",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":25,"d":"25.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FH43C0","Head for illuminated push button, Harmony XB5, grey bezel, red projecting, 30mm, universal LED, push-push, unmarked",0]
["ZB5FH01C0","Ovládacia hlavica, zapustené, BI,",1,"ks",{"v":13.2685875,"d":"13.269"},"3606489772888",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":25,"d":"25.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FH01C0","Harmony XB5, Flush mounted push button head, plastic, white, Ø30, push-push, grey bezel",0]
["ZB5FG6","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3606481339423",9.14,5.33,4.32,{"v":60,"d":"60.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FG6","Head for key selector switch, Harmony XB5, flush mounted 455 2 pos return right to left",0]
["ZB5FG4","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3606481339393",5.33,8.89,4.57,{"v":70,"d":"70.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FG4","Head for key selector switch, Harmony XB5, Harmony XALF, flush mounted 455 2 pos stay put",0]
["ZB5FG2D","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":28.824862499999995,"d":"28.825"},"3606481339379",8.89,4.57,5.33,{"v":70,"d":"70.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FG2D","Head for key selector switch, Harmony XB5, flush mounted 8D1 2 pos stay put",0]
["ZB5FG2","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3606481339362",{"v":5.2,"d":"5.20"},{"v":8.6,"d":"8.60"},{"v":4.3,"d":"4.30"},{"v":73,"d":"73.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FG2","Head for key selector switch, Harmony XB5, Harmony XALF, flush mounted 455 2 pos stay put",0]
["ZB5FG02","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3606481340085",5.33,8.89,4.57,{"v":70,"d":"70.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FG02","Head for key selector switch, Harmony XB5, flush mounted 455 2 pos stay put",0]
["ZB5FD8","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":9.681493499999998,"d":"9.681"},"3606481339300",5.33,5.59,4.57,{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FD8","Harmony XB5, Antimikrobiálna hlavica otočného ovládača, zapustené prevedenie, plast, čierna, Ø30, 3 polohy, s návratom sprava do stredu",""]
["ZB5FD5C0","Ovládacia hlavica, zapustené, ČI Ovládač",1,"ks",{"v":10.5233625,"d":"10.523"},"3606489771928",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FD5C0","Harmony XB5, Flush mounted selector switch head, plastic, black, Ø30, 3 positions, spring return to center, grey bezel",0]
["ZB5FD5","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":10.065825,"d":"10.066"},"3606481339287",{"v":5.2,"d":"5.20"},{"v":5.7,"d":"5.70"},{"v":4.3,"d":"4.30"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FD5","Harmony XB5, Antimikrobiálna hlavica otočného ovládača, zapustené prevedenie, plast, čierna, Ø30, 3 polohy, s návratom do stredu",0]
["ZB5FD4","Zapustené prevedenie,  Otočný ovládač",1,"ks",{"v":9.681493499999998,"d":"9.681"},"3606481339263",5.33,5.59,4.57,{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FD4","Harmony XB5, Antimikrobiálna hlavica otočného ovládača, zapustené prevedenie, plast, čierna, Ø30, 2 polohy, s návratom sprava doľava",""]
["ZB5FD3","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":8.55595125,"d":"8.556"},"3606481339256",{"v":6.2,"d":"6.20"},{"v":4.4,"d":"4.40"},{"v":5.3,"d":"5.30"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FD3","Harmony XB5, Antimikrobiálna hlavica otočného ovládača, zapustené prevedenie, plast, čierna, Ø30, 3 polohy, pevná pozícia",0]
["ZB5FD29","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":10.5233625,"d":"10.523"},"3606481339225",5.59,5.33,4.32,{"v":30,"d":"30.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FD29","Head for selector switch, Harmony XB5, flush mounted black knurled knob 2 pos stay put",0]
["ZB5FD203","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3606481339195",5.59,5.33,4.32,{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FD203","Head for selector switch, Harmony XB5, flush mounted green 2 pos stay put",0]
["ZB5FD201","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3606481339188",5.59,5.33,4.32,{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FD201","Head for selector switch, Harmony XB5, flush mounted white 2 pos stay put",0]
["ZB5FD2","Zapustené prevedenie, Otočný ovládač",1,"ks",{"v":7.549368749999999,"d":"7.549"},"3606481339232",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":28,"d":"28.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FD2","Harmony XB5, Antimikrobiálna hlavica otočného ovládača, zapustené prevedenie, plast, čierna, Ø30, 2 polohy, pevná pozícia",0]
["ZB5FA8C0","Ovládacia hlavica, zapustené, ŠE,",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3606489771324",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FA8C0","Harmony XB5, Flush mounted push button head, plastic, grey, Ø30, spring return, unmarked, grey bezel",0]
["ZB5FA8","Zapustené prevedenie, ovládacia hlavica",1,"ks",{"v":5.2159275,"d":"5.216"},"3606481339164",{"v":5.2,"d":"5.20"},5.45,{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FA8","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, grey, Ø30, s návratom, bez symbolu",0]
["ZB5FA6","Zapustené prevedenie, ovládacia hlavica",1,"ks",{"v":5.44469625,"d":"5.445"},"3606481339140",{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":24,"d":"24.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FA6","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, modrá, Ø30, s návratom, bez symbolu",0]
["ZB5FA5","Zapustené prevedenie, ovládacia hlavica",1,"ks",{"v":4.9505557499999995,"d":"4.951"},"3606481339126",{"v":5.3,"d":"5.30"},{"v":5.8,"d":"5.80"},{"v":4.5,"d":"4.50"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FA5","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, žltá, Ø30, s návratom, bez symbolu",""]
["ZB5FA432","Ovl. hlavica stláčacia so symbolom",1,"ks",{"v":5.17017375,"d":"5.170"},"3606481361356",{"v":5.8,"d":"5.80"},{"v":5.3,"d":"5.30"},{"v":4.3,"d":"4.30"},{"v":23.6,"d":"23.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5FA432","Harmony XB5, Antimicrobial Flush mounted push button head, plastic, red, Ø30, spring return, marked O, dark grey bezel",0]
["ZB5FA4","Zapustené prevedenie, ovládacia hlavica",1,"ks",{"v":5.2159275,"d":"5.216"},"3606481339102",{"v":5.4,"d":"5.40"},{"v":3.6,"d":"3.60"},{"v":5,"d":"5.00"},{"v":23,"d":"23.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FA4","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, červená, Ø30, s návratom, bez symbolu",0]
["ZB5FA333","Ovl. Hlavica stláčacia so symbolom",1,"ks",{"v":5.161022999999999,"d":"5.161"},"3606481361271",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.3,"d":"5.30"},{"v":24,"d":"24.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5FA333","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, zelená, Ø30, s návratom, symbol START",""]
["ZB5FA331","Ovl. Hlavica stláčacia so symbolom",1,"ks",{"v":5.161022999999999,"d":"5.161"},"3606481361264",{"v":5.8,"d":"5.80"},{"v":5.3,"d":"5.30"},{"v":4.3,"d":"4.30"},{"v":23.6,"d":"23.60"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5FA331","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, zelená, Ø30, s návratom, symbol I",""]
["ZB5FA3","Zapustené prevedenie, ovládacia hlavica,",1,"ks",{"v":5.2159275,"d":"5.216"},"3606481339072",{"v":6.3,"d":"6.30"},{"v":4.6,"d":"4.60"},{"v":5.4,"d":"5.40"},{"v":24,"d":"24.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FA3","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, zelená, Ø30, s návratom, bez symbolu",0]
["ZB5FA232","Ovl. Hlavica stláčacia so symbolom",1,"ks",{"v":6.1310025,"d":"6.131"},"3606481361219",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.3,"d":"5.30"},{"v":24,"d":"24.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5FA232","Harmony XB5, Antimicrobial Flush mounted push button head, plastic, black, Ø30, spring return, marked O, dark grey bezel",0]
["ZB5FA2","Zapustené prevedenie, ovládacia hlavica,",1,"ks",{"v":5.2159275,"d":"5.216"},"3606481339058",{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":5.4,"d":"5.40"},{"v":24,"d":"24.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5FA2","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, čierna, Ø30, s návratom, bez symbolu",0]
["ZB5FA1","Zapustené prevedenie, ovládacia hlavica",1,"ks",{"v":5.2159275,"d":"5.216"},"3606481339034",{"v":5.2,"d":"5.20"},{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FA1","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, biela, Ø30, s návratom, bez symbolu",0]
["ZB5FA0","Zapustené prevedenie, ovládacia hlavica",1,"ks",{"v":4.721787,"d":"4.722"},"3606481339027",{"v":5.2,"d":"5.20"},{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5FA0","Harmony XB5, Antimikrobiálna hlavica stláčacieho ovládača, zapustené prevedenie, plast, bez hmatníka, Ø30, s návratom",""]
["ZB5CW343","OVL. HLAVICA STLÁČ. PRESVETL. ČERVENÁ",1,"ks",{"v":25.6221,"d":"25.622"},"3389110934847",{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5CW343","štvorcová hlavica osvetleného tlačidla – Ø 22 – červená – na vloženie štítku",0]
["ZB5CW333","OVL. HLAVICA STLÁČ. PRESVETL. ZELENÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110934830",{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":5,"d":"5.00"},{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5CW333","štvorcová hlavica osvetleného tlačidla – Ø 22 – zelená – na vloženie štítku",0]
["ZB5CW313","OVL. HLAVICA STLÁČ. PRESVETL. BIELA",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110934823",{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5CW313","štvorcová okrúhla hlavica tlačidla – Ø 22 – biela – na vloženie štítku",0]
["ZB5CV053","SIGNÁL. HLAVICA PRE LED ŽLTÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110934755",{"v":5.4,"d":"5.40"},{"v":4.8,"d":"4.80"},{"v":3.5,"d":"3.50"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5CV053","kryt kontrolky – Ø 22 – štvorcový – žltá hladká šošovka",0]
["ZB5CV043","SIGNÁL. HLAVICA PRE LED ČERVENÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110934748",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5CV043","kryt kontrolky – Ø 22 – štvorcový – červená hladká šošovka",0]
["ZB5CV033","SIGNÁL. HLAVICA PRE LED ZELENÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110934731",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5CV033","kryt kontrolky – Ø 22 – štvorcový – zelená hladká šošovka",0]
["ZB5CV013","SIGNÁL. HLAVICA PRE LED BIELA",1,"ks",{"v":13.726125,"d":"13.726"},"3389110934724",{"v":4.4,"d":"4.40"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5CV013","kryt kontrolky – Ø 22 – štvorcový – biela hladká šošovka",0]
["ZB5AZ905","KĽÚČ NA UPEVNENIE MATICE",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3389110843101",{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":16,"d":"16.00"},"ID","8205598000","https://www.se.com/sk/sk/product/ZB5AZ905","uťahovací kľúč pre upevňovacie matice",0]
["ZB5AZ902","POISTNÁ PODLOŽKA",10,"ks",{"v":1.9674112499999996,"d":"1.967"},"3389110842715",{"v":9,"d":"9.00"},{"v":1,"d":"1.00"},{"v":9,"d":"9.00"},{"v":3,"d":"3.00"},"ID","8538909999","https://www.se.com/sk/sk/product/ZB5AZ902","poistná podložka pre jednotku Ø 22 mm – súprava 10 ks",0]
["ZB5AZ901","UPEVŇOVACIA MATICA",10,"ks",{"v":0.36602999999999997,"d":"0.366"},"3389110842647",{"v":3.048,"d":"3.05"},2.54,{"v":3.048,"d":"3.05"},{"v":4.536,"d":"4.54"},"ID","7318169290","https://www.se.com/sk/sk/product/ZB5AZ901","Upevňovacie matice pre Ø22 hlavu",0]
["ZB5AZ31","ŠTVORCOVÝ / KRUHOVÝ ADAPTÉR",10,"ks",{"v":0.9150749999999999,"d":"0.915"},"3389110102246",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AZ31","prídavná štvorcová lišta pre guľatú hlavicu na jednotku Ø 22 mm – súprava 10 ks",0]
["ZB5AZ141","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110925838",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":38,"d":"38.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ141","teleso pre ovládacie tlačidlo – Ø 22 – 2 NC + 1 NO",0]
["ZB5AZ106","CORPS CONTACS CHEVAUCHANT",1,"ks",{"v":21.5042625,"d":"21.504"},"3389110175844",{"v":4.5,"d":"4.50"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":30,"d":"30.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ106","teleso pre ovládacie tlačidlo – Ø 22 – prekrytie 1 NO + 1 NC",0]
["ZB5AZ1055","POLOZOSTAVA KONTAKTOV-PLA-NO+NC TERMINÁL",1,"ks",{"v":20.13165,"d":"20.132"},"3389119039291",{"v":5.2,"d":"5.20"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":29,"d":"29.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ1055","polozostava kontaktov 1Z+1V bezšróbové svorky",0]
["ZB5AZ105","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110925760",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ105","teleso pre ovládacie tlačidlo – Ø 22 – 1 NO+1 NC",0]
["ZB5AZ1045","POLOZOSTAVA KONTAKTOV-PLAS-2NC TERMINÁLY",1,"ks",{"v":11.4384375,"d":"11.438"},"3389119037754",{"v":4.8,"d":"4.80"},{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":29,"d":"29.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ1045","tel./upevňovacia príruba dotykového bloku - Ø 22 – 2 NC – IP20 – pružin. svorky",0]
["ZB5AZ1044","POLOZOSTAVA KONTAKTOV - NÁSUV. KONEKTOR",1,"ks",{"v":21.5042625,"d":"21.504"},"3389110925739",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ1044","teleso pre ovládacie tlačidlo – Ø 22 – 2 NC",0]
["ZB5AZ1043","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110816013",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":32,"d":"32.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AZ1043","polozostava kontaktov 2V konektor faston",0]
["ZB5AZ104","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110925708",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ104","teleso pre ovládacie tlačidlo – Ø 22 – 2 NC",0]
["ZB5AZ1035","POLOZOSTAVA KONTAKTOV-PLAS-2NO TERMINÁLY",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389119037747",{"v":4.6,"d":"4.60"},{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":29,"d":"29.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ1035","tel./upevňovacia príruba dotykového bloku - Ø 22 – 2 NO – IP20 – pružin. svorky",0]
["ZB5AZ103","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110924435",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29.2,"d":"29.20"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ103","teleso pre ovládacie tlačidlo – Ø 22 – 2 NO",0]
["ZB5AZ1025","POLOZOSTAVA KONTAKTOV-PLAST-NC TERMINÁL",1,"ks",{"v":7.0460775,"d":"7.046"},"3389119037730",{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":5.3,"d":"5.30"},{"v":20,"d":"20.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ1025","tel./upevňovacia príruba dotykového bloku - Ø 22 – 1 NC – IP20 – pružin. svorky",0]
["ZB5AZ1023","POLOZOSTAVA KONTAKTOV - NÁSUV. KONEKTOR",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110816006",{"v":4.5,"d":"4.50"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AZ1023","polozostava kontaktov 1V konektor faston",0]
["ZB5AZ102","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":6.359771249999999,"d":"6.360"},"3389110924411",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":20,"d":"20.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ102","teleso pre ovládacie tlačidlo – Ø 22 – 1 NC",0]
["ZB5AZ1015","POLOZOSTAVA KONTAKTOV-PLAST-NO TERMINÁL",1,"ks",{"v":7.320599999999999,"d":"7.321"},"3389119037723",{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":4.8,"d":"4.80"},{"v":20,"d":"20.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ1015","tel./upevňovacia príruba dotykového bloku - Ø 22 – 1 NO – IP20 – pružin. svorky",0]
["ZB5AZ1014","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":20.13165,"d":"20.132"},"3389110924404",5.33,3.05,4.32,{"v":20,"d":"20.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ1014","teleso pre ovládacie tlačidlo – Ø 22 – 1 NO",0]
["ZB5AZ1013","POLOZOSTAVA KONTAKTOV - NÁSUV. KONEKTOR",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110815931",{"v":4.3,"d":"4.30"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AZ1013","polozostava kontaktov 1Z konektor faston",0]
["ZB5AZ101","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":6.359771249999999,"d":"6.360"},"3389110924398",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":20.2,"d":"20.20"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AZ101","teleso pre ovládacie tlačidlo – Ø 22 – 1 NO",0]
["ZB5AZ079","Špeciálne príslušenstvo",1,"ks",{"v":4.3008525,"d":"4.301"},"3389110102222",{"v":7.1,"d":"7.10"},{"v":9,"d":"9.00"},{"v":7.1,"d":"7.10"},{"v":6,"d":"6.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AZ079","špeciálne príslušenstvo pre montáž do plošných strojov",0]
["ZB5AZ026","Montážná sada plastová zo štítkom 18x27",1,"ks",{"v":3.34002375,"d":"3.340"},"3606485440279",{"v":5.2,"d":"5.20"},{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":9,"d":"9.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AZ026","montážná sada plastová se štítkem 18x27",0]
["ZB5AZ025","Montážná sada plastová zo štítkom 18x27",1,"ks",{"v":3.34002375,"d":"3.340"},"3606485440262",{"v":5.2,"d":"5.20"},{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":17,"d":"17.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AZ025","montážná sada plastová se štítkem 18x27 (ovl. stláčacie a signálky).",0]
["ZB5AZ024","Montážna sada plastová so štítkom 8x27",1,"ks",{"v":4.34660625,"d":"4.347"},"3606485440255",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":8,"d":"8.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AZ024","montážná sada plastová se štítkem 8x27",0]
["ZB5AZ022","Montážná sada plast.(ovl.otoč.,stláč.)",1,"ks",{"v":4.438113749999999,"d":"4.438"},"3606485440231",{"v":5.7,"d":"5.70"},{"v":5.2,"d":"5.20"},{"v":5.5,"d":"5.50"},{"v":7,"d":"7.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AZ022","montážná sada plastová pre Ø22 (ovl. otočné a ovl. stláčacie presvetlené)",0]
["ZB5AZ021","Montážná sada plastová",1,"ks",{"v":4.34660625,"d":"4.347"},"3606485440224",{"v":5.5,"d":"5.50"},{"v":5.2,"d":"5.20"},{"v":4.3,"d":"4.30"},{"v":6,"d":"6.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AZ021","montážná sada plastová pre Ø22 (ovl. stláčacie a signálky).",0]
["ZB5AZ009","SPOJOVACÍ DIEL",10,"ks",{"v":1.60138125,"d":"1.601"},"3389110102215",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AZ009","upevňovacia príruba elektrického bloku pre Ø 22 mm jednotky XB5-A – súpr. 10 ks",0]
["ZB5AX84","Ovl. hlavica núdz. zastav. stlač-ťahaj",1,"ks",{"v":20.13165,"d":"20.132"},"3389119048088",{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":62,"d":"62.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AX84","60MM ČERV. OVL. HLAVICA 22MM NÚDZOVÉHO VYPNUTIA, STLAČ-ŤAHAJ",0]
["ZB5AW933","OVL. HLAVICA STLÁČ. PRESVETL. ZELENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110924336",{"v":5.4,"d":"5.40"},{"v":3.3,"d":"3.30"},{"v":4.5,"d":"4.50"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW933","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB5AW913","OVL. HLAVICA STLÁČ. PRESVETL. BIELA",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110924329",{"v":5.5,"d":"5.50"},{"v":3,"d":"3.00"},{"v":4.5,"d":"4.50"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW913","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB5AW7L3741","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3389119043380",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7L3741","zelená lícujúca/červená s presah.ovl.hlavica dvojtlač.so signálkou Ø22 s popisom",0]
["ZB5AW7L3740","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":13.726125,"d":"13.726"},"3389119043373",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7L3740","zelená lícujúca/červená s presah.ovl.hlavica dvojtlač.so sig. Ø22 neoznačená",0]
["ZB5AW7A9","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389119043410",{"v":4.8,"d":"4.80"},{"v":2.8,"d":"2.80"},{"v":4.8,"d":"4.80"},{"v":23.8,"d":"23.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7A9","zapuš./zapuš. ovl. hlavica dvojtlač. so signálkou Ø22 bez šošovky",0]
["ZB5AW7A3741","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":13.726125,"d":"13.726"},"3389119043366",{"v":5.5,"d":"5.50"},{"v":3,"d":"3.00"},{"v":5.5,"d":"5.50"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7A3741","zelená lícujúca/červená lícujúca ovl.hlavica dvojtlač.so signálkou Ø22 s popisom",0]
["ZB5AW7A3740","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389119043359",{"v":5.8,"d":"5.80"},{"v":3.3,"d":"3.30"},{"v":5.3,"d":"5.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7A3740","zelená lícujúca/červená lícujúca ovl.hlavica dvojtlač.so sig. Ø22 neoznačená",0]
["ZB5AW7A1724","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389119603478",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7A1724","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač.so signálkou Ø22 s popisom",0]
["ZB5AW7A1721","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":13.726125,"d":"13.726"},"3389119043342",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7A1721","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač.so signálkou Ø22 s popisom",0]
["ZB5AW7A1720","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389119043335",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7A1720","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač.so signálkou Ø22 neoznačená",0]
["ZB5AW7A1715","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3389119043403",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW7A1715","čer. Ø40 ovl.tlač.núdz.zastav.Ø22 vyp.s aretáciou \"uvolniť otočením\" 1Z+2V",0]
["ZB5AW763","OV.HLAVICA S HRÍBOM LED MODRÁ ODB. OTOČ",1,"ks",{"v":32.485162499999994,"d":"32.485"},"3389110666878",{"v":8.7,"d":"8.70"},{"v":4.2,"d":"4.20"},{"v":5.2,"d":"5.20"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW763","modrá Ø40 presvet. hlavica s hríbovým tlačítkom Ø22 s aretáciou pre integ. LED",0]
["ZB5AW753","OV.HLAVICA S HRÍBOM LED ORANŽ. ODB. OTOČ",1,"ks",{"v":32.485162499999994,"d":"32.485"},"3389110666861",{"v":8.8,"d":"8.80"},{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW753","oranžová Ø40 presvet.hlavica s hríbovým tlačítkom Ø22 s aretáciou pre integ.LED",0]
["ZB5AW743","OV.HLAVICA S HRÍBOM LED ČERVENÁ ODB.OTOČ",1,"ks",{"v":33.857775,"d":"33.858"},"3389110666854",{"v":5.4,"d":"5.40"},{"v":8.6,"d":"8.60"},{"v":4.2,"d":"4.20"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW743","biela Ø40 presvet. hlavica s hríbovým tlačítkom Ø22 s aretáciou pre integ. LED",0]
["ZB5AW733","OV.HLAVICA S HRÍBOM LED ZELENÁ ODB. OTOČ",1,"ks",{"v":33.857775,"d":"33.858"},"3389110666847",{"v":5.2,"d":"5.20"},{"v":5.4,"d":"5.40"},{"v":4.3,"d":"4.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW733","zelená Ø40 presvet. hlavica s hríbovým tlačítkom Ø22 s aretáciou pre integ. LED",0]
["ZB5AW563","OVL. HLAVICA STLÁČ. PRESVETL. MODRÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110924077",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.8,"d":"4.80"},{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW563","modrá ovl. hlavica stláčacia presvetlená-lícujúca Ø22 s návratom pre integ. LED",0]
["ZB5AW553","OVL. HLAVICA STLÁČ. PRESVETL. ŽLTÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110924060",{"v":4.5,"d":"4.50"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW553","oranžová ovl. hlavica stláčacia presvet.-lícujúca Ø22 s návratom pre integ. LED",0]
["ZB5AW543","OVL. HLAVICA STLÁČ. PRESVETL. ČERVENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110924053",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW543","červená ovl. hlavica presvet. stláčacia-lícujúca Ø22 s návratom pre integ. LED",0]
["ZB5AW533","OVL. HLAVICA STLÁČ. PRESVETL. ZELENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110924046",{"v":2.6,"d":"2.60"},{"v":4,"d":"4.00"},{"v":4.8,"d":"4.80"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW533","hlavica osvetleného tlačidla – Ø 22 – zelená – krytá",0]
["ZB5AW513","OVL. HLAVICA STLÁČ. PRESVETL. BIELA",1,"ks",{"v":10.065825,"d":"10.066"},"3389110922448",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW513","hlavica osvetleného tlačidla – Ø 22 – biela – krytá",0]
["ZB5AW383","OVL. HLAVICA STLÁČ. PRESVETL. ŽLTÁ",1,"ks",{"v":8.1441675,"d":"8.144"},"3606481206411",{"v":5.4,"d":"5.40"},{"v":3.6,"d":"3.60"},{"v":4.6,"d":"4.60"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW383","Head for illuminated push button, Harmony XB5, yellow flush, 22mm, universal LED, spring return, plain, unmarked",0]
["ZB5AW37","OVL. HLAVICA STLÁČ. PRESVETL. ČÍRA",1,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110137071",{"v":5.3,"d":"5.30"},{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":17,"d":"17.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW37","hlavica osvetleného tlačidla – Ø 22 – číra",0]
["ZB5AW363","OVL. HLAVICA STLÁČ. PRESVETL. MODRÁ",1,"ks",{"v":8.1441675,"d":"8.144"},"3389110922035",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW363","hlavica osvetleného tlačidla – Ø 22 – modrá",0]
["ZB5AW36","OVL. HLAVICA STLÁČ. PRESVETL. MODRÁ",1,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110909999",{"v":4.4,"d":"4.40"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW36","hlavica osvetleného tlačidla – Ø 22 – modrá",0]
["ZB5AW353","OVL. HLAVICA STLÁČ. PRESVETL. ŽLTÁ",1,"ks",{"v":8.1441675,"d":"8.144"},"3389110909982",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW353","hlavica osvetleného tlačidla – Ø 22 – žltá",0]
["ZB5AW35","OVL. HLAVICA STLÁČ. PRESVETL. ŽLTÁ",1,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110909975",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":18,"d":"18.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW35","hlavica osvetleného tlačidla – Ø 22 – žltá",0]
["ZB5AW343S","OVLÁDAČ STLÁČACÍ PRESVETLENÝ, ČERVENÝ",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110175899",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW343S","červená ovl hlavice stláčacia Prosveta .-Lícujúca Ø22 s návratom pre integ. LED",0]
["ZB5AW343C0","ČE Ovládacia hlavica stláčacia presvetle",1,"ks",{"v":7.549368749999999,"d":"7.549"},"3606489769987",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW343C0","Head for illuminated push button, Harmony XB5, grey bezel, red flush, 22mm, universal LED, spring return, plain lens",0]
["ZB5AW343","OVL. HLAVICA STLÁČ. PRESVETL. ČERVENÁ",1,"ks",{"v":8.1441675,"d":"8.144"},"3389110909968",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW343","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB5AW34","OVL. HLAVICA STLÁČ. PRESVETL. ČERVENÁ",1,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110909951",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW34","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB5AW333S","OVL. HLAVICA STLÁČ. PRESVETL. ZELENÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110175882",{"v":3.1,"d":"3.10"},{"v":4.5,"d":"4.50"},{"v":3.1,"d":"3.10"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW333S","zelená ovl hlavica stláčacia Prosveta . - Lícujúca Ø22 s návratom pre integ. LED",0]
["ZB5AW333","OVL. HLAVICA STLÁČ. PRESVETL. ZELENÁ",1,"ks",{"v":8.1441675,"d":"8.144"},"3389110909944",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW333","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB5AW33","OVL. HLAVICA STLÁČ. PRESVETL. ZELENÁ",1,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110909937",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW33","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB5AW313S","OVL. HLAVICA STLÁČ. PRESVETL. BIELA",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110175875",{"v":3.1,"d":"3.10"},{"v":4.5,"d":"4.50"},{"v":3.1,"d":"3.10"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW313S","biela ovl hlavica stláčacia Prosveta . - Licujúca Ø22 s návratom pre integ. LED",0]
["ZB5AW313","OVL. HLAVICA STLÁČ. PRESVETL. BIELA",1,"ks",{"v":8.1441675,"d":"8.144"},"3389110909920",{"v":5.1,"d":"5.10"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW313","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB5AW31","OVL. HLAVICA STLÁČ. PRESVETL. BIELA",1,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110909913",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":18,"d":"18.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW31","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB5AW163","OVL. HLAVICA STLÁČ. PRESVETL. MODRÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110909906",{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":4.8,"d":"4.80"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW163","modrá ovl. hlavica presvet. stláčacia s presahom Ø22 s návratom pre integ. LED",0]
["ZB5AW153","OVL. HLAVICA STLÁČ. PRESVETL. ŽLTÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110909883",{"v":4.4,"d":"4.40"},{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW153","oranžová ovl.hlavica presvet.stláčacia s presahom Ø22 s návratom pre integ.LED",0]
["ZB5AW15","OVL. HLAVICA STLÁČ. PRESVETL. ŽLTÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110909876",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW15","oranžová ovl.hlav. presvet.stláčacia s presahomØ22 s návratom pre BA9s žiarovku",0]
["ZB5AW143","OVL. HLAVICA STLÁČ. PRESVETL. ČERVENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110909869",{"v":5.3,"d":"5.30"},{"v":3.6,"d":"3.60"},{"v":4.7,"d":"4.70"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW143","červená ovl. hlavica presvet. stláčacia s presahom Ø22 s návratom pre integ. LED",0]
["ZB5AW14","OVL. HLAVICA STLÁČ. PRESVETL. ČERVENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110909852",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":16,"d":"16.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW14","červená ovl. hlavica presvet. stláčacia-lícujúca Ø22 s návratom pre integ. LED",0]
["ZB5AW133","OVL. HLAVICA STLÁČ. PRESVETL. ZELENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110909845",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW133","zelená ovl. hlavica presvet. stláčacia s presahom Ø22 s návratom pre integ. LED",0]
["ZB5AW13","OVL. HLAVICA STLÁČ. PRESVETL. ZELENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110909838",{"v":3.6,"d":"3.60"},{"v":4,"d":"4.00"},{"v":6.4,"d":"6.40"},{"v":16,"d":"16.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AW13","zelená ovl.hlavica presvet.stláčacia s prsahom Ø22 s návratom pre BA9s žiarovku",0]
["ZB5AW113","OVL. HLAVICA STLÁČ. PRESVETL. BIELA",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110909821",{"v":4.6,"d":"4.60"},{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AW113","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB5AW0M15","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110909197",{"v":5.4,"d":"5.40"},{"v":5.7,"d":"5.70"},{"v":3.4,"d":"3.40"},{"v":38,"d":"38.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AW0M15","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 1 NO + 1 NC",0.01]
["ZB5AW0M13","POLOZOSTAVA OBJÍMKY LED+ SP.JEDNOTKY",1,"ks",{"v":23.334412499999996,"d":"23.334"},"3389110909173",{"v":3.2,"d":"3.20"},{"v":5.2,"d":"5.20"},{"v":5.2,"d":"5.20"},{"v":40,"d":"40.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AW0M13","biela polozostava objímky s integ. LED 230...240V 2Z",0.01]
["ZB5AW0M11","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":19.216575,"d":"19.217"},"3389110909135",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AW0M11","biela polozostava objímky s integ. LED 230...240V 1Z",0]
["ZB5AW0G15","POLOZOSTAVA OBJÍMKY LED+ SP.JEDNOTKY",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3389110908794",{"v":5.5,"d":"5.50"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AW0G15","biela polozostava objímky s integ. LED 110...120V 1Z+1V",0.01]
["ZB5AW0G11","POLOZOSTAVA OBJÍMKY LED+ SP.JEDNOTKY",1,"ks",{"v":19.216575,"d":"19.217"},"3389110908732",{"v":5.6,"d":"5.60"},{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":31,"d":"31.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AW0G11","biela polozostava objímky s integ. LED 110...120V 1Z",0]
["ZB5AW0B15","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":18.301499999999997,"d":"18.302"},"3389110908398",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":38,"d":"38.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB5AW0B15","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 1 NO + 1 NC",0.01]
["ZB5AW0B13","POLOZOSTAVA OBJÍMKY LED+ SP.JEDNOTKY",1,"ks",{"v":18.301499999999997,"d":"18.302"},"3389110908374",{"v":5,"d":"5.00"},{"v":3.2,"d":"3.20"},{"v":4.6,"d":"4.60"},{"v":38,"d":"38.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB5AW0B13","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 2 NO",0.01]
["ZB5AW0B12","POLOZOSTAVA OBJÍMKY LED+ SP.JEDNOTKY",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110908350",{"v":5.4,"d":"5.40"},{"v":5.7,"d":"5.70"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB5AW0B12","biela polozostava objímky s integ. LED 24V 1V",0]
["ZB5AW0B11","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110908336",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB5AW0B11","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 1 NO",0]
["ZB5AW065","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389110909784",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":4.6,"d":"4.60"},{"v":37,"d":"37.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AW065","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – základňa BA 9s 1 NO + 1 NC",0]
["ZB5AW063","POLOZOSTAVA OBJÍMKY PRE ŽIAROVKU",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110909753",{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":38,"d":"38.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AW063","polozostava objímky s pre BA9s žiarovka <lt/>=250V 2Z",0]
["ZB5AW062","POLOZOSTAVA OBJÍMKY PRE ŽIAROVKU",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110909722",{"v":5.5,"d":"5.50"},{"v":3.7,"d":"3.70"},{"v":4.7,"d":"4.70"},{"v":28,"d":"28.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AW062","polozostava objímky s pre BA9s žiarovka <lt/>=250V 1V",0]
["ZB5AW061","POLOZOSTAVA OBJÍMKY PRE ŽIAROVKU",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110909692",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AW061","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – základňa BA 9s 1 NO",0]
["ZB5AW045","POLOZOSTAVA OBJÍMKY PRE ŽIAROVKU",1,"ks",{"v":40.2633,"d":"40.263"},"3389110909616",{"v":3.2,"d":"3.20"},{"v":8.2,"d":"8.20"},{"v":5.2,"d":"5.20"},{"v":118,"d":"118.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AW045","polozostava objímky s BA9s žiarovkou 220...240V 1Z+1V",0.02]
["ZB5AW035","POLOZOSTAVA OBJÍMKY S TR",1,"ks",{"v":40.2633,"d":"40.263"},"3389110909593",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":115,"d":"115.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AW035","polozostava objímky s BA9s žiarovkou 110...120V 1Z+1V",0.02]
["ZB5AVM1","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110907957",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":20,"d":"20.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AVM1","teleso pre kontrolku – ZB5 – biela zabud. LED – 230 - 240 V",0]
["ZB5AVJ1","POLOZOSTAVA OBJÍMKY S LED 12V BIELA",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110069853",{"v":5.3,"d":"5.30"},{"v":5.7,"d":"5.70"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AVJ1","biela polozostava objímky s integ. LED 12V",0]
["ZB5AVG6","Polozostava objímky s LED",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3389110907933",{"v":5.7,"d":"5.70"},{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":20,"d":"20.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AVG6","modrá polozostava objímky s integ. LED 110...120V",0]
["ZB5AVG14","POLOZOSTAVA S LED - NÁSUVNÝ KONEKTOR",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3389110907865",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AVG14","biela polozostava objímky s integ. LED 110...120V",0]
["ZB5AVG1","Polozostava objímky s LED",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110907858",{"v":5.2,"d":"5.20"},{"v":2.4,"d":"2.40"},{"v":4.8,"d":"4.80"},{"v":20,"d":"20.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AVG1","biela polozostava objímky s integ. LED 110...120V",0]
["ZB5AVBG1","POLOZOSTAVA OBJÍMKY 24-120AC/DC BIELA",1,"ks",{"v":20.13165,"d":"20.132"},"3389110070354",{"v":5.6,"d":"5.60"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":20.4,"d":"20.40"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AVBG1","teleso pre kontrolku – ZB5 – biela zabud. LED – 24 - 120 V",0]
["ZB5AVB1","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":10.065825,"d":"10.066"},"3389110907759",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":20,"d":"20.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AVB1","teleso pre kontrolku – ZB5 – biela zabud. LED – 24 V",0]
["ZB5AV8","Polozostava objímky pre žiarovku s TR",1,"ks",{"v":28.367324999999997,"d":"28.367"},"3389110908312",{"v":9.2,"d":"9.20"},{"v":3.6,"d":"3.60"},{"v":5.5,"d":"5.50"},{"v":95,"d":"95.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV8","polozostava objímky s BA9s žiarovkou 440...480V",0]
["ZB5AV6","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":5.581957499999999,"d":"5.582"},"3389110908282",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":19,"d":"19.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV6","teleso pre kontrolku – ZB5 – základňa BA 9s – 250 V",0]
["ZB5AV5D4","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110908251",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":102,"d":"102.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV5D4","čierna polozostava objímky s BA9s LED žiarovka 400V",0]
["ZB5AV5D3","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110908244",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":102,"d":"102.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV5D3","zelená polozostava objímky s BA9s LED žiarovka 400V",0]
["ZB5AV5D1","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110908237",{"v":8,"d":"8.00"},{"v":3.2,"d":"3.20"},{"v":5.2,"d":"5.20"},{"v":98,"d":"98.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV5D1","biela polozostava objímky s BA9s LED žiarovka 400V",0]
["ZB5AV5","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":27.909787499999997,"d":"27.910"},"3389110908220",{"v":3.4,"d":"3.40"},{"v":8.4,"d":"8.40"},{"v":5,"d":"5.00"},{"v":98,"d":"98.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV5","polozostava objímky s BA9s žiarovkou 400V",0]
["ZB5AV4","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":26.537175,"d":"26.537"},"3389110908213",{"v":9.3,"d":"9.30"},{"v":3.5,"d":"3.50"},{"v":5.7,"d":"5.70"},{"v":97,"d":"97.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV4","teleso pre kontrolku – ZB5 – číra žiarovka BA 9s – 230 V",0]
["ZB5AV3","Polozostava objímky pre žiarovku s TR",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110908152",{"v":9.1,"d":"9.10"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":97,"d":"97.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV3","polozostava objímky s BA9s žiarovkou 110...120V",0]
["ZB5AV18B1","Polozostava LED, 24V, biela",1,"ks",{"v":27.45225,"d":"27.452"},"3389110841329",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":23,"d":"23.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB5AV18B1","biela blikajúca - polozostava objímky s integ. LED 24V",0]
["ZB5AV083S","SIGNÁLKA PRE LED, ŽLTÁ, RÝHOVANÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3606481202307",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","85319000","https://www.se.com/sk/sk/product/ZB5AV083S","Head for pilot light, Harmony XB5, plastic, yellow, 22mm, universal LED, grooved lens",0]
["ZB5AV083","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":4.666882499999999,"d":"4.667"},"3606481202284",{"v":5.4,"d":"5.40"},{"v":3.7,"d":"3.70"},{"v":4.8,"d":"4.80"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV083","Head for pilot light, Harmony XB5, plastic, yellow, 22mm, universal LED, plain lens",0]
["ZB5AV07","SIGNÁLNA HLAVICA ČÍRA",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110137002",{"v":5.5,"d":"5.50"},{"v":3.4,"d":"3.40"},{"v":4.7,"d":"4.70"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV07","kryt kontrolky – Ø 22 – okrúhly – číra hladká šošovka",0]
["ZB5AV063","SIGNÁL. HLAVICA PRE LED MODRÁ",1,"ks",{"v":4.71263625,"d":"4.713"},"3389110908145",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV063","kryt kontrolky – Ø 22 – okrúhly – modrá hladká šošovka",0]
["ZB5AV06","SIGNÁLNA HLAVICA MODRÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110908138",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.7,"d":"4.70"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV06","kryt kontrolky – Ø 22 – okrúhly – modrá hladká šošovka",0]
["ZB5AV05S","SIGNÁLNA HLAVICA PRE BA9S ŽLTÁ",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110072198",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV05S","oranžová signálna hlavica Ø22 rýhovaná šošovka pre BA9s žiarovku",0]
["ZB5AV053S","SIGNÁLKA PRE LED, ORANŽOVÁ, RÝHOVANÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110291025",{"v":5,"d":"5.00"},{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV053S","oranžová signálna hlavica Ø22 ryhovaná šošovka pre integ. LED",0]
["ZB5AV053","SIGNÁL. HLAVICA PRE LED ŽLTÁ",1,"ks",{"v":4.71263625,"d":"4.713"},"3389110908121",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV053","kryt kontrolky – Ø 22 – okrúhly – žltá hladká šošovka",0]
["ZB5AV05","SIGNÁLNA HLAVICA ŽLTÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110908114",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV05","kryt kontrolky – Ø 22 – okrúhly – žltá hladká šošovka",0]
["ZB5AV04S","SIGNÁLNA HLAVICA PRE BA9S ČERVENÁ",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110072181",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV04S","červená signálna hlavica Ø22 rýhovaná šošovka pre BA9s žiarovku",0]
["ZB5AV043","SIGNÁL. HLAVICA PRE LED ČERVENÁ",1,"ks",{"v":4.71263625,"d":"4.713"},"3389110908107",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":15,"d":"15.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV043","kryt kontrolky – Ø 22 – okrúhly – červená hladká šošovka",0]
["ZB5AV04","SIGNÁLNA HLAVICA ČERVENÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110908091",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV04","kryt kontrolky – Ø 22 – okrúhly – červená hladká šošovka",0]
["ZB5AV03S","SIGNÁLNA HLAVICA NEÓNOVÁ RÝHOVANÁ ZELENÁ",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110072174",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV03S","zelená hlava sig. Ø22 drážkovaná šošovka pre žiarovku BA9s",0]
["ZB5AV033","SIGNÁL. HLAVICA PRE LED ZELENÁ",1,"ks",{"v":4.71263625,"d":"4.713"},"3389110908084",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":15,"d":"15.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV033","kryt kontrolky – Ø 22 – okrúhly – zelená hladká šošovka",0]
["ZB5AV03","SIGNÁLNA HLAVICA ZELENÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110908077",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":15,"d":"15.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV03","kryt kontrolky – Ø 22 – okrúhly – zelená hladká šošovka",0]
["ZB5AV013","SIGNÁL. HLAVICA PRE LED BIELA",1,"ks",{"v":4.71263625,"d":"4.713"},"3389110908060",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":15,"d":"15.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV013","kryt kontrolky – Ø 22 – okrúhly – biela hladká šošovka",0]
["ZB5AV01","SIGNÁLNA HLAVICA BIELA",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110908053",{"v":5.3,"d":"5.30"},{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":15,"d":"15.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV01","kryt kontrolky – Ø 22 – okrúhly – biela hladká šošovka",0]
["ZB5AV003S","SIGNÁLNA HLAVICA +5 FAREB. ČOČIEK",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110137040",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":25.5,"d":"25.50"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV003S","signálna hlavica Ø22 s 5 - farebná rýhovaná šošovka s pre integ. LED",0]
["ZB5AV003","SIGNÁLNA HLAVICA +5 FAREB. ČOČIEK",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110137026",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":24.4,"d":"24.40"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB5AV003","kryt kontrolky – Ø 22 – okrúhly – hladká šošovka s výberom 5 farieb",0]
["ZB5AT8643M","OV. HLAVICA S HRÍBOM ČERVENÁ S MECH. IND",1,"ks",{"v":29.282399999999996,"d":"29.282"},"3389119003766",{"v":8.2,"d":"8.20"},{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":34,"d":"34.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AT8643M","červená Ø40 presvet.hlavica stískacia núdzové zastav. Ø22 vypnuté a s aretáciou",0]
["ZB5AT84TQ","EMERGENCY STOP OP. HEAD",100,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110885125",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":34,"d":"34.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AT84TQ","hlava tlačítka núdzového zastavenia ZB5AT84, predaj po 100",0]
["ZB5AT844","Ovlád.hlavica núdz.vypnutia, stlač-ťahaj",1,"ks",{"v":19.216575,"d":"19.217"},"3389119048057",{"v":9.3,"d":"9.30"},{"v":4.7,"d":"4.70"},{"v":5.4,"d":"5.40"},{"v":48,"d":"48.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AT844","30MM ČERV. OVL. HLAVICA 22MM NÚDZOVÉHO VYPNUTIA, STLAČ-ŤAHAJ",0]
["ZB5AT84","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389110907742",{"v":8.8,"d":"8.80"},{"v":4.5,"d":"4.50"},{"v":5.4,"d":"5.40"},{"v":50,"d":"50.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AT84","okrúhla hríb. hlavica pre núdzové vypnutie Ø 40 – ťažná/tlačná – Ø 22 – červená",0]
["ZB5AT24","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":21.5042625,"d":"21.504"},"3389110906981",{"v":8.4,"d":"8.40"},{"v":4.2,"d":"4.20"},{"v":5.4,"d":"5.40"},{"v":46,"d":"46.00"},"CZ","85389099","https://www.se.com/sk/sk/product/ZB5AT24","čierna Ø30 hlavica s hríbovým tlačítkom Ø22 s aretáciou \"stiskni - tiahni\"",0]
["ZB5AT2","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110906974",{"v":8.8,"d":"8.80"},{"v":4.5,"d":"4.50"},{"v":5.3,"d":"5.30"},{"v":49,"d":"49.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AT2","čierna Ø40 hlavica s hríbovým tlačítkom Ø22 s aretáciou \"stiskni - tiahni\"",0]
["ZB5AS964","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":32.485162499999994,"d":"32.485"},"3389110135183",{"v":9.398,"d":"9.40"},{"v":7.366,"d":"7.37"},{"v":7.366,"d":"7.37"},{"v":81.647,"d":"81.65"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS964","červená Ø60 ovl.hlav.stískacia nudz.zastav.Ø22 vypnuté a s aret.\"uvolniť kľúčom\"",0]
["ZB5AS944D","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110135169",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":71,"d":"71.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS944D","červená Ø40 ovl.hlav.stískacia nudz.zastav.Ø22 vypnuté a s aret.\"uvolniť kľúčom\"",0]
["ZB5AS94412","OVLÁDAČ NÚDZOVÉHO ZASTAVENIA",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3389110135091",{"v":8.8,"d":"8.80"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":70,"d":"70.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS94412","červené Ø40 ovl.hlav.stlač.núdzov.zastav.Ø22 vypnuté a s aret.\"uvoľniť kľúčom\"",0]
["ZB5AS94410","OVLÁDAČ NÚDZOVÉHO ZASTAVENIA",1,"ks",{"v":34.77285,"d":"34.773"},"3389110135107",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":71,"d":"71.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS94410","červené Ø40 ovl.hlav.stlač.núdzov.zastav.Ø22 vypnuté a s aret.\"uvoľniť kľúčom\"",0]
["ZB5AS944","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":23.334412499999996,"d":"23.334"},"3389110906967",{"v":4.3,"d":"4.30"},{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":68,"d":"68.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS944","okrúhla hríb. hlav. pre núdz. vyp. Ø 40 – uvoľň. kl. – Ø 22 – červ. – Ronis 455",0]
["ZB5AS934","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":27.909787499999997,"d":"27.910"},"3389110906943",{"v":8.8,"d":"8.80"},{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":66,"d":"66.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS934","červená Ø30 ovl.hlav.stískacia nudz.zastav.Ø22 vypnuté a s aret.\"uvolniť kľúčom\"",0]
["ZB5AS864","NÚDZOVÉ ZASTAVENIE 60MM, TRIGGER",1,"ks",{"v":19.216575,"d":"19.217"},"3389118187801",{"v":7,"d":"7.00"},{"v":8.8,"d":"8.80"},{"v":7,"d":"7.00"},{"v":55,"d":"55.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS864","červená Ø60 ovl.hlav.stláč.núdz.zastav.Ø22 vypnuté a s aret.\"uvolniť kľúčom\"",0]
["ZB5AS84W3B","OVL. HLAVICA NÚDZ. ZASTAV. UVOL. POOTOC.",1,"ks",{"v":34.3153125,"d":"34.315"},"3606489744977",{"v":7.5,"d":"7.50"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":63,"d":"63.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS84W3B","Harmony XB5, Antimikrobiálna hlavica podsvieteného ovládača núdzového zastavenia, plast, červená, Ø22, uvoľnenie pootočením, biela/červená LED, 24 V AC/DC",0]
["ZB5AS84W2M","OVL. HLAVICA NÚDZ. ZASTAV. UVOĽ. POOTOČ.",1,"ks",{"v":27.45225,"d":"27.452"},"3606489744960",{"v":7,"d":"7.00"},{"v":8.6,"d":"8.60"},{"v":7,"d":"7.00"},{"v":65,"d":"65.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS84W2M","Harmony XB5, Antimikrobiálna hlavica podsvieteného ovládača núdzového zastavenia, plast, červená, Ø22, uvoľnenie pootočením, červená LED, 230...240 V AC",0]
["ZB5AS84W2B","OVL. HLAVICA NÚDZ. ZASTAV. UVOĽ. POOTOČ.",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3606489744946",{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":7,"d":"7.00"},{"v":63,"d":"63.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS84W2B","Harmony XB5, Antimikrobiálna hlavica podsvieteného ovládača núdzového zastavenia, plast, červená, Ø22, uvoľnenie pootočením, červená LED, 24 V AC/DC",0]
["ZB5AS84W00","OVL. HLAVICA NÚDZ. ZASTAV. UVOĽ. POOTOČ.",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3606489744939",{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":7,"d":"7.00"},{"v":79,"d":"79.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS84W00","Harmony XB5, Antimikrobiálna hlavica ovládača núdzového zastavenia , plast, červená, Ø22, uvoľnenie pootočením, červená",0]
["ZB5AS844TQ","OVLÁDACIA HLAVICA NOUZOVÉHO VYPNUTÍ  (10",100,"ks",{"v":15.01638075,"d":"15.016"},"3389110885095",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":30,"d":"30.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS844TQ","hlava tlačítka núdzového zastavenia ZB5AS844, predaj po 100",""]
["ZB5AS844","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110906929",{"v":8.8,"d":"8.80"},{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":42,"d":"42.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS844","okrúhla hríb. hlavica pre núdzové vypnutie Ø 40 – uvoľ. otoč. – Ø 22 – červená",0]
["ZB5AS834","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110906912",{"v":8.9,"d":"8.90"},{"v":4.6,"d":"4.60"},{"v":5.5,"d":"5.50"},{"v":39,"d":"39.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS834","okrúhla hríb. hlavica pre núdzové vypnutie Ø 30 – uvoľ. otoč. – Ø 22 – červená",0]
["ZB5AS72","OVL. HLAVICA S HRÍBOM ČIERNA-30MM",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3389110906899",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS72","čierna Ø30 hlavica s hríbovým tlačítkom Ø22 s aretáciou \"uvoľniť kľúčom\"",0]
["ZB5AS62","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110906875",{"v":7.2,"d":"7.20"},{"v":9,"d":"9.00"},{"v":7.2,"d":"7.20"},{"v":64,"d":"64.00"},"CZ","85389099","https://www.se.com/sk/sk/product/ZB5AS62","čierna Ø60 hlavica s hríbovým tlačítkom Ø22 s aretáciou \"uvolniť otočením\"",0]
["ZB5AS55","OVL. HLAVICA S HRÍBOM ŽLTÁ",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110906868",{"v":8.8,"d":"8.80"},{"v":4.5,"d":"4.50"},{"v":5.3,"d":"5.30"},{"v":42,"d":"42.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS55","žltá Ø40 hlavica s hríbovým tlačítkom Ø22 s aretáciou \"uvolniť otočením\"",0]
["ZB5AS52","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110906844",{"v":8.8,"d":"8.80"},{"v":4.5,"d":"4.50"},{"v":5.3,"d":"5.30"},{"v":42,"d":"42.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS52","okrúhla hlavica pre tlačidlo Ø 22 – uzamykateľná – čierna – s hríbom Ø 40 mm",0]
["ZB5AS42","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110906820",{"v":8.7,"d":"8.70"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":39,"d":"39.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AS42","okrúhla hlavica pre tlačidlo Ø 22 – uzamykateľná – čierna – s hríbom Ø 30 mm",0]
["ZB5AS12","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":27.45225,"d":"27.452"},"3389110906790",{"v":8.8,"d":"8.80"},{"v":4.5,"d":"4.50"},{"v":5.3,"d":"5.30"},{"v":69,"d":"69.00"},"CZ","85389099","https://www.se.com/sk/sk/product/ZB5AS12","čierna Ø40 hlavica s hríbovým tlačítkom Ø22 s aretáciou \"uvoľniť kľúčom\"",0]
["ZB5AR5","OVL. HLAVICA S HRÍBOM ŽLTÁ",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110906769",{"v":9.398,"d":"9.40"},{"v":7.366,"d":"7.37"},{"v":7.366,"d":"7.37"},{"v":58.968,"d":"58.97"},"CZ","85389099","https://www.se.com/sk/sk/product/ZB5AR5","žltá Ø60 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB5AR416","MUSHROOMM PUSH BUT HEAD",1,"ks",{"v":17.386425,"d":"17.386"},"3389110066364",{"v":8.8,"d":"8.80"},{"v":7.2,"d":"7.20"},{"v":7.2,"d":"7.20"},{"v":48,"d":"48.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AR416","červená Ø60 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB5AR4","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":16.9288875,"d":"16.929"},"3389110906752",{"v":9.2,"d":"9.20"},{"v":7.2,"d":"7.20"},{"v":7.4,"d":"7.40"},{"v":59,"d":"59.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AR4","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – červená – s hríbom Ø 60 mm",0]
["ZB5AR3","OVL. HLAVICA S HRÍBOM ZELENÁ",1,"ks",{"v":16.9288875,"d":"16.929"},"3389110906745",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":60,"d":"60.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AR3","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zelená – s hríbom Ø 60 mm",0]
["ZB5AR216","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":26.537175,"d":"26.537"},"3389110066227",{"v":7.6,"d":"7.60"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":49,"d":"49.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AR216","čierna Ø60 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB5AR2","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":16.9288875,"d":"16.929"},"3389110906738",{"v":7.2,"d":"7.20"},{"v":9.2,"d":"9.20"},{"v":7.6,"d":"7.60"},{"v":60,"d":"60.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AR2","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – čierna – s hríbom Ø 60 mm",0]
["ZB5APA1","Ovládacie hlavice, biela",1,"ks",{"v":10.834487999999999,"d":"10.834"},"3389110966374",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":20,"d":"20.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5APA1","biela zapuš. hlava tlačítka Ø22 s návratom neoznačený",""]
["ZB5AP6S","OVL. HLAVICA S KRYT. MODRÁ",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110999419",{"v":4.5,"d":"4.50"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP6S","modrá zapus. hlavica tlačidla Ø22 s návratom neoznačená",0]
["ZB5AP6","OVL. HLAVICA S KRYTKOU MODRÁ",1,"ks",{"v":7.82389125,"d":"7.824"},"3389110906714",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP6","modrá ovl. hlavica stískacia s presahom Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AP5","OVL. HLAVICA S KRYTKOU ŽLTÁ",1,"ks",{"v":7.82389125,"d":"7.824"},"3389110906691",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP5","žltá zapustená hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB5AP4S","OVL. HLAVICA S KRYT. ČERVENÁ ",1,"ks",{"v":8.784719999999998,"d":"8.785"},"3389110999396",{"v":5.6,"d":"5.60"},{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP4S","červená zapuš. hlava tlačítka Ø22 s návratom neoznačený",""]
["ZB5AP4","OVL. HLAVICA S KRYTKOU ČERVENÁ",1,"ks",{"v":7.82389125,"d":"7.824"},"3389110906677",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP4","okrúhla hlav. pre tlač. Ø 22 – vr. pružina – červ. – vystupujúca – bez označ.",0]
["ZB5AP3S","OVL. HLAVICA S KRYT. ZELENÁ",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110999389",{"v":5.6,"d":"5.60"},{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP3S","zelená zapuš. hlava tlačítka Ø22 s návratom neoznačený",0]
["ZB5AP38","OVL. HLAVICA S KRYT. PRE ŠTÍTOK ZELENÁ",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389110906660",{"v":8.8,"d":"8.80"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP38","zelená zapustená hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB5AP3","OVL. HLAVICA S KRYTKOU ZELENÁ",1,"ks",{"v":7.82389125,"d":"7.824"},"3389110906653",{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":20.5,"d":"20.50"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP3","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zelená – vystupujúca – bez označ.",0]
["ZB5AP2S","OVL. HLAVICA S KRYTKOU ČIERNA",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110999372",{"v":5.7,"d":"5.70"},{"v":4.7,"d":"4.70"},{"v":3.6,"d":"3.60"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP2S","čierna zapustená hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB5AP2","OVL. HLAVICA S KRYTKOU ČIERNA",1,"ks",{"v":7.82389125,"d":"7.824"},"3389110906646",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP2","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – čierna – vystupujúca – bez označ.",0]
["ZB5AP18","OVL. HLAVICA S KRYT. PRE ŠTÍTOK BIELA",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389110906639",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP18","biela lícujúca ovl. hlavica stískacia Ø22 s návratom neoznačená",0]
["ZB5AP1","OVL. HLAVICA S KRYTKOU BIELA",1,"ks",{"v":7.82389125,"d":"7.824"},"3389110906622",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AP1","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – biela – vystupujúca – bez označ.",0]
["ZB5AL7341","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA IP66",1,"ks",{"v":12.81105,"d":"12.811"},"3389119043311",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL7341","zelená lícujúca/červená lícujúca ovl. hlavica dvojtlač. Ø22 s popisom",0]
["ZB5AL7340","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA IP66",1,"ks",{"v":10.5233625,"d":"10.523"},"3389119043304",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL7340","zelená lícujúca/červená lícujúca ovl. hlavica dvojtlač. Ø22 neoznačená",0]
["ZB5AL5","OVL. HLAVICA STLÁČACIA ŽLTÁ",1,"ks",{"v":5.993741249999999,"d":"5.994"},"3389110906516",{"v":4.6,"d":"4.60"},{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL5","žltá ovl. hlavice stláčacia s presahom. Ø22 s návratom neoznačená",0]
["ZB5AL434","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":7.2290925,"d":"7.229"},"3389110906486",{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":4.8,"d":"4.80"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL434","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – červená – vystupujúca – STOP",0]
["ZB5AL432","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":7.36635375,"d":"7.366"},"3389110906462",{"v":5.4,"d":"5.40"},{"v":4.3,"d":"4.30"},{"v":3.5,"d":"3.50"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL432","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – červená – vystupujúca – O",0]
["ZB5AL4","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":5.993741249999999,"d":"5.994"},"3389110906455",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL4","okrúhla hlav. pre tlač. Ø 22 – vr. pružina – červ. – vystupujúca – bez označ.",0]
["ZB5AL3","OVL. HLAVICA STLÁČACIA ZELENÁ",1,"ks",{"v":5.993741249999999,"d":"5.994"},"3389110906431",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL3","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zelená – vystupujúca – bez označ.",0]
["ZB5AL232","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":7.36635375,"d":"7.366"},"3389110906394",{"v":5.3,"d":"5.30"},{"v":0.5,"d":"0.50"},{"v":4.3,"d":"4.30"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL232","čierna ovl. hlavica stláčacia s presahom. Ø22 s návratom \"O\"",0]
["ZB5AL2","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":5.993741249999999,"d":"5.994"},"3389110906387",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17.8,"d":"17.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AL2","čierna ovl. hlavica stláčacia s presahom. Ø22 s návratom neoznačená",0]
["ZB5AK1883C0","ŽL Ovládacia hlavica otocná presvetlená",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606489767884",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1883C0","Head for illuminated selector switch, Harmony XB5, grey bezel, yellow handle, 22mm, universal LED, 3 positions, right to center spring return",0]
["ZB5AK1843C0","ČE Ovládacia hlavica otočná presvetlená,",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606489767822",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1843C0","Head for illuminated selector switch, Harmony XB5, grey bezel, red handle, 22mm, universal LED, 3 positions, right to center",0]
["ZB5AK1843","OVL. HLAVICA OTOČ. PRESVETL. ČERVENÁ",1,"ks",{"v":19.674112499999996,"d":"19.674"},"3389110906325",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1843","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – červená",0]
["ZB5AK1833","OVL. HLAVICA OTOČ. PRESVETL. ZELENÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110906318",{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":5.2,"d":"5.20"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1833","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB5AK1813","OVL. HLAVICA OTOČ. PRESVETL. BIELA",1,"ks",{"v":20.13165,"d":"20.132"},"3389110138061",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1813","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB5AK1763C0","MO Ovládacia hlavica otočná presvetlená",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606489767747",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1763C0","Head for illuminated selector switch, Harmony XB5, grey bezel, blue handle, 22mm, universal LED, 3 positions, left to center",0]
["ZB5AK1743C0","ČE Ovládacia hlavica otočná presvetlená",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606489767709",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1743C0","Head for illuminated selector switch, Harmony XB5, grey bezel, red handle, 22mm, universal LED, 3 positions, left to center",0]
["ZB5AK1733","OVL. HLAVICA OTOČ. PRESVETL. ZELENÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110906264",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1733","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB5AK1713","OVL. HLAVICA OTOČ. PRESVETL. BIELA",1,"ks",{"v":20.13165,"d":"20.132"},"3389110138122",{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":2.1,"d":"2.10"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1713","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB5AK1583C0","ŽL Ovládacia hlavica otočná presvetlená,",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3606489767648",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1583C0","Head for illuminated selector switch, Harmony XB5, grey bezel, yellow handle, 22mm, universal LED, 3 positions, to center spring return",0]
["ZB5AK1563","OVL. HLAVICA OTOČ. PRESVETL. MODRÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110906240",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1563","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – modrá",0]
["ZB5AK1553","OVL. HLAVICA OTOČ. PRESVETL. ŽLTÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110906233",{"v":3.3,"d":"3.30"},{"v":4.5,"d":"4.50"},{"v":5.2,"d":"5.20"},{"v":23.4,"d":"23.40"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1553","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – žltá",0]
["ZB5AK1543","OVL. HLAVICA OTOČ. PRESVETL. ČERVENÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110906226",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1543","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – červená",0]
["ZB5AK1533","OVL. HLAVICA OTOČ. PRESVETL. ZELENÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110906219",{"v":6,"d":"6.00"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1533","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB5AK1513C0","BI Ovládacia hlavica otočná presvetlená",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606489767549",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1513C0","Head for illuminated selector switch, Harmony XB5, grey bezel, white handle, 22mm, universal LED, 3 positions, to center",0]
["ZB5AK1513","OVL. HLAVICA OTOČ. PRESVETL. BIELA",1,"ks",{"v":20.13165,"d":"20.132"},"3389110138047",{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1513","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB5AK1483","Hlavica podsvieteného otočného ovládača",1,"ks",{"v":23.334412499999996,"d":"23.334"},"3606481206251",{"v":5.2,"d":"5.20"},{"v":4.8,"d":"4.80"},{"v":3.3,"d":"3.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1483","Hlavica podsvieteného otočného ovládača, Harmony XB5, plast, žltá, 22mm, universal LED, 2 polohy",0]
["ZB5AK1463C0","MO Ovládacia hlavica otočná presvetlená,",1,"ks",{"v":35.687925,"d":"35.688"},"3606489767501",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1463C0","Head for illuminated selector switch, Harmony XB5, grey bezel, blue handle, 22mm, universal LED, 3 positions,",0]
["ZB5AK1453","OVL. HLAVICA OTOČ. PRESVETL. ŽLTÁ",1,"ks",{"v":35.687925,"d":"35.688"},"3389110906189",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1453","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – žltá",0]
["ZB5AK1433","OVL. HLAVICA OTOČ. PRESVETL. ZELENÁ",1,"ks",{"v":35.687925,"d":"35.688"},"3389110906165",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1433","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – zelená",0]
["ZB5AK1413","OVL. HLAVICA OTOČ. PRESVETL. BIELA",1,"ks",{"v":35.687925,"d":"35.688"},"3389110137927",{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1413","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – biela",0]
["ZB5AK1383","OVL. HLAVICA OTOČ. PRESVETL. ŽLTÁ",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3606481206268",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":5.2,"d":"5.20"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1383","Head for illuminated selector switch, Harmony XB5, dark grey plastic, yellow handle, 22mm, universal LED, 3 positions",0]
["ZB5AK1363","OVL. HLAVICA OTOČ. PRESVETL. MODRÁ",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110906141",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1363","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – modrá",0]
["ZB5AK1353","OVL. HLAVICA OTOČ. PRESVETL. ŽLTÁ",1,"ks",{"v":17.386425,"d":"17.386"},"3389110906134",{"v":5.2,"d":"5.20"},{"v":3.2,"d":"3.20"},{"v":5,"d":"5.00"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1353","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – žltá",0]
["ZB5AK1343","OVL. HLAVICA OTOČ. PRESVETL. ČERVENÁ",1,"ks",{"v":18.301499999999997,"d":"18.302"},"3389110906127",{"v":5.2,"d":"5.20"},{"v":3.2,"d":"3.20"},{"v":4.8,"d":"4.80"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1343","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – červená",0]
["ZB5AK1333C0","Ovládacia hlavica otočná presvetlená, 3 ",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606489767327",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1333C0","Head for illuminated selector switch, Harmony XB5, grey bezel, green handle, 22mm, universal LED, 3 positions",0]
["ZB5AK1333","OVL. HLAVICA OTOČ. PRESVETL. ZELENÁ",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110906110",{"v":5.9,"d":"5.90"},{"v":3.5,"d":"3.50"},{"v":5.6,"d":"5.60"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1333","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB5AK1313","OVL. HLAVICA OTOČ. PRESVETL. BIELA",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110137989",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":4.8,"d":"4.80"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1313","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB5AK1283","OVL. HLAVICA OTOČ. PRESVETL. ŽLTÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3606481206244",{"v":5.8,"d":"5.80"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1283","ovládacia hlavica otočná presvetlená Ø22 2-polohová",0]
["ZB5AK1263","OVL. HLAVICA OTOČ. PRESVETL. MODRÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110906097",{"v":5.9,"d":"5.90"},{"v":3.5,"d":"3.50"},{"v":5.3,"d":"5.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1263","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – modrá",0]
["ZB5AK1253","OVL. HLAVICA OTOČ. PRESVETL. ŽLTÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110906080",{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1253","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – žltá",0]
["ZB5AK1243","OVL. HLAVICA OTOČ. PRESVETL. ČERVENÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110906073",{"v":3.3,"d":"3.30"},{"v":5.5,"d":"5.50"},{"v":5.2,"d":"5.20"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1243","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – červená",0]
["ZB5AK1233","OVL. HLAVICA OTOČ. PRESVETL. ZELENÁ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110906066",{"v":3.3,"d":"3.30"},{"v":5.7,"d":"5.70"},{"v":5.2,"d":"5.20"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1233","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – zelená",0]
["ZB5AK1213","OVL. HLAVICA OTOČ. PRESVETL. BIELA",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110137903",{"v":6,"d":"6.00"},{"v":3.4,"d":"3.40"},{"v":5.6,"d":"5.60"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AK1213","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – biela",0]
["ZB5AJ8","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110906059",5.08,4.83,3.56,{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AJ8","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AJ7","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110906042",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AJ7","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AJ5","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110906035",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.2,"d":"5.20"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AJ5","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AJ4C0","ČI Ovládacia hlavica otočná Dlhá rukoväť",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3606489767105",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AJ4C0","Harmony XB5, Selector switch head, plastic, black, Ø22, long handle, 2 positions, spring return from right to left, grey bezel",0]
["ZB5AJ3","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110906011",{"v":5.2,"d":"5.20"},{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AJ3","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AJ2","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110906004",{"v":5.4,"d":"5.40"},{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AJ2","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB5AH53","OVL. HLAVICA STISKNI-STISKNI ŽLTÁ",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110905960",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH53","hlavica osvetleného tlačidla – Ø 22 – žltá",0]
["ZB5AH5","OVL. HLAVICA STISKNI-STISKNI ŽLTÁ",1,"ks",{"v":20.589187499999998,"d":"20.589"},"3389110905953",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH5","žltá ovládateľná hlavica stískacia s presahom Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AH43","OVL. HLAVICA \"STISKNI-STISKNI\" ČERVENÁ",1,"ks",{"v":21.961799999999997,"d":"21.962"},"3389110905946",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH43","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB5AH4","OVL. HLAVICA STISKNI-STISKNI ČERVENÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110905939",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH4","červená ovládateľná hlav. stískacia s presahom Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AH33","OVL. HLAVICA STISKNI-STISKNI ZELENÁ",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3389110905922",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AH33","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB5AH2","OVL. HLAVICA STISKNI-STISKNI ČIERNA",1,"ks",{"v":12.81105,"d":"12.811"},"3389110905908",{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH2","čierna ovládateľná hlavica stískacia s presahom Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AH063C0","Ovládacia hlavica „Stlačením zapni-stlač",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3606489766764",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH063C0","Head for illuminated push button, Harmony XB5, grey bezel, blue flush, 22mm, universal LED, push-push, unmarked",0]
["ZB5AH063","OVL. HLAVICA STISKNI-STISKNI MODRÁ",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110137859",{"v":4.2,"d":"4.20"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH063","hlavica osvetleného tlačidla – Ø 22 – modrá",0]
["ZB5AH06","OVL. HLAVICA STISKNI-STISKNI MODRÁ",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110134902",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH06","modrá zapustená hlava tlačítka Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AH053","OVL. HLAVICA STISKNI-STISKNI ŽLTÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110137774",{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":5,"d":"5.00"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH053","hlavica osvetleného tlačidla – Ø 22 – žltá",0]
["ZB5AH05","OVL. HLAVICA STISKNI-STISKNI ŽLTÁ",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110134889",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH05","žltá zapustená hlava tlačítka Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AH043","OVL. HLAVICA STISKNI-STISKNI ČERVENÁ",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110137750",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH043","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB5AH04","OVL. HLAVICA STISKNI-STISKNI ČERVENÁ",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110134872",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH04","červená zapustená hlava tlačítka Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AH033","OVL. HLAVICA STISKNI-STISKNI ZELENÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110137705",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH033","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB5AH03","OVL. HLAVICA STISKNI-STISKNI ZELENÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110134865",{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH03","zelená zapustená hlava tlačítka Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AH02","OVL. HLAVICA STISKNI-STISKNI ČIERNA",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110134841",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":18.5,"d":"18.50"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH02","okrúhla hlavica pre tlačidlo Ø 22 – stač-stlač – čierna – zapustená",0]
["ZB5AH0183","Hlavica pre pods. tlačidlo, stlač-stlač",1,"ks",{"v":30.197474999999997,"d":"30.197"},"3389110067965",{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":1.7,"d":"1.70"},{"v":54,"d":"54.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AH0183","Hlavica pre podsvietené tlačidlo, Harmony XB5, okrúhla biela, 22mm, integral LED, stlačením zapni - stlačením vypni, bez symbolu",0]
["ZB5AH013","OVL. HLAVICA STISKNI-STISKNI BIELA",1,"ks",{"v":13.726125,"d":"13.726"},"3389110137682",{"v":5.4,"d":"5.40"},{"v":4.7,"d":"4.70"},{"v":3.5,"d":"3.50"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH013","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB5AH01","OVL. HLAVICA STISKNI-STISKNI BIELA",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110134834",{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AH01","biela lícujúca ovládateľná hlavica stískacia Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB5AG9","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110905878",{"v":5.2,"d":"5.20"},{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":67,"d":"67.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG9","ovládateľná otočná hlavica Ø22 3-polohy pevné Ronis 455",0]
["ZB5AG8","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110905861",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":5,"d":"5.00"},{"v":68,"d":"68.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG8","ovládateľná otočná hlavica Ø22 3-polohy s návratom Ronis 455",0]
["ZB5AG7D","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3389110136746",{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":5.3,"d":"5.30"},{"v":67,"d":"67.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG7D","ovládateľná otočná hlavica Ø22 3-polohy s návratom Dom 8D1",0]
["ZB5AG7","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3389110905854",{"v":9.2,"d":"9.20"},{"v":3.7,"d":"3.70"},{"v":5.7,"d":"5.70"},{"v":67,"d":"67.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG7","hlav. pre uzamyk. voliaci sp. Ø 22 – 3 pol. vrat. pružiny – Ronis 455 – v strede",0]
["ZB5AG6D","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":30.197474999999997,"d":"30.197"},"3389110136524",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG6D","hlav. pre uzamyk. voliaci sp. Ø 22 – 2 polohy vrat. pružiny – Dom 8D1 – vľavo",0]
["ZB5AG614","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3389110135329",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG614","ovládateľná otočná hlavica Ø22 2-polohy s návratom Ronis 520E",0]
["ZB5AG612","OVL. HLAVICA OTOČ. S KLÚČOM - 2 POLOHY",1,"ks",{"v":37.9756125,"d":"37.976"},"3389110135220",{"v":8.2,"d":"8.20"},{"v":3.2,"d":"3.20"},{"v":5.4,"d":"5.40"},{"v":68,"d":"68.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5AG612","ovládateľná otočná hlavica Ø22 2-polohy s návratom Ronis 421E",0]
["ZB5AG610","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3389110135268",8.89,5.33,3.56,{"v":70,"d":"70.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG610","hlav. pre uzamyk. voliaci sp. Ø 22 – 2 polohy vrat. pružiny – Ronis 458A – vľavo",0]
["ZB5AG6","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":27.45225,"d":"27.452"},"3389110905847",{"v":9.1,"d":"9.10"},{"v":3.7,"d":"3.70"},{"v":5.5,"d":"5.50"},{"v":69,"d":"69.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG6","hlav. pre uzamyk. voliaci sp. Ø 22 – 2 polohy vrat. pružiny – Ronis 455 – vľavo",0]
["ZB5AG5","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110905830",{"v":8.6,"d":"8.60"},{"v":3.3,"d":"3.30"},{"v":5.2,"d":"5.20"},{"v":57,"d":"57.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG5","hlav. pre uzamyk. voliaci sp. Ø22 – 3 polohy usad. – Ronis 455 – vľavo + vpravo",0]
["ZB5AG4D","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":27.45225,"d":"27.452"},"3389110136500",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":66,"d":"66.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG4D","hlav. pre uzamyk. voliaci sp. Ø 22 – 2 polohy usad. – Dom 8D1, akákoľvek pol.",0]
["ZB5AG420","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":45.296212499999996,"d":"45.296"},"3389110135367",8.64,5.33,4.32,{"v":130,"d":"130.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG420","hlavica pre uzamykateľný voliaci spínač Ø 22 – 2 polohy usadenia – Ronis 3131A",0]
["ZB5AG412","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":44.3811375,"d":"44.381"},"3389110135213",{"v":9,"d":"9.00"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":66,"d":"66.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG412","hlav. pre uzamyk. voliaci sp. Ø22 – 2 polohy usad. – Ronis 421E – akákoľvek pol.",0]
["ZB5AG410","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":44.3811375,"d":"44.381"},"3389110135251",8.64,5.33,3.56,{"v":70,"d":"70.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG410","hlav. pre uzamyk. voliaci sp. Ø22 – 2 polohy usad. – Ronis 458A – akákoľvek pol.",0]
["ZB5AG4","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":27.45225,"d":"27.452"},"3389110905823",{"v":3.3,"d":"3.30"},{"v":9,"d":"9.00"},{"v":5.2,"d":"5.20"},{"v":66,"d":"66.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG4","hlav. pre uzamyk. voliaci sp. Ø22 – 2 polohy usad. – Ronis 455 – akákoľvek pol.",0]
["ZB5AG3D","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3389110136548",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":67.4,"d":"67.40"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5AG3D","hlavica pre uzamykateľ. voliaci sp. Ø 22 – 3 polohy usad. – Dom 8D1 – v strede",0]
["ZB5AG3","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110905816",{"v":9,"d":"9.00"},{"v":3.6,"d":"3.60"},{"v":5.5,"d":"5.50"},{"v":68,"d":"68.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG3","hlavica pre uzamykateľ. voliaci sp. Ø 22 – 3 polohy usad. – Ronis 455 – v strede",0]
["ZB5AG2D","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":27.45225,"d":"27.452"},"3389110136463",{"v":9.1,"d":"9.10"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":66,"d":"66.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG2D","hlavica pre uzamykateľný voliaci sp. Ø 22 – 2 polohy usadenia – Dom 8D1 – vľavo",0]
["ZB5AG2C0","Ovládacia hlavica otočná so zámkom Kľúč",1,"ks",{"v":26.537175,"d":"26.537"},"3606489765286",{"v":5.2,"d":"5.20"},{"v":8.6,"d":"8.60"},{"v":3.3,"d":"3.30"},{"v":67,"d":"67.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5AG2C0","Harmony XB5, Key switch selector head, plastic, black, Ø22, key 455, 2 positions, stay put, grey bezel",0]
["ZB5AG2C","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":51.2442,"d":"51.244"},"3389110851007",{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":51,"d":"51.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AG2C","Harmony XB5C, Key switch selector head, plastic, black, Ø22, key n°455, 2 positions, stay put",0]
["ZB5AG220","OVLÁDACIA HLAVICA S KĽÚČOM",1,"ks",{"v":44.3811375,"d":"44.381"},"3389110135343",8.89,3.56,5.33,{"v":70,"d":"70.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG220","ovl. hlavica otočná Ø22 2-poloha pevná Ronis 3131A",0]
["ZB5AG214","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":42.09345,"d":"42.093"},"3389110135282",{"v":5.2,"d":"5.20"},{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":67,"d":"67.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG214","hlavica pre uzamykateľ. voliaci sp. Ø 22 – 2 polohy usad. – Ronis 520E – vľavo",0]
["ZB5AG212","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":44.3811375,"d":"44.381"},"3389110135206",{"v":9.1,"d":"9.10"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":67,"d":"67.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG212","hlavica pre uzamykateľ. voliaci sp. Ø 22 – 2 polohy usad. – Ronis 421E – vľavo",0]
["ZB5AG210","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":42.09345,"d":"42.093"},"3389110135244",{"v":8.2,"d":"8.20"},{"v":3.2,"d":"3.20"},{"v":5.4,"d":"5.40"},{"v":66,"d":"66.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG210","hlavica pre uzamykateľ. voliaci sp. Ø 22 – 2 polohy usad. – Ronis 458A – vľavo",0]
["ZB5AG2","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":27.45225,"d":"27.452"},"3389110905809",{"v":9.1,"d":"9.10"},{"v":3.8,"d":"3.80"},{"v":5.5,"d":"5.50"},{"v":66,"d":"66.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG2","hlavica pre uzamykateľ. voliaci sp. Ø 22 – 2 polohy usad. – Ronis 455 – vľavo",0]
["ZB5AG1","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3389110905793",5.33,8.64,{"v":3.3,"d":"3.30"},{"v":70,"d":"70.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG1","ovládateľná otočná hlavica Ø22 3-polohy s návratom Ronis 455",0]
["ZB5AG0D","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110136623",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG0D","hlav. pre uzamyk. voliaci sp. Ø 22 – 3 polohy usad. – Dom 8D1, akákoľvek pol.",0]
["ZB5AG09","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":29.7399375,"d":"29.740"},"3389110905786",{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":5.2,"d":"5.20"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG09","ovládateľná otočná hlavica Ø22 3-polohy pevné Ronis 455",0]
["ZB5AG0820","Ovl. hlavica s kľúčom, 3 polohy s návrat",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3389110136340",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG0820","ovl. hlavica otočná Ø22 3-polohy s návratom Ronis 3131A",0]
["ZB5AG08","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110905779",{"v":5.2,"d":"5.20"},{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG08","ovládateľná otočná hlavica Ø22 3-polohy s návratom Ronis 455",0]
["ZB5AG05C0","Ovládacia hlavica otočná so zámkom Kľúč",1,"ks",{"v":33.857775,"d":"33.858"},"3606489764548",{"v":5.2,"d":"5.20"},{"v":8.6,"d":"8.60"},{"v":3.3,"d":"3.30"},{"v":58,"d":"58.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG05C0","Harmony, Key switch selector head, plastic, black, Ø22, key 455, 3 positions, spring return right to center, withdrawal left and center, grey bezel",0]
["ZB5AG05","OVLÁDACIA HLAVICA S KĽÚČOM",1,"ks",{"v":49.8715875,"d":"49.872"},"3389110223514",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":50,"d":"50.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5AG05","ovl. hlavica otočná Ø22 3-poloha s návratom Ronis 455",0]
["ZB5AG03D","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110136609",{"v":5.2,"d":"5.20"},{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":65,"d":"65.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG03D","hlav. pre uzamyk. voliaci sp. Ø 22 – 3 polohy usad. – Dom 8D1 – vľavo+v strede",0]
["ZB5AG02K","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3389110884128",{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":50,"d":"50.00"},"FR","85365080","https://www.se.com/sk/sk/product/ZB5AG02K","Head for key selector switch, Harmony XB5, XB4, Ø22 mm 2 position stay put 4 multichips",0]
["ZB5AG02D","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":27.45225,"d":"27.452"},"3389110136487",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":68,"d":"68.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG02D","hlavica pre uzamykateľný voliaci sp. Ø 22 – 2 polohy usadenia – Dom 8D1 – vpravo",0]
["ZB5AG02","OVL. HLAVICA OTOC. SO ZÁMKOM",1,"ks",{"v":27.45225,"d":"27.452"},"3389110651867",{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG02","ovládateľná otočná hlavica Ø22 2-polohy pevné Ronis 455",0]
["ZB5AG012","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":51.2442,"d":"51.244"},"3389110135381",{"v":3.5,"d":"3.50"},{"v":8.7,"d":"8.70"},{"v":5.2,"d":"5.20"},{"v":66,"d":"66.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB5AG012","ovládateľná otočná hlavica Ø22 3-polohy pevné Ronis 421E",0]
["ZB5AG0","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110905762",{"v":8.4,"d":"8.40"},{"v":3.6,"d":"3.60"},{"v":5.2,"d":"5.20"},{"v":67,"d":"67.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AG0","hlav. pre uzamyk. voliaci sp. Ø22 – 3 polohy usad. – Ronis 455 – akákoľvek pol.",0]
["ZB5AFDA","OVL. HLAVICA UZAMYKATEĽNÁ",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110905403",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AFDA","hlavica pre uzamykateľné tlačidlo Ø 22 – okrúhla – Dom 4A185 – v oboch polohách",0]
["ZB5AD922","HLAVICA PRE POTENCIOMETER",1,"ks",{"v":19.674112499999996,"d":"19.674"},"3389110905380",{"v":6.3,"d":"6.30"},{"v":4.7,"d":"4.70"},{"v":5.4,"d":"5.40"},{"v":33,"d":"33.00"},"FR","8533900000","https://www.se.com/sk/sk/product/ZB5AD922","vrúbkovaná hlavica potenciometra – Ø 22 – čierna – 6,35 mm hriadeľ",0]
["ZB5AD912","HLAVICA PRE POTENCIOMETER",1,"ks",{"v":38.43315,"d":"38.433"},"3389110905373",{"v":5.5,"d":"5.50"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":32,"d":"32.00"},"FR","8533900000","https://www.se.com/sk/sk/product/ZB5AD912","vrúbkovaná hlavica potenciometra – Ø 22 – čierna – 6 mm hriadeľ",0]
["ZB5AD8","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110905311",{"v":5.4,"d":"5.40"},{"v":3.3,"d":"3.30"},{"v":5.2,"d":"5.20"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD8","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AD7","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110905250",{"v":5.8,"d":"5.80"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD7","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AD5C0","ČI Ovládacia hlavica otočná, 3 pozície s",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3606489763626",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":25,"d":"25.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD5C0","Harmony XB5, Selector switch head, plastic, black, Ø22, 3 positions, spring return to center, grey bezel",0]
["ZB5AD59","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110905243",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.2,"d":"4.20"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD59","vrúbkovaná hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AD506","MO Ovládacia hlavica otočná, 3 pozície",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110815900",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD506","modrá ovl. hlavica otočná Ø22 3-polohy s návratom",0]
["ZB5AD503","OVL. HLAVICA OTOČNÁ ZELENÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110905212",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD503","hlavica voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB5AD501","OVL. HLAVICA OTOČNÁ BIELA",1,"ks",{"v":12.81105,"d":"12.811"},"3389110905205",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD501","hlavica voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB5AD5","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110905199",{"v":5.9,"d":"5.90"},{"v":3.7,"d":"3.70"},{"v":5.4,"d":"5.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD5","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AD405C0","ŽL Ovládacia hlavica otočná, 2 pozície s",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3606489763404",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD405C0","Harmony XB5, Selector switch head, plastic, yellow, Ø22, 2 positions, spring return from right to left, grey bezel",0]
["ZB5AD4","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110905120",{"v":5.8,"d":"5.80"},{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":27.3,"d":"27.30"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD4","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB5AD3C0","ČI Ovládacia hlavica otočná, 3 pozície p",1,"ks",{"v":8.3271825,"d":"8.327"},"3606489763329",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD3C0","Harmony XB5, Selector switch head, plastic, black, Ø22, 3 positions, stay put, grey bezel modif image",0]
["ZB5AD39","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110905113",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD39","vrúbkovaná hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AD306","OVL. HLAVICA OTOČNÁ MODRÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110815825",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD306","hlavica voliaceho spínača – 3 polohy – Ø 22 – modrá",0]
["ZB5AD305","OVL. HLAVICA OTOČNÁ ŽLTÁ",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110905106",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD305","hlavica voliaceho spínača – 3 polohy – Ø 22 – žltá",0]
["ZB5AD304","OVL. HLAVICA OTOČNÁ ČERVENÁ",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110905090",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD304","hlavica voliaceho spínača – 3 polohy – Ø 22 – červená",0]
["ZB5AD303","OVL. HLAVICA OTOČNÁ ZELENÁ",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110905083",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD303","hlavica voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB5AD301","OVL. HLAVICA OTOČNÁ BIELA",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110905076",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD301","hlavica voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB5AD3","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":8.098413749999999,"d":"8.098"},"3389110905069",{"v":5.9,"d":"5.90"},{"v":3.7,"d":"3.70"},{"v":5.4,"d":"5.40"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD3","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB5AD2C0","ČI Ovládacia hlavica otočná, 2 pozície p",1,"ks",{"v":7.0460775,"d":"7.046"},"3606489763183",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD2C0","Selector switch head, Harmony XB5, plastic, black, 22mm, 2 positions, stay put, grey bezel",0]
["ZB5AD29","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":10.065825,"d":"10.066"},"3389110905052",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD29","vrúbkovaná hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB5AD2801","OVL. HL. PRE PÁČK. SPÍNAČ BIELA",1,"ks",{"v":34.77285,"d":"34.773"},"3389110905021",{"v":6.6,"d":"6.60"},{"v":2.4,"d":"2.40"},{"v":5.9,"d":"5.90"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD2801","hlavica pákového spínača – 2 polohy – Ø 22 – biela",0]
["ZB5AD28","OVL. HL. PRE PÁČK. SPÍNAČ ČIERNA",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3389110905014",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":22,"d":"22.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD28","hlavica pákového spínača – 2 polohy – Ø 22 – čierna",0]
["ZB5AD206","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110815818",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD206","hlavica voliaceho spínača – 2 polohy – Ø 22 – modrá",0]
["ZB5AD205","OVL. HLAVICA OTOČNÁ ŽLTÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110905007",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD205","hlavica voliaceho spínača – 2 polohy – Ø 22 – žltá",0]
["ZB5AD204","OVL. HLAVICA OTOČNÁ ČERVENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110904994",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD204","hlavica voliaceho spínača – 2 polohy – Ø 22 – červená",0]
["ZB5AD203","OVL. HLAVICA OTOČNÁ ZELENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110904987",{"v":4.8,"d":"4.80"},{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD203","hlavica voliaceho spínača – 2 polohy – Ø 22 – zelená",0]
["ZB5AD201","OVL. HLAVICA OTOČNÁ BIELA",1,"ks",{"v":10.065825,"d":"10.066"},"3389110904970",{"v":5,"d":"5.00"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD201","hlavica voliaceho spínača – 2 polohy – Ø 22 – biela",0]
["ZB5AD2","OVL. HLAVICA OTOČNÁ ČIERNA",1,"ks",{"v":7.7323837499999994,"d":"7.732"},"3389110904963",{"v":6,"d":"6.00"},{"v":3.7,"d":"3.70"},{"v":5.4,"d":"5.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AD2","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB5AC680","OVL. HLAVICA ROBUSTNÁ MODRÁ",1,"ks",{"v":21.5042625,"d":"21.504"},"3606480444845",{"v":14.5,"d":"14.50"},{"v":2.4,"d":"2.40"},{"v":10.7,"d":"10.70"},{"v":25,"d":"25.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AC680","hlava tlačítka pre nepriaznivé prostredie - tmavě modrá - bez ozn.",0]
["ZB5AC6","OVL. HLAVICA S HRÍBOM MODRÁ",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110904949",{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":46,"d":"46.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AC6","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – modrá – s hríbom Ø 40 mm",0]
["ZB5AC54","OVL. HLAVICA S HRÍBOM ŽLTÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110904932",{"v":9,"d":"9.00"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":45,"d":"45.00"},"CZ","85389099","https://www.se.com/sk/sk/product/ZB5AC54","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – žltá – s hríbom Ø 30 mm",0]
["ZB5AC5","OVL. HLAVICA S HRÍBOM ŽLTÁ",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110904925",{"v":9.4,"d":"9.40"},{"v":4.5,"d":"4.50"},{"v":5.6,"d":"5.60"},{"v":48,"d":"48.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AC5","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – žltá – s hríbom Ø 40 mm",0]
["ZB5AC480","OVL. HLAVICA ROBUSTNÁ ČERVENÁ",1,"ks",{"v":21.5042625,"d":"21.504"},"3606480444821",{"v":3.8,"d":"3.80"},{"v":3.7,"d":"3.70"},{"v":3.7,"d":"3.70"},{"v":23,"d":"23.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AC480","hlava tlačítka pre nepriaznivé prostredie - červená - bez ozn.",0]
["ZB5AC44","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110904918",{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":27,"d":"27.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AC44","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – červená – s hríbom Ø 30 mm",0]
["ZB5AC4","OVL. HLAVICA S HRÍBOM ČERVENÁ",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110904901",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":48,"d":"48.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AC4","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – červená – s hríbom Ø 40 mm",0]
["ZB5AC380","OVL. HLAVICA ROBUSTNÁ ZELENÁ",1,"ks",{"v":21.5042625,"d":"21.504"},"3606480444814",{"v":3.8,"d":"3.80"},{"v":3.7,"d":"3.70"},{"v":3.7,"d":"3.70"},{"v":23,"d":"23.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AC380","hlava tlačítka pre nepriaznivé prostredie - zelená - bez ozn.",0]
["ZB5AC34","OVL. HLAVICA S HRÍBOM ZELENÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110904895",{"v":8.8,"d":"8.80"},{"v":4.2,"d":"4.20"},{"v":5.4,"d":"5.40"},{"v":27,"d":"27.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AC34","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zelená – s hríbom Ø 30 mm",0]
["ZB5AC3","OVL. HLAVICA S HRÍBOM ZELENÁ",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110904888",{"v":9,"d":"9.00"},{"v":4.5,"d":"4.50"},{"v":5,"d":"5.00"},{"v":48,"d":"48.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AC3","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zelená – s hríbom Ø 40 mm",0]
["ZB5AC280","OVL. HLAVICA ROBUSTNÁ ČIERNA",1,"ks",{"v":21.5042625,"d":"21.504"},"3606480444807",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":24,"d":"24.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB5AC280","hlava tlačítka pre nepriaznivé prostredie - černá - bez ozn.",0]
["ZB5AC24","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":13.726125,"d":"13.726"},"3389110904871",{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":45,"d":"45.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AC24","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – čierna – s hríbom Ø 30 mm",0]
["ZB5AC2","OVL. HLAVICA S HRÍBOM ČIERNA",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110904864",{"v":8.5,"d":"8.50"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":46,"d":"46.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB5AC2","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – čierna – s hríbom Ø 40 mm",0]
["ZB5AA98","OVL. HLAVICA PRESVETLENÁ + 6 FAREB",1,"ks",{"v":8.46444375,"d":"8.464"},"3606481357052",{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA98","Harmony XB5, OVLÁDACIA HLAVICA",0]
["ZB5AA9","OVL. HLAVICA STLÁČ. + 6 FAREB. HMATNÍKOV",1,"ks",{"v":7.45786125,"d":"7.458"},"3389110134544",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA9","zapustená hlava tlačítka Ø22 s návratom s ž farbami neoznačený",0]
["ZB5AA8","OVL. HLAVICA STLÁČACIA ŠEDÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110904772",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA8","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – sivá – zapustená – bez označenia",0]
["ZB5AA791","DVOJTL. PLAST. OVLÁD. HLAVICA. BEZ HMATN",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389119043502",{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":5.3,"d":"5.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA791","zapuš./červená s presah./zapuš. trojtlač. hlavica tlač. Ø22 bez šošovky",0]
["ZB5AA79","DVOJTL. PLAST. OVLÁD. HLAVICA. BEZ HMATN",1,"ks",{"v":10.065825,"d":"10.066"},"3389119043328",{"v":3,"d":"3.00"},{"v":4.8,"d":"4.80"},{"v":4.8,"d":"4.80"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA79","dvojruká kontrolná stanica bez kontrolných zariadení - oranžová",0]
["ZB5AA7341","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA IP66",1,"ks",{"v":10.5233625,"d":"10.523"},"3389119043298",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA7341","zelená lícujúca/červená lícujúca ovl. hlavica dvojtlač. Ø22 s popisom",0]
["ZB5AA7340","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA IP66",1,"ks",{"v":10.5233625,"d":"10.523"},"3389119043281",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA7340","zelená lícujúca/červená lícujúca ovl. hlavica dvojtlač. Ø22 neoznačená",0]
["ZB5AA73134","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA+STOP",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389119043441",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA73134","zel. lícujúca/červená s presah./zel. zapuš.trojtlač.hlavica tlač.Ø22 s popisom",0]
["ZB5AA7213","Dvojtlačidlová ovládacia hlavica šípky",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3606481198624",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":26,"d":"26.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA7213","Dvojtlačidlová plastová ovládacia hlavica - šípky Ľ+P biela a čierna",0]
["ZB5AA72124","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA+STOP",1,"ks",{"v":20.589187499999998,"d":"20.589"},"3389119043496",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA72124","čierna zapuš./červená s presah./čierna zapuš.trojtlač.hlavica tlač.Ø22 s popisom",0]
["ZB5AA7121","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA IP66",1,"ks",{"v":11.4384375,"d":"11.438"},"3389119043274",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":25,"d":"25.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA7121","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač. Ø22 s popisom",0]
["ZB5AA7120","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA IP66",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389119043267",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":23,"d":"23.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA7120","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač. Ø22 neoznačená",0]
["ZB5AA71124","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA+STOP",1,"ks",{"v":16.9288875,"d":"16.929"},"3389119603492",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA71124","biela zapuš./červená s presah./čierna zapuš.trojtlač.hlavica tlač.Ø22 s popisom",0]
["ZB5AA71123","DVOJTLAČ. PLAST. OVLÁDACIA HLAVICA+STOP",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389119603485",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA71123","biela zapuš./červená s presah./čierna zapuš.trojtlač.hlavica tlač.Ø22 s popisom",0]
["ZB5AA71114","Ovládacia hlavica trojtlačidlová",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389119043489",{"v":5.2,"d":"5.20"},{"v":3.2,"d":"3.20"},{"v":4.8,"d":"4.80"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA71114","biela zapuš./čierna s presah./biela zapuš.trojtlač.hlavica tlač. Ø22 s popisom",0]
["ZB5AA68","OVL. HLAVICA STLÁČACIA MODRÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110904765",{"v":8.2,"d":"8.20"},{"v":3.2,"d":"3.20"},{"v":5.2,"d":"5.20"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA68","hlavica osvetleného tlačidla – Ø 22 – modrá – na vloženie štítku",0]
["ZB5AA66","OVL. HLAVICA STLÁČACIA MODRÁ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110291551",5.08,4.57,3.56,{"v":180,"d":"180.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA66","modrá zapuš. ovl. hlavica stis. Ø22 s návratom neoznačená",0]
["ZB5AA650","Modrá zapus. hlava tlačítka Ø22 s návrat",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389119023870",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":18,"d":"18.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA650","modrá zapus. hlava tlačítka Ø22 s návratom \"šipky hore a dole\"",0]
["ZB5AA6","OVL. HLAVICA STLÁČACIA MODRÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110904758",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":16.8,"d":"16.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA6","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – modrá – zapustená – bez označenia",0]
["ZB5AA5C0","ŽL Ovládacia hlavica stláčacia,  ŠE",1,"ks",{"v":7.503614999999998,"d":"7.504"},"3606489762629",{"v":5.2,"d":"5.20"},{"v":4.2,"d":"4.20"},{"v":3.3,"d":"3.30"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA5C0","Push button head, Harmony XB5, plastic, flush, yellow, 22mm, spring return, unmarked, grey bezel",0]
["ZB5AA58","OVL. HLAVICA STLÁČACIA ŽLTÁ",1,"ks",{"v":7.091831249999999,"d":"7.092"},"3389110904741",{"v":5.5,"d":"5.50"},{"v":9.2,"d":"9.20"},{"v":3.7,"d":"3.70"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA58","hlavica osvetleného tlačidla – Ø 22 – žltá – na vloženie štítku",0]
["ZB5AA56","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110291544",5.08,4.57,3.56,{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA56","žltá zapuš. ovl. hlavica stis. Ø22 s návratom neoznačená",0]
["ZB5AA551","OVL. HLAVICA STLÁČACIA ŽLTÁ, SYMBOL",1,"ks",{"v":7.0460775,"d":"7.046"},"3389119023887",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA551","žltá zapust. hlava tlačítka Ø22 s návratom \"značka zvonka\"",0]
["ZB5AA5","OVL. HLAVICA STLÁČACIA ŽLTÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110904734",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA5","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – žltá – zapustená – bez označenia",0]
["ZB5AA48","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":7.137584999999999,"d":"7.138"},"3389110904727",{"v":9,"d":"9.00"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA48","hlavica osvetleného tlačidla – Ø 22 – červená – na vloženie štítku",0]
["ZB5AA46","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110291537",4.57,5.33,3.56,{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA46","červená zapuš. ovl. hlavica stis. Ø22 s návratom neoznačená",0]
["ZB5AA435","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110904710",{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA435","červená zapust. hlava tlačítka Ø22 s návratom \"OFF\"",0]
["ZB5AA434","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110904703",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA434","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – červená – zapustená – STOP",0]
["ZB5AA432","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110904680",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA432","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – červená – zapustená – O",0]
["ZB5AA4","OVL. HLAVICA STLÁČACIA ČERVENÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110904673",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA4","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – červená – zapustená – bez označ.",0]
["ZB5AA38","OVL. HLAVICA STLÁČACIA ZELENÁ",1,"ks",{"v":7.137584999999999,"d":"7.138"},"3389110904666",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA38","hlavica osvetleného tlačidla – Ø 22 – zelená – na vloženie štítku",0]
["ZB5AA36","OVL. HLAVICA STLÁČACIA ZELENÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110291520",{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA36","zelená zapuš. ovl. hlavica stis. Ø22 s návratom neoznačená",0]
["ZB5AA344","OVL. HLAVICA STLÁČACIA ČIERNA DOWN",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110134605",4.83,4.32,3.56,{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA344","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – čierna – zapustená – dole",0]
["ZB5AA343","OVL. HLAVICA STLÁČACIA BIELA UP",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110134575",5.08,4.32,3.56,{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA343","biela lícujúca ovl. hlavica stláčacia Ø22 s návratom \"UP\"",0]
["ZB5AA341","OVL. HLAVICA STLÁČACIA ZELENÁ",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110904642",{"v":3,"d":"3.00"},{"v":3.6,"d":"3.60"},{"v":4.8,"d":"4.80"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA341","zelená zapust. hlava tlačítka Ø22 s návratom \"ON\"",0]
["ZB5AA336","OVL. HLAVICA STLÁČACIA ZELENÁ",1,"ks",{"v":6.314017499999999,"d":"6.314"},"3389110904635",{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":15,"d":"15.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA336","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zelená – zapustená – II",0]
["ZB5AA335","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110134612",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA335","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – čierna – zapustená – šípka hore",0]
["ZB5AA334","OVL. HLAVICA STLÁČACIA BIELA",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110134582",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":16.8,"d":"16.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA334","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – biela – zapustená – šípka hore",0]
["ZB5AA333","OVL. HLAVICA STLÁČACIA ZELENÁ",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110904543",{"v":5.5,"d":"5.50"},{"v":3.6,"d":"3.60"},{"v":4.7,"d":"4.70"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA333","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zelená – zapustená – START",0]
["ZB5AA331","OVL. HLAVICA STLÁČACIA ZELENÁ",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110904536",{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":4.3,"d":"4.30"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA331","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zelená – zapustená – I",0]
["ZB5AA3","OVL. HLAVICA STLÁČACIA ZELENÁ",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110904529",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":16.8,"d":"16.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA3","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zelená – zapustená – bez označ.",0]
["ZB5AA2TQ","OVL. HLAVICA STLÁČACIA ČIERNA (100 ks)",100,"ks",{"v":4.98715875,"d":"4.987"},"3389110883930",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":20,"d":"20.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA2TQ","hlava tlačítka ZB5AA2 množ. 100",0]
["ZB5AA2C0","Ovládacia hlavica, ČI ŠE",1,"ks",{"v":4.34660625,"d":"4.347"},"3606489762087",{"v":5.4,"d":"5.40"},{"v":3.3,"d":"3.30"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA2C0","Push button head, Harmony XB5, plastic, flush, black, 22mm, spring return, unmarked, grey bezel",0]
["ZB5AA26","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":7.2748462499999995,"d":"7.275"},"3389110291414",{"v":4.3,"d":"4.30"},{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA26","černý zapust. ovl. hlavice stláčacia Ø22 s návratom neoznačená",0]
["ZB5AA253","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":7.91539875,"d":"7.915"},"3389119023900",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA253","čierna zapus. hlava tlačítka Ø22 s návratom \"značka svetla\"",0]
["ZB5AA24","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110134735",{"v":5.3,"d":"5.30"},{"v":4.3,"d":"4.30"},{"v":3.4,"d":"3.40"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA24","čierna zapust. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB5AA234","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":6.314017499999999,"d":"6.314"},"3389110904505",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA234","čierna zapust. hlava tlačítka Ø22 s návratom \"STOP\"",0]
["ZB5AA232","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":6.314017499999999,"d":"6.314"},"3389110904444",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":16.3,"d":"16.30"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA232","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – čierna – zapustená – O",0]
["ZB5AA2","OVL. HLAVICA STLÁČACIA ČIERNA",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110904437",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA2","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – čierna – zapustená – bez označ.",0]
["ZB5AA18","OVL. HLAVICA STLÁČACIA BIELA",1,"ks",{"v":7.137584999999999,"d":"7.138"},"3389110904420",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA18","osvetlená hlavica tlačidla – Ø 22 – biela – na vloženie štítku",0]
["ZB5AA145","Ovládacia hlavica stískacia",1,"ks",{"v":7.45786125,"d":"7.458"},"3389110842012",{"v":5.3,"d":"5.30"},{"v":3.3,"d":"3.30"},{"v":4.4,"d":"4.40"},{"v":17.5,"d":"17.50"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB5AA145","biela zapuš. ovl. hlavica stis. Ø22 s návratom \"T\"",0]
["ZB5AA14","OVL. HLAVICA STLÁČACIA BIELA",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110134728",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":20,"d":"20.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA14","biela lícujúca ovl. hlavica stláčacia Ø22 s návratom neoznačená",0]
["ZB5AA131","OVL. HLAVICA STLÁČACIA BIELA",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110904376",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.8,"d":"4.80"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA131","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – biela – zapustená – I",0]
["ZB5AA1","OVL. HLAVICA STLÁČACIA BIELA",1,"ks",{"v":4.80414375,"d":"4.804"},"3389110904369",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":17,"d":"17.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA1","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – biela – zapustená – bez označenia",0]
["ZB5AA0","OVL. HLAV. STLÁČ. BEZ HMATNÍKA",1,"ks",{"v":4.575374999999999,"d":"4.575"},"3389110904352",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":15.5,"d":"15.50"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB5AA0","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – bez krytu",0]
["ZB4SZ3","ZASLEPOVACIA KRYTKA",10,"ks",{"v":5.44469625,"d":"5.445"},"3389110099577",{"v":2.8,"d":"2.80"},{"v":2.3,"d":"2.30"},{"v":2.8,"d":"2.80"},{"v":23,"d":"23.00"},"FR","7326909890","https://www.se.com/sk/sk/product/ZB4SZ3","okrúhla zaslepovacia krytka pre Ø 22 mm jednotky – pochrómovaná – súprava 10 ks",0]
["ZB4RTA5","NEZÁVISLÉ TLAČ. VYSIELAČ, KOV, ŽLTÁ",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480334542",{"v":5.3,"d":"5.30"},{"v":8.6,"d":"8.60"},{"v":3.4,"d":"3.40"},{"v":45,"d":"45.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB4RTA5","XB5 vysielač - Ø22 mm kovová hlava - žltá",0]
["ZB4RTA4","NEZÁVISLÉ TLAČ. VYSIELAČ, KOV, ČERVENÁ",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480334528",{"v":8.7,"d":"8.70"},{"v":3.5,"d":"3.50"},{"v":5.2,"d":"5.20"},{"v":82,"d":"82.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB4RTA4","XB5 vysielač - Ø22 mm kovová hlava - červená",0]
["ZB4RTA3","NEZÁVISLÉ TLAČ. VYSIELAČ, KOV, ZELENÁ",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480334504",{"v":8.7,"d":"8.70"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":93,"d":"93.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB4RTA3","XB5 vysielač - Ø22 mm kovová hlava - zelená",0]
["ZB4RTA2","NEZÁVISLÉ TLAČ. VYSIELAČ, KOV, ČIERNA",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480334498",{"v":8.4,"d":"8.40"},{"v":3,"d":"3.00"},{"v":5.6,"d":"5.60"},{"v":94,"d":"94.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB4RTA2","XB5 vysielač - Ø22 mm kovová hlava - čierna",0]
["ZB4RTA1","NEZÁVISLÉ TLAČ. VYSIELAČ, KOV, BIELA",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480334481",{"v":5.3,"d":"5.30"},{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":45,"d":"45.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZB4RTA1","XB5 vysielač - Ø22 mm kovová hlava - biela",0]
["ZB4FW383","Hlavica pre tl. Harmony XB4, kov, žltá",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3606489582708",{"v":5.5,"d":"5.50"},{"v":4.4,"d":"4.40"},{"v":5.2,"d":"5.20"},{"v":60,"d":"60.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FW383","Hlavica pre podsvietené tlačidlo, Harmony XB4, kovová, žltá, zapustené prevedenie, 30 mm, univerzálna LED",0]
["ZB4FK1533","Hlavica podsvieteného otočného ovládača,",1,"ks",{"v":21.046725,"d":"21.047"},"3606489582210",{"v":5.2,"d":"5.20"},{"v":5.5,"d":"5.50"},{"v":4.4,"d":"4.40"},{"v":68.6,"d":"68.60"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FK1533","Hlavica podsvieteného otočného ovládača, Harmony XB4, kov, zelená, 30mm, universal LED, 3 polohy, do stredu",0]
["ZB4FK1253","Otočný ovládač presvetlený, Oranžový, 2",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606489582050",{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":5.3,"d":"5.30"},{"v":68,"d":"68.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FK1253","Head for illuminated selector switch, Harmony XB4, metal, orange handle, flush mounted, 30mm, universal LED, 2 positions",0]
["ZB4FK1243","Hlavica pre podsvietený otočný ovládač",1,"ks",{"v":17.386425,"d":"17.386"},"3606489582043",{"v":4.3,"d":"4.30"},{"v":5.5,"d":"5.50"},{"v":5.2,"d":"5.20"},{"v":68.8,"d":"68.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FK1243","Hlavica pre podsvietený otočný ovládač, Harmony XB4, kov, červená, 30mm, universal LED, 2 polohy, bez návratu",0]
["ZB4FK1213","Otočný ovládač presvetlený, Biely, 2 poz",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606489582029",{"v":5.2,"d":"5.20"},{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":69,"d":"69.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FK1213","Head for illuminated selector switch, Harmony XB4, metal, white handle, 30mm, universal LED, 2 positions, stay put",0]
["ZB4FG6","Otočný ovládač so zámkom 455, 2 pozicie",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3606489581503",{"v":5.2,"d":"5.20"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":130,"d":"130.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FG6","Head for key selector switch, Harmony XB4, black key, flush, 30mm, 2 positions, left key withdrawal, key 455",0]
["ZB4FG2","Otočný ovládač so zámkom 455, 2 pozicie",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3606489581466",{"v":5.2,"d":"5.20"},{"v":8.6,"d":"8.60"},{"v":4.3,"d":"4.30"},{"v":131,"d":"131.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FG2","Head for key selector switch, Harmony XB4, flush mounted, 455, 2 positions, stay put",0]
["ZB4FD3","Otočný ovládač, Čierny, 3 pozicie pevné",1,"ks",{"v":11.4384375,"d":"11.438"},"3606489581282",{"v":4.3,"d":"4.30"},{"v":5.5,"d":"5.50"},{"v":5.2,"d":"5.20"},{"v":72,"d":"72.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FD3","Head for selector switch, Harmony XB4, black handle, flush, 30mm, 3 positions, stay put",0]
["ZB4FA8","Ovládacia hlavica, Šedá, Lícujúca",1,"ks",{"v":6.268263749999999,"d":"6.268"},"3606489581183",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":58,"d":"58.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FA8","Head for non illuminated push button, Harmony XB4, flush mounted grey flush caps pushbutton",0]
["ZB4FA68","Ovládacia hlavica, Modrá, Lícujúca, Pre",1,"ks",{"v":13.2685875,"d":"13.269"},"3606489581176",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":58,"d":"58.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB4FA68","Head for illuminated push button, Harmony XB4, metal, blue flush mounted, 30mm, universal LED, for legend of insertion",0]
["ZB4FA5","Ovládacia hlavica, Žltá, Lícujúca,",1,"ks",{"v":5.993741249999999,"d":"5.994"},"3606489581121",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":58,"d":"58.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FA5","Flush mounted push button head, Harmony XB4, metal, yellow, 30mm, spring return, unmarked",0]
["ZB4FA2","Ovládacia hlavica, Čierna, Lícujúca,",1,"ks",{"v":5.993741249999999,"d":"5.994"},"3606489580889",{"v":5.5,"d":"5.50"},{"v":4.4,"d":"4.40"},{"v":5.2,"d":"5.20"},{"v":58,"d":"58.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4FA2","Flush mounted push button head, Harmony XB4, metal, black, 30mm, spring return, unmarked",0]
["ZB4FA18","Ovládacia hlavica, Biela, Lícujúca, Pre",1,"ks",{"v":8.098413749999999,"d":"8.098"},"3606489580872",{"v":5.5,"d":"5.50"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":60,"d":"60.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB4FA18","Head for illuminated push button, Harmony XB4, metal, white flush mounted, 30mm, universal LED, for legend of insertion",0]
["ZB4BZ66","UZAMYKATEĽNÝ KRYT HLAVICE",1,"ks",{"v":36.932427,"d":"36.932"},"3389110069754",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":96,"d":"96.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB4BZ66","modrá uzamykatelná klapka pre Ø22 zapuš. tlač.",""]
["ZB4BZ65","ZÁMOK NA TLAČÍTKO",1,"ks",{"v":38.8906875,"d":"38.891"},"3389110069747",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":76,"d":"76.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB4BZ65","žltá uzamykateľná klapka pre Ø22 zapustené tlačítko",0]
["ZB4BZ64","UZAMYKATEĽNÝ KRYT HLAVICE",1,"ks",{"v":38.8906875,"d":"38.891"},"3389110069730",{"v":5.2,"d":"5.20"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":96,"d":"96.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB4BZ64","uzamykateľný ochranný uzáver pre Ø 22 mm jednotky – červený",0]
["ZB4BZ62","UZAMYKATEĽNÝ KRYT HLAVICE",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3389110069723",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.7,"d":"4.70"},{"v":96,"d":"96.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB4BZ62","uzamykateľný ochranný uzáver pre Ø 22 mm jednotky – čierny",0]
["ZB4BZ2105","KRYTKA ŽLTÁ",1,"ks",{"v":7.778137499999999,"d":"7.778"},"785901787365",{"v":21.3,"d":"21.30"},{"v":4.1,"d":"4.10"},{"v":15.2,"d":"15.20"},{"v":58,"d":"58.00"},"MX","3926909790","https://www.se.com/sk/sk/product/ZB4BZ2105","Round guard for 40mm Emergency stop, Harmony XB4, plastic, yellow, 76.2mm",0]
["ZB4BZ2005","KRYTKA ŽLTÁ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"785901675976",{"v":6.5,"d":"6.50"},{"v":4,"d":"4.00"},{"v":4,"d":"4.00"},{"v":30,"d":"30.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB4BZ2005","Narrow flange guard for 40mm Emergency stop, Harmony XB4, plastic, yellow",0]
["ZB4BZ1905","OCHRANNÝ NADSTAVEC PRE XB4/XB5 OVLÁDAČE",1,"ks",{"v":36.602999999999994,"d":"36.603"},"785901230687",{"v":20.3,"d":"20.30"},{"v":3.8,"d":"3.80"},{"v":14,"d":"14.00"},{"v":40.8,"d":"40.80"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB4BZ1905","tvarovaný žltý nadstavec",0]
["ZB4BZ141","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110889420",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":70,"d":"70.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ141","teleso pre ovládacie tlačidlo – Ø 22 – 2 NC + 1 NO",0]
["ZB4BZ106","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":37.9756125,"d":"37.976"},"3389110173192",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.4,"d":"4.40"},{"v":61,"d":"61.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ106","polozostava kontaktov 1Z+1V skrutková svorka",0]
["ZB4BZ1055","POLOZOSTAVA KONTAKTOV-KOV-NO+NC TERMINÁL",1,"ks",{"v":13.2685875,"d":"13.269"},"3389119039284",{"v":3.6,"d":"3.60"},{"v":4.7,"d":"4.70"},{"v":5.3,"d":"5.30"},{"v":60,"d":"60.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ1055","polozostava spínacej jednotky - 1Z+1V",0]
["ZB4BZ105","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110889413",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":61,"d":"61.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ105","teleso pre ovládacie tlačidlo – Ø 22 – 1 NO+1 NC",0]
["ZB4BZ1045","POLOZOSTAVA KONTAKTOV-KOV-2NC TERMINÁLY",1,"ks",{"v":13.2685875,"d":"13.269"},"3389119037716",{"v":4.6,"d":"4.60"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":61,"d":"61.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ1045","teleso pre ovládacie tlačidlo – Ø 22 – 2 NC – pružin.svorky",0]
["ZB4BZ104","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110889406",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":61,"d":"61.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ104","teleso pre ovládacie tlačidlo – Ø 22 – 2 NC",0]
["ZB4BZ1035","POLOZOSTAVA KONTAKTOV-KOV-2NO TERMINÁLY",1,"ks",{"v":13.2685875,"d":"13.269"},"3389119037709",{"v":7.8,"d":"7.80"},{"v":3.2,"d":"3.20"},{"v":5.8,"d":"5.80"},{"v":61,"d":"61.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ1035","teleso pre ovládacie tlačidlo – Ø 22 – 2 NO – pružin.svorky",0]
["ZB4BZ103","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110889390",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":61,"d":"61.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ103","teleso pre ovládacie tlačidlo – Ø 22 – 2 NO",0]
["ZB4BZ1025","POLOZOSTAVA KONTAKTOV-KOV-NC TERMINÁL",1,"ks",{"v":8.05266,"d":"8.053"},"3389119037693",{"v":5.2,"d":"5.20"},{"v":4.3,"d":"4.30"},{"v":3.4,"d":"3.40"},{"v":52,"d":"52.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ1025","teleso pre ovládacie tlačidlo – Ø 22 – 1 NC – pružin.svorky",0]
["ZB4BZ102","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":7.36635375,"d":"7.366"},"3389110889383",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":52,"d":"52.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ102","teleso pre ovládacie tlačidlo – Ø 22 – 1 NC",0]
["ZB4BZ1015","POLOZOSTAVA KONTAKTOV-KOV-NO TERMINÁL",1,"ks",{"v":8.05266,"d":"8.053"},"3389119037686",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":3.4,"d":"3.40"},{"v":52,"d":"52.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ1015","teleso pre ovládacie tlačidlo – Ø 22 – 1 NO – pružin.svorky",0]
["ZB4BZ101","POLOZOSTAVA KONTAKTOV",1,"ks",{"v":7.36635375,"d":"7.366"},"3389110889376",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":52,"d":"52.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BZ101","teleso pre ovládacie tlačidlo – Ø 22 – 1 NO",0]
["ZB4BZ079","SPOJOVACÍ DIEL",10,"ks",{"v":3.0197474999999994,"d":"3.020"},"3389110102031",{"v":9.6,"d":"9.60"},{"v":7.2,"d":"7.20"},{"v":7.2,"d":"7.20"},{"v":3,"d":"3.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BZ079","špeciálne príslušenstvo pre montáž do tlačených spojov",0]
["ZB4BZ021","Montážna sada kovová (ovl.stláč.a sign.)",1,"ks",{"v":7.183338749999999,"d":"7.183"},"3606485440200",{"v":5.5,"d":"5.50"},{"v":4.4,"d":"4.40"},{"v":5.3,"d":"5.30"},{"v":19,"d":"19.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BZ021","montážna sada kovová Ø22 (ovl. stláčacie a signálky)",0]
["ZB4BZ009","SPOJOVACÍ DIEL",10,"ks",{"v":3.29427,"d":"3.294"},"3389110102024",{"v":4.6,"d":"4.60"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":37,"d":"37.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BZ009","upevňovacia príruba elektrického bloku pre Ø 22 mm jednotky XB4-B – súpr. 10 ks",0]
["ZB4BX84","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA, ",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389119048064",{"v":7,"d":"7.00"},{"v":8.8,"d":"8.80"},{"v":7,"d":"7.00"},{"v":88,"d":"88.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BX84","ovládacia hlavica núdzového zastavenia s aretáciou, stlač-ťahaj",0]
["ZB4BW943","OVL. HLAVICA STLÁČ. PRESVETL.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110889925",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW943","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB4BW933","OVL. HLAVICA STLÁČ. PRESVETL.",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110889901",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW933","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB4BW7L3741","DVOJTLAČ. KOV. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":21.046725,"d":"21.047"},"3389119043779",{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":5.3,"d":"5.30"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7L3741","zelená lícujúca/červená lícujúca ovl.hlavica dvojtlač.so sig. Ø22 neoznačená",0]
["ZB4BW7L3740","DVOJTLAČ. KOV. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":19.216575,"d":"19.217"},"3389119043762",{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":5.3,"d":"5.30"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7L3740","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač. so signálkou Ø22 s popisom",0]
["ZB4BW7A9","DVOJTL. KOV. OVLÁD. HL. S LED BEZ HMATN.",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389119043809",{"v":5.3,"d":"5.30"},{"v":5.9,"d":"5.90"},{"v":3.5,"d":"3.50"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7A9","zapuš./zapuš. ovl. hlavica dvojtlač. so signálkou Ø22 bez šošovky",0]
["ZB4BW7A3741","DVOJTLAČ. KOV. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389119043755",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7A3741","zelená lícujúca/červená lícujúca ovl.hlavica dvojtlač.so signálkou Ø22 s popisom",0]
["ZB4BW7A3740","DVOJTLAČ. KOV. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389119043748",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7A3740","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač. so signálkou Ø22 neoznačená",0]
["ZB4BW7A1724","DVOJTLAČ. KOV. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389119603546",{"v":4.8,"d":"4.80"},{"v":2.8,"d":"2.80"},{"v":4.4,"d":"4.40"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7A1724","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač. so signálkou Ø22 s popisom",0]
["ZB4BW7A1721","DVOJTLAČ. KOV. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389119043731",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7A1721","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač. so signálkou Ø22 s popisom",0]
["ZB4BW7A1720","DVOJTLAČ. KOV. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":16.471349999999997,"d":"16.471"},"3389119043724",{"v":3.2,"d":"3.20"},{"v":5.2,"d":"5.20"},{"v":4,"d":"4.00"},{"v":54,"d":"54.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7A1720","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač. so signálkou Ø22 neoznačená",0]
["ZB4BW7A1715","DVOJTLAČ. KOV. OVLÁDACIA HLAVICA S LED",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389119043793",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW7A1715","biela zapuš./čierna zapuš. ovl. hlavica dvojtlač. so signálkou Ø22 s popisom",0]
["ZB4BW653","OVL. HLAVICA S HRÍBOM LED STLAČ-ŤAHAJ",1,"ks",{"v":44.838674999999995,"d":"44.839"},"3389110666625",{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":9.2,"d":"9.20"},{"v":51,"d":"51.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW653","oranžová Ø40 presvet.hlavica s hríbovým tlačítkom Ø22 s aretáciou pre integ.LED",0]
["ZB4BW643","OV. HLAV. S HRÍBOM LED ČERV. STLAČ ŤAHAJ",1,"ks",{"v":44.838674999999995,"d":"44.839"},"3389110666618",{"v":5.6,"d":"5.60"},{"v":4.3,"d":"4.30"},{"v":5.2,"d":"5.20"},{"v":51,"d":"51.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW643","hlavica osvetleného tlačidla – Ø 40 – ťažná/tlačná – Ø 22 – červená",0]
["ZB4BW633","OV. HLAV. S HRÍBOM LED ZEL. STLAČ ŤAHAj",1,"ks",{"v":44.838674999999995,"d":"44.839"},"3389110666601",{"v":8.8,"d":"8.80"},{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW633","zelená Ø40 presvet. hlavica s hríbovým tlačítkom Ø22 s aretáciou pre integ. LED",0]
["ZB4BW613","OVLÁDACIA HLAVICA STLAČ-STLAČ",1,"ks",{"v":41.178374999999996,"d":"41.178"},"3389110666595",{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":57,"d":"57.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW613","hlavica osvetleného tlačidla – Ø 40 – ťažná/tlačná – Ø 22 – biela",0]
["ZB4BW563","OVL. HLAVICA STLÁČACIA PRESVETLENÁ",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110892826",{"v":4.8,"d":"4.80"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW563","modrá ovl. hlavica stláčacia presvetlená-lícujúca Ø22 s návratom pre integ. LED",0]
["ZB4BW553","OVL. HLAV. STLÁČ. PODSVIE., ZEL SILIKON",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110892819",{"v":4.8,"d":"4.80"},{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW553","oranžová ovl.hlavica stískacia presvet.-lícujúca Ø22 s návratom pre integ. LED",0]
["ZB4BW543","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110892802",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW543","červená ovl. hlavica stis. presvetlená - lícujúca Ø22 s návratom pre integ. LED",0]
["ZB4BW533","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110892796",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW533","hlavica osvetleného tlačidla – Ø 22 – zelená – krytá",0]
["ZB4BW513","OVL.HLAVICA STLAČ.PRESVETLENÁ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110892789",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW513","hlavica osvetleného tlačidla – Ø 22 – biela – krytá",0]
["ZB4BW463","OV. HLAVICA S HRÍBOM LED MODRÁ OD. OTOČ.",1,"ks",{"v":38.43315,"d":"38.433"},"3389110666519",{"v":9.3,"d":"9.30"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":62,"d":"62.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW463","hlavica osvetleného tlačidla – Ø 40 – Ø 22 – modrá",0]
["ZB4BW453","OV. HLAVICA S HRÍBOM LED ORANŽ. OD.OTOČ.",1,"ks",{"v":38.43315,"d":"38.433"},"3389110666502",{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":51,"d":"51.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW453","hlavica osvetleného tlačidla – Ø 40 – Ø 22 – žltá",0]
["ZB4BW443","OV.HLAVICA S HRÍBOM LED ČERVENÁ OD.OTOČ.",1,"ks",{"v":39.80576249999999,"d":"39.806"},"3389110666496",{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":62,"d":"62.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW443","hlavica osvetleného tlačidla – Ø 40 – Ø 22 – červená",0]
["ZB4BW433","OV. HLAVICA S HRÍBOM LED ZELENÁ OD.OTOČ.",1,"ks",{"v":39.80576249999999,"d":"39.806"},"3389110666489",{"v":8.5,"d":"8.50"},{"v":5.3,"d":"5.30"},{"v":4.2,"d":"4.20"},{"v":63,"d":"63.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW433","hlavica osvetleného tlačidla – Ø 40 – Ø 22 – zelená",0]
["ZB4BW413","OV. HLAVICA S HRÍBOM LED BIELA OD. OTOČ.",1,"ks",{"v":39.80576249999999,"d":"39.806"},"3389110666472",{"v":8.5,"d":"8.50"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":51,"d":"51.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW413","hlavica osvetleného tlačidla – Ø 40 – Ø 22 – biela",0]
["ZB4BW383","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3606481206305",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW383","Head for illuminated push button, Harmony XB4, metal, metal, yellow, 22mm, universal LED, spring return, plain lens",0]
["ZB4BW37","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110123227",{"v":5.2,"d":"5.20"},{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":26,"d":"26.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BW37","hlavica osvetleného tlačidla – Ø 22 – číra",0]
["ZB4BW3637","Ovládací hlavica stiskací",1,"ks",{"v":27.122822999999997,"d":"27.123"},"3389110840094",{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":4.4,"d":"4.40"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW3637","hlava ovládača, ovládač Ø22 pružinový návrat pre integr. LED",""]
["ZB4BW363","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110889833",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW363","hlavica osvetleného tlačidla – Ø 22 – modrá",0]
["ZB4BW36","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110889734",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BW36","hlavica osvetleného tlačidla – Ø 22 – modrá",0]
["ZB4BW353","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110889826",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW353","hlavica osvetleného tlačidla – Ø 22 – žltá",0]
["ZB4BW35","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110889727",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BW35","hlavica osvetleného tlačidla – Ø 22 – žltá",0]
["ZB4BW343","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110889819",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW343","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB4BW34","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110889710",{"v":4.5,"d":"4.50"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BW34","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB4BW333","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110889802",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW333","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB4BW33","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110889703",{"v":4.5,"d":"4.50"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BW33","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB4BW313","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":10.065825,"d":"10.066"},"3389110889796",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW313","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB4BW31","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110889697",{"v":4.5,"d":"4.50"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BW31","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB4BW163","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110889888",{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":4.8,"d":"4.80"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW163","modrá ovl. hlavica presvet. stis. s presahom Ø22 s návratom pre integ. LED",0]
["ZB4BW16","OVLÁDACIA HLAVICA STLÁČACIA PRESVETLENÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110889789",{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":27,"d":"27.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BW16","hlavica osvetleného tlačidla – Ø 22 – modrá",0]
["ZB4BW153","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110889871",{"v":5.6,"d":"5.60"},{"v":3.5,"d":"3.50"},{"v":4.6,"d":"4.60"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW153","hlavica osvetleného tlačidla – Ø 22 – žltá",0]
["ZB4BW143","OVLÁDACIA HLAVICA STLÁČACIA PRESVETLENÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110889864",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW143","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB4BW133","OVLÁDACIA HLAVICA STLÁČACIA PRESVETLENÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110889857",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.8,"d":"4.80"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW133","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB4BW13","OVL. HLAVICA STLÁČ. PRESVETLENÁ",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110889758",{"v":5.3,"d":"5.30"},{"v":4.7,"d":"4.70"},{"v":3.5,"d":"3.50"},{"v":24,"d":"24.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BW13","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB4BW113","OVLÁDACIA HLAVICA STLÁČACIA PRESVETLENÁ",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110889840",{"v":4.6,"d":"4.60"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":28.8,"d":"28.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BW113","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB4BW0M15","OVL.HLAVICA STLÁČACIA PRESVETLENÁ 230V",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110893533",{"v":5.9,"d":"5.90"},{"v":3.6,"d":"3.60"},{"v":5.3,"d":"5.30"},{"v":70,"d":"70.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BW0M15","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 1 NO + 1 NC",0]
["ZB4BW0G15","OVL.HLAVICA STLÁČACIA PRESVETLENÁ 120V",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3389110893311",{"v":6.3,"d":"6.30"},{"v":3.5,"d":"3.50"},{"v":5.7,"d":"5.70"},{"v":70,"d":"70.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BW0G15","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 1 NO + 1 NC",0]
["ZB4BW0B15","POLOZOSTAVA S LED SO SP. JEDNOTKOU",1,"ks",{"v":19.216575,"d":"19.217"},"3389110893113",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":70,"d":"70.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB4BW0B15","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 1 NO + 1 NC",0]
["ZB4BW0B13","POLOZOSTAVA S LED SO SP. JEDNOTKOU",1,"ks",{"v":19.216575,"d":"19.217"},"3389110893106",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":69,"d":"69.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB4BW0B13","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 2 NO",0]
["ZB4BW0B12","POLOZOSTAVA S LED SO SP. JEDNOTKOU",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110893090",{"v":5.2,"d":"5.20"},{"v":3.2,"d":"3.20"},{"v":4.6,"d":"4.60"},{"v":60,"d":"60.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB4BW0B12","biela polozostava objímky s integ. LED 24V 1V",0]
["ZB4BW0B11","POLOZOSTAVA S LED SO SP. JEDNOTKOU",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110893083",{"v":5.2,"d":"5.20"},{"v":5.7,"d":"5.70"},{"v":3.4,"d":"3.40"},{"v":61,"d":"61.00"},"FR","8536501190","https://www.se.com/sk/sk/product/ZB4BW0B11","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – biela zabud. LED 1 NO",0]
["ZB4BW065","POLOZOSTAVA PRE ŽIAROVKU SO SP. JEDNOT.",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389110891157",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":70,"d":"70.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BW065","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – základňa BA 9s 1 NO + 1 NC",0]
["ZB4BW063","POLOZOSTAVA PRE ŽIAROVKU SO SP. JEDNOT.",1,"ks",{"v":18.301499999999997,"d":"18.302"},"3389110891140",{"v":5.5,"d":"5.50"},{"v":3.6,"d":"3.60"},{"v":4.7,"d":"4.70"},{"v":69,"d":"69.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BW063","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – základňa BA 9s 2 NO",0]
["ZB4BW062","POLOZOSTAVA PRE ŽIAROVKU SO SP. JEDNOT.",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110891133",{"v":5.3,"d":"5.30"},{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":60,"d":"60.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BW062","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – základňa BA 9s 1 NC",0]
["ZB4BW061","POLOZOSTAVA PRE ŽIAROVKU SO SP. JEDNOT.",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110891126",{"v":5.4,"d":"5.40"},{"v":4.3,"d":"4.30"},{"v":3.5,"d":"3.50"},{"v":60,"d":"60.00"},"FR","8536508090","https://www.se.com/sk/sk/product/ZB4BW061","teleso pre osvetlené ovládacie tlačidlo – Ø 22 – základňa BA 9s 1 NO",0]
["ZB4BVM1","POLOZOSTAVA OBJÍMKY S LED",1,"ks",{"v":18.301499999999997,"d":"18.302"},"3389110892482",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":52,"d":"52.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BVM1","teleso pre kontrolku – ZB4 – biela zabud. LED – 230 - 240 V",0.01]
["ZB4BVJ1","POLOZOSTAVA OBJÍMKY S LED",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110069761",5.33,5.84,3.56,{"v":50,"d":"50.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BVJ1","biela polozostava objímky s integ. LED 12V",0]
["ZB4BVG1","POLOZOSTAVA OBJÍMKY S LED",1,"ks",{"v":17.386425,"d":"17.386"},"3389110892437",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":52,"d":"52.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BVG1","teleso pre kontrolku – ZB4 – biela zabud. LED – 48 - 120 V",0.01]
["ZB4BVBG1","POLOZOSTAVA OBJÍMKY S LED BIELA",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110070163",{"v":5.6,"d":"5.60"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":51,"d":"51.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BVBG1","bílá polozostava objímky s integ. LED 24...120V",0.01]
["ZB4BVB1","POLOZOSTAVA OBJÍMKY S LED",1,"ks",{"v":11.4384375,"d":"11.438"},"3389110892383",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":52,"d":"52.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BVB1","teleso pre kontrolku – ZB4 – biela zabud. LED – 24 V",0]
["ZB4BV8","POLOZOSTAVA OBJÍMKY S LED",1,"ks",{"v":36.602999999999994,"d":"36.603"},"3389110889673",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":126,"d":"126.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV8","polozostava objímky s BA9s LED žiarovka 400V...480V",0.02]
["ZB4BV6","POLOZOSTAVA PRE ŽIAROVKU SO SP. JEDNOT.",1,"ks",{"v":8.418689999999998,"d":"8.419"},"3389110889628",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":50.9,"d":"50.90"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV6","teleso pre kontrolku – ZB4 – základňa BA 9s – 250 V",0]
["ZB4BV5D6","POLOZOSTAVA LED 400VAC",1,"ks",{"v":52.159274999999994,"d":"52.159"},"3389110892628",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":131,"d":"131.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV5D6","teleso pre kontrolku – ZB4 – modrá LED BA 9s – 400 V",0.02]
["ZB4BV5D4","ČERVENÁ LED TRAFO 400V",1,"ks",{"v":42.09345,"d":"42.093"},"3389110892604",{"v":3.2,"d":"3.20"},{"v":8.4,"d":"8.40"},{"v":5.2,"d":"5.20"},{"v":130,"d":"130.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV5D4","červená polozostava objímky s BA9s LED žiarovka 400V",0.02]
["ZB4BV5D3","ZELENÁ LED TRAFO 400V",1,"ks",{"v":42.09345,"d":"42.093"},"3389110892598",{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":131,"d":"131.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV5D3","zelená polozostava objímky s BA9s LED žiarovka 400V",0.02]
["ZB4BV5D1","POLOZOSTAVA LED BA9S A TR 400VAC",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3389110892581",{"v":5.4,"d":"5.40"},{"v":9.2,"d":"9.20"},{"v":3.5,"d":"3.50"},{"v":130,"d":"130.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV5D1","teleso pre kontrolku – ZB4 – biela LED BA 9s – 400 V",0.02]
["ZB4BV5","POLOZOSTAVA OBJÍMKY SO ŽIAROVKOU A TR",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3389110889666",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":131,"d":"131.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV5","teleso pre kontrolku – ZB4 – číra žiarovka BA 9s – 400 V",0.02]
["ZB4BV4","POLOZOSTAVA OBJÍMKY",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3389110889659",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":129,"d":"129.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV4","teleso pre kontrolku – ZB4 – číra žiarovka BA 9s – 230 V",0.02]
["ZB4BV3","120 V TRANSFO PILOT LIGHT",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3389110895766",{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":129,"d":"129.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV3","polozostava objímky s BA9s žiarovkou 110...120V",0.02]
["ZB4BV156","KONTROLKA TEST",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3389110071689",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":61,"d":"61.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZB4BV156","polozostava objímky s pro BA9s žiarovka <lt/>=250V",0.01]
["ZB4BV083","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":6.039494999999999,"d":"6.039"},"3606481202253",{"v":5.5,"d":"5.50"},{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":26,"d":"26.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV083","Head for pilot light, Harmony XB4, yellow, 22mm, with plain lens, universal LED",0]
["ZB4BV07","SIGNÁLNA HLAVICA",1,"ks",{"v":5.764972499999999,"d":"5.765"},"3389110123241",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":23,"d":"23.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV07","kryt kontrolky – Ø 22 – okrúhly – číra hladká šošovka",0]
["ZB4BV063S","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110290851",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV063S","modrá signálna hlavica Ø22 ryhovaná šošovka pre integ. LED",0]
["ZB4BV063","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":6.08524875,"d":"6.085"},"3389110895018",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV063","kryt kontrolky – Ø 22 – okrúhly – modrá hladká šošovka",0]
["ZB4BV06","SIGNÁLNA HLAVICA",1,"ks",{"v":5.62771125,"d":"5.628"},"3389110889536",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":23,"d":"23.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV06","kryt kontrolky – Ø 22 – okrúhly – modrá hladká šošovka",0]
["ZB4BV053S","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110290844",{"v":4.8,"d":"4.80"},{"v":2.8,"d":"2.80"},{"v":3.8,"d":"3.80"},{"v":26,"d":"26.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV053S","oranžová signálna hlavica Ø22 ryhovaná šošovka pre integ. LED",0]
["ZB4BV053E","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":7.5951225,"d":"7.595"},"3389110290332",{"v":4.8,"d":"4.80"},{"v":3,"d":"3.00"},{"v":3.6,"d":"3.60"},{"v":27,"d":"27.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV053E","oranžová signálna hlavica Ø22 plná šošovka pre integ. LED",0]
["ZB4BV053","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":6.08524875,"d":"6.085"},"3389110894981",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV053","kryt kontrolky – Ø 22 – okrúhly – žltá hladká šošovka",0]
["ZB4BV05","SIGNÁLNA HLAVICA",1,"ks",{"v":5.62771125,"d":"5.628"},"3389110889529",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":23,"d":"23.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV05","kryt kontrolky – Ø 22 – okrúhly – žltá hladká šošovka",0]
["ZB4BV043S","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110290837",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":27,"d":"27.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV043S","červená signálna hlavica Ø22 ryhovaná šošovka pre integ. LED",0]
["ZB4BV043E","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":7.5951225,"d":"7.595"},"3389110290325",{"v":4.8,"d":"4.80"},{"v":2.6,"d":"2.60"},{"v":3.8,"d":"3.80"},{"v":27.4,"d":"27.40"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV043E","červená signálna hlavica Ø22 plná šošovka pre integ. LED",0]
["ZB4BV043","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":6.08524875,"d":"6.085"},"3389110894998",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV043","kryt kontrolky – Ø 22 – okrúhly – červená hladká šošovka",0]
["ZB4BV04","SIGNÁLNA HLAVICA",1,"ks",{"v":5.673464999999999,"d":"5.673"},"3389110889512",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV04","kryt kontrolky – Ø 22 – okrúhly – červená hladká šošovka",0]
["ZB4BV033S","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110290820",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":4.8,"d":"4.80"},{"v":26,"d":"26.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV033S","zelená signálna hlavica Ø22 ryhovaná šošovka pre integ. LED",0]
["ZB4BV033E","SIGNÁLNA HLAVICA PRE LED",1,"ks",{"v":7.640876249999998,"d":"7.641"},"3389110290318",{"v":5.3,"d":"5.30"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":27.5,"d":"27.50"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV033E","zelená signálna hlavica Ø22 plná šošovka pre integ. LED",0]
["ZB4BV033","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":6.08524875,"d":"6.085"},"3389110895001",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV033","kryt kontrolky – Ø 22 – okrúhly – zelená hladká šošovka",0]
["ZB4BV03","SIGNÁLNA HLAVICA",1,"ks",{"v":5.90223375,"d":"5.902"},"3389110889505",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":23,"d":"23.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV03","kryt kontrolky – Ø 22 – okrúhly – zelená hladká šošovka",0]
["ZB4BV013S","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110290479",{"v":5.2,"d":"5.20"},{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":27,"d":"27.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV013S","biela signálna hlavica Ø22 ryhovaná šošovka pre integ. LED",0]
["ZB4BV013E","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":7.640876249999998,"d":"7.641"},"3389110290295",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":27,"d":"27.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV013E","biela signálna hlavica Ø22 plná šošovka pre integ. LED",0]
["ZB4BV013","SIGNÁL. HLAVICA PRE LED",1,"ks",{"v":6.08524875,"d":"6.085"},"3389110123234",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":26,"d":"26.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV013","kryt kontrolky – Ø 22 – okrúhly – biela hladká šošovka",0]
["ZB4BV01","SIGNÁLNA HLAVICA",1,"ks",{"v":5.673464999999999,"d":"5.673"},"3389110889499",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":23.4,"d":"23.40"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB4BV01","kryt kontrolky – Ø 22 – okrúhly – biela hladká šošovka",0]
["ZB4BV003","SIGNÁLNA HLAVICA",1,"ks",{"v":8.510197499999999,"d":"8.510"},"3389110889611",{"v":8.2,"d":"8.20"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":37,"d":"37.00"},"","","https://www.se.com/sk/sk/product/ZB4BV003","signálna hlavica Ø22 s 5 - farebná plná šošovka s pre integ. LED",0]
["ZB4BT847","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA, ",1,"ks",{"v":28.28496825,"d":"28.285"},"3389110824261",{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":76.5,"d":"76.50"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BT847","červená Ø40 ovl.hlav.tlač.núdzov.zastav.Ø22 vypnuté a s aretáciou \"stlač-ťahaj\"",""]
["ZB4BT844","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA, ",1,"ks",{"v":28.367324999999997,"d":"28.367"},"3389119048040",{"v":4.4,"d":"4.40"},{"v":9,"d":"9.00"},{"v":5.5,"d":"5.50"},{"v":72,"d":"72.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BT844","červená Ø30 ovl.hlav.tlač.núdzov.zastav.Ø22 vypnuté a s aretáciou \"stlač-ťahaj\"",0]
["ZB4BT84","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":23.334412499999996,"d":"23.334"},"3389110892376",{"v":8.8,"d":"8.80"},{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":76,"d":"76.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BT84","okrúhla hlavica pre tlačidlo Ø 22 – ťažná/tlačná – s hríbom Ø 40 mm – červená",0]
["ZB4BT5","OVL. HLAVICA S HRÍBOM 40MM",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3389110171709",{"v":4.5,"d":"4.50"},{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":75,"d":"75.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BT5","Mushroom push button head 40mm, Harmony XB4, metal, yellow, 22mm, latching push pull",0]
["ZB4BT2","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110888638",{"v":4.5,"d":"4.50"},{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":76,"d":"76.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BT2","okrúhla hlavica pre tlačidlo Ø 22 – ťažná/tlačná – s hríbom Ø 40 mm – čierna",0]
["ZB4BS964","OVLÁDAČ S HRÍBOM",1,"ks",{"v":42.55098749999999,"d":"42.551"},"3389110888904",{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":115,"d":"115.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS964","červená Ø60 ovl.hlav.stlač.nouz.zastav.Ø22 vypnuté a s aret.\"uvoľniľ klúčom\"",0]
["ZB4BS94412","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA, ",1,"ks",{"v":35.98989975,"d":"35.990"},"3389110122985",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":98,"d":"98.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS94412","červená Ø40 ovl.hlav.stisk.nouz.zastav.Ø22 vypnuto a s aretací \"uvolnit klíčem\"",""]
["ZB4BS94410","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA, ",1,"ks",{"v":35.98989975,"d":"35.990"},"3389110122961",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":98,"d":"98.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS94410","červená Ø40 ovl.hlav.stisk.nouz.zastav.Ø22 vypnuto a s aretací \"uvolnit klíčem\"",""]
["ZB4BS944","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":37.0605375,"d":"37.061"},"3389110888881",{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":5.3,"d":"5.30"},{"v":103,"d":"103.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS944","okrúh. hlav. pre tlač. Ø 22 – uvoľň. kl. – s hríb. Ø 40 mm – červ. – Ronis 455",0]
["ZB4BS934K","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA, ",1,"ks",{"v":56.61569024999999,"d":"56.616"},"3389110846263",{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":94,"d":"94.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS934K","červená Ø30 ovl.hlav.stisk.nouz.zastav.Ø22 vypnuto a s aretací \"uvolnit klíčem\"",""]
["ZB4BS934","OVLÁDACIA HLAVICA NÚDZOVÉHO ZASTAVENIA",1,"ks",{"v":30.655012499999998,"d":"30.655"},"3389110888874",{"v":9,"d":"9.00"},{"v":4,"d":"4.00"},{"v":5.5,"d":"5.50"},{"v":99,"d":"99.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS934","červená Ø30 ovl.hlav.stisk.núdz.zastav.Ø22 vypnutá a s aret.\"uvolniť kľúčom\"",0]
["ZB4BS864","OVLÁDACIA HLAVICA NÚDZOVÉHO ZASTAVENIA",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3389110801828",{"v":9.2,"d":"9.20"},{"v":7,"d":"7.00"},{"v":7.4,"d":"7.40"},{"v":88,"d":"88.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS864","červená Ø60 ovl.hlav.stisk.nouz.zastav.Ø22 vypnuto a s aretací \"uvolnit klíčem\"",0]
["ZB4BS844S45","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA, ",10,"ks",{"v":22.565749499999995,"d":"22.566"},"3606480623691",{"v":4.3,"d":"4.30"},{"v":9,"d":"9.00"},{"v":5.3,"d":"5.30"},{"v":44,"d":"44.00"},"CZ","7907000090","https://www.se.com/sk/sk/product/ZB4BS844S45","ovládacia hlavica núdzového zastavenia-hríbová Ø40 mm hlavica Ø23",""]
["ZB4BS8447","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110858754",{"v":9.3,"d":"9.30"},{"v":4.5,"d":"4.50"},{"v":5.6,"d":"5.60"},{"v":75,"d":"75.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS8447","červená Ø40 ovl.hlav.stisk.núdz.zastav.Ø22 vypnutá a s aret.\"uvolniť otočením\"",0]
["ZB4BS84430","OVLÁDACIA HLAVICA S HRÍBOVÝM TLAČ., 22MM",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3606480502842",{"v":8.6,"d":"8.60"},{"v":4.4,"d":"4.40"},{"v":5.2,"d":"5.20"},{"v":75,"d":"75.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS84430","ovládací hlavice s hřibovým knoflíkem s aretací, 22 mm",0]
["ZB4BS844","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":19.674112499999996,"d":"19.674"},"3389110888867",{"v":9.2,"d":"9.20"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":75,"d":"75.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS844","okrúhla hlavica pre tlačidlo Ø 22 – uvoľ. otočením – s hríbom Ø 40 mm – červená",0]
["ZB4BS8347","OVLÁDACIA HLAVICA NUDZOVÉHO ZASTAVENIA",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110856545",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":68,"d":"68.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS8347","červená Ø30 ovl.hlav.stisk.núdz.zastav.Ø22 vypnutá a s aret.\"uvolniť otočením\"",0]
["ZB4BS834","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":23.334412499999996,"d":"23.334"},"3389110888850",{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":72,"d":"72.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS834","okrúhla hlavica pre tlačidlo Ø 22 – uvoľ. otočením – s hríbom Ø 30 mm – červená",0]
["ZB4BS55","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":22.876875,"d":"22.877"},"3389110894974",{"v":4.5,"d":"4.50"},{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":75,"d":"75.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS55","okrúhla hlavica pre tlačidlo Ø 22 – uvoľ. otočením – s hríbom Ø 40 mm – žltá",0]
["ZB4BS52","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110888713",{"v":8.8,"d":"8.80"},{"v":4.5,"d":"4.50"},{"v":5.3,"d":"5.30"},{"v":70,"d":"70.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS52","okrúhla hlavica pre tlačidlo Ø 22 – uvoľ. otočením – s hríbom Ø 40 mm – čierna",0]
["ZB4BS42","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110888690",{"v":4.5,"d":"4.50"},{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":72,"d":"72.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS42","čierna Ø30 hlavica s hríbovým tlačítkom Ø22 s aretáciou \"uvolniť otočením\"",0]
["ZB4BS15","OVL HLAVICA NUDZOVÉHO ZASTAVENIA, ODBLOK",1,"ks",{"v":31.551785999999993,"d":"31.552"},"3606480625046",{"v":8.8,"d":"8.80"},{"v":4.5,"d":"4.50"},{"v":5.4,"d":"5.40"},{"v":102.8,"d":"102.80"},"CZ","7907000090","https://www.se.com/sk/sk/product/ZB4BS15","žltá hribová hlavica Ø40 mm núdzové zastavenie Ø22 uvoľnenie kľúčom 455E",""]
["ZB4BS12","EMERGENCY STOP OP. HEAD",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3389110888812",{"v":9,"d":"9.00"},{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":70,"d":"70.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BS12","okrúhla hlavica pre tlačidlo Ø 22 – uvoľňovač kláves – s hríbom Ø 40 mm – čierna",0]
["ZB4BR5","Ovládacia hlavica s hríbom",1,"ks",{"v":19.674112499999996,"d":"19.674"},"3389110888515",{"v":7.2,"d":"7.20"},{"v":9.4,"d":"9.40"},{"v":7.2,"d":"7.20"},{"v":87,"d":"87.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BR5","žltá Ø60 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB4BR4","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":19.216575,"d":"19.217"},"3389110888508",{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":90,"d":"90.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BR4","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – s hríbom Ø 60 mm – červená",0]
["ZB4BR316","OVL. HLAVICA STLÁČACIA S HRÍBOM",1,"ks",{"v":36.602999999999994,"d":"36.603"},"3389110066166",{"v":7.2,"d":"7.20"},{"v":9,"d":"9.00"},{"v":7.2,"d":"7.20"},{"v":72,"d":"72.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BR316","polguľová hlavica pre tlačidlo Ø 22 – vratná pružina – s hríbom Ø 60 mm – zelená",0]
["ZB4BR3","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":19.216575,"d":"19.217"},"3389110888492",{"v":7.2,"d":"7.20"},{"v":9,"d":"9.00"},{"v":7.2,"d":"7.20"},{"v":90,"d":"90.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BR3","zelená Ø40 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB4BR216","OVL. HLAVICA STLÁČACIA S HRÍBOM",1,"ks",{"v":28.367324999999997,"d":"28.367"},"3389110066142",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":70,"d":"70.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BR216","polguľová hlavica pre tlačidlo Ø 22 – vratná pružina – s hríbom Ø 60 mm – čierna",0]
["ZB4BR2","MUSHROOMM PUSH BUT HEAD",1,"ks",{"v":19.216575,"d":"19.217"},"3389110888485",{"v":9.1,"d":"9.10"},{"v":7.5,"d":"7.50"},{"v":7.1,"d":"7.10"},{"v":88,"d":"88.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BR2","čierna Ø40 presvet. hlavica s hríbovým tlačítkom Ø22 s aretáciou pre integ. LED",0]
["ZB4BP683","OVLÁDACIE TLAČIDLO S OCHRANNOU KRYTKOU",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3389110110166",{"v":8.7,"d":"8.70"},{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP683","modrá zapust. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BP68","PUSHBUTTON OPERATOR HEAD",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110888225",{"v":8.7,"d":"8.70"},{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":32.5,"d":"32.50"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP68","modrá zapuš. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BP6","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110888027",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP6","modrá ovl. hlavica stískacia s presahom Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB4BP5","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110888010",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP5","žltá ovl. hlavica stískacia s presahom Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB4BP4837","OVLÁDACIA HLAVICA",1,"ks",{"v":21.046725,"d":"21.047"},"3389110222241",{"v":8.7,"d":"8.70"},{"v":3.4,"d":"3.40"},{"v":5.3,"d":"5.30"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP4837","červená zapust. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BP483","OVLÁDACIA HLAVICA",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110109917",{"v":8.7,"d":"8.70"},{"v":5.2,"d":"5.20"},{"v":5.4,"d":"5.40"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP483","červená zapust. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BP48","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110888058",{"v":3.2,"d":"3.20"},{"v":8.2,"d":"8.20"},{"v":5.2,"d":"5.20"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP48","Head for non illuminated push button, Harmony XB4, red flush, 22mm, spring return, clear boot, unmarked",0]
["ZB4BP4","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":10.065825,"d":"10.066"},"3389110888003",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":31.8,"d":"31.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP4","okrúhla hlavica pre tlač. Ø 22 – vystupujúca – červená – krytá (čistý silikón)",0]
["ZB4BP3S","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":9.104996249999997,"d":"9.105"},"3389110999303",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28.6,"d":"28.60"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP3S","zelená zapuš. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BP3837","OVLÁDACIA HLAVICA",1,"ks",{"v":21.046725,"d":"21.047"},"3389110222234",{"v":8.7,"d":"8.70"},{"v":3.3,"d":"3.30"},{"v":5.2,"d":"5.20"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP3837","zelená zapust. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BP383","OVLÁDACIA HLAVICA",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110109863",{"v":8.7,"d":"8.70"},{"v":3.3,"d":"3.30"},{"v":5.3,"d":"5.30"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP383","zelená zapust. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BP38","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":12.81105,"d":"12.811"},"3389110888034",{"v":9.1,"d":"9.10"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":33,"d":"33.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP38","zelená zapustená hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BP3","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":10.065825,"d":"10.066"},"3389110887990",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":31,"d":"31.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP3","okrúhla hlavica pre tlačidlo Ø 22 – vystupujúca – zelená – krytá (čistý silikón)",0]
["ZB4BP2","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":10.065825,"d":"10.066"},"3389110887983",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP2","okrúhla hlavica pre tlačidlo Ø 22 – vystupujúca – čierna – krytá (čistý silikón)",0]
["ZB4BP1","OVL. HLAVICA S KRYTKOU",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110887976",{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":5.2,"d":"5.20"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BP1","okrúhla hlavica pre tlačidlo Ø 22 – vystupujúca – biela – krytá (čistý silikón)",0]
["ZB4BL7341","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA IP66",1,"ks",{"v":17.386425,"d":"17.386"},"3389119043861",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":57,"d":"57.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL7341","zelená lícujúca/červená lícujúca ovl. hlavica dvojtlač. Ø22 s popisom",0]
["ZB4BL7340","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA IP66",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389119043854",{"v":2.8,"d":"2.80"},{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL7340","zelená lícujúca/červená lícujúca ovl. hlavica dvojtlač. Ø22 neoznačená",0]
["ZB4BL6","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":7.137584999999999,"d":"7.138"},"3389110887822",{"v":4.6,"d":"4.60"},{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":29.4,"d":"29.40"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL6","modrá ovl. hlavica stláčacia s presahom Ø22 \"stlač-stlač\" neoznačená",0]
["ZB4BL5","OVL. HLAVICA STLÁČACIA S PRESAHOM",1,"ks",{"v":7.137584999999999,"d":"7.138"},"3389110887808",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL5","žltá ovl. hlavice stláčacia s presahom. Ø22 s návratom neoznačená",0]
["ZB4BL434","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":8.418689999999998,"d":"8.419"},"3389110887853",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29.5,"d":"29.50"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL434","červená ovl. hlavica stláčacia s presahom Ø22 s návratom \"STOP\"",0]
["ZB4BL432","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":8.418689999999998,"d":"8.419"},"3389110887839",{"v":4.6,"d":"4.60"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL432","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – vystupujúca – červená – O",0]
["ZB4BL4","OVL. HLAVICA STLÁČACIA S PRESAHOM",1,"ks",{"v":7.2748462499999995,"d":"7.275"},"3389110889970",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL4","okrúhla hlav. pre tlač. Ø 22 – vr. pružina – vystupujúca – červ. – bez označ.",0]
["ZB4BL3","OVL. HLAVICA STLÁČACIA S PRESAHOM",1,"ks",{"v":7.137584999999999,"d":"7.138"},"3389110887792",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL3","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – vystupujúca – zelená – bez označ.",0]
["ZB4BL234","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":7.878795749999998,"d":"7.879"},"3389110887891",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL234","čierna ovl. hlavica stláčacia s presahom Ø22 s návratom \"STOP\"",0]
["ZB4BL232","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":8.738966249999999,"d":"8.739"},"3389110887877",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":4.9,"d":"4.90"},{"v":29.4,"d":"29.40"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL232","čierna ovl. hlavica stis. s presah. Ø22 s návratom \"O\"",0]
["ZB4BL2","OVL. HLAVICA STLÁČACIA S PRESAHOM",1,"ks",{"v":7.137584999999999,"d":"7.138"},"3389110887761",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL2","čierna ovl. hlavice stláčacia s presahom. Ø22 s návratom neoznačená",0]
["ZB4BL1","OVL. HLAVICA STLÁČACIA S PRESAHOM",1,"ks",{"v":7.137584999999999,"d":"7.138"},"3389110887754",{"v":3,"d":"3.00"},{"v":3.6,"d":"3.60"},{"v":5.2,"d":"5.20"},{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BL1","biela ovl. hlavice stláčacia s presahom. Ø22 s návratom neoznačená",0]
["ZB4BK1883","Ovl. otočná presvetlená hlavica, žltá,3p",1,"ks",{"v":21.046725,"d":"21.047"},"3606481206220",{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1883","Ovládacia otočná presvetlená hlavica, žltá, 3 polohy",0]
["ZB4BK1863","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891065",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1863","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – modrá",0]
["ZB4BK1853","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891058",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1853","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – žltá",0]
["ZB4BK1843","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891041",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1843","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – červená",0]
["ZB4BK1833","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110891034",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1833","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB4BK1813","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891027",5.59,5.59,{"v":3.3,"d":"3.30"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1813","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB4BK1763","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110891119",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1763","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – modrá",0]
["ZB4BK1753","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891102",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1753","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – žltá",0]
["ZB4BK1743","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891096",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1743","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – červená",0]
["ZB4BK1733","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891089",{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":5.2,"d":"5.20"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1733","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB4BK1713","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891072",{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":5.2,"d":"5.20"},{"v":42,"d":"42.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1713","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB4BK1563","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891010",{"v":5.9,"d":"5.90"},{"v":3.6,"d":"3.60"},{"v":5.4,"d":"5.40"},{"v":41.7,"d":"41.70"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1563","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – modrá",0]
["ZB4BK15537","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110841039",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK15537","oranžová presvetlená ovl. hlavica otočná Ø22 3-polohy s návratom",0]
["ZB4BK1553","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110891003",{"v":5.5,"d":"5.50"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1553","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – žltá",0]
["ZB4BK1543","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110890952",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1543","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – červená",0]
["ZB4BK15337","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":30.197474999999997,"d":"30.197"},"3389110841008",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK15337","ovládacia hlavica otočná presvet., 3 p., návrat. do stredu, zelená",0]
["ZB4BK1533","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110890884",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1533","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB4BK15137","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":28.824862499999995,"d":"28.825"},"3389110840995",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK15137","biela presvetlená ovládateľná otočná hlavica Ø22 3-polohy s návratom",0]
["ZB4BK1513","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110890877",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1513","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB4BK1463","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":19.216575,"d":"19.217"},"3389110894967",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":37,"d":"37.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1463","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – modrá",0]
["ZB4BK1453","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":19.216575,"d":"19.217"},"3389110894950",{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":5.2,"d":"5.20"},{"v":37,"d":"37.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1453","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – žltá",0]
["ZB4BK1443","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":19.216575,"d":"19.217"},"3389110890495",{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":5.2,"d":"5.20"},{"v":37,"d":"37.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1443","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – červená",0]
["ZB4BK1433","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":19.216575,"d":"19.217"},"3389110890488",{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":5.2,"d":"5.20"},{"v":37,"d":"37.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1433","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – zelená",0]
["ZB4BK1413","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3389110890471",{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":5.2,"d":"5.20"},{"v":37,"d":"37.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1413","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – biela",0]
["ZB4BK1363","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3389110890860",{"v":5.3,"d":"5.30"},{"v":3.5,"d":"3.50"},{"v":5.3,"d":"5.30"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1363","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – modrá",0]
["ZB4BK1353","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3389110890853",{"v":3.3,"d":"3.30"},{"v":5,"d":"5.00"},{"v":5.2,"d":"5.20"},{"v":42,"d":"42.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1353","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – žltá",0]
["ZB4BK1343","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3389110890747",{"v":3.3,"d":"3.30"},{"v":5,"d":"5.00"},{"v":5.2,"d":"5.20"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1343","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – červená",0]
["ZB4BK13337","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":30.197474999999997,"d":"30.197"},"3389110840926",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK13337","zelená presvetl. ovl. hlavica otočná Ø22 3-polohy pevné",0]
["ZB4BK1333","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3389110890723",{"v":5.4,"d":"5.40"},{"v":3.6,"d":"3.60"},{"v":5.3,"d":"5.30"},{"v":41.2,"d":"41.20"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1333","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – zelená",0]
["ZB4BK13137","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110840919",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK13137","Head for illuminated selector switch, Harmony XB4, metal, white handle, 22mm, universal LED, 3 positions, stay put",0]
["ZB4BK1313","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3389110890709",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":5,"d":"5.00"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1313","hlavica osvetleného voliaceho spínača – 3 polohy – Ø 22 – biela",0]
["ZB4BK1263","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":20.589187499999998,"d":"20.589"},"3389110890464",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":42,"d":"42.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1263","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – modrá",0]
["ZB4BK1253","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110890457",{"v":5.4,"d":"5.40"},{"v":3.6,"d":"3.60"},{"v":5.3,"d":"5.30"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1253","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – žltá",0]
["ZB4BK1243","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110890440",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.2,"d":"5.20"},{"v":41.4,"d":"41.40"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1243","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – červená",0]
["ZB4BK1233","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110890433",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.3,"d":"5.30"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1233","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – zelená",0]
["ZB4BK1213","OVL. HLAVICA OTOČNÁ PRESVETLENÁ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110890426",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.3,"d":"5.30"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BK1213","hlavica osvetleného voliaceho spínača – 2 polohy – Ø 22 – biela",0]
["ZB4BJ891","OVL. HLAVICA OTOČNÁ 3 POL. UZAMYKATEĽNÁ",1,"ks",{"v":54.9045,"d":"54.905"},"3389110173703",{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"v":3.1,"d":"3.10"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ891","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BJ8","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110889086",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.3,"d":"5.30"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ8","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BJ7","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110889109",{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":45,"d":"45.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ7","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BJ593","OVL. HLAVICA OTOČNÁ 3 POL. UZAMYKATEĽNÁ",1,"ks",{"v":56.734649999999995,"d":"56.735"},"3389110173680",{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"v":3.1,"d":"3.10"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ593","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BJ5","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110889079",{"v":5.4,"d":"5.40"},{"v":3.6,"d":"3.60"},{"v":5.4,"d":"5.40"},{"v":45.2,"d":"45.20"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ5","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BJ4","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110889048",{"v":5.4,"d":"5.40"},{"v":3.3,"d":"3.30"},{"v":5.2,"d":"5.20"},{"v":41,"d":"41.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ4","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BJ397","OVL. HLAVICA OTOČNÁ 3 POL. UZAMYKATEĽNÁ",1,"ks",{"v":54.9045,"d":"54.905"},"3389110173642",{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ397","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BJ393","OVL. HLAVICA OTOČNÁ 3 POL. UZAMYKATEĽNÁ",1,"ks",{"v":56.734649999999995,"d":"56.735"},"3389110173550",{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"v":3.1,"d":"3.10"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ393","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BJ3","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110889062",{"v":5.5,"d":"5.50"},{"v":3.6,"d":"3.60"},{"v":5.4,"d":"5.40"},{"v":45.4,"d":"45.40"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ3","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BJ294","OVL. HLAVICA OTOČNÁ 2 POL. UZAMYKATEĽNÁ",1,"ks",{"v":50.329125,"d":"50.329"},"3389110173390",{"v":4.6,"d":"4.60"},{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":51,"d":"51.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ294","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BJ292","OVL. HLAVICA OTOČNÁ 2 POL. UZAMYKATEĽNÁ",1,"ks",{"v":50.329125,"d":"50.329"},"3389110173376",{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"v":3.1,"d":"3.10"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ292","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BJ291","OVL. HLAVICA OTOČNÁ 2 POL. UZAMYKATEĽNÁ",1,"ks",{"v":52.159274999999994,"d":"52.159"},"3389110173338",{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":4.4,"d":"4.40"},{"v":52,"d":"52.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ291","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BJ27","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":17.386425,"d":"17.386"},"3389110827590",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ27","čierna ovl. hlavica otočná Ø22 2-polohy pevné",0]
["ZB4BJ2","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110889024",{"v":5.5,"d":"5.50"},{"v":3.6,"d":"3.60"},{"v":5.2,"d":"5.20"},{"v":45.2,"d":"45.20"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BJ2","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BH63","ILLUMINATED PUSH / PUSH H",1,"ks",{"v":22.876875,"d":"22.877"},"3389110890419",{"v":4.8,"d":"4.80"},{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":29.4,"d":"29.40"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH63","modrá ovl. Hlavica presvet. stis. s presahomØ22 \"Stiskni-stiskni\" pre integ.LED",0]
["ZB4BH2","Ovládací hlavica, černá",1,"ks",{"v":19.811373749999998,"d":"19.811"},"3389110888553",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.8,"d":"4.80"},{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH2","čierna ovl. hlavica stis. s presah. Ø22 \"Stiskni-stiskni\" neoznačená",""]
["ZB4BH063","OVL. HLAVICA \"STLAČ-STLAČ\"",1,"ks",{"v":19.216575,"d":"19.217"},"3389110122732",{"v":7.2,"d":"7.20"},{"v":3.2,"d":"3.20"},{"v":5,"d":"5.00"},{"v":25,"d":"25.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH063","modrá ovl. hlavica stis. presvet. - lícujúca Ø22 \"Stiskni-stiskni\" pre integ.LED",0]
["ZB4BH06","OVL. HLAVICA STISKNI-STISKNI",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110122725",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH06","modrá zapustená hlava tlačítka Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB4BH053","OVL. HLAVICA STISKNI-STISKNI",1,"ks",{"v":19.216575,"d":"19.217"},"3389110122718",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH053","hlavica osvetleného tlačidla – Ø 22 – žltá",0]
["ZB4BH05","OVL. HLAVICA STISKNI-STISKNI",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110122701",{"v":4.4,"d":"4.40"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH05","žltá zapustená hlava tlačítka Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB4BH043","OVL. HLAVICA STISKNI-STISKNI",1,"ks",{"v":19.216575,"d":"19.217"},"3389110122671",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH043","hlavica osvetleného tlačidla – Ø 22 – červená",0]
["ZB4BH04","Ovládacia hlavica stlač - stlač, červen.",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110122657",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH04","červená zapuš. hlava tlačítka Ø22 \"stiskni-stiskni\" neoznačená",0]
["ZB4BH033","OVL. HLAVICA STISKNI-STISKNI",1,"ks",{"v":19.216575,"d":"19.217"},"3389110122633",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH033","hlavica osvetleného tlačidla – Ø 22 – zelená",0]
["ZB4BH03","Ovládací hlavica stiskni - stiskni",1,"ks",{"v":11.227970249999998,"d":"11.228"},"3389110122619",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH03","zelená zapuš. hlava tlačítka Ø22 \"stiskni-stiskni\" neoznačená",""]
["ZB4BH02","PUSHBUTTON OPERATOR HEAD",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110122602",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH02","čierna zapustená hlava tlačítka Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB4BH013","OVL. HLAVICA STISKNI-STISKNI",1,"ks",{"v":19.216575,"d":"19.217"},"3389110122541",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":26,"d":"26.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH013","hlavica osvetleného tlačidla – Ø 22 – biela",0]
["ZB4BH01","OVL. HLAVICA STISKNI-STISKNI",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110122527",{"v":4.4,"d":"4.40"},{"v":3.2,"d":"3.20"},{"v":3.8,"d":"3.80"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BH01","biela lícujúca ovládateľná hlavica stískacia Ø22 \"Stiskni-stiskni\" neoznačený",0]
["ZB4BG9","Ovl. hlavica se zamkom, 3 polohy",1,"ks",{"v":44.838674999999995,"d":"44.839"},"3389110889307",{"v":9,"d":"9.00"},{"v":3.4,"d":"3.40"},{"v":5.5,"d":"5.50"},{"v":102,"d":"102.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG9","ovl. hlavica otočná Ø22 3-polohy pevné Ronis 455",0]
["ZB4BG8","OVL. HLAVICA OTOČNÁ SO ZÁMKOM-3 POZÍCIE",1,"ks",{"v":36.602999999999994,"d":"36.603"},"3389110889291",{"v":9.1,"d":"9.10"},{"v":3.4,"d":"3.40"},{"v":5.5,"d":"5.50"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG8","ovládateľná otočná hlavica Ø22 3-polohy s návratom Ronis 455",0]
["ZB4BG7K","OVL. HLAVICA OTOČNÁ SO ZÁMKOM 3113",1,"ks",{"v":53.53188749999999,"d":"53.532"},"3389110846232",{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":70,"d":"70.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG7K","Head for key selector switch, Harmony XB4, Ø22 mm 3 position spring return 4 multichips",0]
["ZB4BG712","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":53.53188749999999,"d":"53.532"},"3389110122299",{"v":8.7,"d":"8.70"},{"v":5.3,"d":"5.30"},{"v":3.4,"d":"3.40"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG712","ovládateľná otočná hlavica Ø22 3-polohy s návratom Ronis 421E",0]
["ZB4BG7","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110889284",{"v":9.1,"d":"9.10"},{"v":3.6,"d":"3.60"},{"v":5.5,"d":"5.50"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG7","okrúhla hlavica pre voliaci spínač – Ø 22 – 3 polohy – Ronis 455 – stredná",0]
["ZB4BG6TEC10","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":75.03614999999999,"d":"75.036"},"3389110058208",{"v":3,"d":"3.00"},{"v":5.8,"d":"5.80"},{"v":3,"d":"3.00"},{"v":130,"d":"130.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB4BG6TEC10","ovládateľná otočná hlavica Ø22 2-polohy s návratom CES TEC10",0]
["ZB4BG620","OVL. HLAVICA OTOČNÁ SO ZÁMKOM 3131A",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3389110122046",8.64,5.33,3.56,{"v":100,"d":"100.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG620","ovládateľná otočná hlavica Ø22 2-polohy s návratom Ronis 3131A",0]
["ZB4BG614","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3389110122039",{"v":3.3,"d":"3.30"},{"v":8.6,"d":"8.60"},{"v":5.2,"d":"5.20"},{"v":69,"d":"69.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG614","ovl. hlavica otočná Ø22 2-polohy s návratom Ronis 520E",0]
["ZB4BG612","OVL. HLAVICA OTOČNÁ SO ZÁMKOM 421E",1,"ks",{"v":43.92359999999999,"d":"43.924"},"3389110122022",{"v":9.1,"d":"9.10"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG612","ovládateľná otočná hlavica Ø22 2-polohy s návratom Ronis 421E",0]
["ZB4BG610","OVL. HLAVICA OTOCNÁ SO ZÁMKOM 458A",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3389110122015",{"v":8.636,"d":"8.64"},{"v":5.334,"d":"5.33"},{"v":3.556,"d":"3.56"},{"v":104.327,"d":"104.33"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG610","ovládateľná otočná hlavica Ø22 2-polohy s návratom Ronis 458A",0]
["ZB4BG6","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110889246",{"v":9.1,"d":"9.10"},{"v":3.6,"d":"3.60"},{"v":5.4,"d":"5.40"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG6","okrúhla hlavica pre voliaci spínač – Ø 22 – 2 polohy – Ronis 455 – ľavá",0]
["ZB4BG5","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110889239",{"v":3.3,"d":"3.30"},{"v":8.8,"d":"8.80"},{"v":5.2,"d":"5.20"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG5","ovládateľná otočná hlavica Ø22 3-polohy pevné Ronis 455",0]
["ZB4BG4K","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":42.55098749999999,"d":"42.551"},"3389110843903",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":70,"d":"70.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG4K","ovládateľná otočná hlavica Ø22 2-polohy pevné 4 multičipy",0]
["ZB4BG4E7","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":160.138125,"d":"160.138"},"3389110965902",{"v":3,"d":"3.00"},{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":130,"d":"130.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG4E7","ovl. hlavica s kľúčom",0]
["ZB4BG420","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":45.296212499999996,"d":"45.296"},"3389110121902",8.64,5.33,3.56,{"v":100,"d":"100.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG420","ovládateľná otočná hlavica Ø22 2-polohy pevné Ronis 3131A",0]
["ZB4BG414","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":45.296212499999996,"d":"45.296"},"3389110121896",8.64,5.33,3.56,{"v":100,"d":"100.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG414","ovládateľná otočná hlavica Ø22 2-polohy pevné Ronis 520E",0]
["ZB4BG412","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":42.55098749999999,"d":"42.551"},"3389110121889",{"v":9.2,"d":"9.20"},{"v":3.6,"d":"3.60"},{"v":5.4,"d":"5.40"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG412","okrúhla hlavica pre voliaci sp. – Ø 22 – 2 polohy – Ronis 421E – akákoľvek pol.",0]
["ZB4BG410","OVL.HLAVICA OTOČNÁ SO ZÁMKOM, 2 POLOHY",1,"ks",{"v":42.55098749999999,"d":"42.551"},"3389110121872",{"v":8.6,"d":"8.60"},{"v":3.3,"d":"3.30"},{"v":5.2,"d":"5.20"},{"v":98,"d":"98.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG410","ovládateľná otočná hlavica Ø22 2-polohy pevné Ronis 458A",0]
["ZB4BG4","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110889222",{"v":9.1,"d":"9.10"},{"v":3.6,"d":"3.60"},{"v":5.6,"d":"5.60"},{"v":102,"d":"102.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG4","okrúhla hlavica pre voliaci sp. – Ø 22 – 2 polohy – Ronis 455 – akákoľvek poloha",0]
["ZB4BG312","OVLÁDACIA HLAVICA S KĽÚČOM",1,"ks",{"v":45.296212499999996,"d":"45.296"},"3389110121803",{"v":3.3,"d":"3.30"},{"v":8.7,"d":"8.70"},{"v":5.2,"d":"5.20"},{"v":105,"d":"105.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG312","ovl. hlavica otočná Ø22 3-poloha pevná Ronis 421E",0]
["ZB4BG310","KEY SELECTOR OPERATING HE",1,"ks",{"v":43.46606249999999,"d":"43.466"},"3389110121469",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG310","ovl. hlavica otočná Ø22 3-polohy pevné Ronis 458A",0]
["ZB4BG3","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":42.55098749999999,"d":"42.551"},"3389110889277",{"v":9.2,"d":"9.20"},{"v":4,"d":"4.00"},{"v":5.4,"d":"5.40"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG3","okrúhla hlavica pre voliaci spínač – Ø 22 – 3 polohy – Ronis 455 – stredná",0]
["ZB4BG2TEC10","OVL.HLAVICA SE ZÁMKOM",1,"ks",{"v":102.4884,"d":"102.488"},"3389110967517",{"v":8.7,"d":"8.70"},{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":162,"d":"162.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG2TEC10","ovl. hlavica otočná Ø22 2-polohy pevné CES TEC10",""]
["ZB4BG27","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":36.145462499999994,"d":"36.145"},"3389110828313",{"v":8.6,"d":"8.60"},{"v":3.5,"d":"3.50"},{"v":5.2,"d":"5.20"},{"v":102,"d":"102.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG27","ovl. hlavica otočná Ø22 2-polohy pevné Ronis 455",0]
["ZB4BG220","OVLÁDACIA HLAVICA",1,"ks",{"v":40.720837499999995,"d":"40.721"},"3389110121384",{"v":3.3,"d":"3.30"},{"v":8.6,"d":"8.60"},{"v":5.2,"d":"5.20"},{"v":104,"d":"104.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG220","ovl. hlavica otočná Ø22 2-polohy pevné Ronis 455",0]
["ZB4BG214","OVL. HLAVICA OTOČNÁ SO ZÁMKOM E520",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3389110121377",{"v":3.3,"d":"3.30"},{"v":8.6,"d":"8.60"},{"v":5.2,"d":"5.20"},{"v":105,"d":"105.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG214","ovládateľná otočná hlavica Ø22 2-polohy pevné Ronis 520E",0]
["ZB4BG212","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":52.616812499999995,"d":"52.617"},"3389110121360",{"v":9.2,"d":"9.20"},{"v":3.6,"d":"3.60"},{"v":5.5,"d":"5.50"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG212","okrúhla hlavica pre voliaci spínač – Ø 22 – 2 polohy – Ronis 421E – ľavá",0]
["ZB4BG210","OVL. HLAVICA OTOČNÁ SO ZÁMKOM 2 POZÍCIE",1,"ks",{"v":41.178374999999996,"d":"41.178"},"3389110121353",{"v":9.1,"d":"9.10"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":104,"d":"104.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG210","ovládateľná otočná hlavica Ø22 2-polohy pevné Ronis 458A",0]
["ZB4BG2","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110889215",{"v":9.1,"d":"9.10"},{"v":3.8,"d":"3.80"},{"v":5.4,"d":"5.40"},{"v":104,"d":"104.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG2","okrúhla hlavica pre voliaci spínač – Ø 22 – 2 polohy – Ronis 455 – ľavá",0]
["ZB4BG1","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":37.0605375,"d":"37.061"},"3389110889260",{"v":3.3,"d":"3.30"},{"v":8.6,"d":"8.60"},{"v":5.2,"d":"5.20"},{"v":98,"d":"98.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG1","ovládateľná otočná hlavica Ø22 3-polohy s návratom Ronis 455",0]
["ZB4BG09","Ovládacia hlavica otočná so zámkom",1,"ks",{"v":45.75375,"d":"45.754"},"3389110889314",{"v":8.6,"d":"8.60"},{"v":3.5,"d":"3.50"},{"v":5.2,"d":"5.20"},{"v":69,"d":"69.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG09","ovl. hlavica otočná Ø22 3-polohy pevné Ronis 455",0]
["ZB4BG08","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":42.55098749999999,"d":"42.551"},"3389110889321",{"v":9.2,"d":"9.20"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":103,"d":"103.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG08","okrúhla hlavica pre voliaci spínač – Ø 22 – 3 polohy – Ronis 455 – ľavá",0]
["ZB4BG03","Ovládacia hlavica s klíčom",1,"ks",{"v":44.838674999999995,"d":"44.839"},"3389110362701",9.14,{"v":3.3,"d":"3.30"},5.33,{"v":100,"d":"100.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG03","ovl. hlavica otočná Ø22 3-polohy pevné Ronis 455",0]
["ZB4BG020","OVLÁDAČIA HLAVICA KOV",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110121025",8.89,5.33,3.56,{"v":100,"d":"100.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG020","ovl. hlavica otočná Ø22 3-polohy pevné Ronis 3131A",0]
["ZB4BG02","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":32.485162499999994,"d":"32.485"},"3389110368611",{"v":5.2,"d":"5.20"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":104,"d":"104.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG02","ovládateľná otočná hlavica Ø22 2-polohy pevné Ronis 455",0]
["ZB4BG012","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":69.0881625,"d":"69.088"},"3389110121001",{"v":8.636,"d":"8.64"},{"v":5.334,"d":"5.33"},{"v":3.556,"d":"3.56"},{"v":99.791,"d":"99.79"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG012","ovládateľná otočná hlavica Ø22 3-polohy pevné Ronis 421E",0]
["ZB4BG010","Ovládacia hlavica s kľúčom",1,"ks",{"v":47.1263625,"d":"47.126"},"3389110120981",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":69,"d":"69.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG010","ovládacia halvica so zámkom, Ø22 3 polohy s návratom Ronis 458A",0]
["ZB4BG0","OVL. HLAVICA OTOČNÁ SO ZÁMKOM",1,"ks",{"v":41.178374999999996,"d":"41.178"},"3389110889253",{"v":3.4,"d":"3.40"},{"v":8.8,"d":"8.80"},{"v":5.2,"d":"5.20"},{"v":102,"d":"102.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BG0","okrúhla hlavica pre voliaci sp. – Ø 22 – 3 polohy – Ronis 455 – akákoľvek poloha",0]
["ZB4BD922","OVL. HLAVICA PRE POTENCIOMETER",1,"ks",{"v":50.7866625,"d":"50.787"},"3389110896886",{"v":5.5,"d":"5.50"},{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":74,"d":"74.00"},"FR","8533900000","https://www.se.com/sk/sk/product/ZB4BD922","vrúbkovaná hlavica potenciometra – Ø 22 – čierna – 6,35 mm hriadeľ",0]
["ZB4BD912","HLAVICA PRE POTENCIOMETER",1,"ks",{"v":50.7866625,"d":"50.787"},"3389110896879",{"v":5.5,"d":"5.50"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":80,"d":"80.00"},"FR","8533900000","https://www.se.com/sk/sk/product/ZB4BD912","vrúbkovaná hlavica potenciometra – Ø 22 – čierna – 6 mm hriadeľ",0]
["ZB4BD8","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110889000",{"v":5.6,"d":"5.60"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD8","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BD7","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110889017",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD7","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BD59","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110889178",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.5,"d":"4.50"},{"v":48,"d":"48.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD59","vrúbkovaná hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BD5","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110888973",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.3,"d":"5.30"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD5","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BD47","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3389110827026",{"v":5.4,"d":"5.40"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":44,"d":"44.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB4BD47","čierna ovl. hlavica otočná Ø22 2-polohy s návratom",0]
["ZB4BD4","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110888959",{"v":5.5,"d":"5.50"},{"v":3.6,"d":"3.60"},{"v":5.4,"d":"5.40"},{"v":51,"d":"51.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD4","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BD37","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389110827255",{"v":5.2,"d":"5.20"},{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD37","čierna ovl. hlavica otočná Ø22 3-polohy pevné",0]
["ZB4BD3","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110888966",{"v":5.3,"d":"5.30"},{"v":3.6,"d":"3.60"},{"v":5.3,"d":"5.30"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD3","hlavica voliaceho spínača – 3 polohy – Ø 22 – čierna",0]
["ZB4BD29","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":12.81105,"d":"12.811"},"3389110889123",{"v":5,"d":"5.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":43,"d":"43.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD29","vrúbkovaná hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BD28","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":18.301499999999997,"d":"18.302"},"3389110889352",{"v":5.4,"d":"5.40"},{"v":3.6,"d":"3.60"},{"v":4.7,"d":"4.70"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD28","čierna ovládateľná otočná hlavica Ø22 2-polohy pevné",0]
["ZB4BD27","SELECTOR OPERATING HEAD",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110826920",{"v":5.4,"d":"5.40"},{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":43.8,"d":"43.80"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD27","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BD205","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110801651",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB4BD205","žltá ovládateľná otočná hlavica Ø22 2-polohy pevné",0]
["ZB4BD204","OVL. HLAVICA PRE POTENCIOMETER",1,"ks",{"v":16.9288875,"d":"16.929"},"3389110801590",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD204","červená ovl. hlavica otočná Ø22 2-polohy pevné",0]
["ZB4BD203","OVLÁDACIA HLAVICA OTOČNÁ",1,"ks",{"v":13.726125,"d":"13.726"},"3389110801514",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD203","zelená ovládateľná otočná hlavica Ø22 2-polohy pevné",0]
["ZB4BD201","Ovl. hlavica otočná, 2 polohy",1,"ks",{"v":16.9288875,"d":"16.929"},"3389110801453",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":40,"d":"40.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB4BD201","biela ovl. hlavica otočná Ø22 2-polohy pevné",0]
["ZB4BD2","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110888935",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BD2","hlavica voliaceho spínača – 2 polohy – Ø 22 – čierna",0]
["ZB4BC680","OVL. HLAVICA ROBUSTNÁ MODRÁ",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3606480444685",{"v":3.7,"d":"3.70"},{"v":3.8,"d":"3.80"},{"v":3.7,"d":"3.70"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BC680","hlava tlačítka pre nepriaznivé prostredie - tmavě modrá - bez ozn.",0]
["ZB4BC64","MUSHROOMM PUSH BUT HEAD",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110888423",{"v":8.8,"d":"8.80"},{"v":4.3,"d":"4.30"},{"v":5.4,"d":"5.40"},{"v":75,"d":"75.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC64","modrá Ø30 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB4BC6","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110888478",{"v":8.6,"d":"8.60"},{"v":4.2,"d":"4.20"},{"v":5,"d":"5.00"},{"v":77,"d":"77.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC6","modrá Ø40 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB4BC580","OVL. HLAVICA ROBUSTNÁ ŽLTÁ",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3606480444654",{"v":3.7,"d":"3.70"},3.76,{"v":3.7,"d":"3.70"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BC580","hlava tlačítka pre nepriaznivé prostredie - žlutá - bez ozn.",0]
["ZB4BC54","MUSHROOMM PUSH BUT HEAD",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110888416",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":74,"d":"74.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC54","žltá Ø30 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB4BC5","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":13.726125,"d":"13.726"},"3389110888461",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":77,"d":"77.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC5","žltá Ø40 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB4BC48021","OVL. HLAVICA ROBUST ČERV. SYMBOL \"0\"",1,"ks",{"v":31.5700875,"d":"31.570"},"3606480444647",{"v":7,"d":"7.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":33,"d":"33.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BC48021","hlava tlačítka pre nepriaznivé prostredie - zelená - s ozn.",0]
["ZB4BC480","OVLÁDACIA HLAVICA ROBUSTNÁ ČERVENÁ",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3606480444616",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":33,"d":"33.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BC480","hlava tlačítka pre nepriaznivé prostredie - červená - bez ozn.",0]
["ZB4BC44","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389110888409",{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":73,"d":"73.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC44","červená Ø30 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB4BC4","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110888454",{"v":5.4,"d":"5.40"},{"v":9,"d":"9.00"},{"v":4.4,"d":"4.40"},{"v":77,"d":"77.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC4","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – s hríbom Ø 40 mm – červená",0]
["ZB4BC380","OVLÁDACIA HLAVICA ROBUSTNÁ ZELENÁ",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3606480444326",{"v":8,"d":"8.00"},{"v":4,"d":"4.00"},{"v":5,"d":"5.00"},{"v":33,"d":"33.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BC380","hlava tlačítka pre nepriaznivé prostredie - zelená - bez ozn.",0]
["ZB4BC34","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110888393",{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":74,"d":"74.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC34","zelená Ø30 hlavica s hríbovým tlačítkom Ø22 s návratom",0]
["ZB4BC3","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110888447",{"v":5.4,"d":"5.40"},{"v":9.4,"d":"9.40"},{"v":4.5,"d":"4.50"},{"v":76,"d":"76.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC3","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – s hríbom Ø 40 mm – zelená",0]
["ZB4BC28001","OVL.HLAVICA ROBUST. ČIERNA SYM. ZVONČEK",1,"ks",{"v":31.5700875,"d":"31.570"},"3606480444128",{"v":3.7,"d":"3.70"},{"v":3.7,"d":"3.70"},{"v":3.7,"d":"3.70"},{"v":36,"d":"36.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BC28001","hlava tlačítka pre nepriaznivé prostredie - černá - s ozn.",0]
["ZB4BC280","OVL. HLAVICA ROBUSTNÁ ČIERNA",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3606480444111",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":33,"d":"33.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BC280","hlava tlačítka pre nepriaznivé prostredie - černá - bez ozn.",0]
["ZB4BC24","OVLÁDACIA HLAVICA STLÁČACIA",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110888386",{"v":8.8,"d":"8.80"},{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":66,"d":"66.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC24","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – s hríbom Ø 30 mm – čierna",0]
["ZB4BC2","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110888430",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":4.4,"d":"4.40"},{"v":76,"d":"76.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/ZB4BC2","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – s hríbom Ø 40 mm – čierna",0]
["ZB4BB4","Hlavica krížového ovládača, červená",1,"ks",{"v":60.394949999999994,"d":"60.395"},"3389110173307",{"v":3.1,"d":"3.10"},{"v":10.5,"d":"10.50"},{"v":3.1,"d":"3.10"},{"v":68,"d":"68.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BB4","Head for joystick controller, Harmony XB4, red Ø22 mm omnidirectional spring return",0]
["ZB4BB2","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":47.58389999999999,"d":"47.584"},"3389110173239",{"v":12.8,"d":"12.80"},{"v":5.2,"d":"5.20"},{"v":4.4,"d":"4.40"},{"v":58,"d":"58.00"},"FR","85389099","https://www.se.com/sk/sk/product/ZB4BB2","krížový ovládač – Ø 22 – viacsmerový, vratná pružina",0]
["ZB4BA98","Ovládacia hlavica stlačacia, so sadou",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3606481357045",{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":34,"d":"34.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA98","Head for illuminated push button, Harmony XB4, metal, 6 colors flush, universal LED, 22mm, spring return, unmarked",0]
["ZB4BA9","Ovládacia hlavica stláčacia,so sadou 6ba",1,"ks",{"v":8.46444375,"d":"8.464"},"3389110120059",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":38,"d":"38.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA9","zapuš. ovl. hlavica stis. Ø22 s návratom s 6 farbami neoznačená",0]
["ZB4BA8","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110887501",{"v":3.5,"d":"3.50"},{"v":4.7,"d":"4.70"},{"v":5.4,"d":"5.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA8","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zapustená – sivá – bez označenia",0]
["ZB4BA791","DVOJTLAČ. KOVOVÝ OVLÁDAČ BEZ HMATNÍKA",1,"ks",{"v":17.386425,"d":"17.386"},"3389119043717",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.3,"d":"3.30"},{"v":57,"d":"57.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA791","zapuš./červená s presah./zapuš. trojtlač. hlavica tlač. Ø22 bez šošovky",0]
["ZB4BA79","DVOJTLAČ. KOVOVÝ OVLÁDAČ BEZ HMATNÍKA",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389119043878",{"v":5.4,"d":"5.40"},{"v":3.2,"d":"3.20"},{"v":5.2,"d":"5.20"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA79","zapuš./zapuš. ovl. hlavica dvojtlač. Ø22 bez šošovky",0]
["ZB4BA7341","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA IP66",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389119043847",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA7341","zelená lícujúca/červená lícujúca ovl. hlavica dvojtlač. Ø22 s popisom",0]
["ZB4BA7340","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA IP66",1,"ks",{"v":18.301499999999997,"d":"18.302"},"3389119043830",{"v":5.3,"d":"5.30"},{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA7340","zelená lícujúca/červená lícujúca ovl. hlavica dvojtlač. Ø22 neoznačená",0]
["ZB4BA73134","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA +STOP",1,"ks",{"v":21.5042625,"d":"21.504"},"3389119043656",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA73134","lená lícujúca/červená s presah./zelená zapuš.trojtlač hlavica tlač.Ø22 s popisom",0]
["ZB4BA73133","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA +STOP",1,"ks",{"v":21.5042625,"d":"21.504"},"3389119043649",{"v":5.7,"d":"5.70"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":58,"d":"58.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA73133","lená lícujúca/červená s presah./zelená zapuš.trojtlač hlavica tlač.Ø22 s popisom",0]
["ZB4BA7121","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA",1,"ks",{"v":19.216575,"d":"19.217"},"3389119043823",{"v":5,"d":"5.00"},{"v":3.2,"d":"3.20"},{"v":4.6,"d":"4.60"},{"v":57,"d":"57.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA7121","zelená zapuš./čierna zapuš. ovl.hlavica dvojtlač. Ø22 s popisom",0]
["ZB4BA7120","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389119043816",{"v":5.9,"d":"5.90"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":57,"d":"57.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA7120","zelená zapuš./čierna zapuš. ovl.hlavica dvojtlač. Ø22 neoznačená",0]
["ZB4BA71124","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA +STOP",1,"ks",{"v":21.5042625,"d":"21.504"},"3389119603539",{"v":5.2,"d":"5.20"},{"v":3.6,"d":"3.60"},{"v":4.6,"d":"4.60"},{"v":56,"d":"56.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA71124","biela zapuš./červená s presah./čierna zapuš.trojtlač.hlavica tlač.Ø22 s popisom",0]
["ZB4BA71115","DVOJTLAČ. KOVOVÁ OVLÁDACIA HLAVICA +STOP",1,"ks",{"v":21.961799999999997,"d":"21.962"},"3389119043670",{"v":5.3,"d":"5.30"},{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA71115","biela zapuš./červená s presah./biela zapuš.trojtlač.hlavica tlač.Ø22 s popisom",0]
["ZB4BA68","OVL. HLAVICA STLÁČ. S PRIEHĽ. HMATNÍKOM",1,"ks",{"v":8.601705,"d":"8.602"},"3389110887747",{"v":5.6,"d":"5.60"},{"v":9.2,"d":"9.20"},{"v":3.8,"d":"3.80"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA68","hlavica osvetleného tlačidla – Ø 22 – modrá – na vloženie štítku",0]
["ZB4BA6","OVL. HLAVICA STLÁČACIA BEZ SYMBOLU",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110887495",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA6","modrá zapust. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BA58","OVL. HLAVICA STLÁČ. S PRIEHĽ. HMATNÍKOM",1,"ks",{"v":8.601705,"d":"8.602"},"3389110887730",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":29.6,"d":"29.60"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA58","hlavica osvetleného tlačidla – Ø 22 – žltá – na vloženie štítku",0]
["ZB4BA56","OVL. HLAVICA STLÁČ. S PRIEHĽ. HMATNÍKOM",1,"ks",{"v":12.81105,"d":"12.811"},"3389110887952",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":33.5,"d":"33.50"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA56","žltá zapuš. ovl. hlavica stis. Ø22 s návratom neoznačená",0]
["ZB4BA5","OVL. HLAVICA STLÁČACIA BEZ SYMBOLU",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110887488",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA5","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zapustená – žltá – bez označenia",0]
["ZB4BA48","OVL. HLAVICA STLÁČ. S PRIEHĽ. HMATNÍKOM",1,"ks",{"v":8.92198125,"d":"8.922"},"3389110887723",{"v":5.3,"d":"5.30"},{"v":5.6,"d":"5.60"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA48","hlavica osvetleného tlačidla – Ø 22 – červená – na vloženie štítku",0]
["ZB4BA47","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":20.13165,"d":"20.132"},"3389110220094",{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA47","červená zapust. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BA46","Ovl. hlavica stláčacia, červená",1,"ks",{"v":20.13165,"d":"20.132"},"3389110887945",{"v":5.3,"d":"5.30"},{"v":3.6,"d":"3.60"},{"v":4.7,"d":"4.70"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA46","červená zapuš. ovl. hlavica stis. Ø22 s návratom neoznačená",0]
["ZB4BA434","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110887587",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA434","červená zapust. hlava tlačítka Ø22 s návratom \"STOP\"",0]
["ZB4BA432","OVL. HLAVICA STLÁČACIA SO SYMBOLOM",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110887563",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA432","červená zapust. hlava tlačítka Ø22 s návratom \"O\"",0]
["ZB4BA4","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110887471",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA4","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zapustená – červená – bez označ.",0]
["ZB4BA387","Ovládacia hlavica stláčacia",1,"ks",{"v":20.589187499999998,"d":"20.589"},"3389110222739",{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA387","zelená zapus. hlava tlačidla Ø22 s návratom neoznačená",0]
["ZB4BA38","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":8.92198125,"d":"8.922"},"3389110887709",{"v":5.4,"d":"5.40"},{"v":9,"d":"9.00"},{"v":3.4,"d":"3.40"},{"v":30.4,"d":"30.40"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA38","hlavica osvetleného tlačidla – Ø 22 – zelená – na vloženie štítku",0]
["ZB4BA367","Ovládacia hlavica, zelená",1,"ks",{"v":28.541189249999995,"d":"28.541"},"3389110223262",{"v":2.8,"d":"2.80"},{"v":3.8,"d":"3.80"},{"v":5.2,"d":"5.20"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA367","zelená zapus. hlava tlačidla Ø22 s návratom neoznačená",""]
["ZB4BA36","Ovl. hlavica stláčacia, zelená",1,"ks",{"v":20.13165,"d":"20.132"},"3389110887938",{"v":4.6,"d":"4.60"},{"v":3.4,"d":"3.40"},{"v":4,"d":"4.00"},{"v":33.4,"d":"33.40"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA36","zelená zapuš. ovl. hlavica stis. Ø22 s návratom neoznačená",0]
["ZB4BA335","OVL. HLAVICA STLÁČACIA SO SYMBOLOM",1,"ks",{"v":7.091831249999999,"d":"7.092"},"3389110120745",{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA335","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zapustená – čierna – šípka hore",0]
["ZB4BA334","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110120080",{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA334","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zapustená – biela – šípka hore",0]
["ZB4BA333","OVL. HLAVICA STLÁČACIA SO SYMBOLOM",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110887532",{"v":5.2,"d":"5.20"},{"v":3.5,"d":"3.50"},{"v":4.6,"d":"4.60"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA333","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zapustená – zelená – START",0]
["ZB4BA331","OVL. HLAVICA STLÁČACIA SO SYMBOLOM",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110887518",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":29,"d":"29.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA331","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zapustená – zelená – I",0]
["ZB4BA3","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110895742",{"v":5.4,"d":"5.40"},{"v":4.8,"d":"4.80"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA3","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zapustená – zelená – bez označ.",0]
["ZB4BA27","PUSHBUTTON OPERATOR HEAD",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110220070",{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":4.6,"d":"4.60"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA27","čierna zapuš. hlava tlačítka Ø22 s návratom neoznačená",0]
["ZB4BA26","OVLÁDACIA HLAVICA STLÁČACIA",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389110887921",{"v":3.2,"d":"3.20"},{"v":3.6,"d":"3.60"},{"v":4.8,"d":"4.80"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA26","čierna zapust. ovl. hlavica stláčacia Ø22 s návratom neoznačená",0]
["ZB4BA234","OVL. HLAVICA STLÁČACIA SO SYMBOLOM",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110887686",{"v":4.4,"d":"4.40"},{"v":3.5,"d":"3.50"},{"v":5.3,"d":"5.30"},{"v":30,"d":"30.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA234","čierna zapust. hlava tlačítka Ø22 s návratom \"STOP\"",0]
["ZB4BA232","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110887655",{"v":5.4,"d":"5.40"},{"v":3.6,"d":"3.60"},{"v":4.7,"d":"4.70"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA232","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – zapustená – čierna – O",0]
["ZB4BA2","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110887464",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA2","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zapustená – čierna – bez označ.",0]
["ZB4BA18","OVL. HLAVICA STLÁČ. S PRIEHĽ. HMATNÍKOM",1,"ks",{"v":8.92198125,"d":"8.922"},"3389110887716",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA18","osvetlená hlavica tlačidla – Ø 22 – biela – na vloženie štítku",0]
["ZB4BA133","OVL. HLAVICA STLÁČACIA SO SYMBOLOM",1,"ks",{"v":7.4121074999999985,"d":"7.412"},"3389110887624",5.08,{"v":4.572,"d":"4.57"},{"v":3.556,"d":"3.56"},{"v":27.216,"d":"27.22"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA133","biela lícujúca ovl. hlavice stláčacia Ø22 s návratom \"START\"",0]
["ZB4BA131","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":7.4121074999999985,"d":"7.412"},"3389110887600",{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA131","biela lícujúca ovl. hlavica stláčacia Ø22 s návratom \"I\"",0]
["ZB4BA1","OVL. HLAVICA STLÁČACIA",1,"ks",{"v":5.947987499999999,"d":"5.948"},"3389110887457",{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":28,"d":"28.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA1","okrúhla hlavica pre tlač. Ø 22 – vr. pružina – zapustená – biela – bez označenia",0]
["ZB4BA0","OVL. HLAV. STLÁČ. BEZ HMATNÍKA",1,"ks",{"v":5.62771125,"d":"5.628"},"3389110887440",{"v":5.4,"d":"5.40"},{"v":4.4,"d":"4.40"},{"v":3.4,"d":"3.40"},{"v":27,"d":"27.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB4BA0","okrúhla hlavica pre tlačidlo Ø 22 – vratná pružina – bez krytu",0]
["ZB2SZ4","OVLÁDAČ PRE XAC",1,"ks",{"v":7.091831249999999,"d":"7.092"},"3389110313277",{"v":3,"d":"3.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB2SZ4","sivá zaslepovacia krytka pre riadiacu stanicu",0]
["ZB2SZ3","ZASLEPOVACIA KRYTKA",1,"ks",{"v":4.34660625,"d":"4.347"},"3389110614602",{"v":15,"d":"15.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":5,"d":"5.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZB2SZ3","čierna zaslepovacia krytka pre riadiacu stanicu alebo závesnú riadiacu stanicu",0]
["ZB2BZ105","SPÍNACIA JEDNOTKA",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110614343",{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":56,"d":"56.00"},"ID","8536501190","https://www.se.com/sk/sk/product/ZB2BZ105","spínacia jednotka s upevnením",0]
["ZB2BZ102","SPÍNACIA JEDNOTKA",10,"ks",{"v":10.5233625,"d":"10.523"},"3389110614312",{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":4.5,"d":"4.50"},{"v":41.5,"d":"41.50"},"ID","8536508090","https://www.se.com/sk/sk/product/ZB2BZ102","spínacia jednotka s upevnením",0]
["ZB2BZ101","SPÍNACIA JEDNOTKA",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110614305",{"v":4.5,"d":"4.50"},{"v":3.3,"d":"3.30"},{"v":4.5,"d":"4.50"},{"v":41,"d":"41.00"},"ID","8536508090","https://www.se.com/sk/sk/product/ZB2BZ101","spínacia jednotka s upevnením",0]
["ZB2BY9330","ŠTÍTOK",10,"ks",{"v":3.43153125,"d":"3.432"},"3389110598070",{"v":6,"d":"6.00"},{"v":0.1,"d":"0.10"},{"v":6,"d":"6.00"},{"v":2.6,"d":"2.60"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY9330","ŠTÍTOK (E",0]
["ZB2BY9101","ŠTÍTOK",1,"ks",{"v":3.0197474999999994,"d":"3.020"},"3389110615265",{"v":6,"d":"6.00"},{"v":0.1,"d":"0.10"},{"v":6,"d":"6.00"},{"v":2.6,"d":"2.60"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY9101","štítok - Ø 22 - Ø 90 mm - neoznačený",0]
["ZB2BY4985","STITOK OBDcSNIKOVY - SO SYMBOL",1,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615357",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4985","štítok - 30x40 mm - biely - start klaxon",0]
["ZB2BY4982","STITOK OBDcSNIKOVY - SO SYMBOL",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615333",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4982","štítok - 30x40 mm - biely - klaxon",0]
["ZB2BY4980","ŠTÍTOK OBDĹŽNIKOVÝ",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615319",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":4,"d":"4.00"},{"v":0.9,"d":"0.90"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4980","štítok - 30x40 mm - biely - I",0]
["ZB2BY4965","ŠTÍTOK SO SYMBOLOM - PRE XAC",1,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615296",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4965","štítok - 30x40 mm - biely - forward - slow - fast",0]
["ZB2BY4964","ŠTÍTOK OBDĹŽNIKOVÝ",1,"ks",{"v":1.7386424999999999,"d":"1.739"},"3389110615272",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4964","Etiketa pre závesný ovládač",0]
["ZB2BY4963","STITOK OBDcSNIKOVY - SO SYMBOL",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615258",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4963","štítok - 30x40 mm - biely - forward - slow",0]
["ZB2BY4953","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615210",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4953","štítok - 30x40 mm - biely - raise - slow - fast",0]
["ZB2BY4952","ŠTÍTOK OBDĹŽNIKOVÝ",1,"ks",{"v":1.7386424999999999,"d":"1.739"},"3389110615197",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4952","Etiketa pre závesný ovládač",0]
["ZB2BY4951","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615173",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4951","štítok - 30x40 mm - biely - raise - slow",0]
["ZB2BY4935","ŠTÍTOK SO SYMBOLOM - PRE XAC",1,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645699",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4935","štítok - 30x40 mm - biely - start klaxon",0]
["ZB2BY4934","LEGEND PLATE",1,"ks",{"v":1.7386424999999999,"d":"1.739"},"3389110645682",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4934","štítok - 30x40 mm - biely - fast",0]
["ZB2BY4933","STITOK OBDcSNIKOVY - SO SYMBOL",1,"ks",{"v":1.7386424999999999,"d":"1.739"},"3389110645675",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4933","štítok - 30x40 mm - biely - slow",0]
["ZB2BY4932","ŠTÍTOK SO SYMBOLOM - PRE XAC",1,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645668",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4932","štítok - 30x40 mm - biely - klaxon",0]
["ZB2BY4930","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645651",{"v":4,"d":"4.00"},0.11,{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4930","štítok - 30x40 mm - biely - I",0]
["ZB2BY4921","ŠTÍTOK OBDĹŽNIKOVÝ - ROTÁCIA VPRAVO",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645644",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4921","štítok - 30x40 mm - biely - slew pravý - slow - fast",0]
["ZB2BY4920","ŠTÍTOK OBDĹŽNIKOVÝ SO SYMBOLOM",1,"ks",{"v":1.2811049999999997,"d":"1.281"},"3389110645637",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4920","štítok - 30x40 mm - biely - slew pravý - fast",0]
["ZB2BY4919","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.2811049999999997,"d":"1.281"},"3389110645620",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4919","štítok - 30x40 mm - biely - slew pravý - slow",0]
["ZB2BY4915","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645613",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4915","štítok - 30x40 mm - biely - forward - slow - fast",0]
["ZB2BY4914","ŠTÍTOK SO SYMBOLOM - PRE XAC",1,"ks",{"v":1.2811049999999997,"d":"1.281"},"3389110645606",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4914","štítok - 30x40 mm - biely - forward - fast",0]
["ZB2BY4913","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645590",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4913","štítok - 30x40 mm - biely - forward - slow",0]
["ZB2BY4912","ŠTÍTOK",1,"ks",{"v":2.4249487499999995,"d":"2.425"},"3389110321111",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4912","legend - 30 x 40 mm - yellow - ARRET",0]
["ZB2BY4909","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645583",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4909","štítok - 30x40 mm - biely - pravý - slow - fast",0]
["ZB2BY4908","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.3268587499999998,"d":"1.327"},"3389110645576",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1.1,"d":"1.10"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4908","štítok - 30x40 mm - biely - pravý - fast",0]
["ZB2BY4907","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645569",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4907","štítok - 30x40 mm - biely - pravý - slow",0]
["ZB2BY4906","ŠTÍTOK",1,"ks",{"v":2.3791949999999997,"d":"2.379"},"3389110321081",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4906","etiketa na závesný ovládač",0]
["ZB2BY4904","ŠTÍTOK SO SYMBOLOM - PRE XAC",1,"ks",{"v":2.3791949999999997,"d":"2.379"},"3389110321067",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","39269097","https://www.se.com/sk/sk/product/ZB2BY4904","legend plate 30x40 mm",0]
["ZB2BY4903","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645552",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4903","štítok - 30x40 mm - biely - raise alebo pravý - slow - fast",0]
["ZB2BY4902","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645545",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4902","štítok - 30x40 mm - biely - raise alebo pravý - fast",0]
["ZB2BY4901","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645538",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4901","štítok - 30x40 mm - biely - raise alebo pravý - slow",0]
["ZB2BY4101","ŠTÍTOK",1,"ks",{"v":1.1895974999999999,"d":"1.190"},"3389110614855",{"v":4.5,"d":"4.50"},{"v":0.1,"d":"0.10"},{"v":3.5,"d":"3.50"},{"v":0.8,"d":"0.80"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4101","štítok - 30x40 mm - 1 biela strana - 1 žltá strana - neoznačený",0]
["ZB2BY4001","ŠTÍTOK",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110146172",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY4001","Etiketa pre závesný ovládač",0]
["ZB2BY2968","ŠTÍTOK SO SYMBOLOM - PRE XAC",1,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615159",{"v":4.5,"d":"4.50"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2968","štítok - 30x40 mm - čierny - reverse - slow - fast",0]
["ZB2BY2967","ŠTÍTOK OBDĹŽNIKOVÝ - SO SYMBOL",1,"ks",{"v":1.7386424999999999,"d":"1.739"},"3389110615135",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2967","Etiketa pre závesný ovládač",0]
["ZB2BY2966","STITOK OBDcSNIKOVY - SO SYMBOL",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615098",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.8,"d":"0.80"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2966","štítok - 30x40 mm - čierny - reverse - slow",0]
["ZB2BY2956","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615074",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2956","štítok - 30x40 mm - čierny - lower - slow - fast",0]
["ZB2BY2955","ŠTÍTOK OBDĹŽNIKOVÝ SO SYMBOLOM",1,"ks",{"v":1.7386424999999999,"d":"1.739"},"3389110615050",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2955","Etiketa pre závesný ovládač",0]
["ZB2BY2954","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110615036",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2954","štítok - 30x40 mm - čierny - lower - slow",0]
["ZB2BY2931","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645521",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2931","štítok - 30x40 mm - červený - 0",0]
["ZB2BY2924","ŠTÍTOK OBDĹŽNIKOVÝ - ROTÁCIA VĽAVO",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645514",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2924","štítok - 30x40 mm - čierny - slew left - slow - fast",0]
["ZB2BY2923","ŠTÍTOK OBDĹŽNIKOVÝ - SO SYMBOL",1,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645507",{"v":3.9,"d":"3.90"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2923","štítok - 30x40 mm - čierny - slew left - fast",0]
["ZB2BY2922","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.2811049999999997,"d":"1.281"},"3389110645491",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2922","štítok - 30x40 mm - čierny - slew left - slow",0]
["ZB2BY2918","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645484",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2918","štítok - 30x40 mm - čierny - reverse - slow - fast",0]
["ZB2BY2917","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645477",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2917","štítok - 30x40 mm - čierny - reverse - fast",0]
["ZB2BY2916","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645460",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2916","štítok - 30x40 mm - čierny - reverse - slow",0]
["ZB2BY2912","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645453",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2912","štítok - 30x40 mm - čierny - left - slow - fast",0]
["ZB2BY2911","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645446",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","4911990000","https://www.se.com/sk/sk/product/ZB2BY2911","štítok - 30x40 mm - čierny - left - fast",0]
["ZB2BY2910","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645439",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2910","štítok - 30x40 mm - čierny - left - slow",0]
["ZB2BY2906","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645422",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2906","štítok - 30x40 mm - čierny - left alebo lower - slow - fast",0]
["ZB2BY2905","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.3268587499999998,"d":"1.327"},"3389110645415",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2905","štítok - 30x40 mm - čierny - left alebo lower - fast",0]
["ZB2BY2904","ŠTÍTOK SO SYMBOLOM - PRE XAC",10,"ks",{"v":1.7843962499999997,"d":"1.784"},"3389110645408",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":1,"d":"1.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2904","štítok - 30x40 mm - čierny - left alebo lower - slow",0]
["ZB2BY2367","ŠTÍTOK PRE ZÁV. OVL. POPIS ANG",1,"ks",{"v":1.8759037499999995,"d":"1.876"},"3389110597967",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2367","štítok 30 x 40 mm - čierny - OFF-ON",0]
["ZB2BY2310","ŠTÍTOK",1,"ks",{"v":1.8850545,"d":"1.885"},"3389110597912",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2310","Marked legend, Harmony XAC, nameplate, 30 x 40mm, plastic, black, 22mm push button, white marked LEFT",""]
["ZB2BY2308","ŠTÍTOK",1,"ks",{"v":1.8759037499999995,"d":"1.876"},"3389110614923",{"v":4.1,"d":"4.10"},{"v":0.1,"d":"0.10"},{"v":3.1,"d":"3.10"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2308","štítok - 30 x 40 mm - čierny - DOWN",0]
["ZB2BY2307","ŠTÍTOK OBDĹŽNIKOVÝ - SO SYMBOL",1,"ks",{"v":1.8759037499999995,"d":"1.876"},"3389110614916",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2307","ŠTÍTOK OBDĹŽNIKOVÝ - SO SYMBOL",0]
["ZB2BY2304","ŠTÍTOK",10,"ks",{"v":1.8759037499999995,"d":"1.876"},"3389110614848",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.8,"d":"0.80"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2304","štítok - 30 x 40 mm - červený - STOP",0]
["ZB2BY2303","ŠTÍTOK",10,"ks",{"v":1.8759037499999995,"d":"1.876"},"3389110615166",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3,"d":"3.00"},{"v":0.9,"d":"0.90"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2303","štítok - 30 x 40 mm - čierny - START",0]
["ZB2BY2101","ŠTÍTOK",10,"ks",{"v":1.1895974999999999,"d":"1.190"},"3389110614411",{"v":4,"d":"4.00"},{"v":0.1,"d":"0.10"},{"v":3.5,"d":"3.50"},{"v":0.8,"d":"0.80"},"CZ","3926909790","https://www.se.com/sk/sk/product/ZB2BY2101","štítok - 30 x 40 mm - 1 čierna strama, 1 červená strana - neoznačený",0]
["ZB2BV007","OBJIMKA",1,"ks",{"v":20.589187499999998,"d":"20.589"},"3389110645392",{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":4.3,"d":"4.30"},{"v":33,"d":"33.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB2BV007","hlavice na signálky",0]
["ZB2BV006","OBJIMKA",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110645385",{"v":4.5,"d":"4.50"},{"v":3.2,"d":"3.20"},{"v":4.5,"d":"4.50"},{"v":15,"d":"15.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZB2BV006","Montážna objímka pre XACA PILOT LITE",0]
["ZB2BE201","SPÍNACIA JEDNOTKA",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110612547",{"v":4,"d":"4.00"},{"v":1.5,"d":"1.50"},{"v":4,"d":"4.00"},{"v":15,"d":"15.00"},"ES","8536508090","https://www.se.com/sk/sk/product/ZB2BE201","SPÍNACIA JEDNOTKA ZB2 1NO PRUŽINOVÝ",0]
["ZB2BE102","SPÍNACIA JEDNOTKA",10,"ks",{"v":4.849897499999999,"d":"4.850"},"3389110612615",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},"ID","8536508090","https://www.se.com/sk/sk/product/ZB2BE102","spínací blok",0]
["ZB2BE101","SPÍNACIA JEDNOTKA",10,"ks",{"v":6.1310025,"d":"6.131"},"3389110612608",{"v":4,"d":"4.00"},{"v":2,"d":"2.00"},{"v":4,"d":"4.00"},{"v":14,"d":"14.00"},"ID","8536508090","https://www.se.com/sk/sk/product/ZB2BE101","spínací blok",0]
["ZB2BD3","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110612417",{"v":6,"d":"6.00"},{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":44,"d":"44.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZB2BD3","ovládacia hlavica, 3 polohy",0]
["ZART8L","EXLHOIST DIAĽKOVÝ OVLÁDAČ – 8 TLAČIDIEL",1,"ks",{"v":663.4293749999999,"d":"663.429"},"3606480610356",{"v":33.6,"d":"33.60"},{"v":10.7,"d":"10.70"},{"v":10.2,"d":"10.20"},{"v":734,"d":"734.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZART8L","základné funkcie – 2 pomocné tlačidlá LED",0]
["ZART8D","EXLHOIST DIAĽKOVÝ OVLÁDAČ – 8 TLAČIDIEL",1,"ks",{"v":741.21075,"d":"741.211"},"3606480610363",{"v":33.6,"d":"33.60"},{"v":10.7,"d":"10.70"},{"v":10.5,"d":"10.50"},{"v":732,"d":"732.00"},"FR","8526920090","https://www.se.com/sk/sk/product/ZART8D","základné funkcie – 2 pomocné tlačidlá displej",0]
["ZART12D","EXLHOIST DIAĽKOVÝ OVLÁDAČ – 12 TLAČIDIEL",1,"ks",{"v":1052.3362499999998,"d":"1052.336"},"3606480610370",{"v":33.7,"d":"33.70"},{"v":10.2,"d":"10.20"},{"v":10.7,"d":"10.70"},{"v":650,"d":"650.00"},"FR","85269200","https://www.se.com/sk/sk/product/ZART12D","ExLhoist dálkový ovládač – 12 tlačítek",0]
["ZARC54","Kit pre výmenu batérie",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3606480982590",{"v":33.7,"d":"33.70"},{"v":10.5,"d":"10.50"},{"v":10.5,"d":"10.50"},{"v":295,"d":"295.00"},"","85299097","https://www.se.com/sk/sk/product/ZARC54","KIT REMOTE BACK COVER",0]
["ZARC20","Sada tesnení",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3606480705618",{"v":20,"d":"20.00"},{"v":2.2,"d":"2.20"},{"v":13,"d":"13.00"},{"v":20,"d":"20.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZARC20","Harmony eXLhoist krytky",0]
["ZARC08","EXLHOIST SADA ŠTÍTKOV",1,"ks",{"v":57.46670999999999,"d":"57.467"},"3606480662355",{"v":30,"d":"30.00"},{"v":0.1,"d":"0.10"},{"v":20,"d":"20.00"},{"v":88,"d":"88.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZARC08","ExLhoist sada štítků",""]
["ZARC07","EXLHOIST SADA ŠTÍTKOV",1,"ks",{"v":57.46670999999999,"d":"57.467"},"3606480662348",{"v":20,"d":"20.00"},{"v":0.1,"d":"0.10"},{"v":12,"d":"12.00"},{"v":10,"d":"10.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZARC07","ExLhoist sada štítků",""]
["ZARC04","EXLHOIST DRŽIAK OVLÁDAČA",1,"ks",{"v":70.0032375,"d":"70.003"},"3606480662317",{"v":11.2,"d":"11.20"},{"v":12.6,"d":"12.60"},{"v":25.8,"d":"25.80"},{"v":250,"d":"250.00"},"FR","3926909790","https://www.se.com/sk/sk/product/ZARC04","ExLhoist držák ovládače",0.04]
["ZARC02","EXLHOIST RAMENNÝ A PÁSOVÝ POPRUH",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3606480662294",{"v":19.2,"d":"19.20"},{"v":4.6,"d":"4.60"},{"v":7.7,"d":"7.70"},{"v":98,"d":"98.00"},"FR","6307909899","https://www.se.com/sk/sk/product/ZARC02","ExLhoist ramenní a pásový popruh",0]
["ZARC01","EXLHOIST NABÍJAČKA",1,"ks",{"v":205.891875,"d":"205.892"},"3606480662287",{"v":14,"d":"14.00"},{"v":6.5,"d":"6.50"},{"v":7.5,"d":"7.50"},{"v":260,"d":"260.00"},"FR","8504406090","https://www.se.com/sk/sk/product/ZARC01","ExLhoist nabíječka",0.03]
["ZARB18W","EXLHOIST PRIJÍMAČ - 18 REL. VÝST. – KÁBL",1,"ks",{"v":1147.50405,"d":"1147.504"},"3606480610400",{"v":30.2,"d":"30.20"},{"v":10,"d":"10.00"},{"v":28.7,"d":"28.70"},{"v":1700,"d":"1,700.00"},"FR","8537109899","https://www.se.com/sk/sk/product/ZARB18W","exlhoist prijímač - 18 rel. výst. – kábl. piechod",""]
["ZARB12W","EXLHOIST PRIJÍMAČ - 12 REL. VÝST. – KÁBL",1,"ks",{"v":828.1428749999999,"d":"828.143"},"3606480610387",{"v":30.2,"d":"30.20"},{"v":10,"d":"10.00"},{"v":28.6,"d":"28.60"},{"v":1450,"d":"1,450.00"},"FR","8537109899","https://www.se.com/sk/sk/product/ZARB12W","exlhoist prijímač - 12 rel. výst. – kábl. priechod",0]
["ZALVM1","OBJÍMKA LED",5,"ks",{"v":12.81105,"d":"12.811"},"3389110115215",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},{"v":10.4,"d":"10.40"},"FR","8536619090","https://www.se.com/sk/sk/product/ZALVM1","objímka pre riadiacu stanicu – biela – vstavaná LED – 230 - 240 V",0]
["ZALVG1","OBJÍMKA LED",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110115161",{"v":5.6,"d":"5.60"},{"v":4.4,"d":"4.40"},{"v":5.4,"d":"5.40"},{"v":11,"d":"11.00"},"FR","8536619090","https://www.se.com/sk/sk/product/ZALVG1","objímka pre riadiacu stanicu – biela – vstavaná LED – 48 - 120 V",0]
["ZALVB1","OBJÍMKA LED",5,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110115093",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},{"v":10,"d":"10.00"},"FR","8536619090","https://www.se.com/sk/sk/product/ZALVB1","objímka pre riadiacu stanicu – biela – vstavaná LED – 24 V",0]
["ZA2VA12","RIADIACI BLOK",1,"ks",{"v":141.836625,"d":"141.837"},"3389110648973",{"v":11.1,"d":"11.10"},{"v":3.6,"d":"3.60"},{"v":4.5,"d":"4.50"},{"v":56,"d":"56.00"},"FR","8531202090","https://www.se.com/sk/sk/product/ZA2VA12","teleso číselného zobrazenia – Ø 22 – BCD + LACH",0]
["ZA2VA11","TELO NUM. ZOBRAZOVAČA",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110648966",{"v":10.8,"d":"10.80"},{"v":3,"d":"3.00"},{"v":4.2,"d":"4.20"},{"v":57,"d":"57.00"},"FR","8531807000","https://www.se.com/sk/sk/product/ZA2VA11","TELO NUM. ZOBRAZOVAČA",0]
["ZA2VA05","HLAVICA NUM. ZOBRAZOVAČA",1,"ks",{"v":57.192187499999996,"d":"57.192"},"3389110648959",{"v":4.3,"d":"4.30"},{"v":3.2,"d":"3.20"},{"v":4.3,"d":"4.30"},{"v":21,"d":"21.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZA2VA05","žltá digitálna displejová hlava Ø22",0]
["ZA2VA04","HLAVICA NUM. ZOBRAZOVAČA",1,"ks",{"v":56.277112499999994,"d":"56.277"},"3389110648942",{"v":4.2,"d":"4.20"},{"v":3.2,"d":"3.20"},{"v":4.2,"d":"4.20"},{"v":20,"d":"20.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZA2VA04","červená digitálna displejová hlava Ø22",0]
["ZA2VA03","HLAVICA NUM. ZOBRAZOVAČA",1,"ks",{"v":56.277112499999994,"d":"56.277"},"3389110648935",{"v":4.2,"d":"4.20"},{"v":3,"d":"3.00"},{"v":4.2,"d":"4.20"},{"v":21,"d":"21.00"},"FR","8531900000","https://www.se.com/sk/sk/product/ZA2VA03","zelená digitálna displejová hlava Ø22",0]
["ZA2BZ905","KĽÚČIK",1,"ks",{"v":17.386425,"d":"17.386"},"3389110316100",{"v":11.4,"d":"11.40"},{"v":3.3,"d":"3.30"},{"v":3.4,"d":"3.40"},{"v":60,"d":"60.00"},"FR","8205598000","https://www.se.com/sk/sk/product/ZA2BZ905","Kľúčik",0]
["ZA2BV07","OVLÁDAČ PRE XAC",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110648287",{"v":3.8,"d":"3.80"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":15,"d":"15.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BV07","kryt kontrolky – Ø 22 – číry",0]
["ZA2BV05","OVLÁDAČ PRE XAC",10,"ks",{"v":10.5233625,"d":"10.523"},"3389110648249",{"v":9.7,"d":"9.70"},{"v":3.6,"d":"3.60"},{"v":7.2,"d":"7.20"},{"v":15,"d":"15.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BV05","kryt kontrolky – Ø 22 – žltý",0]
["ZA2BV04","OVLÁDAČ PRE XAC",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110645378",{"v":4,"d":"4.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":15,"d":"15.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BV04","kryt kontrolky – Ø 22 – červený",0]
["ZA2BV03","OVLÁDAČ PRE XAC",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110645361",{"v":4,"d":"4.00"},{"v":3.5,"d":"3.50"},{"v":4,"d":"4.00"},{"v":15,"d":"15.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BV03","kryt kontrolky – Ø 22 – zelený",0]
["ZA2BV01","OVLÁDAČ PRE XAC",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110647402",{"v":4,"d":"4.00"},{"v":4,"d":"4.00"},{"v":3.5,"d":"3.50"},{"v":15,"d":"15.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BV01","kryt kontrolky – Ø 22 – biely",0]
["ZA2BS944","OVL. HLAVICA S HRÍBOM",1,"ks",{"v":51.2442,"d":"51.244"},"3389110591781",{"v":9,"d":"9.00"},{"v":4,"d":"4.00"},{"v":4,"d":"4.00"},{"v":65,"d":"65.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BS944","hlavica tlačidla núdzového zastavenia Ø 40 mm - uvoľniť kľúčom - Ø 22 - červená",0]
["ZA2BS934","OVL. HLAV. STLÁČ. HRÍB. S ODBL. ČERV.",1,"ks",{"v":53.98942499999999,"d":"53.989"},"3389110591774",{"v":10.1,"d":"10.10"},{"v":4.2,"d":"4.20"},{"v":5.2,"d":"5.20"},{"v":60,"d":"60.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BS934","hlavica tlačidla núdzového zastavenia Ø 30 mm - uvoľniť kľúčom - Ø 22 - červená",0]
["ZA2BS844","OVLÁDAČ PRE XAC",1,"ks",{"v":26.537175,"d":"26.537"},"3389110591767",{"v":10,"d":"10.00"},{"v":4.1,"d":"4.10"},{"v":11,"d":"11.00"},{"v":42.6,"d":"42.60"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BS844","hlavica tlačidla núdzového zastavenia Ø 40 mm-uvoľniť pootočením-Ø 22-červená",0]
["ZA2BS834","OVLÁDAČ PRE XAC",1,"ks",{"v":28.367324999999997,"d":"28.367"},"3389110591750",{"v":4.4,"d":"4.40"},{"v":4.4,"d":"4.40"},{"v":9.3,"d":"9.30"},{"v":40,"d":"40.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BS834","hlavica tlačidla núdzového zastavenia Ø 30 mm-uvoľniť pootočením-Ø 22-červená",0]
["ZA2BP2","OVLÁDAČ PRE XAC",1,"ks",{"v":10.065825,"d":"10.066"},"3389110647969",{"v":6,"d":"6.00"},{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":16,"d":"16.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BP2","hlavica tlačidla - Ø 22 - čierna - booted",0]
["ZA2BG6","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3389110648645",{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":3,"d":"3.00"},{"v":50.9,"d":"50.90"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BG6","ovládacia hlavica s kľúčom",0]
["ZA2BG5","OVLÁDAČ PRE XAC",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3389110645330",{"v":9.7,"d":"9.70"},{"v":3.9,"d":"3.90"},{"v":6.9,"d":"6.90"},{"v":42,"d":"42.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BG5","ovl. hlavica otočná s kľúčom-3 polohy-Ø 22-čierna",0]
["ZA2BG4","OVLÁDAČ PRE XAC",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3389110645323",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":49,"d":"49.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BG4","ovl. hlavica otočná s kľúčom-2 polohy-Ø 22-čierna",0]
["ZA2BG3","OVL. HLAVICA OTOČ. SO ZÁMKOM",1,"ks",{"v":38.43315,"d":"38.433"},"3389110648669",{"v":10.1,"d":"10.10"},{"v":3.4,"d":"3.40"},{"v":6.9,"d":"6.90"},{"v":50,"d":"50.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BG3","Selector switch, Harmony XAC, plastic, black, 3 positions, left withdrawal position, stay put",0]
["ZA2BG2","OVLÁDAČ PRE XAC",1,"ks",{"v":40.2633,"d":"40.263"},"3389110648621",{"v":9.8,"d":"9.80"},{"v":3.8,"d":"3.80"},{"v":7.2,"d":"7.20"},{"v":42,"d":"42.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BG2","ovl. hlavica otočná s kľúčom-2 polohy-Ø 22-čierna",0]
["ZA2BD5","OVL. HLAVICA OTOČNÁ",1,"ks",{"v":6.9545699999999995,"d":"6.955"},"3389110648560",{"v":3,"d":"3.00"},{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BD5","Selector switch, Harmony XAC, plastic, black handle, 22mm, 3 positions, unmarked",0]
["ZA2BD3","OVLÁDAČ PRE XAC",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110645316",{"v":4.5,"d":"4.50"},{"v":4.2,"d":"4.20"},{"v":3,"d":"3.00"},{"v":21,"d":"21.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BD3","ovl. hlavica otočná s kľúčom-3 polohy-Ø 22-čierna",0]
["ZA2BD2","OVLÁDAČ PRE XAC",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110645309",{"v":5,"d":"5.00"},{"v":4,"d":"4.00"},{"v":4,"d":"4.00"},{"v":18,"d":"18.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BD2","ovl. hlavica otočná s kľúčom-2 polohy-Ø 22-čierna",0]
["ZA2BB2","OVLÁDAČ PRE XAC",1,"ks",{"v":100.65825,"d":"100.658"},"3389110591224",{"v":10.5,"d":"10.50"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":60,"d":"60.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ZA2BB2","čierny WOBBLESTICK ZA2BB2",0]
["XVUZ800","Upevňov.podstavec s Al trubkou,800m,čier",1,"ks",{"v":77.3238375,"d":"77.324"},"3606485433172",{"v":96.5,"d":"96.50"},{"v":9,"d":"9.00"},{"v":9.5,"d":"9.50"},{"v":430,"d":"430.00"},"ID","3926909790","https://www.se.com/sk/sk/product/XVUZ800","upevňujúci podstavec s Al rúrkou, 800 mm, čierna",0]
["XVUZ400T","СКОБА МЕТАЛНА WITH 400MM POLE, BLACK",1,"ks",{"v":51.70173749999999,"d":"51.702"},"3606480887147",{"v":56.7,"d":"56.70"},{"v":9.3,"d":"9.30"},{"v":9,"d":"9.00"},{"v":320,"d":"320.00"},"ID","8536699099","https://www.se.com/sk/sk/product/XVUZ400T","konzola s Al rúrkou na montáž na zvislé plochy, 400 mm, čierna",0.08]
["XVUZ400","Upevňovací podstavec s Al trubkou, 400 m",1,"ks",{"v":48.498974999999994,"d":"48.499"},"3606485433165",{"v":56.7,"d":"56.70"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":236,"d":"236.00"},"ID","8536699099","https://www.se.com/sk/sk/product/XVUZ400","upevňujúci podstavec s Al rúrkou, 400 mm, čierna",0]
["XVUZ250T","Konzola s Al trubkou pre montáž na zvisl",1,"ks",{"v":42.09345,"d":"42.093"},"3606480887130",{"v":36.6,"d":"36.60"},{"v":9,"d":"9.00"},{"v":9.5,"d":"9.50"},{"v":240,"d":"240.00"},"ID","7616999099","https://www.se.com/sk/sk/product/XVUZ250T","konzola s Al rúrkou na montáž na zvislé plochy, 250 mm, čierna",0]
["XVUZ12","Konzola pre montáž na zvislé plochy,čier",1,"ks",{"v":21.5042625,"d":"21.504"},"3606480887154",{"v":11.412,"d":"11.41"},{"v":5.068,"d":"5.07"},{"v":6.844,"d":"6.84"},{"v":360,"d":"360.00"},"ID","7907000090","https://www.se.com/sk/sk/product/XVUZ12","konzola na montáž na zvislé plochy, čierna",0]
["XVUZ100T","Konzola s Al trub.mont.zvis.plochy 100mm",1,"ks",{"v":28.367324999999997,"d":"28.367"},"3606480887123",{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":19,"d":"19.00"},{"v":220,"d":"220.00"},"ID","7616999099","https://www.se.com/sk/sk/product/XVUZ100T","konzola s Al rúrkou na montáž na zvislé plochy, 100 mm, čierna",0]
["XVUZ06","Nastaviteľný kĺb XVU, čierna",1,"ks",{"v":47.58389999999999,"d":"47.584"},"3606480555992",{"v":26.8,"d":"26.80"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":193,"d":"193.00"},"CZ","8531900000","https://www.se.com/sk/sk/product/XVUZ06","nastaviteľný kĺb pre montáž na šikmé a zvislé plochy, IP 55 - čierny",0]
["XVUZ05","Výškovo nastaviteľ.podstavec XVU, čierna",1,"ks",{"v":100.65825,"d":"100.658"},"3606480556005",{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":26.8,"d":"26.80"},{"v":253,"d":"253.00"},"CZ","8531900000","https://www.se.com/sk/sk/product/XVUZ05","výškovo nastaviteľný podstavec - čierny",0]
["XVUZ04","Nástavec pre priamu montáž XVU, 4 piny",1,"ks",{"v":25.1645625,"d":"25.165"},"3606480711572",{"v":13,"d":"13.00"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":66,"d":"66.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVUZ04","nástavec pre priamu mont.XVU, 4 piny - čierny",0]
["XVUZ03","Nástavec pre priamu montáž, 2 piny",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3606480711565",{"v":13,"d":"13.00"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":60,"d":"60.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVUZ03","nástavec pre priamu mont.XVU, 2 piny - čierny",0]
["XVUZ02Q","Fixný upevňovací podst.XVU 100mm,strieb.",1,"ks",{"v":27.45225,"d":"27.452"},"3606480556029",{"v":26.8,"d":"26.80"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":132,"d":"132.00"},"CZ","8536699099","https://www.se.com/sk/sk/product/XVUZ02Q","fixný upevňoavcí podstavec 100 mm - strieborná",0]
["XVUZ02","Fixný upevňovací podst.XVU 100mm, čierna",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3606480556012",{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":26.8,"d":"26.80"},{"v":132,"d":"132.00"},"CZ","8531900000","https://www.se.com/sk/sk/product/XVUZ02","fixný upevňovací podstavec, 100 mm - čierny",0]
["XVUZ01Q","Nástavec pre priamu montáž XVU, strieb.",1,"ks",{"v":27.45225,"d":"27.452"},"3606480556043",{"v":13.3,"d":"13.30"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":63,"d":"63.00"},"CZ","9030337000","https://www.se.com/sk/sk/product/XVUZ01Q","nástavec pre priamu montáž - strieborná",0]
["XVUZ01","Nástavec pre priamu montáž XVU, čierna",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3606480556036",{"v":9.1,"d":"9.10"},{"v":9,"d":"9.00"},{"v":13.3,"d":"13.30"},{"v":63,"d":"63.00"},"CZ","8531900000","https://www.se.com/sk/sk/product/XVUZ01","nástavec pre priamu montáž - čierny",0]
["XVUC9VP","PWM zvukový modul, čierna",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3606480711558",{"v":26.7,"d":"26.70"},{"v":9,"d":"9.00"},{"v":9.3,"d":"9.30"},{"v":219,"d":"219.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVUC9VP","Ø 60 mm XVU PWM zvukový modul, čierna",0]
["XVUC9V","Zvukový modul 0...86 dB,( 4 vstupy),čier",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3606480555893",{"v":26.5,"d":"26.50"},{"v":9,"d":"9.00"},{"v":9.5,"d":"9.50"},{"v":219,"d":"219.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XVUC9V","zvukový modul XVU, Ø 60 mm - čierny IP54 - 24 V AC/DC",0]
["XVUC9SQ","Zvukový modul XVU, strieborná",1,"ks",{"v":61.310024999999996,"d":"61.310"},"3606480555886",{"v":13.3,"d":"13.30"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":77,"d":"77.00"},"CZ","8531804090","https://www.se.com/sk/sk/product/XVUC9SQ","zvuková signalizácia - strieborná",0]
["XVUC9S","Zvukový modul XVU, čierna",1,"ks",{"v":51.70173749999999,"d":"51.702"},"3606480555879",{"v":9.1,"d":"9.10"},{"v":9,"d":"9.00"},{"v":13.3,"d":"13.30"},{"v":77,"d":"77.00"},"CZ","8531804090","https://www.se.com/sk/sk/product/XVUC9S","zvuková signalizácia - čierna",0]
["XVUC65","Svetelný modul XVU, prerušovaná sig.",1,"ks",{"v":66.34293749999999,"d":"66.343"},"3606480887086",{"v":13.4,"d":"13.40"},{"v":9,"d":"9.00"},{"v":9.5,"d":"9.50"},{"v":164,"d":"164.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVUC65","Signálny sloup",0.02]
["XVUC64","Svetelný modul XVU",1,"ks",{"v":65.4278625,"d":"65.428"},"3606480887079",{"v":13.3,"d":"13.30"},{"v":9.2,"d":"9.20"},{"v":9.2,"d":"9.20"},{"v":164,"d":"164.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVUC64","Harmony XVU, Illuminated LED unit for modular tower lights, red, Ø60, high flashing, IP65, 24 V AC/DC",0.02]
["XVUC48","Svetelný modul XVU, preruš.signaliz.žltá",1,"ks",{"v":64.51278749999999,"d":"64.513"},"3606480886997",{"v":13.3,"d":"13.30"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":64,"d":"64.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVUC48","svetelný modul XVU - svetelný modul XVU, prerušovaná signalizácia, žltá",0.02]
["XVUC47","Svetelný modul XVU,preruš.signaliz.biela",1,"ks",{"v":63.140175,"d":"63.140"},"3606480886980",{"v":13.3,"d":"13.30"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":64,"d":"64.00"},"ID","85319000","https://www.se.com/sk/sk/product/XVUC47","svetelný modul XVU - svetelný modul XVU, prerušovaná signalizácia, biela",0.02]
["XVUC46","Svetelný modul XVU, prerušovaná signaliz",1,"ks",{"v":64.51278749999999,"d":"64.513"},"3606480886973",{"v":13.3,"d":"13.30"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":64,"d":"64.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVUC46","svetelný modul XVU - svetelný modul XVU, prerušovaná signalizácia, modrá",0.02]
["XVUC45","Svetel.modul XVU, preruš.signaliz.oranž.",1,"ks",{"v":53.07435,"d":"53.074"},"3606480886966",{"v":13.1,"d":"13.10"},{"v":9,"d":"9.00"},{"v":9.2,"d":"9.20"},{"v":64,"d":"64.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVUC45","svetelný modul XVU - svetelný modul XVU, prerušovaná signalizácia , oranžová",0.02]
["XVUC44","XVU ЧЕРВЕН FLASH LED UNIT",1,"ks",{"v":53.07435,"d":"53.074"},"3606480886959",{"v":13.1,"d":"13.10"},{"v":9,"d":"9.00"},{"v":9.2,"d":"9.20"},{"v":64,"d":"64.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVUC44","svetelný modul XVU - svetelný modul XVU, prerušovaná signalizácia , červená",0.02]
["XVUC43","Svetelný modul XVU,preruš.signal. zelená",1,"ks",{"v":53.07435,"d":"53.074"},"3606480886942",13.46,{"v":9.4,"d":"9.40"},{"v":9.4,"d":"9.40"},{"v":64,"d":"64.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVUC43","svetelný modul XVU - svetelný modul XVU, prerušovaná signalizácia, zelená",0.02]
["XVUC29P","PWM viacfarebný LED modul XVU",1,"ks",{"v":100.65825,"d":"100.658"},"3606480711541",{"v":13,"d":"13.00"},{"v":9.3,"d":"9.30"},{"v":9.2,"d":"9.20"},{"v":69,"d":"69.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVUC29P","PWM viacfarebný LED modul XVU",0.03]
["XVUC29","Viacfarebný modul XVU",1,"ks",{"v":100.65825,"d":"100.658"},"3606480555862",{"v":13.3,"d":"13.30"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":64,"d":"64.00"},"CZ","8531807000","https://www.se.com/sk/sk/product/XVUC29","Ø 60 mm podsviet.jednotka LED-trvalá/blesk./otočná-viacfareb.jednotka-IP65-24 V",0.03]
["XVUC28","Svetelný modul XVU, žltá",1,"ks",{"v":44.838674999999995,"d":"44.839"},"3606480711589",{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":13,"d":"13.00"},{"v":64,"d":"64.00"},"CZ","8531807000","https://www.se.com/sk/sk/product/XVUC28","svetelný modul XVU, Ø 60 mm žltý - IP65 - 24 V AC/DC",0.02]
["XVUC27","Svetelný modul XVU, biela",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3606480555855",{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":13.3,"d":"13.30"},{"v":64,"d":"64.00"},"CZ","8531807000","https://www.se.com/sk/sk/product/XVUC27","Ø 60 mm sveteľný LED modul - stála signalizácia, IP65 - 24 V - biela",0.02]
["XVUC26","Svetelný modul XVU, modrá",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3606480555848",{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":13.3,"d":"13.30"},{"v":64,"d":"64.00"},"CZ","8531807000","https://www.se.com/sk/sk/product/XVUC26","Ø 60 mm sveteľný LED modul - stála signalizácia, IP65 - 24 V - modrá",0.02]
["XVUC25","Svetelný modul XVU, oranžová",1,"ks",{"v":37.518074999999996,"d":"37.518"},"3606480555831",{"v":9.1,"d":"9.10"},{"v":9,"d":"9.00"},{"v":13.3,"d":"13.30"},{"v":64,"d":"64.00"},"CZ","8531807000","https://www.se.com/sk/sk/product/XVUC25","Ø 60 mm sveteľný LED modul - stála signalizácia, IP65 - 24 V - oranžová",0.02]
["XVUC24","Svetelný modul XVU, červená",1,"ks",{"v":37.518074999999996,"d":"37.518"},"3606480555824",{"v":9.1,"d":"9.10"},{"v":9,"d":"9.00"},{"v":13.3,"d":"13.30"},{"v":64,"d":"64.00"},"CZ","8531807000","https://www.se.com/sk/sk/product/XVUC24","Ø 60 mm sveteľný LED modul - stála signalizácia, IP65 - 24 V - červená",0.02]
["XVUC23","Svetelný modul XVU, zelená",1,"ks",{"v":37.518074999999996,"d":"37.518"},"3606480555817",{"v":9.1,"d":"9.10"},{"v":9,"d":"9.00"},{"v":13.3,"d":"13.30"},{"v":64,"d":"64.00"},"CZ","8531807000","https://www.se.com/sk/sk/product/XVUC23","Ø 60 mm sveteľný LED modul - stála signalizácia, IP65 - 24 V - zelená",0.02]
["XVUC21MP","Objímka XVU 100 - 240 V AC, PNP, čierna",1,"ks",{"v":63.140175,"d":"63.140"},"3606480616747",{"v":27,"d":"27.00"},{"v":9.1,"d":"9.10"},{"v":9.5,"d":"9.50"},{"v":235,"d":"235.00"},"CZ","8531900000","https://www.se.com/sk/sk/product/XVUC21MP","objímka s horným krytom 100 - 240 V AC (PNP) - čierna",0]
["XVUC21M","Objímka XVU (AC) NPN, čierna",1,"ks",{"v":65.88539999999999,"d":"65.885"},"3606480555930",{"v":26.8,"d":"26.80"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":235,"d":"235.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVUC21M","Base unit with top cover for modular tower lights, Harmony XVU, black, 60mm, NPN, 100...240V AC",0]
["XVUC21BQ","Objímka XVU 24 V AC/DC, strieborná",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3606480555923",{"v":26.8,"d":"26.80"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":110,"d":"110.00"},"CZ","8531900000","https://www.se.com/sk/sk/product/XVUC21BQ","objímka s horným krytom 24 V AC/DC - strieborná",0]
["XVUC21B","Objímka XVU, 24 V AC/DC, čierna",1,"ks",{"v":29.7399375,"d":"29.740"},"3606480555916",{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":26.8,"d":"26.80"},{"v":110,"d":"110.00"},"CZ","8531900000","https://www.se.com/sk/sk/product/XVUC21B","objímka s horným krytom 24 V AC/DC - čierna",0]
["XVUC020","Dištančný diel XVU 24 V AC/DC, čierna",1,"ks",{"v":30.655012499999998,"d":"30.655"},"3606480555978",{"v":26.8,"d":"26.80"},{"v":9,"d":"9.00"},{"v":9.1,"d":"9.10"},{"v":93,"d":"93.00"},"CZ","8531900000","https://www.se.com/sk/sk/product/XVUC020","distančný diel 24 V AC/DC - čierna",0]
["XVS72BMWP","VIACTÓNOVÝ ALARM",1,"ks",219.618,"3606480032912",{"v":9.5,"d":"9.50"},{"v":10.5,"d":"10.50"},{"v":9.3,"d":"9.30"},{"v":180,"d":"180.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS72BMWP","elektronický alarm XVS - 16 tónov - 0..90 dB - NPN výstup - biela - IP54",0.03]
["XVS72BMWN","VIACTÓNOVÝ ALARM",1,"ks",{"v":164.71349999999998,"d":"164.714"},"3606480032936",{"v":9.4,"d":"9.40"},{"v":10.4,"d":"10.40"},{"v":9.4,"d":"9.40"},{"v":180,"d":"180.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS72BMWN","elektronický alarm XVS - 16 tónov - 0..90 dB - NPN výstup - biela - IP54",0.03]
["XVS72BMBP","VIACTÓNOVÝ ALARM",1,"ks",219.618,"3606480032905",{"v":9.5,"d":"9.50"},{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":180,"d":"180.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS72BMBP","elektronický alarm XVS - 16 tónov - 0..90 dB - NPN výstup - čierna - IP54",0.03]
["XVS72BMBN","VIACTÓNOVÝ ALARM",1,"ks",{"v":164.71349999999998,"d":"164.714"},"3606480032929",10.41,{"v":9.4,"d":"9.40"},{"v":9.4,"d":"9.40"},{"v":270,"d":"270.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS72BMBN","elektronický alarm XVS - 16 tónov - 0..90 dB - NPN výstup - čierna - IP54",0.03]
["XVS14MMW","VIACTÓNOVÁ ALARM SIRÉNA 240V AC",1,"ks",{"v":338.57775,"d":"338.578"},"3606480072055",{"v":27.5,"d":"27.50"},{"v":15.5,"d":"15.50"},{"v":15.5,"d":"15.50"},{"v":1200,"d":"1,200.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS14MMW","viactónová siréna XVS - 43 tónov - 0..105 dB - biela - IP53",0.19]
["XVS14BMW","VIACTÓNOVÁ ALARM SIRÉNA",1,"ks",{"v":311.1255,"d":"311.126"},"3606480032943",{"v":18.5,"d":"18.50"},{"v":30,"d":"30.00"},{"v":18,"d":"18.00"},{"v":1307,"d":"1,307.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS14BMW","viactónová siréna XVS - 43 tónov - 0..105 dB - biela - IP53",0.16]
["XVS10MMW","SIRÉNA 106dB",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389119045360",{"v":14,"d":"14.00"},{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":1242,"d":"1,242.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS10MMW","sirena - 2 tóny - 106 dB - biela - IP53",0.15]
["XVS10GMW","SIRÉNA 106dB",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389119045353",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":14,"d":"14.00"},{"v":1226,"d":"1,226.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS10GMW","sirena - 2 tóny - 106 dB - biela - IP53",0.15]
["XVS10BMW","SIRÉNA 106dB",1,"ks",{"v":187.59037499999997,"d":"187.590"},"3389119045346",{"v":14,"d":"14.00"},{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":800,"d":"800.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVS10BMW","sirena - 2 tóny - 106 dB - biela - IP53",0.12]
["XVR3M06S","Rotačný maják, bzučiak, AC 100～230V, mod",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3606480611919",{"v":13.6,"d":"13.60"},{"v":18.1,"d":"18.10"},{"v":13.6,"d":"13.60"},{"v":678,"d":"678.00"},"CN","8531804090","https://www.se.com/sk/sk/product/XVR3M06S","rotačný maják, bzučiak, AC 100～230 V, modrá",0.1]
["XVR3M06","Rotačný maják, bez bzučiaku, AC 100～230V",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611834",{"v":13.6,"d":"13.60"},{"v":18.1,"d":"18.10"},{"v":13.6,"d":"13.60"},{"v":484,"d":"484.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XVR3M06","rotačný maják, bez bzučiaku, AC 100～230 V, modrá",0.1]
["XVR3M05S","Rotačný maják, bzučiak, AC 100～230V, ora",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3606480611902",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":538,"d":"538.00"},"CN","8531804090","https://www.se.com/sk/sk/product/XVR3M05S","rotačný maják, bzučiak, AC 100～230 V, oranžová",0]
["XVR3M05","Rotačný maják, bez bzučiaku, AC 100～230V",1,"ks",{"v":169.288875,"d":"169.289"},"3606480611827",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":484,"d":"484.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XVR3M05","rotačný maják, bez bzučiaku, AC 100～230 V, oranžová",0.09]
["XVR3M04S","Rotačný maják, bzučiak, AC 100～230V, čer",1,"ks",{"v":205.891875,"d":"205.892"},"3606480611896",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":538,"d":"538.00"},"CN","8531804090","https://www.se.com/sk/sk/product/XVR3M04S","rotačný maják, bzučiak, AC 100～230 V, červená",0.07]
["XVR3M04","Rotačný maják, bez bzučiaku, AC 100～230V",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611810",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":484,"d":"484.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XVR3M04","rotačný maják, bez bzučiaku, AC 100～230 V, červená",0.07]
["XVR3M03S","Rotačný maják, bzučiak, AC 100～230V, zel",1,"ks",{"v":205.891875,"d":"205.892"},"3606480611889",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":538,"d":"538.00"},"CN","8531804090","https://www.se.com/sk/sk/product/XVR3M03S","rotačný maják, bzučiak, AC 100～230 V, zelená",0.1]
["XVR3M03","Rotačný maják, bez bzučiaku, AC 100～230V",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611803",{"v":13.7,"d":"13.70"},{"v":18.1,"d":"18.10"},{"v":13.5,"d":"13.50"},{"v":484,"d":"484.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XVR3M03","rotačný maják, bez bzučiaku, AC 100～230 V, zelená",0.1]
["XVR3E06","Rotačný maják, bez bzučiaku, DC48V, modr",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611957",{"v":10.2,"d":"10.20"},{"v":10.2,"d":"10.20"},{"v":15.6,"d":"15.60"},{"v":546,"d":"546.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XVR3E06","rotačný maják, bez bzučiaku, DC 48 V, modrá",0.08]
["XVR3E05","Rotačný maják, bez bzučiaku, DC48V, oran",1,"ks",{"v":169.288875,"d":"169.289"},"3606480611940",{"v":13.6,"d":"13.60"},{"v":18.2,"d":"18.20"},{"v":13.5,"d":"13.50"},{"v":642,"d":"642.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XVR3E05","rotačný maják, bez bzučiaku, DC 48 V, oranžová",0.1]
["XVR3E04","Rotačný maják, bez bzučiaku, DC48V, červ",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611933",{"v":13.6,"d":"13.60"},{"v":18.2,"d":"18.20"},{"v":13.5,"d":"13.50"},{"v":649,"d":"649.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XVR3E04","rotačný maják, bez bzučiaku, DC 48 V, červená",0.1]
["XVR3E03","Rotačný maják, bez bzučiaku, DC48V, zele",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611926",{"v":10.2,"d":"10.20"},{"v":10.2,"d":"10.20"},{"v":15.6,"d":"15.60"},{"v":484,"d":"484.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XVR3E03","rotačný maják, bez bzučiaku, DC 48 V, zelená",0.08]
["XVR3B06S","Rotačný maják, bzučiak, DC 12～24V, modrá",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3606480611872",{"v":13.8,"d":"13.80"},{"v":18.5,"d":"18.50"},{"v":14.3,"d":"14.30"},3.68,"CN","8531804090","https://www.se.com/sk/sk/product/XVR3B06S","rotačný maják, bzučiak, DC 12～24 V, modrá",0.1]
["XVR3B06","Rotačný maják, bez bzučiaku, DC 12～24V,",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611797",{"v":13.8,"d":"13.80"},{"v":18.5,"d":"18.50"},{"v":14.3,"d":"14.30"},{"v":3680,"d":"3,680.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XVR3B06","rotačný maják, bez bzučiaku, DC 12～24 V, modrá",0]
["XVR3B05S","Rotačný maják, bzučiak, DC 12～24V, oranž",1,"ks",{"v":201.3165,"d":"201.317"},"3606480611865",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":538,"d":"538.00"},"CN","8531804090","https://www.se.com/sk/sk/product/XVR3B05S","rotačný maják, bzučiak, DC 12～24 V, oranžová",0]
["XVR3B05","Rotačný maják, bez bzučiaku, DC 12～24V,",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611780",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":484,"d":"484.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XVR3B05","rotačný maják, bez bzučiaku, DC 12～24 V, oranžová",0]
["XVR3B04S","Rotačný maják, bzučiak, DC 12～24V, červe",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3606480611858",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":538,"d":"538.00"},"CN","8531804090","https://www.se.com/sk/sk/product/XVR3B04S","rotačný maják, bzučiak, DC 12～24 V, červená",0.07]
["XVR3B04","Rotačný maják, bez bzučiaku, DC 12～24V,",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611773",{"v":18.5,"d":"18.50"},{"v":13.5,"d":"13.50"},13.85,{"v":484,"d":"484.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XVR3B04","rotačný maják, bez bzučiaku, DC 12～24 V, červená",0.07]
["XVR3B03S","Rotačný maják, bzučiak, DC 12～24V, zelen",1,"ks",{"v":205.891875,"d":"205.892"},"3606480611841",{"v":13.8,"d":"13.80"},{"v":18.5,"d":"18.50"},{"v":14.3,"d":"14.30"},{"v":3680,"d":"3,680.00"},"CN","8531804090","https://www.se.com/sk/sk/product/XVR3B03S","rotačný maják, bzučiak, DC 12～24 V, zelená",0.1]
["XVR3B03","Rotačný maják, bez bzučiaku, DC 12～24V",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480611766",{"v":13.8,"d":"13.80"},{"v":18.5,"d":"18.50"},{"v":14.3,"d":"14.30"},{"v":3680,"d":"3,680.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XVR3B03","rotačný maják, bez bzučiaku, DC 12～24 V, zelená",0]
["XVR13M05L","ROTAČNÝ MAJÁK LED, 230V ORANŽ.",1,"ks",{"v":242.494875,"d":"242.495"},"3389119045339",{"v":26.5,"d":"26.50"},{"v":19.5,"d":"19.50"},{"v":19.5,"d":"19.50"},{"v":990,"d":"990.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR13M05L","Ø 130 mm predzapojený rotačný maják bez bzučiaka - oranžová - 230 V",0.2]
["XVR13M04L","ROTAČNÝ MAJÁK LED, 230V ČERV.",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3389119045322",{"v":19,"d":"19.00"},{"v":27.5,"d":"27.50"},{"v":19,"d":"19.00"},{"v":990,"d":"990.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR13M04L","Ø 130 mm predzapojený rotačný maják bez bzučiaka - červená - 230 V",0.2]
["XVR13G05L","ROTAČNÝ MAJÁK LED, 120V ORANŽ.",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3389119045315",{"v":18.8,"d":"18.80"},{"v":27,"d":"27.00"},{"v":18.7,"d":"18.70"},{"v":990,"d":"990.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR13G05L","Ø 130 mm predzapojený rotačný maják bez bzučiaka - oranžová - 120 V",0.2]
["XVR13G04L","ROTAČNÝ MAJÁK LED, 120V ČERV.",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3389119045308",{"v":20,"d":"20.00"},{"v":30.5,"d":"30.50"},{"v":20,"d":"20.00"},{"v":990,"d":"990.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR13G04L","Ø 130 mm predzapojený rotačný maják bez bzučiaka - červená - 120 V",0.2]
["XVR13B05L","ROTAČNÝ MAJÁK LED, 24V ORANŽ.",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389119045292",{"v":18.7,"d":"18.70"},{"v":27,"d":"27.00"},{"v":18.7,"d":"18.70"},{"v":1142,"d":"1,142.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR13B05L","Ø 130 mm predzapojený rotačný maják bez bzučiaka - oranžová - 24 V",0.17]
["XVR13B05","ROTAČNÝ MAJÁK LED, 130 MM 24 V, ORANŽ.",1,"ks",{"v":224.193375,"d":"224.193"},"3606480033308",{"v":18.8,"d":"18.80"},{"v":26.5,"d":"26.50"},{"v":18.8,"d":"18.80"},{"v":800,"d":"800.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVR13B05","Ø 130 mm predzapojený rotačný maják bez bzučiakom - oranžová - 24 V",0.18]
["XVR13B04L","ROTAČNÝ MAJÁK LED, 24V ČERV.",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389119045285",{"v":18.8,"d":"18.80"},{"v":26.5,"d":"26.50"},{"v":18.7,"d":"18.70"},{"v":820,"d":"820.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR13B04L","Ø 130 mm predzapojený rotačný maják bez bzučiaka - červená - 24 V",0.17]
["XVR13B04","ROTAČNÝ MAJÁK LED 130MM 24V ČERV.",1,"ks",{"v":215.042625,"d":"215.043"},"3606480033292",{"v":26.6,"d":"26.60"},{"v":18.7,"d":"18.70"},{"v":18.7,"d":"18.70"},{"v":800,"d":"800.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR13B04","Ø 130 mm predzapojený rotačný maják bez bzučiakom - červená - 24 V",0.18]
["XVR12B06S","ROTAČNÝ MAJÁK LED 120MM ZVUKOVÁ SIGN.",1,"ks",{"v":205.891875,"d":"205.892"},"3606480033261",{"v":14,"d":"14.00"},{"v":19.5,"d":"19.50"},{"v":13.8,"d":"13.80"},{"v":617,"d":"617.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR12B06S","Ø Ø20 mm predzapojený rotačný maják bez bzučiaka - modrá - 24 V",0.09]
["XVR12B06","ROTAČNÝ MAJÁK LED 120MM 24V MOD.",1,"ks",{"v":169.288875,"d":"169.289"},"3606480033186",{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":14.2,"d":"14.20"},{"v":634,"d":"634.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR12B06","Ø Ø20 mm predzapojený rotačný maják bez bzučiaka - modrá - 24 V",0.09]
["XVR12B05S","ROTAČNÝ MAJÁK LED 120MM BZUČIAK.",1,"ks",{"v":205.891875,"d":"205.892"},"3606480033247",{"v":19.5,"d":"19.50"},{"v":13.8,"d":"13.80"},{"v":13.8,"d":"13.80"},{"v":659,"d":"659.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR12B05S","Ø Ø20 mm predzapojený rotačný maják bez bzučiaka - oranžová - 24 V",0.1]
["XVR12B05","ROTAČNÝ MAJÁK LED 120MM 24V ORANŽ",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480033162",{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":14.2,"d":"14.20"},{"v":637,"d":"637.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR12B05","Ø Ø20 mm predzapojený rotačný maják bez bzučiakom - oranžová - 24 V",0.09]
["XVR12B04S","ROTAČNÝ MAJÁK LED 120MM BZUČIAK",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3606480033230",{"v":14,"d":"14.00"},{"v":19.5,"d":"19.50"},{"v":13.8,"d":"13.80"},{"v":652,"d":"652.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR12B04S","Ø Ø20 mm predzapojený rotačný maják bez bzučiaka - červená - 24 V",0.1]
["XVR12B04","ROTAČNÝ MAJÁK LED 120MM 24V ČER.",1,"ks",{"v":205.891875,"d":"205.892"},"3606480033155",{"v":14,"d":"14.00"},{"v":19.5,"d":"19.50"},{"v":13.8,"d":"13.80"},{"v":612,"d":"612.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVR12B04","Ø Ø20 mm predzapojený rotačný maják bez bzučiakom - červená - 24 V",0.09]
["XVR10B05","Rotačný maják, 106mm, LED 24V, Oranž.",1,"ks",{"v":160.138125,"d":"160.138"},"3606480033087",{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":14,"d":"14.00"},{"v":500,"d":"500.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVR10B05","Ø 106 mm predzapojený rotačný maják bez bzučiakom - oranžová - 24 V",0.09]
["XVR10B04","ROTAČNÝ MAJÁK LED 106MM 24V ČERV.",1,"ks",{"v":155.56275,"d":"155.563"},"3606480033070",{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":14,"d":"14.00"},{"v":500,"d":"500.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVR10B04","Ø 106 mm predzapojený rotačný maják bez bzučiaka - červená - 24 V",0.09]
["XVR08B06","ROTAČNÝ MAJÁK LED 84MM 24V MOD.",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480033025",{"v":9.5,"d":"9.50"},{"v":18.5,"d":"18.50"},{"v":9.5,"d":"9.50"},{"v":390,"d":"390.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR08B06","Ø 84 mm predzapojený rotačný maják bez bzučiaka - modrá - 24 V",0.06]
["XVR08B04","ROTAČNÝ MAJÁK LED 84MM 24V ČER.",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480032998",{"v":9.8,"d":"9.80"},{"v":18.5,"d":"18.50"},{"v":9.8,"d":"9.80"},{"v":395,"d":"395.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR08B04","Ø 84 mm predzapojený rotačný maják bez bzučiaka - červená - 24 V",0.06]
["XVR08B03","ROTAČNÝ MAJÁK LED 84MM 24V ZEL.",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480033018",{"v":10,"d":"10.00"},{"v":19,"d":"19.00"},{"v":9.8,"d":"9.80"},{"v":300,"d":"300.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVR08B03","Ø 84 mm predzapojený rotačný maják bez bzučiaka - zelená - 24 V",0.06]
["XVR012L","UPEVŇOVACIA DOSKA VERTIKÁLNA",1,"ks",{"v":34.3153125,"d":"34.315"},"3389119049337",{"v":22.5,"d":"22.50"},{"v":10,"d":"10.00"},{"v":17,"d":"17.00"},{"v":1177,"d":"1,177.00"},"JP","8531900000","https://www.se.com/sk/sk/product/XVR012L","konzola pre zvislú montáž",0]
["XVMZ06","PLASTOVÝ STOJAN",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389119053167",{"v":7.5,"d":"7.50"},{"v":5,"d":"5.00"},{"v":7.5,"d":"7.50"},{"v":50,"d":"50.00"},"ID","39269097","https://www.se.com/sk/sk/product/XVMZ06","XVM plastový podstavec",0.01]
["XVMZ04T","Potrubie 400mm + L konzola",1,"ks",{"v":48.498974999999994,"d":"48.499"},"3389119004428",{"v":40,"d":"40.00"},{"v":4.4,"d":"4.40"},{"v":6,"d":"6.00"},{"v":287,"d":"287.00"},"ID","7616999099","https://www.se.com/sk/sk/product/XVMZ04T","Hliníková trubka s kovovým držiakom l=400 mm - XVM",0]
["XVMZ04","HLINÍKOVÝ PODSTAVEC, 400 MM",1,"ks",{"v":25.1645625,"d":"25.165"},"3389119004398",{"v":41,"d":"41.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":202,"d":"202.00"},"ID","7616999099","https://www.se.com/sk/sk/product/XVMZ04","signálny stĺp s upevňovacou doskou l=400 mm - hliník biela - XVM",0]
["XVMZ03T","HLINÍKOVÁ TRUBICA 250MM VERTIKÁLNA",1,"ks",{"v":19.216575,"d":"19.217"},"3389119004411",{"v":6.1,"d":"6.10"},{"v":29.1,"d":"29.10"},{"v":3.5,"d":"3.50"},{"v":242,"d":"242.00"},"ID","7616999099","https://www.se.com/sk/sk/product/XVMZ03T","hliníková trubka s kovovým držiakom l=250 mm - XVM",0]
["XVMZ03","HLINÍKOVÝ PODSTAVEC, 250 MM",1,"ks",{"v":19.216575,"d":"19.217"},"3389119004381",{"v":7.1,"d":"7.10"},{"v":26,"d":"26.00"},{"v":7.1,"d":"7.10"},{"v":148,"d":"148.00"},"ID","7616999099","https://www.se.com/sk/sk/product/XVMZ03","signálny stĺp s upevňovacou doskou l=250 mm - hliník biela - XVM",0]
["XVMZ02T","HLINÍKOVÁ TRUBICA 100MM VERTIKÁLNA",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389119004404",{"v":18,"d":"18.00"},{"v":4,"d":"4.00"},{"v":13,"d":"13.00"},{"v":198,"d":"198.00"},"ID","7616999099","https://www.se.com/sk/sk/product/XVMZ02T","hliníková trubka s kovovým držiakom l=100 mm - XVM",0]
["XVMZ02","HLINÍKOVÝ PODSTAVEC 100 MM",1,"ks",{"v":19.216575,"d":"19.217"},"3389119004374",{"v":17.8,"d":"17.80"},{"v":7,"d":"7.00"},{"v":7.6,"d":"7.60"},{"v":81,"d":"81.00"},"ID","7616999099","https://www.se.com/sk/sk/product/XVMZ02","signálny stĺp s upevňovacou doskou l=100 mm - hliník biela - XVM",0]
["XVMM2RGSSB","230VAC ČER+ZEL STÁLA 250MM ZVUK ZVIS.",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389119050166",{"v":54,"d":"54.00"},{"v":5.8,"d":"5.80"},{"v":8.5,"d":"8.50"},{"v":529,"d":"529.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMM2RGSSB","signálka s bzučiakom + 2 svietiace jednotky - Ø 45 mm - 230 V AC",0.08]
["XVMM2RGSB","230VAC ČERVENÁ+ZELENÁ STÁLA 250MM ZVIS.",1,"ks",{"v":82.81428749999999,"d":"82.814"},"3389119050159",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":525,"d":"525.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMM2RGSB","signálka s bzučiakom + 2 svietiace jednotky - Ø 45 mm - 230 V AC",0.06]
["XVMM2RAGSSB","230VAC LED ČER+OR+ZEL STÁL ZVUK ZVIS",1,"ks",{"v":150.987375,"d":"150.987"},"3389119050180",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":453,"d":"453.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMM2RAGSSB","signálka s bzučiakom + 3 svietiace jednotky - Ø 45 mm - 230 V AC",0.09]
["XVMM2RAGSB","230VAC ČER+OR+ZEL STÁLA 250MM ZVIS.",1,"ks",109.809,"3389119050135",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":443,"d":"443.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMM2RAGSB","signálka s bzučiakom + 3 svietiace jednotky - Ø 45 mm - 230 V AC",0.07]
["XVMM2R6AGSB","230VAC LED OR+ZEL STÁL ČER ZÁBL ZVIS",1,"ks",{"v":164.71349999999998,"d":"164.714"},"3389119050098",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":456,"d":"456.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMM2R6AGSB","Pre assembled and pre cabled indicator bank, Harmony XVM, without buzzer + 3 illuminated units, Ø 45 mm, 230 VAC",0]
["XVMM1RAG","KOMPLET STĹP, 230 V",1,"ks",{"v":87.38966249999999,"d":"87.390"},"3389119004893",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.3,"d":"8.30"},{"v":545,"d":"545.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMM1RAG","signálny stĺp bez bzučiaku + 3 svetelné návestia - Ø 45 mm - 230 V AC/DC - IP42",0.08]
["XVMG2RAGSB","120VAC ČER+OR+ZEL STÁLA 250MM ZVIS.",1,"ks",109.809,"3389119049993",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":443,"d":"443.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMG2RAGSB","Harmony XVM, Modular tower lights, aluminium, support tube with bracket, red/orange/green, Ø45, steady, super bright LED, 120 V AC",0]
["XVMC37","SVETEL. BANKA BIELA PRE XVM",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389119004282",{"v":4.8,"d":"4.80"},{"v":7.9,"d":"7.90"},{"v":4.8,"d":"4.80"},{"v":45,"d":"45.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVMC37","svetelné návestie - Ø 45 - číra - BA 15d - bez žiarovky - <lt/>= 230V AC DC",0]
["XVMC36","SVETEL. BANKA MODRÁ PRE XVM",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389119004275",{"v":7.9,"d":"7.90"},{"v":4.8,"d":"4.80"},{"v":4.8,"d":"4.80"},{"v":40,"d":"40.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVMC36","svetelné návestie - Ø 45 - modrá - BA 15d - bez žiarovky - <lt/>= 230V AC DC",0]
["XVMC35","SVETEL. BANKA ŽLTÁ PRE XVM",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389119004268",{"v":10.1,"d":"10.10"},{"v":5.1,"d":"5.10"},{"v":7.2,"d":"7.20"},{"v":48,"d":"48.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVMC35","svetelné návestie - Ø 45 - žltá - BA 15d - bez žiarovky - <lt/>= 230V AC DC",0]
["XVMC34","SVETEL. BANKA ČERVENÁPRE XVM",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389119004251",{"v":12.9,"d":"12.90"},{"v":5.1,"d":"5.10"},{"v":7.2,"d":"7.20"},{"v":48,"d":"48.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVMC34","svetelné návestie - Ø 45 - červená - BA 15d - bez žiarovky - <lt/>= 230V AC DC",0]
["XVMC33","SVETEL. BANKA ZELENÁ PRE XVM",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389119004244",{"v":10.4,"d":"10.40"},{"v":5.1,"d":"5.10"},{"v":6.8,"d":"6.80"},{"v":40,"d":"40.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVMC33","svetelné návestie - Ø 45 - zelená - BA 15d - bez žiarovky - <lt/>= 230V AC DC",0]
["XVMC29M","ZÁKLADŇA SO ZVUK. SIGNALIZÁCIOU 230V",1,"ks",{"v":65.4278625,"d":"65.428"},"3389119004329",{"v":6.5,"d":"6.50"},{"v":4.8,"d":"4.80"},{"v":4.8,"d":"4.80"},{"v":65,"d":"65.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMC29M","objímka s bzučiakom a krytom - Ø 45 - 230 V - 4 kHz - biela - XVM",0.01]
["XVMC29B","ZÁKLADNÁ OBJÍMKA S BZUČIAKOM 24V",1,"ks",{"v":54.4469625,"d":"54.447"},"3389119004305",{"v":9.9,"d":"9.90"},{"v":5.2,"d":"5.20"},{"v":9.5,"d":"9.50"},{"v":72,"d":"72.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMC29B","objímka s bzučákom a krytom - biela - 24 V - Ø 45",0.01]
["XVMC21","ZÁKLADŇA + KRYT",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389119004299",{"v":4.8,"d":"4.80"},{"v":6,"d":"6.00"},{"v":4.8,"d":"4.80"},{"v":55,"d":"55.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVMC21","základná jednotka s krytom XVM - Ø 45 mm - biela - šróbové svorky - IP40",0]
["XVMB2RSWSB","24VAC/DC LED ČERVENÁ STÁLA ZVUK VOD.",1,"ks",{"v":64.05524999999999,"d":"64.055"},"3389119053044",{"v":16.5,"d":"16.50"},{"v":7.6,"d":"7.60"},{"v":7.6,"d":"7.60"},{"v":153,"d":"153.00"},"ID","9030337000","https://www.se.com/sk/sk/product/XVMB2RSWSB","maják s bzučiakom + 1 svietiaca jednotka- Ø 45 mm - 230 V AC/DC",0.03]
["XVMB2RSB","24VAC/DC LED ČERVENÁ STÁLA ZVIS.",1,"ks",{"v":64.51278749999999,"d":"64.513"},"3389119051217",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":456,"d":"456.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RSB","Harmony XVM, Modular tower lights, aluminium, support tube with bracket, red, Ø45, steady, super bright LED, 24 V AC/DC",0.07]
["XVMB2RGSSB","24VAC/DC ČER+ZEL STÁLA 250MM ZVUK ZVIS.",1,"ks",{"v":91.5075,"d":"91.508"},"3389119050319",{"v":54,"d":"54.00"},{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},{"v":404,"d":"404.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RGSSB","signálka s bzučiakom + 2 svietiace jednotky - Ø 45 mm - 24 V AC/DC",0.06]
["XVMB2RGSB","24VAC/DC ČERVENÁ+ZELENÁ STÁLA 250MM ZVIS",1,"ks",{"v":64.97032499999999,"d":"64.970"},"3389119050296",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.3,"d":"8.30"},{"v":395,"d":"395.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RGSB","signálka bez bzučiaka + 2 svietiace jednotky - Ø 45 mm - 24 V AC/DC",0.06]
["XVMB2RAGWSB","24VAC/DC ČERVENÁ+ORANŽ+ZELENÁ STÁLA VOD.",1,"ks",{"v":86.4745875,"d":"86.475"},"3389119052986",{"v":50.4,"d":"50.40"},{"v":7.8,"d":"7.80"},{"v":8.5,"d":"8.50"},{"v":241,"d":"241.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RAGWSB","signálka bez bzučiaka + 3 svietiace jednotky - Ø 45 mm - 24 V AC",0.04]
["XVMB2RAGSWSB","24VAC/DC ČER+OR+ZEL STÁLA ZVUK VOD.",1,"ks",{"v":118.95975,"d":"118.960"},"3389119053105",{"v":50.4,"d":"50.40"},{"v":7.8,"d":"7.80"},{"v":8.5,"d":"8.50"},{"v":251,"d":"251.00"},"ID","9030337000","https://www.se.com/sk/sk/product/XVMB2RAGSWSB","signálka s bzučiakom + 3 svietiace jednotky - Ø 45 mm - 24 V AC",0.04]
["XVMB2RAGSSB","24VAC/DC LED ČER+OR+ZEL STÁL ZVUK ZVIS",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389119050302",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8,"d":"8.00"},{"v":453,"d":"453.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RAGSSB","signálka s bzučiakom + 3 svietiace jednotky - Ø 45 mm - 24 V AC/DC",0.07]
["XVMB2RAGSHSB","24VAC/DC ČER+OR+ZEL STÁLA 250MM ZVUK VOD",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389119050906",{"v":63.4,"d":"63.40"},{"v":7.8,"d":"7.80"},{"v":8.5,"d":"8.50"},{"v":380,"d":"380.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RAGSHSB","signálka s bzučiakom + 3 svietiace jednotky - Ø 45 mm - 24 V AC",0.06]
["XVMB2RAGSB","24VAC/DC ČER+OR+ZEL STÁLA 250MM ZVIS.",1,"ks",{"v":78.69644999999998,"d":"78.696"},"3389119050272",{"v":53.5,"d":"53.50"},{"v":5.3,"d":"5.30"},{"v":8.4,"d":"8.40"},{"v":443,"d":"443.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RAGSB","Harmony XVM, Modular tower lights, aluminium, red/orange/green, Ø45, steady, super bright LED, 24 V AC/DC",0.08]
["XVMB2RAGHSB","24VAC/DC ČER+OR+ZEL STÁLA 250MM VOD.",1,"ks",{"v":86.93212499999998,"d":"86.932"},"3389119050890",{"v":63.4,"d":"63.40"},{"v":7.8,"d":"7.80"},{"v":8.5,"d":"8.50"},{"v":380,"d":"380.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RAGHSB","signálka bez bzučiaka + 3 svietiace jednotky - Ø 45 mm - 24 V AC",0.05]
["XVMB2RAGBSSB","24VAC/DC LED ČER+OR+ZEL+MO STÁL ZVUK ZVI",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389119050333",{"v":67,"d":"67.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":501,"d":"501.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RAGBSSB","signálka s bzučiakom + 4 svietiace jednotky - Ø 45 mm - 24 V AC/DC",0.08]
["XVMB2RAGBSB","24VAC/DC LED ČER+OR+ZEL+MO STÁL ZVISL",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389119050289",{"v":67,"d":"67.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":491,"d":"491.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2RAGBSB","signálka bez bzučiaka + 4 svietiace jednotky - Ø 45 mm - 24 V AC/DC",0.06]
["XVMB2R6AGSSB","24VAC/DC LED OR+ZEL STÁL ČER ZÁBLE Z Z",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389119050340",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":466,"d":"466.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2R6AGSSB","signálka s bzučiakom + 3 svietiace jednotky - Ø 45 mm - 24 V AC/DC",0.06]
["XVMB2R5A5GSB","24VAC/DC LED ZEL STÁL ČER+OR BLIK ZVIS.",1,"ks",{"v":100.65825,"d":"100.658"},"3389119050258",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":443,"d":"443.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB2R5A5GSB","Pre assembled and pre cabled indicator bank, Harmony XVM, without buzzer + 3 illuminated units, Ø 45 mm, 24VAC/DC",0]
["XVMB1RGS","SVETELNÝ STĹP KOMPLETNÝ",1,"ks",{"v":155.56275,"d":"155.563"},"3389119005142",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":518,"d":"518.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB1RGS","signálny stĺp bez bzučiaku + 2 svetelné návestia - Ø 45 mm - 24 V AC/DC - IP42",0.06]
["XVMB1RG","COMPLETE TOWER",1,"ks",{"v":90.13488749999999,"d":"90.135"},"3389119004817",{"v":54,"d":"54.00"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":392,"d":"392.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB1RG","signálny stĺp bez bzučiaku + 2 sveteľné návestia - Ø 45 mm - 24 V AC/DC - IP42",0.06]
["XVMB1RAGS","SVETELNÝ STĹP KOMPLETNÝ 24V ŽIAROVKA",1,"ks",{"v":137.26125,"d":"137.261"},"3389119005203",{"v":55,"d":"55.00"},{"v":5.4,"d":"5.40"},{"v":9.2,"d":"9.20"},{"v":565,"d":"565.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB1RAGS","blok ukazovateľov s bzučiakom+3 osvetl. jednotky – Ø 45 mm – 24 V AC/DC – IP42",0.07]
["XVMB1RAG","SVETELNÝ STĹP KOMPLETNÝ 24V ŽIAROVKA",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389119005081",{"v":53.7,"d":"53.70"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":550,"d":"550.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVMB1RAG","signálny stĺp bez bzučiaku + 3 svetelné návestia - Ø 45 mm - 24 V AC/DC - IP42",0.07]
["XVLZ912","TESNENIE",10,"ks",{"v":0.8693212499999999,"d":"0.869"},"3389110621969",{"v":1.3,"d":"1.30"},{"v":0.1,"d":"0.10"},{"v":1.3,"d":"1.30"},0.12,"FR","4016930090","https://www.se.com/sk/sk/product/XVLZ912","tesn. IP 65 pre jednotku + 12 mm – súprava 10 ks",0]
["XVLZ911","TESNENIE",10,"ks",{"v":0.8693212499999999,"d":"0.869"},"3389110621945",{"v":1,"d":"1.00"},{"v":1E-3,"d":"0.00"},{"v":1,"d":"1.00"},{"v":0.067,"d":"0.07"},"FR","4016930090","https://www.se.com/sk/sk/product/XVLZ911","tesn. IP 65 pre jednotku + 8 mm – súprava 10 ks",0]
["XVLA345","SIGNÁLKA S LED - 12 MM , 48 V , ŽL-OR",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110651768",{"v":6.2,"d":"6.20"},{"v":2.2,"d":"2.20"},{"v":5.2,"d":"5.20"},{"v":7.3,"d":"7.30"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA345","okrúhla kontrolka Ø 12 – IP40 – žltooranžová – krytá LED – 48 V – očká",0]
["XVLA344","SIGNÁLKA S LED - 12 MM , 48 V , ČERV",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110651744",{"v":6.3,"d":"6.30"},{"v":2.2,"d":"2.20"},{"v":3.9,"d":"3.90"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA344","okrúhla kontrolka Ø 12 – IP40 – červená – krytá LED – 48 V – očká",0]
["XVLA343","SIGNÁLKA S LED - 12 MM , 48 V , ZE",1,"ks",{"v":10.5233625,"d":"10.523"},"3389110651720",{"v":2.7,"d":"2.70"},{"v":2,"d":"2.00"},{"v":7.2,"d":"7.20"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA343","okrúhla kontrolka Ø 12 – IP40 – zelená – krytá LED – 48 V – očká",0]
["XVLA335","SIGNÁLKA S LED - 12 MM , 24 V,ŽL-OR",1,"ks",{"v":10.065825,"d":"10.066"},"3389110651706",{"v":4.9,"d":"4.90"},{"v":1.6,"d":"1.60"},{"v":1.6,"d":"1.60"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA335","okrúhla kontrolka Ø 12 – IP40 – žltooranžová – krytá LED – 24 V – očká",0]
["XVLA334","SIGNÁLKA S LED - 12 MM , 24 V,ČERV",1,"ks",{"v":10.065825,"d":"10.066"},"3389110651683",{"v":4.5,"d":"4.50"},{"v":2.5,"d":"2.50"},{"v":2.5,"d":"2.50"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA334","okrúhla kontrolka Ø 12 – IP40 – červená – krytá LED – 24 V – očká",0]
["XVLA333","SIGNÁLKA S LED - 12 MM , 24 V, ZE",1,"ks",{"v":10.065825,"d":"10.066"},"3389110651669",{"v":4.9,"d":"4.90"},{"v":1.6,"d":"1.60"},{"v":1.6,"d":"1.60"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA333","okrúhla kontrolka Ø 12 – IP40 – zelená – krytá LED – 24 V – očká",0]
["XVLA325","SIGNÁLKA S LED - 12 MM, 12 V , ŽL-OR",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110651645",{"v":6.4,"d":"6.40"},{"v":2.1,"d":"2.10"},{"v":4.9,"d":"4.90"},{"v":6,"d":"6.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA325","okrúhla kontrolka Ø 12 – IP40 – žltooranžová – krytá LED – 12 V – očká",0]
["XVLA324","SIGNÁLKA S LED - 12 MM, 12 V , ČERV",1,"ks",{"v":9.6082875,"d":"9.608"},"3389110651621",{"v":5,"d":"5.00"},{"v":1.5,"d":"1.50"},{"v":1.5,"d":"1.50"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA324","okrúhla kontrolka Ø 12 – IP40 – červená – krytá LED – 12 V – očká",0]
["XVLA323","SIGNÁLKA S LED - 12 MM, 12 V , ZE",1,"ks",{"v":10.065825,"d":"10.066"},"3389110651607",{"v":6.4,"d":"6.40"},{"v":1.8,"d":"1.80"},{"v":4.8,"d":"4.80"},{"v":6,"d":"6.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA323","okrúhla kontrolka Ø 12 – IP40 – zelená – krytá LED – 12 V – očká",0]
["XVLA314","SIGNÁLKA S LED - 12 MM , 5 V,ČERV",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3389110651560",{"v":5,"d":"5.00"},{"v":1.5,"d":"1.50"},{"v":1.5,"d":"1.50"},{"v":7,"d":"7.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA314","okrúhla kontrolka Ø 12 – IP40 – červená – krytá LED – 5 V – očká",0]
["XVLA244","SIGNÁLKA S LED - 8 MM, 48 V,ČERV",1,"ks",{"v":7.2290925,"d":"7.229"},"3389110651447",{"v":5.3,"d":"5.30"},{"v":1.7,"d":"1.70"},{"v":4.5,"d":"4.50"},{"v":2.5,"d":"2.50"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA244","okrúhla kontrolka Ø 8 – IP40 – červená – krytá LED – 48 V – faston",0]
["XVLA243","SIGNÁLKA S LED - 8 MM, 48 V,ZE",1,"ks",{"v":7.2290925,"d":"7.229"},"3389110651423",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},"FR","9030337000","https://www.se.com/sk/sk/product/XVLA243","okrúhla kontrolka Ø 8 – IP40 – zelená – krytá LED – 48 V – faston",0]
["XVLA235","SIGNÁLKA S LED - 8 MM,24 V,ŽL-OR",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3389110651409",{"v":4.2,"d":"4.20"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA235","okrúhla kontrolka Ø 8 – IP40 – žltooranžová – krytá LED – 24 V – faston",0]
["XVLA234","SIGNÁLKA S LED - 8 MM,24 V,ČERV",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3389110651386",{"v":4,"d":"4.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA234","okrúhla kontrolka Ø 8 – IP40 – červená – krytá LED – 24 V – faston",0]
["XVLA233","SIGNÁLKA S LED - 8 MM,24 V,ZE",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3389110651362",{"v":4.2,"d":"4.20"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA233","okrúhla kontrolka Ø 8 – IP40 – zelená – krytá LED – 24 V – faston",0]
["XVLA225","SIGNÁLKA S LED - 8 MM , 12 V ,ŽL-OR",1,"ks",{"v":6.542786249999999,"d":"6.543"},"3389110651348",{"v":7,"d":"7.00"},{"v":1,"d":"1.00"},{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA225","okrúhla kontrolka Ø 8 – IP40 – žltooranžová – krytá LED – 12 V – faston",0]
["XVLA224","SIGNÁLKA S LED - 8 MM , 12 V ,ČERV",1,"ks",{"v":6.542786249999999,"d":"6.543"},"3389110651324",{"v":7.3,"d":"7.30"},{"v":1.5,"d":"1.50"},{"v":1.9,"d":"1.90"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA224","okrúhla kontrolka Ø 8 – IP40 – červená – krytá LED – 12 V – faston",0]
["XVLA223","SIGNÁLKA S LED - 8 MM , 12 V ,ZE",1,"ks",{"v":6.771555,"d":"6.772"},"3389110651300",{"v":7.2,"d":"7.20"},{"v":1.5,"d":"1.50"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA223","okrúhla kontrolka Ø 8 – IP40 – zelená – krytá LED – 12 V – faston",0]
["XVLA144","SIGNÁLKA S LED - 8 MM,48 V,ČERV",1,"ks",{"v":7.2290925,"d":"7.229"},"3389110651140",{"v":6.6,"d":"6.60"},{"v":1.7,"d":"1.70"},{"v":3.9,"d":"3.90"},{"v":2.7,"d":"2.70"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA144","okrúhla kontrolka Ø 8 – IP40 – červená – vyčnievajúca LED – 48 V – faston",0]
["XVLA143","SIGNÁLKA S LED - 8 MM,48 V,ZE",1,"ks",{"v":7.2290925,"d":"7.229"},"3389110651126",{"v":6.5,"d":"6.50"},{"v":1.6,"d":"1.60"},{"v":4.1,"d":"4.10"},{"v":2,"d":"2.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA143","okrúhla kontrolka Ø 8 – IP40 – zelená – vyčnievajúca LED – 48 V – faston",0]
["XVLA135","SIGNÁLKA S LED - 8 MM,24 V,ŽL-OR",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3389110651102",{"v":4.2,"d":"4.20"},{"v":1.2,"d":"1.20"},{"v":1.2,"d":"1.20"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA135","okrúhla kontrolka Ø 8 – IP40 – žltooranžová – vyčnievajúca LED – 24 V – faston",0]
["XVLA134","SIGNÁLKA S LED - 8 MM,24 V,ČERV",1,"ks",{"v":7.091831249999999,"d":"7.092"},"3389110651089",{"v":4.2,"d":"4.20"},{"v":1.2,"d":"1.20"},{"v":1.2,"d":"1.20"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA134","okrúhla kontrolka Ø 8 – IP40 – červená – vyčnievajúca LED – 24 V – faston",0]
["XVLA133","SIGNÁLKA S LED - 8 MM,24 V, ZE",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3389110651065",{"v":4.2,"d":"4.20"},{"v":1.2,"d":"1.20"},{"v":1.2,"d":"1.20"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA133","okrúhla kontrolka Ø 8 – IP40 – zelená – vyčnievajúca LED – 24 V – faston",0]
["XVLA125","SIGNÁLKA S LED - 8 MM, 12 V,ŽL-OR",1,"ks",{"v":6.771555,"d":"6.772"},"3389110651041",{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA125","okrúhla kontrolka Ø 8 – IP40 – žltooranžová – vyčnievajúca LED – 12 V – faston",0]
["XVLA124","SIGNÁLKA S LED - 8 MM, 12 V,ČERV",1,"ks",{"v":6.908816249999999,"d":"6.909"},"3389110651027",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA124","okrúhla kontrolka Ø 8 – IP40 – červená – vyčnievajúca LED – 12 V – faston",0]
["XVLA123","SIGNÁLKA S LED - 8 MM, 12 V, ZE",1,"ks",{"v":6.771555,"d":"6.772"},"3389110651003",{"v":4,"d":"4.00"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":3,"d":"3.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVLA123","okrúhla kontrolka Ø 8 – IP40 – zelená – vyčnievajúca LED – 12 V – faston",0]
["XVGU3SWV","USB SVET.STĹP, PRIAMA MONTÁŽ",1,"ks",{"v":288.24862499999995,"d":"288.249"},"3606480530944",{"v":31.1,"d":"31.10"},{"v":7.9,"d":"7.90"},{"v":7.9,"d":"7.90"},{"v":300,"d":"300.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVGU3SWV","signálny stĺp zostavený a predzapoj.- viacfarebný s USB-Ø 60 -priama montáž",0]
["XVGU3SHAV","USB SVET.STĹP, 100MM",1,"ks",{"v":315.700875,"d":"315.701"},"3606480530937",{"v":41.5,"d":"41.50"},{"v":8.2,"d":"8.20"},{"v":13,"d":"13.00"},{"v":300,"d":"300.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVGU3SHAV","signálny stĺp zostavený a predzapoj.- viacfarebný s USB-Ø 60-100 mm podstavec",0.07]
["XVCZ31","XVC4 upevňovací podstavec na zvislé pl.",1,"ks",{"v":37.0605375,"d":"37.061"},"3606485435688",{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":14,"d":"14.00"},"ID","85319000","https://www.se.com/sk/sk/product/XVCZ31","Harmony XVC, wall mounting bracket, for support tube mounting",0]
["XVCZ23","UHLOVÁ UPEVŇOVAICA KONZOLA",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3606480032868",{"v":15,"d":"15.00"},{"v":8,"d":"8.00"},{"v":11,"d":"11.00"},{"v":382,"d":"382.00"},"JP","7326909890","https://www.se.com/sk/sk/product/XVCZ23","kovová konzola pre montáž na vertikálny držiak",0]
["XVC6M15S","Zmontovaný signáln. stĺp, 60 mm, LED, 10",1,"ks",{"v":235.17427499999997,"d":"235.174"},"3606480072703",{"v":77,"d":"77.00"},{"v":8.7,"d":"8.70"},{"v":8.7,"d":"8.70"},{"v":950,"d":"950.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6M15S","signálny stĺp 60 mm 100..240 V bzučiak - trvalé/prerušované LED - červená",""]
["XVC6B5","Zmontovaný signál. stĺp, 60 mm, LED, 24",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3606480032585",{"v":78.5,"d":"78.50"},{"v":8.3,"d":"8.30"},{"v":8.3,"d":"8.30"},{"v":820,"d":"820.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B5","signálny stĺp 60 mm 24 V trvalé LED - čirá/modrá/zelená/oranžová/červená",0.1]
["XVC6B45SK","Smontovaný signál. stĺp, 60 mm, LED, 24",1,"ks",{"v":215.042625,"d":"215.043"},"3606480032721",{"v":50.5,"d":"50.50"},{"v":8.8,"d":"8.80"},{"v":9,"d":"9.00"},{"v":350,"d":"350.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B45SK","signálny stĺp 60 mm 24 V bzučiak-trvalé/preruš.LED-modrá/zelená/oranžová/čer.",0.07]
["XVC6B45S","Smontovaný signál. stĺp, 60 mm, LED, 24",1,"ks",{"v":361.45462499999996,"d":"361.455"},"3606480032677",{"v":78.5,"d":"78.50"},{"v":8.3,"d":"8.30"},{"v":8.3,"d":"8.30"},{"v":990,"d":"990.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B45S","signálny stĺp 60 mm 24 V bzučiak-trvalé/preruš.LED-modrá/zelená/oranžová/čer.",0.12]
["XVC6B4","Smontovaný signál. stĺp, 60 mm, LED, 24",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3606480032578",{"v":77.5,"d":"77.50"},{"v":8.5,"d":"8.50"},{"v":8.5,"d":"8.50"},{"v":820,"d":"820.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B4","signálny stĺp 60 mm 24 V trvalé LED - modrá/zelená/oranžová/červená",0.13]
["XVC6B3K","Zmontovaný signálny stĺp,60 mm,LED,24 V",1,"ks",{"v":137.26125,"d":"137.261"},"3606480032615",{"v":50.5,"d":"50.50"},{"v":8.7,"d":"8.70"},{"v":8.7,"d":"8.70"},{"v":300,"d":"300.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B3K","signálny stĺp 60 mm 24 V trvalé LED - zelená/oranžová/červená",0.04]
["XVC6B35SK","Zmontovaný signálny stĺp., 60 mm,LED,24V",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3606480032714",{"v":50.5,"d":"50.50"},{"v":8.8,"d":"8.80"},{"v":8.5,"d":"8.50"},{"v":533,"d":"533.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B35SK","signálny stĺp 60 mm 24 V bzučiak-trvalé/prerušované LED-zelená/oranžová/červená",0.04]
["XVC6B35S","Zmontovaný signál.s.,60mm,LED,24V,bzuč.",1,"ks",{"v":384.33149999999995,"d":"384.332"},"3606480032660",{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":74.9,"d":"74.90"},{"v":900,"d":"900.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B35S","signálny stĺp 60 mm 24 V bzučiak-trvalé/prerušované LED-zelená/oranžová/červená",0.14]
["XVC6B3","Zmontovaný signálny s.,60 mm,LED, 24 V",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3606480032561",{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":78,"d":"78.00"},{"v":1045,"d":"1,045.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B3","signálny stĺp 60 mm 24 V trvalé LED - zelená/oranžová/červená",0.13]
["XVC6B15SK","Smontovaný signál. stĺp.,60 mm, LED, 24V",1,"ks",{"v":137.26125,"d":"137.261"},"3606480032691",{"v":50.8,"d":"50.80"},8.64,8.64,{"v":440,"d":"440.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC6B15SK","signálny stĺp 60 mm 24 V bzučiak - trvalé/prerušované LED - červená",0.05]
["XVC4M15S","Zmontovaný signálne stĺpik , 40 mm, LED,",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3606480072857",{"v":74.9,"d":"74.90"},{"v":6.7,"d":"6.70"},{"v":7,"d":"7.00"},{"v":986,"d":"986.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4M15S","signálny stĺp 40 mm 100..240 V bzučiak - trvalé/prerušované LED - červená",""]
["XVC4B5","40 mm signálnín sloupek ROGBC ",1,"ks",{"v":187.59037499999997,"d":"187.590"},"3606480032417",{"v":6.8,"d":"6.80"},{"v":6.7,"d":"6.70"},{"v":75,"d":"75.00"},{"v":580,"d":"580.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B5","signálny stĺp 40 mm 24 V trvalé LED - čirá/modrá/zelená/oranžová/červená",0.09]
["XVC4B4","Zmontovaný signál. stĺp, 40 mm,LED,24V",1,"ks",{"v":187.59037499999997,"d":"187.590"},"3606480032400",{"v":6.8,"d":"6.80"},{"v":6.7,"d":"6.70"},{"v":74.9,"d":"74.90"},{"v":560,"d":"560.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B4","signálny stĺp 40 mm 24 V trvalé LED - modrá/zelená/oranžová/červená",0.07]
["XVC4B3K","Zmontovaný signál. stĺp, 40 mm,LED,24V",1,"ks",{"v":155.56275,"d":"155.563"},"3606480032448",{"v":46.7,"d":"46.70"},{"v":6.4,"d":"6.40"},{"v":7.4,"d":"7.40"},{"v":306,"d":"306.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B3K","signálny stĺp 40 mm 24 V trvalé LED - zelená/oranžová/červená",0.04]
["XVC4B35S","Zmontovaný signálny s.,40 mm, LED, 24V",1,"ks",{"v":283.67325,"d":"283.673"},"3606480032493",{"v":75,"d":"75.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":697,"d":"697.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B35S","signálny stĺp 40 mm 24 V bzučiak-trvalé/prerušované LED-zelená/oranžová/červená",0.08]
["XVC4B3","Zmontovaný signál. stĺp, 40 mm, LED, 24V",1,"ks",183.015,"3606480032394",{"v":75.2,"d":"75.20"},{"v":6.8,"d":"6.80"},{"v":6.8,"d":"6.80"},{"v":540,"d":"540.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B3","signálny stĺp 40 mm 24 V trvalé LED - zelená/oranžová/červená",0.06]
["XVC4B25S","Smontovaný signál. stĺp,40 mm,LED,24V",1,"ks",{"v":131.77079999999998,"d":"131.771"},"3606480032486",{"v":75,"d":"75.00"},{"v":6.6,"d":"6.60"},{"v":6.6,"d":"6.60"},{"v":850,"d":"850.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B25S","signálny stĺp 40 mm 24 V bzučiak - trvalé/prerušované LED - oranžová/červená",""]
["XVC4B1K","Zmont. signálny stĺp, 40mm, LED, 24V RED",1,"ks",{"v":82.35674999999999,"d":"82.357"},"3606480032424",46.99,6.35,7.62,{"v":260,"d":"260.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B1K","signálny stĺp 40 mm 24 V trvalé LED - červená",0.04]
["XVC4B15S","Zmontovaný signálny stĺp., 40 mm,LED,24V",1,"ks",{"v":187.59037499999997,"d":"187.590"},"3606480032479",{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":75,"d":"75.00"},{"v":676,"d":"676.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B15S","signálny stĺp 40 mm 24 V bzučiak - trvalé/prerušované LED - červená",0.1]
["XVC4B1","Zmontovaný signálny stĺp, 40mm, LED, 24V",1,"ks",{"v":74.57861249999999,"d":"74.579"},"3606480032370",{"v":6.8,"d":"6.80"},{"v":6.7,"d":"6.70"},{"v":75,"d":"75.00"},{"v":500,"d":"500.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVC4B1","Zmontovaný signálny stĺp, 40mm, LED, 24V",0]
["XVC1M3HK","SVET.STĹP S TRV.SVET.,100mm,LED,100-240V",1,"ks",{"v":704.6077499999999,"d":"704.608"},"3606480072499",{"v":65,"d":"65.00"},{"v":21,"d":"21.00"},{"v":22,"d":"22.00"},{"v":4125,"d":"4,125.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVC1M3HK","sig.sloup 100 mm 100..240 V siréna-trvalé/blikajúce LED-zelená/oranžová/čer.",0.5]
["XVC1M1HK","Zložený signálny stĺpik,100 mm, LED",1,"ks",{"v":512.4419999999999,"d":"512.442"},"3606480072475",{"v":44.5,"d":"44.50"},{"v":20,"d":"20.00"},{"v":21,"d":"21.00"},{"v":2414,"d":"2,414.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVC1M1HK","signálny stĺp 100 mm 100..240 V siréna - trvalé/blikajúce LED - červená",0.25]
["XVC1B3SK","Zmontovaný signálny s.100 mm, LED, 24V",1,"ks",{"v":443.81137499999994,"d":"443.811"},"3606480032837",{"v":44.5,"d":"44.50"},{"v":20.3,"d":"20.30"},{"v":20.7,"d":"20.70"},{"v":1958,"d":"1,958.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVC1B3SK","signálny stĺp 100 mm 24 V bzučiak-trvalé/blikajúce LED-zelená/oranžová/červená",0.29]
["XVC1B3K","Zmontovaný signálny stĺpik",1,"ks",{"v":407.20837499999993,"d":"407.208"},"3606480032783",{"v":45.5,"d":"45.50"},{"v":21.5,"d":"21.50"},{"v":22,"d":"22.00"},{"v":1922,"d":"1,922.00"},"JP","8531900000","https://www.se.com/sk/sk/product/XVC1B3K","signálny stĺp 100 mm 24 V trvalé/blikajúce LED - zelená/oranžová/červená",0.29]
["XVC1B2HK","SIGNÁLNY STĹPIK 100 MM",1,"ks",{"v":539.8942499999999,"d":"539.894"},"3606480072451",{"v":63,"d":"63.00"},{"v":18,"d":"18.00"},{"v":18,"d":"18.00"},{"v":1780,"d":"1,780.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVC1B2HK","signálny stĺp 100 mm 24 V siréna - trvalé/blikajúce LED - oranžová/červená",0.21]
["XVC1B1K","SIGNÁLNY STĹPIK 100 MM",1,"ks",{"v":324.85162499999996,"d":"324.852"},"3606480032769",{"v":44.5,"d":"44.50"},{"v":21,"d":"21.00"},{"v":21.5,"d":"21.50"},{"v":1488,"d":"1,488.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVC1B1K","signálny stĺp 100 mm 24 V trvalé/blikajúce LED - červená",0.22]
["XVC1B1HK","Signálny stĺp,100 mm, LED, 24V,siréna",1,"ks",{"v":498.715875,"d":"498.716"},"3606480072444",{"v":18,"d":"18.00"},{"v":18,"d":"18.00"},{"v":43,"d":"43.00"},{"v":1580,"d":"1,580.00"},"JP","8531807000","https://www.se.com/sk/sk/product/XVC1B1HK","signálny stĺp 100 mm 24 V siréna - trvalé/blikajúce LED - červená",0.24]
["XVBZ04","TRUBKA 800 MM + UPEVŇOVACÍ PODSTAVEC",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3389110673678",{"v":7,"d":"7.00"},{"v":82.1,"d":"82.10"},{"v":7,"d":"7.00"},{"v":299,"d":"299.00"},"FR","7616999099","https://www.se.com/sk/sk/product/XVBZ04","nosná rúra + montážna základňa d = 800 mm – hliníková čierna – XVB",0]
["XVBZ03A","UPEVŇOVAICA KONZOLA",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3389110673531",{"v":42.5,"d":"42.50"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":178,"d":"178.00"},"FR","7616999099","https://www.se.com/sk/sk/product/XVBZ03A","upevňovací podstavec s čiernou Al trubicou",0]
["XVBZ03","TRUBKA 400 MM + UPEVŇOVACÍ PODSTAVEC",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110673616",{"v":47.5,"d":"47.50"},{"v":7.3,"d":"7.30"},{"v":11.6,"d":"11.60"},{"v":185,"d":"185.00"},"FR","7616999099","https://www.se.com/sk/sk/product/XVBZ03","nosná rúra + montážna základňa d = 400 mm – hliníková čierna – XVB",0]
["XVBZ02A","TRUBKA 100 MM + UPEVŇOVACÍ PODSTAVEC",1,"ks",{"v":29.282399999999996,"d":"29.282"},"3389110673524",{"v":13,"d":"13.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":86,"d":"86.00"},"FR","7616999099","https://www.se.com/sk/sk/product/XVBZ02A","nosná rúra + montážna základňa d = 80 mm – hliníková – XVB",0]
["XVBZ02","TRUBKA 100 MM + UPEVŇOVACÍ PODSTAVEC",1,"ks",{"v":29.282399999999996,"d":"29.282"},"3389110673579",{"v":11.973,"d":"11.97"},6.97,{"v":6.993,"d":"6.99"},{"v":86,"d":"86.00"},"FR","7616999099","https://www.se.com/sk/sk/product/XVBZ02","nosná rúra + montážna základňa d = 80 mm – hliníková čierna – XVB",0]
["XVBZ01","PLASTOVÝ PODSTAVEC PRE AL TUBU",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110673517",{"v":10,"d":"10.00"},{"v":8,"d":"8.00"},{"v":10,"d":"10.00"},{"v":55,"d":"55.00"},"FR","3926909790","https://www.se.com/sk/sk/product/XVBZ01","montážna základňa pre nosnú rúru – pre maják XVB - čierny zalisovaný plast",0]
["XVBL8M5","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":228.76874999999998,"d":"228.769"},"3389110844986",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":473,"d":"473.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8M5","maják s 10 J oranžovým svetlom XVB – svetelná trubica – 230 V AC – IP 65",0.07]
["XVBL8M4","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":228.76874999999998,"d":"228.769"},"3389110844979",{"v":8.2,"d":"8.20"},{"v":8,"d":"8.00"},{"v":25.4,"d":"25.40"},{"v":460,"d":"460.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8M4","maják s 10 J červeným svetlom XVB – svetelná trubica – 230 V AC – IP 65",0.07]
["XVBL8G8","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844894",{"v":8,"d":"8.00"},{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":460,"d":"460.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8G8","maják s 10 J žltým svetlom XVB – svetelná trubica – 120 V AC – IP 65",0.07]
["XVBL8G6","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844870",{"v":8,"d":"8.00"},{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":460,"d":"460.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8G6","maják s 10 J modrým svetlom XVB – svetelná trubica – 120 V AC – IP 65",0.07]
["XVBL8G5","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844863",{"v":8,"d":"8.00"},{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":460,"d":"460.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8G5","maják s 10 J oranžovým svetlom XVB – svetelná trubica – 120 V AC – IP 65",0.07]
["XVBL8G4","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844856",{"v":8,"d":"8.00"},{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":460,"d":"460.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8G4","maják s 10 J červeným svetlom XVB – svetelná trubica – 120 V AC – IP 65",0.07]
["XVBL8B8","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844771",{"v":8,"d":"8.00"},{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":450,"d":"450.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8B8","maják s 10 J žltým svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL8B7","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844764",{"v":8,"d":"8.00"},{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":450,"d":"450.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8B7","maják s 10 J čírymsvetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL8B6","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844757",{"v":8,"d":"8.00"},{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":450,"d":"450.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8B6","maják s 10 J modrým svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL8B5","Svet. stĺp s vybíjacím obvodom 10J",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844740",{"v":25.6,"d":"25.60"},{"v":7.8,"d":"7.80"},{"v":8,"d":"8.00"},{"v":461,"d":"461.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8B5","maják s 10 J oranžovým svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL8B4","SVET. STĹP S VYBÍJ. OBVODOM",1,"ks",{"v":224.193375,"d":"224.193"},"3389110844733",{"v":9,"d":"9.00"},{"v":25.3,"d":"25.30"},{"v":9,"d":"9.00"},{"v":464,"d":"464.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL8B4","maják s 10 J červeným svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL6M5","Svet. stĺp s vybíjacím obvodom 5J",1,"ks",183.015,"3389110844924",{"v":8,"d":"8.00"},{"v":7.8,"d":"7.80"},{"v":25.8,"d":"25.80"},{"v":434,"d":"434.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6M5","maják s 5 J oranžovým svetlom XVB – svetelná trubica – 230 V AC – IP 65",0.07]
["XVBL6M4","SVET. STĹP S VYBÍJ. OBVODOM",1,"ks",183.015,"3389110844917",{"v":25.5,"d":"25.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":427,"d":"427.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6M4","maják s 5 J červeným svetlom XVB – svetelná trubica – 230 V AC – IP 65",0.06]
["XVBL6G5","Svet. stĺp s vybíjacím obvodom 5J",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110844801",{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":417,"d":"417.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6G5","maják s 5 J oranžovým svetlom XVB – svetelná trubica – 120 V AC – IP 65",0.06]
["XVBL6G4","Svet. stĺp s vybíjacím obvodom 5J",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110844795",{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":417,"d":"417.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6G4","maják s 5 J červeným svetlom XVB – svetelná trubica – 120 V AC – IP 65",0.06]
["XVBL6B8","Svet. stĺp s vybíjacím obvodom 5J",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110844719",{"v":8,"d":"8.00"},{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":439.5,"d":"439.50"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6B8","maják s 5 J žltým svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL6B7","Svet. stĺp s vybíjacím obvodom 5J",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110844702",{"v":25.2,"d":"25.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":435,"d":"435.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6B7","maják s 5 J čírym svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL6B6","Svet. stĺp s vybíjacím obvodom 5J",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110844696",{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":26,"d":"26.00"},{"v":440,"d":"440.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6B6","maják s 5 J modrým svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.06]
["XVBL6B5","Svet. stĺp s vybíjacím obvodom 5J",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110844689",{"v":8.2,"d":"8.20"},{"v":8,"d":"8.00"},{"v":25.4,"d":"25.40"},{"v":440,"d":"440.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6B5","maják s 5 J oranžovým svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL6B4","Svet. stĺp s vybíjacím obvodom 5J",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110844672",{"v":8,"d":"8.00"},{"v":25.3,"d":"25.30"},{"v":8,"d":"8.00"},{"v":437,"d":"437.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL6B4","maják s 5 J červeným svetlom XVB – svetelná trubica – 24 V AC DC – IP 65",0.07]
["XVBL4M8","Svet. stĺp so vstavaným zábl. svetlom",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110844290",{"v":8,"d":"8.00"},{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":280,"d":"280.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL4M8","maják s blikajúcim žltým svetlom XVB – základňa BA 15d – 48 - 230 V max – IP 65",0.04]
["XVBL4M5","Svet. stĺp so vstavaným zábl. svetlom",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110844269",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":275,"d":"275.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL4M5","maják s blikajúcim oranžovým svetl. XVB – zákl. BA 15d – 48 - 230 V max – IP 65",0.04]
["XVBL4M4","SVET. STĹP SO ZÁBL. SVETLOM",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110844252",{"v":15,"d":"15.00"},{"v":8,"d":"8.00"},{"v":8.2,"d":"8.20"},{"v":277,"d":"277.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL4M4","maják sblikajúcim červeným svetl. XVB – zákl. BA 15d – 48 - 230 V max – IP 65",0.04]
["XVBL4B5","SVET. STĹP SO ZÁBL. SVETLOM",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110844207",{"v":8.2,"d":"8.20"},{"v":8,"d":"8.00"},{"v":14.8,"d":"14.80"},{"v":280,"d":"280.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL4B5","maják s blik. oranž. svetl. XVB – zákl. BA 15d – 24 - 48 V DC 24 V AC – IP 65",0.04]
["XVBL4B4","Svet. stĺp so vstavaným zábl. svetlom",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110844191",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":275,"d":"275.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL4B4","maják s blik. červ. svetl. XVB – zákl. BA 15d – 24 - 48 V DC 24 V AC – IP 65",0.04]
["XVBL4B3","Svet. stĺp so vstavaným zábl. svetlom",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110844184",{"v":8,"d":"8.00"},{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":280,"d":"280.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL4B3","maják s blikajúcim zel. svetl. XVB – zákl. BA 15d – 24 - 48 V DC 24 V AC – IP 65",0.04]
["XVBL38","Svet. stĺp s trvalým svetlom žltý",1,"ks",{"v":62.22509999999999,"d":"62.225"},"3389110844177",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":261,"d":"261.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL38","maják s neprerušovaným žltým svetlom XVB – základňa BA 15d – 250 V max – IP 65",0.04]
["XVBL37","Svet. stĺp s trvalým svetlom číry",1,"ks",{"v":62.22509999999999,"d":"62.225"},"3389110844160",{"v":8.2,"d":"8.20"},{"v":7.8,"d":"7.80"},{"v":14.8,"d":"14.80"},{"v":260,"d":"260.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL37","maják s neprerušovaným čírym svetlom XVB – základňa BA 15d – 250 V max – IP 65",0.04]
["XVBL36","Svet.stĺp s trvalým svetlom modrý",1,"ks",{"v":62.22509999999999,"d":"62.225"},"3389110844153",{"v":8.2,"d":"8.20"},{"v":8.2,"d":"8.20"},{"v":15,"d":"15.00"},{"v":260,"d":"260.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL36","maják s neprerušovaným modrým svetlom XVB – základňa BA 15d – 250 V max – IP 65",0.04]
["XVBL35","SVET. STĹP S TRVAL. SVETLOM",1,"ks",{"v":62.22509999999999,"d":"62.225"},"3389110844146",{"v":8,"d":"8.00"},{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":255,"d":"255.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL35","maják s nepreruš. oranžovým svetlom XVB – základňa BA 15d – 250 V max – IP 65",0.04]
["XVBL34","SVET. STĹP S TRVAL. SVETLOM",1,"ks",{"v":62.22509999999999,"d":"62.225"},"3389110844139",{"v":14.8,"d":"14.80"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":260,"d":"260.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL34","maják s nepreruš. červeným svetlom XVB – základňa BA 15d – 250 V max – IP 65",0.04]
["XVBL33","Svet. stĺp s trvalým svetlom zel.",1,"ks",{"v":62.22509999999999,"d":"62.225"},"3389110844092",{"v":8.2,"d":"8.20"},{"v":7.8,"d":"7.80"},{"v":14.8,"d":"14.80"},{"v":266,"d":"266.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL33","maják s neprerušovaným zeleným svetlom XVB – základňa BA 15d – 250 V max – IP 65",0.04]
["XVBL1M5","SVET. STĹP SO ZÁBL. SVETLOM",1,"ks",{"v":169.288875,"d":"169.289"},"3389110844627",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":274,"d":"274.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL1M5","maják s blikajúcim oranžovým svetlom XVB – zabud. LED – 230 V AC – IP 65",0.04]
["XVBL1M4","SVET. STĹP SO ZÁBL. SVETLOM",1,"ks",{"v":169.288875,"d":"169.289"},"3389110844610",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":15,"d":"15.00"},{"v":280,"d":"280.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL1M4","maják s blikajúcim červeným svetlom XVB – zabud. LED – 230 V AC – IP 65",0.04]
["XVBL1B8","STĹP SO VSTAVANÝM ZÁBL. SVETLOM S LED",1,"ks",{"v":169.288875,"d":"169.289"},"3389110124408",{"v":9,"d":"9.00"},{"v":16,"d":"16.00"},{"v":9,"d":"9.00"},{"v":280,"d":"280.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL1B8","maják s blikajúcim žltým svetlom XVB – zabud. LED – 24 VAC DC – IP 65",0.04]
["XVBL1B6","STĹP SO VSTAVANÝM ZÁBL. SVETLOM S LED",1,"ks",183.015,"3389110844399",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":280,"d":"280.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL1B6","maják s blikajúcim modrým svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL1B5","STĹP SO VSTAVANÝM ZÁBL. SVETLOM S LED",1,"ks",{"v":169.288875,"d":"169.289"},"3389110844382",{"v":8.2,"d":"8.20"},{"v":8.2,"d":"8.20"},{"v":15,"d":"15.00"},{"v":280,"d":"280.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL1B5","maják s blikajúcim oranžovým svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL1B4","STĹP SO VSTAVANÝM ZÁBL. SVETLOM S LED",1,"ks",{"v":169.288875,"d":"169.289"},"3389110844375",{"v":8.2,"d":"8.20"},{"v":7.8,"d":"7.80"},{"v":15,"d":"15.00"},{"v":280,"d":"280.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL1B4","maják s blikajúcim červeným svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL1B3","SVET. STĹP SO ZÁBL. SVETLOM",1,"ks",{"v":169.288875,"d":"169.289"},"3389110844368",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":271,"d":"271.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL1B3","maják s blikajúcim zeleným svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL0M7","Svet.stĺp s trvalým svetlom s LED číry",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110844580",{"v":14.6,"d":"14.60"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":268,"d":"268.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0M7","maják s neprerušovaným čírym svetlom XVB – zabud. LED – 230 V AC – IP 65",0.04]
["XVBL0M6","Svet.stĺp s trvalým svetlom s LED MO",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110844573",{"v":8,"d":"8.00"},{"v":14.6,"d":"14.60"},{"v":8,"d":"8.00"},{"v":270,"d":"270.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0M6","maják s neprerušovaným modrým svetlom XVB – zabud. LED – 230 V AC – IP 65",0.04]
["XVBL0M5","Svet.stĺp s trvalým svetlom s LED oranž.",1,"ks",109.809,"3389110844566",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":269,"d":"269.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0M5","maják s neprerušovaným oranžovým svetlom XVB – zabud. LED – 230 V AC – IP 65",0.04]
["XVBL0M4","Svet.stĺp s trvalým svetlom s LED červ.",1,"ks",109.809,"3389110844559",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":268,"d":"268.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0M4","maják s neprerušovaným červeným svetlom XVB – zabud. LED – 230 V AC – IP 65",0.04]
["XVBL0M3","Svet.stĺp s trvalým svetlom s LED ZE",1,"ks",109.809,"3389110844542",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":267,"d":"267.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0M3","maják s neprerušovaným zeleným svetlom XVB – zabud. LED – 230 V AC – IP 65",0.04]
["XVBL0G4","Svet.stĺp s trvalým svetlom s LED červ.",1,"ks",109.809,"3389110844436",{"v":8,"d":"8.00"},{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":269,"d":"269.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0G4","maják s neprerušovaným červeným svetlom XVB – zabud. LED – 120 V AC – IP 65",0.04]
["XVBL0G3","Svet.stĺp s trvalým svetlom s LED ZE",1,"ks",109.809,"3389110844429",{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":267,"d":"267.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0G3","maják s neprerušovaným zeleným svetlom XVB – zabud. LED – 120 V AC – IP 65",0.04]
["XVBL0B8","Svet.stĺp s trvalým svetlom s LED ŽL",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110124392",{"v":8,"d":"8.00"},{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":270,"d":"270.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0B8","maják s neprerušovaným žltým svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL0B7","Svet.stĺp s trvalým svetlom s LED číry",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110844344",{"v":8,"d":"8.00"},{"v":14.6,"d":"14.60"},{"v":8,"d":"8.00"},{"v":270,"d":"270.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0B7","maják s neprerušovaným čírym svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL0B6","Svet.stĺp s trvalým svetlom s LED MO",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110844337",{"v":8.2,"d":"8.20"},{"v":8,"d":"8.00"},{"v":15,"d":"15.00"},{"v":270,"d":"270.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0B6","maják s neprerušovaným modrým svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL0B5","SVET. STĹP S TRVAL. SVETLOM",1,"ks",109.809,"3389110844320",{"v":8,"d":"8.00"},{"v":14.5,"d":"14.50"},{"v":8,"d":"8.00"},{"v":269,"d":"269.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0B5","maják s neprerušovaným oranžovým svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL0B4","SVET. STĹP S TRVAL. SVETLOM",1,"ks",109.809,"3389110844313",{"v":15,"d":"15.00"},{"v":8.2,"d":"8.20"},{"v":8.2,"d":"8.20"},{"v":270,"d":"270.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0B4","maják s neprerušovaným červeným svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBL0B3","Svet.stĺp s trvalým svetlom s LED ZE",1,"ks",109.809,"3389110844306",{"v":14.6,"d":"14.60"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":269,"d":"269.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBL0B3","maják s neprerušovaným zeleným svetlom XVB – zabud. LED – 24 V AC DC – IP 65",0.04]
["XVBC9M","BZUČIAK",1,"ks",{"v":201.3165,"d":"201.317"},"3389110845976",{"v":8,"d":"8.00"},{"v":10,"d":"10.00"},{"v":8.2,"d":"8.20"},{"v":170,"d":"170.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC9M","zvuk. jednotka – nepretrž. alebo prerušov. bzučiak – 75 - 90 dB – 120 - 230 V AC",0.02]
["XVBC9B","BZUČIAK",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110845969",{"v":9.6,"d":"9.60"},{"v":7.8,"d":"7.80"},{"v":8,"d":"8.00"},{"v":166,"d":"166.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC9B","zvuk.jednotka – nepretrž. alebo prerušov. bzučiak – 75 - 90 dB – 12 - 48 V AC DC",0.02]
["XVBC8M6","Svet. návesť s vybíjacím obvodom 10J",1,"ks",219.618,"3389110845938",{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":329,"d":"329.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8M6","osvetlená jednotka – 10 Joulová blikajúca – modrá – 230 V AC",0.05]
["XVBC8M5","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110845921",{"v":8,"d":"8.00"},{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":334,"d":"334.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8M5","osvetlená jednotka – 10 Joulová blikajúca – oranžová – 230 V AC",0.05]
["XVBC8M4","SVET. NÁVESŤ S VYBÍJ. OBVODOM",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110845914",{"v":8.2,"d":"8.20"},{"v":7.8,"d":"7.80"},{"v":19,"d":"19.00"},{"v":340,"d":"340.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8M4","osvetlená jednotka – 10 Joulová blikajúca – červená – 230 V AC",0.05]
["XVBC8G8","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":251.64562499999997,"d":"251.646"},"3389110845839",19.05,{"v":8.128,"d":"8.13"},{"v":8.128,"d":"8.13"},{"v":312.982,"d":"312.98"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBC8G8","osvetlená jednotka – 10 Joulová blikajúca – žltá – 120 V AC",0.05]
["XVBC8G6","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":251.64562499999997,"d":"251.646"},"3389110845815",{"v":8,"d":"8.00"},{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":315,"d":"315.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8G6","osvetlená jednotka – 10 Joulová blikajúca – modrá – 120 V AC",0.05]
["XVBC8G5","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":251.64562499999997,"d":"251.646"},"3389110845808",{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":315,"d":"315.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBC8G5","osvetlená jednotka – 10 Joulová blikajúca – oranžová – 120 V AC",0.05]
["XVBC8G4","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":251.64562499999997,"d":"251.646"},"3389110845792",{"v":8,"d":"8.00"},{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":315,"d":"315.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBC8G4","osvetlená jednotka – 10 Joulová blikajúca – červená – 120 V AC",0.05]
["XVBC8B8","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3389110845716",{"v":8,"d":"8.00"},{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":316,"d":"316.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8B8","osvetlená jednotka – 10 Joulová blikajúca – žltá – 24 V AC DC",0.05]
["XVBC8B7","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3389110845709",{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":305,"d":"305.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8B7","osvetlená jednotka – 10 Joulová blikajúca – číra – 24 V AC DC",0.05]
["XVBC8B6","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3389110845693",{"v":10,"d":"10.00"},{"v":19,"d":"19.00"},{"v":10,"d":"10.00"},{"v":305,"d":"305.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8B6","osvetlená jednotka – 10 Joulová blikajúca – modrá – 24 V AC DC",0.05]
["XVBC8B5","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3389110845686",{"v":8,"d":"8.00"},{"v":7.8,"d":"7.80"},{"v":19,"d":"19.00"},{"v":305,"d":"305.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8B5","osvetlená jednotka – 10 Joulová blikajúca – oranžová – 24 V AC DC",0.05]
["XVBC8B4","Svet. návesť s vybíjacím obvodom 10J",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3389110845679",{"v":19,"d":"19.00"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":320,"d":"320.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC8B4","osvetlená jednotka – 10 Joulová blikajúca – červená – 24 V AC DC",0.05]
["XVBC6M8","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389110845891",{"v":8,"d":"8.00"},{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":282.9,"d":"282.90"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6M8","osvetlená jednotka – 5 Joulová blikajúca – žltá – 230 V AC",0.04]
["XVBC6M7","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389110845884",{"v":8,"d":"8.00"},{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":283.9,"d":"283.90"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6M7","osvetlená jednotka – 5 Joulová blikajúca – číra – 230 V AC",0.04]
["XVBC6M6","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389110845877",{"v":8,"d":"8.00"},{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":282.9,"d":"282.90"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6M6","osvetlená jednotka – 5 Joulová blikajúca – modrá – 230 V AC",0.04]
["XVBC6M5","SVET. NÁVESŤ S VYBÍJ. OBVODOM",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3389110845860",{"v":8,"d":"8.00"},{"v":18.5,"d":"18.50"},{"v":8,"d":"8.00"},{"v":285.9,"d":"285.90"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6M5","osvetlená jednotka – 5 Joulová blikajúca – oranžová – 230 V AC",0.04]
["XVBC6M4","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3389110845853",{"v":19.5,"d":"19.50"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":281,"d":"281.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6M4","osvetlená jednotka – 5 Joulová blikajúca – červená – 230 V AC",0.04]
["XVBC6M3","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3389110845846",{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":281,"d":"281.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6M3","osvetlená jednotka – 5 Joulová blikajúca – zelená – 230 V AC",0.04]
["XVBC6G5","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110845747",{"v":9,"d":"9.00"},{"v":20,"d":"20.00"},{"v":9,"d":"9.00"},{"v":276,"d":"276.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6G5","osvetlená jednotka – 5 Joulová blikajúca – oranžová – 120 V AC",0.04]
["XVBC6G4","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110845730",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":19,"d":"19.00"},{"v":276,"d":"276.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6G4","osvetlená jednotka – 5 Joulová blikajúca – červená – 120 V AC",0.04]
["XVBC6B8","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110845655",{"v":21.6,"d":"21.60"},{"v":8,"d":"8.00"},{"v":9.8,"d":"9.80"},{"v":296,"d":"296.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6B8","osvetlená jednotka – 5 Joulová blikajúca – žltá – 24 V AC DC",0.05]
["XVBC6B7","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110845648",{"v":8,"d":"8.00"},{"v":7.8,"d":"7.80"},{"v":19.2,"d":"19.20"},{"v":298,"d":"298.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6B7","osvetlená jednotka – 5 Joulová blikajúca – číra – 24 V AC DC",0.04]
["XVBC6B6","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110845631",{"v":9.4,"d":"9.40"},{"v":8.2,"d":"8.20"},{"v":20,"d":"20.00"},{"v":295,"d":"295.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBC6B6","osvetlená jednotka – 5 Joulová blikajúca – modrá – 24 V AC DC",0.04]
["XVBC6B5","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110845624",{"v":19.5,"d":"19.50"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":297,"d":"297.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBC6B5","osvetlená jednotka – 5 Joulová blikajúca – oranžová – 24 V AC DC",0.04]
["XVBC6B4","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110845617",{"v":19.2,"d":"19.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":295,"d":"295.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XVBC6B4","osvetlená jednotka – 5 Joulová blikajúca – červená – 24 V AC DC",0.04]
["XVBC6B3","Svet. návesť s vybíjacím obvodom 5J",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110845600",{"v":9,"d":"9.00"},{"v":18.7,"d":"18.70"},{"v":9,"d":"9.00"},{"v":291,"d":"291.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC6B3","osvetlená jednotka – 5 Joulová blikajúca – zelená – 24 V AC DC",0.04]
["XVBC5M8","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110147919",{"v":9.5,"d":"9.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":137,"d":"137.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5M8","osvetlená jednotka – blikajúce svetlo – žlté – 230 V AC",0.02]
["XVBC5M6","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110147896",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":140.9,"d":"140.90"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5M6","osvetlená jednotka – blikajúce svetlo – modré – 230 V AC",0.02]
["XVBC5M5","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110147889",{"v":9.2,"d":"9.20"},{"v":8,"d":"8.00"},{"v":8.2,"d":"8.20"},{"v":138,"d":"138.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5M5","osvetlená jednotka – blikajúce svetlo – oranžové – 230 V AC",0.02]
["XVBC5M4","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110147872",{"v":9.6,"d":"9.60"},{"v":8.2,"d":"8.20"},{"v":8.4,"d":"8.40"},{"v":139,"d":"139.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5M4","osvetlená jednotka – blikajúce svetlo – červené – 230 V AC",0.02]
["XVBC5M3","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110147865",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":141.9,"d":"141.90"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5M3","70 MM SVET. NÁVESTIE S PRERUŠ. ZELEN. SVETLOM S LED IP65 230V",0.02]
["XVBC5G5","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110145809",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":141,"d":"141.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5G5","70 MM SVET. NÁVESTIE S PRERUŠ. ORANŽ. SVETLOM S LED IP65 120V",0.02]
["XVBC5G4","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110145670",{"v":8,"d":"8.00"},{"v":9.2,"d":"9.20"},{"v":8,"d":"8.00"},{"v":141,"d":"141.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5G4","70 MM SVET. NÁVESTIE S PRERUŠ. ČERV. SVETLOM S LED IP65 120V",0.02]
["XVBC5B8","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110144901",{"v":9.5,"d":"9.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":137,"d":"137.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5B8","osvetlenájednotka – blikajúce svetlo – žlté – 24 V AC DC",0.02]
["XVBC5B7","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110144888",{"v":9.5,"d":"9.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":138,"d":"138.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5B7","osvetlená jednotka – blikajúce svetlo – číre – 24 V AC DC",0.02]
["XVBC5B6","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110144840",{"v":8,"d":"8.00"},{"v":9.2,"d":"9.20"},{"v":8,"d":"8.00"},{"v":141,"d":"141.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5B6","osvetlená jednotka – blikajúce svetlo – modré – 24 V AC DC",0.02]
["XVBC5B5","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110144789",{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":8,"d":"8.00"},{"v":140,"d":"140.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5B5","osvetlená jednotka – blikajúce svetlo – oranžové – 24 V AC DC",0.02]
["XVBC5B4","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110144710",{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":137,"d":"137.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5B4","osvetlená jednotka – blikajúce svetlo – červené – 24 V AC DC",0.02]
["XVBC5B3","NÁVESTIE S PRERUŠOVANÝM SVETLOM S LED",1,"ks",{"v":118.95975,"d":"118.960"},"3389110144697",{"v":9.5,"d":"9.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":134,"d":"134.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC5B3","osvetlená jednotka – blikajúce svetlo – zelené – 24 V AC DC",0]
["XVBC4M8","SVET. NÁVESŤ S PRERUŠ. SVETLOM",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845235",9.14,7.87,7.87,{"v":150,"d":"150.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4M8","osvetlená jednotka – blikajúce svetlo – žlté – 48 - 230 V AC",0.02]
["XVBC4M6","Svet. návesť s prerušovaným svetlom",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845211",{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":145,"d":"145.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4M6","osvetlená jednotka – blikajúce svetlo – modré – 48 - 230 V AC",0.02]
["XVBC4M5","Svet. návesť s prerušovaným svetlom",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845204",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":149,"d":"149.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4M5","osvetlená jednotka – blikajúce svetlo – oranžové – 48 - 230 V AC",0.02]
["XVBC4M4","Svet. návesť s prerušovaným svetlom",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845198",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":146,"d":"146.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4M4","osvetlená jednotka – blikajúce svetlo – červené – 48 - 230 V AC",0.02]
["XVBC4M3","Svet. návesť s prerušovaným svetlom",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845181",{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":151,"d":"151.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4M3","osvetlená jednotka – blikajúce svetlo – zelené – 48 - 230 V AC",0.02]
["XVBC4B8","Svet. návesť s prerušovaným svetlom",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845174",{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":144,"d":"144.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4B8","osvetlená jednotka – blikajúce svetlo – žlté – 24 - 48 V DC 24 V AC",0.02]
["XVBC4B6","Svet. návesť s prerušovaným svetlom",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845150",{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":150,"d":"150.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4B6","osvetlená jednotka – blikajúce svetlo – modré – 24 - 48 V DC 24 V AC",0.02]
["XVBC4B5","SVET. NÁVESŤ S PRERUŠ. SVETLOM",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845143",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":146,"d":"146.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4B5","osvetlená jednotka – blikajúce svetlo – oranžové – 24 - 48 V DC 24 V AC",0.02]
["XVBC4B4","Svet. návesť s prerušovaným svetlom",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845136",{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":146,"d":"146.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4B4","osvetlená jednotka – blikajúce svetlo – červené – 24 - 48 V DC 24 V AC",0.02]
["XVBC4B3","Svet. návesť s prerušovaným svetlom",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110845129",{"v":11.5,"d":"11.50"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":144,"d":"144.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC4B3","osvetlená jednotka – blikajúce svetlo – zelené – 24 - 48 V DC 24 V AC",0.02]
["XVBC38","SVET. NÁVESŤ S TRVAL. SVETLOM",1,"ks",{"v":48.956512499999995,"d":"48.957"},"3389110845112",{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":136,"d":"136.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC38","osvetlená jednotka – trvalé svetlo – žlté – 250 V max",0.02]
["XVBC37","SVET. NÁVESŤ S TRVAL. SVETLOM",1,"ks",{"v":48.956512499999995,"d":"48.957"},"3389110845105",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":135,"d":"135.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC37","osvetlená jednotka – trvalé svetlo – číre – 250 V max",0.02]
["XVBC36","Svet.návesť s trvalým svetlom MO",1,"ks",{"v":48.956512499999995,"d":"48.957"},"3389110845099",{"v":14.4,"d":"14.40"},{"v":7.8,"d":"7.80"},{"v":10.6,"d":"10.60"},{"v":137,"d":"137.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC36","osvetlená jednotka – trvalé svetlo – modré – 250 V max",0.02]
["XVBC35","SVET. NÁVESŤ S TRVAL. SVETLOM",1,"ks",{"v":53.07435,"d":"53.074"},"3389110845082",{"v":8.2,"d":"8.20"},{"v":8.2,"d":"8.20"},{"v":9.5,"d":"9.50"},{"v":135,"d":"135.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC35","osvetlená jednotka – trvalé svetlo – oranžové – 250 V max",0.02]
["XVBC34","SVET. NÁVESŤ S TRVAL. SVETLOM",1,"ks",{"v":53.07435,"d":"53.074"},"3389110845075",{"v":10,"d":"10.00"},{"v":10.5,"d":"10.50"},{"v":10,"d":"10.00"},{"v":136,"d":"136.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC34","osvetlená jednotka – trvalé svetlo – červené – 250 V max",0.02]
["XVBC33","SVET. NÁVESŤ S TRVAL. SVETLOM",1,"ks",{"v":53.53188749999999,"d":"53.532"},"3389110845068",{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":132,"d":"132.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC33","osvetlená jednotka – trvalé svetlo – zelené – 250 V max",0.02]
["XVBC2M8","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":83.27182499999999,"d":"83.272"},"3389110147858",{"v":9.4,"d":"9.40"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":141,"d":"141.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2M8","Ø 70 mm svetelné návestie - trvalé svetlo - žltá - IP65 - 230 V",0.02]
["XVBC2M7","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":83.27182499999999,"d":"83.272"},"3389110147841",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":140.9,"d":"140.90"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2M7","Ø 70 mm svetelné návestie - trvalé svetlo - číra - IP65 - 230 V",0.02]
["XVBC2M6","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":87.38966249999999,"d":"87.390"},"3389110147834",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":140.9,"d":"140.90"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2M6","70 MM SVET. NÁVESTIE S TRVALÝM MODR. SVETLOM S LED IP65 230V",0.02]
["XVBC2M5","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":76.40876249999998,"d":"76.409"},"3389110147827",{"v":9.2,"d":"9.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":140,"d":"140.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2M5","osvetlená jednotka – trvalé svetlo – oranžové – 230 V AC",0.02]
["XVBC2M4","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":73.66353749999999,"d":"73.664"},"3389110147810",{"v":9.2,"d":"9.20"},{"v":8,"d":"8.00"},{"v":8.1,"d":"8.10"},{"v":140,"d":"140.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2M4","osvetlená jednotka – trvalé svetlo – červené – 230 V AC",0.02]
["XVBC2M3","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":72.74846249999999,"d":"72.748"},"3389110147803",{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":139,"d":"139.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2M3","osvetlená jednotka – trvalé svetlo – zelené – 230 V AC",0.02]
["XVBC2G8","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":83.27182499999999,"d":"83.272"},"3389110144666",{"v":9.5,"d":"9.50"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":138,"d":"138.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2G8","70 MM SVET. NÁVESTIE S TRVALÝM ŽLT. SVETLOM S LED IP65 120V",0.02]
["XVBC2G6","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":83.27182499999999,"d":"83.272"},"3389110145441",{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":139,"d":"139.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2G6","70 MM SVET. NÁVESTIE S TRVALÝM MODR. SVETLOM S LED IP65 120V",0.02]
["XVBC2G5","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":72.74846249999999,"d":"72.748"},"3389110145427",{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":141,"d":"141.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2G5","70 MM SVET. NÁVESTIE S TRVALÝM ORANŽ. SVETLOM S LED IP65 120V",0.02]
["XVBC2G4","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":72.74846249999999,"d":"72.748"},"3389110145007",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.2,"d":"9.20"},{"v":140,"d":"140.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2G4","70 MM SVET. NÁVESTIE S TRVALÝM ČERV. SVETLOM S LED IP65 120V",0.02]
["XVBC2G3","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":72.74846249999999,"d":"72.748"},"3389110144925",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.2,"d":"9.20"},{"v":141,"d":"141.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2G3","70 MM SVET. NÁVESTIE S TRVALÝM ZEL. SVETLOM S LED IP65 120V",0.02]
["XVBC2B8D","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":77.781375,"d":"77.781"},"3389119026468",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":150,"d":"150.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B8D","Ø 70 mm svetelné návestie s svet difuzorom-trvalé svetlo-žltá - IP65 - 24 V",0.02]
["XVBC2B8","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":83.27182499999999,"d":"83.272"},"3389110144543",{"v":9.019,"d":"9.02"},{"v":7.867,"d":"7.87"},7.88,{"v":137.8,"d":"137.80"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B8","osvetlená jednotka – trvalé svetlo – žlté – 24 V AC DC",0.02]
["XVBC2B7D","Svetelné návestie, Harmony XVB Universal",1,"ks",{"v":63.140175,"d":"63.140"},"3389119026451",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":153,"d":"153.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B7D","Svetelné návestie, Harmony XVB Universal, 70mm, svetelná jednotka, rozptýlené svetlo, číre, IP65, 24V",0]
["XVBC2B7","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":87.38966249999999,"d":"87.390"},"3389110144529",{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":10,"d":"10.00"},{"v":133,"d":"133.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B7","osvetlená jednotka – trvalé svetlo – číre – 24 V AC DC",0.02]
["XVBC2B6D","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":70.9183125,"d":"70.918"},"3389119026444",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":150,"d":"150.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B6D","Ø 70 mm svetelné návestie s svet difuzorom-trvalé svetlo- modrá - IP65 - 24 V",0.02]
["XVBC2B6","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":87.38966249999999,"d":"87.390"},"3389110144468",{"v":8,"d":"8.00"},{"v":9.3,"d":"9.30"},{"v":8,"d":"8.00"},{"v":136,"d":"136.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B6","osvetlená jednotka – trvalé svetlo – modré – 24 V AC DC",0.02]
["XVBC2B5D","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":77.781375,"d":"77.781"},"3389119026437",{"v":9.2,"d":"9.20"},{"v":9,"d":"9.00"},{"v":9.5,"d":"9.50"},{"v":150,"d":"150.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B5D","Ø 70 mm svetelné návestie s svet difuzorom-trvalé svetlo-oranžová-IP65-24 V",0.02]
["XVBC2B5","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":70.9183125,"d":"70.918"},"3389110144444",{"v":9.2,"d":"9.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":136,"d":"136.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B5","osvetlená jednotka – trvalé svetlo – oranžové – 24 V AC DC",0.02]
["XVBC2B4D","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":77.781375,"d":"77.781"},"3389119026420",{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":10,"d":"10.00"},{"v":150,"d":"150.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B4D","Ø 70 mm svetelné návestie s svet difuzorom-trvalé svetlo-červená-IP65-24 V",0.02]
["XVBC2B4","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":70.9183125,"d":"70.918"},"3389110144420",{"v":10,"d":"10.00"},{"v":9.3,"d":"9.30"},{"v":10,"d":"10.00"},{"v":135,"d":"135.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B4","osvetlená jednotka – trvalé svetlo – červené – 24 V AC DC",0.02]
["XVBC2B3D","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":77.781375,"d":"77.781"},"3389119026413",{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":150,"d":"150.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B3D","Ø 70 mm svetelné návestie s svet difuzorom-trvalé svetlo-zelená-IP65-24 V",0.02]
["XVBC2B3","SVET. NÁVESTIE S TRVALÝM SVETLOM S LED",1,"ks",{"v":70.9183125,"d":"70.918"},"3389110144260",{"v":9.137,"d":"9.14"},7.96,{"v":8.067,"d":"8.07"},{"v":137,"d":"137.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XVBC2B3","osvetlená jednotka – trvalé svetlo – zelené – 24 V AC DC",0.02]
["XVBC21B","Objímka ASi",1,"ks",{"v":311.1255,"d":"311.126"},"3389110421002",{"v":9.2,"d":"9.20"},{"v":9.4,"d":"9.40"},{"v":15.8,"d":"15.80"},{"v":276,"d":"276.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC21B","Ø 70 mm základná jednotka + kryt - s AS - aj pripojenie - čierna",0]
["XVBC21A","OBJÍMKA + KRYT (PRE AS-I)",1,"ks",{"v":329.42699999999996,"d":"329.427"},"3389110845044",{"v":7.8,"d":"7.80"},{"v":9.2,"d":"9.20"},{"v":7.8,"d":"7.80"},{"v":190,"d":"190.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC21A","základná jednotka + kryt pre blok XVB – s pripojením AS-i – čierna – IP 65",0]
["XVBC21","OBJÍMKA+KRYT",1,"ks",{"v":57.192187499999996,"d":"57.192"},"3389110845020",{"v":9.5,"d":"9.50"},{"v":8.5,"d":"8.50"},{"v":10,"d":"10.00"},{"v":190,"d":"190.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC21","zákl. jednotka+kryt pre blok XVB – bez trubky s impulz. výbojom – čier. – IP65",0]
["XVBC14","ADAPTÉR",1,"ks",{"v":7.686629999999999,"d":"7.687"},"3389110846027",{"v":3.5,"d":"3.50"},{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":14,"d":"14.00"},"FR","3926909790","https://www.se.com/sk/sk/product/XVBC14","súprava pre bočný vstup kábla s káblovým hrdlom Pg 13,5 – XVB",0]
["XVBC081","KRYT PRE XVBC",1,"ks",{"v":5.307434999999999,"d":"5.307"},"3389110514933",{"v":7.6,"d":"7.60"},{"v":2.4,"d":"2.40"},{"v":7.6,"d":"7.60"},{"v":33,"d":"33.00"},"FR","3926909790","https://www.se.com/sk/sk/product/XVBC081","krycia jednotka pre blok XVB – čierna – IP 65",0]
["XVBC07","OBJÍMKA",1,"ks",{"v":49.414049999999996,"d":"49.414"},"3389110845037",{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":12,"d":"12.00"},{"v":160,"d":"160.00"},"ID","8531900000","https://www.se.com/sk/sk/product/XVBC07","základná jednotka pre blok XVB – s trubkou s impulzným výbojom – čierna – IP 65",0]
["XVBC020","KRYT TRUBKY",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110846089",{"v":7,"d":"7.00"},{"v":7.4,"d":"7.40"},{"v":7,"d":"7.00"},{"v":62,"d":"62.00"},"FR","9030337000","https://www.se.com/sk/sk/product/XVBC020","kryt rúry d = 100 mm – hliníkový čierny – XVB",0]
["XVBC00","ADAPTÉR TRUBKA 1 2NPT",1,"ks",{"v":27.45225,"d":"27.452"},"3389110860481",{"v":9.6,"d":"9.60"},{"v":3.8,"d":"3.80"},{"v":4,"d":"4.00"},{"v":90,"d":"90.00"},"FR","8531900000","https://www.se.com/sk/sk/product/XVBC00","Harmony XVB, indicating blanc, 1/2\" NPT conduit adaptor for customer supplied tubing",0]
["XPSUS32AP","BEZPEČNOSTNÝ MODUL PREVENTA, skrutk.",1,"ks",{"v":310.59000000000003,"d":"310.590"},"3606489601836",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.8,"d":"13.80"},{"v":287,"d":"287.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUS32AP","safety module, Harmony XPSU, Cat 4, features 2 x XPSUAF with enabling movement, 48 to 240V AC or DC, screw",0.03]
["XPSUS32AC","BEZPEČNOSTNÝ MODUL PREVENTA, pruž.",1,"ks",{"v":310.59000000000003,"d":"310.590"},"3606489601829",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":289,"d":"289.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUS32AC","safety module, Harmony XPSU, Cat 4, features 2 x XPSUAF with enabling movement, 48 to 240V AC or DC, spring",0.03]
["XPSUS12AP","BEZPELNOSTNY MODUL PREVENTA, skrutkové s",1,"ks",305.235,"3606489601812",{"v":16,"d":"16.00"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":275,"d":"275.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUS12AP","safety module, Harmony XPSU, Cat 4, features 2 x XPSUAF with enabling movement, 24V AC or DC, screw",0.03]
["XPSUS12AC","BEZPEČNOSTNÝ MODUL PREVENTA, pruž.",1,"ks",{"v":310.59000000000003,"d":"310.590"},"3606489601805",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":200,"d":"200.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUS12AC","safety module, Harmony XPSU, Cat 4, features 2 x XPSUAF with enabling movement, 24V AC or DC, spring",0.03]
["XPSUEP34AP","BEZPECNOSTNY MODUL PREVENTA, skrutkové s",1,"ks",{"v":315.94500000000005,"d":"315.945"},"3606489601799",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":200,"d":"200.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUEP34AP","safety module, Harmony XPSU, Cat 4, expansion use with universal range, 48 to 240V AC or DC, screw",0.04]
["XPSUEP34AC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":315.94500000000005,"d":"315.945"},"3606489601782",{"v":15.8,"d":"15.80"},{"v":6.8,"d":"6.80"},{"v":14,"d":"14.00"},{"v":180,"d":"180.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUEP34AC","Safety module, Harmony Safety Automation, Cat.4, Expansion use with Universal range, 48-240v AC/DC, spring",0.04]
["XPSUEP14AP","BEZPELNOSTNY MODUL PREVENTA, skrutkové s",1,"ks",{"v":310.59000000000003,"d":"310.590"},"3606489601775",{"v":13.5,"d":"13.50"},{"v":6.5,"d":"6.50"},{"v":15.5,"d":"15.50"},{"v":200,"d":"200.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUEP14AP","safety module, Harmony XPSU, Cat 4, expansion use with universal range, 24V AC or DC, screw",0.03]
["XPSUEP14AC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":310.59000000000003,"d":"310.590"},"3606489601768",{"v":16,"d":"16.00"},{"v":7,"d":"7.00"},{"v":13.8,"d":"13.80"},{"v":295,"d":"295.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUEP14AC","safety module, Harmony XPSU, Cat 4, expansion use with universal range, 24V AC or DC, spring",0.03]
["XPSUDN33AP","BEZPECNOSTNY MODUL PREVENTA, skrutkové s",1,"ks",{"v":342.72,"d":"342.720"},"3606489601751",{"v":15.5,"d":"15.50"},{"v":7,"d":"7.00"},{"v":13.5,"d":"13.50"},{"v":340,"d":"340.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUDN33AP","safety module, Harmony XPSU, Cat 4, features 6 x XPSUAF, 48 to 240V AC or DC, screw",0.05]
["XPSUDN33AC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":342.72,"d":"342.720"},"3606489601744",{"v":15.8,"d":"15.80"},{"v":7,"d":"7.00"},{"v":14,"d":"14.00"},{"v":350,"d":"350.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUDN33AC","Safety module, Harmony Safety Automation, Cat.4, features 6*XPSUAF, 48-240v AC/DC, spring",0.05]
["XPSUDN13AP","BEZPELNOSTNY MODUL PREVENTA, skrutkové",1,"ks",{"v":342.72,"d":"342.720"},"3606489601737",{"v":13.5,"d":"13.50"},{"v":13.5,"d":"13.50"},{"v":13.5,"d":"13.50"},{"v":350,"d":"350.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUDN13AP","safety module, Harmony XPSU, Cat 4, features 6 x XPSUAF, 24V AC or DC, screw",0.05]
["XPSUDN13AC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":342.72,"d":"342.720"},"3606489601720",{"v":15.5,"d":"15.50"},{"v":7,"d":"7.00"},{"v":13.5,"d":"13.50"},{"v":417,"d":"417.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUDN13AC","safety module, Harmony XPSU, Cat 4, features 6 x XPSUAF, 24V AC or DC, spring",0.05]
["XPSUAT33A3AP","BEZPELCNOSTNY MODUL PREVENTA, skrutkové",1,"ks",369.495,"3606489601713",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.7,"d":"13.70"},{"v":450,"d":"450.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUAT33A3AP","safety module, Harmony XPSU, Cat4, features XPSUAK with delayed outputs, 48 to 240V AC or DC, screw",0.05]
["XPSUAT33A3AC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":342.72,"d":"342.720"},"3606489601706",{"v":15.8,"d":"15.80"},{"v":6.8,"d":"6.80"},{"v":14,"d":"14.00"},{"v":350,"d":"350.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUAT33A3AC","safety module, Harmony XPSU, Cat4, features XPSUAK with delayed outputs, 48 to 240V AC or DC, spring",0.05]
["XPSUAT13A3AP","BEZPELNOSTNY MODUL PREVENTA, skrutkové s",1,"ks",{"v":342.72,"d":"342.720"},"3606489601690",{"v":13.5,"d":"13.50"},{"v":6.5,"d":"6.50"},{"v":15.5,"d":"15.50"},{"v":350,"d":"350.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAT13A3AP","safety module, Harmony XPSU, Cat4, features XPSUAK with delayed outputs, 24V AC or DC, screw",0.05]
["XPSUAT13A3AC","BEZPELNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":342.72,"d":"342.720"},"3606489601683",{"v":13.5,"d":"13.50"},{"v":6.5,"d":"6.50"},{"v":15.5,"d":"15.50"},{"v":449,"d":"449.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAT13A3AC","safety module, Harmony XPSU, Cat4, features XPSUAK with delayed outputs, 24V AC or DC, spring",0.05]
["XPSUAK32AP","BEZPELCNOSTNY MODUL PREVENTA, skrutkové",1,"ks",{"v":198.13500000000002,"d":"198.135"},"3606489601676",{"v":16,"d":"16.00"},{"v":7,"d":"7.00"},{"v":14,"d":"14.00"},{"v":200,"d":"200.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAK32AP","Safety module, Harmony XPSU, Cat 4, features XPSUAF with PNP or NPN, safety mat, 48 to 240V AC or DC, screw",0.03]
["XPSUAK32AC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":198.13500000000002,"d":"198.135"},"3606489601669",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":200,"d":"200.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAK32AC","safety module, Harmony XPSU, Cat 4, features XPSUAF with PNP or NPN, safety mat, 48 to 240V AC or DC, spring",0.04]
["XPSUAK12AP","BEZPELCNOSTNY MODUL PREVENTA, skrutkové",1,"ks",{"v":192.78,"d":"192.780"},"3606489601652",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":277,"d":"277.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAK12AP","safety module, Harmony XPSU, Cat 4, features XPSUAF with PNP or NPN, safety mat, 24V AC or DC, screw",0.03]
["XPSUAK12AC","BEZPECNOSTNÝ MODUL PREVENTA, pružinové s",1,"ks",{"v":192.78,"d":"192.780"},"3606489601645",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":280,"d":"280.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAK12AC","safety module, Harmony XPSU, Cat 4, features XPSUAF with PNP or NPN, safety mat, 24V AC or DC, spring",0.03]
["XPSUAF33AP","BEZPECNOSTNY MODUL PREVENTA, skrutkové s",1,"ks",{"v":192.78,"d":"192.780"},"3606489601638",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.7,"d":"13.70"},{"v":286,"d":"286.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAF33AP","safety module, Harmony XPSU, Cat 4, potential free 2 NC, NO NC, 2 PNP, 48 to 240V AC or DC, screw",0.03]
["XPSUAF33AC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":192.78,"d":"192.780"},"3606489601621",{"v":15.8,"d":"15.80"},{"v":6.8,"d":"6.80"},{"v":14,"d":"14.00"},{"v":200,"d":"200.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAF33AC","safety module, Harmony XPSU, Cat 4, potential free 2 NC, NO NC, 2 PNP, 48 to 240V AC or DC, spring",0.03]
["XPSUAF13AP","BEZPELCNOSTNY MODUL PREVENTA, skrutkové",1,"ks",187.425,"3606489601614",{"v":15.5,"d":"15.50"},{"v":6.7,"d":"6.70"},{"v":13.7,"d":"13.70"},{"v":276,"d":"276.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAF13AP","safety module, Harmony XPSU, Cat 4, potential free 2 NC, NO NC, 2 PNP, 24V AC or DC, screw",0.03]
["XPSUAF13AC","BEZPELNOSTNY MODUL PREVENTA, pružinové s",1,"ks",187.425,"3606489601607",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":14,"d":"14.00"},{"v":279,"d":"279.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAF13AC","safety module, Harmony XPSU, Cat 4, potential free 2 NC, NO NC, 2 PNP, 24V AC or DC, spring",0.03]
["XPSUAB31CP","BEZPECNOSTNY MODUL PREVENTA, skrutkové s",1,"ks",{"v":267.75,"d":"267.750"},"3606489601591",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":262,"d":"262.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUAB31CP","safety module, Harmony XPSU, Cat 1, potential free 2 NC, NO NC, 2 PNP, 48 to 240V AC or DC, screw",0.03]
["XPSUAB31CC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":267.75,"d":"267.750"},"3606489601584",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":14,"d":"14.00"},{"v":200,"d":"200.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSUAB31CC","safety module, Harmony XPSU, Cat 1, potential free 2 NC, NO NC, 2 PNP, 48 to 240V AC or DC, spring",0.03]
["XPSUAB11CP","BEZPELNOSTNY MODUL PREVENTA, skrutkové s",1,"ks",{"v":267.75,"d":"267.750"},"3606489601577",{"v":13.5,"d":"13.50"},{"v":6.5,"d":"6.50"},{"v":15.5,"d":"15.50"},{"v":250,"d":"250.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAB11CP","safety module, Harmony XPSU, Cat 1, potential free 2 NC, NO NC, 2 PNP, 24V AC or DC, screw",0.03]
["XPSUAB11CC","BEZPECNOSTNY MODUL PREVENTA, pružinové s",1,"ks",{"v":267.75,"d":"267.750"},"3606489601560",{"v":15.5,"d":"15.50"},{"v":6.8,"d":"6.80"},{"v":14,"d":"14.00"},{"v":261,"d":"261.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSUAB11CC","safety module, Harmony XPSU, Cat 1, potential free 2 NC, NO NC, 2 PNP, 24V AC or DC, spring",0.03]
["XPSPVT1180","MODUL PREVENTA",1,"ks",797.895,"3389110724837",{"v":8.3,"d":"8.30"},{"v":11.3,"d":"11.30"},{"v":13.2,"d":"13.20"},{"v":540,"d":"540.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSPVT1180","module XPS-PV - hydraulic valves on linear presses - 24 V DC",0.07]
["XPSPVK3784","PREVENTA SLED. SOLENOID. VENTILOV 230V",1,"ks",1012.095,"3389110727951",{"v":22.5,"d":"22.50"},{"v":9,"d":"9.00"},{"v":14.5,"d":"14.50"},{"v":1016,"d":"1,016.00"},"ID","8537109899","https://www.se.com/sk/sk/product/XPSPVK3784","module XPSPV - double-bodied solenoid valves - 230 V AC",0.12]
["XPSPVK3484","PREVENTA SLED. SOLENOID. VENTILOV 115V",1,"ks",1012.095,"3389110727944",{"v":22.5,"d":"22.50"},{"v":9,"d":"9.00"},{"v":14.5,"d":"14.50"},{"v":900,"d":"900.00"},"ID","8537109899","https://www.se.com/sk/sk/product/XPSPVK3484","module XPSPV - double-bodied solenoid valves - 115 V AC",0.12]
["XPSPVK1184","BEZPELNOSTNY MODUL PREVENTA",1,"ks",{"v":963.9,"d":"963.900"},"3389110727937",{"v":22.5,"d":"22.50"},{"v":9,"d":"9.00"},{"v":14.2,"d":"14.20"},{"v":700,"d":"700.00"},"ID","8537109899","https://www.se.com/sk/sk/product/XPSPVK1184","module XPSPV - double-bodied solenoid valves - 24 V DC",0.09]
["XPSOT3744","BEZP. MODUL PREVENTA",1,"ks",{"v":1285.2,"d":"1285.200"},"3389110724769",{"v":22.2,"d":"22.20"},{"v":8.8,"d":"8.80"},{"v":14.2,"d":"14.20"},{"v":1100,"d":"1,100.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSOT3744","module XPSOT - stop at top dead center with automatic overtravel - 230 V AC",0.14]
["XPSOT3444","BEZPELNOSTNY MODUL PREVENTA",1,"ks",{"v":1285.2,"d":"1285.200"},"3389110724752",{"v":14.5,"d":"14.50"},{"v":9,"d":"9.00"},{"v":22.5,"d":"22.50"},{"v":1225,"d":"1,225.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSOT3444","module XPSOT - stop at top dead center with automatic overtravel - 115 V AC",0.15]
["XPSMCTS32","KONEKTOR SO SKRUT. SVORKAMI PRE XPSMC32X",1,"ks",144.585,"3389110710298",{"v":7.5,"d":"7.50"},{"v":4.8,"d":"4.80"},{"v":5.7,"d":"5.70"},{"v":114,"d":"114.00"},"ZZ","8536901000","https://www.se.com/sk/sk/product/XPSMCTS32","zasúvací skrutkový konektor – pre konfigurovateľný bezpečnostný ovládač XPSMC32Z",0]
["XPSMCTS16","KONEKTOR SO SKRUT. SVORKAMI PRE XPSMC16X",1,"ks",88.893,"3389110710281",{"v":7.5,"d":"7.50"},{"v":5.5,"d":"5.50"},{"v":3.5,"d":"3.50"},{"v":80,"d":"80.00"},"DE","8536901000","https://www.se.com/sk/sk/product/XPSMCTS16","zasúvací skrutkový konektor – pre konfigurovateľný bezpečnostný ovládač XPSMC16Z",0]
["XPSMCTC32","KONEKTOR S PRUŽ. SVORKAMI PRE XPSMC32X",1,"ks",{"v":128.52,"d":"128.520"},"3389110710274",{"v":7.6,"d":"7.60"},{"v":4.6,"d":"4.60"},{"v":5.3,"d":"5.30"},{"v":80,"d":"80.00"},"DE","85369010","https://www.se.com/sk/sk/product/XPSMCTC32","zasúvací pružinový konektor – pre konfigurovateľný bezpečnostný ovládač XPSMC32Z",0]
["XPSMCTC16","TERMINALS WITH CAGE CLAMP CONNECTION FOR",1,"ks",86.751,"3389110710267",{"v":4.7,"d":"4.70"},{"v":5.4,"d":"5.40"},{"v":7.6,"d":"7.60"},{"v":57,"d":"57.00"},"DE","8536901000","https://www.se.com/sk/sk/product/XPSMCTC16","KONEKTOR S PRUŽ. SVORKAMI PRE XPSMC16X",0]
["XPSMCSCY","Prepojovací kábel",1,"ks",95.319,"3389119012317",{"v":16,"d":"16.00"},{"v":1.7,"d":"1.70"},{"v":10,"d":"10.00"},{"v":62,"d":"62.00"},"FR","8544429090","https://www.se.com/sk/sk/product/XPSMCSCY","Modbus sériový prepoj. kábel - 1 RJ45/1 SUB - D 25 - 0.3 m",0.01]
["XPSMCMRO0004G","Bezpečnostný rozširujúci modul, 4 relé",1,"ks",{"v":594.4050000000001,"d":"594.405"},"3606480748882",{"v":12.2,"d":"12.20"},{"v":4.6,"d":"4.60"},{"v":16.2,"d":"16.20"},{"v":288,"d":"288.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMRO0004G","Bezpečnostný rozširujúci modul, 4 relé, pružinové svorky",0]
["XPSMCMRO0004DA","Bezpečnostný rozširujúci modul",1,"ks",583.695,"3606480748875",{"v":12.2,"d":"12.20"},{"v":4.4,"d":"4.40"},{"v":15.8,"d":"15.80"},{"v":308,"d":"308.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMRO0004DA","bezpečnostný rozširujúci modul, 4 reléové výstupy, 8 stavových výstupů",0.04]
["XPSMCMRO0004","Bezpečnostný rozširujúci modul",1,"ks",{"v":535.5,"d":"535.500"},"3606480748899",{"v":16.1,"d":"16.10"},{"v":4.2,"d":"4.20"},{"v":12.5,"d":"12.50"},{"v":294,"d":"294.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMRO0004","bezpečnostný rozširujúci modul, 4 reléové výstupy",0.03]
["XPSMCMMX0804G","Bezpečnostný rozširovací modul Modicon M",1,"ks",{"v":658.6650000000001,"d":"658.665"},"3606481987174",{"v":4.3,"d":"4.30"},{"v":16,"d":"16.00"},{"v":12.5,"d":"12.50"},{"v":250,"d":"250.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMMX0804G","Bezpečnostný rozširovací modul Modicon MCM, 8 DI 4 DO, pružinové svorky",0.03]
["XPSMCMMX0802G","Bezp. rozš. modul 8 vstupov, 2 výstupy",1,"ks",{"v":396.27000000000004,"d":"396.270"},"3606480748844",{"v":12.4,"d":"12.40"},{"v":4.4,"d":"4.40"},{"v":15.8,"d":"15.80"},{"v":242,"d":"242.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMMX0802G","Bezpečnostný rozširujúci modul 8 vstupov, 2 výstupy, 2 OSSD, 4 test.vstup.okruhov, pružné svorky",0.03]
["XPSMCMMX0802","Bezpečn.rozšir.modul vstupov/výstupov",1,"ks",423.045,"3606480748851",{"v":16,"d":"16.00"},{"v":4.4,"d":"4.40"},{"v":12.2,"d":"12.20"},{"v":253,"d":"253.00"},"FR","8536909500","https://www.se.com/sk/sk/product/XPSMCMMX0802","bezpečnostný rozširujúci modul 8 vstupov/ 2výstupy so skrutk. svorkami",0.03]
["XPSMCMME0000","Pamäťová karta",1,"ks",51.408,"3606480748837",{"v":5.2,"d":"5.20"},{"v":2.6,"d":"2.60"},{"v":10,"d":"10.00"},{"v":18,"d":"18.00"},"IT","8523519000","https://www.se.com/sk/sk/product/XPSMCMME0000","pamäťová karta pre ukladanie konfigurácie a prenos údajov do nového zariad.",0]
["XPSMCMER0004G","Bezpečnostný rozširovací modul Modicon M",1,"ks",358.785,"3606480748813",{"v":16.2,"d":"16.20"},{"v":4.5,"d":"4.50"},{"v":12.8,"d":"12.80"},{"v":294,"d":"294.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMER0004G","Bezpečnostný rozširovací modul Modicon MCM, 4 reléové výstupy, pružinové svorky",0.04]
["XPSMCMER0004","Bezpečnostný rozširujúcí modul, 4 relé",1,"ks",{"v":315.94500000000005,"d":"315.945"},"3606480748820",{"v":16.2,"d":"16.20"},{"v":4.6,"d":"4.60"},{"v":12.4,"d":"12.40"},{"v":305,"d":"305.00"},"FR","8536909500","https://www.se.com/sk/sk/product/XPSMCMER0004","bezpečnostný rozširujúcí modul, 4 releové výstupy so skrutkovými svorkami",0.03]
["XPSMCMER0002","Bezpečnostný rozširujúci modul",1,"ks",{"v":230.26500000000001,"d":"230.265"},"3606480748806",{"v":12.2,"d":"12.20"},{"v":4.4,"d":"4.40"},{"v":15.8,"d":"15.80"},{"v":236,"d":"236.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMER0002","bezpečnostný rozširujúci modul, 2 reléové výstupy so skrutkovými svorkami",0.03]
["XPSMCMEN0200SC","Bezpečnostný rozširujúci modul",1,"ks",{"v":838.5930000000001,"d":"838.593"},"3606480748769",{"v":16.1,"d":"16.10"},{"v":4.2,"d":"4.20"},{"v":12.5,"d":"12.50"},{"v":236,"d":"236.00"},"IT","8537109899","https://www.se.com/sk/sk/product/XPSMCMEN0200SC","bezp.rozširujúci modul pre monit.rýchlosti, 2x IRC so skrutkovými svorkami",""]
["XPSMCMEN0200","Bezpečnostný rozširujúci modul",1,"ks",{"v":615.8249999999999,"d":"615.825"},"3606480748912",{"v":16.2,"d":"16.20"},{"v":4.6,"d":"4.60"},{"v":12.2,"d":"12.20"},{"v":224,"d":"224.00"},"IT","9031808000","https://www.se.com/sk/sk/product/XPSMCMEN0200","bezp.rozširujúci modul pre monitorování rychlosti so skrutkovými svorkami",0.03]
["XPSMCMEN0100SC","Bezpečnostný rozširujúci modul",1,"ks",887.859,"3606480748707",{"v":16.1,"d":"16.10"},{"v":4.2,"d":"4.20"},{"v":12.5,"d":"12.50"},{"v":227,"d":"227.00"},"IT","9031808000","https://www.se.com/sk/sk/product/XPSMCMEN0100SC","bezp.rozširujúci modul pre monit.rýchlosti, 1x IRC so skrutkovými svorkami",""]
["XPSMCMDO00042AG","Bezp. rozš. modul, 4 single OSSD výstupy",1,"ks",{"v":508.72499999999997,"d":"508.725"},"3606481987112",{"v":16.5,"d":"16.50"},{"v":4.6,"d":"4.60"},{"v":12.6,"d":"12.60"},{"v":249,"d":"249.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMDO00042AG","Bezpečnostný rozširujúci modul, 4 single OSSD výstupy 2A, pružné svorky",0.03]
["XPSMCMDO00042A","Bezp. rozš. modul, 4 single/dual OSSD",1,"ks",{"v":508.72499999999997,"d":"508.725"},"3606481987105",{"v":12.5,"d":"12.50"},{"v":16,"d":"16.00"},{"v":4.3,"d":"4.30"},{"v":250,"d":"250.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMDO00042A","Bezpečnostný rozširujúci modul, 4 single alebo 2 dual OSSD výstupy 2A",0.03]
["XPSMCMDO0004","Bezpečnostný rozširujúci modul",1,"ks",{"v":406.98,"d":"406.980"},"3606480748660",{"v":16.2,"d":"16.20"},{"v":4.4,"d":"4.40"},{"v":12.2,"d":"12.20"},{"v":250,"d":"250.00"},"FR","8536909500","https://www.se.com/sk/sk/product/XPSMCMDO0004","bezpečnostný rozširujúci modul, 4 + 4 výstupy so skrutkovými svorkami",0.03]
["XPSMCMDO0002","Bezpečnostný rozširujúci modul",1,"ks",{"v":353.43,"d":"353.430"},"3606480748646",{"v":16.2,"d":"16.20"},{"v":4.2,"d":"4.20"},{"v":12.4,"d":"12.40"},{"v":228,"d":"228.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMDO0002","bezpečnostný rozširujúci modul, 2 + 2 výstupy so skrutkovými svorkami",0.03]
["XPSMCMDI1600G","Bezpeč.rozš. modul, 16 vstupov",1,"ks",380.205,"3606480748615",{"v":16.2,"d":"16.20"},{"v":4.5,"d":"4.50"},{"v":12.8,"d":"12.80"},{"v":242,"d":"242.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMDI1600G","Bezpečnostný rozširujúci modul, 16 vstupov, 4 test.vstup.okruhov, pružné svorky",0]
["XPSMCMDI1600","Bezpečnostný rozširujúci modul",1,"ks",390.915,"3606480748622",{"v":16,"d":"16.00"},{"v":4.4,"d":"4.40"},{"v":12.2,"d":"12.20"},{"v":251,"d":"251.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMDI1600","bezpečnostný rozširujúci modul, 16 vstupov so skrutkovými svorkami",0.03]
["XPSMCMDI1200MT","Bezpečnostný rozširujúci modul",1,"ks",536.571,"3606480748608",{"v":16.1,"d":"16.10"},{"v":4.2,"d":"4.20"},{"v":12.5,"d":"12.50"},{"v":226,"d":"226.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMDI1200MT","bezpečnostný rozširujúci modul, 12 vstupov so skrutkovými svorkami",""]
["XPSMCMDI0800","Bezpečnostný rozširujúci modul",1,"ks",{"v":342.72,"d":"342.720"},"3606480748585",{"v":12.2,"d":"12.20"},{"v":4.6,"d":"4.60"},{"v":16.2,"d":"16.20"},{"v":216,"d":"216.00"},"FR","8536909500","https://www.se.com/sk/sk/product/XPSMCMDI0800","bezpečnostný rozširujúci modul, 8 vstupov so skrutkovými svorkami",0.03]
["XPSMCMCP0802BCG","XPSMC CPU, 8 vstupov + 2 OSSD výstupy",1,"ks",{"v":546.21,"d":"546.210"},"3606480992056",{"v":16.5,"d":"16.50"},{"v":4.5,"d":"4.50"},{"v":12.5,"d":"12.50"},{"v":256,"d":"256.00"},"IT","8537109899","https://www.se.com/sk/sk/product/XPSMCMCP0802BCG","Centrálná procesorová jednotka, 8 vstupov + 2 OSSD výstupy, 4 test.vstup.okruhov, pružné svorky",0.03]
["XPSMCMCP0802BC","Centrálna procesorová jednotka, 8I 2O",1,"ks",530.145,"3606480992049",{"v":16,"d":"16.00"},{"v":4.2,"d":"4.20"},{"v":12.5,"d":"12.50"},{"v":263,"d":"263.00"},"IT","8537109899","https://www.se.com/sk/sk/product/XPSMCMCP0802BC","Centrálna procesorová jednotka, 8 vstupov a 2 výstupy, skrutkové svorky",0]
["XPSMCMCP0802","Centr.procesor.jednotka,8 vstup+2 výstup",1,"ks",{"v":498.01500000000004,"d":"498.015"},"3606480748561",{"v":16.5,"d":"16.50"},{"v":4.5,"d":"4.50"},{"v":12.5,"d":"12.50"},{"v":249,"d":"249.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XPSMCMCP0802","centrálná procesorová jednotka, 8 vstupov + 2 výstupy so skrutkovými svorkami",0.03]
["XPSMCMCO0000S2","Bezpečnostný komunikačný modul RS 485",1,"ks",358.785,"3606480748523",{"v":16.1,"d":"16.10"},{"v":4.5,"d":"4.50"},{"v":12.5,"d":"12.50"},{"v":219,"d":"219.00"},"FR","85365080","https://www.se.com/sk/sk/product/XPSMCMCO0000S2","bezpečnostný komunikačný modul RS 485, dvojkanálový so skrutkovými svorkami",0.03]
["XPSMCMCO0000S1","Bezpečnostný komunikačný modul RS 485",1,"ks",{"v":332.01,"d":"332.010"},"3606480748509",{"v":15.8,"d":"15.80"},{"v":4.2,"d":"4.20"},{"v":12.2,"d":"12.20"},{"v":209,"d":"209.00"},"FR","85365080","https://www.se.com/sk/sk/product/XPSMCMCO0000S1","bezpečnostný komunikačný modul RS 485, jednokanálový so skrutkovými svorkami",0.02]
["XPSMCMCO0000PB","Profibus DP komunikačný modul",1,"ks",{"v":578.34,"d":"578.340"},"3606480748486",{"v":16.2,"d":"16.20"},{"v":4.5,"d":"4.50"},{"v":12.8,"d":"12.80"},{"v":213,"d":"213.00"},"IT","8536909500","https://www.se.com/sk/sk/product/XPSMCMCO0000PB","Profibus DP komunikačný modul",0.03]
["XPSMCMCO0000EM","Komunikačný modul Modbus TCP",1,"ks",{"v":578.34,"d":"578.340"},"3606480748424",{"v":16.2,"d":"16.20"},{"v":4.5,"d":"4.50"},{"v":12.7,"d":"12.70"},{"v":233,"d":"233.00"},"IT","8517620000","https://www.se.com/sk/sk/product/XPSMCMCO0000EM","komunikačný modul Modbus TCP so skrutkovými svorkami",0.03]
["XPSMCMCO0000EIG","Ethernet/IP komunikačný modul RJ45",1,"ks",{"v":658.6650000000001,"d":"658.665"},"3606480748394",{"v":16.3,"d":"16.30"},{"v":4.5,"d":"4.50"},{"v":12.7,"d":"12.70"},{"v":209,"d":"209.00"},"IT","8517620000","https://www.se.com/sk/sk/product/XPSMCMCO0000EIG","expansion module, Modicon MCM, Ethernet/IP diagnostic, spring",0.03]
["XPSMCMCO0000EI","Komunikačný modul Ethernet/IP",1,"ks",{"v":578.34,"d":"578.340"},"3606480748400",{"v":16.2,"d":"16.20"},{"v":4.5,"d":"4.50"},{"v":12.7,"d":"12.70"},{"v":228,"d":"228.00"},"IT","8517620000","https://www.se.com/sk/sk/product/XPSMCMCO0000EI","komunikačný modul Ethernet/IP so skrutkovými svorkami",0.03]
["XPSMCMCO0000EC","Diagnostický modul ETHERCAT pro Preventu",1,"ks",{"v":599.76,"d":"599.760"},"3606480748387",{"v":12.4,"d":"12.40"},{"v":16,"d":"16.00"},{"v":4.3,"d":"4.30"},{"v":305,"d":"305.00"},"IT","8517620000","https://www.se.com/sk/sk/product/XPSMCMCO0000EC","EtherCAT diagnostic expansion module, Modicon MCM, screw term",0.04]
["XPSMCMCN0000SG","Prepojovací konektor",1,"ks",24.633,"3606480748325",{"v":4.5,"d":"4.50"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":18,"d":"18.00"},"FR","8536909500","https://www.se.com/sk/sk/product/XPSMCMCN0000SG","prepojovací konektor na pripojene rozširovacieho modulu",0]
["XPSMCMC10804BG","Bezpečnostný kontrolér Modicon MCM, 8 vs",1,"ks",{"v":610.47,"d":"610.470"},"3606481987082",{"v":16.4,"d":"16.40"},{"v":4.5,"d":"4.50"},{"v":12.8,"d":"12.80"},{"v":262,"d":"262.00"},"IT","8537109199","https://www.se.com/sk/sk/product/XPSMCMC10804BG","Bezpečnostný kontrolér Modicon MCM, 8 vstupov 4 výstupy, pružinové svorky",0.03]
["XPSMCMC10804","Modulárny safety kontrolér s 8/4 V/V",1,"ks",{"v":578.34,"d":"578.340"},"3606481987068",{"v":4.3,"d":"4.30"},{"v":16,"d":"16.00"},{"v":12.5,"d":"12.50"},{"v":257,"d":"257.00"},"IT","8537109199","https://www.se.com/sk/sk/product/XPSMCMC10804","Modulárny safety kontrolér s 8/4 V/V so skrutkovými svorkami",0.03]
["XPSMCCPC","ADAPTÉR MINI DIN-RJ45",1,"ks",{"v":139.23000000000002,"d":"139.230"},"3389110356427",{"v":12,"d":"12.00"},{"v":1.4,"d":"1.40"},{"v":8.6,"d":"8.60"},{"v":11,"d":"11.00"},"DE","8536909500","https://www.se.com/sk/sk/product/XPSMCCPC","Preventa Safety - adaptor RJ45 socket/PC connection cables",0]
["XPSMC32ZP","BEZPEČNOSTNÝ KONTROLÉR 32 VST. PROFIBUS",1,"ks",{"v":2302.65,"d":"2302.650"},"3389119010290",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":18,"d":"18.00"},{"v":840,"d":"840.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XPSMC32ZP","bezpečnostný ovládač XPS-MC – 24 V DC – 32 vstupov – 48 LED signalizácií",0.15]
["XPSMC32ZC","BEZPEČNOSTNÝ KONTROLÉR 32 VST. CANOPEN",1,"ks",{"v":2142,"d":"2142.000"},"3389119010283",{"v":25.8,"d":"25.80"},{"v":9.4,"d":"9.40"},{"v":17.8,"d":"17.80"},{"v":1280,"d":"1,280.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XPSMC32ZC","bezpečnostný ovládač XPS-MC – 24 V DC – 32 vstupov – 48 LED signalizácií",0.15]
["XPSMC32Z","BEZPEČNOSTNÝ KONTROLÉR 32 VST. MODBUS",1,"ks",{"v":2142,"d":"2142.000"},"3389119010276",{"v":26,"d":"26.00"},{"v":9.3,"d":"9.30"},{"v":18,"d":"18.00"},{"v":1199,"d":"1,199.00"},"ZZ","8537109899","https://www.se.com/sk/sk/product/XPSMC32Z","bezpečnostný ovládač XPS-MC – 24 V DC – 32 vstupov – 46 LED signalizácií",0.14]
["XPSMC16ZP","BEZPEČNOSTNÝ KONTROLÉR 16 VST. PROFIBUS",1,"ks",{"v":1767.1499999999999,"d":"1767.150"},"3389119010269",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":18,"d":"18.00"},{"v":1278,"d":"1,278.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XPSMC16ZP","bezpečnostný ovládač XPS-MC – 24 V DC – 16 vstupov – 32 LED signalizácií",0.15]
["XPSMC16ZC","BEZPEČNOSTNÝ KONTROLÉR 16 VSTUPOV",1,"ks",{"v":1660.05,"d":"1660.050"},"3389119010252",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":18,"d":"18.00"},{"v":1265,"d":"1,265.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XPSMC16ZC","bezpečnostný ovládač XPS-MC – 24 V DC – 16 vstupov – 32 LED signalizácií",0.15]
["XPSMC16Z","BEZPEČNOSTNÝ KONTROLÉR 16 VST. MODBUS",1,"ks",{"v":1499.4,"d":"1499.400"},"3389119010245",{"v":26,"d":"26.00"},{"v":9.6,"d":"9.60"},{"v":18,"d":"18.00"},{"v":1200,"d":"1,200.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XPSMC16Z","bezpečnostný ovládač XPS-MC – 24 V DC – 16 vstupov – 30 LED signalizácií",0.14]
["XPSES","Plomba predného krytu, Harmony Safety",1,"ks",5.355,"3606489601553",{"v":21.5,"d":"21.50"},{"v":0.8,"d":"0.80"},{"v":15,"d":"15.00"},{"v":21,"d":"21.00"},"ID","3926909790","https://www.se.com/sk/sk/product/XPSES","Plomba predného krytu, Harmony Safety",0]
["XPSCM1144P","BEZP. MODUL ZÁVORA TYP2",1,"ks",605.115,"3389110274134",{"v":11.8,"d":"11.80"},{"v":16,"d":"16.00"},{"v":6.2,"d":"6.20"},{"v":411,"d":"411.00"},"ID","8536508090","https://www.se.com/sk/sk/product/XPSCM1144P","modul XPS - CM - single - beam fotoelektrické snímače - 24 V DC",0.05]
["XPSCM1144","BEZP. MODUL ZÁVORA TYP2",1,"ks",{"v":589.05,"d":"589.050"},"3389110274127",{"v":16,"d":"16.00"},{"v":6.4,"d":"6.40"},{"v":11.6,"d":"11.60"},{"v":400,"d":"400.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSCM1144","modul XPS - CM - single - beam fotoelektrické snímače - 24 V DC",0.05]
["XPSBAT12A1AP","Bezpečnostný modul Preventa",1,"ks",{"v":257.04,"d":"257.040"},"3606482034044",{"v":15.5,"d":"15.50"},{"v":6.8,"d":"6.80"},{"v":13.8,"d":"13.80"},{"v":287,"d":"287.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSBAT12A1AP","Bezpečnostný modul Preventa",0.03]
["XPSBAC34AP","XPS Basic,48-240V AC/DC, Estop, Guard sw",1,"ks",{"v":224.91000000000003,"d":"224.910"},"3606482034020",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":305,"d":"305.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSBAC34AP","Bezpečnostný modul Harmony XPS Basic, 48-240V AC/DC, E-stop, Guard switch",0.04]
["XPSBAC34AC","Bezpečnostný modul Preventa pre núdzové",1,"ks",{"v":192.78,"d":"192.780"},"3606482039308",{"v":15.7,"d":"15.70"},{"v":6.9,"d":"6.90"},{"v":13.5,"d":"13.50"},{"v":313,"d":"313.00"},"ID","8536490099","https://www.se.com/sk/sk/product/XPSBAC34AC","Bezpečnostný modul Preventa pre núdzové zastavenie,  48-240 V AC, žiadny výstup, pružinové svorky",0.04]
["XPSBAC14AP","XPS Basic, 24V AC/DC, E-stop, Guard sw",1,"ks",{"v":208.84500000000003,"d":"208.845"},"3606482034013",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":302,"d":"302.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSBAC14AP","Bezpečnostný modul Harmony XPS Basic, 24V AC/DC, E-stop, Guard switch",0.04]
["XPSBAC14AC","Bezpečnostný modul Preventa pre núdzové",1,"ks",{"v":171.36,"d":"171.360"},"3606481916815",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":301,"d":"301.00"},"ID","8536419089","https://www.se.com/sk/sk/product/XPSBAC14AC","Bezpečnostný modul Preventa pre núdzové zastavenie, 24 V ACDC, žiadny výstup, pružinové svorky",0.04]
["XPEZ913","RUKOVÄŤ NA OCHRANNÝ KRYT",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389110764857",{"v":63,"d":"63.00"},{"v":5,"d":"5.00"},{"v":15.5,"d":"15.50"},{"v":554,"d":"554.00"},"FR","85389099","https://www.se.com/sk/sk/product/XPEZ913","rukoväť – pre XPE-Z901/Z911",0]
["XPEZ911","OCHRANNÝ KRYT PRE XPE",1,"ks",{"v":91.5075,"d":"91.508"},"3389110471274",{"v":23.6,"d":"23.60"},{"v":16.2,"d":"16.20"},{"v":18,"d":"18.00"},{"v":1170,"d":"1,170.00"},"MA","8538909999","https://www.se.com/sk/sk/product/XPEZ911","ochranný kryt – pre XPE-R",0]
["XPEZ903","ZARÁŽKA PRE XPE",1,"ks",{"v":21.046725,"d":"21.047"},"3389110600407",{"v":13.2,"d":"13.20"},{"v":2.5,"d":"2.50"},{"v":10.6,"d":"10.60"},{"v":188,"d":"188.00"},"FR","8538909999","https://www.se.com/sk/sk/product/XPEZ903","Preventa XPE – spúšťací mechanizmus – pre kovový nožný spínač XPEM XPER",0]
["XPEZ902","OPIERKA PÄTY PRE NOŽ.SP. XPE-M",1,"ks",{"v":64.05524999999999,"d":"64.055"},"3389110662467",{"v":22,"d":"22.00"},{"v":5,"d":"5.00"},{"v":11,"d":"11.00"},{"v":236,"d":"236.00"},"FR","7616991099","https://www.se.com/sk/sk/product/XPEZ902","Preventa XPE – opierka päty – pre kovový nožný spínač XPEM",0]
["XPEZ901","NOŽNÝ SPÍNAČ",1,"ks",{"v":75.03614999999999,"d":"75.036"},"3389110600391",{"v":21,"d":"21.00"},{"v":17.5,"d":"17.50"},{"v":20,"d":"20.00"},{"v":1180,"d":"1,180.00"},"MA","8538909999","https://www.se.com/sk/sk/product/XPEZ901","ochranný kryt – pre XPE-M",0]
["XPEY611","NOŽNÝ SPÍNAČ-2KROKOVÝ-ŽLTÝ S KRYTOM",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389119004190",{"v":28.4,"d":"28.40"},{"v":16.8,"d":"16.80"},{"v":17.2,"d":"17.20"},{"v":909,"d":"909.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEY611","samostatný nožný spínač – XPEY – s ochranným krytom – žltý – 2 NC + NO",0]
["XPEY511","NOŽNÝ SPÍNAČ ŽLTÝ S KRYTOM",1,"ks",109.809,"3389119004183",{"v":28.5,"d":"28.50"},{"v":16.5,"d":"16.50"},{"v":17.2,"d":"17.20"},{"v":905,"d":"905.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEY511","Jednonožový spínač - IP66 - s kryrtom - plastový - žltý - 2 NC + NO",0]
["XPEY510","NOŽ. SPÍNAČ ŽLTÝ NONC BLOK. S OCHR. KRYT",1,"ks",{"v":88.30473749999999,"d":"88.305"},"3389110221145",{"v":28.4,"d":"28.40"},{"v":16.8,"d":"16.80"},{"v":17.2,"d":"17.20"},{"v":700,"d":"700.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEY510","samostatný nožný spínač XPE-Y – s krytom – plastový – žltý – 1 NC + 1 NO",0]
["XPEY310","NOŽNÝ SPÍNAČ ŽLTÝ NO+NCS OCHR. KRYTOM",1,"ks",{"v":81.89921249999999,"d":"81.899"},"3389110221435",{"v":28.6,"d":"28.60"},{"v":16.6,"d":"16.60"},{"v":17,"d":"17.00"},{"v":690,"d":"690.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEY310","samostatný nožný spínač XPE-Y – s krytom – plastový – žltý – 1 NC + 1 NO",0]
["XPEY110","NOŽNÝ SPÍNAČ ŽLTÝ NO+NC",1,"ks",{"v":77.3238375,"d":"77.324"},"3389110221282",{"v":28.5,"d":"28.50"},{"v":8.5,"d":"8.50"},{"v":17,"d":"17.00"},{"v":700,"d":"700.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEY110","samostatný nožný spínač XPE-Y – bez krytu – plastový – žltý – 1 NC + 1 NO",0]
["XPER911","NOŽNÝ SPÍNAČ",1,"ks",{"v":301.97475,"d":"301.975"},"3389110147469",{"v":19.5,"d":"19.50"},{"v":16.2,"d":"16.20"},{"v":16.5,"d":"16.50"},{"v":1625,"d":"1,625.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER911","Single foot switch, Harmony XPE, metal, orange, without cover, trigger mechanism, 2 steps, 2 contacts 1NC+NO, IP66",0]
["XPER811","NOŽNÝ SPÍNAČ",1,"ks",{"v":205.891875,"d":"205.892"},"3389110147445",{"v":20,"d":"20.00"},{"v":16,"d":"16.00"},{"v":16.5,"d":"16.50"},{"v":2660,"d":"2,660.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER811","Jednonožový spínač - IP66 - bez krytu - kovový - oranžový - 2 NC + NO",0]
["XPER810","NOŽNÝ SPÍNAČ",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3389110147438",{"v":19.8,"d":"19.80"},{"v":17,"d":"17.00"},{"v":17,"d":"17.00"},{"v":1200,"d":"1,200.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER810","Single foot switch, Harmony XPE, metal, orange, without cover, trigger mechanism, 1 step, 1 contact 1NC+NO, IP66",0]
["XPER711","NOŽNÝ SPÍNAČ",1,"ks",{"v":233.344125,"d":"233.344"},"3389110471014",{"v":21,"d":"21.00"},{"v":16.6,"d":"16.60"},{"v":16.8,"d":"16.80"},{"v":2688,"d":"2,688.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER711","samostatný nožný spínač XPE-R – s krytom – kovový – oranžový – 2 NC + 2 NO",0]
["XPER611","NOŽNÝ SPÍNAČ",1,"ks",219.618,"3389110470994",{"v":16.5,"d":"16.50"},{"v":16.5,"d":"16.50"},{"v":19.5,"d":"19.50"},{"v":2420,"d":"2,420.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER611","samostatný nožný spínač XPE-R – s krytom – kovový – oranžový – 2 NC + 2 NO",0]
["XPER529","NOŽNÝ SPÍNAČ",1,"ks",{"v":562.771125,"d":"562.771"},"3389110470987",{"v":17.7,"d":"17.70"},{"v":15.1,"d":"15.10"},{"v":15.3,"d":"15.30"},{"v":2924,"d":"2,924.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPER529","samostatný nožný spínač XPE-R – s krytom – kovový – oranžový – 2 NC + 2 NO",0]
["XPER5110D","DVOJITÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":663.4293749999999,"d":"663.429"},"3389110094572",{"v":60,"d":"60.00"},{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":7469,"d":"7,469.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER5110D","dvojitý spínač - IP66 - s krytom - kov - oranžový - 4 1V + 4 1Z",0]
["XPER511","NOŽNÝ SPÍNAČ",1,"ks",{"v":228.76874999999998,"d":"228.769"},"3389110470970",{"v":19.6,"d":"19.60"},{"v":16,"d":"16.00"},{"v":17.2,"d":"17.20"},{"v":2639,"d":"2,639.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER511","samostatný nožný spínač XPE-R – s krytom – kovový – oranžový – 2 NC + 2 NO",0]
["XPER5100D","DVOJITÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":613.10025,"d":"613.100"},"3389110093353",{"v":60,"d":"60.00"},{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":7424,"d":"7,424.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER5100D","dvojitý nožný spínač XPE-R – s krytom – kovový – oranžový – 2 NC + 2 NO",0]
["XPER510","NOŽNÝ SPÍNAČ",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110470956",{"v":20,"d":"20.00"},{"v":16.5,"d":"16.50"},{"v":16.5,"d":"16.50"},{"v":2570,"d":"2,570.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER510","samostatný nožný spínač XPE-R – s krytom – kovový – oranžový – 1 NC + 1 NO",0]
["XPER410","NOŽNÝ SPÍNAČ",1,"ks",{"v":251.64562499999997,"d":"251.646"},"3389110470932",{"v":20,"d":"20.00"},{"v":16.3,"d":"16.30"},{"v":16.5,"d":"16.50"},{"v":2690,"d":"2,690.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER410","samostatný nožný sp. XPE-R – s ochranným krytom – kov. – oranžový – 1 NC + 1 NO",0]
["XPER3110D","DVOJITÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":471.26362499999993,"d":"471.264"},"3389110108750",{"v":60,"d":"60.00"},{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":8370,"d":"8,370.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER3110D","dvojitý nožný spínač XPE-R – s krytom – kovový – oranžový – 4 NC + 4 NO",0]
["XPER311","NOŽNÝ SPÍNAČ",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3389110470895",{"v":20,"d":"20.00"},{"v":16.4,"d":"16.40"},{"v":16.6,"d":"16.60"},{"v":2420,"d":"2,420.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER311","samostatný nožný spínač XPE-R – s krytom – kovový – oranžový – 2 NC +2 NO",0]
["XPER3100D","DVOJITÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":443.81137499999994,"d":"443.811"},"3389110094602",{"v":47,"d":"47.00"},{"v":18.5,"d":"18.50"},{"v":19.5,"d":"19.50"},{"v":5900,"d":"5,900.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER3100D","dvojitý nožný spínač XPE-R – s krytom – kovový – oranžový – 2 NC + 2 NO",0]
["XPER310","NOŽNÝ SPÍNAČ",1,"ks",{"v":160.138125,"d":"160.138"},"3389110470871",{"v":19.8,"d":"19.80"},{"v":16,"d":"16.00"},{"v":16.6,"d":"16.60"},{"v":2398,"d":"2,398.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER310","samostatný nožný spínač XPE-R – s krytom – kovový – oranžový – 1 NC + 1 NO",0]
["XPER229","NOŽNÝ SPÍNAČ",1,"ks",{"v":466.68825,"d":"466.688"},"3389110900064",{"v":23.3,"d":"23.30"},{"v":13.2,"d":"13.20"},{"v":8.8,"d":"8.80"},{"v":1514,"d":"1,514.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPER229","samostatný nožný spínač XPE-R – bez krytu – kovový – oranžový – 2 NC + 2 NO",0]
["XPER211","NOŽNÝ SPÍNAČ",1,"ks",{"v":155.56275,"d":"155.563"},"3389110470864",{"v":18.5,"d":"18.50"},{"v":8.5,"d":"8.50"},{"v":12,"d":"12.00"},{"v":1369,"d":"1,369.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER211","samostatný nožný spínač XPE-R – bez krytu – kovový – oranžový – 2 NC + 2 NO",0]
["XPER111","NOŽNÝ SPÍNAČ",1,"ks",{"v":141.836625,"d":"141.837"},"3389110470833",{"v":18.8,"d":"18.80"},{"v":8.8,"d":"8.80"},{"v":12.2,"d":"12.20"},{"v":1200,"d":"1,200.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER111","samostatný nožný spínač XPE-R – bez krytu – kovový – oranžový – 2 NC + 2 NO",0]
["XPER110","NOŽNÝ SPÍNAČ",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110470819",{"v":18.6,"d":"18.60"},{"v":7.4,"d":"7.40"},{"v":12,"d":"12.00"},{"v":1200,"d":"1,200.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPER110","samostatný nožný spínač XPE-R – bez krytu – kovový – oranžový – 1 NC + 1 NO",0]
["XPEM810","NOŽNÝ SPÍNAČ",1,"ks",{"v":187.59037499999997,"d":"187.590"},"3389110147391",{"v":19.5,"d":"19.50"},{"v":16.2,"d":"16.20"},{"v":16.5,"d":"16.50"},{"v":1547,"d":"1,547.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM810","Single foot switch, Harmony XPE, metal, blue, without cover, trigger mechanism, 1 step, 1 contact 1NC+NO, IP66",0]
["XPEM711","NOŽNÝ SPÍNAČ",1,"ks",{"v":233.344125,"d":"233.344"},"3389110650181",{"v":20,"d":"20.00"},{"v":20,"d":"20.00"},{"v":20,"d":"20.00"},{"v":2646,"d":"2,646.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM711","samostatný nožný spínač XPE-M – s krytom – kovový – modrý – 2 NC + 2 NO",0]
["XPEM611","NOŽNÝ SPÍNAČ",1,"ks",219.618,"3389110664638",{"v":20,"d":"20.00"},{"v":16,"d":"16.00"},{"v":17,"d":"17.00"},{"v":2420,"d":"2,420.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM611","samostatný nožný spínač XPE-M – s ochranným krytom – kov. – modrý – 2 NC + 2 NO",0]
["XPEM529","NOŽNÝ SPÍNAČ",1,"ks",{"v":562.771125,"d":"562.771"},"3389110147384",{"v":26,"d":"26.00"},{"v":15.5,"d":"15.50"},{"v":22,"d":"22.00"},{"v":3030,"d":"3,030.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEM529","samostatný nožný spínač XPE-M – s krytom – kovový – modrý – 2 NC + 2 NO",0]
["XPEM5110D","DVOJITÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":663.4293749999999,"d":"663.429"},"3389110093452",{"v":60,"d":"60.00"},{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":7444,"d":"7,444.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM5110D","dvojitý nožný spínač XPE-M – s krytom – kovový – modrý – 4 NC + 4NO",0]
["XPEM511","NOŽNÝ SPÍNAČ",1,"ks",{"v":224.193375,"d":"224.193"},"3389110650167",{"v":21.3,"d":"21.30"},{"v":20,"d":"20.00"},{"v":23,"d":"23.00"},{"v":2618,"d":"2,618.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM511","samostatný nožný spínač XPE-M – s krytom – kovový – modrý – 2 NC + 2 NO",0]
["XPEM5100D","DVOJITÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":613.10025,"d":"613.100"},"3389110092837",{"v":46.2,"d":"46.20"},{"v":18.6,"d":"18.60"},{"v":20.4,"d":"20.40"},{"v":6070,"d":"6,070.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM5100D","dvojitý nožný spínač XPE-M – s krytom – kovový – modrý – 2 NC + 2 NO",0]
["XPEM510","NOŽNÝ SPÍNAČ",1,"ks",{"v":169.288875,"d":"169.289"},"3389110650143",{"v":21.5,"d":"21.50"},{"v":21.2,"d":"21.20"},{"v":21.5,"d":"21.50"},{"v":2570,"d":"2,570.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM510","samostatný nožný spínač XPE-M – s krytom – kovový – modrý – 1 NC + 1 NO",0]
["XPEM410","NOŽNÝ SPÍNAČ",1,"ks",{"v":224.193375,"d":"224.193"},"3389110600384",{"v":20,"d":"20.00"},{"v":16.8,"d":"16.80"},{"v":16.8,"d":"16.80"},{"v":2610,"d":"2,610.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM410","samostatný nožný spínač XPE-M – s krytom – kovový – modrý – 1 NC + 1 NO",0]
["XPEM329","NOŽNÝ SPÍNAČ",1,"ks",{"v":544.469625,"d":"544.470"},"3389110147377",{"v":27,"d":"27.00"},{"v":16.5,"d":"16.50"},{"v":21.7,"d":"21.70"},{"v":2747,"d":"2,747.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEM329","samostatný nožný spínač XPE-M – s krytom – kovový – modrý – 2 NC + 2 NO",0]
["XPEM3110D","DVOJITÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":471.26362499999993,"d":"471.264"},"3389110094831",{"v":58.6,"d":"58.60"},{"v":30.4,"d":"30.40"},{"v":39.6,"d":"39.60"},{"v":7069,"d":"7,069.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM3110D","dvojitý nožný spínač XPE-M – s krytom – kovový – modrý – 4 NC + 4 NO",0]
["XPEM311","NOŽNÝ SPÍNAČ",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110600377",{"v":22,"d":"22.00"},{"v":22.1,"d":"22.10"},{"v":22,"d":"22.00"},{"v":2420,"d":"2,420.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM311","samostatný nožný spínač XPE-M – s krytom – kovový – modrý – 2 NC + 2 NO",0]
["XPEM3100D","DVOJITÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":443.81137499999994,"d":"443.811"},"3389110094589",{"v":47,"d":"47.00"},{"v":19,"d":"19.00"},{"v":19.5,"d":"19.50"},{"v":7060,"d":"7,060.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM3100D","dvojitý nožný spínač XPE-M – s krytom – kovový – modrý – 2 NC + 2 NO",0]
["XPEM310","NOŽNÝ SPÍNAČ",1,"ks",{"v":160.138125,"d":"160.138"},"3389110600360",{"v":16.8,"d":"16.80"},{"v":16.4,"d":"16.40"},{"v":20,"d":"20.00"},{"v":2400,"d":"2,400.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM310","samostatný nožný spínač XPE-M – s krytom – kovový – modrý – 1 NC + 1 NO",0]
["XPEM211EX","EX KOVOVÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":338.57775,"d":"338.578"},"3389118031203",{"v":20,"d":"20.00"},{"v":9,"d":"9.00"},{"v":17,"d":"17.00"},{"v":1.296,"d":"1.30"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEM211EX","Harmony XPE, Single foot switch, metal, blue, without cover, 2 steps, 2 contacts 1 NC+NO, protection against dust",0]
["XPEM211","NOŽNÝ SPÍNAČ",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3389110600353",{"v":18.5,"d":"18.50"},{"v":8.8,"d":"8.80"},{"v":12,"d":"12.00"},{"v":1360,"d":"1,360.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM211","samostatný nožný spínač XPE-M – bez krytu – kovový – modrý – 2 NC + 2 NO",0]
["XPEM129","NOŽNÝ SPÍNAČ",1,"ks",{"v":489.56512499999997,"d":"489.565"},"3389110600346",{"v":23.2,"d":"23.20"},{"v":9,"d":"9.00"},{"v":13.1,"d":"13.10"},{"v":1538,"d":"1,538.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEM129","Single foot switch, Harmony XPE, metal, blue, without cover, 1 step with analog output, 1 contact 2 NC+2 NO, IP66",0]
["XPEM111H2","NOŽNÝ SPÍNAČ",1,"ks",{"v":150.987375,"d":"150.987"},"3389118127760",{"v":12.3,"d":"12.30"},{"v":14.2,"d":"14.20"},{"v":21.5,"d":"21.50"},{"v":1220,"d":"1,220.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM111H2","Single foot switch, Harmony XPE, metal, blue, without cover, 1 step, 2 contacts 1NC+NO, IP66, CSA",0]
["XPEM111EX","EX KOVOVÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":301.97475,"d":"301.975"},"3389118031159",{"v":22,"d":"22.00"},{"v":9.5,"d":"9.50"},{"v":17.5,"d":"17.50"},{"v":1486,"d":"1,486.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEM111EX","Single foot switch, Harmony XPE, metal, blue, without cover, 1 step, 2 contacts 1NC+NO, protection against dust",0]
["XPEM111","NOŽNÝ SPÍNAČ",1,"ks",{"v":150.987375,"d":"150.987"},"3389110650129",{"v":18.8,"d":"18.80"},{"v":8.8,"d":"8.80"},{"v":12,"d":"12.00"},{"v":1338,"d":"1,338.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM111","samostatný nožný spínač XPE-M – bez krytu – kovový – modrý – 2 NC + 2 NO",0]
["XPEM110H2","NOŽNÝ SPÍNAČ",1,"ks",{"v":137.26125,"d":"137.261"},"3389118127777",{"v":12,"d":"12.00"},{"v":8.5,"d":"8.50"},{"v":18.5,"d":"18.50"},{"v":1378,"d":"1,378.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM110H2","Single foot switch, Harmony XPE, metal, blue, without cover, 1 step, 1 contact 1NC+NO, IP66, CSA",0]
["XPEM110EX","EX KOVOVÝ NOŽNÝ SPÍNAČ",1,"ks",{"v":269.94712499999997,"d":"269.947"},"3389118031142",{"v":21.5,"d":"21.50"},{"v":9.5,"d":"9.50"},{"v":17.5,"d":"17.50"},{"v":1460,"d":"1,460.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEM110EX","nožný sp. XPE-M – bez krytu – kov. – modrý – 1 NC + 1 NO – ochrana proti prachu",0]
["XPEM110","NOŽNÝ SPÍNAČ",1,"ks",109.809,"3389110650105",{"v":19,"d":"19.00"},{"v":9,"d":"9.00"},{"v":12,"d":"12.00"},{"v":1360,"d":"1,360.00"},"MA","8536508090","https://www.se.com/sk/sk/product/XPEM110","samostatný nožný spínač XPE-M – bez krytu – kovový – modrý – 1 NC + 1 NO",0]
["XPEG611","NOŽNÝ PLASTOVÝ SPÍNAČ ŠEDÝ",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110166415",{"v":28.5,"d":"28.50"},{"v":16.5,"d":"16.50"},{"v":17.4,"d":"17.40"},{"v":1018,"d":"1,018.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEG611","samostatný nožný spínač XPE-G – s krytom – plastový – sivý – 2 NC + 2 NO",0]
["XPEG510","NOŽNÝ PLASTOVÝ SPÍNAČ ŠEDÝ",1,"ks",{"v":90.59242499999999,"d":"90.592"},"3389110166330",{"v":17.2,"d":"17.20"},{"v":16.6,"d":"16.60"},{"v":28.6,"d":"28.60"},{"v":700,"d":"700.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEG510","samostatný nožný spínač XPE-G – s krytom – plastový – sivý – 1 NC + 1 NO",0]
["XPEG310","NOŽNÝ PLASTOVÝ SPÍNAČ ŠEDÝ",1,"ks",{"v":84.1869,"d":"84.187"},"3389110166361",{"v":28.6,"d":"28.60"},{"v":16.8,"d":"16.80"},{"v":17.2,"d":"17.20"},{"v":690,"d":"690.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEG310","samostatný nožný spínač XPE-G – s krytom – plastový – sivý – 1 NC + 1 NO",0]
["XPEG110","NOŽNÝ PLASTOVÝ SPÍNAČ ŠEDÝ",1,"ks",{"v":79.61152499999999,"d":"79.612"},"3389110166637",{"v":28.5,"d":"28.50"},{"v":11,"d":"11.00"},{"v":18,"d":"18.00"},{"v":795,"d":"795.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEG110","samostatný nožný spínač XPE-G – bez krytu – plastový – sivý – 1 NC + 1 NO",0]
["XPEB711","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110164770",{"v":28.6,"d":"28.60"},{"v":16.8,"d":"16.80"},{"v":17.2,"d":"17.20"},{"v":1014,"d":"1,014.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB711","samostatný nožný spínač XPE-B – s krytom – plastový – modrý – 2 NC + 2 NO",0]
["XPEB611","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110165647",{"v":28.4,"d":"28.40"},{"v":16.6,"d":"16.60"},{"v":17,"d":"17.00"},{"v":996,"d":"996.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB611","samostatný nožný spínač XPE-B – s krytom – plastový – modrý – 2 NC + 2 NO",0]
["XPEB511","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":100.65825,"d":"100.658"},"3389110158793",{"v":28.6,"d":"28.60"},{"v":16.8,"d":"16.80"},{"v":17.2,"d":"17.20"},{"v":992,"d":"992.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB511","samostatný nožný spínač XPE-B – s krytom – plastový – modrý – 2 NC + 2 NO",0]
["XPEB510","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":90.59242499999999,"d":"90.592"},"3389110157093",{"v":28.5,"d":"28.50"},{"v":17,"d":"17.00"},{"v":17.2,"d":"17.20"},{"v":973,"d":"973.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB510","samostatný nožný spínač XPE-B – s krytom – plastový – modrý – 1 NC + 1 NO",0]
["XPEB311","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":100.65825,"d":"100.658"},"3389110164794",{"v":28.5,"d":"28.50"},{"v":17,"d":"17.00"},{"v":17,"d":"17.00"},{"v":973,"d":"973.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB311","samostatný nožný spínač XPE-B – s krytom – plastový – modrý – 2 NC + 2 NO",0]
["XPEB310","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":84.1869,"d":"84.187"},"3389110164787",{"v":29,"d":"29.00"},{"v":18.5,"d":"18.50"},{"v":18.5,"d":"18.50"},{"v":962,"d":"962.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB310","samostatný nožný spínač XPE-B – s krytom – plastový – modrý – 1 NC + 1 NO",0]
["XPEB211","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389110214062",{"v":28.5,"d":"28.50"},{"v":8.5,"d":"8.50"},{"v":17,"d":"17.00"},{"v":841,"d":"841.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB211","samostatný nožný spínač XPE-B – bez krytu – plastový – modrý – 2 NC + 2 NO",0]
["XPEB111","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":90.59242499999999,"d":"90.592"},"3389110166323",{"v":28.5,"d":"28.50"},{"v":9,"d":"9.00"},{"v":17.2,"d":"17.20"},{"v":802,"d":"802.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB111","samostatný nožný spínač XPE-B – bez krytu – plastový – modrý – 2 NC + 2 NO",0]
["XPEB110","NOŽNÝ PLASTOVÝ SPÍNAČ MODRÝ",1,"ks",{"v":79.61152499999999,"d":"79.612"},"3389110165654",{"v":28.4,"d":"28.40"},{"v":8.6,"d":"8.60"},{"v":17.2,"d":"17.20"},{"v":817,"d":"817.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XPEB110","samostatný nožný spínač XPE-B – bez krytu – plastový – modrý – 1 NC + 1 NO",0]
["XPEA111","NOŽNÝ SPÍNAČ",1,"ks",{"v":65.4278625,"d":"65.428"},"3389110600339",{"v":18.7,"d":"18.70"},{"v":8.5,"d":"8.50"},{"v":12,"d":"12.00"},{"v":370,"d":"370.00"},"BR","8536508090","https://www.se.com/sk/sk/product/XPEA111","samostatný nožný sp. XPE-A – bez ochran. krytu – plast. – čierny – 2NC + 2NO",0]
["XPEA110","NOŽNÝ SPÍNAČ",1,"ks",{"v":56.734649999999995,"d":"56.735"},"3389110650006",{"v":18.9,"d":"18.90"},{"v":12.5,"d":"12.50"},{"v":9.4,"d":"9.40"},{"v":275,"d":"275.00"},"BR","8536508090","https://www.se.com/sk/sk/product/XPEA110","samostatný nožný spínač XPE-A – bez krytu – plastový – čierny – 1 NC + 1 NO",0]
["XESD2241","SPÍNACIA JEDNOTKA 2 TL. 1 RÝCHL.",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389110644029",{"v":10,"d":"10.00"},{"v":7.5,"d":"7.50"},{"v":7.5,"d":"7.50"},{"v":275,"d":"275.00"},"CZ","85389099","https://www.se.com/sk/sk/product/XESD2241","dotykový blok s vratnou pružinou – 3 NO + 1 NO – pred. montáž, 40 mm stredy",0]
["XESD2201","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389110644005",{"v":7.2,"d":"7.20"},{"v":9.2,"d":"9.20"},{"v":7.6,"d":"7.60"},{"v":260,"d":"260.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XESD2201","dotykový blok s vratnou pružinou – 3 NO– pred. montáž, 40 mm stredy",0]
["XESD1291","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":155.56275,"d":"155.563"},"3389110641127",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":188,"d":"188.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XESD1291","dotykový blok s vratnou pružinou – 2 NO + 1 OC – pred. montáž, 40 mm stredy",0]
["XESD1281","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":91.5075,"d":"91.508"},"3389110641103",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":185,"d":"185.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XESD1281","dotykový blok s vratnou pružinou – 1 OC + 1 NO – pred. montáž, 40 mm stredy",0]
["XESD1191","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110641080",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":158,"d":"158.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XESD1191","dotykový blok s vratnou pružinou – 2 NO – pred. montáž, 40 mm stredy",0]
["XESD1181","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":82.81428749999999,"d":"82.814"},"3389110641066",{"v":8.9,"d":"8.90"},{"v":7.1,"d":"7.10"},{"v":7.2,"d":"7.20"},{"v":156,"d":"156.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XESD1181","dotykový blok s vratnou pružinou – 1 OC – pred. montáž, 40 mm stredy",0]
["XESB2011","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110607987",{"v":8.6,"d":"8.60"},{"v":4.3,"d":"4.30"},{"v":6.4,"d":"6.40"},{"v":30,"d":"30.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XESB2011","dotykový blok s vratnou pružinou – 1 OC – pred. montáž, 40 mm stredy",0]
["XESB1011","SPÍNACIA JEDNOTKA VZ",1,"ks",{"v":21.5042625,"d":"21.504"},"3389110641042",{"v":10.3,"d":"10.30"},{"v":3.9,"d":"3.90"},{"v":5.2,"d":"5.20"},{"v":29,"d":"29.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XESB1011","prepínací kontakt",0]
["XENT2991","POLOHOVÝ SPÍNAČ",1,"ks",{"v":79.61152499999999,"d":"79.612"},"3389110470796",{"v":9.7,"d":"9.70"},{"v":3.8,"d":"3.80"},{"v":5.4,"d":"5.40"},{"v":40,"d":"40.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XENT2991","Harmony XAC-spínacia jednotka pre závesný ovládač XAC-koncový spínač-XEN-T",0]
["XENT1991","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":49.414049999999996,"d":"49.414"},"3389110609103",{"v":5.9,"d":"5.90"},{"v":3.6,"d":"3.60"},{"v":5.3,"d":"5.30"},{"v":42,"d":"42.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XENT1991","dotykový blok s vratnou pružinou – 3 NC – pred. montáž",0]
["XENT1192","BLOK KONTAKTOV",1,"ks",{"v":83.7293625,"d":"83.729"},"3389110426915",{"v":10.1,"d":"10.10"},{"v":3.6,"d":"3.60"},{"v":4.7,"d":"4.70"},{"v":67,"d":"67.00"},"FR","8538909999","https://www.se.com/sk/sk/product/XENT1192","samost. izolač. blok XEN-T – pre riadiaci obvod",0]
["XENG3791","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":35.687925,"d":"35.688"},"3389110645880",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":91,"d":"91.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XENG3791","blokovací dotykový blok – 1 NC + 1 NO – pred. montáž",0]
["XENG3781","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":35.687925,"d":"35.688"},"3389110645866",{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":4,"d":"4.00"},{"v":90,"d":"90.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XENG3781","blokovací dotykový blok – 2 NO – pred. montáž",0]
["XENG1491","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":30.655012499999998,"d":"30.655"},"3389110645712",{"v":5.5,"d":"5.50"},{"v":3,"d":"3.00"},{"v":3.5,"d":"3.50"},{"v":40,"d":"40.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENG1491","dotykový blok s vratnou pružinou – 1 NC + 2 NO – pred. montáž",0]
["XENG1191","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":29.282399999999996,"d":"29.282"},"3389110645705",{"v":5.5,"d":"5.50"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":40,"d":"40.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENG1191","dotykový blok s vratnou pružinou – 1 NC + 2 NO – pred. montáž",0]
["XEND2641","SPÍNACIA JEDNOTKA 2 TL. V+Z+Z OSTUPŇ.",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389110607802",{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},{"v":7,"d":"7.00"},{"v":110,"d":"110.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XEND2641","dotykový blok s vratnou pružinou – 1 OC + 1 NO – pred. montáž, 40 mm stredy",0]
["XEND2611","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":75.951225,"d":"75.951"},"3389110607772",{"v":7,"d":"7.00"},{"v":6,"d":"6.00"},{"v":6.5,"d":"6.50"},{"v":96,"d":"96.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XEND2611","dotykový blok s vratnou pružinou – 2 NO – pred. montáž, 40 mm stredy",0]
["XENC2151","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389110607727",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":28,"d":"28.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENC2151","dotykový blok – XENC – 1 NC + 1 NO",0]
["XENC2121","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":20.589187499999998,"d":"20.589"},"3389110607697",{"v":5.2,"d":"5.20"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":28,"d":"28.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENC2121","Contact block, Harmony XAC, single contact, spring return, single speed, front mounting, 1NC",0]
["XENC1151","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":25.6221,"d":"25.622"},"3389110643084",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":29,"d":"29.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENC1151","dotyk. blok s vr. pružinou – 1 NC + 1 NO – pred. montáž, 30 alebo 40 mm stredy",0]
["XENC1141","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":25.6221,"d":"25.622"},"3389110643060",{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":4,"d":"4.00"},{"v":28,"d":"28.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENC1141","dotykový blok s vratnou pružinou – 2 NC – pred. montáž, 30 alebo 40 mm stredy",0]
["XENC1131","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":25.6221,"d":"25.622"},"3389110643046",{"v":9.7,"d":"9.70"},{"v":3.4,"d":"3.40"},{"v":5.1,"d":"5.10"},{"v":29,"d":"29.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENC1131","dotykový blok s vratnou pružinou – 2 NO – pred. montáž, 30 alebo 40 mm stredy",0]
["XENC1121","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":19.674112499999996,"d":"19.674"},"3389110643022",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":3.5,"d":"3.50"},{"v":20,"d":"20.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENC1121","dotykový blok s vratnou pružinou – 1 NC – pred. montáž, 30 alebo 40 mm stredy",0]
["XENC1111","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":20.13165,"d":"20.132"},"3389110643008",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":3.5,"d":"3.50"},{"v":20,"d":"20.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENC1111","dotykový blok s vratnou pružinou – 1 NO – pred. montáž, 30 alebo 40 mm stredy",0]
["XENB1491","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":43.46606249999999,"d":"43.466"},"3389110607673",{"v":6.5,"d":"6.50"},{"v":3,"d":"3.00"},{"v":5,"d":"5.00"},{"v":54,"d":"54.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENB1491","dotyk. blok s vr. pružinou – 1 OC + 1 NO – pred. montáž, 30 alebo 40 mm stredy",0]
["XENB1191","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":44.838674999999995,"d":"44.839"},"3389110607666",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":5,"d":"5.00"},{"v":50,"d":"50.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENB1191","dotyk. blok s vr. pružinou – 1 OC + 1 NO – pred. montáž, 30 alebo 40 mm stredy",0]
["XENB1181","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110607659",{"v":7.5,"d":"7.50"},{"v":3.4,"d":"3.40"},{"v":9.7,"d":"9.70"},{"v":46,"d":"46.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XENB1181","dotykový blok s vratnou pružinou – 2 NO – pred. montáž",0]
["XEDS3231","SPÍNACIA JEDNOTKA PRE ZÁV. OVL. 2 RÝCHL.",1,"ks",{"v":228.76874999999998,"d":"228.769"},"3389110922073",{"v":9.1,"d":"9.10"},{"v":7,"d":"7.00"},{"v":7.2,"d":"7.20"},{"v":138,"d":"138.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEDS3231","spring return contact block - 2-pole - front mounting",0]
["XEDS3121","SPÍNACIA JEDNOTKA",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110922066",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":120,"d":"120.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEDS3121","dotykový blok s vratnou pružinou – 2-pól.– pred. montáž",0]
["XEDS3111","SPÍNACIA JEDNOTKA PRE ZÁV. OVL. 1 RÝCHL.",1,"ks",{"v":155.56275,"d":"155.563"},"3389110922059",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7.1,"d":"7.10"},{"v":111,"d":"111.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEDS3111","dotykový blok s vratnou pružinou – 2-pól.– pred. montáž",0]
["XEDS2231","SPÍNACIA JEDNOTKA PRE ZÁV. OVL. 2 RÝCHL.",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3389110310528",{"v":9.1,"d":"9.10"},{"v":7.1,"d":"7.10"},{"v":7.1,"d":"7.10"},{"v":139,"d":"139.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEDS2231","dotykový blok s vratnou pružinou – 2-pól.– pred. montáž",0]
["XEDS2121","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3389110922028",{"v":40,"d":"40.00"},{"v":15,"d":"15.00"},{"v":30,"d":"30.00"},{"v":90,"d":"90.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEDS2121","dotykový blok s vratnou pružinou – 2-pól.– pred. montáž",0]
["XEDS2111","SPÍNACIA JEDNOTKA PRE ZÁV. OVL. 1 RÝCHL.",1,"ks",{"v":141.836625,"d":"141.837"},"3389110922011",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":112,"d":"112.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEDS2111","spring return contact block - 2-pole - front mounting",0]
["XEDS1231","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110921991",{"v":9.1,"d":"9.10"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":122,"d":"122.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEDS1231","Contact block, Harmony XAC, double contact, spring return, 2-speed, snap action and staggered, 2NO",0]
["XEAC25361","SPÍNACIE JEDNOTKY PRE ZÁV. OVLÁDAČ",1,"ks",{"v":347.72849999999994,"d":"347.729"},"3389110661231",{"v":6.7,"d":"6.70"},{"v":4.3,"d":"4.30"},{"v":6.2,"d":"6.20"},{"v":98,"d":"98.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEAC25361","nekryté tlačidlo – pre riadiaci obvod – analóg. výstup – 0 - 15 V DC",0]
["XEAB25361","AKUSTICKÝ PRVOK",1,"ks",{"v":329.42699999999996,"d":"329.427"},"3389110655117",{"v":4,"d":"4.00"},{"v":6.6,"d":"6.60"},{"v":5.6,"d":"5.60"},{"v":65,"d":"65.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEAB25361","kryté tlačidlo – pre riadiaci obvod – analóg. výstup – 0 - 15 V DC",0]
["XEAB15361","TLAČIDLO S KONTAKTOM PRE XAC-B",1,"ks",{"v":320.27625,"d":"320.276"},"3389110655100",{"v":4,"d":"4.00"},{"v":6.2,"d":"6.20"},{"v":6.5,"d":"6.50"},{"v":65,"d":"65.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XEAB15361","kryté tlačidlo – pre riadiaci obvod – analóg. výstup – 0 - 15 V DC",0]
["XE2SP4151B","BLOK KONTAKTOV",1,"ks",{"v":17.386425,"d":"17.386"},"3389110418484",{"v":4.5,"d":"4.50"},{"v":2.5,"d":"2.50"},{"v":2.5,"d":"2.50"},{"v":20,"d":"20.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XE2SP4151B","kontaktný blok pre 2 krokový nožný spínač-1V+1Z",0]
["XE2SP4151","BLOK KONTAKTOV",1,"ks",{"v":12.81105,"d":"12.811"},"3389110415834",{"v":4,"d":"4.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":20,"d":"20.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XE2SP4151","okamihový dotyk. blok – pre 1 krokový alebo 2 krokový nožný sp. – 1 NC + 1 NO",0]
["XDRB14","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":237.9195,"d":"237.920"},"3389110606942",{"v":20.5,"d":"20.50"},{"v":8,"d":"8.00"},{"v":10.5,"d":"10.50"},{"v":1120,"d":"1,120.00"},"FR","85365080","https://www.se.com/sk/sk/product/XDRB14","Complete joystick controller, Harmony XD2, 30mm, 2 directions, 2C/O per direction, with spring return",0]
["XDAV11431","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":517.017375,"d":"517.017"},"3389110350050",{"v":15,"d":"15.00"},{"v":5.5,"d":"5.50"},{"v":9,"d":"9.00"},{"v":199,"d":"199.00"},"FR","85365011","https://www.se.com/sk/sk/product/XDAV11431","Pre cabled 2 axis joystick controller, Harmony XDA, analog omnidirectional with preferred 12...24 V DC",0]
["XDAV11131","ANALÓGOVÝ JOYSTICK",1,"ks",439.236,"3389110350036",{"v":15,"d":"15.00"},{"v":5.4,"d":"5.40"},{"v":8.6,"d":"8.60"},{"v":191,"d":"191.00"},"FR","85365011","https://www.se.com/sk/sk/product/XDAV11131","Pre cabled single axis joystick controller, Harmony XDA, analog 2 directions, 12...24 V DC",0]
["XDAV11122","ANALÓGOVÝ JOYSTICK",1,"ks",439.236,"3389110310306",{"v":15.3,"d":"15.30"},{"v":5.5,"d":"5.50"},{"v":8.8,"d":"8.80"},{"v":170,"d":"170.00"},"FR","85365011","https://www.se.com/sk/sk/product/XDAV11122","Pre cabled single axis joystick controller, Harmony XDA, analog 2 directions, 6...12 V DC",0]
["XDAL11431","ANALÓGOVÝ JOYSTICK",1,"ks",{"v":484.98975,"d":"484.990"},"3389110350029",{"v":5.4,"d":"5.40"},{"v":9,"d":"9.00"},{"v":15.2,"d":"15.20"},{"v":178,"d":"178.00"},"FR","8536501190","https://www.se.com/sk/sk/product/XDAL11431","Pre cabled 2 axis joystick controller, Harmony XDA, analog omnidirectional with preferred 12...24 V DC",0]
["XDAL11331","ANALÓGOVÝ JOYSTICK",1,"ks",{"v":484.98975,"d":"484.990"},"3389110350012",{"v":15.5,"d":"15.50"},{"v":5.5,"d":"5.50"},{"v":9,"d":"9.00"},{"v":150,"d":"150.00"},"FR","8536501190","https://www.se.com/sk/sk/product/XDAL11331","Pre cabled 2 axis joystick controller, Harmony XDA, analog omnidirectional, 12...24 V DC",0]
["XDAL11322","ANALÓGOVÝ JOYSTICK",1,"ks",{"v":484.98975,"d":"484.990"},"3389110310283",{"v":15.5,"d":"15.50"},{"v":5.2,"d":"5.20"},{"v":8.8,"d":"8.80"},{"v":150,"d":"150.00"},"FR","8536501190","https://www.se.com/sk/sk/product/XDAL11322","Pre cabled 2 axis joystick controller, Harmony XDA, analog omnidirectional, 6...12 V DC",0]
["XDAL11131","ANALOG JOYSTICK",1,"ks",{"v":443.81137499999994,"d":"443.811"},"3389110350005",{"v":15,"d":"15.00"},{"v":5.4,"d":"5.40"},{"v":8.8,"d":"8.80"},{"v":174,"d":"174.00"},"FR","8536501190","https://www.se.com/sk/sk/product/XDAL11131","Pre cabled single axis joystick controller, Harmony XDA, analog 2 directions, 12...24 V DC",0]
["XDAL11122","ANALÓGOVÝ JOYSTICK",1,"ks",{"v":443.81137499999994,"d":"443.811"},"3389110310276",{"v":15.5,"d":"15.50"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":150,"d":"150.00"},"FR","8536501190","https://www.se.com/sk/sk/product/XDAL11122","Pre cabled single axis joystick controller, Harmony XDA, analog 2 directions, 6...12 V DC",0]
["XD5PA24","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":76.40876249999998,"d":"76.409"},"3389110904307",{"v":12.5,"d":"12.50"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":77,"d":"77.00"},"FR","8538909999","https://www.se.com/sk/sk/product/XD5PA24","pákový ovládač Ø 22 – 5-polohová vratná pružina do polohy 0 – 1 NO",0]
["XD5PA22","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":59.479875,"d":"59.480"},"3389110904291",{"v":5.3,"d":"5.30"},{"v":12.8,"d":"12.80"},{"v":4.4,"d":"4.40"},{"v":64,"d":"64.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD5PA22","pákový ovládač Ø 22 – 3-polohová vratná pružina do polohy 0 – 1 NO",0]
["XD5PA14","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":74.57861249999999,"d":"74.579"},"3389110904284",{"v":13,"d":"13.00"},{"v":4.5,"d":"4.50"},{"v":5.4,"d":"5.40"},{"v":77,"d":"77.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD5PA14","pákový ovládač Ø 22 – 5-polohový usadený – 1 NO",0]
["XD5PA12","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":61.310024999999996,"d":"61.310"},"3389110904277",{"v":12.8,"d":"12.80"},{"v":4.4,"d":"4.40"},{"v":5.3,"d":"5.30"},{"v":64,"d":"64.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD5PA12","pákový ovládač Ø 22 – 3-polohový usadený – 1 NO",0]
["XD4PA247","Krížový ovládač - priemer 22 mm",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389110218695",{"v":4.8,"d":"4.80"},{"v":12.8,"d":"12.80"},{"v":3.4,"d":"3.40"},{"v":133,"d":"133.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD4PA247","krížový ovládač - priemer 22 mm",0]
["XD4PA24","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":86.01705,"d":"86.017"},"3389110887433",{"v":13,"d":"13.00"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":137,"d":"137.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD4PA24","4-smerový pákový ovládač – Ø 22 – 5 polôh, s vratnou pružinou",0]
["XD4PA22","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":70.0032375,"d":"70.003"},"3389110887419",{"v":12.5,"d":"12.50"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":116,"d":"116.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD4PA22","2-smerový pákový ovládač – Ø 22 – 3 polohy, s vratnou pružinou",0]
["XD4PA14","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":86.93212499999998,"d":"86.932"},"3389110887426",{"v":13,"d":"13.00"},{"v":5.4,"d":"5.40"},{"v":4.5,"d":"4.50"},{"v":133,"d":"133.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD4PA14","4-smerový pákový ovládač – Ø 22 – 5 polôh, usadený",0]
["XD4PA12","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":70.9183125,"d":"70.918"},"3389110887402",{"v":4.8,"d":"4.80"},{"v":12.8,"d":"12.80"},{"v":3.4,"d":"3.40"},{"v":122,"d":"122.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD4PA12","2-smerový pákový ovládač– Ø 22 – 3 polohy, usadený",0]
["XD4DA138","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":567.3465,"d":"567.347"},"3389110345605",{"v":20.5,"d":"20.50"},{"v":8.5,"d":"8.50"},{"v":10.5,"d":"10.50"},{"v":552,"d":"552.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD4DA138","Complete joystick controller, Harmony XDA, 30mm rotating actuator spring return  2NO + 2NO per direction",0]
["XD4CB08","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":590.2233749999999,"d":"590.223"},"3389110345483",{"v":20.5,"d":"20.50"},{"v":8,"d":"8.00"},{"v":10.5,"d":"10.50"},{"v":515,"d":"515.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD4CB08","Complete joystick controller, Harmony XDA, Ø 30 2 directions spring return 1 NO + 1NC per direction",0]
["XD4CB02","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":585.6479999999999,"d":"585.648"},"3389110345506",{"v":23,"d":"23.00"},{"v":13,"d":"13.00"},{"v":8.8,"d":"8.80"},{"v":513.5,"d":"513.50"},"FR","85365080","https://www.se.com/sk/sk/product/XD4CB02","Complete joystick controller, Harmony XDA, Ø 30 2 directions stay put 1 NO + 1NC per direction",0]
["XD4CA05","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":585.6479999999999,"d":"585.648"},"3389110345469",{"v":16.5,"d":"16.50"},{"v":9.5,"d":"9.50"},{"v":10,"d":"10.00"},{"v":492,"d":"492.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD4CA05","Complete joystick controller, Harmony XDA, Ø 30 2 directions stay put 1 NO + 1NC per direction",0]
["XD2PA247","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",109.809,"3389110607581",{"v":15,"d":"15.00"},{"v":3.3,"d":"3.30"},{"v":4.3,"d":"4.30"},{"v":145,"d":"145.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2PA247","krížový ovládač",0]
["XD2PA24","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110611625",{"v":14.8,"d":"14.80"},{"v":3.1,"d":"3.10"},{"v":4.2,"d":"4.20"},{"v":158,"d":"158.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2PA24","krížový ovládač - Ø22 - 4 smery - 1 NO na smer",0]
["XD2PA227","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":88.762275,"d":"88.762"},"3389110607574",{"v":15,"d":"15.00"},{"v":3.3,"d":"3.30"},{"v":4.3,"d":"4.30"},{"v":115,"d":"115.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2PA227","krížový ovládač - Ø22 - 2 smery - 1 NO na smer",0]
["XD2PA22","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":87.38966249999999,"d":"87.390"},"3389110611601",{"v":3.2,"d":"3.20"},{"v":4,"d":"4.00"},{"v":14.2,"d":"14.20"},{"v":115,"d":"115.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2PA22","krížový ovládač - Ø22 - 2 smery - 1 NO na smer",0]
["XD2PA14","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110611526",{"v":14.4,"d":"14.40"},{"v":3,"d":"3.00"},{"v":4.2,"d":"4.20"},{"v":158,"d":"158.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2PA14","krížový ovládač - Ø22 - 4 smery - 1 NO na smer",0]
["XD2PA12","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":86.4745875,"d":"86.475"},"3389110611502",{"v":3.8,"d":"3.80"},{"v":3,"d":"3.00"},{"v":14.4,"d":"14.40"},{"v":115,"d":"115.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2PA12","krížový ovládač - Ø22 - 2 smery - 1 NO na smer",0]
["XD2LC21","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":631.40175,"d":"631.402"},"3389110633856",{"v":18,"d":"18.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":350,"d":"350.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2LC21","krížový ovládač - Ø30 - 2 smery - 2 NC na smer",0]
["XD2HL3333","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":690.881625,"d":"690.882"},"3389110607536",{"v":16.5,"d":"16.50"},{"v":11.5,"d":"11.50"},{"v":11,"d":"11.00"},{"v":468,"d":"468.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2HL3333","krížový ovládač - Ø30 - 4 smery - 2 NO na smer",0]
["XD2HL1111","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":690.881625,"d":"690.882"},"3389110607529",{"v":16.5,"d":"16.50"},{"v":11,"d":"11.00"},{"v":11.5,"d":"11.50"},{"v":488,"d":"488.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2HL1111","complete joystick controller - Ø30 - 4 directions - 2 NO per direction",0]
["XD2HL1010","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":690.881625,"d":"690.882"},"3389110310511",{"v":16.5,"d":"16.50"},{"v":11.5,"d":"11.50"},{"v":10.5,"d":"10.50"},{"v":381,"d":"381.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2HL1010","Complete joystick controller, Harmony XD2, 30mm, 2 directions, 2NO per direction",0]
["XD2GA8451","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3389110611472",{"v":15,"d":"15.00"},{"v":9,"d":"9.00"},{"v":9.5,"d":"9.50"},{"v":550,"d":"550.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8451","Complete joystick controller, Harmony XB5, Ø22 mm 4 directions 2 NO per direction",0]
["XD2GA84417","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":228.76874999999998,"d":"228.769"},"3389110607512",{"v":14.5,"d":"14.50"},{"v":9.1,"d":"9.10"},{"v":9.2,"d":"9.20"},{"v":550,"d":"550.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA84417","krížový ovládač - priemer 22 mm",0]
["XD2GA8441","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":205.891875,"d":"205.892"},"3389110611458",{"v":14.2,"d":"14.20"},{"v":9.2,"d":"9.20"},{"v":9.4,"d":"9.40"},{"v":550,"d":"550.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8441","krížový ovládač - priemer 22 mm",0]
["XD2GA8431","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3389110607499",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":570,"d":"570.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8431","krížový ovládač - priemer 22 mm",0]
["XD2GA84217","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":141.836625,"d":"141.837"},"3389110664164",{"v":9.4,"d":"9.40"},{"v":9.2,"d":"9.20"},{"v":15,"d":"15.00"},{"v":330,"d":"330.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA84217","krížový ovládač - priemer 22 mm",0]
["XD2GA8421","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":118.95975,"d":"118.960"},"3389110611465",{"v":14.5,"d":"14.50"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":330,"d":"330.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8421","krížový ovládač - priemer 22 mm",0]
["XD2GA8411","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110611441",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":330,"d":"330.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8411","krížový ovládač Ø22",0]
["XD2GA8251","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":141.836625,"d":"141.837"},"3389110611434",{"v":15,"d":"15.00"},{"v":9,"d":"9.00"},{"v":9.5,"d":"9.50"},{"v":453,"d":"453.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8251","Complete joystick controller, Harmony XB5, Ø22 mm 2 directions 2 NO per direction",0]
["XD2GA82417","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":150.987375,"d":"150.987"},"3389110607444",{"v":14.8,"d":"14.80"},{"v":9,"d":"9.00"},{"v":9.4,"d":"9.40"},{"v":455,"d":"455.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2GA82417","krížový ovládač - priemer 22 mm",0]
["XD2GA8241","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389110611410",{"v":14.5,"d":"14.50"},{"v":9.2,"d":"9.20"},{"v":9.2,"d":"9.20"},{"v":452,"d":"452.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8241","krížový ovládač - priemer 22 mm",0]
["XD2GA8231","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":141.836625,"d":"141.837"},"3389110607420",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":446,"d":"446.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8231","Complete joystick controller, Harmony XB5, Ø22 mm 2 directions 2 NO per direction",0]
["XD2GA82217","KRÍŽOVÝ OVLÁDAČ",1,"ks",109.809,"3389110607413",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":300,"d":"300.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2GA82217","Complete joystick controller, Harmony XB5, Ø22 mm 2 directions 1 NO per direction",0]
["XD2GA8221","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389110611427",{"v":14.8,"d":"14.80"},{"v":9.2,"d":"9.20"},{"v":9.6,"d":"9.60"},{"v":366,"d":"366.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8221","krížový ovládač - priemer 22 mm",0]
["XD2GA8211","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389110611403",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":366,"d":"366.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA8211","krížový ovládač - priemer 22 mm",0]
["XD2GA419448","KRÍŽOVÝ OVLÁDAČ",1,"ks",183.015,"3389118164710",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":342,"d":"342.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2GA419448","Krížová ovládač",""]
["XD2EL1111H2","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389118381094",{"v":40,"d":"40.00"},{"v":15,"d":"15.00"},{"v":30,"d":"30.00"},{"v":350,"d":"350.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2EL1111H2","complete joystick controller - Ø30 - 8 directions - 1 or 2 C/O per direction",0]
["XD2EL1111","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389110317121",{"v":16.6,"d":"16.60"},{"v":9.6,"d":"9.60"},{"v":10,"d":"10.00"},{"v":358,"d":"358.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2EL1111","krížový ovládač - priemer 30 mm",0]
["XD2EC3333","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389110663259",{"v":16.5,"d":"16.50"},{"v":9.8,"d":"9.80"},{"v":9.8,"d":"9.80"},{"v":353,"d":"353.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2EC3333","krížový ovládač - priemer 30 mm",0]
["XD2EC1111H2","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389118381117",{"v":40,"d":"40.00"},{"v":15,"d":"15.00"},{"v":30,"d":"30.00"},{"v":350,"d":"350.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2EC1111H2","JOYSTICK 600VAC 10AMP 22MM XD2 +OPTIONS",0]
["XD2EC1111","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389110316483",{"v":18,"d":"18.00"},{"v":9.4,"d":"9.40"},{"v":9.8,"d":"9.80"},{"v":300,"d":"300.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2EC1111","krížový ovládač - priemer 30 mm",0]
["XD2CL3030","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389110317602",{"v":16.5,"d":"16.50"},{"v":9.6,"d":"9.60"},{"v":9.6,"d":"9.60"},{"v":296,"d":"296.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CL3030","complete joystick controller - Ø30 - 2 directions - 1 C/O per direction",0]
["XD2CL1111","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":137.26125,"d":"137.261"},"3389110317589",{"v":9.8,"d":"9.80"},{"v":9.8,"d":"9.80"},{"v":16.6,"d":"16.60"},{"v":362,"d":"362.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CL1111","krížový ovládač",0]
["XD2CL1010","KRÍŽOVÝ OVLÁDAČ 30,5MM",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389110317565",{"v":16.5,"d":"16.50"},{"v":9.8,"d":"9.80"},{"v":10,"d":"10.00"},{"v":296,"d":"296.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CL1010","complete joystick controller - Ø30 - 2 directions - 1 C/O per direction",0]
["XD2CG1111","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":777.8137499999999,"d":"777.814"},"3606486925799",{"v":18.5,"d":"18.50"},{"v":13,"d":"13.00"},{"v":12.5,"d":"12.50"},{"v":509,"d":"509.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CG1111","complete joystick controller - Ø30 - 4 directions - 2 NO + 1 NC per direction",0]
["XD2CD3333","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389110607192",{"v":16.5,"d":"16.50"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":369,"d":"369.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CD3333","krížový ovládač",0]
["XD2CD3113","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":228.76874999999998,"d":"228.769"},"3389110607185",{"v":16.5,"d":"16.50"},{"v":9.5,"d":"9.50"},{"v":10,"d":"10.00"},{"v":367,"d":"367.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2CD3113","XD2-C Ø30 joystick controller",0]
["XD2CD3030","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":160.138125,"d":"160.138"},"3389110345407",{"v":16.5,"d":"16.50"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":300,"d":"300.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CD3030","complete joystick controller - Ø30 - 2 directions - 1 C/O per direction",0]
["XD2CD1111","KRÍŽOVÝ OVLÁDAČ 30MM",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389110326444",{"v":16.5,"d":"16.50"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":335,"d":"335.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CD1111","krížový ovládač",0]
["XD2CD1010","KRÍŽOVÝ OVLÁDAČ 30MM",1,"ks",{"v":160.138125,"d":"160.138"},"3389110345384",{"v":16.5,"d":"16.50"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":303,"d":"303.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CD1010","krížový ovládač",0]
["XD2CC3333","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":137.26125,"d":"137.261"},"3389110317541",{"v":16.7,"d":"16.70"},{"v":9.8,"d":"9.80"},{"v":9.8,"d":"9.80"},{"v":348,"d":"348.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2CC3333","krížový ovládač",0]
["XD2CC3330","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":155.56275,"d":"155.563"},"3389118318397",{"v":16.5,"d":"16.50"},{"v":9.5,"d":"9.50"},{"v":10,"d":"10.00"},{"v":315,"d":"315.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2CC3330","complete joystick controller - Ø30 - 3 directions - 1 C/O per direction",0]
["XD2CC3030","KRÍŽOVÝ OVLÁDAC 22MM",1,"ks",{"v":118.95975,"d":"118.960"},"3389110317527",{"v":16.5,"d":"16.50"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":292,"d":"292.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2CC3030","krížový ovládač",0]
["XD2CC1111H2","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389118381452",{"v":40,"d":"40.00"},{"v":15,"d":"15.00"},{"v":30,"d":"30.00"},{"v":350,"d":"350.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2CC1111H2","Complete joystick controller, Harmony XD2, 30mm, 4 directions, 1 C/O per direction, with spring return",0]
["XD2CC1111","KRÍŽOVÝ OVLÁDAČ 30MM",1,"ks",{"v":137.26125,"d":"137.261"},"3389110317503",{"v":17,"d":"17.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":300,"d":"300.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2CC1111","krížový ovládač",0]
["XD2CC1101","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":155.56275,"d":"155.563"},"3389110661217",{"v":16.5,"d":"16.50"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":325,"d":"325.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2CC1101","Complete joystick controller, Harmony XD2, 30mm, 4 directions, 1 C/O per direction",0]
["XD2CC1010","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389110317466",{"v":16.5,"d":"16.50"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":292,"d":"292.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2CC1010","complete joystick controller - Ø30 - 2 directions - 1 C/O per direction",0]
["XD2AL221","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":155.56275,"d":"155.563"},"3389110348743",{"v":17.5,"d":"17.50"},{"v":8.5,"d":"8.50"},{"v":8.5,"d":"8.50"},{"v":273,"d":"273.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2AL221","complete joystick controller - Ø30 - 2 directions - 1 C/O per direction",0]
["XD2AL201","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":155.56275,"d":"155.563"},"3389110348705",{"v":17.5,"d":"17.50"},{"v":8.5,"d":"8.50"},{"v":8.5,"d":"8.50"},{"v":272,"d":"272.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2AL201","krížový ovládač - priemer 30 mm",0]
["XD2AC231","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":155.56275,"d":"155.563"},"3389110661200",{"v":12,"d":"12.00"},{"v":6,"d":"6.00"},{"v":7.5,"d":"7.50"},{"v":238.5,"d":"238.50"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2AC231","krížový ovládač - priemer 30 mm",0]
["XD2AC222","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":224.193375,"d":"224.193"},"3389110348682",{"v":17.5,"d":"17.50"},{"v":8.5,"d":"8.50"},{"v":8.5,"d":"8.50"},{"v":346.5,"d":"346.50"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2AC222","Complete joystick controller, Harmony XD2, 30mm, 2 directions, 2 C/O  per direction, with return position 0",0]
["XD2AC221H2","KRÍŽOVÝ OVLÁDAČ",1,"ks",183.015,"3389118381551",{"v":40,"d":"40.00"},{"v":15,"d":"15.00"},{"v":30,"d":"30.00"},{"v":350,"d":"350.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2AC221H2","22MM JOYSTICK 600VAC 10AMP",0]
["XD2AC2219H2","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":201.3165,"d":"201.317"},"3389110606966",{"v":12,"d":"12.00"},{"v":6,"d":"6.00"},{"v":7.3,"d":"7.30"},{"v":220,"d":"220.00"},"FR","85365080","https://www.se.com/sk/sk/product/XD2AC2219H2","Complete joystick controller, Harmony XD2, 30mm, 2 directions, 1 C/O  per direction, with return position 0/spring return",0]
["XD2AC221","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":155.56275,"d":"155.563"},"3389110348668",{"v":12,"d":"12.00"},{"v":6,"d":"6.00"},{"v":7,"d":"7.00"},{"v":243,"d":"243.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2AC221","krížový ovládač - priemer 30 mm",0]
["XD2AC202","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":224.193375,"d":"224.193"},"3389110348644",{"v":17.5,"d":"17.50"},{"v":8.5,"d":"8.50"},{"v":8.5,"d":"8.50"},{"v":344,"d":"344.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2AC202","Complete joystick controller, Harmony XD2, 30mm, 2 directions, 2 C/O per direction, without return",0]
["XD2AC201H2","KRÍŽOVÝ OVLÁDAČ",1,"ks",183.015,"3389118381575",{"v":11.938,"d":"11.94"},6.35,7.62,{"v":240.406,"d":"240.41"},"FR","85365080","https://www.se.com/sk/sk/product/XD2AC201H2","complete joystick controller - Ø30 - 2 directions - 1 C/O per direction",0]
["XD2AC2019H2","KRÍŽOVÝ OVLÁDAČ",1,"ks",{"v":201.3165,"d":"201.317"},"3389110606959",{"v":12,"d":"12.00"},{"v":5.8,"d":"5.80"},{"v":7.3,"d":"7.30"},{"v":258.5,"d":"258.50"},"FR","85365080","https://www.se.com/sk/sk/product/XD2AC2019H2","krížový ovládač - Ø30 - 2 smery - 1 C/O na smer",0]
["XD2AC201","KRÍŽOVÝ OVLÁDAČ 22MM",1,"ks",{"v":155.56275,"d":"155.563"},"3389110348620",{"v":12.2,"d":"12.20"},{"v":6,"d":"6.00"},{"v":6.6,"d":"6.60"},{"v":242,"d":"242.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XD2AC201","krížový ovládač - priemer 30 mm",0]
["XBTZGUSB","KÁBEL PRE USB VZDIALENÉ PRIPOJENIE",1,"ks",{"v":63.6174,"d":"63.617"},"3595863885507",{"v":12,"d":"12.00"},{"v":5,"d":"5.00"},{"v":22,"d":"22.00"},{"v":120,"d":"120.00"},"TW","8544429090","https://www.se.com/sk/sk/product/XBTZGUSB","rozšírenie USB typ A port - 1 m",0]
["XBTZGUMP","BRÁNA MODBUSPLUS PRE XBTGT/GK",1,"ks",1708.245,"3595863936346",{"v":30,"d":"30.00"},{"v":9.5,"d":"9.50"},{"v":21.5,"d":"21.50"},{"v":647,"d":"647.00"},"FR","8517620000","https://www.se.com/sk/sk/product/XBTZGUMP","Magelis XBT-USB gateway-pre XBTGK - XBTGT terminal-Modbus Plus bus",0]
["XBTZGPEN","DOTYKOVÉ PERO PRE XBT GH",1,"ks",{"v":51.24734999999999,"d":"51.247"},"3595864003375",{"v":12,"d":"12.00"},{"v":1,"d":"1.00"},{"v":10.5,"d":"10.50"},{"v":22,"d":"22.00"},"JP","3926909790","https://www.se.com/sk/sk/product/XBTZGPEN","stylus pre dotykový panel - Magelis XBTGH - pokročilý ruční panel",0]
["XBTZGJBOX","PREPOJOVACÍ ZDRUŽOVACÍ MODUL",1,"ks",553.707,"3595864003191",{"v":27.5,"d":"27.50"},{"v":16.3,"d":"16.30"},{"v":21.6,"d":"21.60"},{"v":1172,"d":"1,172.00"},"JP","8536909500","https://www.se.com/sk/sk/product/XBTZGJBOX","pripojovací a združovací modul napájania a zbernice (RS232/485, Ethernet)",0]
["XBTZGHL10","PREPOJOVACÍ KÁBEL 10M PRE XBT GH",1,"ks",{"v":647.9549999999999,"d":"647.955"},"3595864003313",30.48,{"v":5.842,"d":"5.84"},{"v":23.368,"d":"23.37"},{"v":2000,"d":"2,000.00"},"JP","8544429090","https://www.se.com/sk/sk/product/XBTZGHL10","kábel rozhranný - L = 10 m - medzi rozšír. ručný panel a prepoj.box",0]
["XBTZGCO4","REDUKCIA OTVORU Z XBTG53XX NA XBTGT53XX",1,"ks",176.715,"3595863885682",{"v":30,"d":"30.00"},{"v":9,"d":"9.00"},{"v":42,"d":"42.00"},{"v":759,"d":"759.00"},"JP","7326909890","https://www.se.com/sk/sk/product/XBTZGCO4","Magelis XBT-redukčný rámček pre panely XBTG5330 na XBTGT 5330.",0]
["XBTZGCO3","REDUKCIA OTVORU Z XBTF034 NA XBTGT53XX.",1,"ks",200.277,"3595863885675",{"v":30,"d":"30.00"},{"v":14.5,"d":"14.50"},{"v":50,"d":"50.00"},{"v":616,"d":"616.00"},"JP","7326909890","https://www.se.com/sk/sk/product/XBTZGCO3","Magelis XBT-redukčný rámček pre panely XBTF034 na XBTGT 53x0.",0]
["XBTZGCO1","REDUKCIA OTVORU Z XBTF032XXX NA XBTGT200",1,"ks",{"v":206.1675,"d":"206.168"},"3595863885651",{"v":16,"d":"16.00"},{"v":8.5,"d":"8.50"},{"v":22,"d":"22.00"},{"v":350,"d":"350.00"},"JP","7326909890","https://www.se.com/sk/sk/product/XBTZGCO1","Magelis XBT-redukčný rámček pre panely XBTF032.10 na XBTGT2..0",0]
["XBTZG9721","KÁBEL PRE SPOJENIE S SIEMENS PPI",1,"ks",{"v":63.6174,"d":"63.617"},"3595863885538",{"v":15,"d":"15.00"},{"v":1.5,"d":"1.50"},{"v":14,"d":"14.00"},{"v":116,"d":"116.00"},"CN","8544429090","https://www.se.com/sk/sk/product/XBTZG9721","Magelis XBT - prepojovací kábel pre XBTGk - XBTGT - XBTGR - 2.5 m",0]
["XBTZG939","KÁBLOVÝ ADAPTÉR RJ45 K XBT GT1000",1,"ks",{"v":19.43865,"d":"19.439"},"3595863885460",{"v":19.2,"d":"19.20"},{"v":1.5,"d":"1.50"},{"v":5.6,"d":"5.60"},{"v":55,"d":"55.00"},"CN","8544429090","https://www.se.com/sk/sk/product/XBTZG939","Magelis XBT-káblový adaptér (SubD25-RJ45) pre RS485 k XBT GT",0]
["XBTZG935","KÁBEL PRE DOWNLOAD KONFIGURÁCIE CEZ USB",1,"ks",247.401,"3595863885705",{"v":15,"d":"15.00"},{"v":2.5,"d":"2.50"},{"v":15,"d":"15.00"},{"v":197,"d":"197.00"},"ZZ","8544429090","https://www.se.com/sk/sk/product/XBTZG935","programovací prepojovací kábel PC - 2 m",0]
["XBTZG66","OCHRANNÁ FÓLIA PRE RADU XBGT 5XXX, 5KS",1,"ks",129.591,"3595863885385",{"v":23,"d":"23.00"},{"v":0.1,"d":"0.10"},{"v":31,"d":"31.00"},{"v":183,"d":"183.00"},"JP","3926909790","https://www.se.com/sk/sk/product/XBTZG66","ochranná fólia pre radu XBTGT63x0/5230 - sada 5",0]
["XBTZG65","OCHRANNÁ FÓLIA PRE RADU XBTGT53XX, 5 KS",1,"ks",{"v":95.4261,"d":"95.426"},"3595863885392",{"v":20.5,"d":"20.50"},{"v":0.3,"d":"0.30"},{"v":26,"d":"26.00"},{"v":150,"d":"150.00"},"JP","3926909790","https://www.se.com/sk/sk/product/XBTZG65","ochranná fólia pre radu XBTGT53x0/XBTGT54x0 - sada 5",0]
["XBTZG62","OCHRANNÁ FÓLIA PRE XBT GT2000, 5KS",1,"ks",{"v":63.028349999999996,"d":"63.028"},"3595863885415",{"v":13,"d":"13.00"},{"v":0.3,"d":"0.30"},{"v":18.5,"d":"18.50"},{"v":10,"d":"10.00"},"JP","3926909790","https://www.se.com/sk/sk/product/XBTZG62","ochranná fólia pre radu XBTGT21x0/2220/2x30 - sada 5",0]
["XBTZ9982","PREP.KÁBEL OP(RJ45)-MODIC.M340(RJ45),10M",1,"ks",{"v":68.91885,"d":"68.919"},"3595864000053",{"v":19,"d":"19.00"},{"v":3.5,"d":"3.50"},{"v":17.5,"d":"17.50"},{"v":362,"d":"362.00"},"CN","8544429090","https://www.se.com/sk/sk/product/XBTZ9982","prepojovací kábel XBT N/R GT/GK/GH a HMI STO/STU Modicon M238, M258, M340 - 10m",0.04]
["XBTZ9980","PREP. KÁBEL MEDZI M340 A XBTNX00,XBTRX00",1,"ks",{"v":35.93205,"d":"35.932"},"3389118316508",{"v":18.6,"d":"18.60"},{"v":2.4,"d":"2.40"},{"v":17.5,"d":"17.50"},{"v":93,"d":"93.00"},"ID","8544429090","https://www.se.com/sk/sk/product/XBTZ9980","prep.kábel XBT N/R - GT/GK/GH a HMI STO/STU-Modicon M238, M258, M340 , 2,5m",0]
["XBTZ9782","PREP.KÁBEL OP(RJ45) - PLC(MINI DIN), 10M",1,"ks",{"v":68.91885,"d":"68.919"},"3595864000046",{"v":19,"d":"19.00"},{"v":3,"d":"3.00"},{"v":19,"d":"19.00"},{"v":320,"d":"320.00"},"CN","8544429090","https://www.se.com/sk/sk/product/XBTZ9782","Uni-Telway/Modbus prepojovací kábel - L = 10 m - 1 samice mini DIN + 1 RJ45",0]
["XBTZ9780","PREP.KÁBEL OP XBT S RJ45 - PLC(MINI DIN)",1,"ks",{"v":40.0554,"d":"40.055"},"3389119003582",{"v":14.2,"d":"14.20"},{"v":1.8,"d":"1.80"},{"v":16.5,"d":"16.50"},{"v":114,"d":"114.00"},"FR","8544429090","https://www.se.com/sk/sk/product/XBTZ9780","Uni-Telway/Modbus prepojovací kábel - L = 2.5 m - 1 samice mini DIN + 1 RJ45",0]
["XBTZ9733","PREP.KÁBEL OP(RJ45)-DF1 ROCKWELL(MINIDIN",1,"ks",{"v":65.38455,"d":"65.385"},"3595864000077",{"v":20,"d":"20.00"},{"v":2,"d":"2.00"},{"v":20,"d":"20.00"},{"v":97,"d":"97.00"},"CN","8544429090","https://www.se.com/sk/sk/product/XBTZ9733","prepojovací kábel - L = 2.5 m - 1 Micro-logix 1000 - DF1",0]
["XBTZ915","PROGR. KÁBEL OP(SUB D25) - PC(SUB D9)",1,"ks",{"v":98.37134999999999,"d":"98.371"},"3389110633535",{"v":18,"d":"18.00"},{"v":3,"d":"3.00"},{"v":15,"d":"15.00"},{"v":200,"d":"200.00"},"FR","8544429090","https://www.se.com/sk/sk/product/XBTZ915","Magelis XBT-prepojovací kábel OP.-PC RS 232 univ.pre prog.-ser.tlačiareň.-2.5m",0]
["XBTZ9008","MAGELIS XBT-OT MODBUS KABEL SUB-D9/RJ45",1,"ks",{"v":47.71305,"d":"47.713"},"3595863961706",{"v":15,"d":"15.00"},{"v":2,"d":"2.00"},{"v":15,"d":"15.00"},{"v":125,"d":"125.00"},"CN","8544429090","https://www.se.com/sk/sk/product/XBTZ9008","prepoj.kábel XBT k Modbus zariadeniam SubD9 a Modicon M238, M258, M340 2,5m",0]
["XBH1AA0R4","Displej Harmony",1,"ks",{"v":118.95975,"d":"118.960"},"3606489737221",{"v":13,"d":"13.00"},{"v":4,"d":"4.00"},{"v":8.5,"d":"8.50"},{"v":67,"d":"67.00"},"CZ","9030337000","https://www.se.com/sk/sk/product/XBH1AA0R4","Display module, Harmony XB5, Digital panel meter, plastic, black, 22mm, 4 digit red LED display, 4...20mA input",0.01]
["XBH1AA0G4","Displej Harmony",1,"ks",{"v":118.95975,"d":"118.960"},"3606489737214",{"v":12.9,"d":"12.90"},{"v":3.9,"d":"3.90"},{"v":8.3,"d":"8.30"},{"v":67,"d":"67.00"},"CZ","9030337000","https://www.se.com/sk/sk/product/XBH1AA0G4","Display module, Harmony XB5, Digital panel meter, plastic, black, 22mm, 4 digit green LED display, 4...20mA input",0.01]
["XBFX13","PRÍPRAVOK NA DEMONTÁŽ ŽIAROVIEK",1,"ks",{"v":6.63429375,"d":"6.634"},"3389110341966",{"v":6,"d":"6.00"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":4,"d":"4.00"},"FR","8205598000","https://www.se.com/sk/sk/product/XBFX13","vyťahovač žiaroviek pre Ø 22 a 30 mm jednotky",0]
["XB7NW34B1","Ovl. hl. Harmony XB7, plast, červená, 1Z",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3606480470790",{"v":3.2,"d":"3.20"},{"v":6,"d":"6.00"},{"v":3.2,"d":"3.20"},{"v":23,"d":"23.00"},"ID","8536508090","https://www.se.com/sk/sk/product/XB7NW34B1","Ovládacia hlavica Harmony XB7, plastová, presvetlená, červená, 1Z, 24V",0]
["XB7NS9444","Ovládač núdzového zastavenia",10,"ks",{"v":26.994712499999995,"d":"26.995"},"3606480465642",{"v":8,"d":"8.00"},{"v":15,"d":"15.00"},{"v":16,"d":"16.00"},{"v":35,"d":"35.00"},"ID","8536508090","https://www.se.com/sk/sk/product/XB7NS9444","Monolithic emergency stop, Harmony XB7, plastic, red mushroom 40mm, 22mm, latching key release, 2NC",0]
["XB7NG21","OVL.HLAVICA S KĽÚČOM",10,"ks",{"v":18.301499999999997,"d":"18.302"},"3606480470271",{"v":3.3,"d":"3.30"},{"v":3.3,"d":"3.30"},{"v":6.1,"d":"6.10"},{"v":50,"d":"50.00"},"ID","8536508090","https://www.se.com/sk/sk/product/XB7NG21","Monolithic key switch selector, Harmony XB7, plastic, black, 22mm, key 455, 2 positions, stay put, 1NO",0]
["XB7NA45","Tlačítko, Červené, NO+NC",10,"ks",{"v":13.2685875,"d":"13.269"},"3606480470172",{"v":3,"d":"3.00"},{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":21,"d":"21.00"},"ID","8536508090","https://www.se.com/sk/sk/product/XB7NA45","Monolithic push button, Harmony XB7, plastic, red, 22mm, spring return, unmarked, 1NO+1NC",0]
["XB7NA35","Olávač stláčacie, zelený",10,"ks",{"v":12.353512499999999,"d":"12.354"},"3606480470110",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":22.4,"d":"22.40"},"ID","8536508090","https://www.se.com/sk/sk/product/XB7NA35","Monolithic push button, Harmony XB7, plastic, green, 22mm, spring return, unmarked, 1NO+1NC",0]
["XB7EV07MP","SIGNÁLKA S LED 230V ČÍRA IP65",10,"ks",{"v":11.895974999999998,"d":"11.896"},"3389119041249",{"v":14.5,"d":"14.50"},{"v":5.5,"d":"5.50"},{"v":10,"d":"10.00"},{"v":20,"d":"20.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XB7EV07MP","Monolithic pilot light, Harmony XB7, plastic, clear, 22mm, integral LED, 230…240V AC",0]
["XB7EV07GP","SIGNÁLKA S LED 110…120 V , BIELA",1,"ks",{"v":9.6082875,"d":"9.608"},"3389119041225",{"v":5.5,"d":"5.50"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":19,"d":"19.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XB7EV07GP","Harmony XB7, SIGNÁLKA, Ø22, integral LED, 110...120 V AC",0]
["XB7EV04MP","SIGNÁLKA S LED 230 VAC ČERVENÁ",10,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110839760",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":20,"d":"20.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XB7EV04MP","Monolithic pilot light, Harmony XB7, plastic, red, 22mm, integral LED, 230…240V AC",0]
["XB7EV03MP","SIGNÁLKA S LED 230 VAC ZELENÁ",10,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110839753",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":19,"d":"19.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XB7EV03MP","Monolithic pilot light, Harmony XB7, plastic, green, 22mm, integral LED, 230…240V AC",0]
["XB7EV03GP","SIGNÁLKA S LED 110…120 V , ZELENÁ",1,"ks",{"v":9.6082875,"d":"9.608"},"3389119022781",{"v":5.1,"d":"5.10"},{"v":2.8,"d":"2.80"},{"v":2.8,"d":"2.80"},{"v":21,"d":"21.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XB7EV03GP","Harmony XB7, SIGNÁLKA, Ø22, integral LED, 110...120 V AC",0]
["XB6ETN521P","OVLÁDAČ NÚDZOVÉHO ZASTAVENIA",5,"ks",{"v":32.485162499999994,"d":"32.485"},"3606480597664",{"v":4.3,"d":"4.30"},{"v":6.6,"d":"6.60"},{"v":4.3,"d":"4.30"},{"v":19.4,"d":"19.40"},"CN","8536508090","https://www.se.com/sk/sk/product/XB6ETN521P","Complete non illuminated mushroom head push button, Harmony XB6E, 16mm, red pushbutton 32mm, trigger turn/pull to release, 2NC",0]
["XB6ETI523P","OVLÁDAČ NÚDZOVÉHO ZASTAVENIA",5,"ks",{"v":56.277112499999994,"d":"56.277"},"3606480597688",{"v":4.3,"d":"4.30"},{"v":6.6,"d":"6.60"},{"v":4.3,"d":"4.30"},{"v":20.1,"d":"20.10"},"CN","8536508090","https://www.se.com/sk/sk/product/XB6ETI523P","Complete illuminated mushroom head push button, Harmony XB6E, 16mm, red pushbutton, 32mm, trigger turn pull to release, 2NC",0]
["XB6EDW4B1P","OVLÁDAČ STLÁČACÍ ČERVENÝ",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3389110630848",{"v":9,"d":"9.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":10,"d":"10.00"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6EDW4B1P","Illuminated monolithic push button, Harmony XB6E, rectangle red flush, 16mm, spring return, 24V DC, 1CO",0]
["XB6EDW3B1P","OVLÁDAČ STLÁČACÍ ZELENÝ",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3389110630824",{"v":20,"d":"20.00"},{"v":3,"d":"3.00"},{"v":9.5,"d":"9.50"},{"v":6,"d":"6.00"},"CN","8536508090","https://www.se.com/sk/sk/product/XB6EDW3B1P","Illuminated monolithic push button, Harmony XB6E, rectangle green flush, 16mm, spring return, 24V DC, 1CO",0]
["XB6EDW1B1P","Presvetlené tlačidlo",1,"ks",{"v":24.707024999999998,"d":"24.707"},"3389110630770",{"v":20,"d":"20.00"},{"v":3,"d":"3.00"},{"v":9.5,"d":"9.50"},{"v":12,"d":"12.00"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6EDW1B1P","ovládač presvetlený Ø16, 24 V - 1CO, biel",0]
["XB6ECW5J1P","TLAČIDLO PODSVIETENÉ ŽLTÉ-PRIEMER 16 12V",1,"ks",{"v":17.386425,"d":"17.386"},"3389110626766",{"v":20,"d":"20.00"},{"v":2.5,"d":"2.50"},{"v":12,"d":"12.00"},{"v":10,"d":"10.00"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6ECW5J1P","Illuminated monolithic push button, Harmony XB6E, square yellow flush, 16mm, spring return 12VDC, 1CO",0]
["XB6ECW1B2P","TLAČIDLO PODSVIETENÉ BIELE-PRIEM 16-24V",1,"ks",{"v":20.13165,"d":"20.132"},"3389110627664",{"v":9,"d":"9.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":12.6,"d":"12.60"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6ECW1B2P","Illuminated monolithic push button, Harmony XB6E, square white flush, 16mm, spring return, 24V DC, 2CO",0]
["XB6ECV5BP","SIGNÁLKA S LED 24V ŽLTÁ 16MM",5,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110626490",{"v":9,"d":"9.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":11,"d":"11.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XB6ECV5BP","Monolithic pilot light, Harmony XB6E, square Ø 16, IP65, yellow, integral LED 24VDCpolarised, connector",0]
["XB6ECV4BP","SIGNÁLKA S LED 24V ČERVENÁ 16MM",5,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110626483",{"v":9,"d":"9.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":11,"d":"11.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XB6ECV4BP","Monolithic pilot light, Harmony XB6E, square red, 16mm, plastic, IP65, integral LED, 24V DC",0]
["XB6ECV3BP","SIGNÁLKA S LED 24V ZELENÁ 16MM",5,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110626476",{"v":9,"d":"9.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":11,"d":"11.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XB6ECV3BP","Monolithic pilot light, Harmony XB6E, square green, 16mm, plastic, IP65, integral LED, 24V DC",0]
["XB6ECV1BP","SIGNÁLKA S LED 24V BIELA 16MM",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110626421",{"v":18.5,"d":"18.50"},{"v":2.8,"d":"2.80"},{"v":7.3,"d":"7.30"},{"v":9,"d":"9.00"},"CN","8531807000","https://www.se.com/sk/sk/product/XB6ECV1BP","Monolithic pilot light, Harmony XB6E, square Ø 16, IP65, white, integral LED 24VDCpolarised, connector",0]
["XB6ECF5B2P","SIGNÁLKA S LED 24V ŽLTÁ 16MM",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389110629415",{"v":18.5,"d":"18.50"},{"v":2.8,"d":"2.80"},{"v":7.3,"d":"7.30"},{"v":10,"d":"10.00"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6ECF5B2P","Illuminated monolithic push button, Harmony XB6E, square yellow flush, 16mm, latching, 24V DC, 2CO",0]
["XB6ECF4B2P","SIGNÁLKA S LED 24V ČERVENÁ 16MM",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110629347",{"v":9,"d":"9.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":12.4,"d":"12.40"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6ECF4B2P","ovládač stláčací presvetlený 24 V 2 CO,",0]
["XB6ECF1B2P","SIGNÁLKA S LED 24V BIELA 16MM",1,"ks",{"v":17.8439625,"d":"17.844"},"3389110629279",{"v":20,"d":"20.00"},{"v":9,"d":"9.00"},{"v":3,"d":"3.00"},{"v":12,"d":"12.00"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6ECF1B2P","Illuminated monolithic push button, Harmony XB6E, square white flush, 16mm, latching, 24V DC, 2CO",0]
["XB6EAW4B1P","Tlačidlo presvetlené",1,"ks",{"v":17.386425,"d":"17.386"},"3389110625035",{"v":9,"d":"9.00"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":10,"d":"10.00"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6EAW4B1P","Illuminated monolithic push button, Harmony XB6E, round red flush, 16mm, spring return, 24V DC, 1CO",0]
["XB6EAW3B1P","Tlačidlo presvetlené",1,"ks",{"v":17.386425,"d":"17.386"},"3389110625028",{"v":20,"d":"20.00"},{"v":3,"d":"3.00"},{"v":9.5,"d":"9.50"},{"v":6,"d":"6.00"},"CN","8536501190","https://www.se.com/sk/sk/product/XB6EAW3B1P","Illuminated monolithic push button, Harmony XB6E, round green flush, 16mm, spring return, 24V DC, 1CO",0]
["XB6EAV4BP","Signálka",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110624748",10.16,3.81,3.81,{"v":10,"d":"10.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XB6EAV4BP","kruhová kontrolka Ø 16 - IP 65 - červená - integral LED - 24 V - konektor",0]
["XB6EAV3BP","SIGNÁLKA PRIEM 16 IP65 ZELENA",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389110624731",{"v":20,"d":"20.00"},{"v":9,"d":"9.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},"CN","9030337000","https://www.se.com/sk/sk/product/XB6EAV3BP","Monolithic pilot light, Harmony XB6E, round green, 16mm, plastic, IP65, integral LED, 24V DC",0]
["XB6EAD222P","OTOČNÝ OVLÁDAČ 2-POLOHOVÝ 16MM",5,"ks",{"v":16.471349999999997,"d":"16.471"},"3389110640069",{"v":20,"d":"20.00"},{"v":3,"d":"3.00"},{"v":9.5,"d":"9.50"},{"v":12,"d":"12.00"},"CN","8536508090","https://www.se.com/sk/sk/product/XB6EAD222P","okrúhly čierny prepínač Ø16-vyčnievajúca rukoväť 2 polohy-2CO",0]
["XB6EAD221P","OTOČNÝ OVLÁDAČ 2-POLOHOVÝ 16MM",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110640021",{"v":20,"d":"20.00"},{"v":3,"d":"3.00"},{"v":9.5,"d":"9.50"},{"v":11,"d":"11.00"},"CN","8536508090","https://www.se.com/sk/sk/product/XB6EAD221P","Monolithic selector switch, Harmony XB6E, round black, 16mm, 2 positions, projecting handle, stay put, 1CO",0]
["XB6EAA41P","Tlačítko okrúhle červené NO IP65",1,"ks",{"v":10.065825,"d":"10.066"},"3389110624458",{"v":20,"d":"20.00"},{"v":9,"d":"9.00"},{"v":3,"d":"3.00"},{"v":10,"d":"10.00"},"CN","8536508090","https://www.se.com/sk/sk/product/XB6EAA41P","ovl. stláčací kruhový červený Ø 16 - lícujúcí s návratom - 1OC",0]
["XB6EAA31P","OTOČNÝ OVLÁDAČ, ZELENÝ",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110624441",{"v":20,"d":"20.00"},{"v":3,"d":"3.00"},{"v":9.5,"d":"9.50"},{"v":7,"d":"7.00"},"CN","8536508090","https://www.se.com/sk/sk/product/XB6EAA31P","ovládač kruhový zelený Ø 16 - zapust. pružinový návrat - 1OC",0]
["XB6EAA21P","OSTISKACÍ OVLÁDAČ, ČIERNY",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110624427",{"v":20,"d":"20.00"},{"v":9,"d":"9.00"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"CN","8536508090","https://www.se.com/sk/sk/product/XB6EAA21P","ovládač kruhový čierny Ø 16 - zapust. pružinový návrat - 1OC",0]
["XB6DV4BB","SIGNÁLKA",1,"ks",{"v":17.386425,"d":"17.386"},"3389110764512",{"v":11,"d":"11.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":12,"d":"12.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XB6DV4BB","obdĺžniková kontrolka Ø 16 – IP 65 – červená – zabud. LED – 24 V – konektor",0]
["XB6DA31B","TLAČIDLO OBDĹŽNIK. ZELENÉ Z",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110764277",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":12,"d":"12.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB6DA31B","zelené tlačidlo Ø 16 – zapust. vrat. pružina – 1 NO",0]
["XB6CV5BB","SIGNÁLKA",1,"ks",{"v":17.386425,"d":"17.386"},"3389110764536",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":11,"d":"11.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XB6CV5BB","štvorcová kontrolka Ø 16 – IP 65 – žltá – zabud. LED – 24 V – konektor",0]
["XB6CA25B","TLAČIDLO ŠTVORC. ČIERNE Z/V",1,"ks",{"v":21.046725,"d":"21.047"},"3389110764413",{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":14,"d":"14.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB6CA25B","čierne tlačidlo Ø 16 – zapust. vrat. pružina – 1 NO + 1 NC",0]
["XB6AV3BB","SIGNÁLKA",1,"ks",{"v":17.386425,"d":"17.386"},"3389110764468",{"v":11.1,"d":"11.10"},{"v":2,"d":"2.00"},{"v":11.1,"d":"11.10"},{"v":11,"d":"11.00"},"FR","9030337000","https://www.se.com/sk/sk/product/XB6AV3BB","okrúhla kontrolka Ø 16 – IP 65 – zelená – zabud. LED – 24 V – konektor",0]
["XB6AA42B","TLAČIDLO OKRÚHLE ČERVENÉ V",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110764314",{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":11,"d":"11.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB6AA42B","červené tlačidlo Ø 16 – zapust. vrat. pružina – 1 NC",0]
["XB5S7B2M12","SNÍMAČ ODTLAČKOV PRSTOV BISTABILNÝ",1,"ks",549.045,"3606489824938",{"v":18.5,"d":"18.50"},{"v":6.6,"d":"6.60"},{"v":9.5,"d":"9.50"},{"v":160,"d":"160.00"},"FR","8543709099","https://www.se.com/sk/sk/product/XB5S7B2M12","Biometric switch monostable RGPD, Harmony XB5S, plastic, 22mm, connection by M12 connector, 24V AC DC",0.02]
["XB5KS2M4","Bzučiak, trvalý alebo prerušovaný",1,"ks",{"v":74.121075,"d":"74.121"},"3606481352453",{"v":6,"d":"6.00"},{"v":3.4,"d":"3.40"},{"v":3.4,"d":"3.40"},{"v":24,"d":"24.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XB5KS2M4","Harmony XB5, Illuminated buzzer, plastic, red, Ø22, continuous or intermittent tone, 230…240 V AC",0]
["XB5FW33B5","Ovl. Stláčací presvetlený, zapustené, s ",1,"ks",{"v":21.5042625,"d":"21.504"},"3606481361035",{"v":5.3,"d":"5.30"},{"v":8.6,"d":"8.60"},{"v":4.3,"d":"4.30"},{"v":62,"d":"62.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5FW33B5","Harmony XB5, Antimikrobiálny podsvietený stláčací ovládač , zapustené prevedenie, plast, zelená, Ø30, integral LED, 24 V AC/DC, 1 NO + 1 NC",0.01]
["XB5FVB4","Signálka, zapustené, 24V, Ce",1,"ks",{"v":13.726125,"d":"13.726"},"3606481360878",{"v":5.3,"d":"5.30"},{"v":8.6,"d":"8.60"},{"v":4.3,"d":"4.30"},{"v":41,"d":"41.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XB5FVB4","Harmony XB5, Antimikrobiálna signálka , zapustené prevedenie, plast, červená, Ø30, priesvitná šošovka s  integral LED, 24 V AC/DC",0]
["XB5FA31","Ovl. Stláčací, zapustené, 1Z, Ze",1,"ks",{"v":8.876227499999999,"d":"8.876"},"3606481360465",{"v":5.3,"d":"5.30"},{"v":8.6,"d":"8.60"},{"v":4.3,"d":"4.30"},{"v":43,"d":"43.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5FA31","Harmony XB5, Antimikrobiálny stláčací ovládač , zapustené prevedenie, plast, zelená, Ø30, s návratom, bez symbolu, 1 NO",0]
["XB5EVM6","Kontrolka 230V, modrá",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389119041676",{"v":5.8,"d":"5.80"},{"v":3.3,"d":"3.30"},{"v":3.4,"d":"3.40"},{"v":25,"d":"25.00"},"ID","8531807000","https://www.se.com/sk/sk/product/XB5EVM6","SIGNÁLKA MODRÁ 22MM BEZ INT LED 230...240V",0]
["XB5DTB24","Časovač, montáž na panel, oneskorené zap",1,"ks",{"v":71.8333875,"d":"71.833"},"3606481205483",{"v":7.5,"d":"7.50"},{"v":3.2,"d":"3.20"},{"v":3.2,"d":"3.20"},{"v":28,"d":"28.00"},"FR","9107000090","https://www.se.com/sk/sk/product/XB5DTB24","časovač, montáž na panel, oneskorené zopnutie, 0,5 min až 10 min, 24 V DC",0]
["XB5AW73731B5","KOMPLETNÝ DVOJTLAČIDLOVÝ PLAST. OVLÁDAČ",1,"ks",{"v":33.857775,"d":"33.858"},"3389119043540",{"v":5.3,"d":"5.30"},{"v":8.6,"d":"8.60"},{"v":3.3,"d":"3.30"},{"v":61,"d":"61.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5AW73731B5","zel. lícujúca/červená s presah.ovl.hlavica dvojtlač.so signálkou Ø22 1Z+1V 24V",0.01]
["XB5AW33G5","OVLÁDAČ STLÁČACÍ PRESVETLENÝ ZELENÝ",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3389110904079",{"v":9.1,"d":"9.10"},{"v":3.5,"d":"3.50"},{"v":5.3,"d":"5.30"},{"v":55,"d":"55.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5AW33G5","zelené osvetlené tlačidlo Ø 22 – zapust. vrat. pružina – 120 V – 1 NO + 1 NC",0.01]
["XB5AVB5","SIGNÁLKA S LED ŽLTÁ",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110903799",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":35.2,"d":"35.20"},"FR","8531807000","https://www.se.com/sk/sk/product/XB5AVB5","okrúhla kontrolka Ø 22 – IP 65 – žltá – zabud. LED – 24 V – očká",0]
["XB5AVB1","SIGNÁLKA S LED BIELA",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110903768",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":35.3,"d":"35.30"},"FR","8531807000","https://www.se.com/sk/sk/product/XB5AVB1","okrúhla kontrolka Ø 22 – IP 65 – biela – zabud. LED – 24 V – očká",0]
["XB5AS84W3B41","OVLÁDAČ NUDZOVÉHO ZASTAVENIA VE SKRÍNI",1,"ks",{"v":45.75375,"d":"45.754"},"3606489745622",{"v":10,"d":"10.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":124,"d":"124.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XB5AS84W3B41","Harmony XB5, Antimikrobiálny podsvietený ovládač núdzového zastavenia, plast, Ø22, uvoľnenie pootočením, biela/červená LED, 24 V AC/DC, 1 NO + 2 NC",0]
["XB5AK135B5","Ovládac otocný presv. s LED, 3 polohy",1,"ks",{"v":32.485162499999994,"d":"32.485"},"3389118223356",{"v":9.1,"d":"9.10"},{"v":5.4,"d":"5.40"},{"v":3.5,"d":"3.50"},{"v":60,"d":"60.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5AK135B5","Illuminated selector switch, Harmony XB5, grey plastic, orange handle, 22mm, universal LED, 3 positions, 1NO + 1NC, 24V AC DC",0.01]
["XB5AK124M5","OVLÁDAČ OTOČNÝ PRESV. S LED ČERVENÝ",1,"ks",{"v":42.09345,"d":"42.093"},"3389110903591",{"v":3.3,"d":"3.30"},{"v":8.6,"d":"8.60"},{"v":5.2,"d":"5.20"},{"v":56,"d":"56.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5AK124M5","červený osvetlený voliaci spínač Ø 22 rukoväť 2 polohy – 240 V – 1 NO + 1 NC",0.01]
["XB5AD53","OVLÁDAČ OTOČNÝ ČIERNY",1,"ks",{"v":21.961799999999997,"d":"21.962"},"3389110903461",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":51,"d":"51.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5AD53","voliaci spínač Ø 22 – 3 polohy vrat. pružiny – štandard. rukoväť – čierny – 2 NO",0]
["XB5AC21","OVLÁDAČ S HRÍBOM ČIERNY",1,"ks",{"v":17.386425,"d":"17.386"},"3389110134452",{"v":9,"d":"9.00"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":63,"d":"63.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XB5AC21","čierne tlačidlo Ø 22 – hríb. hlavica Ø 40",0]
["XB5AA41","BOUTON POUSSOIR",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110085129",{"v":5.4,"d":"5.40"},{"v":9.1,"d":"9.10"},{"v":3.6,"d":"3.60"},{"v":36,"d":"36.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5AA41","ovládač na stlačenie s návratom",0]
["XB5AA3311","OVLÁDAČ STLÁČACÍ ZELENÝ",1,"ks",{"v":12.353512499999999,"d":"12.354"},"3389110903416",{"v":9.1,"d":"9.10"},{"v":3.5,"d":"3.50"},{"v":5.4,"d":"5.40"},{"v":36,"d":"36.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB5AA3311","zelené tlačidlo Ø 22 – zapust. vrat. pružina – 1 NO",0]
["XB4BW73731B5","KOMPLETNÝ DVOJTLAČIDLOVÝ KOVOVÝ OVLÁDAČ",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3389119043601",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":124.8,"d":"124.80"},"FR","8536508090","https://www.se.com/sk/sk/product/XB4BW73731B5","zel. lícujúca/červená s presah.ovl.hlavica dvojtlač.so signálkou Ø22 1Z+1V 24V",0]
["XB4BW3345","OVLÁDAC STLÁCACÍ PRESVETLENÝ 220..240V",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110887365",{"v":4.3,"d":"4.30"},{"v":12.8,"d":"12.80"},{"v":5.3,"d":"5.30"},{"v":177,"d":"177.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XB4BW3345","zelený ovladač stis. presvetlený lícujúci Ø22 s návratom 1Z+1V 220...240V",0]
["XB4BVM5","SIGNÁLKA S LED",1,"ks",{"v":22.876875,"d":"22.877"},"3389110892024",{"v":8.8,"d":"8.80"},{"v":3.4,"d":"3.40"},{"v":5.4,"d":"5.40"},{"v":80,"d":"80.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XB4BVM5","okrúhla kontrolka Ø 22 – IP65 – žltá – zabud. LED – 240 V – očká",0.01]
["XB4BVBM5GEX","Signálka Oranžová ATEX D/G",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3606489486099",{"v":15,"d":"15.00"},{"v":3,"d":"3.00"},{"v":10.5,"d":"10.50"},{"v":106,"d":"106.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XB4BVBM5GEX","Complete pilot light, Harmony XB4 - ATEX D, orange, integral LED, 24...240V",0.01]
["XB4BVB5","SIGNÁLKA S LED",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389110891942",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":79.5,"d":"79.50"},"FR","8531807000","https://www.se.com/sk/sk/product/XB4BVB5","okrúhla kontrolka Ø 22 – IP65 – žltá – zabud. LED – 24 V – očká",0.01]
["XB4BV5B4","Signálka s transformátorom 400V-50Hz",1,"ks",{"v":48.041437499999994,"d":"48.041"},"3389119039505",{"v":12.8,"d":"12.80"},{"v":3.8,"d":"3.80"},{"v":4,"d":"4.00"},{"v":175,"d":"175.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XB4BV5B4","signálka s LED 400 V, Ø22",0.03]
["XB4BV34","SIGNÁLKA SO ŽIAROVKOU",1,"ks",{"v":37.9756125,"d":"37.976"},"3389110887235",{"v":3,"d":"3.00"},{"v":8.2,"d":"8.20"},{"v":5.2,"d":"5.20"},{"v":146,"d":"146.00"},"FR","8531807000","https://www.se.com/sk/sk/product/XB4BV34","červená kompletná signálka Ø22 plná šošovka s BA9s žiarovkou 110...120V",0.02]
["XB4BS8444","OVlÁDAČ NÚDZOVÉHO ZASTAVENIA",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3389110959000",{"v":9.4,"d":"9.40"},{"v":4.7,"d":"4.70"},{"v":5.5,"d":"5.50"},{"v":133,"d":"133.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XB4BS8444","tlačidlo núdz. vyp. Ø 22 – hríb. hlavica Ø 40 červené – uvoľ. otočením – 2 NC",0]
["XB4BP381EX","EX OVLÁDAČ STLÁČACÍ",1,"ks",{"v":66.80047499999999,"d":"66.800"},"3389118030510",{"v":12,"d":"12.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":87,"d":"87.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB4BP381EX","zelené tlačidlo Ø 22 – vratná pružina – na vloženie štítka – 1 NO – ATEX",0]
["XB4BK135B5","ovládač otočný podsvietený Ø22 3-polohy",1,"ks",{"v":35.687925,"d":"35.688"},"3389118223264",{"v":8.7,"d":"8.70"},{"v":5.2,"d":"5.20"},{"v":3.4,"d":"3.40"},{"v":110,"d":"110.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB4BK135B5","ovládač otočný podsvietený Ø22 3-polohy pevné 1Z+1V 24V",0]
["XB4BG61EX","EX PREPÍNAČ S KĽÚČOM",1,"ks",{"v":118.95975,"d":"118.960"},"3389118030558",{"v":23.5,"d":"23.50"},{"v":3.5,"d":"3.50"},{"v":16,"d":"16.00"},{"v":164,"d":"164.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB4BG61EX","Complete selector switch, Harmony XB4, black key Ø22 mm, 2 positions 90°- spring return, 1 NO, ATEX",0]
["XB4BD912R4K7","XB4 kompletný potenciometer, lineárny, 4",1,"ks",{"v":57.192187499999996,"d":"57.192"},"3606480985003",{"v":8.7,"d":"8.70"},{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":95,"d":"95.00"},"FR","8533409000","https://www.se.com/sk/sk/product/XB4BD912R4K7","XB4 kompletný potenciometer, lineárny, 4,7 kOhm",0]
["XB4BD21","OVLÁDAČ OTOČNÝ",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3389110887075",{"v":9.1,"d":"9.10"},{"v":3.7,"d":"3.70"},{"v":5.5,"d":"5.50"},{"v":95,"d":"95.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB4BD21","voliaci spínač Ø 22 – 2-polohový usadený – štandard. rukoväť – čierny – 1 NO",0]
["XB4BA61","OVLÁDAČ STLÁČACÍ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389110118438",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":79,"d":"79.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB4BA61","modré tlačidlo Ø 22 – zapust. vrat. pružina – 1 NO",0]
["XB4BA11","OVLÁDAČ STLÁČACÍ",1,"ks",{"v":13.2685875,"d":"13.269"},"3389118377929",{"v":5.4,"d":"5.40"},{"v":9.1,"d":"9.10"},{"v":3.6,"d":"3.60"},{"v":80,"d":"80.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB4BA11","P/B,biely,1N/O,vratná pružina",0]
["XB2BN411","OVLÁDAČ",1,"ks",{"v":68.1730875,"d":"68.173"},"3389110675467",{"v":7.7,"d":"7.70"},{"v":4.2,"d":"4.20"},{"v":4.2,"d":"4.20"},{"v":103,"d":"103.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XB2BN411","Complete push button, Harmony XAP, Pushbutton XB2B, diameter Ø22 mm, 600 VAC, 10 A",0]
["XAWF178EX","EX KOVOVÁ SKRINKA JEDEN NÚDZOVÝ STOP",1,"ks",{"v":855.595125,"d":"855.595"},"3606480620201",{"v":23,"d":"23.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":845,"d":"845.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XAWF178EX","riadiaca stanica - XAW-F - metal - 1 NC + 1 NC - červená - Núdzové zastavenie",0]
["XAPO2602","Prázdna skrinka, Harmony XAP, zinková zl",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389119013536",{"v":13,"d":"13.00"},{"v":7.7,"d":"7.70"},{"v":8,"d":"8.00"},{"v":937,"d":"937.00"},"MA","7325100099","https://www.se.com/sk/sk/product/XAPO2602","Prázdna skrinka, Harmony XAP, zinková zliatina, oranžová, M20, 2 otvory Ø30mm, 80x130x77 mm",0]
["XAPG29703","KOVOVÉ PUZDRO",1,"ks",{"v":75.4936875,"d":"75.494"},"3389118381810",{"v":15.5,"d":"15.50"},{"v":9.5,"d":"9.50"},{"v":8.9,"d":"8.90"},{"v":687,"d":"687.00"},"FR","85381000","https://www.se.com/sk/sk/product/XAPG29703","Die cast empty control station, Harmony XAP, zinc alloy, grey, 3 cut outs, 22mm, 130x80x51.5mm",0]
["XAPE903","ZADNYKRYTPREDOSKUXAPE303",1,"ks",{"v":16.9288875,"d":"16.929"},"3389110628142",{"v":17,"d":"17.00"},{"v":6.3,"d":"6.30"},{"v":11.7,"d":"11.70"},{"v":60,"d":"60.00"},"FR","85389099","https://www.se.com/sk/sk/product/XAPE903","prázdny zapustený kryt - XAP-E - izolačný materiál - bez otvoru - IP 65",0]
["XAPD5508","Prázdna skrinka, Harmony XAP, zinková zl",1,"ks",183.015,"3389119013055",{"v":31,"d":"31.00"},{"v":7.7,"d":"7.70"},{"v":8.5,"d":"8.50"},{"v":810,"d":"810.00"},"MA","7907000090","https://www.se.com/sk/sk/product/XAPD5508","Prázdna skrinka, Harmony XAP, zinková zliatina, sivá, M32, 8 otvorov Ø22mm, 85x310x77 mm",0]
["XAPD3504","Prázdna skrinka, kov, sivá, M25,4 otvory",1,"ks",{"v":84.1869,"d":"84.187"},"3389118324855",{"v":18.7,"d":"18.70"},{"v":9,"d":"9.00"},{"v":12,"d":"12.00"},{"v":1420,"d":"1,420.00"},"MA","7907000090","https://www.se.com/sk/sk/product/XAPD3504","Prázdna skrinka, zinková zliatina, sivá, M25, 4 otvory Ø22mm",0]
["XAPD2204","Prázdna skrinka, Harmony XAP, zinková zl",1,"ks",{"v":67.71555,"d":"67.716"},"3389110001082",{"v":13,"d":"13.00"},5.15,{"v":8,"d":"8.00"},{"v":600,"d":"600.00"},"MA","7907000090","https://www.se.com/sk/sk/product/XAPD2204","Prázdna skrinka, Harmony XAP, zinková zliatina, sivá, M20, 4 otvory Ø22mm, 80x130x51,5 mm",0]
["XAPA3100","PRÁZDNA SKRINKA",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110313178",{"v":24.5,"d":"24.50"},{"v":13,"d":"13.00"},{"v":16.6,"d":"16.60"},{"v":860,"d":"860.00"},"FR","8538100000","https://www.se.com/sk/sk/product/XAPA3100","prázd. riad. stanica – XAP-A – plastová – bez otvoru",0]
["XALKW01","PRÁZDNA SKRINKA NÚDZOVÉHO",1,"ks",{"v":13.726125,"d":"13.726"},"3606489745592",{"v":7.5,"d":"7.50"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":115,"d":"115.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XALKW01","Empty enclosure, Harmony XALK, XALD, plastic, yellow lid, for illuminated emergency stop push button 22mm, 1 cut out",0]
["XALK178SAQ","OVLÁDAČ NUDZOVÉHO ZASTAVENIA VE SKRÍNI",1,"ks",{"v":29.593525500000002,"d":"29.594"},"3606480669019",{"v":7,"d":"7.00"},{"v":9.6,"d":"9.60"},{"v":7,"d":"7.00"},{"v":172,"d":"172.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XALK178SAQ","ovládač núdzového zastavenia s aretáciou v skrini",""]
["XALG03","PRÁZDNA SKRINKA 3 OTVORY",1,"ks",{"v":40.2633,"d":"40.263"},"3389119019347",{"v":18.7,"d":"18.70"},{"v":8,"d":"8.00"},{"v":10,"d":"10.00"},{"v":321,"d":"321.00"},"DE","85381000","https://www.se.com/sk/sk/product/XALG03","prázd. riad. stanica – XAL-G – 3 výrezy",0]
["XALE1341","SKRINKA XAL, 2 VSTUPY",1,"ks",{"v":50.7866625,"d":"50.787"},"3389119017749",{"v":8.3,"d":"8.30"},{"v":9.8,"d":"9.80"},{"v":11.4,"d":"11.40"},{"v":120,"d":"120.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XALE1341","ovl. skriňa XAL-E - prepínač 2 polohy - biela - 1Z - O - I",0]
["XALD361M","SKRINKA XAL TROJTLAČIDLOVÁ",1,"ks",{"v":62.22509999999999,"d":"62.225"},"3389110114522",{"v":14,"d":"14.00"},{"v":7,"d":"7.00"},{"v":9.7,"d":"9.70"},{"v":293,"d":"293.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XALD361M","riad. stanica XAL-D – funkcia štart alebo stop – 1 NO + 1 NC",0]
["XALD222","SKRINKA XAL DVOJTLAČIDLOVÁ",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3389110114164",{"v":11,"d":"11.00"},{"v":7,"d":"7.00"},{"v":9.8,"d":"9.80"},{"v":224,"d":"224.00"},"FR","8536508090","https://www.se.com/sk/sk/product/XALD222","riad. stanica XAL-D – dve funkcie – 2 NO",0]
["XALD164","SKRINKA XAL JEDNOTLAČIDLOVÁ",1,"ks",{"v":29.282399999999996,"d":"29.282"},"3389110113525",{"v":9.7,"d":"9.70"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":165,"d":"165.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/XALD164","riad. stanica XAL-D – funkcia štart alebo stop – 1 NC",0]
["XALD05","PRÁZDNA SKRINKA",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110114843",{"v":7.6,"d":"7.60"},{"v":19.7,"d":"19.70"},{"v":7,"d":"7.00"},{"v":303,"d":"303.00"},"CZ","3926909790","https://www.se.com/sk/sk/product/XALD05","prázd. riad. stanica – XAL-D – plastová – 5 horizont.ch otvorov",0]
["XALD01CUST01","PRÁZDNA SKRINKA, 1 OTVOR",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3606481818430",{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":7,"d":"7.00"},{"v":124,"d":"124.00"},"FR","3926909790","https://www.se.com/sk/sk/product/XALD01CUST01","Prázdná skrina, I otvor\n",0]
["XACD23A0105","ZÁVESNÝ OVLÁDAČ",1,"ks",{"v":256.22099999999995,"d":"256.221"},"3389110920949",{"v":31.6,"d":"31.60"},{"v":12.3,"d":"12.30"},{"v":9,"d":"9.00"},{"v":557,"d":"557.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XACD23A0105","Pendant control station, Harmony XAC, 1 speed, 1 2-directional push button, 1 emergency stop key release, for ZB2BE102/ZB2BE102 + ZB2BE101",0]
["XACB960","OCHRANNÝ KRYT NA KÁBEL",1,"ks",{"v":40.720837499999995,"d":"40.721"},"3389110642063",{"v":23,"d":"23.00"},{"v":4.5,"d":"4.50"},{"v":6,"d":"6.00"},{"v":110,"d":"110.00"},"CZ","4016999790","https://www.se.com/sk/sk/product/XACB960","ochranná káblová priech.XAC - B - 10..22 mm",0]
["XACB9214","OVLÁDACIE TLAČIDLO",1,"ks",{"v":3.2027625,"d":"3.203"},"3389110640984",{"v":13,"d":"13.00"},{"v":3,"d":"3.00"},{"v":13,"d":"13.00"},{"v":5,"d":"5.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XACB9214","krytá hlavica pre tlačidlo XAC-B – červená – 16 mm, - 25 - + 70 °C",0]
["XACB691","ZÁVESNÝ OVLÁDAČ",1,"ks",{"v":507.86662499999994,"d":"507.867"},"3389110640458",{"v":70,"d":"70.00"},{"v":9,"d":"9.00"},{"v":10,"d":"10.00"},{"v":1735,"d":"1,735.00"},"CZ","8537109899","https://www.se.com/sk/sk/product/XACB691","Pendant control station, Harmony XAC, plastic, yellow, 12A, 6 push buttons, cable 10…22mm, for XESD1191",0]
["XACB2291","ZÁVESNÝ OVLÁDAČ",1,"ks",{"v":297.39937499999996,"d":"297.399"},"3389110367225",{"v":27,"d":"27.00"},{"v":11.5,"d":"11.50"},{"v":10.5,"d":"10.50"},{"v":920.5,"d":"920.50"},"CZ","85381000","https://www.se.com/sk/sk/product/XACB2291","Pendant control station, Harmony XAC, plastic, yellow, 2 push buttons, 1 emergency stop, cable 10…22mm, for XESD1291",0]
["XACB065","ZÁVESNÝ OVLÁDAČ PRÁZDNY 6 OTVO",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389110300338",{"v":70,"d":"70.00"},{"v":9,"d":"9.00"},{"v":10,"d":"10.00"},{"v":1360,"d":"1,360.00"},"CZ","8538100000","https://www.se.com/sk/sk/product/XACB065","prázd. závesná riad. stanica XAC-B – 6 vertikálnych otvorov",0]
["XACB020","ZÁVESNÝ OVLÁDAČ PRÁZDNY",1,"ks",{"v":91.5075,"d":"91.508"},"3389110665550",{"v":26.5,"d":"26.50"},{"v":11.5,"d":"11.50"},{"v":10.5,"d":"10.50"},{"v":625,"d":"625.00"},"CZ","8538100000","https://www.se.com/sk/sk/product/XACB020","prázd. závesná riad. stanica XAC-B – 2 vert. otvory",0]
["XACA9412","OVL. HLAVICA STLÁČACIA",10,"ks",{"v":5.0786662499999995,"d":"5.079"},"3389110645149",{"v":3,"d":"3.00"},{"v":2.2,"d":"2.20"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/XACA9412","okrúhla hlavica pre tlačidlo –s vratnou pružinou – XAC-A – čierna – krytá",0]
["XACA67131","ZÁVESNÝ OVLÁDAČ 6 TLAČIDIEL",1,"ks",{"v":311.1255,"d":"311.126"},"3389110501094",{"v":57.5,"d":"57.50"},{"v":8.5,"d":"8.50"},{"v":9,"d":"9.00"},{"v":880,"d":"880.00"},"CZ","8537109899","https://www.se.com/sk/sk/product/XACA67131","závesný riadiaci ovládač XAC-A - 6 tlačidlá 1 núdzové zastavenie",0]
["XACA49231","ZÁVESNÝ OVLÁDAČ 4 TLAČIDLÁ",1,"ks",{"v":338.57775,"d":"338.578"},"3389110501070",{"v":50,"d":"50.00"},{"v":8,"d":"8.00"},{"v":9,"d":"9.00"},{"v":735,"d":"735.00"},"CZ","8537109899","https://www.se.com/sk/sk/product/XACA49231","závesná riad. stanica XAC-A – 4 tlačidlá, 1 núdzový vypínač",0]
["XACA291","ZÁVESNÝ OVLÁDAČ",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110367201",{"v":34.6,"d":"34.60"},{"v":8.4,"d":"8.40"},{"v":9,"d":"9.00"},{"v":558,"d":"558.00"},"CZ","8537109899","https://www.se.com/sk/sk/product/XACA291","závesný riadiaci ovládač XAC-A 2 tlačidlá",0]
["XACA2713","ZÁVESNÝ OVLÁDAČ",1,"ks",109.809,"3389110426809",{"v":52.5,"d":"52.50"},{"v":10,"d":"10.00"},{"v":12,"d":"12.00"},{"v":633,"d":"633.00"},"CZ","8537109899","https://www.se.com/sk/sk/product/XACA2713","závesná riad. stanica XAC-A – 2 tlačidlá, 1 núdzový vypínač",0]
["XACA201","ZÁVESNÝ OVLÁDAČ",1,"ks",{"v":60.852487499999995,"d":"60.852"},"3389110645002",{"v":27,"d":"27.00"},{"v":7.5,"d":"7.50"},{"v":6,"d":"6.00"},{"v":252,"d":"252.00"},"FR","8537109899","https://www.se.com/sk/sk/product/XACA201","závesná stanica XAC-A pištoľová rukoväť– 2 tlačidlá",0]
["XACA06H7","ZÁVESNÝ OVLÁDAČ",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110306491",{"v":80,"d":"80.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":665,"d":"665.00"},"CZ","8538100000","https://www.se.com/sk/sk/product/XACA06H7","Empty pendant control station, Harmony XAC, plastic, yellow, 6 cut outs, UL CSA certified",0]
["WDE000651","Prep. sériový (rad.5) orient. IP44 šedý",1,"ks",{"v":6.894026999999999,"d":"6.894"},"3303432400279",{"v":8,"d":"8.00"},{"v":5,"d":"5.00"},{"v":6.5,"d":"6.50"},{"v":102.2,"d":"102.20"},"PL","8536508090","https://www.se.com/sk/sk/product/WDE000651","Prepínač sériový (5So), Cedar Plus, IP44, Šedá",0]
["WDE000584","Zásuvka 2P+PE + prep. (rad.6), IP44biela",1,"ks",{"v":8.606555999999998,"d":"8.607"},"3303432400873",{"v":13.5,"d":"13.50"},{"v":5,"d":"5.00"},{"v":7.5,"d":"7.50"},{"v":192,"d":"192.00"},"PL","8536699099","https://www.se.com/sk/sk/product/WDE000584","Zásuvka 2P+PE + prepínač (6), Cedar Plus, IP44, Biela",0]
["WDE000525","ZÁSUVKA 2x2P+SE 16A CL IP44 CEDAR BIE/TR",1,"ks",{"v":9.660419999999997,"d":"9.660"},"3303432400491",{"v":13.5,"d":"13.50"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":201,"d":"201.00"},"PL","8536699099","https://www.se.com/sk/sk/product/WDE000525","Zásuvka SCHUKO 2x2P+SE, Cedar Plus, 16A, clonky, IP44, Biela/Transparentný kryt",0]
["WDE000513","Tlačidlo (rad.1/0) svetlo IP44 biele",1,"ks",{"v":4.391099999999999,"d":"4.391"},"3303432400330",{"v":8,"d":"8.00"},{"v":5,"d":"5.00"},{"v":7,"d":"7.00"},{"v":100,"d":"100.00"},"PL","8536508090","https://www.se.com/sk/sk/product/WDE000513","Tlačidlo svetlo (1/0), Cedar Plus, IP44, Biela",0]
["VZ7","VARIO MODUL-POMOCNÝ KONTAKT 1Z+1V",1,"ks",{"v":16.013812499999997,"d":"16.014"},"3389110551969",{"v":9,"d":"9.00"},{"v":5.5,"d":"5.50"},{"v":3.7,"d":"3.70"},{"v":52,"d":"52.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/VZ7","pomocný dotykový blok s predstihom/oneskorením – VARIO – 1 NO + 1 NC",0]
["VZ408E-15BP01","VENTIL 4-CESTNÝ ZÓNOVÝ VZ408/15/0,25",1,"ks",{"v":59.0625,"d":"59.063"},"3606489661267",{"v":13,"d":"13.00"},{"v":5.5,"d":"5.50"},{"v":10,"d":"10.00"},{"v":250,"d":"250.00"},"IT","8481809990","https://www.se.com/sk/sk/product/VZ408E-15BP01","Zone Valve, 15mm, 3-Way Bypass, G External, Brass, 0.25kvs",0]
["VZ29","VARIO OCHRANNÝ KRYT SVORIEK",1,"ks",{"v":4.3008525,"d":"4.301"},"3389110552058",{"v":10,"d":"10.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},"CZ","8547200090","https://www.se.com/sk/sk/product/VZ29","ochranné kryty svoriek – Mini-VARIO a VARIO - pre pomocné dotykové bloky",0]
["VZ1L040U600T","TLMIVKA 3F 0,6MH 40A",1,"ks",{"v":1556.1,"d":"1556.100"},"3389110890693",{"v":15,"d":"15.00"},{"v":23,"d":"23.00"},{"v":21,"d":"21.00"},{"v":6925,"d":"6,925.00"},"FR","8504500090","https://www.se.com/sk/sk/product/VZ1L040U600T","sieťová a motorová tlmivka pre ATV, ATS a RTV, 0.6 mH, 40 A, IP20",0]
["VZ01","VARIO MODUL-HLAVNÝ KONTAKT 20A",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110448900",{"v":5.5,"d":"5.50"},{"v":3.7,"d":"3.70"},{"v":9,"d":"9.00"},{"v":46,"d":"46.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/VZ01","modul s hlavným kontaktom 20 A – pre V01",0]
["VW3SKR004W40000B","BRZDNÝ REZISTOR 3,3 OHM 40 KW IP20",1,"ks",{"v":7960.05,"d":"7960.050"},"3606481975263",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5600,"d":"5,600.00"},"DE","8504909000","https://www.se.com/sk/sk/product/VW3SKR004W40000B","BRZDNÝ REZISTOR 3,3 OHM, 40 KW, IP20",0.67]
["VW3S5101R30","MOTOROVÝ KÁBEL 4X1,5 TIENENÝ KONEKTOR 3M",1,"ks",{"v":212.05799999999996,"d":"212.058"},"3606485190303",{"v":20.9,"d":"20.90"},{"v":5.2,"d":"5.20"},{"v":19.8,"d":"19.80"},{"v":572,"d":"572.00"},"DE","8544429090","https://www.se.com/sk/sk/product/VW3S5101R30","motorový stienený kábel pre krokový motor- 4x1.5mm² - 3m",0]
["VW3M8502R03","Signálový kábel 2xRJ45,PTO na PTI, 0,3 m",1,"ks",{"v":32.986799999999995,"d":"32.987"},"3606480166808",{"v":13,"d":"13.00"},{"v":2.5,"d":"2.50"},{"v":7,"d":"7.00"},{"v":25,"d":"25.00"},"DE","8544429090","https://www.se.com/sk/sk/product/VW3M8502R03","signálový kábel 2 x RJ45 - PTO na PTI - 0,3 m",0]
["VW3M8102R750","ENKÓDER KÁBEL M23 - RJ45 75M",1,"ks",{"v":806.9984999999999,"d":"806.999"},"3606480166686",{"v":43,"d":"43.00"},{"v":5,"d":"5.00"},{"v":30,"d":"30.00"},{"v":4500,"d":"4,500.00"},"CZ","8544429090","https://www.se.com/sk/sk/product/VW3M8102R750","kábel pre enkoder M23 - RJ45 - 75m- 3 x (2 x 0.14 mm²) + (2 x 0.34 mm²)",0]
["VW3M5105R30","Motor cable 4x6 mm2, 3m, conn. M40",1,"ks",{"v":323.97749999999996,"d":"323.978"},"3606485263854",{"v":43,"d":"43.00"},{"v":5,"d":"5.00"},{"v":30,"d":"30.00"},{"v":2000,"d":"2,000.00"},"CZ","8544429090","https://www.se.com/sk/sk/product/VW3M5105R30","výkonový kábel - medzi servomotor BSH a servopohon - 4 x 6 mm² + 2 x 1 mm² - 3m",0]
["VW3M5103R100","MOTOROVÝ KÁBEL 4MM2, 10M, 1 KONEKTOR",1,"ks",400.554,"3389119207416",{"v":44.7,"d":"44.70"},{"v":7.9,"d":"7.90"},{"v":43.6,"d":"43.60"},{"v":4130,"d":"4,130.00"},"DE","8544429090","https://www.se.com/sk/sk/product/VW3M5103R100","výkonový kábel - medzi servomotor BSH a servopohon - 4 x 4 mm² + 2 x 1 mm² -10m",0]
["VW3M5101R200","MOTOROVÝ KÁBEL 1,5MM2, 20M, 1 KONEKTOR",1,"ks",294.525,"3389119207331",{"v":45.5,"d":"45.50"},{"v":6.6,"d":"6.60"},{"v":41.5,"d":"41.50"},{"v":4452,"d":"4,452.00"},"DE","8544429090","https://www.se.com/sk/sk/product/VW3M5101R200","výkonový kábel - medzi servomotor BDH, BSH a servopohon - 4x1.5mm²+2x1mm² - 20 m",0]
["VW3M3805R010","KÁBEL CANOPEN 1M, SUB-D 9 SAMICA/RJ45",1,"ks",{"v":48.89115,"d":"48.891"},"3389119214599",{"v":18,"d":"18.00"},{"v":2,"d":"2.00"},{"v":13,"d":"13.00"},{"v":70,"d":"70.00"},"CN","8544429090","https://www.se.com/sk/sk/product/VW3M3805R010","kábel zbernice CANopen - pre CANopen zber. - 1 m - 1 RJ45, 1 samica SUB-D 9",0.01]
["VW3L5F000","LXM KIT KONEKTOROV, CANOPEN/RS485",1,"ks",153.153,"3389118367739",{"v":9.8,"d":"9.80"},{"v":3.1,"d":"3.10"},{"v":10.2,"d":"10.20"},{"v":100,"d":"100.00"},"DE","8536901000","https://www.se.com/sk/sk/product/VW3L5F000","connector kits for CANopen/RS485 - 1 male, 1 female connector M12 + cap M12",0]
["VW3L30010R100","Kabel s konektorom M8 - 4 pól pre STO, 1",1,"ks",{"v":159.0435,"d":"159.044"},"3389118367647",{"v":35.2,"d":"35.20"},{"v":3.1,"d":"3.10"},{"v":29.1,"d":"29.10"},{"v":326,"d":"326.00"},"CZ","8544429090","https://www.se.com/sk/sk/product/VW3L30010R100","kábel pre STO bezp. funkcia - 10m - 1 konektor samica - M8",""]
["VW3A9922","GV2 Adaptor (steel sheet)",1,"ks",{"v":40.0995,"d":"40.100"},"3606489559373",{"v":23.1,"d":"23.10"},{"v":7,"d":"7.00"},{"v":16.7,"d":"16.70"},{"v":80,"d":"80.00"},"ID","7326909890","https://www.se.com/sk/sk/product/VW3A9922","support for GV2 mounting - for variable speed drive",0]
["VW3A8306TF10","MODBUS T RJ45 1M",1,"ks",{"v":48.478500000000004,"d":"48.479"},"3389110400526",{"v":11.5,"d":"11.50"},{"v":3,"d":"3.00"},{"v":11,"d":"11.00"},{"v":75,"d":"75.00"},"TW","8544421000","https://www.se.com/sk/sk/product/VW3A8306TF10","„T“ rozvetvenie Modbus, 1 x samčia RJ45 a 2 x samičia RJ45, kábel 1 m",0]
["VW3A8121","MULTI LOADER",1,"ks",1107.225,"3606480145346",{"v":30,"d":"30.00"},{"v":9.6,"d":"9.60"},{"v":30.5,"d":"30.50"},{"v":954,"d":"954.00"},"JP","8471900000","https://www.se.com/sk/sk/product/VW3A8121","nástroj multi loader - pre frekvenčný menič",0]
["VW3A7746","Brzdný rezistor 5 Ohm - 6,9 kW, IP 23",1,"ks",1940.337,"3606480802393",{"v":69.5,"d":"69.50"},{"v":58,"d":"58.00"},{"v":58,"d":"58.00"},{"v":29700,"d":"29,700.00"},"DE","8533290000","https://www.se.com/sk/sk/product/VW3A7746","brzdný rezistor 5 Ohm - 6,9 kW, IP 23",""]
["VW3A7734","Brzdný rezistor 10 Ohm - 1,1 kW, IP 20",1,"ks",495.558,"3606480802287",{"v":65,"d":"65.00"},{"v":25.5,"d":"25.50"},{"v":20,"d":"20.00"},{"v":5095,"d":"5,095.00"},"DE","8533290000","https://www.se.com/sk/sk/product/VW3A7734","brzdný rezistor 10 Ohm - 1,1 kW, IP 20",""]
["VW3A7604R07","BRZDNÝ ODPOR, IP65, 27OHM, 400W, 0.75M",1,"ks",460.845,"3389119207171",{"v":39.4,"d":"39.40"},{"v":4.4,"d":"4.40"},{"v":12.6,"d":"12.60"},{"v":1420,"d":"1,420.00"},"DE","8533290000","https://www.se.com/sk/sk/product/VW3A7604R07","brzdný rezistor - 27 Ohm - 400 W - kábel 0.75 m - IP20",0]
["VW3A5503","Filter súhlasného napätie, 4 - jádrový,",1,"ks",927.675,"3606485435787",{"v":18,"d":"18.00"},{"v":17,"d":"17.00"},{"v":27.7,"d":"27.70"},{"v":2190,"d":"2,190.00"},"TH","8548009099","https://www.se.com/sk/sk/product/VW3A5503","filter súhlasného napätie, 4 - jadrový, D2 = 76 mm, 120 µH",0]
["VW3A5305","Přídavný výstupní dv/dt filtr,  3f 200-2",1,"ks",{"v":1065.33,"d":"1065.330"},"3606480736728",{"v":75,"d":"75.00"},{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":24000,"d":"24,000.00"},"CN","8548009099","https://www.se.com/sk/sk/product/VW3A5305","prídavný výstupný dv/dt filter, 3f 200-240/380-480V, In=95A, IP20",0]
["VW3A4706","Přídavný vstupní EMC filtr, 3f 200-240/3",1,"ks",{"v":1095.2549999999999,"d":"1095.255"},"3606480736551",{"v":53,"d":"53.00"},{"v":28.5,"d":"28.50"},{"v":37.5,"d":"37.50"},{"v":11179,"d":"11,179.00"},"CN","8548009099","https://www.se.com/sk/sk/product/VW3A4706","prídavný vstupný EMC filter, 3f 200-240/380-480V, In=100A, IP20",0]
["VW3A4702","Přídavný vstupní EMC filtr, 3f 200-240/3",1,"ks",{"v":508.72499999999997,"d":"508.725"},"3606480736513",{"v":32,"d":"32.00"},{"v":14.5,"d":"14.50"},{"v":20,"d":"20.00"},{"v":2400,"d":"2,400.00"},"CN","8548009099","https://www.se.com/sk/sk/product/VW3A4702","prídavný vstupný EMC filter, 3f 200-240/380-480V, In=15A, IP20",0]
["VW3A4411","PRÍDAVNÝ VSTUPNÝ EMC FILTER 546A",1,"ks",{"v":2394,"d":"2394.000"},"3389119201360",{"v":120,"d":"120.00"},{"v":50,"d":"50.00"},{"v":80,"d":"80.00"},{"v":68000,"d":"68,000.00"},"DE","8548009099","https://www.se.com/sk/sk/product/VW3A4411","EMC radio interference input filter - 336/546 A - 125 W - 3-phase supply",0]
["VW3A3609","KOMUNIKAČNÁ KARTA DEVICE NET ATV 32",1,"ks",460.845,"3606480198991",{"v":8.9,"d":"8.90"},{"v":4.7,"d":"4.70"},{"v":6.2,"d":"6.20"},{"v":66,"d":"66.00"},"SE","8517620000","https://www.se.com/sk/sk/product/VW3A3609","komunikačný modul DeviceNet pre ATV32 - LXM32M",0]
["VW3A3307","KOMUNIKAČNÁ KARTA PRE PROFIBUS DP",1,"ks",412.965,"3389118067165",{"v":23,"d":"23.00"},{"v":7.2,"d":"7.20"},{"v":17,"d":"17.00"},{"v":281,"d":"281.00"},"FR","8517620000","https://www.se.com/sk/sk/product/VW3A3307","Karta Profibus DP V0 pre ATV 61 a ATV 71",0]
["VW3A31405","FILTER PRE ATV31 U22M2",1,"ks",{"v":215.46,"d":"215.460"},"3389110689471",{"v":27.7,"d":"27.70"},{"v":6.2,"d":"6.20"},{"v":23,"d":"23.00"},{"v":886,"d":"886.00"},"CH","8548009099","https://www.se.com/sk/sk/product/VW3A31405","doplnkový filter EMC S7 M2 – 1-fáz. napáj. – 22 A",0]
["VW3A1104R10","KÁBEL 2XRJ45 PRE PRIP. ATV71 A LCD 1M",1,"ks",16.758,"3389118070257",{"v":16.5,"d":"16.50"},{"v":1.7,"d":"1.70"},{"v":12.5,"d":"12.50"},{"v":55,"d":"55.00"},"TW","8544429090","https://www.se.com/sk/sk/product/VW3A1104R10","kábel pre pripojenie externého grafického terminálu, dĺžka 1 m",0]
["VVE1","VARIO NÚDZOVÝ VYP. 32A",1,"ks",{"v":40.2633,"d":"40.263"},"3389110553123",{"v":11.2,"d":"11.20"},{"v":7.7,"d":"7.70"},{"v":8.4,"d":"8.40"},{"v":183,"d":"183.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/VVE1","spínací odpínač VVE – TeSys – 3 póly – 690 V 32 A – uzamykacia červená rukoväť",0]
["VT3233","Zónový ventil Erie VT3233",1,"ks",{"v":124.03125,"d":"124.031"},"711426633634",7.62,5.08,7.62,{"v":11920,"d":"11,920.00"},"MX","8481809990","https://www.se.com/sk/sk/product/VT3233","Erie Zone Valve, 3-Way, PN16, DN15 (1/2\"), Rp Thread, Kvs 3.5 m³/h (Cv 4.0), Pop-Top Actuator Connection, Brass Body.",0]
["VP229E-25BQSNT","Tlakově nezávislý regulační ventil VP229",1,"ks",{"v":360.28125,"d":"360.281"},"7332552014383",{"v":16.4,"d":"16.40"},{"v":10,"d":"10.00"},{"v":13.2,"d":"13.20"},{"v":1313,"d":"1,313.00"},"SI","8481809990","https://www.se.com/sk/sk/product/VP229E-25BQSNT","SpaceLogic VP229E PIBCV (PICV), 2-Way, PN16, DN25, G1-¼ Ext. Thread, Std Flow: 0.34…1.7 m³/h (…0.47 l/s), No PT plugs.",0]
["VP222F-250CQS","Tlakově nezávislý regulační ventil VP222",1,"ks",{"v":27104.962499999998,"d":"27104.963"},"7332552014611",{"v":73,"d":"73.00"},{"v":73,"d":"73.00"},{"v":97,"d":"97.00"},{"v":342000,"d":"342,000.00"},"SI","8481809990","https://www.se.com/sk/sk/product/VP222F-250CQS","SpaceLogic VP222F PIBCV (PICV), 2-Way, PN16, DN250, Flanged, Standard Flow: 112...300 m³/h (41...103 l/s).",0]
["VP220F-80CQS","Tlakově nezávislý regulační ventil VP220",1,"ks",{"v":5670,"d":"5670.000"},"7332552014536",{"v":31,"d":"31.00"},{"v":31,"d":"31.00"},{"v":41,"d":"41.00"},{"v":45000,"d":"45,000.00"},"SI","8481805990","https://www.se.com/sk/sk/product/VP220F-80CQS","SpaceLogic VP220F PIBCV (PICV), 2-Way, PN16, DN80, Flanged, Standard Flow: 11.2...28 m³/h (3.1...7.8 l/s).",0]
["VLVAW2L150A40A","Kompenzačný rozvádzač VarSet 150kVAR CB",1,"ks",{"v":11025,"d":"11025.000"},"3606480732584",{"v":120,"d":"120.00"},{"v":117,"d":"117.00"},{"v":80,"d":"80.00"},{"v":89000,"d":"89,000.00"},"FR","8537109199","https://www.se.com/sk/sk/product/VLVAW2L150A40A","Kompenzačný rozvádzač VarSet Easy 150kVAR CB Auto",10.68]
["VLVAW0N03503AA","Kompenzačný rozvádzač 22kVAR Easy CB A",1,"ks",{"v":4252.5,"d":"4252.500"},"3606480594236",{"v":80,"d":"80.00"},{"v":82,"d":"82.00"},{"v":60,"d":"60.00"},{"v":28000,"d":"28,000.00"},"FR","8537109199","https://www.se.com/sk/sk/product/VLVAW0N03503AA","automatic PowerLogic PFC Capacitor bank, 022kvar with incomer CB xxB 400V 50Hz",3.36]
["VLVAF3P03514AD","Kompenzačný rozvádzač VARSET AUTO 250K 4",1,"ks",{"v":23039.1,"d":"23039.100"},"3606489476809",{"v":210,"d":"210.00"},{"v":80,"d":"80.00"},{"v":120,"d":"120.00"},{"v":322000,"d":"322,000.00"},"FR","8537109199","https://www.se.com/sk/sk/product/VLVAF3P03514AD","Kompenzačný rozvádzač VARSET AUTO 250KVAR DR4,2 CB",0]
["VLVAF2P03506AC","Kompenzačný rozvádzač VarSet 50kVAR Auto",1,"ks",{"v":13230,"d":"13230.000"},"3606489477110",{"v":120,"d":"120.00"},{"v":150,"d":"150.00"},{"v":80,"d":"80.00"},{"v":400000,"d":"400,000.00"},"FR","8537109199","https://www.se.com/sk/sk/product/VLVAF2P03506AC","Kompenzačný rozvádzač VarSet 75kVAR Auto DR2.7",48]
["VGS211F-65CS","VENTIL REG. 2-CESTNÝ, PRÍRR VGS221/65/63",1,"ks",{"v":1949.0625,"d":"1949.063"},"3606489660987",{"v":27,"d":"27.00"},{"v":36,"d":"36.00"},{"v":20,"d":"20.00"},{"v":20100,"d":"20,100.00"},"SE","8481807100","https://www.se.com/sk/sk/product/VGS211F-65CS","Globe Valve, 65mm, 3-Way, Flanged, stem Up Closed, Stainless Steel, 63kvs, Glycol 25-50% Steam and Water",0]
["VFXP10","Pitotová trubica - rýchlosť vzduchu 10\"",1,"ks",{"v":271.6875,"d":"271.688"},"3606489899721",{"v":30.5,"d":"30.50"},{"v":15.2,"d":"15.20"},{"v":15.2,"d":"15.20"},90.91,"US","90269000","https://www.se.com/sk/sk/product/VFXP10","Air Velocity Averaging Pitot Tube 10 in",0]
["VF209W-65CN","Motýlková klapka VF209W DN65",1,"ks",{"v":189,"d":"189.000"},"634558526615",{"v":10.6,"d":"10.60"},{"v":25,"d":"25.00"},{"v":9,"d":"9.00"},{"v":4050,"d":"4,050.00"},"CN","8481808590","https://www.se.com/sk/sk/product/VF209W-65CN","VF209W High Pressure Butterfly Valve, 2-Way, DN65, Wafer Flanged, Nylon Disc, EPDM Liner, Kvs 243 m³/h, Max ∆P 1200 kPa.",0]
["VF208W-200NZ","KLAPKOVÝ VENTIL VF208W 200",1,"ks",826.875,"3606489660802",19.05,8.89,26.67,{"v":12600,"d":"12,600.00"},"SE","8481808590","https://www.se.com/sk/sk/product/VF208W-200NZ","VF208W Butterfly Valve, 2-Way, DN200, Wafer Flanged, Zinc Plated Disc, EPDM Liner, Kvs 3450 m³/h, Max ∆P 300 kPa.",0]
["VDIR634130","LXH PREM KÁBEL S/STP LSFROH 300M",1,"ks",{"v":413.3524499999999,"d":"413.352"},"3606480186615",{"v":0.1,"d":"0.10"},{"v":0.1,"d":"0.10"},{"v":0.1,"d":"0.10"},{"v":73,"d":"73.00"},"CH","85444920","https://www.se.com/sk/sk/product/VDIR634130","LexCom Home - Premium - horizontal wide band cable Cat.6 S/FTP - 305 m",0.01]
["VCFXGE4","VARIO PRÁZDNA SKRINKA VYPÍNAČA V02-V2",1,"ks",{"v":49.414049999999996,"d":"49.414"},"3389110652369",{"v":20.5,"d":"20.50"},{"v":16.5,"d":"16.50"},{"v":16.5,"d":"16.50"},{"v":660,"d":"660.00"},"CZ","8538100000","https://www.se.com/sk/sk/product/VCFXGE4","skrinka pre VARIO VN02 - V2 + 4 max. doplnky – žltá pred. strana – IP65",0]
["VCF6GEN","VARIO NÚDZOVÝ VYP. V SKRINKE",1,"ks",{"v":352.30387499999995,"d":"352.304"},"3389119413220",{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":20.5,"d":"20.50"},{"v":2908,"d":"2,908.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/VCF6GEN","uzavretý vypínač VARIO VBF 3P",0]
["VCF01GE","VARIO NÚDZOVÝ VYP. 16A V SKRINKE IP65",1,"ks",{"v":51.2442,"d":"51.244"},"3389110194067",{"v":15.8,"d":"15.80"},{"v":14.3,"d":"14.30"},{"v":11,"d":"11.00"},{"v":481,"d":"481.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/VCF01GE","uzatvorený spínací odpínač v skrinke Vario – VCF – 3 póly – 16 A",0]
["VCCDN12","MINIVARIO NÚDZOVÝ HL. VYP. 12A+RUKOVÄŤ",1,"ks",{"v":40.720837499999995,"d":"40.721"},"3389110759938",{"v":25.5,"d":"25.50"},{"v":7.5,"d":"7.50"},{"v":8.8,"d":"8.80"},{"v":314,"d":"314.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/VCCDN12","spínací odpínač VCCDN – 3 póly – 690 V 12 A – uzamykacia červená rukoväť",0]
["VC3504E5000","Releový modul s transformátorom, 5x relé",1,"ks",{"v":230.34375,"d":"230.344"},"3606481807526",12.19,{"v":3.302,"d":"3.30"},{"v":8,"d":"8.00"},{"v":400,"d":"400.00"},"MX","9032102090","https://www.se.com/sk/sk/product/VC3504E5000","Relay Pack for Line-voltage FCU, 90 to 277 VAC 50/60 Hz, 2/4 Pipes, SER models, 4 Ins, On-Off, 1 H/C out, 1 cool out, 3 fan outs",0]
["VBF1GE","VARIO HLAVNÝ VYP. 25A V SKRINKE IP65",1,"ks",{"v":90.59242499999999,"d":"90.592"},"3389110166569",{"v":16,"d":"16.00"},{"v":14.5,"d":"14.50"},{"v":11.5,"d":"11.50"},{"v":472,"d":"472.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/VBF1GE","uzatvorený spínací odpínač v skrinke Vario – VBF – 3 póly – 25 A",0]
["VBF01GE","VARIO HLAVNÝ VYP. 16A V SKRINKE IP65",1,"ks",{"v":51.2442,"d":"51.244"},"3389110201048",{"v":15.5,"d":"15.50"},{"v":11,"d":"11.00"},{"v":14,"d":"14.00"},{"v":477,"d":"477.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/VBF01GE","uzatvorený spínací odpínač v skrinke Vario – VBF – 3 póly – 16 A",0]
["V6","VARIO SPÍNAČI BLOK 3P 175A",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110551747",{"v":10,"d":"10.00"},{"v":11.3,"d":"11.30"},{"v":13.2,"d":"13.20"},{"v":900,"d":"900.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/V6","základňa pre spínací odpínač Vario – 3 póly – 175 A",0]
["TSXCDP203","Prepojovací kábel 2xHE10 2m /0,324mm2",1,"ks",{"v":87.76845,"d":"87.768"},"3389110647778",{"v":25,"d":"25.00"},{"v":4,"d":"4.00"},{"v":25,"d":"25.00"},{"v":325,"d":"325.00"},"ZZ","8544429090","https://www.se.com/sk/sk/product/TSXCDP203","connecting cable - Modicon Premium - 2 m - for sub-base ABE7H16R20",0]
["TSXCDP103","Prepojovací kábel 2xHE10 1m /0,324mm2",1,"ks",{"v":79.52175,"d":"79.522"},"3389110647761",{"v":25,"d":"25.00"},{"v":4,"d":"4.00"},{"v":21,"d":"21.00"},{"v":200,"d":"200.00"},"ZZ","8544429090","https://www.se.com/sk/sk/product/TSXCDP103","connecting cable - Modicon Premium - 1 m - for sub-base ABE7H16R20",0]
["TSXCANCBDD1","CANOPEN KÁBEL SUBD9F-SUBD9M, CB, 1M",1,"ks",{"v":113.09759999999999,"d":"113.098"},"3595863860207",{"v":19,"d":"19.00"},{"v":3,"d":"3.00"},{"v":13.5,"d":"13.50"},{"v":140,"d":"140.00"},"PT","8544429090","https://www.se.com/sk/sk/product/TSXCANCBDD1","CANopen cordset - molded female SUB-D9 connectors - standard - IP20 - UL - 1 m",0]
["TRV00830","5KS RJ45/RJ45 KÁBEL L = 3 M",1,"ks",{"v":92.61,"d":"92.610"},"3606480025310",{"v":30,"d":"30.00"},{"v":4,"d":"4.00"},{"v":35,"d":"35.00"},{"v":816,"d":"816.00"},"CN","8544421000","https://www.se.com/sk/sk/product/TRV00830","prefab. kabel - 2xRJ45 samec - L = 3 m - pre NSX100..250/NSX400..630 - sada 5",0.08]
["TRV00121","MODUL DISPLEJA FDM121 96X96",1,"ks",{"v":255.77999999999994,"d":"255.780"},"3606480025389",{"v":10.375,"d":"10.38"},{"v":5.803,"d":"5.80"},{"v":10.275,"d":"10.28"},{"v":239,"d":"239.00"},"CN","8537109899","https://www.se.com/sk/sk/product/TRV00121","modul čelného displeja FDM 121 - 96*96 mm - IP54 - pre NSX100..630",0.02]
["TR25D3R2502TPE","TR25,250A 3P diaľkové ovl. 230V",1,"ks",{"v":1995.13125,"d":"1995.131"},"3606485952826",{"v":80,"d":"80.00"},{"v":73.5,"d":"73.50"},{"v":60,"d":"60.00"},{"v":25950,"d":"25,950.00"},"CN","8536508090","https://www.se.com/sk/sk/product/TR25D3R2502TPE","TransferPacT Remote, 250A, 230V, 3P, diaľkové ovl., vel. 250A",""]
["TPSISO29","barrier for TA16",1,"ks",{"v":59.0625,"d":"59.063"},"3606481066138",{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":56,"d":"56.00"},"CN","4016999790","https://www.se.com/sk/sk/product/TPSISO29","medzifázové prepážky, TransferPacT, izolačné príslušenstvo, rám 160A, súprava 9",0]
["TPSCON53","Svorky pre neupravené káble, TransferPacT, pre 1 kábel 35 až 300 mm2, vel. 630, 3P, sada 3",1,"ks",{"v":82.6875,"d":"82.688"},"3606485952642",{"v":27,"d":"27.00"},{"v":4,"d":"4.00"},{"v":24.5,"d":"24.50"},{"v":339,"d":"339.00"},"","","https://www.se.com/sk/sk/product/TPSCON53","Svorky pre neupravené káble, TransferPacT, pre 1 kábel 35 až 300 mm2, vel. 630, 3P, sada 3",""]
["TPSCON39","Rozširujúce nástavce svoriek, TransferPacT, doplnok pre vel. 250, 4P",1,"ks",{"v":81.50625,"d":"81.506"},"3606485952772",{"v":24.5,"d":"24.50"},{"v":0.5,"d":"0.50"},{"v":23.5,"d":"23.50"},{"v":380,"d":"380.00"},"","","https://www.se.com/sk/sk/product/TPSCON39","Rozširujúce nástavce svoriek, TransferPacT, doplnok pre vel. 250, 4P",2.65]
["TPRSS065","TeSys island spúšťač motora 30kW SIL",1,"ks",{"v":534.8574,"d":"534.857"},"3606489832827",{"v":17,"d":"17.00"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":1321,"d":"1,321.00"},"FR","8536508090","https://www.se.com/sk/sk/product/TPRSS065","TeSys island spúšťač motora 80A AC-1, 65A AC-3, 30kW / 40HP",1.55]
["TPCDIO15","Ext24VDC CAN",1,"ks",{"v":159.46875,"d":"159.469"},"3606481066053",{"v":2,"d":"2.00"},5.65,{"v":6.9,"d":"6.90"},{"v":40,"d":"40.00"},"CN","8538909189","https://www.se.com/sk/sk/product/TPCDIO15","funkčný modul, TransferPacT, rozšírenie zbernice a pomocné napájanie 24 V DC",0]
["TMC2PACK01","ZÁS.MOD M221 SOLUTION BALIACE APLIKÁCIE",1,"ks",{"v":167.58,"d":"167.580"},"3606480649134",6.86,3.56,4.83,{"v":15,"d":"15.00"},"CN","8536909500","https://www.se.com/sk/sk/product/TMC2PACK01","zásuvný modul M221 - solution balicí stroje, 2x AI - I/O rozšiř.",0]
["TMARTB3","M200 NAPÁJACIA SVORKOVNICA, 3PIN (5KS)",1,"ks",{"v":11.969999999999999,"d":"11.970"},"3606480696312",{"v":9.5,"d":"9.50"},{"v":0.7,"d":"0.70"},{"v":9.4,"d":"9.40"},{"v":30,"d":"30.00"},"CN","8536909500","https://www.se.com/sk/sk/product/TMARTB3","3 PIN TB for Power connection",0]
["TM7NCOM16B","IP67 CANOPEN IO BLOCK/16 DIO/M8",1,"ks",{"v":1295.9099999999999,"d":"1295.910"},"3595864092799",{"v":17.8,"d":"17.80"},{"v":4.5,"d":"4.50"},{"v":5.5,"d":"5.50"},{"v":385,"d":"385.00"},"AT","8536909500","https://www.se.com/sk/sk/product/TM7NCOM16B","blok rozhrania CANopen - IP67 - 16 I/O - M8",0.05]
["TM5SPS1F","NAPÁJACÍ MODUL 24VDC/F=6,3A ŠEDÝ",1,"ks",{"v":104.8509,"d":"104.851"},"3595864074917",{"v":10.5,"d":"10.50"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":37,"d":"37.00"},"AT","8504408390","https://www.se.com/sk/sk/product/TM5SPS1F","TM5 -mod. nap. modul 24V DC/F=6 - 3A šedý",0]
["TM5SE1SC10005","ČÍTACÍ MOD 1HSC SSI 1Mb 5VDC",1,"ks",{"v":541.9259999999999,"d":"541.926"},"3595864074863",{"v":10.5,"d":"10.50"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":39,"d":"39.00"},"AT","9029100090","https://www.se.com/sk/sk/product/TM5SE1SC10005","čítací modul-1 HSC inkrementálny-1 MHz",0]
["TM5SDM12DT","KOMB 24VDC 8DI/4TO 1 VODIČ.",1,"ks",{"v":206.1675,"d":"206.168"},"3595864074504",{"v":10.5,"d":"10.50"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":38,"d":"38.00"},"AT","8538909999","https://www.se.com/sk/sk/product/TM5SDM12DT","digitálny I/O modul-8I-4O-24V DC-1 vodič",0]
["TM5SAI4LK","SET MOD 4AI ±10V/0-20MA/4-20MA 12 BITOV",1,"ks",600.831,"3595864154732",{"v":11,"d":"11.00"},{"v":7,"d":"7.00"},{"v":9.2,"d":"9.20"},{"v":116,"d":"116.00"},"AT","8538909999","https://www.se.com/sk/sk/product/TM5SAI4LK","Analog input module, Modicon TM5, Composition kit of I/O(TM5SAI4L) + term. block(TM5ACTB12) + bus base(TM5ACBM11)",0]
["TM5SAI2TH","MOD 2AI TERMOČLÁNKY J/K/S/N 16 BITOV",1,"ks",{"v":477.1305,"d":"477.131"},"3595864074764",{"v":10.5,"d":"10.50"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":41,"d":"41.00"},"AT","8538909999","https://www.se.com/sk/sk/product/TM5SAI2TH","analógový vstupný modul - 2I - termočlánek J/K/N/S - 16 bitový",0]
["TM5C24D18T","KOMPAKT MODUL 24VDC 24DI /18DO TR",1,"ks",{"v":806.9984999999999,"d":"806.999"},"3595864074351",{"v":11,"d":"11.00"},{"v":7.5,"d":"7.50"},{"v":9,"d":"9.00"},{"v":278,"d":"278.00"},"AT","8536909500","https://www.se.com/sk/sk/product/TM5C24D18T","Compact I/O rozšir. blok TM5 - 42 I/O - 24 DI - 18 DO tranzistor",0.03]
["TM5ACLPL10","PRÍCHYTKA ĽAVÁ NA BÁZU 10KS",1,"ks",47.124,"3595864075228",{"v":12,"d":"12.00"},{"v":2,"d":"2.00"},{"v":8,"d":"8.00"},{"v":37,"d":"37.00"},"CN","3926909790","https://www.se.com/sk/sk/product/TM5ACLPL10","Modicon TM5, left retaining plate for bus base",0]
["TM3SAF5R","TM3 ROZ.BEZPEČ.KARTA, CAT.4",1,"ks",{"v":406.4445,"d":"406.445"},"3606485392998",{"v":12.5,"d":"12.50"},{"v":7.5,"d":"7.50"},{"v":10.6,"d":"10.60"},{"v":190,"d":"190.00"},"DE","8536419089","https://www.se.com/sk/sk/product/TM3SAF5R","Bezpečnostný modul pre PLC TM2xx, 1 funkcia, CAT4, skrutkové svorky",0.03]
["TM3DQ8RG","TM3 ROZ.KARTA, 8DO RELÉ, PRUŽ.SVORKY",1,"ks",{"v":229.7295,"d":"229.730"},"3606480611438",{"v":10.5,"d":"10.50"},{"v":7.5,"d":"7.50"},{"v":12.5,"d":"12.50"},{"v":110,"d":"110.00"},"CN","8536909500","https://www.se.com/sk/sk/product/TM3DQ8RG","modul TM3-rozšír. karta, 8DO relé - pružinové svorky",0.03]
["TM3DM8R","TM3 ROZ.KARTA, 4DI,4DO (RELÉ)",1,"ks",{"v":159.0435,"d":"159.044"},"3606480611520",{"v":10.5,"d":"10.50"},{"v":7.5,"d":"7.50"},{"v":12.5,"d":"12.50"},{"v":230,"d":"230.00"},"CN","8538909999","https://www.se.com/sk/sk/product/TM3DM8R","modul TM3-rozšir. karta, kombinovaná 8DIO (relé)",0.03]
["TM3BCSL","TM3 komunikační adaptér (Bus Coupler)",1,"ks",259.182,"3606489811051",{"v":12.7,"d":"12.70"},{"v":7.6,"d":"7.60"},{"v":10.7,"d":"10.70"},{"v":167,"d":"167.00"},"ID","8517620000","https://www.se.com/sk/sk/product/TM3BCSL","bus coupler module, Modicon TM3, distributed IO, optimized, Serial Line interface, IP20",0.02]
["TM3AI4","TM3 ROZ.KARTA, 4AI (12BIT)",1,"ks",282.744,"3606480648908",{"v":12.814,"d":"12.81"},{"v":7.585,"d":"7.59"},{"v":10.598,"d":"10.60"},{"v":110,"d":"110.00"},"CN","8538909999","https://www.se.com/sk/sk/product/TM3AI4","modul TM3-rozšir. karta, 4AI (+/-10V, 0-10V, 0-24mA, 4-24mA; 12bit)",0.03]
["TM241CE24U","PLC M241 DC, 14DI, 10DO(NEG.LOG.), ETH",1,"ks",{"v":618.5024999999999,"d":"618.503"},"3606480611155",18.76,{"v":11.606,"d":"11.61"},13.17,{"v":650,"d":"650.00"},"ID","8537109199","https://www.se.com/sk/sk/product/TM241CE24U","PLC Modicon M241 24 IO neg. logika Ethernet",0.08]
["TM221M16TG","PLC M221M DC, 8DI, 8DO(POZ.LOG), PRUŽ.SV",1,"ks",329.175,"3606480611308",{"v":12.6,"d":"12.60"},{"v":10.8,"d":"10.80"},{"v":10,"d":"10.00"},{"v":264,"d":"264.00"},"CN","8537109199","https://www.se.com/sk/sk/product/TM221M16TG","PLC Modicon M221 16 IO poz.logika - pružin.svorky",0.05]
["TM221CE24T","PLC M221C DC, 14DI, 10DO(POZ.LOG.), ETH",1,"ks",400.995,"3606480648786",{"v":15.607,"d":"15.61"},{"v":11.133,"d":"11.13"},{"v":14.136,"d":"14.14"},{"v":380,"d":"380.00"},"CN","8537109199","https://www.se.com/sk/sk/product/TM221CE24T","PLC Modicon M221 24 IO poz.logika Ethernet",0.07]
["TM200CE40T","PLC M200 DC, 24DI, 16DO(POZ.LOG.), ETH",1,"ks",{"v":472.81499999999994,"d":"472.815"},"3606480696169",{"v":18.785,"d":"18.79"},9.63,{"v":13.735,"d":"13.74"},{"v":766,"d":"766.00"},"CN","8537109199","https://www.se.com/sk/sk/product/TM200CE40T","controller, Modicon Easy M200, 40 IO, transistor source, Ethernet",0]
["TM1STNTCSF44030","NTC snímač 3,0m FAST IP67 4x40 -50+110°C",5,"ks",23.562,"3606480761737",{"v":12.5,"d":"12.50"},{"v":4,"d":"4.00"},{"v":11,"d":"11.00"},{"v":33,"d":"33.00"},"IT","8533401000","https://www.se.com/sk/sk/product/TM1STNTCSF44030","NTC snímač 3,0m FAST IP67 4x40 -50+110°C sivý",""]
["TCSESM083F23F1","CONNEXIUM SWITCH 8TX",1,"ks",{"v":2474.0099999999998,"d":"2474.010"},"3595864065526",{"v":23,"d":"23.00"},{"v":21.8,"d":"21.80"},{"v":22.5,"d":"22.50"},{"v":1463,"d":"1,463.00"},"DE","8517620000","https://www.se.com/sk/sk/product/TCSESM083F23F1","Ethernet TCP/IP rozšir. ridený spínač - ConneXium - 8 portov pre meď",0.18]
["TCSESB083F2CU0","MANAŽOVANÝ BASIC ETH.SWITCH 6TX/2FX-MM",1,"ks",1354.815,"3595864115436",{"v":23.3,"d":"23.30"},{"v":13.3,"d":"13.30"},{"v":16.1,"d":"16.10"},{"v":596,"d":"596.00"},"DE","85389091","https://www.se.com/sk/sk/product/TCSESB083F2CU0","Ethernet TCP/IP základný riadený spínač - ConneXium - 6TX/2FX - multimode",0.07]
["TCSEAAF1LFH00","CONNEXIUM OPTICKÝ MODUL SFP-LH/LC",1,"ks",{"v":4594.589999999999,"d":"4594.590"},"3595863892529",{"v":17,"d":"17.00"},{"v":3.5,"d":"3.50"},{"v":12,"d":"12.00"},{"v":35,"d":"35.00"},"DE","85389091","https://www.se.com/sk/sk/product/TCSEAAF1LFH00","ConneXium Fiber modul SFP-LH/LC",0]
["TCSCCN1FNX3SA","Kábel priamy, M12, L=3m",1,"ks",{"v":61.2612,"d":"61.261"},"3595864098418",{"v":19,"d":"19.00"},{"v":3.5,"d":"3.50"},{"v":15.5,"d":"15.50"},{"v":195,"d":"195.00"},"PL","8544429090","https://www.se.com/sk/sk/product/TCSCCN1FNX3SA","CANopen připoj. kabel - přímý - M12-A samice-vodič - 3m",0.02]
["TC907-3A2P-24","FC regulátor TC907, proporc,, 2-trub, Sy",1,"ks",{"v":124.03125,"d":"124.031"},"3606481731999",{"v":12.3,"d":"12.30"},{"v":5.5,"d":"5.50"},{"v":10.5,"d":"10.50"},{"v":155,"d":"155.00"},"CN","9032102090","https://www.se.com/sk/sk/product/TC907-3A2P-24","SpaceLogic thermostat, fan coil proportional, standalone, touchscreen, 2P, 3 fan, 24V, white",0.02]
["TC907-3A2LB","FC TC907,on/off,2-trub,Sys,dot.Disp,240V",1,"ks",{"v":114.58125,"d":"114.581"},"3606481011541",{"v":12.3,"d":"12.30"},{"v":5.5,"d":"5.50"},{"v":10.5,"d":"10.50"},{"v":155,"d":"155.00"},"CN","9032102090","https://www.se.com/sk/sk/product/TC907-3A2LB","Thermostat, Spacelogic, fan coil on/off, standalone, touchscreen, 2P, 3 fan, 240V, black",0.02]
["TA63D3S5004TPE","TA63,500A 3P otočné prep. 400V",1,"ks",{"v":4889.193749999999,"d":"4889.194"},"3606485952963",{"v":80,"d":"80.00"},{"v":73,"d":"73.00"},{"v":60,"d":"60.00"},{"v":35000,"d":"35,000.00"},"CN","8536508090","https://www.se.com/sk/sk/product/TA63D3S5004TPE","TransferPacT Automatic, 500A, 400V, 3P, otočné prep., vel. 630A",""]
["TA25D4L1002TPE","TA25,100A 4P LCD 230V",1,"ks",{"v":2598.75,"d":"2598.750"},"3606485953243",{"v":80,"d":"80.00"},{"v":73.5,"d":"73.50"},{"v":60,"d":"60.00"},{"v":26256,"d":"26,256.00"},"CN","8536508090","https://www.se.com/sk/sk/product/TA25D4L1002TPE","TransferPacT Active Automatic, 100A, 230V, 4P, LCD, vel. 250A",""]
["TA16D4S0804TPE","TA16,80A 4P",1,"ks",{"v":1358.4375,"d":"1358.438"},"3606482131637",{"v":40,"d":"40.00"},{"v":13.6,"d":"13.60"},{"v":22,"d":"22.00"},{"v":6423,"d":"6,423.00"},"CN","8536508090","https://www.se.com/sk/sk/product/TA16D4S0804TPE","prepínač zdrojov, TransferPacT automatic, 80A, 4P, otočný prepínač, rám 160A",0.77]
["TA10D4S0504TPE","TA10,050A 4P",1,"ks",{"v":1027.6875,"d":"1027.688"},"3606481065773",{"v":37,"d":"37.00"},{"v":14,"d":"14.00"},{"v":21,"d":"21.00"},{"v":3891,"d":"3,891.00"},"CN","8536508090","https://www.se.com/sk/sk/product/TA10D4S0504TPE","prepínač zdrojov, TransferPacT automatic, 50A, 4P, otočný prepínač, rám 100A",0.39]
["TA10D4L0404TPE","TA10,040A 4P LCD",1,"ks",{"v":1240.3125,"d":"1240.313"},"3606481065582",{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":3941,"d":"3,941.00"},"CN","8536508090","https://www.se.com/sk/sk/product/TA10D4L0404TPE","prepínač zdrojov, TransferPacT Active automatic, 40A, 4P, LCD, rám 100A",0.4]
["TA10D2S0803TPE","TA10,080A 2P",1,"ks",{"v":992.25,"d":"992.250"},"3606481065674",{"v":36.7,"d":"36.70"},{"v":13.6,"d":"13.60"},{"v":21.1,"d":"21.10"},{"v":2950,"d":"2,950.00"},"CN","8536508090","https://www.se.com/sk/sk/product/TA10D2S0803TPE","prepínač zdrojov, TransferPacT automatic, 80A, 2P, otočný prepínač, rám 100A",0.35000000000000003]
["STBXTS2120","KON. NAP. NIM MODULOV, PER. SVORKY, 10KS",1,"ks",35.343,"3595862053716",{"v":17,"d":"17.00"},{"v":1.2,"d":"1.20"},{"v":13.5,"d":"13.50"},{"v":23,"d":"23.00"},"DE","85369010","https://www.se.com/sk/sk/product/STBXTS2120","Modicon STB - konektor 2-svorkový pre nap. 24V DC - typ pruž.",0]
["STBXTS1120","KON. NAP. NIM MODULOV, SKR. SVORKY, 10KS",1,"ks",35.343,"3595862053709",{"v":10,"d":"10.00"},{"v":3,"d":"3.00"},{"v":5,"d":"5.00"},{"v":32,"d":"32.00"},"DE","8536901000","https://www.se.com/sk/sk/product/STBXTS1120","Modicon STB - konektor 2-svorkový pre nap. 24V DC - typ šrób.",0]
["STBXBE1300K","KIT(B,S,M) BOS ZAČIATKU OSTROVA",1,"ks",200.277,"3595863949247",{"v":13,"d":"13.00"},{"v":2.5,"d":"2.50"},{"v":8,"d":"8.00"},{"v":126,"d":"126.00"},"FR","8538909999","https://www.se.com/sk/sk/product/STBXBE1300K","Modicon STB - BOS interný rozšir. modul",0]
["STBXBA2200","ZÁKLADŇA PDT MODULOV, 18.4MM",1,"ks",{"v":54.78164999999999,"d":"54.782"},"3595862062008",{"v":14.1,"d":"14.10"},{"v":2.5,"d":"2.50"},{"v":5,"d":"5.00"},{"v":35,"d":"35.00"},"IN","8536901000","https://www.se.com/sk/sk/product/STBXBA2200","Modicon STB - montážma báza - pre napájací modul - 18.4 mm",0]
["STBDRA3290K","KIT(B,S,M) 2K DO RELE, 7A",1,"ks",{"v":170.82449999999997,"d":"170.825"},"3595863949131",{"v":13,"d":"13.00"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":130,"d":"130.00"},"FR","8538909999","https://www.se.com/sk/sk/product/STBDRA3290K","štand. digitálne výstupy STB - 24 V DC - 6 O",0.02]
["STBDDO3200K","KIT(B,S,M) 2K DO 24VDC 0.5A",1,"ks",{"v":93.65895,"d":"93.659"},"3595864000329",{"v":13,"d":"13.00"},{"v":2.7,"d":"2.70"},{"v":8,"d":"8.00"},{"v":112,"d":"112.00"},"FR","8538909999","https://www.se.com/sk/sk/product/STBDDO3200K","štand. digitálne výstupy - Modicon STB - 24 V DC - 2 O",0.02]
["STBAVO1265K","KIT(B,S,M) 2K AO -/+10V",1,"ks",{"v":312.1965,"d":"312.197"},"3595863948981",{"v":13,"d":"13.00"},{"v":2.7,"d":"2.70"},{"v":8,"d":"8.00"},{"v":115,"d":"115.00"},"FR","8538909999","https://www.se.com/sk/sk/product/STBAVO1265K","zákl. analog. výstupy STB - +/- 10 V - 2 O - 9 bit + znamén.",0.02]
["STBART0200K","KIT(B,S,M) 2K AI RTD",1,"ks",{"v":394.6635,"d":"394.664"},"3595863948691",{"v":13.3,"d":"13.30"},{"v":3,"d":"3.00"},{"v":8.3,"d":"8.30"},{"v":136,"d":"136.00"},"FR","8536909500","https://www.se.com/sk/sk/product/STBART0200K","štand. analogové vstupy STB - 2 I - 15 bit + znam.",0.02]
["SSP3A250BDR","3fázové SSR 530 V AC 50 A 24 V DC, rand.",1,"ks",183.015,"3606480579943",{"v":12.3,"d":"12.30"},{"v":4.3,"d":"4.30"},{"v":8.8,"d":"8.80"},{"v":275,"d":"275.00"},"MX","8536490099","https://www.se.com/sk/sk/product/SSP3A250BDR","polovod.relé SSR-mont.na plech-vstup 4-32 V DC, výstup 48-530 V AC, 50A",0.03]
["SSP1D440BDT","1fázové SSR - panel.mont. - vst. 3,5-32",1,"ks",{"v":45.75375,"d":"45.754"},"3606485442020",{"v":6.5,"d":"6.50"},{"v":3.8,"d":"3.80"},{"v":4.8,"d":"4.80"},{"v":105,"d":"105.00"},"MX","8536490099","https://www.se.com/sk/sk/product/SSP1D440BDT","polovod.relé SSR-mont.na plech-chlad.podl-vstup 3.5-32VDC, výstup 1-150VDC,40 A",0.01]
["SSP1A490BDS","1fázové SSR - panel. mont. - vst. 4-32V ",1,"ks",{"v":69.36268499999998,"d":"69.363"},"3606485442266",{"v":7,"d":"7.00"},{"v":4.8,"d":"4.80"},{"v":4.8,"d":"4.80"},{"v":112,"d":"112.00"},"MX","8536490099","https://www.se.com/sk/sk/product/SSP1A490BDS","SSR-mont.na plech-chlad.podl.-vstup 4-32 VDC,výstup 48-660 VAC,90A s diag.",""]
["SSP1A125BDS","1fázové SSR - panel. mont. - vst. 3-32V ",1,"ks",{"v":71.888292,"d":"71.888"},"3606485442228",{"v":6.5,"d":"6.50"},{"v":4.8,"d":"4.80"},{"v":4.7,"d":"4.70"},{"v":109,"d":"109.00"},"MX","8536490099","https://www.se.com/sk/sk/product/SSP1A125BDS","SSR-mont.na plech-chlad.podl.-vstup 4-32 VDC,výstup 24-300 VAC,25A s diag.",""]
["SSP1A110BDT","1fázové SSR - panel. mont. - vst. 3-32V ",1,"ks",{"v":32.485162499999994,"d":"32.485"},"3606485442037",{"v":6.5,"d":"6.50"},{"v":3.4,"d":"3.40"},{"v":4.8,"d":"4.80"},{"v":97,"d":"97.00"},"MX","8536490099","https://www.se.com/sk/sk/product/SSP1A110BDT","polovod.relé SSR-mont.na plech-chlad.podl.-vstup 3-32V DC,výstup 24-300V AC,10 A",0.01]
["SSM1A16P7","1fázové SSR 280 V AC 6 A 230 V AC",1,"ks",{"v":37.518074999999996,"d":"37.518"},"3606480579387",{"v":9.5,"d":"9.50"},{"v":1,"d":"1.00"},{"v":9,"d":"9.00"},{"v":67,"d":"67.00"},"MX","8536490099","https://www.se.com/sk/sk/product/SSM1A16P7","polovod.relé SSR 1xF-mont.na DIN-vstup 200-265 V AC, výstup 24-280 V AC ,6A",0.01]
["SSL1A12BDPR","Harmony polovodičové relé predmontované",30,"ks",{"v":21.046725,"d":"21.047"},"3606489563073",{"v":7.9,"d":"7.90"},10.04,{"v":0.625,"d":"0.63"},{"v":33,"d":"33.00"},"ID","8536490099","https://www.se.com/sk/sk/product/SSL1A12BDPR","pre-assembled relay,  Harmony Solid State Relays, 2A, zeroVoltage switching, spring sockets, input 16...30V DC, output 24...250V AC",0]
["SSD1A345M7C2","Polovodičové relé Harmony, 1fázové, výst",1,"ks",{"v":90.59242499999999,"d":"90.592"},"3606489808051",{"v":14.5,"d":"14.50"},{"v":5.5,"d":"5.50"},{"v":12,"d":"12.00"},{"v":559,"d":"559.00"},"MX","8536490099","https://www.se.com/sk/sk/product/SSD1A345M7C2","Harmony, Solid state relay, 45 A, DIN rail mount, zero voltage switching, input 90…280 V AC/DC,  output 48...600 V AC",0.07]
["SR3XT101BD","LOG. MODUL ROZŠÍR. 10 I-O 24 VDC",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389110550085",{"v":9,"d":"9.00"},{"v":6.8,"d":"6.80"},{"v":10,"d":"10.00"},{"v":179,"d":"179.00"},"FR","8538909999","https://www.se.com/sk/sk/product/SR3XT101BD","rozširujúci modul s oddeleným I/O – 10 I O – 24 V DC – pre Zelio Logic",0.02]
["SR3PACK2BD","BALÍK 26 I-O 24 VDC",1,"ks",{"v":430.08525,"d":"430.085"},"3389110550047",{"v":23.5,"d":"23.50"},{"v":6.2,"d":"6.20"},{"v":15.5,"d":"15.50"},{"v":523,"d":"523.00"},"FR","8537109899","https://www.se.com/sk/sk/product/SR3PACK2BD","modulárne intel. relé Zelio Logic – základný balík – 26 I O – 24 V DC",0.07]
["SR2E121FU","LOG. MODUL BL 12 I-O 100-240 VAC",1,"ks",{"v":164.71349999999998,"d":"164.714"},"3389110549782",{"v":8.8,"d":"8.80"},{"v":6.5,"d":"6.50"},{"v":10,"d":"10.00"},{"v":212,"d":"212.00"},"FR","8537109899","https://www.se.com/sk/sk/product/SR2E121FU","komp. intel. relé Zelio Logic – 12 I O – 100 - 240 V AC – hodiny – bez displ.",0.03]
["SR2B201BD","LOG. MODUL 20 I-O 24 VDC",1,"ks",{"v":288.24862499999995,"d":"288.249"},"3389110549423",{"v":13.5,"d":"13.50"},{"v":7,"d":"7.00"},{"v":10,"d":"10.00"},{"v":363,"d":"363.00"},"FR","8537109899","https://www.se.com/sk/sk/product/SR2B201BD","kompakt. intel. relé Zelio Logic – 20 I O – 24 V DC – hodiny – displej",0.04]
["SR2A201BD","LOG. MODUL 20 I-O 24 VDC WC",1,"ks",{"v":260.79637499999995,"d":"260.796"},"3389110549416",{"v":13.5,"d":"13.50"},{"v":6.8,"d":"6.80"},{"v":10,"d":"10.00"},{"v":356,"d":"356.00"},"FR","8537109899","https://www.se.com/sk/sk/product/SR2A201BD","kompakt. intel. relé Zelio Logic – 20 I O – 24 V DC – bez hodín – displej",0.04]
["SKBZBY02T67","ŠTÍTOK \"ZAP - VYP\"",1,"ks",{"v":2.3791949999999997,"d":"2.379"},"3606481974259",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10000,"d":"10,000.00"},"CZ","39269097","https://www.se.com/sk/sk/product/SKBZBY02T67","Engraving ZAP - VYP",0]
["SER7350A5045B","Fancoilový regulátor, čidlo vlhkosti, BA",1,"ks",{"v":608.34375,"d":"608.344"},"711426070002",{"v":5.2,"d":"5.20"},{"v":15.2,"d":"15.20"},{"v":10.1,"d":"10.10"},{"v":231,"d":"231.00"},"CA","9032102090","https://www.se.com/sk/sk/product/SER7350A5045B","EBE - fancoilový regulátor, snímač vlhkosti, BACnet",0.05]
["SE8650U0B00","SE8650 prostorový regulátor kvality vzdu",1,"ks",{"v":572.90625,"d":"572.906"},"3606489928414",{"v":12,"d":"12.00"},{"v":2.5,"d":"2.50"},{"v":8.6,"d":"8.60"},{"v":43,"d":"43.00"},"MX","9032102090","https://www.se.com/sk/sk/product/SE8650U0B00","SE8650 priestorový regulátor kvality vzduchu",0.01]
["SDD391803","Rámček trojnásobný bridlica",1,"ks",{"v":9.221309999999999,"d":"9.221"},"3606481483461",{"v":22.5,"d":"22.50"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":58,"d":"58.00"},"PL","39259010","https://www.se.com/sk/sk/product/SDD391803","Rámček trojnásobný, Sedna D/E, bridlica",0]
["SDD381221","Zásuvka dvojnás. 230V 16A SCHUKO wenge",1,"ks",{"v":14.051519999999996,"d":"14.052"},"3606481483270",{"v":8.5,"d":"8.50"},{"v":4.9,"d":"4.90"},{"v":12,"d":"12.00"},{"v":95,"d":"95.00"},"PL","8536699099","https://www.se.com/sk/sk/product/SDD381221","Zásuvka dvojnásobná, Sedna D/E, 230V, 16A, SCHUKO, wenge",0]
["SDD371801","Rámček jednonásobný leštené zlato",1,"ks",{"v":5.664518999999999,"d":"5.665"},"3606481483065",{"v":8.5,"d":"8.50"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":24,"d":"24.00"},"PL","39259010","https://www.se.com/sk/sk/product/SDD371801","Rámček jednonásobný, Sedna D/E, leštené zlato",0]
["SDD314805","Rámček päťnásobný antracit",1,"ks",{"v":6.2353619999999985,"d":"6.235"},"3606481482693",{"v":37,"d":"37.00"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":45,"d":"45.00"},"PL","3925901000","https://www.se.com/sk/sk/product/SDD314805","Rámček päťnásobný, Sedna D/E, antracit",0]
["SDD313221","Zásuvka dvojnás. 230V 16A SCHUKO alu",1,"ks",{"v":9.660419999999997,"d":"9.660"},"3606481482525",{"v":12,"d":"12.00"},{"v":5,"d":"5.00"},{"v":8.5,"d":"8.50"},{"v":99,"d":"99.00"},"PL","8536699099","https://www.se.com/sk/sk/product/SDD313221","Zásuvka dvojnásobná, Sedna D/E, 230V, 16A, SCHUKO, aluminium",0]
["SDD312805","Rámček päťnásobný béžová",1,"ks",{"v":3.5567909999999987,"d":"3.557"},"3606481482457",{"v":37,"d":"37.00"},{"v":0.5,"d":"0.50"},{"v":8.5,"d":"8.50"},{"v":44,"d":"44.00"},"PL","3925901000","https://www.se.com/sk/sk/product/SDD312805","Rámček päťnásobný, Sedna D/E, béžová",0]
["SDD281101","Spínač jednopólový r.1 IP44 wenge",1,"ks",{"v":8.211356999999998,"d":"8.211"},"3606481958396",{"v":7.5,"d":"7.50"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":72,"d":"72.00"},"PL","8536508090","https://www.se.com/sk/sk/product/SDD281101","Spínač jednopólový r.1, Sedna D/E, IP44, wenge",0]
["SDD214132","Tlačidlo r.1So \"svetlo\" IP44 antracit",1,"ks",{"v":6.981848999999999,"d":"6.982"},"3606481482235",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":71,"d":"71.00"},"PL","8536508090","https://www.se.com/sk/sk/product/SDD214132","Tlačidlo 1/0 \"svetlo\", Sedna D/E, IP44, antracit",0]
["SDD213014","Zásuvka 230V 16A IP44 bezskr. alu",1,"ks",{"v":8.079623999999997,"d":"8.080"},"3606481482037",{"v":7.5,"d":"7.50"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":85,"d":"85.00"},"PL","8536699099","https://www.se.com/sk/sk/product/SDD213014","Zásuvka, Sedna D/E, 230V, 16A, IP44, bezskrutková, aluminium",0]
["SDD181904","Záslepný kryt wenge",1,"ks",{"v":7.3770479999999985,"d":"7.377"},"3606481481795",{"v":8.5,"d":"8.50"},{"v":6.2,"d":"6.20"},{"v":8.5,"d":"8.50"},{"v":66,"d":"66.00"},"PL","39259010","https://www.se.com/sk/sk/product/SDD181904","Záslepný kryt, Sedna D/E, wenge",0]
["SDD181481S","TV-SAT-SAT zásuvka koncová 4dB wenge",1,"ks",{"v":24.590159999999994,"d":"24.590"},"3606481468260",{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},{"v":7,"d":"7.00"},{"v":105,"d":"105.00"},"ES","8536691000","https://www.se.com/sk/sk/product/SDD181481S","TV-SAT-SAT zásuvka koncová, Sedna D/E, 4db, wenge",0]
["SDD181466","Dátová zásuvka 1xRJ45 kat. 6A UTP wenge",1,"ks",{"v":16.686179999999993,"d":"16.686"},"3606481468109",{"v":7,"d":"7.00"},{"v":4,"d":"4.00"},{"v":7,"d":"7.00"},{"v":58,"d":"58.00"},"DK","8536699099","https://www.se.com/sk/sk/product/SDD181466","Dátová zásuvka 1xRJ45 kat. 6a UTP, Sedna D/E, wenge",0]
["SDD181132","Tlačidlo r.1So \"svetlo\" wenge",1,"ks",{"v":8.782199999999998,"d":"8.782"},"3606481481603",{"v":7.5,"d":"7.50"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":59,"d":"59.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD181132","Tlačidlo 1/0 \"svetlo\", Sedna D/E, wenge",0]
["SDD181105","Prepínač sériový r.5 wenge",1,"ks",{"v":10.977749999999999,"d":"10.978"},"3606481481436",{"v":7.5,"d":"7.50"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":62,"d":"62.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD181105","Prepínač sériový r.5, Sedna D/E, wenge",0]
["SDD180503","Náhradné diely pre otočný stmievač breza",1,"ks",{"v":14.929739999999997,"d":"14.930"},"3606481467911",{"v":5.5,"d":"5.50"},{"v":2.5,"d":"2.50"},{"v":5.5,"d":"5.50"},{"v":17,"d":"17.00"},"LV","85365080","https://www.se.com/sk/sk/product/SDD180503","Náhradné diely pre otočný stmievač, Sedna D/E, breza",0]
["SDD180469T","Dát. zás. RJ45 kat.6 UTP+TV indiv. breza",1,"ks",{"v":23.272829999999995,"d":"23.273"},"3606481467737",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":95,"d":"95.00"},"DK","8536699099","https://www.se.com/sk/sk/product/SDD180469T","Dátová zásuvka RJ45 kat.6 UTP+TV individuálna, Sedna D/E, breza",0]
["SDD180452","Dátová zásuvka 2xRJ45 kat. 5e UTP breza",1,"ks",{"v":15.807959999999996,"d":"15.808"},"3606481467614",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":67,"d":"67.00"},"DK","8536699099","https://www.se.com/sk/sk/product/SDD180452","Dátová zásuvka 2xRJ45 kat. 5e UTP, Sedna D/E, breza",0]
["SDD180111","Tlačidlo r.1So breza",1,"ks",{"v":7.991801999999997,"d":"7.992"},"3606481480989",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":58,"d":"58.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD180111","Tlačidlo 1/0, Sedna D/E, breza",0]
["SDD170111L","Tlačidlo r.1So orientačná kont. leš.hl",1,"ks",{"v":11.416859999999996,"d":"11.417"},"3606481480590",{"v":7,"d":"7.00"},{"v":4,"d":"4.00"},{"v":7,"d":"7.00"},{"v":61,"d":"61.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD170111L","Tlačidlo 1/0So orientačná kontrolka, Sedna D/E, leštený hliník",0]
["SDD170106L","Prep. striedavý r.6 or. kont. leš. hl",1,"ks",{"v":13.173299999999996,"d":"13.173"},"3606481480538",{"v":7,"d":"7.00"},{"v":4.5,"d":"4.50"},{"v":7,"d":"7.00"},{"v":65,"d":"65.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD170106L","Prepínač striedavý r.6So orientačná kontrolka, Sedna D/E, leštený hliník",0]
["SDD114506","Izbový termostat 16A antracit",1,"ks",{"v":65.42738999999997,"d":"65.427"},"3606481467515",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":9.5,"d":"9.50"},{"v":173,"d":"173.00"},"LV","90321020","https://www.se.com/sk/sk/product/SDD114506","Izbový termostat, Sedna D/E, 16A, antracit",0.02]
["SDD114471","TV zásuvka koncová 4dB antracit",1,"ks",{"v":9.660419999999997,"d":"9.660"},"3606481467324",{"v":7.5,"d":"7.50"},{"v":5,"d":"5.00"},{"v":7.5,"d":"7.50"},{"v":84,"d":"84.00"},"ES","8536691000","https://www.se.com/sk/sk/product/SDD114471","TV zásuvka koncová, Sedna D/E, 4db, antracit",0]
["SDD114462","Dátová zásuvka 2xRJ45 kat. 6 UTP antr",1,"ks",{"v":13.612409999999995,"d":"13.612"},"3606481467249",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":67,"d":"67.00"},"DK","8536699099","https://www.se.com/sk/sk/product/SDD114462","Dátová zásuvka 2xRJ45 kat. 6 UTP, Sedna D/E, antracit",0]
["SDD114122","Tlačidlový ovládač s tiahlom antracit",1,"ks",{"v":21.077279999999995,"d":"21.077"},"3606481480040",{"v":7.5,"d":"7.50"},{"v":5,"d":"5.00"},{"v":7.5,"d":"7.50"},{"v":68,"d":"68.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD114122","Tlačidlový ovládač s tiahlom, Sedna D/E, antracit",0]
["SDD114114","Tlačidlový ovládač žaluzií antracit",1,"ks",{"v":10.977749999999999,"d":"10.978"},"3606481479990",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":67,"d":"67.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD114114","Tlačidlový ovládač žalúzií, Sedna D/E, antracit",0]
["SDD114012","Zásuvka 230V 16A cl. bezskrútková antr",1,"ks",{"v":4.566743999999999,"d":"4.567"},"3606481479747",{"v":7,"d":"7.00"},{"v":4,"d":"4.00"},{"v":7,"d":"7.00"},{"v":67,"d":"67.00"},"PL","8536699099","https://www.se.com/sk/sk/product/SDD114012","Zásuvka, Sedna D/E, 230V, 16A, bezskrutková, clonky, antracit",0]
["SDD113481S","TV-SAT-SAT zásuvka koncová 4dB alu",1,"ks",{"v":18.881729999999994,"d":"18.882"},"3606481467003",{"v":7.5,"d":"7.50"},{"v":5,"d":"5.00"},{"v":7.5,"d":"7.50"},{"v":104,"d":"104.00"},"ES","8536691000","https://www.se.com/sk/sk/product/SDD113481S","TV-SAT-SAT zásuvka koncová, Sedna D/E, 4db, aluminium",0]
["SDD113467","Dátová zásuvka 2xRJ45 kat. 6A UTP alu",1,"ks",{"v":19.320839999999993,"d":"19.321"},"3606481466860",{"v":7.5,"d":"7.50"},{"v":5,"d":"5.00"},{"v":7.5,"d":"7.50"},{"v":68,"d":"68.00"},"DK","8536699099","https://www.se.com/sk/sk/product/SDD113467","Dátová zásuvka 2xRJ45 kat. 6a UTP, Sedna D/E, aluminium",0]
["SDD113466","Dátová zásuvka 1xRJ45 kat. 6A UTP alu",1,"ks",{"v":12.734189999999998,"d":"12.734"},"3606481466846",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":58,"d":"58.00"},"DK","8536699099","https://www.se.com/sk/sk/product/SDD113466","Dátová zásuvka 1xRJ45 kat. 6a UTP, Sedna D/E, aluminium",0]
["SDD113121","Spínač pre hotelové karty alu",1,"ks",{"v":20.638169999999995,"d":"20.638"},"3606481479433",{"v":9.5,"d":"9.50"},{"v":4,"d":"4.00"},{"v":7,"d":"7.00"},{"v":71,"d":"71.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD113121","Spínač pre hotelové karty, Sedna D/E, aluminium",0]
["SDD113102","Spínač dvojpólový r.2 alu",1,"ks",{"v":7.3770479999999985,"d":"7.377"},"3606481479266",{"v":7.5,"d":"7.50"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":63,"d":"63.00"},"PL","8536508090","https://www.se.com/sk/sk/product/SDD113102","Spínač dvojpólový r.2, Sedna D/E, aluminium",0]
["SDD113022","Zásuvka 230V 16A SCHUKO alu",1,"ks",{"v":5.971895999999998,"d":"5.972"},"3606481479150",{"v":7.5,"d":"7.50"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":68,"d":"68.00"},"PL","8536699099","https://www.se.com/sk/sk/product/SDD113022","Zásuvka, Sedna D/E, 230V, 16A, SCHUKO, aluminium",0]
["SDD112484","TV-R-SAT zásuvka priebežná 7dB béžová",1,"ks",{"v":19.320839999999993,"d":"19.321"},"3606481466594",{"v":7.5,"d":"7.50"},{"v":5,"d":"5.00"},{"v":7.5,"d":"7.50"},{"v":105,"d":"105.00"},"ES","8536691000","https://www.se.com/sk/sk/product/SDD112484","TV-R-SAT zásuvka priebežná, Sedna D/E, 7db, béžová",0]
["SDD112471S","TV SAT zásuvka koncová 4dB béžová",1,"ks",{"v":10.099529999999996,"d":"10.100"},"3606481466501",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":98,"d":"98.00"},"ES","8536691000","https://www.se.com/sk/sk/product/SDD112471S","TV SAT zásuvka koncová, Sedna D/E, 4db, béžová",0]
["SDD112411","Zásuvka reproduktor. dvojitá béžová",1,"ks",{"v":9.221309999999999,"d":"9.221"},"3606481478986",{"v":9,"d":"9.00"},{"v":6.5,"d":"6.50"},{"v":8.5,"d":"8.50"},{"v":80,"d":"80.00"},"PL","8536699099","https://www.se.com/sk/sk/product/SDD112411","Zásuvka reproduktorová dvojitá, Sedna D/E, béžová",0]
["SDD112111","Tlačidlo r.1So béžová",1,"ks",{"v":4.083723,"d":"4.084"},"3606481478771",{"v":7,"d":"7.00"},{"v":3.5,"d":"3.50"},{"v":7,"d":"7.00"},{"v":58,"d":"58.00"},"PL","8536508090","https://www.se.com/sk/sk/product/SDD112111","Tlačidlo 1/0, Sedna D/E, béžová",0]
["SDD112105L","Prepínač sériový r.5 or. kont. béžová",1,"ks",{"v":7.991801999999997,"d":"7.992"},"3606481478719",{"v":7,"d":"7.00"},{"v":3.5,"d":"3.50"},{"v":7,"d":"7.00"},{"v":65,"d":"65.00"},"PL","8536508090","https://www.se.com/sk/sk/product/SDD112105L","Prepínač sériový r.5So orientačná kontrolka, Sedna D/E, béžová",0]
["SDD111902","Krabica povrchová viacnásobná biela",1,"ks",{"v":2.8103039999999995,"d":"2.810"},"3606481478481",{"v":8.5,"d":"8.50"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":47,"d":"47.00"},"PL","39269097","https://www.se.com/sk/sk/product/SDD111902","Krabica povrchová viacnásobná, Sedna D/E, Biela",0]
["SDD111503","Náhradné diely pre otočný stmievač biela",1,"ks",{"v":10.977749999999999,"d":"10.978"},"3606481466235",{"v":5.5,"d":"5.50"},{"v":2,"d":"2.00"},{"v":5.5,"d":"5.50"},{"v":17,"d":"17.00"},"LV","85365080","https://www.se.com/sk/sk/product/SDD111503","Náhradné diely pre otočný stmievač, Sedna D/E, Biela",0]
["SDD111474R","TV R zásuvka priebežná 7dB biela",1,"ks",{"v":10.099529999999996,"d":"10.100"},"3606481466105",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":100,"d":"100.00"},"ES","8536691000","https://www.se.com/sk/sk/product/SDD111474R","TV R zásuvka priebežná, Sedna D/E, 7db, Biela",0]
["SDD111441C","Kryt pro RJ45 KRONE UTP kon.biela",1,"ks",{"v":4.961943,"d":"4.962"},"3606481478436",{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":35,"d":"35.00"},"PL","39259010","https://www.se.com/sk/sk/product/SDD111441C","Kryt pro RJ45 KRONE UTP konektor, Sedna D/E, Biela",0]
["SDD111421","Stred. kryt Kyeston HDMI VGA biela",1,"ks",{"v":1.8003509999999994,"d":"1.800"},"3606481478399",{"v":7.5,"d":"7.50"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":48,"d":"48.00"},"PL","39269097","https://www.se.com/sk/sk/product/SDD111421","Stredový kryt Keystone HDMI VGA, Sedna D/E, Biela",0]
["SDD111111","Tlačidlo r.1So biela",1,"ks",{"v":4.083723,"d":"4.084"},"3606481478160",{"v":7.5,"d":"7.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":59,"d":"59.00"},"PL","85365080","https://www.se.com/sk/sk/product/SDD111111","Tlačidlo 1/0, Sedna D/E, Biela",0]
["SDD111101L","Spínač jednopólový r.1 or. kont. biela",1,"ks",{"v":5.664518999999999,"d":"5.665"},"3606481478030",{"v":7,"d":"7.00"},{"v":4,"d":"4.00"},{"v":7,"d":"7.00"},{"v":62,"d":"62.00"},"PL","8536508090","https://www.se.com/sk/sk/product/SDD111101L","Spínač jednopólový r.1So orientačná kontrolka, Sedna D/E, Biela",0]
["SD326RU25S2","KROKOVÝ POHON ( PULSE/DIR.,RM), 1~",1,"ks",{"v":1066.1805000000002,"d":"1066.181"},"3389119224338",{"v":19,"d":"19.00"},{"v":13.5,"d":"13.50"},{"v":16.8,"d":"16.80"},{"v":1255,"d":"1,255.00"},"DE","8504409590","https://www.se.com/sk/sk/product/SD326RU25S2","menič pre krokový motor pulzy/smer - 2,5 A-115/230 V-ovl.parkovacie brzdy-SD328",0.15]
["SD315ON10B400","MENIČ KROKOVÉHO MOTORA SD3 15O",1,"ks",518.364,"3606485186146",{"v":19,"d":"19.00"},{"v":6.8,"d":"6.80"},{"v":12.8,"d":"12.80"},{"v":367,"d":"367.00"},"DE","8504409590","https://www.se.com/sk/sk/product/SD315ON10B400","motion control stepper motor drive - SD315 - pulse direction with oscillator",0.04]
["SC450RMI1U","APC SMART-UPS SC 450VA 230V-1U",1,"ks",{"v":447.69374999999997,"d":"447.694"},"731304222712",{"v":58.9,"d":"58.90"},{"v":16.4,"d":"16.40"},{"v":47.6,"d":"47.60"},{"v":11730,"d":"11,730.00"},"IE","8504409590","https://www.se.com/sk/sk/product/SC450RMI1U","APC Smart-UPS SC 450 VA 230 V 1U montáž na stojan/vežu",""]
["RXZL520","SADA POPISNÝCH ŠTÍTKOV",1,"ks",{"v":4.941405,"d":"4.941"},"3389119404440",{"v":3.9,"d":"3.90"},{"v":2.4,"d":"2.40"},{"v":1.3,"d":"1.30"},{"v":16,"d":"16.00"},"CN","3926909790","https://www.se.com/sk/sk/product/RXZL520","nacvakávacie štítky - pre Zelio relé",0]
["RXZE2M114M","PÄTICA ZMIEŠANÉ SVORKY",10,"ks",{"v":4.666882499999999,"d":"4.667"},"3389119404259",{"v":7.918,"d":"7.92"},{"v":2.686,"d":"2.69"},{"v":4.245,"d":"4.25"},{"v":54,"d":"54.00"},"CN","8536909500","https://www.se.com/sk/sk/product/RXZE2M114M","zás.RXZ – zmieš. kont. – 10A – <lt/> 250V – konektor – pre relé RXM2.., RXMC4..",0]
["RXM4GB2P7","MINIATÚRNE RELÉ 4 CO LOW LEVEL S LED",10,"ks",{"v":9.6082875,"d":"9.608"},"3389119404044",{"v":2.8,"d":"2.80"},{"v":4.1,"d":"4.10"},{"v":2.1,"d":"2.10"},{"v":36,"d":"36.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RXM4GB2P7","miniatúrne zásuv. relé – Zelio RXM – 4 C/O – 230 V AC – 3 A – s LED kontrolkou",0]
["RXM4GB2F7","MINIATÚRNE RELÉ 4 CO LOW LEVEL S LED",10,"ks",{"v":9.6082875,"d":"9.608"},"3389119404013",{"v":2.8,"d":"2.80"},{"v":4.1,"d":"4.10"},{"v":2.1,"d":"2.10"},{"v":38,"d":"38.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RXM4GB2F7","miniatúrne zásuv. relé – Zelio RXM – 4 C/O – 120 V AC – 3 A – s LED kontrolkou",0]
["RXM4AB2BDPVS","MINIATÚRNE RELÉ, 6A, 4 CO S LED 24 V DC",30,"ks",{"v":15.556274999999998,"d":"15.556"},"3606489563189",{"v":8.5,"d":"8.50"},{"v":8.5,"d":"8.50"},{"v":2.8,"d":"2.80"},{"v":102,"d":"102.00"},"ID","8536419089","https://www.se.com/sk/sk/product/RXM4AB2BDPVS","Harmony, Miniature plug-in relay pre-assembled, 6 A, 4 CO, with LED, with lockable test button, separate terminals socket, 24 V DC",0.01]
["RXM4AB1ED","MINIATÚRNE RELÉ 4 CO 48 V DC",10,"ks",{"v":6.8630625,"d":"6.863"},"3389119403733",{"v":4.8,"d":"4.80"},{"v":2.1,"d":"2.10"},{"v":2.8,"d":"2.80"},{"v":35,"d":"35.00"},"CN","8536419089","https://www.se.com/sk/sk/product/RXM4AB1ED","miniatúrne zásuv. relé – Zelio RXM – 4 C/O – 48 V DC – 6 A",0]
["RXM3AB2B7","MINIATÚRNE RELÉ 3 CO S LED 24 V AC",10,"ks",{"v":7.5951225,"d":"7.595"},"3389119403627",{"v":12.5,"d":"12.50"},{"v":3.1,"d":"3.10"},{"v":10.3,"d":"10.30"},{"v":37,"d":"37.00"},"CN","8536419089","https://www.se.com/sk/sk/product/RXM3AB2B7","miniatúrne zásuv. relé – Zelio RXM – 3 C/O – 24 V AC – 10 A – s LED kontrolkou",0]
["RXM2LB2ED","Miniatúrne relé 5A 2CO 48VDC s LED",10,"ks",{"v":4.255098749999999,"d":"4.255"},"3389119215299",1.26,{"v":3.2,"d":"3.20"},1.03,{"v":33,"d":"33.00"},"CN","8536419089","https://www.se.com/sk/sk/product/RXM2LB2ED","Miniature plug in relay, Harmony, 5A, 2CO, with LED, 48V DC",0]
["RXM2AB2P7PVM","Harmony, miniatúrne plug-in relé predmon",30,"ks",{"v":16.471349999999997,"d":"16.471"},"3606489563172",{"v":7.845,"d":"7.85"},{"v":7.9,"d":"7.90"},2.69,{"v":99,"d":"99.00"},"ID","8536490099","https://www.se.com/sk/sk/product/RXM2AB2P7PVM","Miniatúrne plug-in relé predmontované, Harmony, 10 A, 2 CO, s LED, s blokovateľným testovacím tlačidlom, zmiešané svorky, 230 V AC",0.01]
["RXM2AB1E7","MINIATÚRNE RELÉ 2 CO 48 V AC",10,"ks",{"v":7.640876249999998,"d":"7.641"},"3389119403405",{"v":5,"d":"5.00"},{"v":2.1,"d":"2.10"},{"v":2.2,"d":"2.20"},{"v":37,"d":"37.00"},"CN","8536419089","https://www.se.com/sk/sk/product/RXM2AB1E7","miniatúrne zásuv. relé – Zelio RXM – 2 C/O – 48 V AC – 12 A",0]
["RXG23P7PV","Relé Zelio RXG, 2 C/O y, 5 A, 24V DC",30,"ks",{"v":11.895974999999998,"d":"11.896"},"3606489562922",{"v":7.2,"d":"7.20"},7.96,1.56,{"v":65,"d":"65.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RXG23P7PV","interface plug in relay, Harmony Electromechanical Relays, 5A, 2CO, pre assembled, with LED, 230V AC",0]
["RXG22F7","RXG, 2 C/O y, 5 A, 120 V AC, testovacie ",10,"ks",{"v":9.6082875,"d":"9.608"},"3606480689123",{"v":8.6,"d":"8.60"},3.45,9.25,{"v":19.8,"d":"19.80"},"CN","8536490099","https://www.se.com/sk/sk/product/RXG22F7","násuvné relé - Zelio RXG - 2C/O štand.-120VAC-5A - s TLB a LED",0]
["RXG15P7","RXG, 1 C/O , 10 A, 230 V AC, priehľadný",1,"ks",{"v":6.1310025,"d":"6.131"},"3606480688928",{"v":8.6,"d":"8.60"},3.45,9.25,{"v":221,"d":"221.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RXG15P7","násuvné relé - Zelio RXG - 1 C/O priehľadný kryt - 230 V AC - 10 A",0]
["RUZC2M","PÄTICA (CYLIND) ZMIEŠANÉ SVORKY",10,"ks",{"v":4.3008525,"d":"4.301"},"3389119403214",1.46,0.84,0.86,{"v":5,"d":"5.00"},"CN","8536699099","https://www.se.com/sk/sk/product/RUZC2M","zás.RUZ – zmieš. kont. – 10 A – <lt/> 250 V – konektor – pre relé RUMC2..",0]
["RUMF32FD","Univerzálny  3P faston, 10 A, 110 V DC s",10,"ks",{"v":12.81105,"d":"12.811"},"3606480627491",{"v":3.6,"d":"3.60"},{"v":3.5,"d":"3.50"},{"v":6.1,"d":"6.10"},{"v":86.3,"d":"86.30"},"CN","8536490099","https://www.se.com/sk/sk/product/RUMF32FD","univerz. násuvné relé - Zelio RUM - 3 C/O - 110 V DC - 10 A - s LED",0]
["RUMF22B7","Univerzálny  2P faston, 10 A, 24 V AC s",10,"ks",{"v":10.5233625,"d":"10.523"},"3606480627200",{"v":7.2,"d":"7.20"},{"v":3.7,"d":"3.70"},{"v":3.8,"d":"3.80"},{"v":80.5,"d":"80.50"},"CN","85364190","https://www.se.com/sk/sk/product/RUMF22B7","univerz. násuvné relé - Zelio RUM - 2 C/O - 24 V AC - 10 A - s LED",0]
["RUMC31JD","Univerzálny  3P pin, 10 A, 12 V DC, test",10,"ks",{"v":10.980899999999998,"d":"10.981"},"3606480626883",{"v":6.9,"d":"6.90"},{"v":3.6,"d":"3.60"},{"v":3.5,"d":"3.50"},{"v":86,"d":"86.00"},"CN","8536419089","https://www.se.com/sk/sk/product/RUMC31JD","univerz. násuvné relé - Zelio RUM - 3 C/O - 12 V DC - 10 A",0]
["RUMC23F7","Univerzálny  2P pin, 10 A, 120 V AC s LE",10,"ks",{"v":9.6082875,"d":"9.608"},"3606480626777",{"v":3.5,"d":"3.50"},{"v":6.9,"d":"6.90"},3.55,{"v":86,"d":"86.00"},"CN","85364900","https://www.se.com/sk/sk/product/RUMC23F7","univerz. násuvné relé - Zelio RUM - 2 C/O - 120 V AC - 10 A - s LED",0]
["RSZE05P","Pätica Push-in pre relé RSB1",10,"ks",{"v":4.34660625,"d":"4.347"},"3606481465733",10.16,5.84,1.52,{"v":30,"d":"30.00"},"CN","8536909500","https://www.se.com/sk/sk/product/RSZE05P","Push in socket with clamp, Harmony Electromechanical Relays, for RSB1A120 relays, 12A, push in terminals, separate contact",0]
["RSL1PVBU","SLIM RELÉ + PÄTICA 1C/O LED 24VAC/DC",10,"ks",{"v":13.726125,"d":"13.726"},"3606480077838",{"v":9.8,"d":"9.80"},{"v":0.7,"d":"0.70"},{"v":8,"d":"8.00"},{"v":29,"d":"29.00"},"IT","8536419089","https://www.se.com/sk/sk/product/RSL1PVBU","relé pre montáž na pätici so šróbovými svorkami-s LED a ochranným obvodom-24 V",0]
["RSL1AB4ED","SLIM RELÉ 1C/O, 6A, 48VDC",10,"ks",{"v":6.268263749999999,"d":"6.268"},"3606480077999",{"v":2.8,"d":"2.80"},{"v":0.5,"d":"0.50"},{"v":1.5,"d":"1.50"},{"v":6,"d":"6.00"},"CZ","8536419089","https://www.se.com/sk/sk/product/RSL1AB4ED","slim násuvné relé pre rozhranie - Zelio RSL - 1V/Z štandard - 48 V DC - 6 A",0]
["RSB1A160F7","PÄTICOVÉ RELÉ 1P/16A, 110VAC",10,"ks",{"v":9.6082875,"d":"9.608"},"3389110257465",{"v":31.1,"d":"31.10"},{"v":1.7,"d":"1.70"},{"v":2.5,"d":"2.50"},{"v":13,"d":"13.00"},"AT","8536490099","https://www.se.com/sk/sk/product/RSB1A160F7","stykové zásuvné relé – Zelio RSB – 1 C/O – 120 V AC – 16 A",0]
["RSB1A120B7","PÄTICOVÉ RELÉ 1P/12A, 24VAC",10,"ks",{"v":9.6082875,"d":"9.608"},"3389110256710",{"v":31.1,"d":"31.10"},{"v":2.1,"d":"2.10"},{"v":2.5,"d":"2.50"},{"v":13,"d":"13.00"},"AT","8536419089","https://www.se.com/sk/sk/product/RSB1A120B7","stykové zásuvné relé – Zelio RSB – 1 C/O – 24 V AC – 12 A",0]
["RPM42F7","VÝKONOVÉ RELÉ 4 CO S LED 120 V AC",1,"ks",{"v":17.386425,"d":"17.386"},"3389119402248",{"v":5,"d":"5.00"},{"v":2.4,"d":"2.40"},{"v":3.3,"d":"3.30"},{"v":72,"d":"72.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RPM42F7","výkonové zásuvné relé – Zelio RPM – 4 C/O – 120 V AC – 15 A – s LED kontrolkou",0.01]
["RPM32F7","VÝKONOVÉ RELÉ 3 CO S LED 120 V AC",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3389119402088",{"v":3.1,"d":"3.10"},{"v":4.7,"d":"4.70"},{"v":2.8,"d":"2.80"},{"v":54,"d":"54.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RPM32F7","výkonové zásuvné relé – Zelio RPM – 3 C/O – 120 V AC – 15 A – s LED kontrolkou",0.01]
["RPM21P7","VÝKONOVÉ RELÉ 2 CO 230 V AC",1,"ks",{"v":12.81105,"d":"12.811"},"3389119401876",{"v":2.8,"d":"2.80"},{"v":4.7,"d":"4.70"},{"v":2.1,"d":"2.10"},{"v":38,"d":"38.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RPM21P7","výkonové zásuvné relé – Zelio RPM – 2 C/O – 230 V AC – 15 A",0]
["RPM12F7","VÝKONOVÉ RELÉ 1 CO S LED 120 V AC",1,"ks",{"v":10.065825,"d":"10.066"},"3389119401760",{"v":1.4,"d":"1.40"},{"v":4.7,"d":"4.70"},{"v":2.8,"d":"2.80"},{"v":24,"d":"24.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RPM12F7","výkonové zásuvné relé – Zelio RPM – 1 C/O – 120 V AC – 15 A – s LED kontrolkou",0]
["RMPT50BD","PREVODNÍK PRE SONDU PT100 UNIVERZÁL",1,"ks",{"v":251.64562499999997,"d":"251.646"},"3389110108989",{"v":8.5,"d":"8.50"},{"v":2.7,"d":"2.70"},{"v":8.2,"d":"8.20"},{"v":106,"d":"106.00"},"ID","8543709099","https://www.se.com/sk/sk/product/RMPT50BD","vysielač teploty – 0 - 250 °C/32 - 482 °F – pre sondy Universal Pt100",0.01]
["RM35TF30","MULTIFUNKČNÉ SIEŤOVÉ KONTROLNÉ RELÉ",1,"ks",{"v":187.59037499999997,"d":"187.590"},"3389119405263",{"v":9.7,"d":"9.70"},{"v":4.8,"d":"4.80"},{"v":7.8,"d":"7.80"},{"v":133,"d":"133.00"},"ID","8536490099","https://www.se.com/sk/sk/product/RM35TF30","multifunkčné fázové riadiace relé RM35-T – rozsah 194 - 528 V AC",0.02]
["RM35LV14MW","HLADINOVÉ DISKR.VSTUP. KONTROLNÉ RELÉ",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389119405249",{"v":9.7,"d":"9.70"},{"v":4.8,"d":"4.80"},{"v":8,"d":"8.00"},{"v":133,"d":"133.00"},"ID","8536490099","https://www.se.com/sk/sk/product/RM35LV14MW","riadiace relé úrovne tekutiny RM35-L – 24 - 240 V AC/DC – 1 OC",0.02]
["RM22TG20","Kontrolné relé, 3fázové sítě, 183…528 V ",1,"ks",{"v":69.0881625,"d":"69.088"},"3606480792137",{"v":9.5,"d":"9.50"},{"v":2.5,"d":"2.50"},{"v":8.2,"d":"8.20"},{"v":103,"d":"103.00"},"CN","8536490099","https://www.se.com/sk/sk/product/RM22TG20","3xF kontrolné relé 183…528V AC, 2 C/O",0.01]
["RM22JA21MR","Meracie relé, nadprúd, 4mA…1A,2CO,8A",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3606480792281",{"v":2.6,"d":"2.60"},{"v":8.2,"d":"8.20"},{"v":9.5,"d":"9.50"},{"v":110,"d":"110.00"},"ID","8536490099","https://www.se.com/sk/sk/product/RM22JA21MR","meracie relé, nadprúd, 4 mA…1 A, 2 CO, 8 A, 24…240V",0.01]
["RGZE08P","Pätica Push-in pre relé RXG2",10,"ks",{"v":3.52303875,"d":"3.523"},"3606481465726",{"v":10,"d":"10.00"},{"v":1.5,"d":"1.50"},{"v":6.5,"d":"6.50"},{"v":40,"d":"40.00"},"CN","8536909500","https://www.se.com/sk/sk/product/RGZE08P","push in socket with clamp, Harmony Electromechanical Relays, for RXG2 relays, 5A, push-in terminals, separate contact",0]
["RE22R2QTMR","Čas. relé, start-delta, 24…240 AC/DC, 2",1,"ks",{"v":59.93741249999999,"d":"59.937"},"3606480792540",{"v":2.6,"d":"2.60"},{"v":8.2,"d":"8.20"},{"v":9.5,"d":"9.50"},{"v":90,"d":"90.00"},"ID","8536490099","https://www.se.com/sk/sk/product/RE22R2QTMR","trojuh.-Hviezda časové relé - 0.05s…300h - 24…240V AC/DC - 2C/O",0.01]
["RE22R2MMW","Časové relé, multifunkčné - 12..240 V AC",1,"ks",{"v":66.34293749999999,"d":"66.343"},"3606480676574",{"v":9.6,"d":"9.60"},{"v":2.5,"d":"2.50"},{"v":8.3,"d":"8.30"},{"v":93,"d":"93.00"},"ID","8536490099","https://www.se.com/sk/sk/product/RE22R2MMW","časové relé, multifunkčné - 12..240 V AC/DC - 2 C/O",0.01]
["RE22R1MAMR","Čas.relé z. sep., 24…240 AC/DC, 1 P",1,"ks",{"v":63.140175,"d":"63.140"},"3606480792427",{"v":2.6,"d":"2.60"},{"v":8.2,"d":"8.20"},{"v":9.5,"d":"9.50"},{"v":99,"d":"99.00"},"ID","8536490099","https://www.se.com/sk/sk/product/RE22R1MAMR","oneskorené zapnutie - časové relé - 0.05s…300h - 24…240V AC/DC - 1C/O",0.01]
["RE17RLJU","ČASOVÉ RELÉ BLIKAJÚCE 12V AC/DC",1,"ks",{"v":34.77285,"d":"34.773"},"3606480552717",{"v":9.6,"d":"9.60"},{"v":2.7,"d":"2.70"},{"v":7.8,"d":"7.80"},{"v":70,"d":"70.00"},"ID","8536419089","https://www.se.com/sk/sk/product/RE17RLJU","modul.čas.relé-asym.cyklovač - 1 s..100 h - 12 V AC/DC - 1 ZV",0.01]
["RE17LHBM","ČASOVÉ RELÉ ONESKOR. ROZOPNUT. 24-240VAC",1,"ks",{"v":38.8906875,"d":"38.891"},"3606480552649",{"v":9.5,"d":"9.50"},{"v":2.7,"d":"2.70"},{"v":8,"d":"8.00"},{"v":70,"d":"70.00"},"ID","8536490099","https://www.se.com/sk/sk/product/RE17LHBM","modul.čas.relé-oneskorené zopnutie-1 s..100 h-24..240 V AC/DC-polovod. výstup",0.01]
["R9H10977","RESI9 KV ZAPUSTENÁ, 3R, MULTIMEDIA",1,"ks",{"v":242.54999999999995,"d":"242.550"},"3606481330796",{"v":35,"d":"35.00"},{"v":10.5,"d":"10.50"},{"v":63,"d":"63.00"},{"v":4391,"d":"4,391.00"},"DE","8538100000","https://www.se.com/sk/sk/product/R9H10977","Resi9 KV zapustená, 3R, multimedia",0]
["R9H10939","RESI9 KV SPOJOVACIA SADA",1,"ks",22.491,"3606481330727",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":17,"d":"17.00"},"DE","39269097","https://www.se.com/sk/sk/product/R9H10939","Resi9 KV spájacia súprava",0]
["PRA90050","PRAGMA SADA PREPOJ SVORKOVNICE",1,"ks",{"v":10.142999999999999,"d":"10.143"},"3303432360191",{"v":14.5,"d":"14.50"},{"v":0.8,"d":"0.80"},{"v":9.5,"d":"9.50"},{"v":38,"d":"38.00"},"IT","8538909999","https://www.se.com/sk/sk/product/PRA90050","sada prepojovacej svorkovnice, 8 blokov – pre svorkovnicu",0]
["PRA90017G","PRAGMA ČELNÝ PANEL PLNÝ 18 MOD",1,"ks",13.671,"3606480592836",{"v":39.5,"d":"39.50"},{"v":3.5,"d":"3.50"},{"v":15,"d":"15.00"},{"v":242,"d":"242.00"},"IT","3925908000","https://www.se.com/sk/sk/product/PRA90017G","PRAGMA čelný panel plný 18 modulov",0]
["PKY32M723","ZÁSUVKA SPOJOV. FC IP67 32A 250V 2P+E",1,"ks",{"v":11.906999999999998,"d":"11.907"},"3303432010645",{"v":7,"d":"7.00"},{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},{"v":269,"d":"269.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKY32M723","PratiKa-priem.zás.spojovacia-2P+E-32A 250 VAC-IP67-rýchloup. prip.",0]
["PKY32G435","ZÁSUVKA VSTAV.R FC IP44 32A 415V 3P+N+E",1,"ks",11.466,"3303432012243",{"v":10.5,"d":"10.50"},{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},{"v":250,"d":"250.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKY32G435","PratiKa-priem.zás.vstavaná rovná-3P+N+E-32A 415 VAC-IP44-rýchloup. prip.",0]
["PKY16W434","ZÁSUVKA NÁSTEN. FC IP44 16A 415V 3P+E",1,"ks",{"v":10.70748,"d":"10.707"},"3303432416423",{"v":13.1,"d":"13.10"},{"v":7.5,"d":"7.50"},{"v":10.4,"d":"10.40"},{"v":193,"d":"193.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKY16W434","PratiKa-priem. zás. nástenná-3P+E-16 A 415 VAC-IP44-rýchloup. prip.",""]
["PKY16G435","ZÁSUVKA VSTAV.R FC IP44 16A 415V 3P+N+E",1,"ks",{"v":9.260999999999997,"d":"9.261"},"3303432012083",{"v":7,"d":"7.00"},{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},{"v":187,"d":"187.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKY16G435","PratiKa-priem.zás.vstavaná rovná-3P+N+E-16A 415 VAC-IP44-rýchloup. prip.",0]
["PKY16F733","ZÁSUVKA VSTAV.Š FC IP67 16A 415V 2P+E",1,"ks",{"v":11.086739999999999,"d":"11.087"},"3303432011314",{"v":7,"d":"7.00"},{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},{"v":181,"d":"181.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKY16F733","PratiKa-priem.zás.vstavaná šikmá-2P+E-16A 415 VAC-IP67-rýchloup. prip.",0]
["PKX32M733","VIDLICA SPOJOV. FC IP67 32A 415V 2P+E",1,"ks",{"v":26.733419999999995,"d":"26.733"},"3303432009724",{"v":7,"d":"7.00"},{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},{"v":440,"d":"440.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKX32M733","PratiKa wander plug - straight - 32 A - 2P + E - 380...415 V AC - IP67",""]
["PKX32M435","VIDLICA SPOJOV. FC IP44 32A 415V 3P+N+E",1,"ks",{"v":10.583999999999998,"d":"10.584"},"3303432009489",{"v":10.5,"d":"10.50"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":269,"d":"269.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKX32M435","PratiKa-priem.vidlica spojovacia-3P+N+E-32A 415 VAC-IP44-rýchloup. prip.",0]
["PKX16M733","VIDLICA SPOJOV. FC IP67 16A 415V 2P+E",1,"ks",{"v":14.720579999999998,"d":"14.721"},"3303432009571",{"v":7,"d":"7.00"},{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},{"v":217,"d":"217.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKX16M733","PratiKa-priem.vidlica spojovacia-2P+E-16A 415 VAC-IP67-rýchloup. prip.",""]
["PKN51B","ZÁSUVKA 50 BC IP54 16A 250V 2P+E FR BLUE",1,"ks",{"v":6.0858,"d":"6.086"},"3303432319977",{"v":6.3,"d":"6.30"},{"v":4.3,"d":"4.30"},{"v":5.1,"d":"5.10"},{"v":45,"d":"45.00"},"AT","3926909790","https://www.se.com/sk/sk/product/PKN51B","PratiKa-zás.1x2P+PE-10/16 A 250 VAC-50 x 50 mm-IP54-modrá-vstavaná montáž",0]
["PKF32W734","ZÁSUVKA NÁSTEN. SC IP67 32A 415V 3P+E",1,"ks",{"v":12.983039999999999,"d":"12.983"},"3303432417239",{"v":16.1,"d":"16.10"},{"v":10.4,"d":"10.40"},{"v":9.5,"d":"9.50"},{"v":330,"d":"330.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKF32W734","PratiKa-priem. zás. nástenná-3P+E-32 A 415 VAC-IP67-skrut. svorky",0]
["PKF32F723","ZÁSUVKA VSTAV.Š SC IP67 32A 250V 2P+E",1,"ks",{"v":10.583999999999998,"d":"10.584"},"3303432033163",{"v":10,"d":"10.00"},{"v":9.5,"d":"9.50"},{"v":9,"d":"9.00"},{"v":216,"d":"216.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKF32F723","PratiKa-priem.zás.vstavaná šikmá-2P+E-32 A 250 VAC-IP67-skrut. svorky",0]
["PKF16M735","ZÁSUVKA SPOJOV. SC IP67 16A 415V 3P+N+E",1,"ks",{"v":9.260999999999997,"d":"9.261"},"3303432032784",{"v":17,"d":"17.00"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":244,"d":"244.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKF16M735","PratiKa-priem.zás.spojovacia-3P+N+E-16 A 415 VAC-IP67-skrut. svorky",0]
["PKF16G434","ZÁSUVKA VSTAV.R SC IP44 16A 415V 3P+E",1,"ks",{"v":7.258859999999999,"d":"7.259"},"3303432033996",{"v":7,"d":"7.00"},{"v":8,"d":"8.00"},{"v":9,"d":"9.00"},{"v":140,"d":"140.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKF16G434","PratiKa-priem.zás.vstavaná rovná-3P+E-16 A 415 VAC-IP44-skrut. svorky",0]
["PKE32M435","VIDLICA SPOJOV. SC IP44 32A 415V 3P+N+E",1,"ks",{"v":9.260999999999997,"d":"9.261"},"3303432031978",{"v":17,"d":"17.00"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":250,"d":"250.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKE32M435","PratiKa-priem.vidlica spojovacia-3P+N+E-32 A 415 VAC-IP44-skrut. svorky",0]
["PKE16M435","VIDLICA SPOJOV. SC IP44 16A 415V 3P+N+E",1,"ks",{"v":6.879599999999999,"d":"6.880"},"3303432032142",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":182,"d":"182.00"},"IT","8536699099","https://www.se.com/sk/sk/product/PKE16M435","PratiKa-priem.vidlica spojovacia-3P+N+E-16 A 415 VAC-IP44-skrut. svorky",0]
["PAS600L","ESX Panel Server - Universal, 24V DC",1,"ks",{"v":628.4249999999998,"d":"628.425"},"3606481014320",{"v":11,"d":"11.00"},{"v":9,"d":"9.00"},{"v":8.5,"d":"8.50"},{"v":267,"d":"267.00"},"IN","8517620000","https://www.se.com/sk/sk/product/PAS600L","Bezdrôtový koncentátor a modbus brána, EcoStruxure Panel Server - universal, 24 VDC",0.03]
["OVA53174","Piktogramy pre Picto Screen pre Smartexi",1,"ks",{"v":25.334504999999993,"d":"25.335"},"3606481179883",{"v":33,"d":"33.00"},{"v":0.1,"d":"0.10"},{"v":17,"d":"17.00"},{"v":70,"d":"70.00"},"IT","39269097","https://www.se.com/sk/sk/product/OVA53174","Exiway Smartexit Dicube -piktogramy pre Picto Screen pre Smartexit 32m, 7ks",0]
["OVA51128","Exiway - batérie – 12 V 68 Ah",1,"ks",{"v":471.1328999999999,"d":"471.133"},"3606480699290",{"v":360,"d":"360.00"},{"v":200,"d":"200.00"},{"v":155,"d":"155.00"},{"v":21000,"d":"21,000.00"},"FR","8507208090","https://www.se.com/sk/sk/product/OVA51128","Exiway - batérie – 12 V 68 Ah",0]
["OVA48604","Exiway Smartexit DiCube 1.5h, 26m, IP40,",1,"ks",{"v":133.33949999999996,"d":"133.340"},"3606481179739",{"v":28,"d":"28.00"},{"v":7,"d":"7.00"},{"v":17.5,"d":"17.50"},{"v":828,"d":"828.00"},"IT","9405413990","https://www.se.com/sk/sk/product/OVA48604","Exiway Smartexit DiCube 1,5 h – 26 m – IP40 – trvalý režim",0]
["OVA48503","Exiway Smartled DiCube 3h, 180/180lm, tr",1,"ks",{"v":137.78414999999998,"d":"137.784"},"3606481179531",{"v":30,"d":"30.00"},{"v":12.7,"d":"12.70"},{"v":4.5,"d":"4.50"},{"v":660,"d":"660.00"},"IT","9405114090","https://www.se.com/sk/sk/product/OVA48503","Exiway Smartled DiCube 3 h – 180/180 lm – trvalý režim",0.1]
["OVA44115","Exiway Light, autotest 1-3h, 500 lm, IP6",1,"ks",{"v":66.22528499999999,"d":"66.225"},"3606481918161",{"v":23.2,"d":"23.20"},{"v":11.7,"d":"11.70"},{"v":4.3,"d":"4.30"},{"v":450,"d":"450.00"},"IT","9405114090","https://www.se.com/sk/sk/product/OVA44115","Núdzové svietidlo Exiway Light, autotest, 1 až 3 hodiny, až 500 lm, IP65, LiFePO4, LED",0.07]
["OVA44013","Exiway Light 1-3h, 250 lm, IP65 LED",1,"ks",{"v":40.44631499999999,"d":"40.446"},"3606481918086",{"v":23.5,"d":"23.50"},{"v":4.5,"d":"4.50"},{"v":12,"d":"12.00"},{"v":414,"d":"414.00"},"IT","9405114090","https://www.se.com/sk/sk/product/OVA44013","Núdzové svietidlo Exiway Light, 1 až 3 hodiny, až 250 lm, IP65, LiFePO4, LED",0.06]
["OVA38252","Exiway Easysign/IP40/24 m/3h",1,"ks",{"v":93.33764999999998,"d":"93.338"},"3606489729585",{"v":26,"d":"26.00"},{"v":3.1,"d":"3.10"},{"v":20,"d":"20.00"},{"v":610,"d":"610.00"},"IT","9405612090","https://www.se.com/sk/sk/product/OVA38252","Exiway Easysign / IP40 / Standard / 24 m / NM-M / 3h",0.09]
["NU986644","Záslepka 2 modul, Béžová",1,"ks",{"v":1.0538639999999997,"d":"1.054"},"3606481956002",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":4.5,"d":"4.50"},{"v":7,"d":"7.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU986644","Unica - Záslepka 2 modul, Béžová",0]
["NU986418","Záslepka 2x 1/2 modul, Biela",1,"ks",{"v":2.1077279999999994,"d":"2.108"},"3606489459130",{"v":4.5,"d":"4.50"},{"v":1.2,"d":"1.20"},{"v":1.5,"d":"1.50"},{"v":3,"d":"3.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU986418","Unica - Záslepka 2x 1/2 modul, Biela",0]
["NU946418","Cent. doska skos RJ45 Keystone, 2M,Biela",1,"ks",{"v":3.7324349999999993,"d":"3.732"},"3606489459017",{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU946418","Unica - centrálna doska skosená RJ45 Keystone, 2M, Biela",0]
["NU944154","Cent. doska pre TV-R/SAT zásuvku, Antr",1,"ks",{"v":4.6106549999999995,"d":"4.611"},"3606489458881",{"v":4.8,"d":"4.80"},{"v":0.7,"d":"0.70"},{"v":4.8,"d":"4.80"},{"v":7,"d":"7.00"},"ES","8538909999","https://www.se.com/sk/sk/product/NU944154","Unica - centrálna doska pre TV-R/SAT zásuvku, Antracit",0]
["NU941020","Cent. doska RJ45 S-ONE 1M, Antib",1,"ks",{"v":3.381146999999999,"d":"3.381"},"3606489467678",{"v":4.5,"d":"4.50"},{"v":2.4,"d":"2.40"},{"v":2.3,"d":"2.30"},{"v":8,"d":"8.00"},"ES","8538909999","https://www.se.com/sk/sk/product/NU941020","Unica - centrálna doska RJ45 S-ONE 1M, Biela Antibakteriálna",0]
["NU940618","Cent. doska skosená RJ45 S-ONE 1M, Biela",1,"ks",{"v":3.381146999999999,"d":"3.381"},"3606489467074",{"v":4.5,"d":"4.50"},{"v":2.3,"d":"2.30"},{"v":3.5,"d":"3.50"},{"v":8,"d":"8.00"},"ES","8538909999","https://www.se.com/sk/sk/product/NU940618","Unica - centrálna doska skosená RJ45 S-ONE 1M, Biela",0]
["NU910054","Náhradná klapka 1M, Antr",1,"ks",{"v":1.9320839999999997,"d":"1.932"},"3606489458652",{"v":4.5,"d":"4.50"},{"v":1,"d":"1.00"},{"v":2.3,"d":"2.30"},{"v":3,"d":"3.00"},"ES","8538909999","https://www.se.com/sk/sk/product/NU910054","Unica - Náhradná klapka 1M, Antracit",0]
["NU9091","Rychlospojka zásuvky CMS, sada 10ks",1,"ks",{"v":53.13230999999999,"d":"53.132"},"3606489458577",{"v":14.7,"d":"14.70"},{"v":4.7,"d":"4.70"},{"v":11.8,"d":"11.80"},{"v":81,"d":"81.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU9091","Unica - Rychlospojka pre multizásuvky CMS, sada 10ks",0]
["NU7802","Ochranný kryt pre maľovanie",1,"ks",{"v":0.5269319999999998,"d":"0.527"},"3606489458317",{"v":8,"d":"8.00"},{"v":1.5,"d":"1.50"},{"v":7.2,"d":"7.20"},{"v":3,"d":"3.00"},"ES","3926909790","https://www.se.com/sk/sk/product/NU7802","Unica - Ochranný kryt pre maľovanie",0]
["NU553130","KNX Unica tlačidlo 2-nás., alumínium",1,"ks",{"v":85.33727999999998,"d":"85.337"},"3606489699802",{"v":9.5,"d":"9.50"},{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":118,"d":"118.00"},"DE","8536508090","https://www.se.com/sk/sk/product/NU553130","KNX Unica tlačidlo 2-nás., alumínium",0]
["NU501418","Nabíjací konektor USB C (65W), Biela",1,"ks",{"v":67.62293999999999,"d":"67.623"},"3606482068889",{"v":7.5,"d":"7.50"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":135,"d":"135.00"},"CN","8504408390","https://www.se.com/sk/sk/product/NU501418","Unica - nabíjací konektor USB C (65W), Biela",0]
["NU386244","Káblová vývodka, 2M, Béžová",1,"ks",{"v":3.9080789999999994,"d":"3.908"},"3606481955531",{"v":4.5,"d":"4.50"},{"v":4.6,"d":"4.60"},{"v":4.5,"d":"4.50"},{"v":22,"d":"22.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU386244","Unica - Káblová vývodka, 2M, Béžová",0]
["NU3773","Signálne svetlo 12-24V, 2M",1,"ks",{"v":65.86649999999999,"d":"65.867"},"3606489456269",{"v":8.5,"d":"8.50"},{"v":6.3,"d":"6.30"},{"v":8,"d":"8.00"},{"v":61,"d":"61.00"},"ES","8538909999","https://www.se.com/sk/sk/product/NU3773","Unica - Signálne svetlo 12-24V, 2M",0]
["NU354054","Elektronický spínač hotelovej karty,Antr",1,"ks",{"v":58.40162999999998,"d":"58.402"},"3606481955388",{"v":8.6,"d":"8.60"},{"v":6.1,"d":"6.10"},{"v":8.1,"d":"8.10"},{"v":83,"d":"83.00"},"LV","8536508090","https://www.se.com/sk/sk/product/NU354054","Unica - Elektronický spínač hotelovej karty, Antracit",0]
["NU351420","Stmievač otočný univ. LED 5-200W, Antib",1,"ks",{"v":77.72246999999997,"d":"77.722"},"3606485445625",{"v":9.7,"d":"9.70"},{"v":8.2,"d":"8.20"},{"v":9.7,"d":"9.70"},{"v":107,"d":"107.00"},"LV","8536508090","https://www.se.com/sk/sk/product/NU351420","Unica - Stmievač otočný univerzálny LED 5-200W, Biely Antibakteriálny",0]
["NU349730","Zásuvka telefónna RJ12, Alu",1,"ks",{"v":8.782199999999998,"d":"8.782"},"3606489467050",{"v":4.5,"d":"4.50"},{"v":3.4,"d":"3.40"},{"v":4.5,"d":"4.50"},{"v":16,"d":"16.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU349730","Unica - Zásuvka telefónna RJ12, 6 kontaktov, Aluminium",0]
["NU348744","Svorky reproduktorové 1M, Béžová",1,"ks",{"v":5.664518999999999,"d":"5.665"},"3606481955289",{"v":3.2,"d":"3.20"},{"v":4.5,"d":"4.50"},{"v":2.2,"d":"2.20"},{"v":13,"d":"13.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU348744","Unica - Svorky reproduktorové 1M, Béžová",0]
["NU346830","Zásuvka TV F-konektor 1M, Alu",1,"ks",{"v":4.961943,"d":"4.962"},"3606489456054",{"v":4.5,"d":"4.50"},{"v":2.2,"d":"2.20"},{"v":4,"d":"4.00"},{"v":12,"d":"12.00"},"ES","8536691000","https://www.se.com/sk/sk/product/NU346830","Unica - Zásuvka TV F-konektor 1M, Aluminium",0]
["NU346120","Zásuvka TV individuálna 1,5 dB 1M, Antib",1,"ks",{"v":10.099529999999996,"d":"10.100"},"3606489467852",{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":2.3,"d":"2.30"},{"v":42,"d":"42.00"},"ES","8536691000","https://www.se.com/sk/sk/product/NU346120","Unica - Zásuvka TV individuálna 1,5 dB 1M, Biela Antibakteriálna",0]
["NU345154","Zásuvka TV/R indiv., 11 dB, 2M, Antr",1,"ks",{"v":15.807959999999996,"d":"15.808"},"3606489467258",{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":63,"d":"63.00"},"ES","8536691000","https://www.se.com/sk/sk/product/NU345154","Unica - Zásuvka TV/R individuálna, 11 dB, 2M, Antracit",0]
["NU343318","Mini jack audio 3,5mm konektor, 1M,Biely",1,"ks",{"v":15.807959999999996,"d":"15.808"},"3606489456016",{"v":12,"d":"12.00"},{"v":2.5,"d":"2.50"},{"v":12,"d":"12.00"},{"v":21,"d":"21.00"},"FR","8536699099","https://www.se.com/sk/sk/product/NU343318","Unica - Mini jack audio 3,5 mm konektor, 1M, Biely",0]
["NU343154","3 RCA konektory (video&audio), 1M, Antr",1,"ks",{"v":52.69319999999998,"d":"52.693"},"3606489455972",{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":6.5,"d":"6.50"},{"v":21,"d":"21.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU343154","Unica - 3 RCA konektory (video & audio), 1M, Antracit",0]
["NU341854","Dvojitý nabíjací USB A+A 2.1A, 2M, Antr",1,"ks",{"v":37.32434999999999,"d":"37.324"},"3606489455859",{"v":4.5,"d":"4.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":53,"d":"53.00"},"CN","8504408390","https://www.se.com/sk/sk/product/NU341854","Unica - Dvojitý nabíjací USB A+A konektor 2.1A, 2M, Antracit",0]
["NU341818","Dvojitý nabíjací USB A+A 2.1A, 2M, Biely",1,"ks",{"v":30.29858999999999,"d":"30.299"},"3606489455835",{"v":4.5,"d":"4.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":51,"d":"51.00"},"CN","8504408390","https://www.se.com/sk/sk/product/NU341818","Unica - Dvojitý nabíjací USB A+A konektor 2.1A, 2M, Biely",0]
["NU341154","Zásuvka 1xRJ45 Kat.5e UTP, 2M, Antr",1,"ks",{"v":10.977749999999999,"d":"10.978"},"3606489467142",{"v":4.5,"d":"4.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":17,"d":"17.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU341154","Unica - Zásuvka dátová 1xRJ45 Kat.5e UTP, 2M, Antracit",0]
["NU326354","Prepínač striedavý r.6, 2M, 16A, Antr",1,"ks",{"v":10.099529999999996,"d":"10.100"},"3606489455798",{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":22,"d":"22.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU326354","Unica - Prepínač striedavý radenie 6, 2M, 16A, Antracit",0]
["NU326254","Spínač dvojpólový r.2, 16A, 2M, Antr",1,"ks",{"v":10.538639999999997,"d":"10.539"},"3606489455750",{"v":4.5,"d":"4.50"},{"v":3.8,"d":"3.80"},{"v":4.5,"d":"4.50"},{"v":23,"d":"23.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU326254","Unica - Spínač dvojpólový radenie 2, 16A, 2M, Antracit",0]
["NU323244S","Spínač dvojpólový 32A s kontrolkou, Béž",1,"ks",{"v":15.807959999999996,"d":"15.808"},"3606481955012",{"v":4.5,"d":"4.50"},{"v":4.6,"d":"4.60"},{"v":4.5,"d":"4.50"},{"v":47,"d":"47.00"},"IN","8536508090","https://www.se.com/sk/sk/product/NU323244S","Unica - Spínač dvojpólový 32A s kontrolkou, Béžový",0]
["NU321130","Prepínač sériový r.5, Alu",1,"ks",{"v":8.782199999999998,"d":"8.782"},"3606481064042",{"v":4.5,"d":"4.50"},{"v":3.2,"d":"3.20"},{"v":4.5,"d":"4.50"},{"v":30,"d":"30.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU321130","Unica - Prepínač sériový radenie 5, Aluminium",0]
["NU320730","Žalúziový tlačidlový ovl 6A, 2M, Alu",1,"ks",{"v":13.612409999999995,"d":"13.612"},"3606489455439",{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"v":38,"d":"38.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU320730","Unica - Žalúziový tlačidlový ovládač 6A, 2M, Aluminium",0]
["NU320620","Tlačidlo r.1/0, 2M, Antib",1,"ks",{"v":5.8401629999999995,"d":"5.840"},"3606489455286",{"v":4.5,"d":"4.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":19,"d":"19.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU320620","Unica - Tlačidlo radenie 1/0, 2M, Biele Antibakteriálne",0]
["NU320544","Prepínač krížový r.7, 2M, Béžový",1,"ks",{"v":7.816157999999999,"d":"7.816"},"3606481954909",{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":22,"d":"22.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU320544","Unica - Prepínač krížový radenie 7, 2M, Béžový",0]
["NU320154","Spínač jednopólový r.1, 2M, Antr",1,"ks",{"v":6.059717999999998,"d":"6.060"},"3606489455057",{"v":4.5,"d":"4.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":23,"d":"23.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU320154","Unica - Spínač jednopólový radenie 1, 2M, Antracit",0]
["NU316354","Prepínač striedavý r.6, 16A, 1M, Antr",1,"ks",{"v":10.099529999999996,"d":"10.100"},"3606489455026",{"v":4.5,"d":"4.50"},{"v":2.3,"d":"2.30"},{"v":3.5,"d":"3.50"},{"v":20,"d":"20.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU316354","Unica - Prepínač striedavý radenie 6, 16A, 1M, Antracit",0]
["NU310830SC","Žalúziový spínač 10A, 1M, Alu",1,"ks",{"v":13.173299999999996,"d":"13.173"},"3606481954725",{"v":4.5,"d":"4.50"},{"v":2,"d":"2.00"},{"v":3.5,"d":"3.50"},{"v":26,"d":"26.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU310830SC","Unica - Žalúziový spínač 10A, 1M, Aluminium",0]
["NU310654N","Tlačidlo orient. r.1/0So, 1M, Antr",1,"ks",{"v":11.416859999999996,"d":"11.417"},"3606489454937",{"v":6,"d":"6.00"},{"v":2.5,"d":"2.50"},{"v":5,"d":"5.00"},{"v":18,"d":"18.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU310654N","Unica - Tlačidlo s orientačnou kontrolkou radenie 1/0So, 1M, Antracit",0]
["NU310530","Prepínač krížový r.7, 1M, Alu",1,"ks",{"v":9.221309999999999,"d":"9.221"},"3606489454760",{"v":4.5,"d":"4.50"},{"v":2.3,"d":"2.30"},{"v":3.8,"d":"3.80"},{"v":21,"d":"21.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU310530","Unica - Prepínač krížový radenie 7, 1M, Aluminium",0]
["NU310344","Prepínač striedavý r.6, 1M, Béžový",1,"ks",{"v":5.137586999999998,"d":"5.138"},"3606481954572",{"v":4.5,"d":"4.50"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":17,"d":"17.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NU310344","Unica - Prepínač striedavý radenie 6, 1M, Béžový",0]
["NU307930","Zásuvka trojitá 45º 250V/16A, Alu",1,"ks",{"v":17.125289999999996,"d":"17.125"},"3606489454623",{"v":13.5,"d":"13.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":106,"d":"106.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU307930","Unica - Zásuvka trojitá 45º 250V/16A 3x2P+E, clonky, bezskrútková, Aluminium",0]
["NU305920","Zásuvka 250V/16A bezskrút., Antib",1,"ks",{"v":5.313230999999998,"d":"5.313"},"3606489454265",{"v":4.5,"d":"4.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":30,"d":"30.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU305920","Unica - Zásuvka 250V/16A 2P+E, clonky, bezskrútková, Biela Antibakteriálna",0]
["NU305744","Zásuvka SCHUKO 250V/16A, bezskrút., Béž",1,"ks",{"v":5.664518999999999,"d":"5.665"},"3606481954336",{"v":4.5,"d":"4.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":31,"d":"31.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU305744","Unica - Zásuvka SCHUKO 2P+E 250V/16A, clonky, bezskrútková, Béžová",0]
["NU304918","Zásuvka 45º 250V/16A bezskrút., Biela",1,"ks",{"v":4.4350109999999985,"d":"4.435"},"3606489454029",{"v":3.8,"d":"3.80"},{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"v":32,"d":"32.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU304918","Unica - Zásuvka 45º 250V/16A 2P+E, clonky, bezskrútková, Biela",0]
["NU303744","Zásuvka SCHUKO 250V/16A, skrút., Béžová",1,"ks",{"v":5.664518999999999,"d":"5.665"},"3606481954138",{"v":4.5,"d":"4.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":34,"d":"34.00"},"ES","8536699099","https://www.se.com/sk/sk/product/NU303744","Unica - Zásuvka SCHUKO 2P+E 250V/16A, clonky, skrútková, Béžová",0]
["NU301818","Nabíjací USB A+C 2.4A, 2M, Biely",1,"ks",{"v":33.81146999999999,"d":"33.811"},"3606489516833",{"v":4.5,"d":"4.50"},{"v":3.9,"d":"3.90"},{"v":4.5,"d":"4.50"},{"v":54,"d":"54.00"},"CN","8504408390","https://www.se.com/sk/sk/product/NU301818","Unica - Dvojitý nabíjací USB konektor A+C 2.4A, 2M, Biely",0]
["NU280821","Rámček Color 4násobný, Dark grey/Biely",1,"ks",{"v":11.855969999999996,"d":"11.856"},"3606489453602",{"v":29.8,"d":"29.80"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":67,"d":"67.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU280821","Unica Studio Color - Krycí rámček štvornásobný, Dark grey/Biely",0]
["NU280817","Rámček Color 4násobný, Chocolate/Čierny",1,"ks",{"v":11.855969999999996,"d":"11.856"},"3606489453589",{"v":30,"d":"30.00"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":67,"d":"67.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU280817","Unica Studio Color - Krycí rámček štvornásobný, Chocolate/Čierny",0]
["NU280617","Rámček Color 3násobný, Chocolate/Čierny",1,"ks",{"v":8.782199999999998,"d":"8.782"},"3606489453329",{"v":23,"d":"23.00"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":50,"d":"50.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU280617","Unica Studio Color - Krycí rámček trojnásobný, Chocolate/Čierny",0]
["NU280452M","Rámček Metal 2násobný, Bronze/Čierny",1,"ks",{"v":14.929739999999997,"d":"14.930"},"3606482073913",{"v":15.6,"d":"15.60"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":35,"d":"35.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU280452M","Unica Studio Metal - Krycí rámček dvojnásobný, Bronze/Čierny",0]
["NU280414","Rámček Color 2násobný, Plum/Biely",1,"ks",{"v":6.059717999999998,"d":"6.060"},"3606489453039",{"v":15.5,"d":"15.50"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":36,"d":"36.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU280414","Unica Studio Color - Krycí rámček dvojnásobný, Plum/Biely",0]
["NU280228","Rámček Color 1násobný, Taupe/Čierny",1,"ks",{"v":3.2055029999999993,"d":"3.206"},"3606489452872",{"v":8.8,"d":"8.80"},{"v":1,"d":"1.00"},{"v":8.8,"d":"8.80"},{"v":21,"d":"21.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU280228","Unica Studio Color - Krycí rámček jednonásobný, Taupe/Čierny",0]
["NU230418","Rámček Outline dvojnásobný, Biely",1,"ks",{"v":2.0638169999999993,"d":"2.064"},"3606481953124",{"v":15.5,"d":"15.50"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":23,"d":"23.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU230418","Unica Studio Outline - Rámček dvojnásobný, Biely",0]
["NU230014","Dekorativný rámček Outline, Plum",1,"ks",{"v":1.2295079999999996,"d":"1.230"},"3606481953032",{"v":5,"d":"5.00"},{"v":0.5,"d":"0.50"},{"v":5,"d":"5.00"},{"v":2,"d":"2.00"},"ES","3925902000","https://www.se.com/sk/sk/product/NU230014","Unica Studio Outline - Dekorativný rámček, Plum",0]
["NU200844","Rámček Studio štvornásobný, Béžový",1,"ks",{"v":4.039811999999999,"d":"4.040"},"3606489452469",{"v":29.5,"d":"29.50"},{"v":1.5,"d":"1.50"},{"v":8,"d":"8.00"},{"v":45,"d":"45.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU200844","Unica Studio - Krycí rámček štvornásobný, Béžový",0]
["NU200130","Rámček Studio úzky 1M, Alu",1,"ks",{"v":4.786299,"d":"4.786"},"3606489452308",{"v":7.5,"d":"7.50"},{"v":1.5,"d":"1.50"},{"v":3.5,"d":"3.50"},{"v":14,"d":"14.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU200130","Unica Studio - Krycí rámček úzký 1M, Alu",0]
["NU171030","Centr. jedn. 2x10 mod. zapustená, Alu",1,"ks",{"v":69.37937999999998,"d":"69.379"},"3606481812773",{"v":31.5,"d":"31.50"},{"v":8,"d":"8.00"},{"v":18,"d":"18.00"},{"v":776,"d":"776.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU171030","Unica System+ - Centrálna jednotka 2x10 modulov zapustená, Aluminium",0]
["NU122454","Centr. jedn. 2x4 mod. vert. povr., Antr",1,"ks",{"v":30.29858999999999,"d":"30.299"},"3606489452117",{"v":18.5,"d":"18.50"},{"v":8,"d":"8.00"},{"v":18,"d":"18.00"},{"v":464,"d":"464.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NU122454","Unica System+ - Centrálna jednotka 2x4 moduly vertikálna povrchová, Antracit",0]
["NSYZZ554G","RAL7035 SOKEL ZZ 535X410X500 PRE PLAZ(T)",1,"ks",{"v":539.8942499999999,"d":"539.894"},"3606480778124",{"v":56,"d":"56.00"},{"v":13,"d":"13.00"},{"v":73,"d":"73.00"},{"v":13000,"d":"13,000.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NSYZZ554G","7035 sokel ZZ 535x410x500 na PLAZ(T)",0]
["NSYZZ2124G","7035 SOKEL ZZ 1285X410X200 PRE PLAZ(T)",1,"ks",{"v":416.35912499999995,"d":"416.359"},"3606480726309",{"v":129,"d":"129.00"},{"v":9,"d":"9.00"},{"v":46,"d":"46.00"},{"v":9950,"d":"9,950.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NSYZZ2124G","7035 sokel ZZ 1285x410x200 na PLAZ(T)",0]
["NSYZHPLA53G","7035 THAL.POLYEST.SOKEL 500X320 V.900",1,"ks",{"v":425.5098749999999,"d":"425.510"},"3606480777875",{"v":96.5,"d":"96.50"},{"v":11,"d":"11.00"},{"v":86,"d":"86.00"},{"v":16888,"d":"16,888.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NSYZHPLA53G","7035 sokel 500x320x900 na PLAZ(T)",0]
["NSYZA253G","7035 THAL.POLYEST.SOKEL 200X494X250",1,"ks",{"v":242.494875,"d":"242.495"},"3606480777752",{"v":53,"d":"53.00"},{"v":16,"d":"16.00"},{"v":21.5,"d":"21.50"},{"v":5050,"d":"5,050.00"},"ES","3925901000","https://www.se.com/sk/sk/product/NSYZA253G","7035 Sokel ZA 494x250x200 na PLA(T)",0]
["NSYVA272M","PLAST. OKNO PRE MOD. PRÍSTROJE 78X60x15",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3606480185274",{"v":8,"d":"8.00"},{"v":2.5,"d":"2.50"},{"v":8,"d":"8.00"},{"v":50,"d":"50.00"},"ES","85389099","https://www.se.com/sk/sk/product/NSYVA272M","plastové okno s priehľadným krytom IP 65 - L78xŠ60xH15mm.",0]
["NSYUCC270","27CM OTV. SPOJOVACIA SADA PLS",10,"ks",{"v":6.268263749999999,"d":"6.268"},"3606480190032",{"v":12.1,"d":"12.10"},{"v":24,"d":"24.00"},{"v":33.6,"d":"33.60"},{"v":218,"d":"218.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYUCC270","Half open coupling frame length200mm for 27cm faces of PLS box",0]
["NSYTVR7","SADA 2 VERT.PRÁZD.NOSNÍKOV V.750",1,"ks",{"v":39.80576249999999,"d":"39.806"},"3606480185083",{"v":63,"d":"63.00"},{"v":3.5,"d":"3.50"},{"v":6,"d":"6.00"},{"v":1886,"d":"1,886.00"},"IT","8538100000","https://www.se.com/sk/sk/product/NSYTVR7","2 zvislé stĺpy výšky 750mm. pozink. ocel.",0]
["NSYTT8CRN","THAL. VLOŽKA DO TROJH.ZÁMKU 8MM",1,"ks",{"v":5.62771125,"d":"5.628"},"3606480185007",{"v":13,"d":"13.00"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":84,"d":"84.00"},"FR","8301600090","https://www.se.com/sk/sk/product/NSYTT8CRN","trojuholníková vložka 8mm - chrom. pre Spacial CRN a Thalassa PLM",0]
["NSYTRV62TTD","SVORKA RADOVÁ MERACIA ROZPOJ. 6MM2",50,"ks",{"v":11.5171875,"d":"11.517"},"3606480532399",{"v":27,"d":"27.00"},{"v":5,"d":"5.00"},{"v":7,"d":"7.00"},{"v":28.2,"d":"28.20"},"PL","8536901000","https://www.se.com/sk/sk/product/NSYTRV62TTD","Linergy šróbová svorka - meriaca rozpojovacia - 6mm²",0]
["NSYTRV42WH","SVORKA RADOVÁ 4MM2, BIELA",50,"ks",{"v":1.2993750000000002,"d":"1.299"},"3606480531958",{"v":25,"d":"25.00"},{"v":5,"d":"5.00"},{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},"CN","8536901000","https://www.se.com/sk/sk/product/NSYTRV42WH","Linergy šróbová svorka - 2 body - 4mm² biela",0]
["NSYTRV352PE","SVORKA RADOVÁ ZEMN. 25MM2",50,"ks",{"v":12.99375,"d":"12.994"},"3606480532177",{"v":28,"d":"28.00"},{"v":9.5,"d":"9.50"},{"v":18,"d":"18.00"},{"v":85,"d":"85.00"},"TR","8536901000","https://www.se.com/sk/sk/product/NSYTRV352PE","Linergy šróbová svorka - zemniaca - 2 body - 35mm²",0]
["NSYTRV162BL","SVORKA RADOVÁ 16MM2, MODRÁ",50,"ks",{"v":4.4296875,"d":"4.430"},"3606480532139",{"v":36,"d":"36.00"},{"v":9.5,"d":"9.50"},{"v":11.5,"d":"11.50"},{"v":29,"d":"29.00"},"TR","8536901000","https://www.se.com/sk/sk/product/NSYTRV162BL","Linergy šróbová svorka - 2 body - 16mm² modrá",0]
["NSYTRR22","SVORKA RADOVÁ PRUŽ.2BODY 2,5MM2 SIVÁ",50,"ks",{"v":1.2993750000000002,"d":"1.299"},"3606480532504",{"v":4.9,"d":"4.90"},{"v":0.5,"d":"0.50"},{"v":3.5,"d":"3.50"},{"v":5.6,"d":"5.60"},"DE","8536901000","https://www.se.com/sk/sk/product/NSYTRR22","Linergy pružinová svorka - 2 body - 2,5mm² šedá",0]
["NSYTRASB4","DRŽIAK ZNAČENIA SVORIEK",100,"ks",{"v":0.7087499999999999,"d":"0.709"},"3606480534515",{"v":2.5,"d":"2.50"},{"v":1,"d":"1.00"},{"v":2.2,"d":"2.20"},{"v":0.4,"d":"0.40"},"DE","3926909790","https://www.se.com/sk/sk/product/NSYTRASB4","NSYTR držiak označenia svoriek pre krytku",0]
["NSYTRAL210","PREPOJKA 10 BODOV PRE 2,5 MM2",10,"ks",{"v":4.9021875,"d":"4.902"},"3606480534096",{"v":17,"d":"17.00"},{"v":5,"d":"5.00"},{"v":15,"d":"15.00"},{"v":8,"d":"8.00"},"DE","8536901000","https://www.se.com/sk/sk/product/NSYTRAL210","NSYTR prepoj. mostík 10 bodov pre 2,5mm² svorku",0]
["NSYTRAFTYE","Test adapter zamykací žltý",10,"ks",{"v":2.953125,"d":"2.953"},"3606480534454",5.33,0.76,0.76,{"v":2,"d":"2.00"},"PL","3926909790","https://www.se.com/sk/sk/product/NSYTRAFTYE","NSYTR test adapter zamykací žlutý",0]
["NSYTRABPV5","KARTA PRÁZDNYCH ŠTÍTKOV, 6 PÁSIKOV 5MM",10,"ks",{"v":9.272812499999999,"d":"9.273"},"3606480534805",{"v":12.5,"d":"12.50"},{"v":5,"d":"5.00"},{"v":8,"d":"8.00"},{"v":15,"d":"15.00"},"PL","3926909790","https://www.se.com/sk/sk/product/NSYTRABPV5","označovacia karta - 5mm nepotlačená - 72 znakov",0]
["NSYTRAB550","ZNAČENIE SVORIEK 41-50",10,"ks",{"v":1.18125,"d":"1.181"},"3606480534737",{"v":14,"d":"14.00"},{"v":1,"d":"1.00"},{"v":14,"d":"14.00"},{"v":1.3,"d":"1.30"},"DE","3926909790","https://www.se.com/sk/sk/product/NSYTRAB550","označovací pásik - 5mm 10 znakov 41 až 50",0]
["NSYTPLSC3654G","7035 KRYT PC PLS 36X54X4.5",1,"ks",{"v":48.041437499999994,"d":"48.041"},"3606480777547",{"v":38,"d":"38.00"},{"v":6,"d":"6.00"},{"v":56,"d":"56.00"},{"v":905,"d":"905.00"},"ES","3926909790","https://www.se.com/sk/sk/product/NSYTPLSC3654G","Opaque polycarbonate cover 36x54x4.5cm",0]
["NSYTPLS5454","PRIEHĽ. KRYT PLS 54X54X4. 5",1,"ks",{"v":37.518074999999996,"d":"37.518"},"3606480189791",{"v":54,"d":"54.00"},{"v":5,"d":"5.00"},{"v":54,"d":"54.00"},{"v":1560,"d":"1,560.00"},"ES","3926909790","https://www.se.com/sk/sk/product/NSYTPLS5454","Transparent polycarbonate cover 54x54x4.5cm",0]
["NSYTLG2FL","KÁBLOVÝ VSTUP 495X220",1,"ks",{"v":27.909787499999997,"d":"27.910"},"3606480168284",{"v":50,"d":"50.00"},{"v":0.5,"d":"0.50"},{"v":24,"d":"24.00"},{"v":1038,"d":"1,038.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYTLG2FL","S3D príruba s výrezom pre membránu pre rozv. RAL7035. L495xW220",0]
["NSYTLDFL","KÁBL.VSTUP MEMBRÁNA 345x130",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3606480168413",{"v":35.2,"d":"35.20"},{"v":1.2,"d":"1.20"},{"v":13.9,"d":"13.90"},{"v":398,"d":"398.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYTLDFL","káblová vstupná membrána pre S3D rozv. RAL7035. D345xŠ130.",0]
["NSYTK1","THAL. PODLOŽKA POD ZÁMOK",1,"ks",{"v":10.065825,"d":"10.066"},"3606480199110",{"v":13,"d":"13.00"},{"v":3,"d":"3.00"},{"v":12,"d":"12.00"},{"v":76,"d":"76.00"},"FR","8301409000","https://www.se.com/sk/sk/product/NSYTK1","THAL. PODLOŽKA POD ZÁMOK",0]
["NSYTJ4020","3D STRIEŠKA 400X200",1,"ks",{"v":64.51278749999999,"d":"64.513"},"3606480198793",{"v":42,"d":"42.00"},{"v":5,"d":"5.00"},{"v":24,"d":"24.00"},{"v":1593,"d":"1,593.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYTJ4020","Spacial S3D strecha skrine Š400xH200- farba - RAL7035.. vrátene upevnenia",0]
["NSYTHL2433APLM","THAL. RUKOVÄŤ SO ZÁMKOM KĽ.2433A",1,"ks",{"v":8.372936249999999,"d":"8.373"},"3606480192807",{"v":10,"d":"10.00"},{"v":3,"d":"3.00"},{"v":15,"d":"15.00"},{"v":100,"d":"100.00"},"FR","8301409000","https://www.se.com/sk/sk/product/NSYTHL2433APLM","rukoväť so zámkom - kľúč 2433A",0]
["NSYTFPCRN4","PRIEČNA LIŠTA NA DVERE 400MM",1,"ks",{"v":45.75375,"d":"45.754"},"3606480184901",{"v":3,"d":"3.00"},{"v":34,"d":"34.00"},{"v":6,"d":"6.00"},{"v":340,"d":"340.00"},"FR","8538100000","https://www.se.com/sk/sk/product/NSYTFPCRN4","sada 2 dverových priečnikov pre nástenné rozvodnice - šírka 400mm",0]
["NSYTCM274","SADA 2 KRÍDL. SKRUTIEK",1,"ks",{"v":2.7909787499999994,"d":"2.791"},"3606480189609",{"v":10,"d":"10.00"},{"v":1.5,"d":"1.50"},{"v":10,"d":"10.00"},{"v":50,"d":"50.00"},"ES","7318155890","https://www.se.com/sk/sk/product/NSYTCM274","sada 4 krídlových uzamyk. šróbov pre skrinku PLS",0]
["NSYTC12100","ŠPIRÁL. CHRÁNIČKA 50M",1,"ks",{"v":521.5927499999999,"d":"521.593"},"3606480184512",{"v":20,"d":"20.00"},{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":2570,"d":"2,570.00"},"FR","3926909790","https://www.se.com/sk/sk/product/NSYTC12100","držiak pre káble sťahovacia špirála balenie: 1ks=50m",0]
["NSYTBS241910HT","ABS KRABICA 241X192X105 TRANSP VYS.VEKO",1,"ks",{"v":28.824862499999995,"d":"28.825"},"3606480165504",{"v":25.5,"d":"25.50"},{"v":12,"d":"12.00"},{"v":20.5,"d":"20.50"},{"v":720,"d":"720.00"},"HU","9403700000","https://www.se.com/sk/sk/product/NSYTBS241910HT","skrin. ABS IP66 IK07 RAL7035 vnút.V275Š225H80 vonk.V291Š241H88 priehľ.kryt V20",0]
["NSYTBS19168T","ABS KRABICA 192X164X87 TRANSP VEKO",1,"ks",{"v":22.419337499999997,"d":"22.419"},"3606480165467",{"v":20.5,"d":"20.50"},{"v":10,"d":"10.00"},{"v":17,"d":"17.00"},{"v":467,"d":"467.00"},"HU","9403700000","https://www.se.com/sk/sk/product/NSYTBS19168T","skrin. ABS IP66 IK07 RAL7035 vnút.V175Š150H80 vonk.V193Š164H87 priehľ.kryt V20",0]
["NSYTBP342916H","PC KRABICA 341X291X168 VYS. VEKO",1,"ks",{"v":86.93212499999998,"d":"86.932"},"3606480165771",{"v":36,"d":"36.00"},{"v":18.5,"d":"18.50"},{"v":30,"d":"30.00"},{"v":1906,"d":"1,906.00"},"HU","3925908000","https://www.se.com/sk/sk/product/NSYTBP342916H","Thalassa - krabica 341x291x168 PC",0]
["NSYTBP241910HT","PC PRIEM. KRAB. 241X192X105 VYSOKÉ VEKO",1,"ks",{"v":48.956512499999995,"d":"48.957"},"3606480165863",{"v":24.1,"d":"24.10"},{"v":10.5,"d":"10.50"},{"v":19.4,"d":"19.40"},{"v":772,"d":"772.00"},"HU","3925908000","https://www.se.com/sk/sk/product/NSYTBP241910HT","Thalassa - krabica 241x194x107 PC - priehladné veko",0]
["NSYTBP191610H","PC KRABICA 192X164X105 VYS. VEKO",1,"ks",{"v":30.655012499999998,"d":"30.655"},"3606480165672",21.08,12.45,17.02,{"v":1240,"d":"1,240.00"},"HU","3925908000","https://www.se.com/sk/sk/product/NSYTBP191610H","Thalassa - krabica 192x164x105 PC",0]
["NSYTBC385","PRÍPOJNICOVÁ NADSTAVBA 300X800X500",1,"ks",878.472,"3606480068119",{"v":82,"d":"82.00"},{"v":15,"d":"15.00"},{"v":52,"d":"52.00"},{"v":27368,"d":"27,368.00"},"FR","85381000","https://www.se.com/sk/sk/product/NSYTBC385","Spacial SF horné prípojnicové pole - IP55 - 300x800x500 mm",0]
["NSYTBC3128","PRÍPOJNICOVÁ NADSTAVBA 300X1200X800",1,"ks",{"v":1555.6274999999998,"d":"1555.628"},"3606480068027",{"v":121.5,"d":"121.50"},{"v":12.5,"d":"12.50"},{"v":81.5,"d":"81.50"},{"v":26600,"d":"26,600.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYTBC3128","Spacial SF horné prípojnicové pole - IP55 - 300x1200x800 mm",0]
["NSYSUCR9080","2 UNIV. LIŠTY 3 RADOVÁ S 800",1,"ks",{"v":69.0881625,"d":"69.088"},"3606485133690",71.12,{"v":5.842,"d":"5.84"},{"v":9.652,"d":"9.65"},{"v":2182,"d":"2,182.00"},"EG","85381000","https://www.se.com/sk/sk/product/NSYSUCR9080","Spacial SF/SM - 2 univerzálne priečniky - 3 rady - d.800",0]
["NSYSUCR65140","2 UNIV. LIŠTY 2 RADOVÁ S 1400",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3606485133454",{"v":130.5,"d":"130.50"},{"v":6,"d":"6.00"},{"v":7.5,"d":"7.50"},{"v":3278,"d":"3,278.00"},"EG","7326909890","https://www.se.com/sk/sk/product/NSYSUCR65140","Spacial SF/SM - 2 univerzálne priečniky - 2 rady - d.1400",0]
["NSYSUCR4050","2 UNIV. LIŠTY 1 RADOVÁ 500",1,"ks",{"v":40.720837499999995,"d":"40.721"},"3606485133386",{"v":41,"d":"41.00"},{"v":5,"d":"5.00"},{"v":6,"d":"6.00"},{"v":940,"d":"940.00"},"EG","7326909890","https://www.se.com/sk/sk/product/NSYSUCR4050","Spacial SF/SM - 2 univerzálne priečniky - 1 rada - d.500",0]
["NSYSTMP8260","PERF. MP 825 SKRIŇA 600",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3606485133232",{"v":82.5,"d":"82.50"},{"v":2.5,"d":"2.50"},{"v":51,"d":"51.00"},{"v":3826,"d":"3,826.00"},"IT","7326909890","https://www.se.com/sk/sk/product/NSYSTMP8260","Spacial SF/SM perforovaný montážny panel - 600 mm",0]
["NSYSTMP60120","PERF. MP 600 SKRIŇA 1200",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3606485133188",{"v":111,"d":"111.00"},{"v":3,"d":"3.00"},{"v":60.5,"d":"60.50"},{"v":5200,"d":"5,200.00"},"IT","7326909890","https://www.se.com/sk/sk/product/NSYSTMP60120","Spacial SF/SM perforovaný montážny panel - 1200 mm",0]
["NSYST30M6S","SAMOREZNÁ TORX SKRUTKA T30 (M6X12)",100,"ks",{"v":0.41178375,"d":"0.412"},"3606480146817",{"v":2,"d":"2.00"},{"v":1.2,"d":"1.20"},{"v":1.2,"d":"1.20"},{"v":5.1,"d":"5.10"},"ES","7318149190","https://www.se.com/sk/sk/product/NSYST30M6S","samorez. Torx šrób M6x12mm + podložkac. množ.: 100 jednotiek",0]
["NSYSQCR90100","2 PRIEČNIKY 3 RADY 1000",1,"ks",{"v":77.781375,"d":"77.781"},"3606485132747",{"v":9.5,"d":"9.50"},{"v":98,"d":"98.00"},{"v":6.5,"d":"6.50"},{"v":2650,"d":"2,650.00"},"EG","7326909890","https://www.se.com/sk/sk/product/NSYSQCR90100","Spacial SF/SM priečniky s rýchlou mont. - 90 mm",0]
["NSYSPV6100","2 BOČNÉ SOKLOVÉ LIŠTY VENTIL 600X100",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3606485132570",{"v":45,"d":"45.00"},{"v":6,"d":"6.00"},{"v":11,"d":"11.00"},{"v":4620,"d":"4,620.00"},"TN","7326909890","https://www.se.com/sk/sk/product/NSYSPV6100","Spacial SF/SM bočné ventilačné panely sokla - 100x600x600 mm",0]
["NSYSPSX4100H","2 BOČNÉ PANELY SOKLA 400x100 316L",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3606480626173",{"v":21.5,"d":"21.50"},{"v":7.5,"d":"7.50"},{"v":11,"d":"11.00"},{"v":1560,"d":"1,560.00"},"IN","7326909890","https://www.se.com/sk/sk/product/NSYSPSX4100H","Spacial - bočný sokel - H100 D400 nerezová oceľ 316L",0]
["NSYSPS3100SD","2 BOČNÉ PANELY SOKLA 300X100",1,"ks",{"v":18.759037499999998,"d":"18.759"},"3606480287091",{"v":11.3,"d":"11.30"},{"v":5.8,"d":"5.80"},{"v":10.8,"d":"10.80"},{"v":574,"d":"574.00"},"TN","7326909890","https://www.se.com/sk/sk/product/NSYSPS3100SD","2 bočné panely pre sokel 300x100mm. RAL 7022. IP 30. IK 10.",0]
["NSYSPLA75","THAL. SADA 2 DRŽIAKOV V. 750",1,"ks",{"v":45.75375,"d":"45.754"},"3606480194542",{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},{"v":58,"d":"58.00"},{"v":200,"d":"200.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYSPLA75","sada 2 držiakov pre montáž hor.panelu alebo 19\" racku v PLA H750mm",0]
["NSYSPFX10100H","PREDNÝ ZADNÝ PANEL SOKLA 1000x100 316L",1,"ks",{"v":640.5525,"d":"640.553"},"3606480626135",{"v":101.5,"d":"101.50"},{"v":11.5,"d":"11.50"},{"v":20,"d":"20.00"},{"v":5790,"d":"5,790.00"},"IN","7326909890","https://www.se.com/sk/sk/product/NSYSPFX10100H","Spacial - plný predný sokel W1000 H100 nerez 316L",0]
["NSYSPF4200","ČELO SOKLA 400X200",1,"ks",{"v":75.03614999999999,"d":"75.036"},"3606485126661",{"v":40.8,"d":"40.80"},{"v":21.1,"d":"21.10"},{"v":19.2,"d":"19.20"},{"v":6090,"d":"6,090.00"},"TN","7326909890","https://www.se.com/sk/sk/product/NSYSPF4200","Spacial SF predný + zadný panel sokla - 200x400 mm",0]
["NSYSPBC38","2 BOČ. PANELY PRE PRÍPOJ. PRIES. 300X800",1,"ks",{"v":279.097875,"d":"279.098"},"3606480067877",{"v":78,"d":"78.00"},{"v":6,"d":"6.00"},{"v":28,"d":"28.00"},{"v":6250,"d":"6,250.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYSPBC38","Spacial SF boční panely pre oddiel zbernice - 300x800 mm",0]
["NSYSMX201250H","SMX 316L 2000X1200X500",1,"ks",{"v":6588.54,"d":"6588.540"},"3606480155871",{"v":58,"d":"58.00"},{"v":213,"d":"213.00"},{"v":125,"d":"125.00"},{"v":180000,"d":"180,000.00"},"BG","9403208000","https://www.se.com/sk/sk/product/NSYSMX201250H","SMX 316L nerez. monoblok skriňa - H2000xŠ1200xH500mm - povrch Scotch Brite®",0]
["NSYSMX16840","SMX 304L 1600X800X400",1,"ks",{"v":2928.24,"d":"2928.240"},"3606480155741",{"v":173,"d":"173.00"},{"v":48,"d":"48.00"},{"v":85,"d":"85.00"},{"v":81000,"d":"81,000.00"},"BG","9403208000","https://www.se.com/sk/sk/product/NSYSMX16840","SMX 304L nerez. monoblok skriňa - H1600xŠ800xH400mm - povrch Scotch Brite®",0]
["NSYSMPSB","4 PRAVOUHLÉ DRŽIAKY",1,"ks",{"v":34.77285,"d":"34.773"},"3606485132181",{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":8,"d":"8.00"},{"v":250,"d":"250.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYSMPSB","Spacial SF 4 lomené držiaky",0]
["NSYSMP2D4","KIT 2 ŠASI PRE 2-DVEROVÚ SKRIŇU 400",1,"ks",{"v":274.5225,"d":"274.523"},"3606485132082",{"v":33,"d":"33.00"},{"v":7,"d":"7.00"},{"v":19.5,"d":"19.50"},{"v":2428,"d":"2,428.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYSMP2D4","Spacial SF sada držiakov mp pre dvojdverové skrine - hĺ. 400 mm",0]
["NSYSMDR","MECHAN. ZARÁŽKA DVERÍ SM",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3606485132075",{"v":25,"d":"25.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":433,"d":"433.00"},"ES","8302420090","https://www.se.com/sk/sk/product/NSYSMDR","Spacial SM mech. zarážka dverí - 105° otvorenie",0]
["NSYSM20640P","SM S MONT. PLECHOM 2000X600X400",1,"ks",{"v":960.8287499999999,"d":"960.829"},"3606485120324",{"v":48,"d":"48.00"},{"v":213,"d":"213.00"},{"v":84.5,"d":"84.50"},{"v":116843,"d":"116,843.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYSM20640P","Spacial SM kompaktný rozv. s mont. plechom - 2000x600x400 mm",0]
["NSYSM2012402D","SM BEZ MONT. PLECHU 2D 2000X1200X400",1,"ks",{"v":1326.8587499999999,"d":"1326.859"},"3606485120850",{"v":49,"d":"49.00"},{"v":213,"d":"213.00"},{"v":124.5,"d":"124.50"},{"v":131000,"d":"131,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSM2012402D","Spacial SM kompaktný rozv. bez mont. plechu - 2000x1200x400 mm",0]
["NSYSM18850P","SM S MONT. PLECHOM 1800X800X500",1,"ks",{"v":1098.09,"d":"1098.090"},"3606485120232",{"v":59,"d":"59.00"},{"v":193,"d":"193.00"},{"v":84.5,"d":"84.50"},{"v":129000,"d":"129,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSM18850P","Spacial SM kompaktný rozv. s mont. plechom - 1800x800x500 mm",0]
["NSYSM18630","SM BEZ MONT. PLECHU 1800X600X300",1,"ks",{"v":759.5122499999999,"d":"759.512"},"3606485120638",{"v":39,"d":"39.00"},{"v":193,"d":"193.00"},{"v":64.5,"d":"64.50"},{"v":64000,"d":"64,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSM18630","Spacial SM kompaktný rozv. bez mont. plechu - 1800x600x300 mm",0]
["NSYSM1812402DP","SM S MONT. PLECHOM 2D 1800X1200X400",1,"ks",{"v":1464.12,"d":"1464.120"},"3606485120270",{"v":48,"d":"48.00"},{"v":192,"d":"192.00"},{"v":124,"d":"124.00"},{"v":147412,"d":"147,412.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSM1812402DP","Spacial SM kompaktný rozv. s mont. plechom - 1800x1200x400 mm",0]
["NSYSM16830","SM BEZ MONT. PLECHU 1600X800X300",1,"ks",{"v":786.9644999999999,"d":"786.965"},"3606485120577",{"v":39,"d":"39.00"},{"v":173,"d":"173.00"},{"v":84.5,"d":"84.50"},{"v":64000,"d":"64,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSM16830","Spacial SM kompaktný rozv. bez mont. plechu - 1600x800x300 mm",0]
["NSYSM1610402DP","SM S MONT. PLECHOM 2D 1600X1000X400",1,"ks",{"v":1189.5974999999999,"d":"1189.598"},"3606485120157",{"v":49,"d":"49.00"},{"v":173,"d":"173.00"},{"v":104.5,"d":"104.50"},{"v":120500,"d":"120,500.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYSM1610402DP","Spacial SM kompaktný rozv. s mont. plechom - 1600x1000x400 mm",0]
["NSYSM1412402DP","SM S MONT. PLECHOM 2D 1400X1200X400",1,"ks",1281.105,"3606485120096",{"v":49,"d":"49.00"},{"v":153,"d":"153.00"},{"v":124.5,"d":"124.50"},{"v":119000,"d":"119,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSM1412402DP","Spacial SM kompaktný rozv. s mont. plechom - 1400x1200x400 mm",0]
["NSYSLCR50","2 PRIEČNIKY PRE SKRIŇU 500",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3606485132044",{"v":48.5,"d":"48.50"},{"v":3.5,"d":"3.50"},{"v":5,"d":"5.00"},{"v":660,"d":"660.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYSLCR50","Spacial SF/SM priečniky pre malé zaťaženie - 500 mm",0]
["NSYSFX18840","SFX 304L 1800X800X400",1,"ks",{"v":4392.36,"d":"4392.360"},"3606480155642",{"v":192,"d":"192.00"},{"v":50,"d":"50.00"},{"v":85,"d":"85.00"},{"v":90000,"d":"90,000.00"},"BG","9403208000","https://www.se.com/sk/sk/product/NSYSFX18840","SFX 304L nerez. rozv. - H1800xŠ800xH400mm - povrch Scotch Brite®",0]
["NSYSFSPLMG","7035 THAL.POLYEST.FIX.PILIER V.800",1,"ks",{"v":576.4972499999999,"d":"576.497"},"3606480777301",{"v":82,"d":"82.00"},{"v":22,"d":"22.00"},{"v":42,"d":"42.00"},{"v":6600,"d":"6,600.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYSFSPLMG","7035 Polyesterový pilier v. 800mm na PLM54/64",0]
["NSYSFP300","THAL. UPEVNENIE NA STĹP Š. 300",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3606480192500",{"v":32,"d":"32.00"},{"v":4.5,"d":"4.50"},{"v":20,"d":"20.00"},{"v":1687,"d":"1,687.00"},"ES","8302420090","https://www.se.com/sk/sk/product/NSYSFP300","upevnenie na stĺp priem. max 215mm záťaž 100kg pre PLM43",0]
["NSYSFHD20840","SPACIAL SF HD 2000x800x400MM",1,"ks",{"v":2104.6724999999997,"d":"2104.673"},"3606480676307",{"v":219,"d":"219.00"},{"v":49,"d":"49.00"},{"v":85,"d":"85.00"},{"v":97000,"d":"97,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYSFHD20840","Spacial SFHD vonkajšie odolné prevedenie-rozmont.rozvádzače-H2062 W800 D430-IP55",0]
["NSYSFD226T","PRESKLENÉ DVERE SF/SM 2200X600",1,"ks",{"v":599.3741249999999,"d":"599.374"},"3606485119731",{"v":227,"d":"227.00"},{"v":5.5,"d":"5.50"},{"v":58,"d":"58.00"},{"v":21450,"d":"21,450.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYSFD226T","Spacial SF priehladné dvere - 2200x600 mm",0]
["NSYSFD203","PLNÉ DVERE SF/SM 2000X300",1,"ks",{"v":256.22099999999995,"d":"256.221"},"3606485119472",{"v":208,"d":"208.00"},{"v":5,"d":"5.00"},{"v":28,"d":"28.00"},{"v":14300,"d":"14,300.00"},"FR","9403991090","https://www.se.com/sk/sk/product/NSYSFD203","Spacial SF plné dvere - 2000x300 mm",0]
["NSYSFD1882D","DVOJITÉ PLNÉ DVERE SF/SM 1800X400",1,"ks",475.839,"3606480067594",{"v":189,"d":"189.00"},{"v":8,"d":"8.00"},{"v":44,"d":"44.00"},{"v":32000,"d":"32,000.00"},"FR","9403991090","https://www.se.com/sk/sk/product/NSYSFD1882D","Spacial SF dvojkrídlové plné dvere - 1800x800 mm",0]
["NSYSFD166","PLNÉ DVERE SF/SM 1600X600",1,"ks",{"v":311.1255,"d":"311.126"},"3606485119403",{"v":170,"d":"170.00"},{"v":5,"d":"5.00"},{"v":58,"d":"58.00"},{"v":20000,"d":"20,000.00"},"FR","9403991090","https://www.se.com/sk/sk/product/NSYSFD166","Spacial SF plné dvere - 1600x600 mm",0]
["NSYSFC36","ZÁKL. RÁM HORNÝ A DOLNÝ SF 300X600",1,"ks",{"v":274.5225,"d":"274.523"},"3606485118895",{"v":63,"d":"63.00"},{"v":15,"d":"15.00"},{"v":33,"d":"33.00"},{"v":15200,"d":"15,200.00"},"FR","9403991090","https://www.se.com/sk/sk/product/NSYSFC36","Spacial SF horný a spodný rám - 300x600 mm",0]
["NSYSFC128","ZÁKL. RÁM HORNÝ A DOLNÝ SF 1200X800",1,"ks",{"v":430.08525,"d":"430.085"},"3606485119090",{"v":123,"d":"123.00"},{"v":15,"d":"15.00"},{"v":89,"d":"89.00"},{"v":38300,"d":"38,300.00"},"FR","9403991090","https://www.se.com/sk/sk/product/NSYSFC128","Spacial SF horný a spodný rám - 1200x800 mm",0]
["NSYSF22880E","SF ELECTRONIC 2200X800X800",1,"ks",{"v":2470.7024999999994,"d":"2470.703"},"3606485127453",{"v":233,"d":"233.00"},{"v":84.5,"d":"84.50"},{"v":89,"d":"89.00"},{"v":147000,"d":"147,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYSF22880E","Spacial SF skriňa pre elektronické aplikácie - 2200x800x800 mm",0]
["NSYSF22860","SF BEZ MONT. PLECHU 2200X800X600",1,"ks",{"v":1006.5824999999999,"d":"1006.583"},"3606485118536",{"v":69,"d":"69.00"},{"v":233,"d":"233.00"},{"v":84.5,"d":"84.50"},{"v":118720,"d":"118,720.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF22860","Spacial SF skriňa bez mont. panelu - 2200x800x600 mm",0]
["NSYSF221060","SF BEZ MONT. PLECHU 2200X1000X600",1,"ks",1281.105,"3606485118550",{"v":233,"d":"233.00"},{"v":69,"d":"69.00"},{"v":104.5,"d":"104.50"},{"v":113500,"d":"113,500.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF221060","Spacial SF skriňa bez mont. panelu - 2200x1000x600 mm",0]
["NSYSF20680P","SF S MONT. PLECHOM 2000X600X800",1,"ks",{"v":1052.3362499999998,"d":"1052.336"},"3606485117669",{"v":89,"d":"89.00"},{"v":213,"d":"213.00"},{"v":64.5,"d":"64.50"},{"v":144734,"d":"144,734.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYSF20680P","Spacial SF skriňa s mont. panelom - 2000x600x800 mm",0]
["NSYSF20660","SF BEZ MONT. PLECHU 2000X600X600",1,"ks",{"v":832.7182499999999,"d":"832.718"},"3606485118291",{"v":213,"d":"213.00"},{"v":64.5,"d":"64.50"},{"v":69,"d":"69.00"},{"v":78000,"d":"78,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF20660","Spacial SF skriňa bez mont. panelu - 2000x600x600 mm",0]
["NSYSF20440","SF BEZ MONT. PLECHU 2000X400X400",1,"ks",{"v":782.3891249999999,"d":"782.389"},"3606485118239",{"v":213,"d":"213.00"},{"v":44.5,"d":"44.50"},{"v":49,"d":"49.00"},{"v":61000,"d":"61,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF20440","Spacial SF skriňa bez mont. panelu - 2000x400x400 mm",0]
["NSYSF2012602DP","SF S MONT. PLECHOM 2D 2000X1200X600",1,"ks",{"v":1555.6274999999998,"d":"1555.628"},"3606485117812",{"v":213,"d":"213.00"},{"v":69,"d":"69.00"},{"v":124.5,"d":"124.50"},{"v":173000,"d":"173,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF2012602DP","Spacial SF skriňa s mont. panelom - 2000x1200x600 mm",0]
["NSYSF201040P","SF S MONT. PLECHOM 2000X1000X400",1,"ks",{"v":1189.5974999999999,"d":"1189.598"},"3606485117720",{"v":46,"d":"46.00"},{"v":213,"d":"213.00"},{"v":104,"d":"104.00"},{"v":157661,"d":"157,661.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYSF201040P","Spacial SF skriňa s mont. panelom - 2000x1000x400 mm",0]
["NSYSF18680PC","SF PC APPLICATION 1800X600X800",1,"ks",{"v":2745.2249999999995,"d":"2745.225"},"3606485118772",{"v":193,"d":"193.00"},{"v":64.5,"d":"64.50"},{"v":89,"d":"89.00"},{"v":106000,"d":"106,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYSF18680PC","Spacial SF PC rack. skriňa- 1800x600x800 mm",0]
["NSYSF18640T","SF PRESKLENÉ DVERE BEZ MP 1800X600X400",1,"ks",{"v":1143.84375,"d":"1143.844"},"3606485118581",{"v":193,"d":"193.00"},{"v":49,"d":"49.00"},{"v":64.5,"d":"64.50"},{"v":63000,"d":"63,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF18640T","Spacial SF skriňa s priehľadnými dverami - 1800x600x400 mm",0]
["NSYSF1810402DP","SF S MONT. PLECHOM 2D 1800X1000X400",1,"ks",1281.105,"3606485117560",{"v":213,"d":"213.00"},{"v":49,"d":"49.00"},{"v":105,"d":"105.00"},{"v":124000,"d":"124,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF1810402DP","Spacial SF skriňa s mont. panelom - 1800x1000x400 mm",0]
["NSYSF16880","SF BEZ MONT. PLECHU 1600X800X800",1,"ks",{"v":960.8287499999999,"d":"960.829"},"3606485118024",{"v":89,"d":"89.00"},{"v":173,"d":"173.00"},{"v":84.5,"d":"84.50"},{"v":132500,"d":"132,500.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF16880","Spacial SF skriňa bez mont. panelu - 1600x800x800 mm",0]
["NSYSF12840","SF BEZ MONT. PLECHU 1200X800X400",1,"ks",805.266,"3606485117959",{"v":133,"d":"133.00"},{"v":49,"d":"49.00"},{"v":84.5,"d":"84.50"},{"v":60000,"d":"60,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF12840","Spacial SF skriňa bez mont. panelu - 1200x800x400 mm",0]
["NSYSF12640P","SF S MONT. PLECHOM 1200X600X400",1,"ks",{"v":777.8137499999999,"d":"777.814"},"3606485117386",{"v":133,"d":"133.00"},{"v":49,"d":"49.00"},{"v":64.5,"d":"64.50"},{"v":64000,"d":"64,000.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSF12640P","Spacial SF skriňa s mont. panelom - 1200x600x400 mm",0]
["NSYSDP6M","OCEĽ. SCHRÁNKA NA DVERE NA DOKUM. 600",1,"ks",{"v":41.635912499999996,"d":"41.636"},"3606485131429",{"v":46.5,"d":"46.50"},{"v":6.5,"d":"6.50"},{"v":28,"d":"28.00"},{"v":1565,"d":"1,565.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYSDP6M","Spacial kovové vrecko na dokumenty - nominálna šírka: 600 mm",0]
["NSYSDCR400","3D SADA 4 BOČNÝCH DRŽIAKOV HĹBKA=400MM",1,"ks",{"v":58.10726249999999,"d":"58.107"},"3606480184291",{"v":37,"d":"37.00"},{"v":5,"d":"5.00"},{"v":13.5,"d":"13.50"},{"v":1120,"d":"1,120.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYSDCR400","sada 4 posuvných držiakov pre hĺbku 400mm",0]
["NSYSDC42","KONZOLA 400X200",1,"ks",{"v":526.1681249999999,"d":"526.168"},"3606480154485",{"v":51,"d":"51.00"},{"v":28,"d":"28.00"},{"v":41.5,"d":"41.50"},{"v":12000,"d":"12,000.00"},"CZ","9403208000","https://www.se.com/sk/sk/product/NSYSDC42","modulárna konzola Spacial SD Compact so zadným panelom - Š400xH200",0]
["NSYSCX12050","STRECHA SFX SMX 304L 1200X500",1,"ks",{"v":855.595125,"d":"855.595"},"3606480155451",{"v":126,"d":"126.00"},{"v":9.5,"d":"9.50"},{"v":56,"d":"56.00"},{"v":12500,"d":"12,500.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYSCX12050","nerezová strecha 304L - povrch Scotch Brite® - pre rozv. SFX/SMX Š1200xH500 mm.",0]
["NSYSC850","STRIEŠKA 800X500",1,"ks",{"v":205.891875,"d":"205.892"},"3606485131313",{"v":82,"d":"82.00"},{"v":9.5,"d":"9.50"},{"v":53.5,"d":"53.50"},{"v":7364,"d":"7,364.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYSC850","Spacial SF/SM strecha - 800x500 mm",0]
["NSYSBX204012","Priemyselná skrinka 200x400x120 mm, 304L",1,"ks",{"v":306.550125,"d":"306.550"},"3606481715210",{"v":13.5,"d":"13.50"},{"v":41.5,"d":"41.50"},{"v":21.5,"d":"21.50"},{"v":3078,"d":"3,078.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYSBX204012","Stainless steel wall mounted industrial box, Spacial SBX, 200x400x120 mm, IP66",0]
["NSYSBM306012","KOV. PRIEMYSEL. SKRINKA 300X600X120",1,"ks",109.809,"3606480520235",{"v":62.5,"d":"62.50"},{"v":15,"d":"15.00"},{"v":31.5,"d":"31.50"},{"v":6724,"d":"6,724.00"},"IN","9403208000","https://www.se.com/sk/sk/product/NSYSBM306012","kovová priemyslová skrinka-plné dvere-300x600x120 IP66 IK10 RAL 7035",0]
["NSYSBM20208","KOV. PRIEMYSEL. SKRINKA 200x200x80",1,"ks",{"v":53.53188749999999,"d":"53.532"},"3606480520051",{"v":21.5,"d":"21.50"},{"v":10,"d":"10.00"},{"v":21.5,"d":"21.50"},{"v":1620,"d":"1,620.00"},"IN","9403208000","https://www.se.com/sk/sk/product/NSYSBM20208","kovová priemyslová skrinka-plné dvere-200x200x80 IP66 IK10 RAL 7035",0]
["NSYS3X6420H","S3X 316L 600X400X200",1,"ks",{"v":915.0749999999999,"d":"915.075"},"3606480155222",{"v":61,"d":"61.00"},{"v":22,"d":"22.00"},{"v":41.5,"d":"41.50"},{"v":9520,"d":"9,520.00"},"BG","9403208000","https://www.se.com/sk/sk/product/NSYS3X6420H","Spacial S3X nerez 316L - povrch Scotch Brite® - V600xŠ400xH200 mm.",0]
["NSYS3X4420H","S3X 316L 400X400X200",1,"ks",{"v":672.580125,"d":"672.580"},"3606480155154",{"v":41.5,"d":"41.50"},{"v":22,"d":"22.00"},{"v":41.5,"d":"41.50"},{"v":6766,"d":"6,766.00"},"BG","9403208000","https://www.se.com/sk/sk/product/NSYS3X4420H","Spacial S3X nerez 316L - povrch Scotch Brite® - V400xŠ400xH200 mm.",0]
["NSYS3X12830H","S3X 316L 1200X800X300",1,"ks",{"v":3660.2999999999997,"d":"3660.300"},"3606480155024",{"v":124,"d":"124.00"},{"v":33,"d":"33.00"},{"v":83,"d":"83.00"},{"v":44000,"d":"44,000.00"},"BG","9403208000","https://www.se.com/sk/sk/product/NSYS3X12830H","Spacial S3X nerez 316L - povrch Scotch Brite® - V1200xŠ800xH300 mm.",0]
["NSYS3X101030H","S3X 316L 1000X1000X300",1,"ks",{"v":4392.36,"d":"4392.360"},"3606480154959",{"v":32.6,"d":"32.60"},{"v":102.1,"d":"102.10"},{"v":102.1,"d":"102.10"},{"v":47000,"d":"47,000.00"},"BG","9403208000","https://www.se.com/sk/sk/product/NSYS3X101030H","Spacial S3X nerez 316L - povrch Scotch Brite® - V1000xŠ1000xH300 mm.",0]
["NSYS3DEX7525","86500 ROZVODNICA EEX 700X500X200",1,"ks",{"v":256.22099999999995,"d":"256.221"},"3606480158605",{"v":72,"d":"72.00"},{"v":29.5,"d":"29.50"},{"v":52,"d":"52.00"},{"v":15056,"d":"15,056.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3DEX7525","Spacial S3DEX (ATEX) V700xŠ500xH250 .IP66 IK10 RAL7035.",0]
["NSYS3D8830T","SPACIAL 3D SKLEN. DVERE 800X800X300",1,"ks",{"v":370.605375,"d":"370.605"},"3606480158834",{"v":35.4,"d":"35.40"},{"v":82.4,"d":"82.40"},{"v":82.6,"d":"82.60"},{"v":31000,"d":"31,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D8830T","Spacial S3D priehľadné dvere bez mont.panelu V800xŠ800xH300.IP66 IK08 RAL7035.",0]
["NSYS3D8830P","SPACIAL 3D MONT. PLECH 800X800X300",1,"ks",{"v":329.42699999999996,"d":"329.427"},"3606480158841",{"v":82.5,"d":"82.50"},{"v":35,"d":"35.00"},{"v":82,"d":"82.00"},{"v":38000,"d":"38,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D8830P","Spacial S3D plné dvere s mont. panelom V800xŠ800xH300.IP66 IK10 RAL7035.",0]
["NSYS3D81030D","SPACIAL 3D 800X1000X300",1,"ks",{"v":443.81137499999994,"d":"443.811"},"3606480159053",{"v":71,"d":"71.00"},{"v":27.5,"d":"27.50"},{"v":46,"d":"46.00"},{"v":26421,"d":"26,421.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D81030D","Spacial S3D dvoj.plné dvere bez mont.dosky V800xŠ1000xH300.IP55 IK10 RAL7035.",0]
["NSYS3D6630","SPACIAL 3D 600X600X300",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3606480159183",{"v":62,"d":"62.00"},{"v":35,"d":"35.00"},{"v":61.5,"d":"61.50"},{"v":16570,"d":"16,570.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D6630","Spacial S3D plné dvere bez mont.panelu V600xŠ600xH300.IP66 IK10 RAL7035.",0]
["NSYS3D6425","SPACIAL 3D 600X400X250",1,"ks",{"v":141.836625,"d":"141.837"},"3606480159305",{"v":62,"d":"62.00"},{"v":29.5,"d":"29.50"},{"v":41.5,"d":"41.50"},{"v":11590,"d":"11,590.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D6425","Spacial S3D plné dvere bez mont.panelu V600xŠ400xH250.IP66 IK10 RAL7035.",0]
["NSYS3D5425P","SPACIAL 3D MONT. PLECH 500X400X250",1,"ks",{"v":137.26125,"d":"137.261"},"3606480159411",{"v":51,"d":"51.00"},{"v":29.5,"d":"29.50"},{"v":41.5,"d":"41.50"},{"v":11428,"d":"11,428.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D5425P","Spacial S3D plné dvere s mont. panelom V500xŠ400xH250 IP66 IK10 RAL7035.",0]
["NSYS3D4620T","SPACIAL 3D SKLEN. DVERE 400X600X200",1,"ks",183.015,"3606480159527",{"v":61,"d":"61.00"},{"v":14,"d":"14.00"},{"v":41.5,"d":"41.50"},{"v":10500,"d":"10,500.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D4620T","Spacial S3D priehľadné dvere bez mont.panelu V400xŠ600xH200 IP66 IK08 RAL7035.",0]
["NSYS3D3420T","SPACIAL 3D SKLENÉ DVERE 300X400X200",1,"ks",{"v":137.26125,"d":"137.261"},"3606480159640",{"v":41,"d":"41.00"},{"v":24.5,"d":"24.50"},{"v":31.5,"d":"31.50"},{"v":5856,"d":"5,856.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D3420T","Spacial S3D priehľadné dvere bez mont.panelu V300xŠ400xH200 IP66 IK08 RAL7035.",0]
["NSYS3D3315P","SPACIAL 3D MONT. PLECH 300X300X150",1,"ks",{"v":100.65825,"d":"100.658"},"3606480159749",{"v":32,"d":"32.00"},{"v":19.5,"d":"19.50"},{"v":32,"d":"32.00"},{"v":4799,"d":"4,799.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D3315P","Spacial S3D plné dvere s mont. panelom V300xŠ300xH150 IP66 IK10 RAL7035.",0]
["NSYS3D12840T","SPACIAL 3D SKLEN. DVERE 1200X800X400",1,"ks",549.045,"3606480159831",{"v":45.4,"d":"45.40"},{"v":122.6,"d":"122.60"},{"v":82.4,"d":"82.40"},{"v":48000,"d":"48,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D12840T","Spacial S3D priehľadné dvere bez mont.panelu V1200xŠ800xH400 IP66 IK08 RAL7035.",0]
["NSYS3D121240D","SPACIAL 3D 1200X1200X400",1,"ks",{"v":1098.09,"d":"1098.090"},"3606480159961",{"v":133,"d":"133.00"},{"v":45,"d":"45.00"},{"v":122,"d":"122.00"},{"v":76000,"d":"76,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D121240D","Spacial S3D plné dvere bez mont.panelu V1200xŠ1200xH400 IP55 IK10 RAL7035.",0]
["NSYS3D10640","SPACIAL 3D 1000X600X400",1,"ks",{"v":306.550125,"d":"306.550"},"3606480160189",{"v":103.5,"d":"103.50"},{"v":45.5,"d":"45.50"},{"v":62,"d":"62.00"},{"v":34000,"d":"34,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D10640","Spacial S3D plné dvere bez mont.panelu V1000xŠ600xH400 IP66 IK10 RAL7035.",0]
["NSYS3D101030DT","SPACIAL 3D SKLEN. DVERE 1000X1000X300",1,"ks",{"v":567.3465,"d":"567.347"},"3606480160318",{"v":35.4,"d":"35.40"},{"v":102.4,"d":"102.40"},{"v":102.6,"d":"102.60"},{"v":45000,"d":"45,000.00"},"FR","9403208000","https://www.se.com/sk/sk/product/NSYS3D101030DT","Spacial S3D dvojité priehľad.dvere bez mont.dosky V1000xŠ1000xH300 IP55",0]
["NSYS16M6HS","SKRUTKA M6,3X16 1KS",100,"ks",{"v":0.27452249999999995,"d":"0.275"},"3606480184154",{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":5,"d":"5.00"},"FR","7318141090","https://www.se.com/sk/sk/product/NSYS16M6HS","samorezný šrób 6.3x16mm + captive washer. obj. množstvo: 100 ks.",0]
["NSYRSW640","SWING RACK BEZ PANELOV 19\" 40U",1,"ks",{"v":832.7182499999999,"d":"832.718"},"3606480067273",{"v":187,"d":"187.00"},{"v":10,"d":"10.00"},{"v":51.5,"d":"51.50"},{"v":18500,"d":"18,500.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYRSW640","Spacial SF/SM 19\" otočný rám bez panelov - 2000x600 mm - 40 mod.",0]
["NSYRETPLAU","THAL. DVER. OBMEDZOVAČ PRE PLA/Z/T/ZT",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3606480193460",{"v":22,"d":"22.00"},{"v":3.5,"d":"3.50"},{"v":13,"d":"13.00"},{"v":444.5,"d":"444.50"},"ES","8302420090","https://www.se.com/sk/sk/product/NSYRETPLAU","držiak dverí pre všetky verzie PLA - 2 polohy otvorenia 90º alebo 120º",0]
["NSYRCK47","PEVNÝ RACK 19\" 47U",1,"ks",{"v":78.2389125,"d":"78.239"},"3606480066894",{"v":4.5,"d":"4.50"},{"v":210,"d":"210.00"},{"v":11,"d":"11.00"},{"v":7200,"d":"7,200.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYRCK47","Spacial SF 19\" stojany pevné - 2200 mm",0]
["NSYRCINT","SPÍNAČ PRE RACK",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3606480066825",{"v":4,"d":"4.00"},{"v":13,"d":"13.00"},{"v":10,"d":"10.00"},{"v":68,"d":"68.00"},"ES","8536508090","https://www.se.com/sk/sk/product/NSYRCINT","spínač pre 19\" rámy",0]
["NSYPUNX","ZÁVESNÁ KONZOLA SFX 4KS",1,"ks",{"v":288.24862499999995,"d":"288.249"},"3606480154898",{"v":21.5,"d":"21.50"},{"v":9.5,"d":"9.50"},{"v":16.5,"d":"16.50"},{"v":4960,"d":"4,960.00"},"ES","85389099","https://www.se.com/sk/sk/product/NSYPUNX","4 lifting brackets for Spacial SFX enclosure. Max. load 2000kg",0]
["NSYPPS205","ODDEĽOVACÍ PANEL SF 2000X500",1,"ks",{"v":155.56275,"d":"155.563"},"3606485127149",{"v":202,"d":"202.00"},{"v":4,"d":"4.00"},{"v":42,"d":"42.00"},{"v":11000,"d":"11,000.00"},"FR","7326199000","https://www.se.com/sk/sk/product/NSYPPS205","Spacial SF oddeľovací panel - pozinkovaná oceľ - 2000x500 mm",0]
["NSYPMP750DLP","THAL. MONT. DOSKA DL. 750",1,"ks",{"v":19.674112499999996,"d":"19.674"},"3606480194788",{"v":2.5,"d":"2.50"},{"v":75,"d":"75.00"},{"v":17,"d":"17.00"},{"v":1532,"d":"1,532.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYPMP750DLP","montážny panel z pozinkovanej ocele pre DLP výška=1rada v rozv. PLA Š500mm",0]
["NSYPMM510","THAL. MONT. PLECH PLNÝ 500X1000",1,"ks",{"v":71.8333875,"d":"71.833"},"3606480193798",{"v":87.5,"d":"87.50"},{"v":0.5,"d":"0.50"},{"v":39,"d":"39.00"},{"v":6270,"d":"6,270.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYPMM510","kovový montážny panel pre PLA skriňu V500xŠ1000mm",0]
["NSYPMM1827","MONT. PLECH 180X270",1,"ks",{"v":8.18992125,"d":"8.190"},"3606480189371",{"v":23,"d":"23.00"},{"v":2,"d":"2.00"},{"v":14.5,"d":"14.50"},{"v":536,"d":"536.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYPMM1827","kovový mont. panel pre PLS 18x27cm",0]
["NSYPMB75","THAL. MONT. PLECH IZOL. 750X500",1,"ks",{"v":55.81957499999999,"d":"55.820"},"3606480194108",{"v":64,"d":"64.00"},{"v":0.5,"d":"0.50"},{"v":37.5,"d":"37.50"},{"v":1460,"d":"1,460.00"},"ES","3926909790","https://www.se.com/sk/sk/product/NSYPMB75","montážny panel pre PLA skriňu V500xŠ750mm alebo V750xŠ500mm - bakelit",0]
["NSYPMB127","THAL. MONT. PLECH IZOL. 1250X750",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606480194207",{"v":114,"d":"114.00"},{"v":0.5,"d":"0.50"},{"v":62.6,"d":"62.60"},{"v":5160,"d":"5,160.00"},"ES","3926909790","https://www.se.com/sk/sk/product/NSYPMB127","montážny panel pre PLA skriňu V1250xŠ750mm - bakelit",0]
["NSYPMA3672G","7035 MP POLYESTER 360X720 PLS",1,"ks",{"v":55.81957499999999,"d":"55.820"},"3606485405391",{"v":32,"d":"32.00"},{"v":0.5,"d":"0.50"},{"v":67.5,"d":"67.50"},{"v":1508,"d":"1,508.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYPMA3672G","Insulating polyester mounting plate for PLS box 36x72cm",0]
["NSYPLSP5454G","7035 MOD.SKRINKA 540X540X180",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3606480777295",{"v":56,"d":"56.00"},{"v":20,"d":"20.00"},{"v":56,"d":"56.00"},{"v":7500,"d":"7,500.00"},"ES","3926909790","https://www.se.com/sk/sk/product/NSYPLSP5454G","7035 priemys. skrinka PLS 540x540x180 IP65",0]
["NSYPLSC2736G","7035 MOD.SKRINKA 27X36X18",1,"ks",{"v":86.01705,"d":"86.017"},"3606480777127",{"v":29,"d":"29.00"},{"v":20,"d":"20.00"},{"v":38,"d":"38.00"},{"v":2300,"d":"2,300.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYPLSC2736G","7035 priemys. skrinka PC PLS 270x360x180 IP65, plné veko",0]
["NSYPLS24","PODP.PIEST 215N",1,"ks",{"v":83.7293625,"d":"83.729"},"3606480154171",{"v":30,"d":"30.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":200,"d":"200.00"},"CZ","8302420090","https://www.se.com/sk/sk/product/NSYPLS24","SD pneumatická pružina, max.24 kg",0]
["NSYPLM86TVG","7035 PLM 47X636X300IP66",1,"ks",{"v":713.7584999999999,"d":"713.759"},"3606480776793",{"v":87,"d":"87.00"},{"v":66,"d":"66.00"},{"v":33,"d":"33.00"},{"v":21239,"d":"21,239.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLM86TVG","7035 WM PLM847x636x300glass 3lock",0]
["NSYPLM64BG","7035 PLM 647X436X250 IP66 IZOL.",1,"ks",{"v":237.9195,"d":"237.920"},"3606480776649",{"v":68,"d":"68.00"},{"v":45,"d":"45.00"},{"v":27.5,"d":"27.50"},{"v":11100,"d":"11,100.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLM64BG","Wall mounted polyester enclosure, Thalassa PLM, plain door, with bakelite plate, 647x436x250mm, IP66, IK10, RAL 7035",0]
["NSYPLM3025BG","7035 PLM PL.DV.310X215X160 IP66 IZOL.",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3606480776441",{"v":32.5,"d":"32.50"},{"v":18.5,"d":"18.50"},{"v":26.5,"d":"26.50"},{"v":3461,"d":"3,461.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLM3025BG","Wall mounted polyester enclosure, Thalassa PLM, plain door, with bakelite plate, 308x255x160mm, IP66, IK10, RAL 7035",0]
["NSYPLAZT774G","7035 PLAZT VETR.NADST.IP44 750X750X420",1,"ks",{"v":960.8287499999999,"d":"960.829"},"3606480776342",{"v":48,"d":"48.00"},{"v":85.3,"d":"85.30"},{"v":78,"d":"78.00"},{"v":29538,"d":"29,538.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLAZT774G","7035 Thalassa PLA samovent. 750x750x420 IP44",0]
["NSYPLAZT15104G","7035 PLAZT VETR.NADST.IP44 1500X1000X420",1,"ks",{"v":1784.3962499999996,"d":"1784.396"},"3606480776120",{"v":38,"d":"38.00"},{"v":160.3,"d":"160.30"},{"v":103,"d":"103.00"},{"v":80274,"d":"80,274.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLAZT15104G","7035 Thalassa PLA samovent. 1500x1000x420 IP44",0]
["NSYPLAZT1253G","7035 PLAZT VETR.NADST.IP44 1250X500X320",1,"ks",{"v":1006.5824999999999,"d":"1006.583"},"3606480776076",{"v":38,"d":"38.00"},{"v":129,"d":"129.00"},{"v":54,"d":"54.00"},{"v":33136,"d":"33,136.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLAZT1253G","7035 Thalassa PLA samovent. 1250x500x320 IP44",0]
["NSYPLAZ574G","7035 PLAZ OTV.DNO IP54 500X750X420",1,"ks",{"v":754.936875,"d":"754.937"},"3606480775864",{"v":45,"d":"45.00"},{"v":56.5,"d":"56.50"},{"v":78,"d":"78.00"},{"v":25820,"d":"25,820.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLAZ574G","7035 Thalassa PLA s otvor.dnom 500x750x420 IP54",0]
["NSYPLAZ1254G","7035 PLAZ OTV.DNO IP54 1250X500X420",1,"ks",{"v":1006.5824999999999,"d":"1006.583"},"3606480775680",{"v":48,"d":"48.00"},{"v":131.5,"d":"131.50"},{"v":56.5,"d":"56.50"},{"v":35129,"d":"35,129.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLAZ1254G","7035 Thalassa PLA s otvor.dnom 1250x500x420 IP54",0]
["NSYPLAZ1054G","7035 PLAZ OTV.DNO IP54 1000X500X420",1,"ks",{"v":837.293625,"d":"837.294"},"3606480775604",{"v":48,"d":"48.00"},{"v":107,"d":"107.00"},{"v":54,"d":"54.00"},{"v":28032,"d":"28,032.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLAZ1054G","7035 Thalassa PLA s otvor.dnom 1000x500x420 IP54",0]
["NSYPLAT773G","7035 PLA VETR.NADST.IP54 750X750X320",1,"ks",{"v":727.4846249999999,"d":"727.485"},"3606480775536",{"v":38,"d":"38.00"},{"v":76,"d":"76.00"},{"v":78,"d":"78.00"},{"v":24130,"d":"24,130.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLAT773G","7035 Thalassa PLA s otvor.strechou 750x750x320 IP44",0]
["NSYPLAT15103G","7035 PLA VETR.NADST.IP54 1500X1000X320",1,"ks",1647.135,"3606480775314",{"v":38,"d":"38.00"},{"v":152,"d":"152.00"},{"v":103,"d":"103.00"},{"v":65500,"d":"65,500.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLAT15103G","7035 Thalassa PLA s otvor.strechou 1500x1000x320 IP44",0]
["NSYPLA774TG","7035 PLA PRIEHĽAD.DV.750X750X420",1,"ks",{"v":915.0749999999999,"d":"915.075"},"3606480775147",{"v":48,"d":"48.00"},{"v":76,"d":"76.00"},{"v":78,"d":"78.00"},{"v":27063,"d":"27,063.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLA774TG","7035 Thalassa PLA 750x750x420 IP65, priehľ. dvere",0]
["NSYPLA753TG","7035 PLA PRIEHĽAD.DV.750X500X320",1,"ks",{"v":915.0749999999999,"d":"915.075"},"3606480775086",{"v":38,"d":"38.00"},{"v":76,"d":"76.00"},{"v":54,"d":"54.00"},{"v":18860,"d":"18,860.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLA753TG","7035 Thalassa PLA 750x500x320 IP65, priehľ. dvere",0]
["NSYPLA553TG","7035 PLA PRIEHĽAD.DV.500X500X320",1,"ks",{"v":663.4293749999999,"d":"663.429"},"3606480774928",{"v":38,"d":"38.00"},{"v":50,"d":"50.00"},{"v":53,"d":"53.00"},{"v":14500,"d":"14,500.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLA553TG","7035 Thalassa PLA 500x500x320 IP65, priehľ. dvere",0]
["NSYPLA15126G","7035 THALASSA PLA 1500X1250X620, IP65",1,"ks",{"v":2196.18,"d":"2196.180"},"3606480772962",{"v":65,"d":"65.00"},{"v":153,"d":"153.00"},{"v":128,"d":"128.00"},{"v":94000,"d":"94,000.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLA15126G","Floor standing polyester enclosure, Thalassa PLA, plain door, completely sealed, 1500x1250x620mm, IP65, IK10",0]
["NSYPLA15103TG","7035 PLA PRIEHĽAD.DV.1500X1000X320",1,"ks",{"v":1921.6574999999998,"d":"1921.658"},"3606480774683",{"v":35,"d":"35.00"},{"v":151,"d":"151.00"},{"v":103,"d":"103.00"},{"v":58651,"d":"58,651.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLA15103TG","7035 Thalassa PLA 1500x1000x320 IP65, priehľ.dvere",0]
["NSYPLA12103TG","7035 PLA PRIEHĽAD.DV.1250X1000X320",1,"ks",{"v":1784.3962499999996,"d":"1784.396"},"3606480774522",{"v":35,"d":"35.00"},{"v":126,"d":"126.00"},{"v":103,"d":"103.00"},{"v":47299,"d":"47,299.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLA12103TG","7035 Thalassa PLA 1250x1000x320 IP65, priehľ. dvere",0]
["NSYPLA1054TG","7035 PLA PRIEHĽAD.DV.1000X500X420",1,"ks",{"v":887.6227499999999,"d":"887.623"},"3606480774461",{"v":45,"d":"45.00"},{"v":101,"d":"101.00"},{"v":53,"d":"53.00"},{"v":27758,"d":"27,758.00"},"ES","9403700000","https://www.se.com/sk/sk/product/NSYPLA1054TG","7035 Thalassa PLA 1000x500x420 IP65, priehľ. dvere",0]
["NSYPIN128","SPACIAL 3D VNÚT.DVERE 1200X800",1,"ks",{"v":237.9195,"d":"237.920"},"3606480168581",{"v":121,"d":"121.00"},{"v":3,"d":"3.00"},{"v":81,"d":"81.00"},{"v":13600,"d":"13,600.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYPIN128","vnútorné dvere pre Spacial S3D H400xŠ300 - RAL7035 nastavitelná hl.",0]
["NSYPFPLM32G","7035 SADA 4 PL.ZÁVESOV NA STENU/300X200",1,"ks",{"v":6.405525,"d":"6.406"},"3606480774348",{"v":10,"d":"10.00"},{"v":2,"d":"2.00"},{"v":9,"d":"9.00"},{"v":26,"d":"26.00"},"ES","3925908000","https://www.se.com/sk/sk/product/NSYPFPLM32G","7035 Thalassa, súprava 4 plastových závesov na PLM32",0]
["NSYPAPLA77G","7035 THALASSA VNÚT.DVERE 750X750",1,"ks",{"v":256.22099999999995,"d":"256.221"},"3606480774324",{"v":66,"d":"66.00"},{"v":4,"d":"4.00"},{"v":66,"d":"66.00"},{"v":2500,"d":"2,500.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYPAPLA77G","7035 vnútorné dvere 750x750 na PLA",0]
["NSYPAPLA107G","7035 THALASSA VNÚT.DVERE 1000X750",1,"ks",{"v":251.64562499999997,"d":"251.646"},"3606480774249",{"v":91,"d":"91.00"},{"v":3.5,"d":"3.50"},{"v":66.5,"d":"66.50"},{"v":5469,"d":"5,469.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYPAPLA107G","7035 vnútorné dvere 1000x750 na PLA",0]
["NSYMW10M","PRIEHĽAD. KRYT IP55",1,"ks",{"v":39.34822499999999,"d":"39.348"},"3606480183874",{"v":22,"d":"22.00"},{"v":4,"d":"4.00"},{"v":14,"d":"14.00"},{"v":280,"d":"280.00"},"DE","3926909790","https://www.se.com/sk/sk/product/NSYMW10M","plastové okno s priehladným krytom IP 55 - L78xŠ180mm.",0]
["NSYMUCH406","ČELNÝ PANEL S PÁNTAMI 400X600",1,"ks",{"v":79.61152499999999,"d":"79.612"},"3606480066399",{"v":50.5,"d":"50.50"},{"v":1.5,"d":"1.50"},{"v":40,"d":"40.00"},{"v":2784,"d":"2,784.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYMUCH406","Spacial SF/SM krycia doska s výrezom - 400x600 mm - vyklápacia",0]
["NSYMUC208","ČELNÝ PANEL SKRUTKOVANÝ 200X800",1,"ks",{"v":43.008525,"d":"43.009"},"3606480066481",{"v":71,"d":"71.00"},{"v":2,"d":"2.00"},{"v":21,"d":"21.00"},{"v":2122,"d":"2,122.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYMUC208","Spacial SF/SM krycia doska s výrezom - 200x800 mm - skrutková",0]
["NSYMR66","3D PERF. MONT. PLECH 600X600",1,"ks",{"v":58.56479999999999,"d":"58.565"},"3606480183720",{"v":55.5,"d":"55.50"},{"v":1.5,"d":"1.50"},{"v":55,"d":"55.00"},{"v":2318,"d":"2,318.00"},"IN","7326909890","https://www.se.com/sk/sk/product/NSYMR66","montážny perforovaný panel V600xŠ600mm s univerzálnou perforáciou 11x26mm.",0]
["NSYMR3025","3D PERF. MONT. PLECH 1000X1000",1,"ks",{"v":19.674112499999996,"d":"19.674"},"3606480183607",{"v":25.5,"d":"25.50"},{"v":2,"d":"2.00"},{"v":23,"d":"23.00"},{"v":454,"d":"454.00"},"IT","85381000","https://www.se.com/sk/sk/product/NSYMR3025","montážny perforovaný panel V300xŠ250mm s univerzálnou perforaciou 11x26mm.",0]
["NSYMPRK10","ZOSILNENIE MONT. PLECHU 1000",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3606485130736",{"v":85.5,"d":"85.50"},{"v":4.5,"d":"4.50"},{"v":5,"d":"5.00"},{"v":2172,"d":"2,172.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYMPRK10","Spacial SM / Spacial SF vystužená sada pre mont. panel",0]
["NSYMPCH208","PLNÝ ČELNÝ PANEL S PÁNTAMI 200X800",1,"ks",{"v":65.88539999999999,"d":"65.885"},"3606480065767",{"v":75,"d":"75.00"},{"v":1.5,"d":"1.50"},{"v":20.5,"d":"20.50"},{"v":2492,"d":"2,492.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYMPCH208","Spacial SF/SM plný kryt - 200x800 mm - otočný",0]
["NSYMPCH156","PLNÝ ČELNÝ PANEL S PÁNTAMI 150X600",1,"ks",{"v":50.7866625,"d":"50.787"},"3606480065736",{"v":50.5,"d":"50.50"},{"v":1.5,"d":"1.50"},{"v":15,"d":"15.00"},{"v":1383,"d":"1,383.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYMPCH156","Spacial SF/SM plný kryt - 150x600 mm - otočný",0]
["NSYMPC306","PLNÝ ČELNÝ PANEL SKRUTKOVANÝ 300X600",1,"ks",{"v":43.92359999999999,"d":"43.924"},"3606480065897",{"v":60,"d":"60.00"},{"v":1.5,"d":"1.50"},{"v":30,"d":"30.00"},{"v":2606,"d":"2,606.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYMPC306","Spacial SF/SM plný kryt - 300x600 mm - skrutkový",0]
["NSYMP188","ŠTD. MONTÁŽNY PLECH 1800X800",1,"ks",{"v":215.042625,"d":"215.043"},"3606485126845",{"v":171,"d":"171.00"},{"v":3.5,"d":"3.50"},{"v":71,"d":"71.00"},{"v":28000,"d":"28,000.00"},"ES","7326199000","https://www.se.com/sk/sk/product/NSYMP188","Spacial SF/SM montážny panel - 1800x800 mm",0]
["NSYMP1412","ŠTD. MONTÁŽNY PLECH 1400X1200",1,"ks",{"v":283.67325,"d":"283.673"},"3606485130699",{"v":4,"d":"4.00"},{"v":131,"d":"131.00"},{"v":111,"d":"111.00"},{"v":38000,"d":"38,000.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYMP1412","Spacial SF/SM montážny panel - 1400x1200 mm",0]
["NSYMM55","3D MONT. PLECH PLNÝ 500X500",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3606480183379",{"v":46,"d":"46.00"},{"v":0.3,"d":"0.30"},{"v":46,"d":"46.00"},{"v":2944,"d":"2,944.00"},"FR","7326199000","https://www.se.com/sk/sk/product/NSYMM55","plný montážny panel V500xŠ500mm - pozink. ocelový plech",0]
["NSYMM36","3D MONT. PLECH PLNÝ 300X600",1,"ks",{"v":17.8439625,"d":"17.844"},"3606480183324",{"v":60,"d":"60.00"},{"v":0.5,"d":"0.50"},{"v":30,"d":"30.00"},{"v":2050,"d":"2,050.00"},"FR","85381000","https://www.se.com/sk/sk/product/NSYMM36","plný montážny panel V300xŠ600mm - pozink. ocelový plech",0]
["NSYMM2540","3D MONT. PLECH PLNÝ 250X400",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3606480183256",{"v":0.2,"d":"0.20"},{"v":35,"d":"35.00"},{"v":21,"d":"21.00"},{"v":1179,"d":"1,179.00"},"FR","8538100000","https://www.se.com/sk/sk/product/NSYMM2540","plný montážní panel V250xŠ400mm - pozink. ocelový plech",0]
["NSYMM11SB","KOV. MONT. PANEL 150x150",1,"ks",{"v":4.255098749999999,"d":"4.255"},"3606480520501",{"v":14,"d":"14.00"},{"v":0.3,"d":"0.30"},{"v":12.8,"d":"12.80"},{"v":178,"d":"178.00"},"IN","7326909890","https://www.se.com/sk/sk/product/NSYMM11SB","plný mont. panel V150xŠ150mm, galvanizovaný",0]
["NSYMFSC60D","LIŠTA NASTAVITEĽNÁ 600",1,"ks",{"v":20.589187499999998,"d":"20.589"},"3606480065545",{"v":49.5,"d":"49.50"},{"v":2.6,"d":"2.60"},{"v":6.5,"d":"6.50"},{"v":530,"d":"530.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYMFSC60D","Spacial SF/SM sada pre hl. nastaviteľné lišty s držiakmi - 600 mm",0]
["NSYMF54","3D PERFOROVANÝ MONT. PLECH 500x400",1,"ks",{"v":36.145462499999994,"d":"36.145"},"3606480183065",{"v":47,"d":"47.00"},{"v":0.3,"d":"0.30"},{"v":35,"d":"35.00"},{"v":2394,"d":"2,394.00"},"ES","9403991090","https://www.se.com/sk/sk/product/NSYMF54","predvŕtaný mantážny panel V500xŠ400 s otvory 3.6mm s rozostupom 12.5mm",0]
["NSYMD108","SYM. DIN RÁM 1000X800",1,"ks",{"v":137.26125,"d":"137.261"},"3606480182792",{"v":94.5,"d":"94.50"},{"v":4.5,"d":"4.50"},{"v":7.5,"d":"7.50"},{"v":3766,"d":"3,766.00"},"FR","8538100000","https://www.se.com/sk/sk/product/NSYMD108","DIN rám symetrický (6 lišt) pre skriňu 1000x800mm",0]
["NSYMCDFIX","DRŽIAK KÁBLOVÝCH ŽĽABOV",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3606480065385",{"v":15.5,"d":"15.50"},{"v":11.5,"d":"11.50"},{"v":14.5,"d":"14.50"},{"v":688,"d":"688.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYMCDFIX","sada 6 Spacial SF/SM upev. držiaky pre káblové kanály - ocel",0]
["NSYLAMLDS","LED SVIETIDLO SO ZÁSUVKOU SCHUKO",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3606481203045",{"v":40,"d":"40.00"},{"v":6,"d":"6.00"},{"v":7.5,"d":"7.50"},{"v":854.4,"d":"854.40"},"CN","9405423190","https://www.se.com/sk/sk/product/NSYLAMLDS","LED svietidlo so zásuvkou Schuko",0.13]
["NSYINT91","VLOŽKA DO ZÁMKU TROJUHOLNÍK 9 MM",1,"ks",{"v":7.2748462499999995,"d":"7.275"},"3606480065088",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":49,"d":"49.00"},"DE","83014090","https://www.se.com/sk/sk/product/NSYINT91","vložka - trojuholníkový trň 9 mm",0]
["NSYINS71","VLOŽKA DO ZÁMKU ŠTVOREC 7 MM",1,"ks",{"v":9.150749999999999,"d":"9.151"},"3606480065002",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":47,"d":"47.00"},"DE","8301600090","https://www.se.com/sk/sk/product/NSYINS71","vložka - štvorcový trň 7 mm",0]
["NSYIN405E1","VLOŽKA DO ZÁMKU 405E",1,"ks",{"v":17.8439625,"d":"17.844"},"3606480064753",{"v":5.5,"d":"5.50"},{"v":2.5,"d":"2.50"},{"v":4.5,"d":"4.50"},{"v":63,"d":"63.00"},"DE","8301600090","https://www.se.com/sk/sk/product/NSYIN405E1","zámok s kľúčom 405E",0]
["NSYIN1242E1","VLOŽKA DO ZÁMKU 1242E",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3606480064593",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":50,"d":"50.00"},"DE","8301600090","https://www.se.com/sk/sk/product/NSYIN1242E1","zámok s kľúčom 1242E",0]
["NSYGFR166P","Sada 50tich skrutiek M6x16 + plast. podl",1,"ks",{"v":13.229999999999997,"d":"13.230"},"3606480173134",{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":5,"d":"5.00"},"FR","7318159589","https://www.se.com/sk/sk/product/NSYGFR166P","sada 50tich skrutiek M6X16 + plast. podložka",0]
["NSYFPLS3636G","7035 PLS DNO 36X36X13,5",1,"ks",{"v":57.64972499999999,"d":"57.650"},"3606480774010",{"v":38,"d":"38.00"},{"v":15,"d":"15.00"},{"v":38,"d":"38.00"},{"v":1500,"d":"1,500.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYFPLS3636G","Polyester rear part of PLS box 36x36x13.5cm",0]
["NSYFMPLA","THAL. SADA 4 ZÁVESOV",1,"ks",{"v":25.1645625,"d":"25.165"},"3606480193569",{"v":11,"d":"11.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":685,"d":"685.00"},"ES","8302419000","https://www.se.com/sk/sk/product/NSYFMPLA","sada ok pre upevnenie na stenu pre PLA alebo PLAT (4 alebo 6 ok podľa výšky)",0]
["NSYETF","COMBI DRŽIAK",10,"ks",{"v":17.386425,"d":"17.386"},"3606480064425",{"v":11.5,"d":"11.50"},{"v":2,"d":"2.00"},{"v":9,"d":"9.00"},{"v":66.8,"d":"66.80"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYETF","komb. držiaky Spacial SF/SM pre inštal. zem. pásku a lišty DIN.",0]
["NSYEL136D6","ZEMNIACI PÁSIK L130MM 6MM2 D6",10,"ks",{"v":2.4249487499999995,"d":"2.425"},"3606480181610",{"v":13,"d":"13.00"},{"v":1,"d":"1.00"},{"v":1,"d":"1.00"},{"v":11,"d":"11.00"},"FR","8544429090","https://www.se.com/sk/sk/product/NSYEL136D6","zemniaci kábel 6mm2 - d=130 mm (obj.množstvo 10ks)",0]
["NSYECPLAZ103G","7035 THAL.POLYEST.KÁBEL.DNO 1000X320",1,"ks",{"v":58.56479999999999,"d":"58.565"},"3606480801150",{"v":96.5,"d":"96.50"},{"v":0.6,"d":"0.60"},{"v":24.5,"d":"24.50"},{"v":200,"d":"200.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYECPLAZ103G","7035 káblové dno na PLA 1000x320",0]
["NSYEC862","2 DIELNY KÁBLOVÝ VSTUP 800X600 SF",1,"ks",{"v":64.97032499999999,"d":"64.970"},"3606485126470",64.77,2.54,24.13,{"v":4082,"d":"4,082.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYEC862","Spacial SF 2 vst. káblové dno - upevnenie sponami - 800x600 mm",0]
["NSYEC662","2 DIELNY KÁBLOVÝ VSTUP 200X600 SF",1,"ks",{"v":57.192187499999996,"d":"57.192"},"3606485126456",{"v":45,"d":"45.00"},{"v":3,"d":"3.00"},{"v":24,"d":"24.00"},{"v":3000,"d":"3,000.00"},"FR","9403991090","https://www.se.com/sk/sk/product/NSYEC662","Spacial SF 2 vst. káblové dno - upevnenie sponami - 600x600 mm",0]
["NSYEC6121","1 DIELNY KÁBLOVÝ VSTUP 600X1200 SF",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3606480064128",{"v":54,"d":"54.00"},{"v":2.2,"d":"2.20"},{"v":44.4,"d":"44.40"},{"v":7140,"d":"7,140.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYEC6121","Spacial SF 1 vst. káblové dno - upevnenie sponami - 600x1200 mm",0]
["NSYEC36","KÁBLOVÝ VSTUP 300X600 SF",1,"ks",{"v":38.43315,"d":"38.433"},"3606485125947",{"v":51.5,"d":"51.50"},{"v":2.5,"d":"2.50"},{"v":15.5,"d":"15.50"},{"v":1050,"d":"1,050.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYEC36","Spacial SF káblové dno jednodielne - upev. nacvaknutím - 300x600 mm",0]
["NSYEC125","KÁBLOVÝ VSTUP 1200X500 SF",1,"ks",{"v":82.81428749999999,"d":"82.814"},"3606485126128",{"v":51.5,"d":"51.50"},{"v":3,"d":"3.00"},{"v":41.5,"d":"41.50"},{"v":5480,"d":"5,480.00"},"FR","7326199000","https://www.se.com/sk/sk/product/NSYEC125","Spacial SF káblové dno jednodielne - upev. nacvaknutím - 1200x500 mm",0]
["NSYEC108","KÁBLOVÝ VSTUP 1000X800 SF",1,"ks",{"v":86.4745875,"d":"86.475"},"3606485126104",{"v":87,"d":"87.00"},{"v":2.5,"d":"2.50"},{"v":71,"d":"71.00"},{"v":8020,"d":"8,020.00"},"FR","7326199000","https://www.se.com/sk/sk/product/NSYEC108","Spacial SF káblové dno jednodielne - upev. nacvaknutím - 1200x400 mm",0]
["NSYDS3D46","Plné dveře S3D 400x600 mm",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3606480426957",{"v":60.5,"d":"60.50"},{"v":5.5,"d":"5.50"},{"v":41,"d":"41.00"},{"v":3524,"d":"3,524.00"},"FR","73269098","https://www.se.com/sk/sk/product/NSYDS3D46","plné dvere pre Spacial S3D H400xW600 RAL 7035, so zámkom",0]
["NSYDPLA3","THAL. SADA 4 VRÚB.POSUV.DRŽIAKOV HL. 420",1,"ks",109.809,"3606480194375",{"v":40,"d":"40.00"},{"v":4,"d":"4.00"},{"v":16,"d":"16.00"},{"v":1081,"d":"1,081.00"},"ES","8302420090","https://www.se.com/sk/sk/product/NSYDPLA3","sada 4 posuvných líšt pre montáž dosky v PLA H420mm",0]
["NSYDLS48","MODUL. PANEL 270X540,4X12",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3606480188497",{"v":52,"d":"52.00"},{"v":9,"d":"9.00"},{"v":25,"d":"25.00"},{"v":1450,"d":"1,450.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYDLS48","modulárny distrib. rám 48 mod. (18mm) pre PLS skriňku 54x72cm",0]
["NSYDLA48PG","RAL7035 THALASSA MODULÁRNY RÁM 600X400",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3606480773846",{"v":58,"d":"58.00"},{"v":15,"d":"15.00"},{"v":38,"d":"38.00"},{"v":4560,"d":"4,560.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYDLA48PG","modulárny distrib. rám 48 modulov na NSYPLM64,NSYS3D64,NSYCRN64,NSYS3X64",0]
["NSYDLA234G","7035 THALASSA MODULÁRNY RÁM 1000X800",1,"ks",{"v":301.97475,"d":"301.975"},"3606480773815",{"v":99,"d":"99.00"},{"v":14,"d":"14.00"},{"v":78,"d":"78.00"},{"v":12500,"d":"12,500.00"},"ES","8538100000","https://www.se.com/sk/sk/product/NSYDLA234G","modulárny distrib. rám 234 mod. f/ NSYPLM108,NSYS3D108,NSYCRN108,NSYS3X108",0]
["NSYCVF850M230PF","VENTILÁTOR 850M3/H 230V IP54",1,"ks",{"v":320.27625,"d":"320.276"},"3606480151347",{"v":34,"d":"34.00"},{"v":23,"d":"23.00"},{"v":32,"d":"32.00"},{"v":4386,"d":"4,386.00"},"DE","8414592590","https://www.se.com/sk/sk/product/NSYCVF850M230PF","ClimaSys ventilátor IP54 - 850m3/h - 230V - s výstupnou mriežkou a filtrom G2",0.55]
["NSYCVF38M48DPF","VENTILÁTOR 38M3/H 48V DC IP54",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3606480151194",{"v":10,"d":"10.00"},{"v":15,"d":"15.00"},{"v":15,"d":"15.00"},{"v":265,"d":"265.00"},"FR","8414592590","https://www.se.com/sk/sk/product/NSYCVF38M48DPF","ClimaSys ventilátor IP54 - 38m3/h - 48V DC - s výstupnou mriežkou a filtrom G2",0.03]
["NSYCVF170M230","VENTILÁTOR 170M3/H 230V",1,"ks",{"v":70.9183125,"d":"70.918"},"3606480151422",{"v":17,"d":"17.00"},{"v":6,"d":"6.00"},{"v":15,"d":"15.00"},{"v":846,"d":"846.00"},"FR","8414592590","https://www.se.com/sk/sk/product/NSYCVF170M230","Climasys ventilátor - 170 m3/h - 230V bez mriežky",0.1]
["NSYCTL600DLM","PREDNÝ PANEL PRE 3D",2,"ks",{"v":37.0605375,"d":"37.061"},"3606480162725",{"v":3,"d":"3.00"},{"v":60,"d":"60.00"},{"v":16,"d":"16.00"},{"v":935,"d":"935.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYCTL600DLM","plný kovový krycí panel - 12 mod. - RAL 7035 - V150xŠ600mm.",0]
["NSYCSH186","JEDNODUCHÉ ŠASI 1800X600",1,"ks",{"v":205.891875,"d":"205.892"},"3606480063794",{"v":185.5,"d":"185.50"},{"v":6.5,"d":"6.50"},{"v":12.5,"d":"12.50"},{"v":8000,"d":"8,000.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYCSH186","Spacial SF/SM samostatný modulární rám - 240 mod. po 18 mm - 1800x600 mm",0]
["NSYCRN75200P","CRN 700X500X200 , PLNÉ DVERE S MP",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3606480211904",{"v":71,"d":"71.00"},{"v":21.5,"d":"21.50"},{"v":51,"d":"51.00"},{"v":19341,"d":"19,341.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYCRN75200P","Spacial CRN plain door with mount.plate. H700xW500xD200 IP66 IK10 RAL7035..",0]
["NSYCRN66300","CRN 600X600X300 , PLNÉ DVERE",1,"ks",{"v":873.896625,"d":"873.897"},"3606480211966",{"v":61,"d":"61.00"},{"v":32,"d":"32.00"},{"v":61,"d":"61.00"},{"v":15498,"d":"15,498.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYCRN66300","Spacial CRN plain door w/o mount.plate. H600xW600xD300 IP66 IK10 RAL7035..",0]
["NSYCRN46250P","CRN 400X600X250, PLNÉ DVERE, MONT. PANEL",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3606480212369",{"v":27,"d":"27.00"},{"v":42,"d":"42.00"},{"v":62,"d":"62.00"},{"v":13628,"d":"13,628.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYCRN46250P","Spacial CRN plain door with mount.plate. H400xW600xD250 IP66 IK10 RAL7035..",0]
["NSYCRN108250","CRN 1000X800X250 , PLNÉ DVERE",1,"ks",{"v":187.59037499999997,"d":"187.590"},"3606480212710",{"v":101.5,"d":"101.50"},{"v":27,"d":"27.00"},{"v":81,"d":"81.00"},{"v":28466,"d":"28,466.00"},"ES","9403208000","https://www.se.com/sk/sk/product/NSYCRN108250","Spacial CRN plain door w/o mount.plate. H1000xW800xD250 IP66 IK10 RAL7035..",0]
["NSYCR55WU1","VYHRIEV.TELESO 55W, 12-24V",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3606480152153",{"v":20,"d":"20.00"},{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},{"v":324,"d":"324.00"},"CN","8516299100","https://www.se.com/sk/sk/product/NSYCR55WU1","ClimaSys PTC topný odpor 55W - 12 - 24V",0.04]
["NSYCR10WU2","VYHRIEV.TELESO 10W, 110-250V",1,"ks",{"v":45.75375,"d":"45.754"},"3606480152115",{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":126,"d":"126.00"},"CN","8516299100","https://www.se.com/sk/sk/product/NSYCR10WU2","ClimaSys PTC topný odpor 10W - 110 - 250V",0.02]
["NSYCR100WU1","VYHRIEV.TELESO 100W, 12-24V",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3606480152184",{"v":19.5,"d":"19.50"},{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},{"v":476,"d":"476.00"},"CN","8516299100","https://www.se.com/sk/sk/product/NSYCR100WU1","ClimaSys PTC topný odpor 100W - 12 - 24V",0.06]
["NSYCMUMC50","SPOJOVACIA KONZOLA OTOČNÁ",1,"ks",{"v":1052.3362499999998,"d":"1052.336"},"3606480213007",{"v":19,"d":"19.00"},{"v":15.5,"d":"15.50"},{"v":18.5,"d":"18.50"},{"v":5750,"d":"5,750.00"},"DE","7326909890","https://www.se.com/sk/sk/product/NSYCMUMC50","horizontálna otočná konzola - štvorec 50 mm RAL 7040. pre S3CM rozv.",0]
["NSYCMT5015","TRUBICA 1,5M",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3606480213175",{"v":151,"d":"151.00"},{"v":6.2,"d":"6.20"},{"v":6.5,"d":"6.50"},{"v":10570,"d":"10,570.00"},"DE","7306900000","https://www.se.com/sk/sk/product/NSYCMT5015","nosný profil - štvorc. 50 mm - dĺžka: 1 - 5m. pre Spacial S3CM",0]
["NSYCL1242ECSX","CHRÓM.ZÁMOK 1242E",1,"ks",{"v":46.66882499999999,"d":"46.669"},"3606480154812",{"v":9,"d":"9.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":144,"d":"144.00"},"DE","83014090","https://www.se.com/sk/sk/product/NSYCL1242ECSX","pochrom. rukoväť zámok 1242 E pre skriňu Spacial S3X",0]
["NSYCEA36","VÝMEN. VZDUCH-VZDUCH 36W/K 230V BOČNÝ",1,"ks",{"v":1098.09,"d":"1098.090"},"3606480620676",{"v":77.1,"d":"77.10"},{"v":9.3,"d":"9.30"},{"v":31.6,"d":"31.60"},{"v":10000,"d":"10,000.00"},"IT","8419508090","https://www.se.com/sk/sk/product/NSYCEA36","Spacial výmeník vzduch-vzduch 36W/K bočná montáž bez T",1.2]
["NSYCCOTH230VID","TERMOSTAT ELEKTRONICKÝ 230V",1,"ks",{"v":283.67325,"d":"283.673"},"3606480152627",{"v":8.5,"d":"8.50"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":70,"d":"70.00"},"ES","9032102090","https://www.se.com/sk/sk/product/NSYCCOTH230VID","Climasys termostat - 40...80°C - 220-240V AC - elektronický",0.01]
["NSYCAP223LZF","KRYT IP55 223X223MM",1,"ks",{"v":361.45462499999996,"d":"361.455"},"3606480151958",{"v":37,"d":"37.00"},{"v":14,"d":"14.00"},{"v":32,"d":"32.00"},{"v":2920,"d":"2,920.00"},"ES","8421392590","https://www.se.com/sk/sk/product/NSYCAP223LZF","Aluzinc kryt pre otvor 223x223mm s filtrom IP55",0]
["NSYCAG317X91M","VETRACIA MRIEŽKA 317X91MM",5,"ks",{"v":11.895974999999998,"d":"11.896"},"3606480151781",{"v":34.5,"d":"34.50"},{"v":0.5,"d":"0.50"},{"v":12,"d":"12.00"},{"v":314,"d":"314.00"},"ES","85381000","https://www.se.com/sk/sk/product/NSYCAG317X91M","Metal Outlet grille - cut-out 317x91mm ext dim 345x118mm IP20",0]
["NSYCAG125LPF","VETRACIA MRIEŽKA 125X125MM",1,"ks",{"v":27.909787499999997,"d":"27.910"},"3606480151538",{"v":18,"d":"18.00"},{"v":4.5,"d":"4.50"},{"v":15.5,"d":"15.50"},{"v":220,"d":"220.00"},"FR","3926909790","https://www.se.com/sk/sk/product/NSYCAG125LPF","výstupná mriežka s výrezom 125x125mm s ext.priemerom 137x117mm IP54",0]
["NSYCAF291","FILTER ŠTANDARDNÝ 291X291MM",5,"ks",{"v":7.0460775,"d":"7.046"},"3606480151637",{"v":28,"d":"28.00"},{"v":1,"d":"1.00"},{"v":28,"d":"28.00"},{"v":12,"d":"12.00"},"FR","5911909990","https://www.se.com/sk/sk/product/NSYCAF291","štand.filter G2 f/vyst.mriežka/výrez filter.vent.92x92mm vnej.rozm.37x117mm",0]
["NSYCAF125L55","FILTER 125X125MM",5,"ks",{"v":16.9288875,"d":"16.929"},"3606480152047",{"v":22,"d":"22.00"},{"v":3,"d":"3.00"},{"v":16,"d":"16.00"},{"v":2,"d":"2.00"},"ES","5911909990","https://www.se.com/sk/sk/product/NSYCAF125L55","náhradný filter pre sadu EMC IP 55 pre otvor 125x125 mm",0]
["NSYBVS400","2 VERT. DRŽIAK PRÍPOJNÍC 3200A 400",1,"ks",{"v":47.1263625,"d":"47.126"},"3606480062988",{"v":39,"d":"39.00"},{"v":7,"d":"7.00"},{"v":15,"d":"15.00"},{"v":1494,"d":"1,494.00"},"FR","8538100000","https://www.se.com/sk/sk/product/NSYBVS400","2 držiaky vertikálnej prípojnice 3200A Š=400",0]
["NSYBP228","ZADNÝ PANEL SF 2200X800",1,"ks",183.015,"3606485119335",{"v":230,"d":"230.00"},{"v":4.5,"d":"4.50"},{"v":79,"d":"79.00"},{"v":24000,"d":"24,000.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYBP228","Spacial SF zadný panel pre vonkajšie upevnenie - 2200x800 mm",0]
["NSYBP146","ZADNÝ PANEL SF 1400X600",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3606485119151",{"v":149,"d":"149.00"},{"v":3.5,"d":"3.50"},{"v":59.5,"d":"59.50"},{"v":12000,"d":"12,000.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYBP146","Spacial SF zadný panel pre vonkajšie upevnenie - 1400x600 mm",0]
["NSYBP126","ZADNÝ PANEL SF 1200X600",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3606485119137",{"v":120,"d":"120.00"},{"v":3.5,"d":"3.50"},{"v":57.5,"d":"57.50"},{"v":11000,"d":"11,000.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYBP126","Spacial SF zadný panel pre vonkajšie upevnenie - 1200x600 mm",0]
["NSYAZ3PLA","SPOJ SADA HĹBKA 320",1,"ks",{"v":141.836625,"d":"141.837"},"3606480194931",{"v":40,"d":"40.00"},{"v":10.5,"d":"10.50"},{"v":10,"d":"10.00"},{"v":1084,"d":"1,084.00"},"ES","7326909890","https://www.se.com/sk/sk/product/NSYAZ3PLA","spojovacia sada pre inštaláciu PLA+NSYZNPLAxx na 900mm sokel NSYZHPLA H320mm",0]
["NSYAPUS10S","1U NAP. LIŠTA 10 ZÁS+VYP VDE",1,"ks",{"v":171.98999999999998,"d":"171.990"},"3606480171956",{"v":99.3,"d":"99.30"},{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},{"v":1700,"d":"1,700.00"},"DE","8544429090","https://www.se.com/sk/sk/product/NSYAPUS10S","Actassi - vertical power distribution rail - 10 sockets+switch VDE",0]
["NSYAPFWM","SADA NA MONTÁŽ SOKLA",1,"ks",{"v":10.065825,"d":"10.066"},"3606480388071",{"v":17,"d":"17.00"},{"v":1.5,"d":"1.50"},{"v":11,"d":"11.00"},{"v":54,"d":"54.00"},"FR","85381000","https://www.se.com/sk/sk/product/NSYAPFWM","S3D upevňovacia sada pre sokel",0]
["NSYAMPM2924TB","MONTÁŽNA DOSKA KOVOVÁ 291X241",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3606480166105",{"v":27,"d":"27.00"},{"v":1.9,"d":"1.90"},{"v":23.2,"d":"23.20"},{"v":680,"d":"680.00"},"IT","7326199000","https://www.se.com/sk/sk/product/NSYAMPM2924TB","mont. panel z pozink. ocele - tl. 15 mm pre skrinky V275xŠ225 mm",0]
["NSYAEUBUSC","SPOJOVACIA SADA",1,"ks",{"v":8.3271825,"d":"8.327"},"3606480168710",{"v":13.5,"d":"13.50"},{"v":2.5,"d":"2.50"},{"v":10,"d":"10.00"},{"v":98,"d":"98.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSYAEUBUSC","spojovacia sada pre montáž rozvodníc vedľa seba",0]
["NSYAEFAHLBSC","SADA NA ZOSIL. ZÁVESOV",1,"ks",{"v":37.0605375,"d":"37.061"},"3606480168772",10.16,1.27,10.16,{"v":360,"d":"360.00"},"ES","8302419000","https://www.se.com/sk/sk/product/NSYAEFAHLBSC","sada pre velké záťaže. sada zložená z dvoch držiakov. max. zaťaženie 400 kg",0]
["NSYAEDLPADS3D","UZAMYKANIE NA VISIACI ZAMOK 3D",1,"ks",{"v":59.0223375,"d":"59.022"},"3606480168871",{"v":18,"d":"18.00"},{"v":7.4,"d":"7.40"},{"v":8.5,"d":"8.50"},{"v":364,"d":"364.00"},"FR","8301409000","https://www.se.com/sk/sk/product/NSYAEDLPADS3D","úprava pre visiaci zámok pre Spacial S3D rozv.",0]
["NSYAEDL4322S3D","KĽUČKA S3D SO ZÁMKOM 4322A",1,"ks",{"v":35.687925,"d":"35.688"},"3606480449840",{"v":16,"d":"16.00"},{"v":3.5,"d":"3.50"},{"v":14,"d":"14.00"},{"v":52,"d":"52.00"},"FR","8301300000","https://www.se.com/sk/sk/product/NSYAEDL4322S3D","Key handle with key 4322A for Spacial S3D encl, attractive and ergonomic design",0]
["NSYAEDHPLM3025","DOOR HINGE FOR NSYPLM3025",1,"ks",{"v":1.60138125,"d":"1.601"},"3606480482014",{"v":0.8,"d":"0.80"},{"v":0.3,"d":"0.30"},{"v":0.3,"d":"0.30"},{"v":10.5,"d":"10.50"},"","","https://www.se.com/sk/sk/product/NSYAEDHPLM3025","Stainless steel hinge for 2 locks door NSYPLM3025 (former version)",0]
["NSY2SPX205","2 BOČNÉ PANELY 304L 2000X500",1,"ks",{"v":1235.3512499999997,"d":"1235.351"},"3606480154799",{"v":200,"d":"200.00"},{"v":7,"d":"7.00"},{"v":52.5,"d":"52.50"},{"v":30044,"d":"30,044.00"},"BG","85381000","https://www.se.com/sk/sk/product/NSY2SPX205","2 side panels stainless 304L, Scotch Brite® finish, for SFX H2000xD500mm",0]
["NSY2SP224","2 ŠTAND. BOČNÉ PANELY 2200X400",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3606485119977",{"v":229,"d":"229.00"},{"v":6,"d":"6.00"},{"v":39,"d":"39.00"},{"v":24000,"d":"24,000.00"},"FR","7326909890","https://www.se.com/sk/sk/product/NSY2SP224","Spacial SF sada 2 bočníc - 2200x400 mm",0]
["NSY2SP185","2 ŠTAND. BOČNÉ PANELY 1800X500",1,"ks",{"v":173.86424999999997,"d":"173.864"},"3606485119908",{"v":180,"d":"180.00"},{"v":5.5,"d":"5.50"},{"v":47.5,"d":"47.50"},{"v":24400,"d":"24,400.00"},"FR","9403991090","https://www.se.com/sk/sk/product/NSY2SP185","Spacial SF sada 2 bočníc - 1800x500 mm",0]
["NSY17998","MRIEŽKA PRE VENTILÁTOR 460 M3/H EMC",1,"ks",549.045,"3606480169434",{"v":34,"d":"34.00"},{"v":4.5,"d":"4.50"},{"v":33,"d":"33.00"},{"v":1174,"d":"1,174.00"},"DE","3926909790","https://www.se.com/sk/sk/product/NSY17998","výstupná mriežka EMC pre mont. otvor 291 x 291",0]
["NHGF36150TW","Istič PowerPact HG 150A 3P",1,"ks",{"v":542.43,"d":"542.430"},"785901556435",{"v":21.433,"d":"21.43"},{"v":13.018,"d":"13.02"},{"v":18.415,"d":"18.42"},{"v":2268,"d":"2,268.00"},"US","8536209090","https://www.se.com/sk/sk/product/NHGF36150TW","PowerPact multistandard - Rám-H - 150 A - 65 KA - jednotka spúští TM",0.27]
["MUR39723","Prepínač striedavý r.6, IP55, biely",1,"ks",{"v":5.0058539999999985,"d":"5.006"},"3606480789083",{"v":7.1,"d":"7.10"},{"v":7.1,"d":"7.10"},{"v":3.6,"d":"3.60"},{"v":54,"d":"54.00"},"PL","85366990","https://www.se.com/sk/sk/product/MUR39723","Prepínač striedavý razenie 6, Mureva Styl, IP55, Biela",0]
["MUR39203","Klapka so štítkom osvetlená, biela",1,"ks",{"v":2.898125999999999,"d":"2.898"},"3606480790249",{"v":7.1,"d":"7.10"},{"v":1.1,"d":"1.10"},{"v":7,"d":"7.00"},{"v":19,"d":"19.00"},"PL","85366990","https://www.se.com/sk/sk/product/MUR39203","Klapka so štítkom osvetlená, Mureva Styl, Biela",0]
["MUR39035","Komplet 2XZásuvka 16A SCHUKO bezskr. bie",1,"ks",{"v":21.077279999999995,"d":"21.077"},"3606480789717",{"v":14.5,"d":"14.50"},{"v":6.5,"d":"6.50"},{"v":7.5,"d":"7.50"},{"v":251.3,"d":"251.30"},"PL","8536699099","https://www.se.com/sk/sk/product/MUR39035","Komplet 2xzásuvka 16A SCHUKO, Mureva Styl, bezskrutková, Biela",0]
["MUR37021","Prepínač striedavý r.6, IP55, antr.",1,"ks",{"v":5.0058539999999985,"d":"5.006"},"3606480789090",{"v":7.1,"d":"7.10"},{"v":4.2,"d":"4.20"},{"v":7.1,"d":"7.10"},{"v":54,"d":"54.00"},"PL","8536508090","https://www.se.com/sk/sk/product/MUR37021","Prepínač striedavý razenie 6, Mureva Styl, IP55, Antracit",0]
["MUR36133","Zásuvka 16A 2P+E,bezskrutková,IP55,antr.",1,"ks",{"v":5.313230999999998,"d":"5.313"},"3606480789588",{"v":7.1,"d":"7.10"},{"v":7.1,"d":"7.10"},{"v":4.5,"d":"4.50"},{"v":62,"d":"62.00"},"PL","8536699099","https://www.se.com/sk/sk/product/MUR36133","Zásuvka 16A 2P+E, Mureva Styl, bezskrutková, clonky, IP55, Antracit",0]
["MUR35042","Tlačidlový ovládač žalúzií, IP55, antrac",1,"ks",{"v":9.221309999999999,"d":"9.221"},"3606480789465",{"v":8.8,"d":"8.80"},{"v":6,"d":"6.00"},{"v":8.6,"d":"8.60"},{"v":89,"d":"89.00"},"PL","85365080","https://www.se.com/sk/sk/product/MUR35042","Tlačidlový ovládač žalúzií, Mureva Styl, IP55, Antracit",0]
["MUR35023","Komplet Prepínač krížový r.7, IP55 antra",1,"ks",{"v":10.977749999999999,"d":"10.978"},"3606480789205",{"v":7.6,"d":"7.60"},{"v":6.5,"d":"6.50"},{"v":7.6,"d":"7.60"},{"v":126,"d":"126.00"},"PL","8536508090","https://www.se.com/sk/sk/product/MUR35023","Komplet prepínač krížový razenie 7, Mureva Styl, IP55, Antracit",0]
["MUR34203","Klapka so štítkom osvetlená, antracit",1,"ks",{"v":2.898125999999999,"d":"2.898"},"3606480790256",{"v":11.3,"d":"11.30"},{"v":4.4,"d":"4.40"},{"v":9,"d":"9.00"},{"v":18,"d":"18.00"},"PL","85365080","https://www.se.com/sk/sk/product/MUR34203","Klapka so štítkom osvetlená, Mureva Styl, Antracit",0]
["MTN689702","KNX Odbočovacia svorka, žltá/biela 50ks",1,"ks",{"v":42.22417499999999,"d":"42.224"},"3606485012414",{"v":7.6,"d":"7.60"},{"v":5.3,"d":"5.30"},{"v":7.6,"d":"7.60"},{"v":91,"d":"91.00"},"DE","8536901000","https://www.se.com/sk/sk/product/MTN689702","Merten KNX - svorka odbočovacia - yellow/white",0.01]
["MTN683901","ZÁLOHA NAPÁJANIA",1,"ks",{"v":186.67529999999996,"d":"186.675"},"3606485100265",{"v":15.9,"d":"15.90"},{"v":8.2,"d":"8.20"},{"v":12.9,"d":"12.90"},{"v":278,"d":"278.00"},"DE","8504406090","https://www.se.com/sk/sk/product/MTN683901","Merten KNX - napájací zdroj núdzový - REG - light grey",0.04]
["MTN6705-0008","KNX Spacelogic spín./žal. 8k,16A Master",1,"ks",{"v":315.57014999999996,"d":"315.570"},"3606481816962",{"v":15.7,"d":"15.70"},{"v":8,"d":"8.00"},{"v":12.4,"d":"12.40"},{"v":380,"d":"380.00"},"LV","8537109899","https://www.se.com/sk/sk/product/MTN6705-0008","SpaceLogic KNX Switch/Blind Master 8ch 10AX/16AC1",0.05]
["MTN663991","KNX SNÍMAČ OSVETLENIA A TEPLOTY",1,"ks",{"v":425.7974699999999,"d":"425.797"},"3606485100142",{"v":12.4,"d":"12.40"},{"v":7.4,"d":"7.40"},{"v":7.7,"d":"7.70"},{"v":156,"d":"156.00"},"DE","8541410000","https://www.se.com/sk/sk/product/MTN663991","Merten KNX - senzor osvetlenia a teploty - IP54 - light grey",0.02]
["MTN649804","KNX ŽALÚZ. PRVOK REG-K/4X/10 S MAN.OVL. ",1,"ks",{"v":382.2398999999999,"d":"382.240"},"3606485011998",{"v":16,"d":"16.00"},{"v":8,"d":"8.00"},{"v":12.5,"d":"12.50"},{"v":385,"d":"385.00"},"DE","8537109899","https://www.se.com/sk/sk/product/MTN649804","Merten KNX-akčný člen žalúziový-REG-K/4x/10 s man.ovládaním-light grey",0.05]
["MTN647893","KNX SPÍN. PRVOK REG-K/8X230/16 MAN. OVL.",1,"ks",{"v":484.4668499999999,"d":"484.467"},"3606485011790",{"v":28,"d":"28.00"},{"v":8.3,"d":"8.30"},{"v":13,"d":"13.00"},{"v":626,"d":"626.00"},"DE","8537109899","https://www.se.com/sk/sk/product/MTN647893","Merten KNX-akčný člen spínací-REG-K/8x230/16 s man.ovládaním-light grey",0.08]
["MTN639126","KNX TERMOELEKTRICKÝ POHON VENTILU 24V",1,"ks",{"v":49.78007999999999,"d":"49.780"},"3606485099989",{"v":8.5,"d":"8.50"},{"v":10.2,"d":"10.20"},{"v":5.5,"d":"5.50"},{"v":134,"d":"134.00"},"DE","85389099","https://www.se.com/sk/sk/product/MTN639126","Merten KNX - termoelektrický pohon ventilu - 24 VDC - polar white",0.02]
["MTN6304-0019","KNX detektor prítomnosti pre vys.str.Z.M",1,"ks",{"v":262.23434999999995,"d":"262.234"},"3606489818715",{"v":16,"d":"16.00"},{"v":9,"d":"9.00"},{"v":12.5,"d":"12.50"},{"v":278,"d":"278.00"},"RO","8536508090","https://www.se.com/sk/sk/product/MTN6304-0019","KNX High Bay presence detector FM",0.03]
["MTN6270-0000","Ochrana proti demontáži",1,"ks",{"v":13.778414999999997,"d":"13.778"},"3606480934674",{"v":7.3,"d":"7.30"},{"v":2.1,"d":"2.10"},{"v":7.3,"d":"7.30"},{"v":8,"d":"8.00"},"DE","73202081","https://www.se.com/sk/sk/product/MTN6270-0000","ochrana proti demontáži",0]
["MTN625160","KRYT PRE TLAČ. MODUL 1NÁS. TPM ALU. SYSM",1,"ks",{"v":5.200240499999999,"d":"5.200"},"3606485010519",{"v":7.4,"d":"7.40"},{"v":2.2,"d":"2.20"},{"v":7.4,"d":"7.40"},{"v":16,"d":"16.00"},"DE","85389099","https://www.se.com/sk/sk/product/MTN625160","Merten KNX - System M - kryt pre tlačidlový modul 1-nás. - aluminium",0]
["MTN6212-0325","KNX TLAČ. PANEL 2-NÁS. RTM SYSM ACTIVE",1,"ks",{"v":257.7896999999999,"d":"257.790"},"3606480210686",{"v":7.7,"d":"7.70"},{"v":5.7,"d":"5.70"},{"v":7.7,"d":"7.70"},{"v":86,"d":"86.00"},"DE","9032108090","https://www.se.com/sk/sk/product/MTN6212-0325","Merten KNX - System M - RTM tlačidlový panel 2-násobný - active white",0.01]
["MTN619425","KRYT TLAČ.MODUL 1NÁS. H/D TPB ACTIV SYSM",1,"ks",{"v":5.866937999999998,"d":"5.867"},"3606485099569",{"v":7.4,"d":"7.40"},{"v":2.2,"d":"2.20"},{"v":7.4,"d":"7.40"},{"v":18,"d":"18.00"},"DE","85389099","https://www.se.com/sk/sk/product/MTN619425","Merten KNX - System M - kryt pre tlač. modul 1-nás. \"UP/DOWN\" - active white",0]
["MTN6191-6052","Krytky pre 1-násobný tl. modul KNX (1ks)",1,"ks",{"v":3.822398999999999,"d":"3.822"},"3606482215542",{"v":8,"d":"8.00"},{"v":0.5,"d":"0.50"},{"v":7.4,"d":"7.40"},{"v":6.047,"d":"6.05"},"CN","3925901000","https://www.se.com/sk/sk/product/MTN6191-6052","Krytky pre 1-násobný tl. modul KNX (1ks) - mocca kov D-life",""]
["MTN6185-0414","KNX Pro T, tlačidlový ovládač antracit,",1,"ks",{"v":147.56237999999996,"d":"147.562"},"3606481047649",{"v":7.7,"d":"7.70"},{"v":5.7,"d":"5.70"},{"v":7.6,"d":"7.60"},{"v":98,"d":"98.00"},"LV","8536501990","https://www.se.com/sk/sk/product/MTN6185-0414","KNX Pro T, tlačidlový ovládač antracit, System M",0]
["MTN617119","KNX TLAČ.PANEL 1NÁS. PLUS TPB POLAR SYSM",1,"ks",{"v":120.00554999999999,"d":"120.006"},"3606485099415",{"v":7.8,"d":"7.80"},{"v":4.5,"d":"4.50"},{"v":7.4,"d":"7.40"},{"v":64,"d":"64.00"},"DE","8536508090","https://www.se.com/sk/sk/product/MTN617119","Merten KNX - System M - tlačidlový panel 1-násobný - polar white",0.01]
["MTN577625","KRYT TLAČ. STMIEVAČA, ACTIVE SYSM",1,"ks",{"v":25.334504999999993,"d":"25.335"},"3606485098883",{"v":7.4,"d":"7.40"},{"v":3.2,"d":"3.20"},{"v":7.4,"d":"7.40"},{"v":31,"d":"31.00"},"DE","85389099","https://www.se.com/sk/sk/product/MTN577625","Merten - System M - kryt so senzorom pre spínač/tlač. ovl./stmievač - active whi",0]
["MTN5711-0325","Modul PIR Argus180, spínač,active",1,"ks",{"v":85.33727999999998,"d":"85.337"},"3606480370403",{"v":7.6,"d":"7.60"},{"v":6.2,"d":"6.20"},{"v":7.6,"d":"7.60"},{"v":36,"d":"36.00"},"LV","8536508090","https://www.se.com/sk/sk/product/MTN5711-0325","ARGUS 180 flush-mounted sensor module w. switch, active white, glossy, System M",0.01]
["MTN567325","KRYT SPÍNAČA VENTILÁTORA, ACTIVE SYSM",1,"ks",{"v":8.889299999999999,"d":"8.889"},"3606485098616",{"v":7.4,"d":"7.40"},{"v":3.2,"d":"3.20"},{"v":7.4,"d":"7.40"},{"v":31,"d":"31.00"},"DE","39269097","https://www.se.com/sk/sk/product/MTN567325","Merten - System M - kryt pre spínač vent otočný 3-rých. \"3/1/2\" - active white",0]
["MTN536400","TERMOSTAT SO PREP. KONTAK. AC230V, 5(2)A",1,"ks",{"v":77.33690999999999,"d":"77.337"},"3606485007359",{"v":7.8,"d":"7.80"},{"v":5.7,"d":"5.70"},{"v":7.8,"d":"7.80"},{"v":78,"d":"78.00"},"DE","9032102090","https://www.se.com/sk/sk/product/MTN536400","Merten - mechanizmus termostat priestor. - 250VAC - prep. kont. - skrut. svorky",0.09]
["MTN514225","Fra. 2g horiz. f.labell. TPb aw M-Pl",1,"ks",{"v":15.556274999999998,"d":"15.556"},"3606485097749",{"v":15.5,"d":"15.50"},{"v":1,"d":"1.00"},{"v":8,"d":"8.00"},{"v":39,"d":"39.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MTN514225","Cover frame, Merten M-Plan, 2 gangs, active white",0]
["MTN5135-0000","STMIEVAČ OTOČNÝ RL 60-1000VA MERTEN",1,"ks",{"v":88.89299999999999,"d":"88.893"},"3606480298035",{"v":8.5,"d":"8.50"},{"v":8.6,"d":"8.60"},{"v":5.8,"d":"5.80"},{"v":124,"d":"124.00"},"DE","8536508090","https://www.se.com/sk/sk/product/MTN5135-0000","Merten - mechanizmus stmievač otočný - 250VAC - RL 60-1000W/VA - skrut. svorky",0.01]
["MTN469825","KRYT 1 NOS.DOSKY A PREP.MOD, ACTIVE SYSM",1,"ks",{"v":8.889299999999999,"d":"8.889"},"3606485095899",{"v":7.9,"d":"7.90"},{"v":3.3,"d":"3.30"},{"v":7.3,"d":"7.30"},{"v":20,"d":"20.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MTN469825","Merten - System M - kryt pre zásuvku dátovú 1xRJ45 Actassi S-One - active whi",0]
["MTN465860","KRYT ZÁSUVKY DÁT. 1xRJ45 SYSM ALUMINIUM",1,"ks",{"v":10.222694999999998,"d":"10.223"},"3606485005027",{"v":7.4,"d":"7.40"},{"v":3.2,"d":"3.20"},{"v":7.4,"d":"7.40"},{"v":21,"d":"21.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MTN465860","Merten - System M - kryt pre zásuvku dátovú 1xRJ45 Actassi S-One - active alu",0]
["MTN4576-0002","ZÁSUVKA DÁT.ACTASSI 2xRJ45 6 UTP MERTEN",1,"ks",{"v":36.44612999999999,"d":"36.446"},"3606480421280",{"v":7.5,"d":"7.50"},{"v":5.6,"d":"5.60"},{"v":7.5,"d":"7.50"},{"v":54,"d":"54.00"},"DE","8536699099","https://www.se.com/sk/sk/product/MTN4576-0002","Merten - mechanizmus zásuvka dátová 2xRJ45 - Cat.6 UTP - Actassi S-One",0]
["MTN4564-0319","UNI. KR. MASKA 2XRJ45 PRACH. POLAR SYSM",1,"ks",{"v":8.667067499999998,"d":"8.667"},"3606480309632",{"v":8.7,"d":"8.70"},{"v":5.1,"d":"5.10"},{"v":6.9,"d":"6.90"},{"v":12,"d":"12.00"},"DE","85389099","https://www.se.com/sk/sk/product/MTN4564-0319","Merten - System M - kryt pre zásuvku dátovú 2xRJ45 modulárny jack - polar wh",0]
["MTN4562-0325","KRYT ZÁSUVKY DÁT. 2xRJ45 UNI SYSM ACTIVE",1,"ks",{"v":6.933653999999999,"d":"6.934"},"3606480309533",{"v":5.6,"d":"5.60"},{"v":2.3,"d":"2.30"},{"v":5.6,"d":"5.60"},{"v":12,"d":"12.00"},"DE","85389099","https://www.se.com/sk/sk/product/MTN4562-0325","Merten - System M - kryt pre zásuvku dátovú 2xRJ45 modulárny jack - active wh",0]
["MTN435514","KRYT ŽALÚZIOVÉHO SPÍN./TLAČ.OVL SYSM ANT",1,"ks",{"v":7.378119,"d":"7.378"},"3606485004488",{"v":5.6,"d":"5.60"},{"v":2.5,"d":"2.50"},{"v":5.6,"d":"5.60"},{"v":24,"d":"24.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MTN435514","Merten - System M - kryt pre žalúziový spínač/tlačidlový ovládač - anthracite",0]
["MTN433314","KRYT SPÍNAČA POPIS. POLE, ANTRACIT SYSM",1,"ks",{"v":6.533635499999999,"d":"6.534"},"3606485004334",{"v":5.4,"d":"5.40"},{"v":2.5,"d":"2.50"},{"v":5.7,"d":"5.70"},{"v":17,"d":"17.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MTN433314","Merten - System M - kryt pre spínač /prepínač/tlač. ovl. jedn. popis. - ant",0]
["MTN432525","KRYT SPÍNAČA DVOJITÝ, AKT. BIELA SYSM",1,"ks",{"v":5.244687,"d":"5.245"},"3606485094731",{"v":6.8,"d":"6.80"},{"v":3.6,"d":"3.60"},{"v":6.8,"d":"6.80"},{"v":20,"d":"20.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MTN432525","Merten - System M - kryt pre prepínač/tlač. ovládač dvojitý - active white",0]
["MTN4123-6035","Contrálna doska D-Life TV 2/3 Lotus W",1,"ks",{"v":4.889114999999999,"d":"4.889"},"3606480890147",{"v":13.8,"d":"13.80"},{"v":2.2,"d":"2.20"},{"v":9.5,"d":"9.50"},{"v":18,"d":"18.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MTN4123-6035","Centrálna doska, Merten D-Life, pre anténnu zásuvku 2/3 otvory, Lotus White",0]
["MTN4075-6052","Zaslepovací kryt, D-Life, mocca kovový",1,"ks",{"v":37.33505999999999,"d":"37.335"},"3606480889646",{"v":7.3,"d":"7.30"},{"v":3.1,"d":"3.10"},{"v":7.3,"d":"7.30"},{"v":62,"d":"62.00"},"DE","85366990","https://www.se.com/sk/sk/product/MTN4075-6052","Zaslepovací kryt, Merten D-Life, kov, Mocca",0]
["MTN403305","M-ELEGANCE KOV TROJRÁMČEK TITAN",1,"ks",{"v":71.11439999999999,"d":"71.114"},"3606485111230",{"v":24,"d":"24.00"},{"v":2.5,"d":"2.50"},{"v":9.5,"d":"9.50"},{"v":317,"d":"317.00"},"DE","7326909890","https://www.se.com/sk/sk/product/MTN403305","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",0]
["MTN391625","ZASLEPOVACÍ KRYT, ACTIVE SYSM",1,"ks",{"v":6.933653999999999,"d":"6.934"},"3606485094113",{"v":8.7,"d":"8.70"},{"v":2.7,"d":"2.70"},{"v":7.8,"d":"7.80"},{"v":32,"d":"32.00"},"DE","85389099","https://www.se.com/sk/sk/product/MTN391625","Merten - System M - kryt zaslepovací - active white",0]
["MTN3714-0000","ŽALÚZIOVÝ SPÍNAČ 1-P 10A PR.KONT. MERTEN",1,"ks",{"v":19.556459999999998,"d":"19.556"},"3606480307379",{"v":7.1,"d":"7.10"},{"v":3.7,"d":"3.70"},{"v":7.1,"d":"7.10"},{"v":64,"d":"64.00"},"DE","85362010","https://www.se.com/sk/sk/product/MTN3714-0000","Merten - mechanizmus žal. spínač 1-pól. príd. kont. - 10A 250VAC - pruž. svorky",0]
["MTN352419","KRYT PRE BZUČIAK, POLAR SYSM",1,"ks",{"v":8.667067499999998,"d":"8.667"},"3606485093963",{"v":7.4,"d":"7.40"},{"v":3.2,"d":"3.20"},{"v":7.4,"d":"7.40"},{"v":22,"d":"22.00"},"DE","39269097","https://www.se.com/sk/sk/product/MTN352419","Merten - System M - kryt pre signalizáciu zvukovú a bzučiak - polar white",0]
["MTN3325-6036","Kryt spínača D-Life priezor zvon Steel",1,"ks",{"v":7.244779499999999,"d":"7.245"},"3606480888618",{"v":7,"d":"7.00"},{"v":2.7,"d":"2.70"},{"v":7.1,"d":"7.10"},{"v":25,"d":"25.00"},"DE","8538909999","https://www.se.com/sk/sk/product/MTN3325-6036","Kryt spínača, Merten D-Life, s priezorom a symbolom zvončeka, Stainless Steel",""]
["MTN3325-6033","Kryt spínača D-Life priezor zvon Sahara",1,"ks",{"v":7.244779499999999,"d":"7.245"},"3606480888601",{"v":7,"d":"7.00"},{"v":2.7,"d":"2.70"},{"v":7.1,"d":"7.10"},{"v":25,"d":"25.00"},"DE","8538909999","https://www.se.com/sk/sk/product/MTN3325-6033","Kryt spínača, Merten D-Life, s priezorom a symbolom zvončeka, Sahara",""]
["MTN3155-0000","MECHANIZMUS TLAČ. OVLÁDAČA DVOJ. 10 A",1,"ks",{"v":14.667344999999996,"d":"14.667"},"3606480307065",{"v":10.7,"d":"10.70"},{"v":4.1,"d":"4.10"},{"v":7.3,"d":"7.30"},{"v":64,"d":"64.00"},"DE","8536508090","https://www.se.com/sk/sk/product/MTN3155-0000","Merten - mechanizmus tlač. ovl. dvojitý (1/0+1/0) - 10A 250VAC - pruž. svorky",0]
["MTN3116-0000","PREPÍNAČ STRIEDAVÝ, RAD. 6, 10A/250V",1,"ks",{"v":6.533635499999999,"d":"6.534"},"3606480306938",{"v":13.7,"d":"13.70"},{"v":4,"d":"4.00"},{"v":7.4,"d":"7.40"},{"v":56,"d":"56.00"},"DE","8536508090","https://www.se.com/sk/sk/product/MTN3116-0000","Merten - mechanizmus prepínač striedavy (6) - 10AX 250VAC - pruž. svorky",0]
["MTN299825","KRYT TV ZÁS. OZN. R/TV+SAT, ACTIVE SYSM",1,"ks",{"v":4.6224359999999995,"d":"4.622"},"3606485093376",{"v":7.4,"d":"7.40"},{"v":2.7,"d":"2.70"},{"v":6,"d":"6.00"},{"v":14,"d":"14.00"},"DE","8538909999","https://www.se.com/sk/sk/product/MTN299825","Merten - System M - kryt pre zásuvku anténnu TV/R-SAT - active white",0]
["MTN296819","KRYT PRE KÁBLOVÝ VSTUP, POLAR SYSM",1,"ks",{"v":10.667159999999997,"d":"10.667"},"3606485093048",{"v":7.3,"d":"7.30"},{"v":3.4,"d":"3.40"},{"v":7.3,"d":"7.30"},{"v":40,"d":"40.00"},"DE","85389099","https://www.se.com/sk/sk/product/MTN296819","Merten - System M - kryt pre vývodku káblovú - Ø10 mm - polar white",0]
["MTN2600-0325","ZÁSUVKA 2P+PE CLONKY, AKTIV BIELA SYSM",1,"ks",{"v":11.111624999999998,"d":"11.112"},"3606480306426",{"v":9.9,"d":"9.90"},{"v":4.5,"d":"4.50"},{"v":7.6,"d":"7.60"},{"v":80,"d":"80.00"},"DE","8536699099","https://www.se.com/sk/sk/product/MTN2600-0325","Merten - System M - zásuvka 1x2P+PE s cl - 16A 250VAC - skrut sv. - active white",0]
["MTN2367-0460","Zásuvka Schuko 230V USB A+C 3A, alu",1,"ks",{"v":97.78229999999998,"d":"97.782"},"3606489905903",{"v":7.6,"d":"7.60"},{"v":7.5,"d":"7.50"},{"v":6,"d":"6.00"},{"v":115,"d":"115.00"},"NL","8536699099","https://www.se.com/sk/sk/product/MTN2367-0460","Zásuvka 250V/16A Merten, System-M, SCHUKO + USB A+C 3A, Aluminium",0]
["MTN213514","KRYT ZÁSUVKY HOLIAC. STROJ., ANTRAC SYSM",1,"ks",{"v":9.333764999999998,"d":"9.334"},"3606485000145",{"v":12.7,"d":"12.70"},{"v":0.7,"d":"0.70"},{"v":5.6,"d":"5.60"},{"v":15,"d":"15.00"},"DE","39269097","https://www.se.com/sk/sk/product/MTN213514","Merten - System M - kryt pre zásuvku holiaceho strojčeka - anthracite",0]
["MP300-SRD","MP300 pohon se zpětnou pružinou (DOWN) p",1,"ks",{"v":378,"d":"378.000"},"7332552014208",{"v":13,"d":"13.00"},{"v":9.6,"d":"9.60"},{"v":12.8,"d":"12.80"},{"v":800,"d":"800.00"},"SI","8501200090","https://www.se.com/sk/sk/product/MP300-SRD","SpaceLogic MP300-SR PIBCV Actuator, Multi-Signal Control, Spring Return (Closed valve), 24 Vac, 300 N.",0]
["MP130-230T","MP130 pohon 2polohový pro VP228E/VP229E,",1,"ks",{"v":159.46875,"d":"159.469"},"7332552014086",{"v":14.1,"d":"14.10"},{"v":5.5,"d":"5.50"},{"v":12.1,"d":"12.10"},{"v":300,"d":"300.00"},"SI","8501200090","https://www.se.com/sk/sk/product/MP130-230T","SpaceLogic MP130 PIBCV Actuator, Two Position, Non-Spring Return, 230Vac, 130N, IP43",0]
["MIP99038","MINIPRAGMA SVORKOVNICA 8 OTVOROV",1,"ks",{"v":5.291999999999999,"d":"5.292"},"3606480168024",{"v":6,"d":"6.00"},{"v":0.6,"d":"0.60"},{"v":1.7,"d":"1.70"},{"v":30,"d":"30.00"},"IT","8536909500","https://www.se.com/sk/sk/product/MIP99038","Mini Pragma - zemniaca svorkovnica - á otvorov",0]
["MIP30108","ČEL. PANEL BIELY 1R 8M ZAP. BIELE DVERE",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3606480150272",{"v":25.2,"d":"25.20"},{"v":3,"d":"3.00"},{"v":22.2,"d":"22.20"},{"v":375,"d":"375.00"},"IT","8538100000","https://www.se.com/sk/sk/product/MIP30108","čelní kryt - plný - 1x8 mod. - pre Mini Pragma zapust. montáž",0]
["MIP22212S","MINI PRAGMA DYMOVÉ DVERE ZAPUST 2R 24M",1,"ks",47.187,"3606480456060",{"v":37.5,"d":"37.50"},{"v":9.5,"d":"9.50"},{"v":29.5,"d":"29.50"},{"v":1426,"d":"1,426.00"},"IT","8538100000","https://www.se.com/sk/sk/product/MIP22212S","Mini Pragma zapustená rozvodnica - 2x12 mod. - dymové dvere",0]
["MIP12312T","MINI PRAGMA PRIEHĽ. DVERE POVRCH 3R 36M",1,"ks",{"v":73.20599999999999,"d":"73.206"},"3606480147913",{"v":47.5,"d":"47.50"},{"v":10,"d":"10.00"},{"v":26.5,"d":"26.50"},{"v":1593,"d":"1,593.00"},"IT","8538100000","https://www.se.com/sk/sk/product/MIP12312T","mini Pragma - povrchová montáž - 3x12 modulov - priehľadné dvere",0]
["MIP12118S","MINI PRAGMA DYMOVÉ DVERE POVRCH 1R 18M",1,"ks",{"v":40.571999999999996,"d":"40.572"},"3606480455988",{"v":37.5,"d":"37.50"},{"v":10,"d":"10.00"},{"v":23,"d":"23.00"},{"v":1095,"d":"1,095.00"},"IT","85381000","https://www.se.com/sk/sk/product/MIP12118S","Mini Pragma rozvodnica pre povrch.mont. - 1x18 mod. - dymové dvere",0]
["MGU8.601","INŠTALAČNÁ KRABICA 1 PM UNICA",1,"ks",{"v":1.4490629999999995,"d":"1.449"},"8420375140699",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":8.4,"d":"8.40"},"ES","39269097","https://www.se.com/sk/sk/product/MGU8.601","Inštalačná krabica 1 modulová, Unica",0]
["MF550-24M","Pohon motýlkové klapky MF550-24M",1,"ks",{"v":8977.5,"d":"8977.500"},"634558526837",{"v":42,"d":"42.00"},{"v":37,"d":"37.00"},{"v":35,"d":"35.00"},{"v":20750,"d":"20,750.00"},"DE","8501109990","https://www.se.com/sk/sk/product/MF550-24M","MF550 Butterfly Valve Actuator, Modulating, 0-10Vdc or 2-10Vdc, Non-Spring Return, 24Vac, 550Nm, SPDT Aux Switch + Integrated Heater, IP65",2.49]
["MF2050-230F","Pohon motýlkové klapky MF2050-230F",1,"ks",{"v":14789.840624999999,"d":"14789.841"},"634558526882",{"v":60,"d":"60.00"},{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":38000,"d":"38,000.00"},"DE","8501109990","https://www.se.com/sk/sk/product/MF2050-230F","MF2050 Butterfly Valve Actuator, On/Off or 3 Position Floating Control, Non-Spring Return, 230Vac, 2050Nm, SPDT Aux Switch + Integrated Heater, IP65",4.5600000000000005]
["METSEPM5650","POWERLOGIC PM5650 POWER & ENERGY METERS",1,"ks",{"v":2132.1562499999995,"d":"2132.156"},"3606489869717",{"v":12.5,"d":"12.50"},{"v":11.5,"d":"11.50"},{"v":12.5,"d":"12.50"},{"v":646,"d":"646.00"},"IN","9028309000","https://www.se.com/sk/sk/product/METSEPM5650","power meter PowerLogic PM5650, 2 ethernet, up to 63th Harmonic, 1,1MB, waveform, 4DI/2DO 52 alarms",0.08]
["METSEPM5341","PM5341 CL0.5 4TARIF 2-IO ETH. 2REL MID",1,"ks",{"v":1178.2968749999998,"d":"1178.297"},"3606480614057",{"v":10.7,"d":"10.70"},{"v":12,"d":"12.00"},{"v":12.4,"d":"12.40"},{"v":430,"d":"430.00"},"IN","9028309000","https://www.se.com/sk/sk/product/METSEPM5341","analyzátor PM5341, ethernet, 2DI/2DO, 2 relé, MID",0.06]
["METSEPM3200","MULTIMETER ZÁKLADNÝ",1,"ks",{"v":335.15999999999997,"d":"335.160"},"3606480481581",{"v":13.7,"d":"13.70"},{"v":8.8,"d":"8.80"},{"v":13.2,"d":"13.20"},{"v":260,"d":"260.00"},"CN","9028309000","https://www.se.com/sk/sk/product/METSEPM3200","PM3200 multimeter",0.05]
["METSECT5MB030","PRÚDOVÝ TRANSFORMÁTOR 300/5",1,"ks",32.193,"3606480618796",{"v":9,"d":"9.00"},{"v":7.2,"d":"7.20"},{"v":7,"d":"7.00"},{"v":315,"d":"315.00"},"IT","8504318090","https://www.se.com/sk/sk/product/METSECT5MB030","mer. transf. prúdu DIN mont. 300/5 pre káble d. 26 - zbernice 12x40 15x32",0.04]
["METSECT5MA030","PRÚDOVÝ TRANSFORMÁTOR 300/5",1,"ks",{"v":26.900999999999996,"d":"26.901"},"3606480618789",{"v":9,"d":"9.00"},{"v":7.2,"d":"7.20"},{"v":7,"d":"7.00"},{"v":313,"d":"313.00"},"IT","8504318090","https://www.se.com/sk/sk/product/METSECT5MA030","mer. transf. prúdu DIN mont. 300/5 pre káble d. 27 - zbernice 10x32 15x25",0.04]
["METSECT5GJ250","MTP 2500A/5A s split pre pásovinu",1,"ks",{"v":379.25999999999993,"d":"379.260"},"3606489608095",{"v":25,"d":"25.00"},{"v":8.5,"d":"8.50"},{"v":19.5,"d":"19.50"},{"v":3400,"d":"3,400.00"},"HU","8504318090","https://www.se.com/sk/sk/product/METSECT5GJ250","PowerLogic Split Core Current Transformer - Type GJ, for bar - 2500A / 5A",0.48]
["METSECT5GG125","MTP 1250A/5A s split pre pásovinu",1,"ks",{"v":291.05999999999995,"d":"291.060"},"3606489608026",{"v":20,"d":"20.00"},{"v":6,"d":"6.00"},{"v":16,"d":"16.00"},{"v":1552,"d":"1,552.00"},"HU","8504318090","https://www.se.com/sk/sk/product/METSECT5GG125","PowerLogic Split Core Current Transformer - Type GG, for bar - 1250A / 5A",0.19]
["METSECT5DD125","PRÚDOVÝ TRANSFORMÁTOR 1250/5",1,"ks",{"v":74.96999999999998,"d":"74.970"},"3303431123711",{"v":13.5,"d":"13.50"},{"v":10.5,"d":"10.50"},{"v":10,"d":"10.00"},{"v":630,"d":"630.00"},"IT","8504318090","https://www.se.com/sk/sk/product/METSECT5DD125","prúdový transformátor, prevod 1250/5 dvojitý výstup, pre lišty s rozmerom 34x84",0.08]
["METSECT5DC250","PRÚDOVÝ TRANSFORMÁTOR 2500/5",1,"ks",{"v":136.70999999999998,"d":"136.710"},"3303431123780",{"v":17,"d":"17.00"},{"v":13.6,"d":"13.60"},{"v":10.4,"d":"10.40"},{"v":1042,"d":"1,042.00"},"IT","8504318090","https://www.se.com/sk/sk/product/METSECT5DC250","prúdový transformátor, prevod 2500/5 dvojitý výstup, pre lišty s rozmerom 52x127",0.12]
["METSECT5CC013","PRÚDOVÝ TRANSFORMÁTOR 125/5",1,"ks",{"v":31.751999999999995,"d":"31.752"},"3303431123445",{"v":8.2,"d":"8.20"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":174,"d":"174.00"},"IT","8504318090","https://www.se.com/sk/sk/product/METSECT5CC013","prúdový trasnformátor, montáž na DIN, prevod 125/5 pre vodiče, d. 21",0.02]
["MEG4053-3473","Rámček M-Elegance 3násobný Walnut",1,"ks",{"v":52.99800659999998,"d":"52.998"},"4042811171544",{"v":23.2,"d":"23.20"},{"v":1,"d":"1.00"},{"v":9,"d":"9.00"},{"v":115,"d":"115.00"},"DE","4421999999","https://www.se.com/sk/sk/product/MEG4053-3473","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["MEG4052-3470","Rámček M-Elegance 2násobný Beech",1,"ks",{"v":36.001664999999996,"d":"36.002"},"4042811171445",{"v":16.1,"d":"16.10"},{"v":1,"d":"1.00"},{"v":9,"d":"9.00"},{"v":85,"d":"85.00"},"DE","4421999999","https://www.se.com/sk/sk/product/MEG4052-3470","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",0]
["MEG4050-3625","Rámček M-Pure 5násobný Active",1,"ks",{"v":12.996156599999997,"d":"12.996"},"4042811181079",{"v":37.5,"d":"37.50"},{"v":1.6,"d":"1.60"},{"v":9.4,"d":"9.40"},{"v":102,"d":"102.00"},"DE","3926909790","https://www.se.com/sk/sk/product/MEG4050-3625","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["MEG4040-3669","Rámček M-Pure Decor 4násobný Slate/Alu",1,"ks",{"v":48.55335659999999,"d":"48.553"},"4042811180980",{"v":30.4,"d":"30.40"},{"v":2.3,"d":"2.30"},{"v":10.6,"d":"10.60"},{"v":80,"d":"80.00"},"DK","3925901000","https://www.se.com/sk/sk/product/MEG4040-3669","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["MEG4030-6535","Rámček D-Life 3násobný Lotus White",1,"ks",{"v":5.982498899999999,"d":"5.982"},"4042811197810",{"v":24.2,"d":"24.20"},{"v":1.9,"d":"1.90"},{"v":10.1,"d":"10.10"},{"v":38,"d":"38.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MEG4030-6535","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["MEG4030-3619","Rámček M-Pure 3násobný Polar",1,"ks",{"v":9.911569499999997,"d":"9.912"},"4042811181116",{"v":25,"d":"25.00"},{"v":2.8,"d":"2.80"},{"v":10.7,"d":"10.70"},{"v":42,"d":"42.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MEG4030-3619","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",0]
["MEG4025-3614","Rámček M-Pure 2násobný bez str Antracit",1,"ks",{"v":15.387378299999995,"d":"15.387"},"4042811181260",{"v":15.4,"d":"15.40"},{"v":1.1,"d":"1.10"},{"v":8.3,"d":"8.30"},{"v":24,"d":"24.00"},"DE","3925901000","https://www.se.com/sk/sk/product/MEG4025-3614","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",0]
["MEG4020-3669","Rámček M-Pure Decor 2násobný Slate/Alu",1,"ks",{"v":26.187877799999995,"d":"26.188"},"4042811180966",{"v":15.8,"d":"15.80"},{"v":1.2,"d":"1.20"},{"v":8.3,"d":"8.30"},{"v":46,"d":"46.00"},"DK","3925901000","https://www.se.com/sk/sk/product/MEG4020-3669","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",0]
["MEG4010-6550","Rámček D-Life 1násobný kov Nikl",1,"ks",{"v":22.223249999999997,"d":"22.223"},"4042811198084",{"v":12.6,"d":"12.60"},{"v":2.7,"d":"2.70"},{"v":9.5,"d":"9.50"},{"v":110,"d":"110.00"},"DE","7907000090","https://www.se.com/sk/sk/product/MEG4010-6550","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",0]
["MEG4010-3671","Rámček M-Pure Decor 1násobný Wenge/Alu",1,"ks",{"v":13.333949999999998,"d":"13.334"},"4042811180836",{"v":8.3,"d":"8.30"},{"v":1,"d":"1.00"},{"v":8.7,"d":"8.70"},{"v":27,"d":"27.00"},"DK","3925901000","https://www.se.com/sk/sk/product/MEG4010-3671","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",0]
["MD10SR-24TS","KLAPKOVÝ POHON S PRUŽINOU MD10SR-24TS",1,"ks",{"v":419.34375,"d":"419.344"},"3606489660291",{"v":29,"d":"29.00"},{"v":10.5,"d":"10.50"},{"v":13,"d":"13.00"},{"v":2100,"d":"2,100.00"},"SE","8501109190","https://www.se.com/sk/sk/product/MD10SR-24TS","MD10-SR Damper Actuator, 2-Position, Spring Return, 24Vac/Vdc, Dual lead, 10Nm, IP54",0.25]
["MCSESM043F23F0","Modicon Managed Switch 4TX",1,"ks",{"v":571.3784999999999,"d":"571.379"},"3606481463241",{"v":24,"d":"24.00"},{"v":16,"d":"16.00"},{"v":6,"d":"6.00"},{"v":498,"d":"498.00"},"DE","8517620000","https://www.se.com/sk/sk/product/MCSESM043F23F0","network switch, Modicon Networking, managed switch, 4 ports for copper",0.06]
["M9XUPC04","Multi9 sada 4 svoriek pre M9XU",1,"ks",{"v":17.198999999999998,"d":"17.199"},"3606481192851",{"v":11.2,"d":"11.20"},{"v":3.1,"d":"3.10"},{"v":9.1,"d":"9.10"},{"v":139,"d":"139.00"},"DE","8536901000","https://www.se.com/sk/sk/product/M9XUPC04","Multi9 súprava 4 svoriek na M9XU",0.02]
["M9U21270","Istič Multi9 C60H-DC 0.5A C 500V-DC",1,"ks",{"v":53.29925999999999,"d":"53.299"},"3606480741722",{"v":7.5,"d":"7.50"},{"v":8.5,"d":"8.50"},{"v":3.6,"d":"3.60"},{"v":221,"d":"221.00"},"CN","8536201090","https://www.se.com/sk/sk/product/M9U21270","modulárny istič Multi9 C60H-DC 0.5A C 500V-DC",""]
["M9U21125","Istič Multi9 C60H-DC 25A C 250V-DC",1,"ks",{"v":24.793019999999995,"d":"24.793"},"3606480741678",{"v":7.9,"d":"7.90"},{"v":8.5,"d":"8.50"},{"v":1.8,"d":"1.80"},{"v":116,"d":"116.00"},"CN","8536201090","https://www.se.com/sk/sk/product/M9U21125","modulárny istič Multi9 C60H-DC 25A C 250V-DC",""]
["M9U21103","Istič Multi9 C60H-DC 3A C 250V-DC",1,"ks",{"v":24.793019999999995,"d":"24.793"},"3606480741609",{"v":7.2,"d":"7.20"},{"v":8.5,"d":"8.50"},{"v":1.8,"d":"1.80"},{"v":116,"d":"116.00"},"CN","8536201090","https://www.se.com/sk/sk/product/M9U21103","modulárny istič Multi9 C60H-DC 3A C 250V-DC",""]
["M9R81225","Prúd. chránic Multi9 2P 25A 26mA A-SI t",1,"ks",{"v":132.29999999999998,"d":"132.300"},"3606481198419",{"v":9.2,"d":"9.20"},{"v":4.1,"d":"4.10"},{"v":8.5,"d":"8.50"},{"v":212,"d":"212.00"},"FR","8536303099","https://www.se.com/sk/sk/product/M9R81225","prúd. chránič Multi9 2P 25A 26mA A-SI type 120-240V",0.03]
["M9R14440","Proudový chránič ID 4P 40A 300mA AC OEM",1,"ks",{"v":71.42436,"d":"71.424"},"3606480578397",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":8.5,"d":"8.50"},{"v":347,"d":"347.00"},"ES","8536303099","https://www.se.com/sk/sk/product/M9R14440","prúdový chránič ID 4P 40A 300mA AC",""]
["M9L22480","Zvodič prepatia PRD1 75r 2P Typ1 20kA",1,"ks",{"v":209.91599999999994,"d":"209.916"},"3606485010786",{"v":11.7,"d":"11.70"},{"v":4.3,"d":"4.30"},{"v":9.4,"d":"9.40"},{"v":272,"d":"272.00"},"ES","8536309090","https://www.se.com/sk/sk/product/M9L22480","surge arrester, Multi9 PRD1 75r, 2P, 240/480 V",0.01]
["M9F43210","Istič Multi9 C60BP 2P D 10A 10kA 480Y/27",1,"ks",{"v":60.85799999999999,"d":"60.858"},"3606481170309",{"v":10.3,"d":"10.30"},{"v":3.6,"d":"3.60"},{"v":7.2,"d":"7.20"},{"v":238,"d":"238.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F43210","istič Multi9 C60BP 2P D 10A 10kA 480Y/277V UL489",0.03]
["M9F42330","Istič Multi9 C60BP 3P C 30A 10kA 480Y/27",1,"ks",{"v":85.55399999999999,"d":"85.554"},"3606481169914",{"v":10.3,"d":"10.30"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":399,"d":"399.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F42330","istič Multi9 C60BP 3P C 30A 10kA 480Y/277V UL489",0.05]
["M9F42301","Istič Multi9 C60BP 3P C 1A 10kA 480Y/277",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3606481170026",{"v":10.3,"d":"10.30"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":376,"d":"376.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F42301","istič Multi9 C60BP 3P C 1A 10kA 480Y/277V UL489",0.05]
["M9F42203","Istič Multi9 C60BP 2P C 3A 10kA 480Y/277",1,"ks",{"v":69.67799999999998,"d":"69.678"},"3606481169839",{"v":10.3,"d":"10.30"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":244,"d":"244.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F42203","istič Multi9 C60BP 2P C 3A 10kA 480Y/277V UL489",0.03]
["M9F42102","Istič Multi9 C60BP 1P C 2A 10kA 277V UL4",1,"ks",29.988,"3606481169662",{"v":10.3,"d":"10.30"},{"v":7.5,"d":"7.50"},{"v":1.8,"d":"1.80"},{"v":123,"d":"123.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F42102","istič Multi9 C60BP 1P C 2A 10kA 277V UL489",0.01]
["M9F23216","Istič Multi9 C60SP 2P D 16A 10kA 480Y/27",1,"ks",29.988,"3606481168979",{"v":8.5,"d":"8.50"},{"v":3.6,"d":"3.60"},{"v":7.5,"d":"7.50"},{"v":227,"d":"227.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F23216","istič Multi9 C60SP 2P D 16A 10kA 480Y/277V UL1077",0.03]
["M9F23101","Istic Multi9 C60SP 1P D 1A 10kA 277V UL1",1,"ks",{"v":26.900999999999996,"d":"26.901"},"3606481168887",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":1.8,"d":"1.80"},{"v":117,"d":"117.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F23101","istič Multi9 C60SP 1P D 1A 10kA 277V UL1077",0.01]
["M9F22325","Istič Multi9 C60SP 3P C 25A 10kA 480Y/27",1,"ks",{"v":42.776999999999994,"d":"42.777"},"3606481168511",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":344.9,"d":"344.90"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F22325","istič Multi9 C60SP 3P C 25A 10kA 480Y/277V UL1077",0.04]
["M9F22205","Istič Multi9 C60SP 2P C 5A 10kA 480Y/277",1,"ks",{"v":56.888999999999996,"d":"56.889"},"3606481168412",{"v":8.5,"d":"8.50"},{"v":3.6,"d":"3.60"},{"v":7.5,"d":"7.50"},{"v":230,"d":"230.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F22205","istič Multi9 C60SP 2P C 5A 10kA 480Y/277V UL1077",0.03]
["M9F21320","Istič Multi9 C60SP 3P B 20A 10kA 480Y/27",1,"ks",{"v":33.074999999999996,"d":"33.075"},"3606481167910",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":346.9,"d":"346.90"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F21320","istič Multi9 C60SP 3P B 20A 10kA 480Y/277V UL1077",0.04]
["M9F21310","Istič Multi9 C60SP 3P B 10A 10kA 480Y/27",1,"ks",{"v":27.782999999999994,"d":"27.783"},"3606481167941",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":337,"d":"337.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F21310","istič Multi9 C60SP 3P B 10A 10kA 480Y/277V UL1077",0.04]
["M9F17410","MULTI9 C60L 4P 10A C 25kA OEM",1,"ks",{"v":68.79599999999999,"d":"68.796"},"3606480578229",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":7,"d":"7.00"},{"v":430,"d":"430.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F17410","istič - C60L - 4P - 10 A - C char. - 415 V - 25 kA",0.05]
["M9F17210","MULTI9 C60L 2P 10A C 25kA OEM",1,"ks",{"v":33.074999999999996,"d":"33.075"},"3606480578045",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":3.5,"d":"3.50"},{"v":214,"d":"214.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F17210","istič - C60L - 2P - 10 A - C char. - 415 V - 25 kA",0.03]
["M9F17125","MULTI9 C60L 1P 25A C 25kA OEM",1,"ks",{"v":14.552999999999997,"d":"14.553"},"3606480577987",{"v":8.4,"d":"8.40"},{"v":7,"d":"7.00"},{"v":1.7,"d":"1.70"},{"v":113,"d":"113.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F17125","istič - C60L - 1P - 25 A - C char. - 240 V - 25 kA",0.01]
["M9F14310","MULTI9 C60H 3P 10A C 15kA OEM",1,"ks",{"v":31.310999999999996,"d":"31.311"},"3606480577291",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":322,"d":"322.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F14310","istič - C60H - 3P - 10 A - C char. - 415 V - 15 kA",0.04]
["M9F14232","MULTI9 C60H 2P 32A C 15kA OEM",1,"ks",{"v":23.372999999999998,"d":"23.373"},"3606480577222",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":237,"d":"237.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F14232","istič - C60H - 2P - 32 A - C char. - 415 V - 15 kA",0.03]
["M9F12232","MULTI9 C60N 2P 32A D 10kA OEM",1,"ks",{"v":35.72099999999999,"d":"35.721"},"3606480576782",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":236,"d":"236.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F12232","istič - C60N - 2P - 32 A - D char. - 415 V - 10 kA",0.03]
["M9F12103","MULTI9 C60N 1P 3A D 10kA OEM",1,"ks",{"v":8.5113,"d":"8.511"},"3606480576607",{"v":8.5,"d":"8.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":108,"d":"108.00"},"BG","8536201090","https://www.se.com/sk/sk/product/M9F12103","istič - C60N - 1P - 3 A - D char. - 240 V - 10 kA",0]
["M9F11410","MULTI9 C60N 4P 10A C 10kA OEM",1,"ks",{"v":47.62799999999999,"d":"47.628"},"3606480576508",{"v":8.5,"d":"8.50"},{"v":7.2,"d":"7.20"},{"v":7.5,"d":"7.50"},{"v":410,"d":"410.00"},"BG","8536201090","https://www.se.com/sk/sk/product/M9F11410","istič - C60N - 4P - 10 A - C char. - 415 V - 10 kA",0.05]
["M9F11250","MULTI9 C60N 2P 50A C 10kA OEM",1,"ks",{"v":23.813999999999997,"d":"23.814"},"3606480576300",{"v":8.5,"d":"8.50"},{"v":3.6,"d":"3.60"},{"v":7.5,"d":"7.50"},{"v":239,"d":"239.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F11250","istič - C60N - 2P - 50 A - C char. - 415 V - 10 kA",0.03]
["M9F11206","MULTI9 C60N 2P 6A C 10kA OEM",1,"ks",{"v":18.080999999999996,"d":"18.081"},"3606480576232",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":207,"d":"207.00"},"FR","8536201090","https://www.se.com/sk/sk/product/M9F11206","istič - C60N - 2P - 6 A - C char. - 415 V - 10 kA",0.03]
["M9F11103","MULTI9 C60N 1P 3A C 10kA OEM",1,"ks",{"v":8.4231,"d":"8.423"},"3606480576089",{"v":8.5,"d":"8.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":108,"d":"108.00"},"BG","8536201090","https://www.se.com/sk/sk/product/M9F11103","istič - C60N - 1P - 3 A - C char. - 240 V - 10 kA",0]
["M9F10206","MULTI9 C60N 2P 6A B 10kA OEM",1,"ks",{"v":18.080999999999996,"d":"18.081"},"3606480921070",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":208,"d":"208.00"},"BG","8536201090","https://www.se.com/sk/sk/product/M9F10206","istič - C60N - 2P - 6A - B char. - 10kA",0.02]
["M9A26917","Signalizačný kontakt Multi9 SD 2-100mA",1,"ks",{"v":21.608999999999998,"d":"21.609"},"3606482129214",{"v":9.3,"d":"9.30"},{"v":1.8,"d":"1.80"},{"v":7.6,"d":"7.60"},{"v":38.8,"d":"38.80"},"CN","8536508090","https://www.se.com/sk/sk/product/M9A26917","Poruchový kontakt Multi9 SD, 2-100 mA",0]
["LZ2H6X53BD","Hybridný spúštač reverzačný 1,5…6,5A pr",1,"ks",{"v":283.67325,"d":"283.673"},"3606485421223",{"v":12,"d":"12.00"},{"v":3.6,"d":"3.60"},{"v":11.7,"d":"11.70"},{"v":256,"d":"256.00"},"DE","8537109899","https://www.se.com/sk/sk/product/LZ2H6X53BD","reverzačný hybridný spúšťač TeSys H 3kW-400V ovládacie nap. 24VDC pruž. svorky",0.03]
["LZ1H6X5BD","Hybridný spúštač 1,5…6,5A šrouby 24VDC",1,"ks",{"v":256.22099999999995,"d":"256.221"},"3606485421131",{"v":12,"d":"12.00"},{"v":3.6,"d":"3.60"},{"v":11.7,"d":"11.70"},{"v":253,"d":"253.00"},"DE","8537109899","https://www.se.com/sk/sk/product/LZ1H6X5BD","hybridný spúšťač TeSys H 3kW-400V ovládacie nap. 24VDC",0.03]
["LXM32MD30N4","LXM32 MODULAR/VOLIT.KOM.3KW 3F 380/480V",1,"ks",{"v":2179.4849999999997,"d":"2179.485"},"3606480076893",{"v":33,"d":"33.00"},{"v":10.5,"d":"10.50"},{"v":27.5,"d":"27.50"},{"v":2700,"d":"2,700.00"},"DE","8504409590","https://www.se.com/sk/sk/product/LXM32MD30N4","servopohon - Lexium 32 - 3 fáz. napájacie napätie 208/480V - 3 kW",0.39]
["LXM32CD72N4","SERVOMENIČ LN / LP = 24 / 72 A, 3 x 400",1,"ks",{"v":2709.63,"d":"2709.630"},"3606480216220",{"v":33,"d":"33.00"},{"v":14.5,"d":"14.50"},{"v":27.5,"d":"27.50"},{"v":4800,"d":"4,800.00"},"DE","8504409590","https://www.se.com/sk/sk/product/LXM32CD72N4","servopohon - Lexium 32 - 3 fáz. napájacie napätie 208/480V - 7 kW",0.66]
["LXM28EU04M3X","Lexium28 Drive 3 x 220V, EtherCAT,  400W",1,"ks",1095.633,"3606481167279",23.88,7.87,23.11,{"v":1260,"d":"1,260.00"},"CN","8537109199","https://www.se.com/sk/sk/product/LXM28EU04M3X","motion servo drive, Lexium 28, single and three phase, 200 to 240V, 400W, EtherCat",0.15]
["LXM28AU01M3X","Lexium28 IO, CAN, 100W",1,"ks",{"v":827.0262,"d":"827.026"},"3606480711763",{"v":23.7,"d":"23.70"},{"v":7.5,"d":"7.50"},{"v":23,"d":"23.00"},{"v":1260,"d":"1,260.00"},"CN","8537109199","https://www.se.com/sk/sk/product/LXM28AU01M3X","motion servo pohon - Lexium 28 - jedno a trojfáz 200...230 V - 100 W",0.27]
["LXD1D7","CIEVKA STÝKAČA 42V",1,"ks",{"v":19.216575,"d":"19.217"},"3389110467703",{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":6.2,"d":"6.20"},{"v":70,"d":"70.00"},"FR","8504500090","https://www.se.com/sk/sk/product/LXD1D7","cievka stýkača - 42V 50/60Hz pre 9... 38A stýkač",0]
["LX4FL220","CIEVKA STÝKAČA",1,"ks",{"v":722.9092499999999,"d":"722.909"},"3389110083743",{"v":22.5,"d":"22.50"},{"v":10,"d":"10.00"},{"v":11.5,"d":"11.50"},{"v":1388,"d":"1,388.00"},"CZ","8504500090","https://www.se.com/sk/sk/product/LX4FL220","cievka stýkača - 220V DC",0]
["LX4F8MW","CIEVKA STÝKAČA",1,"ks",{"v":809.8413749999999,"d":"809.841"},"3389110955552",{"v":22.5,"d":"22.50"},{"v":10.5,"d":"10.50"},{"v":12,"d":"12.00"},{"v":1441,"d":"1,441.00"},"CZ","8504500090","https://www.se.com/sk/sk/product/LX4F8MW","TeSys F - contactor coil - LX4F8 - 220...240 V DC",0]
["LX1G4QLSEA","Riadiaci m.200-500V AC / DC 4P 115/225 p",1,"ks",{"v":283.67325,"d":"283.673"},"3606481946386",{"v":22,"d":"22.00"},{"v":17,"d":"17.00"},{"v":22,"d":"22.00"},{"v":1100,"d":"1,100.00"},"CN","8505909090","https://www.se.com/sk/sk/product/LX1G4QLSEA","Riadiaci modul 200-500V AC / DC pre 4P TeSys G 115/225 pokročilý",0.13]
["LX1G3RKUEN","Riadiaci m.100-250V AC / DC 3P 265/300 s",1,"ks",{"v":247.07024999999996,"d":"247.070"},"3606481946317",{"v":22,"d":"22.00"},{"v":17,"d":"17.00"},{"v":24,"d":"24.00"},{"v":1500,"d":"1,500.00"},"CN","8505909090","https://www.se.com/sk/sk/product/LX1G3RKUEN","Riadiaci modul 100-250V AC / DC pre 3P TeSys G 265/300 štandard",0.18]
["LX1FH3802","CIEVKA STÝKAČA",1,"ks",{"v":343.15312499999993,"d":"343.153"},"3389110553376",9.14,18.54,10.16,{"v":850,"d":"850.00"},"CZ","8504500090","https://www.se.com/sk/sk/product/LX1FH3802","cievka stýkača - 380...415V 40...400Hz",0]
["LX1D6F5","CIEVKA STÝKAČA",1,"ks",{"v":49.8715875,"d":"49.872"},"3389110232745",{"v":12.5,"d":"12.50"},{"v":5.5,"d":"5.50"},{"v":9,"d":"9.00"},{"v":312,"d":"312.00"},"CZ","8505902999","https://www.se.com/sk/sk/product/LX1D6F5","TeSys D - cievka stýkača - LX1D6 - 110 V AC 50 Hz for 80 & 95 A stýkač",0]
["LVSXV318","PrismaSet nástenná 54M (3x18) Media",1,"ks",{"v":70.55999999999999,"d":"70.560"},"3606481099914",{"v":61,"d":"61.00"},{"v":15.5,"d":"15.50"},{"v":44,"d":"44.00"},{"v":9478,"d":"9,478.00"},"IT","8538100000","https://www.se.com/sk/sk/product/LVSXV318","PrismaSet nástenná 54M (3x18) Media",0]
["LVSXQ624","PrismaSet nástenná 144M (6x24) biele dv.",1,"ks",{"v":233.72999999999996,"d":"233.730"},"3606481073075",{"v":113.5,"d":"113.50"},{"v":22,"d":"22.00"},{"v":64,"d":"64.00"},{"v":20918,"d":"20,918.00"},"IT","8538100000","https://www.se.com/sk/sk/product/LVSXQ624","PrismaSet nástenná 144M (6x24) biele dv.",0]
["LVSXQ324","PrismaSet nástenná 72M (3x24) biele dv.",1,"ks",{"v":158.75999999999996,"d":"158.760"},"3606481073044",{"v":69,"d":"69.00"},{"v":21.5,"d":"21.50"},{"v":63.5,"d":"63.50"},{"v":12474,"d":"12,474.00"},"IT","8538100000","https://www.se.com/sk/sk/product/LVSXQ324","PrismaSet nástenná 72M (3x24) biele dv.",0]
["LVSXN624","PrismaSet zapustená 144M (6x24) biele dv",1,"ks",{"v":282.23999999999995,"d":"282.240"},"3606481073273",{"v":113.8,"d":"113.80"},{"v":22,"d":"22.00"},{"v":63.6,"d":"63.60"},{"v":22960,"d":"22,960.00"},"IT","8538100000","https://www.se.com/sk/sk/product/LVSXN624","PrismaSet zapustená 144M (6x24) biele dv.",0]
["LVSXK2","Sada držáku pre svorkovnice 24M",1,"ks",{"v":6.570899999999999,"d":"6.571"},"3606481072849",{"v":46,"d":"46.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":238,"d":"238.00"},"IT","3926909790","https://www.se.com/sk/sk/product/LVSXK2","Sada držáku pre svorkovnice 24M",0]
["LVSXDT124","PrismaSet priehľadné dv. 1 řada 24M",1,"ks",{"v":132.29999999999998,"d":"132.300"},"3606481073396",{"v":63.5,"d":"63.50"},{"v":7,"d":"7.00"},{"v":39,"d":"39.00"},{"v":2900,"d":"2,900.00"},"IT","8538909999","https://www.se.com/sk/sk/product/LVSXDT124","PrismaSet priehľadné dv. 1 řada 24M",0]
["LVSXDP318","PrismaSet biele dv. 54M (3x18)",1,"ks",{"v":18.962999999999997,"d":"18.963"},"3606481099945",{"v":60.5,"d":"60.50"},{"v":6,"d":"6.00"},{"v":45,"d":"45.00"},{"v":1450,"d":"1,450.00"},"BG","8538909999","https://www.se.com/sk/sk/product/LVSXDP318","PrismaSet biele dv. 54M (3x18)",0]
["LVSXDP113","PrismaSet biele dv. 13M (1x13)",1,"ks",{"v":12.347999999999997,"d":"12.348"},"3606482041455",{"v":36,"d":"36.00"},{"v":5,"d":"5.00"},{"v":31,"d":"31.00"},{"v":578,"d":"578.00"},"BG","8538909999","https://www.se.com/sk/sk/product/LVSXDP113","PrismaSet biele dv. 13M (1x13)",0]
["LVS08936","ZÁPADKA DVERÍ + 2 KĽÚČE 405 IP55",1,"ks",{"v":12.99375,"d":"12.994"},"3606481885517",{"v":6,"d":"6.00"},{"v":3.8,"d":"3.80"},{"v":5.5,"d":"5.50"},{"v":122,"d":"122.00"},"FR","8302420090","https://www.se.com/sk/sk/product/LVS08936","IP55 DOOR LATCH+LOCK-2X405KEYS",0]
["LVS08911","PE-VODIČ 6MM2",1,"ks",{"v":6.614999999999998,"d":"6.615"},"3606481870742",{"v":15,"d":"15.00"},{"v":0.5,"d":"0.50"},{"v":4,"d":"4.00"},{"v":45,"d":"45.00"},"FR","8544429090","https://www.se.com/sk/sk/product/LVS08911","Wire, PrismaSeT P & G, with a 5mm² diameter lug at one end and a 6mm² diameter lug on the other, W200mm",0]
["LVS08888","KRYCIA DOSKA PRE PODSTAVEC PRE PREP. ODD",1,"ks",{"v":33.074999999999996,"d":"33.075"},"3606481884138",{"v":29,"d":"29.00"},{"v":2.3,"d":"2.30"},{"v":16,"d":"16.00"},{"v":507,"d":"507.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08888","Gland plate, PrismaSeT G, plinth mounted, for floor-standing enclosure, W300mm, IP31 to IP43, white, RAL 9003",0]
["LVS08867","2 DRŽIAKY KÁBL. ÚCHYTIEK PRE NÁSTEN.-STO",1,"ks",{"v":10.8084375,"d":"10.808"},"3606481866707",{"v":49.7,"d":"49.70"},{"v":2.4,"d":"2.40"},{"v":3,"d":"3.00"},{"v":418,"d":"418.00"},"IT","7326909890","https://www.se.com/sk/sk/product/LVS08867","Cable-tie support, PrismaSeT G, for enclosure W600, Set of 2",0]
["LVS08815","Kombinačná sada, Prisma G, pre IP30",1,"ks",{"v":34.25625,"d":"34.256"},"3606481884060",{"v":31.5,"d":"31.50"},{"v":5,"d":"5.00"},{"v":7.8,"d":"7.80"},{"v":825,"d":"825.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08815","Combination kit, PrismaSeT G, for floor standing enclosure, IP30",0]
["LVS08783","LIŠTA C PRE UPEVNENIE KABELOV, L1600",1,"ks",{"v":218.53125,"d":"218.531"},"3606481883223",{"v":161,"d":"161.00"},{"v":3,"d":"3.00"},{"v":5,"d":"5.00"},{"v":2475,"d":"2,475.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08783","Cable-tie support, PrismaSeT P and G, Form C, L1600",0]
["LVS08748","ZADNÝ PANEL IP55 Š800",1,"ks",{"v":295.3125,"d":"295.313"},"3606481877826",{"v":206.5,"d":"206.50"},{"v":4,"d":"4.00"},{"v":82.5,"d":"82.50"},{"v":21650,"d":"21,650.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08748","Rear panel, PrismaSeT P, for enclosure, W800mm, IP55, white, RAL 9003",0]
["LVS08722","SPÁJACÍ DIEL",1,"ks",{"v":49.021875,"d":"49.022"},"3606481869937",{"v":22.5,"d":"22.50"},{"v":6.5,"d":"6.50"},{"v":15.5,"d":"15.50"},{"v":660,"d":"660.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08722","Reinforcement kit, PrismaSeT P, Combination Kit For Lifting",0]
["LVS08712","Sada rohových prvkov IP30 PRE LINERGY LG",1,"ks",{"v":761.90625,"d":"761.906"},"3606481884077",{"v":82,"d":"82.00"},{"v":16.5,"d":"16.50"},{"v":53.5,"d":"53.50"},{"v":18190,"d":"18,190.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08712","Right-angle kit, PrismaSeT P, corner kit for Linergy LGYE, IP30",0]
["LVS08684","PLNÁ KRYCIA DOSKA IP55 Š400 H600",1,"ks",{"v":111.0375,"d":"111.038"},"3606481877604",{"v":59,"d":"59.00"},{"v":4.5,"d":"4.50"},{"v":32,"d":"32.00"},{"v":3223,"d":"3,223.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08684","Gland plate, PrismaSeT P, Plain type, for enclosure W400mm, D600mm, IP55, white, RAL 9003",0]
["LVS08653","PLNÁ STRIEŠKA IP55 Š300 H600",1,"ks",{"v":71.465625,"d":"71.466"},"3606481877536",{"v":62.5,"d":"62.50"},{"v":4,"d":"4.00"},{"v":32,"d":"32.00"},{"v":2182,"d":"2,182.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08653","Roof plate, PrismaSeT P, for enclosure, W300mm, D600mm, IP55, white, RAL 9003",0]
["LVS08593","DVERE S VÝREZOM PRE MERAČE IP30 Š300",1,"ks",{"v":313.03125,"d":"313.031"},"3606481884305",{"v":197.5,"d":"197.50"},{"v":7,"d":"7.00"},{"v":36,"d":"36.00"},{"v":9550,"d":"9,550.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08593","Door, PrismaSeT P, for floor-standing, HSI cut-out, reversible opening, 36M, W300, 2 locks, IP30, White, RAL 9003",0]
["LVS08514","PLNÉ DVERE IP30 Š400",1,"ks",{"v":189,"d":"189.000"},"3606481878670",{"v":198.5,"d":"198.50"},{"v":7,"d":"7.00"},{"v":46.5,"d":"46.50"},{"v":13650,"d":"13,650.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08514","Door, PrismaSeT P, plain type for enclosure, W400, 36M, IP30, white, RAL 9003",0]
["LVS08483","PLNÁ KRYCIA DOSKA IP55 Š300 H400",1,"ks",{"v":87.4125,"d":"87.413"},"3606481877352",{"v":38,"d":"38.00"},{"v":5,"d":"5.00"},{"v":27.9,"d":"27.90"},{"v":1733,"d":"1,733.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08483","Gland plate, PrismaSeT P, Plain type, for enclosure W300mm, D400mm, IP55, white, RAL 9003",0]
["LVS08408","RÁM Š800 H400",1,"ks",{"v":253.96875,"d":"253.969"},"3606481879219",{"v":203,"d":"203.00"},{"v":9,"d":"9.00"},{"v":42.2,"d":"42.20"},{"v":19900,"d":"19,900.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08408","Framework, PrismaSet P, for Enclosures W800mm, D400mm",0]
["LVS08384","VERTIKÁLNA PREPÁŽKA PRISMA G, IP55",1,"ks",{"v":54.928125,"d":"54.928"},"3606481880055",{"v":55.5,"d":"55.50"},{"v":1,"d":"1.00"},{"v":25.3,"d":"25.30"},{"v":1122,"d":"1,122.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08384","Partition, PrismaSeT G, vertical, IP55",0]
["LVS08349","PLNÉ DVERE IP55 33M",1,"ks",{"v":785.53125,"d":"785.531"},"3606481876713",{"v":174,"d":"174.00"},{"v":11,"d":"11.00"},{"v":34.5,"d":"34.50"},{"v":28870,"d":"28,870.00"},"IT","7326909890","https://www.se.com/sk/sk/product/LVS08349","Rear panel & door, PrismaSeT G, for extension duct, 33M, W300mm, H1750mm, IP55",0]
["LVS08337","PRIEHĽADNÉ DVERE IP55 27M",1,"ks",{"v":490.21875,"d":"490.219"},"3606481878571",{"v":144.5,"d":"144.50"},{"v":7.5,"d":"7.50"},{"v":60,"d":"60.00"},{"v":21300,"d":"21,300.00"},"FR","3926909790","https://www.se.com/sk/sk/product/LVS08337","Door, PrismaSeT G, transparent with frame, 27M, W600, IP55, white, RAL 9003",0]
["LVS08322","PLNÉ DVERE IP55 7M",1,"ks",{"v":236.25,"d":"236.250"},"3606481878441",{"v":60,"d":"60.00"},{"v":8,"d":"8.00"},{"v":44,"d":"44.00"},{"v":7937,"d":"7,937.00"},"FR","3926909790","https://www.se.com/sk/sk/product/LVS08322","Door, PrismaSeT G, plain type with frame, 7M, W600, IP55, white, RAL 9003",0]
["LVS08307","NÁSTENNÁ-STOJACA SKRIŇA IP55 27M",1,"ks",{"v":466.59375,"d":"466.594"},"3606481876553",{"v":146,"d":"146.00"},{"v":11.5,"d":"11.50"},{"v":64,"d":"64.00"},{"v":25850,"d":"25,850.00"},"FR","9403208000","https://www.se.com/sk/sk/product/LVS08307","Enclosure, PrismaSeT G, wall mounted/floor standing, without plinth, 27M, W600mm, H1450mm, IP55",0]
["LVS08283","DVERE PREPOJ. ODDIELU 30M STOJACA SKRIŇA",1,"ks",{"v":147.65625,"d":"147.656"},"3606481878373",{"v":160,"d":"160.00"},{"v":7,"d":"7.00"},{"v":34,"d":"34.00"},{"v":7340,"d":"7,340.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08283","Door, PrismaSeT G, plain type for duct, 30M, W300, IP30, white, RAL 9003",0]
["LVS08215","PRÍDAVNÁ STOJACA SKRIŇA Š600 36M",1,"ks",{"v":454.78125,"d":"454.781"},"3606481876416",{"v":189.5,"d":"189.50"},{"v":10.5,"d":"10.50"},{"v":66,"d":"66.00"},{"v":29500,"d":"29,500.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS08215","Extension enclosure, PrismaSeT G, Floor standing, without side plates, 36M, W600mm, H2030mm, IP30",0]
["LVS08182","DVERE PREPOJ. ODDIELU 6M SKRIŇA",1,"ks",{"v":85.05,"d":"85.050"},"3606481884374",{"v":39.5,"d":"39.50"},{"v":7,"d":"7.00"},{"v":34,"d":"34.00"},{"v":2260,"d":"2,260.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS08182","Door, PrismaSeT G, plain type for duct, 6M, W300, IP30, white, RAL 9003",0]
["LVS08173","PREPOJ. ODDIEL Š300 NÁSTENNÁ SKRIŇA 9M",1,"ks",{"v":147.65625,"d":"147.656"},"3606481877048",{"v":67,"d":"67.00"},{"v":10,"d":"10.00"},{"v":54.5,"d":"54.50"},{"v":7091,"d":"7,091.00"},"FR","9403208000","https://www.se.com/sk/sk/product/LVS08173","Duct, PrismaSeT G, wall mounted, without side plates, 9M, W300mm, H480mm, IP30",0]
["LVS08122","PLNÉ DVERE 6M SKRIŇA",1,"ks",{"v":76.190625,"d":"76.191"},"3606481879004",{"v":64.5,"d":"64.50"},{"v":7,"d":"7.00"},{"v":38,"d":"38.00"},{"v":3500,"d":"3,500.00"},"FR","9403991090","https://www.se.com/sk/sk/product/LVS08122","Door, PrismaSeT G, plain type for enclosure, 6M, W600 , IP30, white, RAL 9003",0]
["LVS08109","NÁSTENNÁ SKRIŇA Š600 27M",1,"ks",{"v":248.0625,"d":"248.063"},"3606481876959",{"v":144,"d":"144.00"},{"v":10,"d":"10.00"},{"v":65.5,"d":"65.50"},{"v":21500,"d":"21,500.00"},"FR","9403208000","https://www.se.com/sk/sk/product/LVS08109","Enclosure, PrismaSeT G, wall mounted, 27M, W600mm, H1380mm, IP30",0]
["LVS07944","VLOŽKA Č. 2433A",1,"ks",{"v":5.197500000000001,"d":"5.198"},"3606481885050",{"v":6,"d":"6.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":44,"d":"44.00"},"FR","8301409000","https://www.se.com/sk/sk/product/LVS07944","Bloc with barrel lock, PrismaSeT P and G, with 2 keys no. 2433A",0]
["LVS07938","KLIKA PRE 2 VISIACE ZÁMKY",1,"ks",{"v":8.8003125,"d":"8.800"},"3606481885180",{"v":14.5,"d":"14.50"},{"v":2.5,"d":"2.50"},{"v":4,"d":"4.00"},{"v":175,"d":"175.00"},"FR","8301409000","https://www.se.com/sk/sk/product/LVS07938","Padlocking device, PrismaSeT P and G, for new rotary handle, 2 locks",0]
["LVS04954","PREPÁŽKA TYP 4 PRE TRANSF. 4/6M",1,"ks",212.625,"3606481880413",{"v":33,"d":"33.00"},{"v":3.5,"d":"3.50"},{"v":29,"d":"29.00"},{"v":2728,"d":"2,728.00"},"HU","7326909890","https://www.se.com/sk/sk/product/LVS04954","Cover, PrismaSeT P, Form 4b, cover for connection transfer assembly in duct for 4 to 6 modules",0]
["LVS04928","Doplň. kryt pripojenia LGYE, Š650, H600",1,"ks",{"v":153.5625,"d":"153.563"},"3606481883759",{"v":58,"d":"58.00"},{"v":2.4,"d":"2.40"},{"v":19.2,"d":"19.20"},{"v":1076,"d":"1,076.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS04928","Connection cover, PrismaSeT P, additional partition of prefabricated connection LGYE D650, D600mm",0]
["LVS04844","KRYT PRED. PRÍVODOV PRE VERT. NS1600 HOR",1,"ks",{"v":555.1875,"d":"555.188"},"3606481883766",{"v":84,"d":"84.00"},{"v":5.5,"d":"5.50"},{"v":64.5,"d":"64.50"},{"v":6124,"d":"6,124.00"},"CZ","7326909890","https://www.se.com/sk/sk/product/LVS04844","Rear connection cover, PrismaSeT P, for NS1600 horizontal fixed",0]
["LVS04772","20 PODLOŽIEK PRIEM. 20 PRE IZOL. FLEXIBI",1,"ks",{"v":1.1221875,"d":"1.122"},"3606481885685",{"v":6.5,"d":"6.50"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":78,"d":"78.00"},"FR","7318220098","https://www.se.com/sk/sk/product/LVS04772","Flat washer, Linergy LGY, M8, 20mm dia, for flexible busbar, set of 20",0]
["LVS04746","IZOLOVANÁ FLEXIBILNÁ ZBERNICA 24X5 D1800",1,"ks",{"v":81.50625,"d":"81.506"},"3606481868251",{"v":193.5,"d":"193.50"},{"v":1.5,"d":"1.50"},{"v":12,"d":"12.00"},{"v":2554,"d":"2,554.00"},"FR","8544499500","https://www.se.com/sk/sk/product/LVS04746","Insulated flexible bar, PrismaSeT P and G, 400 A, busbar size 24 x 5mm, length 1800mm, set of 1",0]
["LVS04694","DRŽIAK PRÍVODOV 115MM ROZTEČ",1,"ks",{"v":53.746874999999996,"d":"53.747"},"3606481867193",{"v":57.8,"d":"57.80"},{"v":6.8,"d":"6.80"},{"v":12,"d":"12.00"},{"v":2549,"d":"2,549.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS04694","Terminal extension support, Linergy BS, rear busbar, 115mm busbar/centres, 2500A",0]
["LVS04685","SPOJKA LINERGY LGYE 2500A, NW",1,"ks",{"v":135.84375,"d":"135.844"},"3606481868091",{"v":23,"d":"23.00"},{"v":9.5,"d":"9.50"},{"v":14.8,"d":"14.80"},{"v":2009.9999999999998,"d":"2,010.00"},"FR","7419809099","https://www.se.com/sk/sk/product/LVS04685","Connection, PrismaSeT P, copper joint on profile Linergy vertical LGYE 2500A for connection NW",0]
["LVS04656","SADA VERTIK. PEN-ZBERNICE LINERGY",1,"ks",{"v":324.84375,"d":"324.844"},"3606481867094",{"v":54,"d":"54.00"},{"v":12.5,"d":"12.50"},{"v":11.3,"d":"11.30"},{"v":4474,"d":"4,474.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LVS04656","Mounting kit, Linergy TB, PEN installation kit with LGY vertical profile",0]
["LVS04620","SPOJKA PRÍPOJNICE LINERGY EVOLUTION 1600",1,"ks",{"v":64.378125,"d":"64.378"},"3606481868008",{"v":12.5,"d":"12.50"},{"v":4,"d":"4.00"},{"v":6.5,"d":"6.50"},{"v":775,"d":"775.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LVS04620","Connection, Linergy LGY, for horizontal busbar joint connection 1600A",0]
["LVS04602","SPOJKA PRÍPOJNICE LINERGY EVOLUTION 1600",1,"ks",{"v":62.015625,"d":"62.016"},"3606481867957",{"v":14.5,"d":"14.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":698,"d":"698.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LVS04602","Connection, Linergy LGY, for vertical straight connection 1600A",0]
["LVS04528","VERTIK. ZBERNICA S OTVORMI 80X10",1,"ks",{"v":490.21875,"d":"490.219"},"3606481870469",{"v":180,"d":"180.00"},{"v":1.8,"d":"1.80"},{"v":14,"d":"14.00"},{"v":11217,"d":"11,217.00"},"IT","7407290000","https://www.se.com/sk/sk/product/LVS04528","Busbar, Linergy BS, drilled busbar, 1800A, vertical, flat bar, 80x10mm, L1675mm",0]
["LVS04512","PE-ZBERNICA S OTVORMI 25X5MM",1,"ks",{"v":90.365625,"d":"90.366"},"3606481870407",{"v":178,"d":"178.00"},{"v":1.5,"d":"1.50"},{"v":11.5,"d":"11.50"},{"v":1974,"d":"1,974.00"},"IT","7407290000","https://www.se.com/sk/sk/product/LVS04512","PE conductor flat bar, Linergy TB, 400A, for a vertical installation, with holes, 25x5, L1675",0]
["LVS04487","PRÍVODY 1600A NS1600 PEVNÝ 3P",1,"ks",{"v":708.75,"d":"708.750"},"3606481867834",{"v":54,"d":"54.00"},{"v":12.5,"d":"12.50"},{"v":11.5,"d":"11.50"},{"v":14818,"d":"14,818.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LVS04487","Connection, Linergy LGY, for NS, 3P, 1600A, vertical fixed",0]
["LVS04482","1600A PRÍVODY PRE INS1600, 4P",1,"ks",{"v":785.53125,"d":"785.531"},"3606481867780",{"v":58,"d":"58.00"},{"v":12,"d":"12.00"},{"v":12,"d":"12.00"},{"v":18267,"d":"18,267.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LVS04482","Connection, Linergy LGY, for INS-INV, 4P, 1600A, vertical fixed",0]
["LVS04454","PRÍVODY NS630 HORIZ. PEVNÝ/PÁK. OVL. 4P",1,"ks",{"v":159.46875,"d":"159.469"},"3606481867643",{"v":30,"d":"30.00"},{"v":4.5,"d":"4.50"},{"v":27.5,"d":"27.50"},{"v":3370,"d":"3,370.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LVS04454","Connection, Linergy LGY, for NSX630, 4P, 630A, horizontal plug-in with toggle",0]
["LVS04331","HORIZ. PREPÁŽKA PRE NÁSTEN.-STOJACU SKRI",1,"ks",{"v":39.571875,"d":"39.572"},"3606481880086",{"v":57.5,"d":"57.50"},{"v":2.5,"d":"2.50"},{"v":15.5,"d":"15.50"},{"v":815,"d":"815.00"},"CZ","7326909890","https://www.se.com/sk/sk/product/LVS04331","Partition, PrismaSeT G, horizontal, W600 IP30/IP55",0]
["LVS04233","KANÁL NA DVERE D2000",1,"ks",{"v":18.9,"d":"18.900"},"3606481866523",{"v":200,"d":"200.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":518,"d":"518.00"},"FR","8544429090","https://www.se.com/sk/sk/product/LVS04233","TRUNKING DOOR L2000",0]
["LVS04215","4 PE-SVORKOVNICE 3X16MM2",1,"ks",{"v":30.7125,"d":"30.713"},"3606481872500",{"v":10,"d":"10.00"},{"v":4.8,"d":"4.80"},{"v":8,"d":"8.00"},{"v":194,"d":"194.00"},"PL","8536901000","https://www.se.com/sk/sk/product/LVS04215","Block, Linergy TB, 4 earth block with spring terminals, 3 x 16mm² clamp",0]
["LVS04192","DRŽIAK VIACRAD. ZBERNICE PRE PREP. ODDIE",1,"ks",{"v":11.694375,"d":"11.694"},"3606481866981",{"v":23.5,"d":"23.50"},{"v":3,"d":"3.00"},{"v":11.3,"d":"11.30"},{"v":202,"d":"202.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS04192","Busbar support, PrismaSeT G, for Linergy BS multistage busbar, 25kA, 630A",0]
["LVS04156","PRÍDAVNÝ BLOK 35MM2 4P",1,"ks",{"v":20.08125,"d":"20.081"},"3606481866769",{"v":14.5,"d":"14.50"},{"v":6,"d":"6.00"},{"v":8.3,"d":"8.30"},{"v":294,"d":"294.00"},"FR","8536901000","https://www.se.com/sk/sk/product/LVS04156","Distribution block, LINERGY DP, Additional block, 4P, 250A, 2 connections: 2 x 35²/pole",0]
["LVS04126","ZBERN. LINERGY BW 160A 4P D1400",1,"ks",{"v":318.9375,"d":"318.938"},"3606481870209",{"v":153,"d":"153.00"},{"v":4.5,"d":"4.50"},{"v":13,"d":"13.00"},{"v":5563,"d":"5,563.00"},"FR","8544499500","https://www.se.com/sk/sk/product/LVS04126","Busbar, Linergy BW, 4P, 160A, insulated busbar, vertical, L1400mm",0]
["LVS04113","ZBERN. LINERGY BW 400A 3P D1000",1,"ks",{"v":336.65625,"d":"336.656"},"3606481870100",{"v":112.5,"d":"112.50"},{"v":4.5,"d":"4.50"},{"v":13,"d":"13.00"},{"v":5200,"d":"5,200.00"},"FR","8544499500","https://www.se.com/sk/sk/product/LVS04113","Busbar, Linergy BW, 3P, 400A, insulated busbar, vertical, L1000mm",0]
["LVS04055","VIACRADOVÁ SVORKOVNICA LINERGY BS630A 4",1,"ks",{"v":248.0625,"d":"248.063"},"3606481870940",{"v":55,"d":"55.00"},{"v":15.5,"d":"15.50"},{"v":25.5,"d":"25.50"},{"v":5596,"d":"5,596.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LVS04055","Multi-stage distribution block, LINERGY BS, 4P Multistage Busbar 630A 52holes",0]
["LVS04052","VIACRADOVÁ SVORKOVNICA LINERGY BS160A 4P",1,"ks",{"v":97.453125,"d":"97.453"},"3606481870919",{"v":55,"d":"55.00"},{"v":15.5,"d":"15.50"},{"v":25.5,"d":"25.50"},{"v":2658,"d":"2,658.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LVS04052","Multi-stage distribution block, LINERGY BS, 4P Multistage Busbar 160A 52holes",0]
["LVS04008","SVORKOVNICA LINERGY FM 4P 63A 1/2 R.",1,"ks",{"v":51.384375,"d":"51.384"},"3606481870803",{"v":23.2,"d":"23.20"},{"v":4.7,"d":"4.70"},{"v":6.2,"d":"6.20"},{"v":450,"d":"450.00"},"PL","8536901000","https://www.se.com/sk/sk/product/LVS04008","Distribution block, LINERGY FM, 4P, 63A, 12M, 20holes",0]
["LVS03932","ČEL. PANEL VIGILHOM XM200-300C",1,"ks",{"v":25.9875,"d":"25.988"},"3606481871572",{"v":51.5,"d":"51.50"},{"v":3,"d":"3.00"},{"v":31.5,"d":"31.50"},{"v":1061,"d":"1,061.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS03932","Front plate, PrismaSeT P, for Vigilohm IM400 with 3 XD301 or with 1 or 2 IFL12 with cut-out, 6M, W600/W650, white, RAL 9003",0]
["LVS03861","PLNÝ ČEL. PANEL 11M Š850",1,"ks",{"v":113.990625,"d":"113.991"},"3606481932945",{"v":76,"d":"76.00"},{"v":4.5,"d":"4.50"},{"v":55.5,"d":"55.50"},{"v":4600,"d":"4,600.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS03861","Front plate, PrismaSeT G, for enclosure W850, plain type, 11M, white, RAL 9003",0]
["LVS03807","PLNÝ ČEL. PANEL 9M",1,"ks",23.625,"3606481873866",{"v":51.4,"d":"51.40"},{"v":3,"d":"3.00"},{"v":46,"d":"46.00"},{"v":1857,"d":"1,857.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS03807","Front plate, PrismaSeT P and G, for enclosure W600/W650, plain type, 9M, white, RAL 9003",0]
["LVS03736","ČEL. PANEL IP55 ISFL 185MM BC 160A Š650",1,"ks",{"v":56.699999999999996,"d":"56.700"},"3606481872333",{"v":56,"d":"56.00"},{"v":3,"d":"3.00"},{"v":51,"d":"51.00"},{"v":1186,"d":"1,186.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS03736","Front plate, PrismaSeT P, for Fupact ISFL160 3P, 11M, Vertical, Through cut-out front plate, white, RAL 9003",0]
["LVS03692","ČEL. PANEL NT VERT. PEVNÝ",1,"ks",{"v":96.271875,"d":"96.272"},"3606481866356",{"v":50,"d":"50.00"},{"v":3,"d":"3.00"},{"v":35,"d":"35.00"},{"v":1440,"d":"1,440.00"},"RO","8538909999","https://www.se.com/sk/sk/product/LVS03692","Front plate, PrismaSeT P, vertical fixed for MTZ1/NT, with cut-out, horizontal fixed, 7M, W650mm",0]
["LVS03652","ČEL. PANEL NS630 HORIZ. PÁK. OVL. 4P",1,"ks",{"v":34.846875,"d":"34.847"},"3606481872487",{"v":51.5,"d":"51.50"},{"v":3,"d":"3.00"},{"v":26.5,"d":"26.50"},{"v":998,"d":"998.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS03652","Front plate, PrismaSeT P, for NS630, 4P, horizontal fixed, toggle type",0]
["LVS03604","PLAST. NSX250 HORIZ.",1,"ks",{"v":31.89375,"d":"31.894"},"3606481866035",{"v":51,"d":"51.00"},{"v":3,"d":"3.00"},{"v":15.5,"d":"15.50"},{"v":625,"d":"625.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS03604","Front plate, PrismaSeT P, for Vigi NSX toggle/CVS rotary, 3P, 250A, 3M, horizontal,fixed, W650",0]
["LVS03572","PERF. MONT. DOSKA 6M",1,"ks",{"v":60.834375,"d":"60.834"},"3606481874917",{"v":58,"d":"58.00"},{"v":3,"d":"3.00"},{"v":30,"d":"30.00"},{"v":2025,"d":"2,025.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS03572","Mounting plate, PrismaSeT P, slotted type, for Universal enclosure, 6M, W400mm/650mm",0]
["LVS03501","MONT. DOSKA NS3200-INS2500",1,"ks",{"v":108.084375,"d":"108.084"},"3606481874641",{"v":58,"d":"58.00"},{"v":3.4,"d":"3.40"},{"v":20,"d":"20.00"},{"v":2944,"d":"2,944.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS03501","MOUNTING PLATE NS3200 INS-INV2500 FIXED VERTICAL IN WIDTH 650",0]
["LVS03420","MONT. DOSKA 3-4NS-INS250 VERT. PEVNÝ/PÁK",1,"ks",42.525,"3606481874313",{"v":58.8,"d":"58.80"},{"v":6.4,"d":"6.40"},{"v":15.1,"d":"15.10"},{"v":1530,"d":"1,530.00"},"IT","7326909890","https://www.se.com/sk/sk/product/LVS03420","Mounting plate, PrismaSeT, 3-4 vertically fixed, NS-INS250 Toggle.",0]
["LVS03409","Montážny panel pre NSXm do 160",1,"ks",{"v":129.9375,"d":"129.938"},"3606481871565",{"v":57.4,"d":"57.40"},{"v":4.8,"d":"4.80"},{"v":14.7,"d":"14.70"},{"v":2069,"d":"2,069.00"},"IT","7326909890","https://www.se.com/sk/sk/product/LVS03409","Mounting plate, PrismaSeT P, for NSXm 3P/4P, horizontal fixed, toggle/direct rotary handle, 3M, W650mm",0]
["LVS03328","ČEL. PANEL HORIZ. ISFT 250 A",1,"ks",{"v":34.25625,"d":"34.256"},"3606481871862",{"v":51.5,"d":"51.50"},{"v":3,"d":"3.00"},{"v":26.5,"d":"26.50"},{"v":778,"d":"778.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS03328","Front plate, PrismaSeT G, for FupacT ISFT 250, 5M, horizontal, fixed, with cut-out, W600",0]
["LVS03299","ČEL. PANEL, VERT., NSX630 VIGI",1,"ks",{"v":49.021875,"d":"49.022"},"3606481873477",{"v":51.5,"d":"51.50"},{"v":3,"d":"3.00"},{"v":26.5,"d":"26.50"},{"v":996,"d":"996.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS03299","Front plate, PrismaSeT P and G, for Vigi NSX400/630, 10M, vertical, fixed, toggle, cut-out, W300, white, RAL 9003",0]
["LVS03275","ČEL. PANEL NS630 VERT. ROT/MOT. MECH.",1,"ks",{"v":46.06875,"d":"46.069"},"3606481873248",{"v":51.5,"d":"51.50"},{"v":3,"d":"3.00"},{"v":46.5,"d":"46.50"},{"v":1733,"d":"1,733.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LVS03275","FR.PL.NSX/CVS630 V.TOG/ROT/PLUG W600 9M",0]
["LVS03249","ZASLEPOVACÍ KRYT VERT. NS-INS250-EZC100",1,"ks",{"v":2.3625,"d":"2.363"},"3606481868381",{"v":14.7,"d":"14.70"},{"v":2.1,"d":"2.10"},{"v":9.3,"d":"9.30"},{"v":48,"d":"48.00"},"FR","3926909790","https://www.se.com/sk/sk/product/LVS03249","Divisible blanking plate, for NSX/CVS250-EZC100, vertical, W147mm",0]
["LVS03220","ZASLEPOVACÍ PÁSIK D1000",1,"ks",{"v":2.953125,"d":"2.953"},"3606481868350",{"v":100,"d":"100.00"},{"v":0.5,"d":"0.50"},{"v":5.8,"d":"5.80"},{"v":139,"d":"139.00"},"FR","3926909790","https://www.se.com/sk/sk/product/LVS03220","Blanking plate, PrismaSeT P & G, for front plate, L1000mm",0]
["LVS03195","4 ŠESŤHR. DIŠT. SEGMETY H9 M6",1,"ks",{"v":8.032499999999999,"d":"8.033"},"3606481871077",{"v":4.5,"d":"4.50"},{"v":1.7,"d":"1.70"},{"v":4.5,"d":"4.50"},{"v":61,"d":"61.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS03195","Hexagonal spacers, PrismaSeT G and P, M6, H9 mm, Set of 4",0]
["LVS03173","PERF. MONT. DOSKA ZAPUST. 9M",1,"ks",{"v":74.41875,"d":"74.419"},"3606481875259",{"v":47,"d":"47.00"},{"v":2.8,"d":"2.80"},{"v":45,"d":"45.00"},{"v":1434,"d":"1,434.00"},"CZ","7326909890","https://www.se.com/sk/sk/product/LVS03173","Mounting plate, PrismaSeT G, recessed slotted type, for enclosure, 9M, W600mm",0]
["LVS03144","MONT.PANEL TARIF NSX250, Š300",1,"ks",{"v":41.34375,"d":"41.344"},"3606481875129",{"v":22,"d":"22.00"},{"v":4.3,"d":"4.30"},{"v":20,"d":"20.00"},{"v":737,"d":"737.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS03144","Mounting plate, PrismaSeT G, for tarif NSX250 4P, vertical fixed, toggle, 9M, W300mm",0]
["LVS03073","MONT. DOSKA NS-INS630 VERT. PEVNÝ/PÁK. O",1,"ks",{"v":67.921875,"d":"67.922"},"3606481874702",{"v":47.5,"d":"47.50"},{"v":8.5,"d":"8.50"},{"v":26.5,"d":"26.50"},{"v":2570,"d":"2,570.00"},"IT","7326909890","https://www.se.com/sk/sk/product/LVS03073","Mounting plate, PrismaSeT G, for NSX/CVS/Vigi/INS 630A, vertical fixed, toggle, W600mm",0]
["LVS03010","PEVNÁ DIN lišta 10M, Š 300",1,"ks",{"v":5.0203125,"d":"5.020"},"3606481875488",{"v":21.8,"d":"21.80"},{"v":5.2,"d":"5.20"},{"v":10.5,"d":"10.50"},{"v":169,"d":"169.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS03010","Rail, PrismaSeT G, for modular device, W300mm",0]
["LVS01224","PLNE DVERE Š650 SPEVNENE",1,"ks",{"v":389.8125,"d":"389.813"},"3606481878700",{"v":198.5,"d":"198.50"},{"v":7,"d":"7.00"},{"v":70,"d":"70.00"},{"v":25220,"d":"25,220.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS01224","Door, PrismaSeT P, reinforced plain door, W650, IP30, IK10, white, RAL 9003",0]
["LVS01105","PRÍSLUŠENSTVO ZATVÁRANIE DVERÍ",1,"ks",{"v":12.99375,"d":"12.994"},"3606481885067",{"v":11,"d":"11.00"},{"v":4,"d":"4.00"},{"v":6.5,"d":"6.50"},{"v":284,"d":"284.00"},"FR","8302420090","https://www.se.com/sk/sk/product/LVS01105","Door locking kit, PrismaSeT P, locking kit for IP31/IP55 door",0]
["LVS01041","IP30 BOČNÝ PANEL 9M SYST. G",1,"ks",{"v":40.753125,"d":"40.753"},"3606481884398",{"v":68,"d":"68.00"},{"v":5,"d":"5.00"},{"v":20.5,"d":"20.50"},{"v":1108,"d":"1,108.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS01041","Side panel, PrismaSeT G, 9M, for enclosure H480mm, IP30, white, RAL 9003",0]
["LVS01035","BOČNÉ PANELY SYSTEM G 27M PÁR",1,"ks",165.375,"3606481877956",{"v":187.8,"d":"187.80"},{"v":5,"d":"5.00"},{"v":20.5,"d":"20.50"},{"v":3236,"d":"3,236.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LVS01035","Side panel, PrismaSeT G, 27M, for enclosure H1580mm, IP30, white, RAL 9003",0]
["LV865307","Riadiaca jednotka Micrologic 7.0X – výsu",1,"ks",2338.875,"3606480823107",{"v":21.5,"d":"21.50"},{"v":6.8,"d":"6.80"},{"v":8,"d":"8.00"},{"v":318,"d":"318.00"},"","","https://www.se.com/sk/sk/product/LV865307","riadiaca jednotka Micrologic 7.0X – výsuvný MTZ1",0.04]
["LV864922SP","Doplnkový blok 4 pom. kontaktov OF – MTZ",1,"ks",239.085,"3606481187987",{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":135,"d":"135.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV864922SP","doplnkový blok 4 pom. kontaktov OF – MTZ2/3",0]
["LV851100SP","Ethernetové rozhranie EIFE - súprava pre",1,"ks",{"v":878.3775,"d":"878.378"},"3606481100436",{"v":8.2,"d":"8.20"},{"v":3.5,"d":"3.50"},{"v":6,"d":"6.00"},{"v":312,"d":"312.00"},"FR","8517620000","https://www.se.com/sk/sk/product/LV851100SP","Ethernetové rozhranie EIFE - súprava pre výsuvný MTZ1",0.04]
["LV850053SP","Priehľadný kryt pre Micrologic X",1,"ks",{"v":28.0665,"d":"28.067"},"3606481158338",{"v":26,"d":"26.00"},{"v":0.5,"d":"0.50"},{"v":18,"d":"18.00"},{"v":40,"d":"40.00"},"FR","3926909790","https://www.se.com/sk/sk/product/LV850053SP","priehľadný kryt pre Micrologic X",0]
["LV850007","Digitálny Modul – ANSI51N/G alarm zemnej",1,"ks",{"v":420.9975,"d":"420.998"},"3606489503000",{"v":0.3,"d":"0.30"},{"v":0.3,"d":"0.30"},{"v":0.2,"d":"0.20"},0.01,"FR","8538909999","https://www.se.com/sk/sk/product/LV850007","digitálny Modul - ANSI51N/G alarm zemnej ochrany pre Micrologic X",0]
["LV848755","Odpínač MTZ2 08HA10 4P výsuvný",1,"ks",{"v":5405.4,"d":"5405.400"},"3606480813979",{"v":0.2,"d":"0.20"},{"v":0.1,"d":"0.10"},{"v":0.1,"d":"0.10"},{"v":1,"d":"1.00"},"","","https://www.se.com/sk/sk/product/LV848755","odpínač MTZ2 08HA10 4P výsuvný",0]
["LV848736","Istič MTZ2 10 H10 4P výsuvný",1,"ks",{"v":6340.95,"d":"6340.950"},"3606480807770",{"v":0.2,"d":"0.20"},{"v":0.1,"d":"0.10"},{"v":0.1,"d":"0.10"},{"v":1,"d":"1.00"},"","","https://www.se.com/sk/sk/product/LV848736","istič MTZ2 10 H10 4P výsuvný",0]
["LV848727","Istič MTZ2 12 H10 3P výsuvný",1,"ks",5145.525,"3606480809347",{"v":0.2,"d":"0.20"},{"v":0.1,"d":"0.10"},{"v":0.1,"d":"0.10"},{"v":1,"d":"1.00"},"","","https://www.se.com/sk/sk/product/LV848727","istič MTZ2 12 H10 3P výsuvný",0]
["LV848599SP","3 medzifázové prepážky – pevný MTZ",1,"ks",{"v":296.25750000000005,"d":"296.258"},"3606481173270",{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":1258,"d":"1,258.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV848599SP","3 medzifázové prepážky – pevný MTZ",0]
["LV848596","Kryt svoriek (CB) pre MTZ2 4P",1,"ks",{"v":85.75875,"d":"85.759"},"3606480805851",{"v":11,"d":"11.00"},{"v":14,"d":"14.00"},{"v":55,"d":"55.00"},{"v":1200,"d":"1,200.00"},"","","https://www.se.com/sk/sk/product/LV848596","kryt svoriek (CB) pre MTZ2 4P",0]
["LV848569","Uzamykanie šasi pozícia Vysunuté, 2 zámk",1,"ks",{"v":192.3075,"d":"192.308"},"3606480809552",{"v":10.5,"d":"10.50"},{"v":1.7,"d":"1.70"},{"v":3.5,"d":"3.50"},{"v":205,"d":"205.00"},"","","https://www.se.com/sk/sk/product/LV848569","uzamykanie šasi pozícia Vysunuté, 2 zámky Profalux, 1 kľúč – MTZ2/3",0]
["LV848557SP","Uzemňovací diel na istič – pevný MTZ2/3",1,"ks",{"v":244.28249999999997,"d":"244.283"},"3606481187680",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":15,"d":"15.00"},{"v":100,"d":"100.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV848557SP","uzemňovací diel na istič – pevný MTZ2/3",0]
["LV848535SP","Mechanické počítadlo operácií CDM – MTZ2",1,"ks",{"v":291.06,"d":"291.060"},"3606481187642",{"v":9,"d":"9.00"},{"v":4,"d":"4.00"},{"v":9,"d":"9.00"},{"v":74,"d":"74.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV848535SP","mechanické počítadlo operácií CDM – MTZ2/3",0]
["LV848526","Motorový pohon MCH 100/130VAC – výsuvný",1,"ks",{"v":1143.45,"d":"1143.450"},"3606480804595",{"v":22.9,"d":"22.90"},{"v":12.6,"d":"12.60"},{"v":12.9,"d":"12.90"},{"v":1720,"d":"1,720.00"},"","","https://www.se.com/sk/sk/product/LV848526","motorový pohon MCH 100/130VAC – výsuvný MTZ2/3",0.21]
["LV848498","Riadiaca jednotka Micrologic 2.0X - výsu",1,"ks",{"v":1351.35,"d":"1351.350"},"3606480811319",{"v":21.5,"d":"21.50"},{"v":6.8,"d":"6.80"},{"v":8,"d":"8.00"},{"v":319,"d":"319.00"},"","","https://www.se.com/sk/sk/product/LV848498","riadiaca jednotka Micrologic 2.0X - výsuvný MTZ2/3",0.04]
["LV848492","Vypínacia spúšť MX 48/60VDC 48VAC – výsu",1,"ks",{"v":223.4925,"d":"223.493"},"3606480807497",{"v":8.3,"d":"8.30"},{"v":3.5,"d":"3.50"},{"v":6,"d":"6.00"},{"v":1164,"d":"1,164.00"},"","","https://www.se.com/sk/sk/product/LV848492","vypínacia spúšť MX 48/60VDC 48VAC – výsuvný MTZ2/3",0.14]
["LV848469","Kontakt „Pripravený na zapnutie“ – výsuv",1,"ks",{"v":119.5425,"d":"119.543"},"3606480804496",{"v":15,"d":"15.00"},{"v":1,"d":"1.00"},{"v":4.7,"d":"4.70"},{"v":42,"d":"42.00"},"","","https://www.se.com/sk/sk/product/LV848469","kontakt „Pripravený na zapnutie“ – výsuvný MTZ2/3",0.01]
["LV848439","Istič MTZ2 32 H2 4P výsuvný N vpravo",1,"ks",{"v":15917.8635,"d":"15917.864"},"3606480809248",{"v":50,"d":"50.00"},{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":9254,"d":"9,254.00"},"","","https://www.se.com/sk/sk/product/LV848439","istič MTZ2 32 H2 4P výsuvný N vpravo",1.11]
["LV848429","Istič MTZ2 16 H2 4P výsuvný N vpravo",1,"ks",{"v":7848.224999999999,"d":"7848.225"},"3606480807244",{"v":50,"d":"50.00"},{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":54653,"d":"54,653.00"},"","","https://www.se.com/sk/sk/product/LV848429","istič MTZ2 16 H2 4P výsuvný N vpravo",6.5600000000000005]
["LV848413","Horné predné prívody – šasi MTZ2 20 3P",1,"ks",{"v":311.84999999999997,"d":"311.850"},"3606480804922",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":18,"d":"18.00"},{"v":6924,"d":"6,924.00"},"","","https://www.se.com/sk/sk/product/LV848413","horné predné prívody – šasi MTZ2 20 3P",0.8300000000000001]
["LV848356","Istič MTZ3 50 H2 4P výsuvný N vpravo",1,"ks",{"v":37381.459500000004,"d":"37381.460"},"3606480807138",{"v":50,"d":"50.00"},{"v":60,"d":"60.00"},{"v":120,"d":"120.00"},{"v":133323,"d":"133,323.00"},"","","https://www.se.com/sk/sk/product/LV848356","istič MTZ3 50 H2 4P výsuvný N vpravo",16]
["LV848353","Odpínač MTZ3 63HA 4P výsuvný",1,"ks",{"v":39317.008499999996,"d":"39317.009"},"3606480816000",{"v":15,"d":"15.00"},{"v":133,"d":"133.00"},{"v":7,"d":"7.00"},{"v":61338,"d":"61,338.00"},"","","https://www.se.com/sk/sk/product/LV848353","odpínač MTZ3 63HA 4P výsuvný",7.36]
["LV848334","Istič MTZ3 50 H1 4P výsuvný N vpravo",1,"ks",{"v":33154.8525,"d":"33154.853"},"3606480807091",{"v":50,"d":"50.00"},{"v":60,"d":"60.00"},{"v":120,"d":"120.00"},{"v":62325,"d":"62,325.00"},"","","https://www.se.com/sk/sk/product/LV848334","istič MTZ3 50 H1 4P výsuvný N vpravo",7.48]
["LV848329","Istič MTZ2 40 H3 4P výsuvný",1,"ks",{"v":23849.2485,"d":"23849.249"},"3606480807060",{"v":49.5,"d":"49.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":54130,"d":"54,130.00"},"","","https://www.se.com/sk/sk/product/LV848329","istič MTZ2 40 H3 4P výsuvný",6.5]
["LV848302","Istič MTZ2 25 H3 3P výsuvný",1,"ks",{"v":10595.6235,"d":"10595.624"},"3606480808937",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":48418,"d":"48,418.00"},"","","https://www.se.com/sk/sk/product/LV848302","istič MTZ2 25 H3 3P výsuvný",5.8100000000000005]
["LV848287","Istič MTZ2 20 H1 3P výsuvný",1,"ks",{"v":6340.95,"d":"6340.950"},"3606480808869",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":48422,"d":"48,422.00"},"","","https://www.se.com/sk/sk/product/LV848287","istič MTZ2 20 H1 3P výsuvný",5.8100000000000005]
["LV848276","Odpínač MTZ2 16NA 3P výsuvný",1,"ks",5561.325,"3606480815850",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47048,"d":"47,048.00"},"","","https://www.se.com/sk/sk/product/LV848276","odpínač MTZ2 16NA 3P výsuvný",5.65]
["LV848265","Istič MTZ2 12 N1 4P výsuvný",1,"ks",4417.875,"3606480808760",{"v":49.5,"d":"49.50"},{"v":29.5,"d":"29.50"},{"v":30.5,"d":"30.50"},{"v":53342,"d":"53,342.00"},"","","https://www.se.com/sk/sk/product/LV848265","istič MTZ2 12 N1 4P výsuvný",6.4]
["LV848251","Istič MTZ2 10 N1 4P výsuvný",1,"ks",3898.125,"3606480808722",{"v":49.5,"d":"49.50"},{"v":29.5,"d":"29.50"},{"v":30.5,"d":"30.50"},{"v":53342,"d":"53,342.00"},"","","https://www.se.com/sk/sk/product/LV848251","istič MTZ2 10 N1 4P výsuvný",6.4]
["LV848238","Istič MTZ2 08 H1 4P výsuvný",1,"ks",{"v":4158,"d":"4158.000"},"3606480808678",{"v":49.5,"d":"49.50"},{"v":29.5,"d":"29.50"},{"v":30.5,"d":"30.50"},{"v":47654,"d":"47,654.00"},"","","https://www.se.com/sk/sk/product/LV848238","istič MTZ2 08 H1 4P výsuvný",5.72]
["LV848226","Istič MTZ2 08 H1 4P výsuvný N vpravo",1,"ks",4521.825,"3606480806902",{"v":50,"d":"50.00"},{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":54654,"d":"54,654.00"},"","","https://www.se.com/sk/sk/product/LV848226","istič MTZ2 08 H1 4P výsuvný N vpravo",6.5600000000000005]
["LV848193","Istič MTZ2 40 H1 4P pevný N vpravo",1,"ks",21336.777,"3606480806865",{"v":50,"d":"50.00"},{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":36251,"d":"36,251.00"},"","","https://www.se.com/sk/sk/product/LV848193","istič MTZ2 40 H1 4P pevný N vpravo",4.3500000000000005]
["LV848174","Spodné vodorovné zadné prívody – MTZ2 25",1,"ks",{"v":441.78749999999997,"d":"441.788"},"3606480804311",{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},{"v":8,"d":"8.00"},{"v":4156,"d":"4,156.00"},"","","https://www.se.com/sk/sk/product/LV848174","spodné vodorovné zadné prívody – MTZ2 25/32 4P",0.5]
["LV848165","Spodné zvislé zadné prívody – MTZ2 40 4P",1,"ks",841.995,"3606480804236",{"v":5,"d":"5.00"},{"v":12.5,"d":"12.50"},{"v":6,"d":"6.00"},{"v":6240,"d":"6,240.00"},"","","https://www.se.com/sk/sk/product/LV848165","spodné zvislé zadné prívody – MTZ2 40 4P",0.75]
["LV848148","Spodné vodorovné zadné prívody – MTZ2 08",1,"ks",176.715,"3606480804120",{"v":7.5,"d":"7.50"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":1690,"d":"1,690.00"},"","","https://www.se.com/sk/sk/product/LV848148","spodné vodorovné zadné prívody – MTZ2 08/20 3P",0.2]
["LV848136","Horné zvislé zadné prívody – MTZ3 40/50",1,"ks",{"v":665.2800000000001,"d":"665.280"},"3606480804014",{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},{"v":8,"d":"8.00"},{"v":5734,"d":"5,734.00"},"","","https://www.se.com/sk/sk/product/LV848136","horné zvislé zadné prívody – MTZ3 40/50 3P",0.6900000000000001]
["LV848123","Odpínač MTZ3 63 HA 4P pevný",1,"ks",{"v":39403.287000000004,"d":"39403.287"},"3606480813474",{"v":25,"d":"25.00"},{"v":28,"d":"28.00"},{"v":22,"d":"22.00"},{"v":62150,"d":"62,150.00"},"","","https://www.se.com/sk/sk/product/LV848123","odpínač MTZ3 63 HA 4P pevný",7.46]
["LV848113","Istič MTZ3 50 H2 3P pevný",1,"ks",{"v":28689.160499999998,"d":"28689.161"},"3606480824005",{"v":120,"d":"120.00"},{"v":75,"d":"75.00"},{"v":75,"d":"75.00"},{"v":133409,"d":"133,409.00"},"","","https://www.se.com/sk/sk/product/LV848113","istič MTZ3 50 H2 3P pevný",16.01]
["LV848098","Istič MTZ2 40 H2 4P pevný",1,"ks",{"v":22076.900999999998,"d":"22076.901"},"3606480806735",{"v":49.5,"d":"49.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47251,"d":"47,251.00"},"","","https://www.se.com/sk/sk/product/LV848098","istič MTZ2 40 H2 4P pevný",5.67]
["LV848085","Odpínač MTZ2 32 HA 3P pevný",1,"ks",{"v":10187.1,"d":"10187.100"},"3606480815720",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47270,"d":"47,270.00"},"","","https://www.se.com/sk/sk/product/LV848085","odpínač MTZ2 32 HA 3P pevný",5.67]
["LV848053","Odpínač MTZ2 16 NA 4P pevný",1,"ks",{"v":4989.599999999999,"d":"4989.600"},"3606480815669",{"v":49.5,"d":"49.50"},{"v":29.5,"d":"29.50"},{"v":30.5,"d":"30.50"},{"v":47270,"d":"47,270.00"},"","","https://www.se.com/sk/sk/product/LV848053","odpínač MTZ2 16 NA 4P pevný",5.67]
["LV848035","Istič MTZ2 12 N1 4P pevný",1,"ks",{"v":4209.974999999999,"d":"4209.975"},"3606480808272",{"v":49.5,"d":"49.50"},{"v":29.5,"d":"29.50"},{"v":30.5,"d":"30.50"},{"v":47252,"d":"47,252.00"},"","","https://www.se.com/sk/sk/product/LV848035","istič MTZ2 12 N1 4P pevný",5.67]
["LV848021","Istič MTZ2 10 N1 4P pevný",1,"ks",3690.225,"3606480808227",{"v":49.5,"d":"49.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47252,"d":"47,252.00"},"","","https://www.se.com/sk/sk/product/LV848021","istič MTZ2 10 N1 4P pevný",5.67]
["LV848004","Odpínač MTZ2 08 NA 3P pevný",1,"ks",3066.525,"3606480813351",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47270,"d":"47,270.00"},"","","https://www.se.com/sk/sk/product/LV848004","odpínač MTZ2 08 NA 3P pevný",5.67]
["LV847968SP","Zvislé zadné prívody horné alebo spodné",1,"ks",{"v":836.7975000000001,"d":"836.798"},"3606481187413",{"v":18.5,"d":"18.50"},{"v":12,"d":"12.00"},{"v":13,"d":"13.00"},{"v":3570,"d":"3,570.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV847968SP","zvislé zadné prívody horné alebo spodné – pevný/výsuvný MTZ2 40 3P (3 ks)",0]
["LV847936SP","Zhášacia komora – MTZ3 (1 ks)",1,"ks",{"v":441.78749999999997,"d":"441.788"},"3606481187284",{"v":18,"d":"18.00"},{"v":12,"d":"12.00"},{"v":12,"d":"12.00"},{"v":2517,"d":"2,517.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV847936SP","zhášacia komora – MTZ3 (1 ks)",0.3]
["LV847914SP","Uzamykanie dverí, pravá strana šasi VPEC",1,"ks",{"v":38.981249999999996,"d":"38.981"},"3606481187215",{"v":9.8,"d":"9.80"},{"v":3.5,"d":"3.50"},{"v":8.8,"d":"8.80"},{"v":191,"d":"191.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV847914SP","uzamykanie dverí, pravá strana šasi VPECD – výsuvný MTZ2/3",0]
["LV847896SP","Motorový pohon MCH 380/415 VAC – MTZ2/3",1,"ks",{"v":1455.3,"d":"1455.300"},"3606481187154",{"v":22.8,"d":"22.80"},{"v":12.5,"d":"12.50"},{"v":13.2,"d":"13.20"},{"v":1979,"d":"1,979.00"},"FR","8501200090","https://www.se.com/sk/sk/product/LV847896SP","motorový pohon MCH 380/415 VAC – MTZ2/3",0.24]
["LV847824","Kalibračný modul 4000A MTZ3 N°23",1,"ks",{"v":0.10395,"d":"0.104"},"3606480811012",{"v":3.5,"d":"3.50"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"","","https://www.se.com/sk/sk/product/LV847824","kalibračný modul 4000A MTZ3 N°23",0]
["LV847522","Uzamykanie v stave VYP., 2 zámky Ronis,",1,"ks",{"v":207.9,"d":"207.900"},"3606480813344",{"v":15,"d":"15.00"},{"v":4,"d":"4.00"},{"v":10,"d":"10.00"},{"v":302,"d":"302.00"},"","","https://www.se.com/sk/sk/product/LV847522","uzamykanie v stave VYP., 2 zámky Ronis, 1 kľúč – MTZ1",0]
["LV847462","Motorový pohon MCH 100/130V DC – výsuvný",1,"ks",{"v":1143.45,"d":"1143.450"},"3606480811937",{"v":12.5,"d":"12.50"},{"v":6,"d":"6.00"},{"v":18,"d":"18.00"},{"v":787,"d":"787.00"},"","","https://www.se.com/sk/sk/product/LV847462","motorový pohon MCH 100/130V DC – výsuvný MTZ1",0.09]
["LV847432","Kontakt PF „Pripravený na zapnutie“ – vý",1,"ks",{"v":119.5425,"d":"119.543"},"3606480811906",{"v":6.5,"d":"6.50"},{"v":1.3,"d":"1.30"},{"v":4.7,"d":"4.70"},{"v":42,"d":"42.00"},"","","https://www.se.com/sk/sk/product/LV847432","kontakt PF „Pripravený na zapnutie“ – výsuvný MTZ1",0.01]
["LV847413","Zapínacia spúšť XF COM 48/60VDC 48VAC –",1,"ks",{"v":254.6775,"d":"254.678"},"3606480815478",{"v":7.7,"d":"7.70"},{"v":0.8,"d":"0.80"},{"v":4.9,"d":"4.90"},{"v":1165,"d":"1,165.00"},"","","https://www.se.com/sk/sk/product/LV847413","zapínacia spúšť XF COM 48/60VDC 48VAC – výsuvný MTZ1",0.14]
["LV847391","Motorový pohon MCH 48/60V DC AC – pevný",1,"ks",{"v":1143.45,"d":"1143.450"},"3606480813153",{"v":18,"d":"18.00"},{"v":7,"d":"7.00"},{"v":13,"d":"13.00"},{"v":1018,"d":"1,018.00"},"","","https://www.se.com/sk/sk/product/LV847391","motorový pohon MCH 48/60V DC AC – pevný MTZ1",0.12]
["LV847365","Vypínacia spúšť MX 380/480V AC – pevný M",1,"ks",{"v":223.4925,"d":"223.493"},"3606480808111",{"v":8.3,"d":"8.30"},{"v":3.5,"d":"3.50"},{"v":6.1,"d":"6.10"},{"v":1158,"d":"1,158.00"},"","","https://www.se.com/sk/sk/product/LV847365","vypínacia spúšť MX 380/480V AC – pevný MTZ",0.14]
["LV847351","Zapínacia spúšť XF 48/60VDC 48VAC – pevn",1,"ks",{"v":223.4925,"d":"223.493"},"3606480806407",{"v":8.3,"d":"8.30"},{"v":3.5,"d":"3.50"},{"v":6,"d":"6.00"},{"v":1158,"d":"1,158.00"},"","","https://www.se.com/sk/sk/product/LV847351","zapínacia spúšť XF 48/60VDC 48VAC – pevný MTZ",0.14]
["LV847329","Spodné predné prívody – pevný MTZ1 06/16",1,"ks",218.295,"3606480812132",{"v":20,"d":"20.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":2632,"d":"2,632.00"},"","","https://www.se.com/sk/sk/product/LV847329","spodné predné prívody – pevný MTZ1 06/16 3P",0.32]
["LV847255","Odpínač MTZ1 12HA 4P výsuvný",1,"ks",{"v":4261.95,"d":"4261.950"},"3606480815423",{"v":30,"d":"30.00"},{"v":41,"d":"41.00"},{"v":39,"d":"39.00"},{"v":4668,"d":"4,668.00"},"","","https://www.se.com/sk/sk/product/LV847255","odpínač MTZ1 12HA 4P výsuvný",0.56]
["LV847252","Odpínač MTZ1 10HA 3P výsuvný",1,"ks",{"v":3534.2999999999997,"d":"3534.300"},"3606480815393",{"v":39,"d":"39.00"},{"v":36,"d":"36.00"},{"v":23,"d":"23.00"},{"v":14079,"d":"14,079.00"},"","","https://www.se.com/sk/sk/product/LV847252","odpínač MTZ1 10HA 3P výsuvný",1.69]
["LV847217","Istič MTZ1 08 L1 4P výsuvný",1,"ks",{"v":4677.75,"d":"4677.750"},"3606480815256",{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":5118,"d":"5,118.00"},"","","https://www.se.com/sk/sk/product/LV847217","istič MTZ1 08 L1 4P výsuvný",0.61]
["LV847164","Odpínač MTZ1 10 HA 4P pevný",1,"ks",{"v":3274.4249999999997,"d":"3274.425"},"3606480815140",{"v":30,"d":"30.00"},{"v":41,"d":"41.00"},{"v":39,"d":"39.00"},{"v":19242,"d":"19,242.00"},"","","https://www.se.com/sk/sk/product/LV847164","odpínač MTZ1 10 HA 4P pevný",2.31]
["LV847160","Odpínač MTZ1 06 HA 4P pevný",1,"ks",{"v":2598.75,"d":"2598.750"},"3606480813078",{"v":30,"d":"30.00"},{"v":41,"d":"41.00"},{"v":39,"d":"39.00"},{"v":19242,"d":"19,242.00"},"","","https://www.se.com/sk/sk/product/LV847160","odpínač MTZ1 06 HA 4P pevný",2.31]
["LV847125","Istič MTZ1 08 H1 4P pevný",1,"ks",{"v":2806.65,"d":"2806.650"},"3606480815027",{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":15690,"d":"15,690.00"},"","","https://www.se.com/sk/sk/product/LV847125","istič MTZ1 08 H1 4P pevný",1.8800000000000001]
["LV847117","Istič MTZ1 06 L1 4P pevný",1,"ks",{"v":4209.974999999999,"d":"4209.975"},"3606480813054",{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":21492,"d":"21,492.00"},"","","https://www.se.com/sk/sk/product/LV847117","istič MTZ1 06 L1 4P pevný",2.58]
["LV847074SP","3-vodičová svorka – pevný MTZ",1,"ks",{"v":19.23075,"d":"19.231"},"3606481186812",{"v":21,"d":"21.00"},{"v":1,"d":"1.00"},{"v":14,"d":"14.00"},{"v":56,"d":"56.00"},"CN","8536699099","https://www.se.com/sk/sk/product/LV847074SP","3-vodičová svorka – pevný MTZ",0.01]
["LV846446","Istič MTZ1 12 H3 4P pevný",1,"ks",4521.825,"3606481155375",{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":12000,"d":"12,000.00"},"","","https://www.se.com/sk/sk/product/LV846446","istič MTZ1 12 H3 4P pevný",1.44]
["LV846436","Istič MTZ1 06 H3 3P pevný",1,"ks",2546.775,"3606481155290",{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":12000,"d":"12,000.00"},"","","https://www.se.com/sk/sk/product/LV846436","istič MTZ1 06 H3 3P pevný",1.44]
["LV836703","Podpäťová spúšť MN DIAG 200/250VDC AC –",1,"ks",{"v":254.6775,"d":"254.678"},"3606481176776",{"v":8.2,"d":"8.20"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":162,"d":"162.00"},"","","https://www.se.com/sk/sk/product/LV836703","podpäťová spúšť MN DIAG 200/250VDC AC – pevný MTZ",0.02]
["LV836669SP","Podpäťová spúšť MN DIAG 48/60VDC 48VAC",1,"ks",{"v":332.64000000000004,"d":"332.640"},"3606481186737",{"v":8.2,"d":"8.20"},{"v":6,"d":"6.00"},{"v":3.2,"d":"3.20"},{"v":223,"d":"223.00"},"FR","","https://www.se.com/sk/sk/product/LV836669SP","podpäťová spúšť MN DIAG 48/60VDC 48VAC",0.03]
["LV833920SP","Blokovanie dverí – MTZ1 pevný",1,"ks",{"v":1143.45,"d":"1143.450"},"3606481186706",{"v":35,"d":"35.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":3200,"d":"3,200.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV833920SP","blokovanie dverí – MTZ1 pevný",0]
["LV833821","Podpäťová spúšť MN 100/130VDC AC – výsuv",1,"ks",{"v":223.4925,"d":"223.493"},"3606480814952",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":169,"d":"169.00"},"","","https://www.se.com/sk/sk/product/LV833821","podpäťová spúšť MN 100/130VDC AC – výsuvný MTZ1",0.02]
["LV833779","Voliteľné uzamykanie polôh",1,"ks",{"v":38.981249999999996,"d":"38.981"},"3606481198631",{"v":0.1,"d":"0.10"},{"v":0.3,"d":"0.30"},{"v":0.2,"d":"0.20"},{"v":1,"d":"1.00"},"","","https://www.se.com/sk/sk/product/LV833779","voliteľné uzamykanie polôh",0]
["LV833772SP","Uzamykanie šasi – adaptačná súprava Kirk",1,"ks",322.245,"3606481186638",{"v":35,"d":"35.00"},{"v":2.5,"d":"2.50"},{"v":29,"d":"29.00"},{"v":161,"d":"161.00"},"IT","","https://www.se.com/sk/sk/product/LV833772SP","uzamykanie šasi – adaptačná súprava Kirk bez zámkov – MTZ1",0]
["LV833752","Kontakt pozícia test MTZ",1,"ks",{"v":44.17875,"d":"44.179"},"3606480803680",{"v":4.2,"d":"4.20"},{"v":0.9,"d":"0.90"},{"v":4.2,"d":"4.20"},{"v":1018,"d":"1,018.00"},"","","https://www.se.com/sk/sk/product/LV833752","kontakt pozícia test MTZ",0]
["LV833723","Šasi MTZ1 16 H1/H2 1600 A 3P",1,"ks",{"v":1351.35,"d":"1351.350"},"3606480812934",{"v":38,"d":"38.00"},{"v":54,"d":"54.00"},{"v":38,"d":"38.00"},{"v":19907,"d":"19,907.00"},"","","https://www.se.com/sk/sk/product/LV833723","šasi MTZ1 16 H1/H2 1600 A 3P",2.39]
["LV833682SP","Oneskorovacia jednotka MNR 200/250 VAC/D",1,"ks",176.715,"3606481173379",{"v":9.2,"d":"9.20"},{"v":8.4,"d":"8.40"},{"v":7.6,"d":"7.60"},{"v":165,"d":"165.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LV833682SP","oneskorovacia jednotka MNR 200/250 VAC/DC",0.02]
["LV833643SP","4P adaptéry pre vertikálne pripojenie –",1,"ks",{"v":670.4775000000001,"d":"670.478"},"3606481186508",{"v":27.5,"d":"27.50"},{"v":5.5,"d":"5.50"},{"v":21.5,"d":"21.50"},{"v":5259,"d":"5,259.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV833643SP","4P adaptéry pre vertikálne pripojenie – MTZ1",0]
["LV833584SP","Zvislé/vodorovné zadné prívody horné ale",1,"ks",{"v":192.3075,"d":"192.308"},"3606481186416",{"v":20,"d":"20.00"},{"v":5,"d":"5.00"},{"v":15,"d":"15.00"},{"v":1331,"d":"1,331.00"},"FR","","https://www.se.com/sk/sk/product/LV833584SP","zvislé/vodorovné zadné prívody horné alebo spodné – pevný MTZ1 3P (3 ks)",0.16]
["LV833210SP","1 súprava 2 tiahlí na blokovanie záskoko",1,"ks",{"v":213.09750000000003,"d":"213.098"},"3606481173232",{"v":104,"d":"104.00"},{"v":3.3,"d":"3.30"},{"v":3.3,"d":"3.30"},{"v":194,"d":"194.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LV833210SP","1 súprava 2 tiahlí na blokovanie záskokov",0]
["LV833173SP","1 zámok Profalux so zhodným kľúčom – náh",1,"ks",{"v":124.74,"d":"124.740"},"3606481173102",{"v":14,"d":"14.00"},{"v":6,"d":"6.00"},{"v":9,"d":"9.00"},{"v":102.5,"d":"102.50"},"FR","8301409000","https://www.se.com/sk/sk/product/LV833173SP","1 zámok Profalux so zhodným kľúčom – náhodná kombinácia",0]
["LV833171SP","Koncový spínač polohy CE/CD/CT (nízkoúro",1,"ks",{"v":62.37,"d":"62.370"},"3606481186270",{"v":5,"d":"5.00"},{"v":1,"d":"1.00"},{"v":5,"d":"5.00"},{"v":63,"d":"63.00"},"FR","8536508090","https://www.se.com/sk/sk/product/LV833171SP","koncový spínač polohy CE/CD/CT (nízkoúrovňový) – výsuvný MTZ",0]
["LV563550","istič CVS630F MA500 3P 36kA",1,"ks",{"v":688.8419999999999,"d":"688.842"},"3606480259326",{"v":30,"d":"30.00"},{"v":16,"d":"16.00"},{"v":24.4,"d":"24.40"},{"v":6039,"d":"6,039.00"},"","8536209090","https://www.se.com/sk/sk/product/LV563550","circuit breaker, EasyPact CVS630F, 36kA at 415VAC, 500A, MA trip unit, 3P3d",""]
["LV563305","ISTIČ CVS630F TM500D 3P3D",1,"ks",{"v":723.2399999999999,"d":"723.240"},"3606480257018",{"v":29,"d":"29.00"},{"v":15.5,"d":"15.50"},{"v":15.5,"d":"15.50"},{"v":5200,"d":"5,200.00"},"FR","8536209090","https://www.se.com/sk/sk/product/LV563305","Easypact CVS - CVS630F TM500D istič - 3P/3d",0.64]
["LV540311","ISTIČ CVS400F TM320D 4P4D",1,"ks",{"v":635.0399999999998,"d":"635.040"},"3606480247231",{"v":30,"d":"30.00"},{"v":21,"d":"21.00"},{"v":24.4,"d":"24.40"},{"v":8039,"d":"8,039.00"},"FR","8536209090","https://www.se.com/sk/sk/product/LV540311","circuit breaker, EasyPact CVS400F, 36kA at 415VAC, 320A, TM-D trip unit, 4P4d",0.96]
["LV525458","CVS250N TM250D 4P3D",1,"ks",{"v":595.3499999999999,"d":"595.350"},"3606480239526",{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":14.5,"d":"14.50"},{"v":2830,"d":"2,830.00"},"","8536209090","https://www.se.com/sk/sk/product/LV525458","circuit breaker EasyPact CVS250N, 50kA at 415VAC, 250A rating thermal magnetic TM-D trip unit, 4P 3d",0.34]
["LV525332","ISTIČ CVS250F TM200D 3P3D",1,"ks",{"v":370.44,"d":"370.440"},"3606480238383",{"v":19,"d":"19.00"},{"v":11,"d":"11.00"},{"v":14,"d":"14.00"},{"v":1929,"d":"1,929.00"},"FR","8536209090","https://www.se.com/sk/sk/product/LV525332","Easypact CVS - CVS250F TM200D istič - 3P/3d",0.23]
["LV516506","CVS160F 160A ETS 2.2 36kA 3P",1,"ks",{"v":357.21,"d":"357.210"},"3606482140899",{"v":8.6,"d":"8.60"},{"v":16.1,"d":"16.10"},{"v":10.5,"d":"10.50"},{"v":1800,"d":"1,800.00"},"","8536209090","https://www.se.com/sk/sk/product/LV516506","circuit breaker, EasyPact CVS160F, 36kA at 415VAC, ETS 2.2, 160A, 3P 3d",0.22]
["LV516352","ISTIČ CVS160F TM125D 4P4D",1,"ks",{"v":370.44,"d":"370.440"},"3606480229374",{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":15.5,"d":"15.50"},{"v":2249,"d":"2,249.00"},"CN","8536209090","https://www.se.com/sk/sk/product/LV516352","circuit breaker EasyPact CVS160F, 36kA at 415VAC, 125A rating thermal magnetic TM-D trip unit, 4P 4d",0.28]
["LV510737","Istič CVS160B TM100G 3P 25kA, char.B",1,"ks",{"v":149.93999999999997,"d":"149.940"},"3606480694479",{"v":8.6,"d":"8.60"},{"v":10.5,"d":"10.50"},{"v":16.1,"d":"16.10"},{"v":1640,"d":"1,640.00"},"CN","8536209090","https://www.se.com/sk/sk/product/LV510737","circuit breaker, EasyPact CVS160B, 25kA at 415VAC, 100A, TM-G trip unit, 3P3d",0.2]
["LV510550","CVS100B 40A ETS 2.2 25kA 3P",1,"ks",{"v":255.77999999999994,"d":"255.780"},"3606482140769",{"v":8.6,"d":"8.60"},{"v":16.1,"d":"16.10"},{"v":10.5,"d":"10.50"},{"v":1800,"d":"1,800.00"},"","8536201090","https://www.se.com/sk/sk/product/LV510550","circuit breaker, EasyPact CVS100B, 25kA at 415VAC, ETS 2.2, 40A, 3P 3d",0.22]
["LV510357","ISTIČ CVS100F TM100D 4P4D",1,"ks",{"v":211.67999999999995,"d":"211.680"},"3606480220647",{"v":19.5,"d":"19.50"},{"v":13.5,"d":"13.50"},{"v":15,"d":"15.00"},{"v":2159,"d":"2,159.00"},"CN","8536209090","https://www.se.com/sk/sk/product/LV510357","circuit breaker EasyPact CVS100F, 36kA at 415VAC, 100A rating thermal magnetic TM-D trip unit, 4P 4d",0.26]
["LV510331","ISTIČ CVS100F TM25D 3P3D",1,"ks",{"v":141.11999999999998,"d":"141.120"},"3606480220388",{"v":19,"d":"19.00"},{"v":11,"d":"11.00"},{"v":14,"d":"14.00"},{"v":1710,"d":"1,710.00"},"CN","8536201090","https://www.se.com/sk/sk/product/LV510331","Easypact CVS - CVS100F TM25D istič - 3P/3d",0.21]
["LV510305","ISTIČ CVS100B TM63D 3P3D",1,"ks",{"v":136.70999999999998,"d":"136.710"},"3606480220128",{"v":19.2,"d":"19.20"},{"v":13.8,"d":"13.80"},{"v":11.4,"d":"11.40"},{"v":1681,"d":"1,681.00"},"PL","8536209090","https://www.se.com/sk/sk/product/LV510305","circuit breaker, EasyPact CVS100B, 25kA at 415VAC, 63A, TM-D trip unit, 3P3d",0.2]
["LV481004","Vigirex RMH 220 až 240 V AC",1,"ks",{"v":1102.4999999999998,"d":"1102.500"},"3606485434735",{"v":15.3,"d":"15.30"},{"v":8.5,"d":"8.50"},{"v":11.1,"d":"11.10"},{"v":300,"d":"300.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LV481004","Vigirex RMH 220 až 240 V AC",0.06]
["LV480890","Svorky 4x240mm2 pre ISFL1250",1,"ks",{"v":463.0499999999999,"d":"463.050"},"3606485445175",{"v":31.5,"d":"31.50"},{"v":20,"d":"20.00"},{"v":27.1,"d":"27.10"},{"v":4705,"d":"4,705.00"},"DE","8536901000","https://www.se.com/sk/sk/product/LV480890","svorky 4x240mm2 na ISFL1250",0.56]
["LV480875","ISFL1250 3P montážna zbernica 185 mm",1,"ks",{"v":1102.4999999999998,"d":"1102.500"},"3606480341335",{"v":116,"d":"116.00"},{"v":21,"d":"21.00"},{"v":25,"d":"25.00"},{"v":14500,"d":"14,500.00"},"DE","8536508090","https://www.se.com/sk/sk/product/LV480875","Fuse switch disconnector, FuPacT ISFL1250, 1250A, 3P (3 poles switchable), connection to 185mm busbars, M12 screws",1.74]
["LV480829","ISFT630 - prismatická svorka pre neuprav",1,"ks",46.305,"3606481165886",{"v":2.2,"d":"2.20"},{"v":17,"d":"17.00"},{"v":17,"d":"17.00"},{"v":720,"d":"720.00"},"DE","8536901000","https://www.se.com/sk/sk/product/LV480829","Pressure plate with contact prism clamp for multiple use terminals, FuPacT ISFT630, 150mm² to 300mm², Cu/Al conductors",0.09]
["LV480816","SFT160 - prizmatická svorka pre neuprav",1,"ks",{"v":11.024999999999999,"d":"11.025"},"3606481165770",{"v":21,"d":"21.00"},{"v":1,"d":"1.00"},{"v":13,"d":"13.00"},{"v":86,"d":"86.00"},"DE","85361090","https://www.se.com/sk/sk/product/LV480816","Pressure plate with contact prism clamp for multiple use terminals,FuPacT ISFT160, 6mm² to 70mm², Cu/Al conductors",0]
["LV480804","ISFT250 3P svorky M10",1,"ks",{"v":158.75999999999996,"d":"158.760"},"3606481165664",{"v":35.2,"d":"35.20"},{"v":15,"d":"15.00"},{"v":20,"d":"20.00"},{"v":2500,"d":"2,500.00"},"DE","8536508090","https://www.se.com/sk/sk/product/LV480804","Fuse switch disconnector, FuPacT ISFT250, 250A, DIN NH01, 3 poles, backplate mounting",0.25]
["LV454442","24VDC napájací modul AD 100/125 VDC",1,"ks",{"v":296.25750000000005,"d":"296.258"},"3606481190949",{"v":12.6,"d":"12.60"},{"v":7.7,"d":"7.70"},{"v":11.4,"d":"11.40"},{"v":386,"d":"386.00"},"CN","8504409590","https://www.se.com/sk/sk/product/LV454442","External power supply module, input voltage 100VDC to 125VDC, output voltage 24VDC, output current 1A",0.05]
["LV438291","Kryty svoriek pre sériové pripojenie NSX",1,"ks",{"v":34.83899999999999,"d":"34.839"},"3606480586040",{"v":20.5,"d":"20.50"},{"v":10.8,"d":"10.80"},{"v":16.5,"d":"16.50"},{"v":345.9,"d":"345.90"},"FR","8547200090","https://www.se.com/sk/sk/product/LV438291","Terminal shield, ComPacT NSX400/630 DC, 3P, upstream/downstream, 3P series connection",0]
["LV434200","NSX KÁBEL L= 0,35 m",1,"ks",{"v":56.888999999999996,"d":"56.889"},"3606480022234",{"v":13,"d":"13.00"},{"v":2.5,"d":"2.50"},{"v":9,"d":"9.00"},{"v":42,"d":"42.00"},"FR","8544429090","https://www.se.com/sk/sk/product/LV434200","kábel- D = 0,35 m – pre NSX100 - 250, NSX400 - 630",0.01]
["LV433694","4P KRÁTKE KRYTY SVORIEK PRE >500V NSX400",1,"ks",{"v":40.13099999999999,"d":"40.131"},"3606485467061",{"v":41.5,"d":"41.50"},{"v":5.5,"d":"5.50"},{"v":27.5,"d":"27.50"},{"v":172,"d":"172.00"},"FR","8547200090","https://www.se.com/sk/sk/product/LV433694","Short terminal shield, ComPacT NSX400/630, Ue above 500VAC, pitch 45mm, IP40, 4 poles",0]
["LV432858","4P 600/5A MODUL PRÚDOVÉHO TRANSF. NSX",1,"ks",{"v":586.53,"d":"586.530"},"3606480020865",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":17,"d":"17.00"},{"v":2720,"d":"2,720.00"},"FR","8504312990","https://www.se.com/sk/sk/product/LV432858","modul meniča napätia 600 A – 4 póly – pre NSX630",0.33]
["LV432641","MOT.POH. 220-240VAC 50/60HZ NSX400-630",1,"ks",{"v":784.9799999999999,"d":"784.980"},"3606480020179",{"v":17.5,"d":"17.50"},{"v":19.8,"d":"19.80"},{"v":17.5,"d":"17.50"},{"v":3150,"d":"3,150.00"},"FR","8501200090","https://www.se.com/sk/sk/product/LV432641","Motorový pohon – MT400/630 – 208 - 277 V 60 Hz/220 - 240 V 50/60 Hz",0.38]
["LV432597T","PRIAMA ČIERNA OTOČNÁ RUKOVÄŤ NSX400-630",1,"ks",{"v":79.37999999999998,"d":"79.380"},"3606482004085",{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":15.5,"d":"15.50"},{"v":488,"d":"488.00"},"CN","8538909999","https://www.se.com/sk/sk/product/LV432597T","PRIAMA ČIERNA OTOČNÁ RUKOVÄŤ NSX400-630",0]
["LV432595","3P DLHÉ ROZŠÍRKRYTY SVORIEK NSX400-630",1,"ks",{"v":25.577999999999996,"d":"25.578"},"3606480019975",{"v":24,"d":"24.00"},{"v":10.1,"d":"10.10"},{"v":15.5,"d":"15.50"},{"v":368,"d":"368.00"},"FR","8547200090","https://www.se.com/sk/sk/product/LV432595","dlhý kryt svorky – 3 póly – pre INS/INV320 - 630, NSX400 - 630",0]
["LV432540","3P NÁSUVNÁ SÚPRAVA VIGI NSX400-630",1,"ks",{"v":436.59,"d":"436.590"},"3606480021008",{"v":12,"d":"12.00"},{"v":20,"d":"20.00"},{"v":11,"d":"11.00"},{"v":4266,"d":"4,266.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV432540","súprava zásuvnej základne – 3 póly – pre Vigi NSX400 - 630",0.51]
["LV432526","2 DLHÉ NADSTAVCESVORIEK NSX400-630",1,"ks",{"v":63.50399999999999,"d":"63.504"},"3606480019869",{"v":16,"d":"16.00"},{"v":3.5,"d":"3.50"},{"v":11,"d":"11.00"},{"v":573,"d":"573.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LV432526","rozšírenie koncoviek – izol. – dlhé – 3 póly – pre zásuv. základňu NS 400 - 630",0]
["LV432500","3 OKÁ PRE CU KÁB 240MM2 + 2M.B. 400-630",1,"ks",44.541,"3606480019470",{"v":13.2,"d":"13.20"},{"v":3,"d":"3.00"},{"v":13,"d":"13.00"},{"v":427,"d":"427.00"},"FR","8536901000","https://www.se.com/sk/sk/product/LV432500","3 káblové oká – pre medený kábel 240 mm² a fázové prepážky",0.05]
["LV432466","3P 440-550VAC 0,3-30A VIGI modul MB",1,"ks",{"v":1014.2999999999998,"d":"1014.300"},"3606481298676",{"v":19.5,"d":"19.50"},{"v":14,"d":"14.00"},{"v":17,"d":"17.00"},{"v":2696,"d":"2,696.00"},"IT","8536309090","https://www.se.com/sk/sk/product/LV432466","3P 440-550VAC 0,3-30A VIGI modul MB",0.32]
["LV432461","PRIEHĽADNÝ KRYT PRE MI2",1,"ks",{"v":20.285999999999998,"d":"20.286"},"3606480021299",{"v":20,"d":"20.00"},{"v":0.5,"d":"0.50"},{"v":12,"d":"12.00"},{"v":32,"d":"32.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV432461","prísluš. vypínacej jednotky – priehľadný kryt – pre Micrologic 2 – NSX400 - 630",0]
["LV431545","MOTOROVÝ POHON 110-130VDC NSX250",1,"ks",{"v":560.0699999999999,"d":"560.070"},"3606480020124",{"v":17,"d":"17.00"},{"v":10.5,"d":"10.50"},{"v":12,"d":"12.00"},{"v":1410,"d":"1,410.00"},"FR","8501200090","https://www.se.com/sk/sk/product/LV431545","Motorový pohon MT250 – 110 - 130 V DC",0.17]
["LV430558","4P 150/5A MODUL PRÚDOVÉHO TRANSF. NSX",1,"ks",{"v":370.44,"d":"370.440"},"3606480020742",{"v":17.5,"d":"17.50"},{"v":14,"d":"14.00"},{"v":14.5,"d":"14.50"},{"v":1160,"d":"1,160.00"},"FR","8504312990","https://www.se.com/sk/sk/product/LV430558","modul meniča napätia 150 A – 4 póly – pre NSX160",0.14]
["LV429494","3P 440-550V AC 0,03-10A VIGI modul MH",1,"ks",{"v":877.5899999999999,"d":"877.590"},"3606481298607",{"v":17.2,"d":"17.20"},{"v":13.4,"d":"13.40"},{"v":14.3,"d":"14.30"},{"v":1102,"d":"1,102.00"},"IT","8536309090","https://www.se.com/sk/sk/product/LV429494","3P 440-550V AC 0,03-10A VIGI modul MH",0.13]
["LV429493","4P 200-440V AC 0,03-10A VIGI modul MH",1,"ks",{"v":877.5899999999999,"d":"877.590"},"3606481298591",{"v":17.2,"d":"17.20"},{"v":13.5,"d":"13.50"},{"v":14.2,"d":"14.20"},{"v":1340,"d":"1,340.00"},"IT","8536309090","https://www.se.com/sk/sk/product/LV429493","4P 200-440V AC 0,03-10A VIGI modul MH",0.16]
["LV429440","MOT 48-60VAC 50/60HZ NSX100-160",1,"ks",{"v":335.15999999999997,"d":"335.160"},"3606480020063",{"v":17,"d":"17.00"},{"v":12,"d":"12.00"},{"v":10.5,"d":"10.50"},{"v":1394,"d":"1,394.00"},"FR","8501200090","https://www.se.com/sk/sk/product/LV429440","Motorový pohon MT100/160 – 48 - 60 V AC 50/60 Hz",0.17]
["LV429407","MN 220-240VAC 50/60HZ PODP. NSX100-630",1,"ks",{"v":80.70299999999999,"d":"80.703"},"3606480018961",{"v":6,"d":"6.00"},{"v":4.5,"d":"4.50"},{"v":4.6,"d":"4.60"},{"v":120,"d":"120.00"},"FR","8536301090","https://www.se.com/sk/sk/product/LV429407","podpäťové vypínanie MN – 208 - 277 V 60 Hz, 220 - 240 V 50/60 Hz",0.02]
["LV429394","MX250VDC VYPÍNACIA CIEVKA NSX100-630",1,"ks",{"v":57.33,"d":"57.330"},"3606480019166",{"v":6.2,"d":"6.20"},{"v":4.5,"d":"4.50"},{"v":4.7,"d":"4.70"},{"v":116,"d":"116.00"},"FR","8536301090","https://www.se.com/sk/sk/product/LV429394","derivačné napäťové relé MX – 250 V DC",0.02]
["LV429371T","UZAMYK.PRE 3VIS.ZÁMKY (BEZ ZÁMK)100-250",1,"ks",16.758,"3606481094537",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":11,"d":"11.00"},{"v":63,"d":"63.00"},"FR","8301600090","https://www.se.com/sk/sk/product/LV429371T","UZAMYK.PRE 3VIS.ZÁMKY (BEZ ZÁMK)100-250",0]
["LV429346","KONTAKT S PREDSTIHOM PRI VYP NSX100-250",1,"ks",{"v":55.124999999999986,"d":"55.125"},"3606480020445",{"v":8.2,"d":"8.20"},{"v":4,"d":"4.00"},{"v":6.5,"d":"6.50"},{"v":66,"d":"66.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LV429346","pomocný kontakt – predstih pri zapnutí 2 OC – NSX100 – 250",0.01]
["LV429313","5 KS NÁHRADNÝCH PREDĹŽNENÍ PÁKY",1,"ks",{"v":15.875999999999998,"d":"15.876"},"3606480021633",{"v":26.5,"d":"26.50"},{"v":1.5,"d":"1.50"},{"v":11,"d":"11.00"},{"v":38,"d":"38.00"},"FR","85389099","https://www.se.com/sk/sk/product/LV429313","predĺženia páky – pre NSX100 - 250 – súprava 5 ks.",0]
["LV429283","PLECHY PRE ISTIČ NÁSUVNÚ SÚP.NSX100-250",1,"ks",{"v":42.33599999999999,"d":"42.336"},"3606480021428",{"v":16,"d":"16.00"},{"v":3,"d":"3.00"},{"v":12.5,"d":"12.50"},{"v":508,"d":"508.00"},"PL","8538909999","https://www.se.com/sk/sk/product/LV429283","bočné dosky pre šasi – 2 póly/3 póly/4 póly – pre NSX100 - 250",0]
["LV429272","9 PÓL RUČNÝ (ZÁSUV/ZÁSTR) NSX100-630",1,"ks",{"v":54.242999999999995,"d":"54.243"},"3606480021565",{"v":27.4,"d":"27.40"},{"v":4.6,"d":"4.60"},{"v":13.2,"d":"13.20"},{"v":163,"d":"163.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LV429272","9-káblový pomocný konektor – NSX100 - 630",0]
["LV429259","3AL SVORKY(1X120-185MM2)DO250A100-250",1,"ks",{"v":24.254999999999995,"d":"24.255"},"3606480019357",{"v":15,"d":"15.00"},{"v":12,"d":"12.00"},{"v":3.5,"d":"3.50"},{"v":200,"d":"200.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LV429259","3 konektory kábla – 120 - 185 mm² – pre INS40 - 160/INV100 - 250/NSX100 - 250",0]
["LV429248","3SVORKY KBL(6X 1,5-35MM2)+2M.B.100-250",1,"ks",{"v":71.88299999999998,"d":"71.883"},"3606480019333",{"v":15.5,"d":"15.50"},{"v":3.3,"d":"3.30"},{"v":9.5,"d":"9.50"},{"v":349.5,"d":"349.50"},"FR","8536909500","https://www.se.com/sk/sk/product/LV429248","3 konektory – 6 káblov – 1,5 - 35 mm² – pre INS250/INV100 - 250/NSX100 - 250",0]
["LV429224","4 SVORKY 45° + MEDZIF. BAR.100-250",1,"ks",{"v":20.285999999999998,"d":"20.286"},"3606480019746",{"v":27,"d":"27.00"},{"v":2,"d":"2.00"},{"v":11,"d":"11.00"},{"v":67,"d":"67.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LV429224","4 45° rozšírenie svoriek – 4 póly – pre INS40 - 250/INV100 - 250/NSX100 - 250",0]
["LV426978","3 CU oka 50mm2 s medz.prepážkami NSXm",1,"ks",{"v":7.408799999999999,"d":"7.409"},"3606481166715",{"v":14.7,"d":"14.70"},{"v":1.3,"d":"1.30"},{"v":22.5,"d":"22.50"},{"v":150,"d":"150.00"},"PL","8536901000","https://www.se.com/sk/sk/product/LV426978","Crimp lugs for copper cable, ComPacT NSXm, 70mm² rigid cable, 50mm² flexible cable, set of 3 parts",0]
["LV426976","3 AL oka 120mm2 s medz.prepážkami NSXm",1,"ks",43.659,"3606481166739",{"v":12,"d":"12.00"},{"v":3,"d":"3.00"},{"v":13,"d":"13.00"},{"v":152,"d":"152.00"},"PL","8536901000","https://www.se.com/sk/sk/product/LV426976","Crimp lugs for aluminium cable, ComPacT NSXm, 120mm² rigid cable, set of 3 parts",0]
["LV426935T","Bočná čierna otočná rukoväť PP-B, GV4,",1,"ks",{"v":76.73399999999998,"d":"76.734"},"3606481995254",{"v":45.8,"d":"45.80"},{"v":9,"d":"9.00"},{"v":9.2,"d":"9.20"},{"v":734,"d":"734.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/LV426935T","Bočná čierna otočná rukoväť; PP-B, GV4, NSXm",0]
["LV426803","MN 110-130V AC/DC pod.spúšť, PP-B, NSXm",1,"ks",{"v":73.20599999999999,"d":"73.206"},"3606485412801",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":6,"d":"6.00"},{"v":64,"d":"64.00"},"FR","8536301090","https://www.se.com/sk/sk/product/LV426803","Standard undervoltage release MN, ComPacT NSXm, 125VDC, 110/130VAC 50/60Hz",0.01]
["LUFW10","TESYS U-MODUL ALARMU NADPRÚDU 1Z",1,"ks",{"v":141.836625,"d":"141.837"},"3389110365511",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":10.4,"d":"10.40"},{"v":54,"d":"54.00"},"FR","8531807000","https://www.se.com/sk/sk/product/LUFW10","TeSys U - tepelný alarm preťaženia funkčnej dosky LUF 1 NO",0.01]
["LUFP7","ROZHRANIE MODBUS-PROFIBUS DP",1,"ks",{"v":2699.4712499999996,"d":"2699.471"},"3389110109368",{"v":17.2,"d":"17.20"},{"v":5.8,"d":"5.80"},{"v":13.7,"d":"13.70"},{"v":218,"d":"218.00"},"SE","8517620000","https://www.se.com/sk/sk/product/LUFP7","komunikačná brána Profibus DP/Modbus – 1 Profibus DP SUB-D9 – 1 RJ45 Modbus",0.03]
["LUCD1XFU","TESYS U-ROZŠ. MODUL 0,35-1,4A 110-240V",1,"ks",109.809,"3389110365030",{"v":8,"d":"8.00"},{"v":10,"d":"10.00"},{"v":5.5,"d":"5.50"},{"v":124,"d":"124.00"},"FR","8537109899","https://www.se.com/sk/sk/product/LUCD1XFU","pokročilá riad. jednotka LUCD – trieda 20 – 0,35-1,4 A – 110-220 V DC/AC",0.02]
["LUCD12ES","TESYS U-ROZŠ. MODUL 3-12A 48-72V",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389110364880",{"v":8.5,"d":"8.50"},{"v":10.5,"d":"10.50"},{"v":5.5,"d":"5.50"},{"v":140,"d":"140.00"},"FR","8536301090","https://www.se.com/sk/sk/product/LUCD12ES","pokročilá riad. jednotka LUCD – trieda 20 – 3-12 A – 48-72 V DC/AC",0.02]
["LUCC1XB","TESYS U-ROZŠ. MODUL 0,35-1,4A 24VAC",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389110364545",{"v":10.2,"d":"10.20"},{"v":5.5,"d":"5.50"},{"v":8.5,"d":"8.50"},{"v":121,"d":"121.00"},"FR","8536301090","https://www.se.com/sk/sk/product/LUCC1XB","pokročilá riad. jednotka LUCC – trieda 10 – 0,35-1,4 A – 24 V AC",0.01]
["LUCB1XES","TESYS U-ROZŠ. MODUL 0,35-1,4A 48-72V",1,"ks",{"v":118.95975,"d":"118.960"},"3389110364194",{"v":5.2,"d":"5.20"},{"v":8.5,"d":"8.50"},{"v":10.3,"d":"10.30"},{"v":120,"d":"120.00"},"FR","8537109899","https://www.se.com/sk/sk/product/LUCB1XES","pokročilá riad. jednotka LUCB – trieda 10 – 0,35-1,4 A – 48-72 V DC/AC",0.02]
["LUCB05ES","TESYS U-ROZŠ. MODUL 1,25-5A 48-72V",1,"ks",109.809,"3389110364200",{"v":8,"d":"8.00"},{"v":10,"d":"10.00"},{"v":5.3,"d":"5.30"},{"v":114,"d":"114.00"},"FR","8537109899","https://www.se.com/sk/sk/product/LUCB05ES","pokročilá riad. jednotka LUCB – trieda 10 – 1,25-5 A – 48-72 V DC/AC",0.01]
["LUCA32B","TESYS U-ZÁKL. MODUL 8-32A 24VAC",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389110363937",{"v":7.874,"d":"7.87"},{"v":10.414,"d":"10.41"},{"v":5.588,"d":"5.59"},{"v":113,"d":"113.00"},"FR","8536301090","https://www.se.com/sk/sk/product/LUCA32B","štandartná riadiaca jednotka LUCA - trieda 10 - 8...32 A - 24 V DC",0.01]
["LUCA05FU","TESYS U-ZÁKL. MODUL 1,25-5A 110-240V",1,"ks",{"v":100.65825,"d":"100.658"},"3389110364026",{"v":5.2,"d":"5.20"},{"v":8.8,"d":"8.80"},{"v":8.2,"d":"8.20"},{"v":114,"d":"114.00"},"FR","8536301090","https://www.se.com/sk/sk/product/LUCA05FU","štandard. riad. jednotka LUCA – trieda 10 – 1,25-5 A – 110-220 V DC/AC",0.01]
["LUALF1","TESYS U-OBMEDZOVAČ 130KA CARTR.",1,"ks",{"v":124.45019999999998,"d":"124.450"},"785901291824",{"v":4.5,"d":"4.50"},{"v":7.6,"d":"7.60"},{"v":4.7,"d":"4.70"},{"v":132,"d":"132.00"},"US","8536303099","https://www.se.com/sk/sk/product/LUALF1","Limiter cartridge, TeSys Ultra, activation 50kA, 130kA at 440V, for use with limiter disconnector LUALB1",""]
["LU9MR1","TESYS U-SVORKOVNICA RIADENIA REVERZÁCIE",1,"ks",{"v":9.0592425,"d":"9.059"},"3389110367584",{"v":5,"d":"5.00"},{"v":3,"d":"3.00"},{"v":3.5,"d":"3.50"},{"v":26,"d":"26.00"},"CZ","8536901000","https://www.se.com/sk/sk/product/LU9MR1","riad. svorkovnica – pre reverzný spúšťač motora TeSys U",0]
["LU9AD7","TESYS U-PROFIBUS DP KONEKTOR",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389119407854",{"v":10.5,"d":"10.50"},{"v":2.5,"d":"2.50"},{"v":5,"d":"5.00"},{"v":44,"d":"44.00"},"DE","8536901000","https://www.se.com/sk/sk/product/LU9AD7","TeSys U PROFIBUS DP konektor LU9 A pre TeSys spúšťače, kontroléry",0.01]
["LU2B32ES","TESYS U-REVERZAČNÝ MODUL 32A 48-72V",1,"ks",{"v":384.33149999999995,"d":"384.332"},"3389110362992",{"v":25.5,"d":"25.50"},{"v":5.5,"d":"5.50"},{"v":14.7,"d":"14.70"},{"v":1270,"d":"1,270.00"},"FR","8536508090","https://www.se.com/sk/sk/product/LU2B32ES","elektrická základňa – TeSys U – ovládanie skrutkovej svorky 32 A – 48-72 V DC",0.15]
["LTMR27EFM","TeSys T Ethernet TCP IP 1,35 27A",1,"ks",{"v":791.5398749999999,"d":"791.540"},"3389119404891",{"v":13.5,"d":"13.50"},{"v":7.2,"d":"7.20"},{"v":10,"d":"10.00"},{"v":530,"d":"530.00"},"CN","8537109199","https://www.se.com/sk/sk/product/LTMR27EFM","kontrolór motora LTM R TeSys T - 100..240 V AC 27 A pre Ethernet TCP/IP",0]
["LTMR100CBD","TESYS T-CANOPEN, 5-100A, 24VDC",1,"ks",{"v":800.6906249999998,"d":"800.691"},"3389119404723",{"v":13.5,"d":"13.50"},{"v":10,"d":"10.00"},{"v":7,"d":"7.00"},{"v":515,"d":"515.00"},"KR","8537109199","https://www.se.com/sk/sk/product/LTMR100CBD","kontrolér motora LTM R TeSys T - 24 V DC 100 A pre CANopen",0.06]
["LTMEV40FM","TESYS T-ROZŠIROVACÍ MODUL, 115-230VAC",1,"ks",{"v":274.5225,"d":"274.523"},"3389119404938",{"v":13.6,"d":"13.60"},{"v":5.5,"d":"5.50"},{"v":7.2,"d":"7.20"},{"v":200,"d":"200.00"},"CN","8536909500","https://www.se.com/sk/sk/product/LTMEV40FM","nástavba modul LTM E TeSys T - 100..240 V AC",0.02]
["LT4706F7S","EL. NADPRÚD. RELÉ 0,5A-6A, 110V AC MAN",1,"ks",{"v":75.951225,"d":"75.951"},"8809755436469",8.38,7.11,9.14,{"v":200,"d":"200.00"},"KR","8536490099","https://www.se.com/sk/sk/product/LT4706F7S","elektronické nadprúdové relé -manuálne-0.5..6A- 100..120V 50Hz",0.02]
["LRD380","Tepelné nadprúdové relé 62-80A tr 10A",1,"ks",{"v":155.56275,"d":"155.563"},"3606481311986",{"v":13.5,"d":"13.50"},{"v":6,"d":"6.00"},{"v":10.5,"d":"10.50"},{"v":375,"d":"375.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LRD380","tepelné nadprúdové relé 62...80A - trieda 10A",0.05]
["LRD350","TEPEL. NADPRÚDOVÉ RELÉ 37-50A",1,"ks",{"v":87.84719999999999,"d":"87.847"},"3389119215503",{"v":13.7,"d":"13.70"},{"v":6.4,"d":"6.40"},{"v":10.5,"d":"10.50"},{"v":394,"d":"394.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LRD350","istiace nadprúdové relé - 37...50A - trieda 10A",0.05]
["LRD332L","TEPEL. NADPR. RELÉ 23-32A, TRIEDA 20",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389119215558",{"v":14,"d":"14.00"},{"v":6.3,"d":"6.30"},{"v":11,"d":"11.00"},{"v":422,"d":"422.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LRD332L","istiace nadprúdové relé - 23...32A - trieda 20",0.05]
["LRD32S183","TEP. NADPRÚD. RELÉ",1,"ks",109.809,"3389118081307",{"v":9,"d":"9.00"},{"v":7.8,"d":"7.80"},{"v":7.8,"d":"7.80"},{"v":148,"d":"148.00"},"FR","85364900","https://www.se.com/sk/sk/product/LRD32S183","TEP.NADPRÚD.RELÉ",0]
["LRD22L","Tepelné relé 17-24 A tr. 20",1,"ks",{"v":91.5075,"d":"91.508"},"3606480609626",{"v":4.5,"d":"4.50"},{"v":8.3,"d":"8.30"},{"v":7.2,"d":"7.20"},{"v":144,"d":"144.00"},"TH","8536490099","https://www.se.com/sk/sk/product/LRD22L","Thermal overload relay, TeSys Deca, 690VAC, 17 to 24A, 1NO+1NC, class 20, for D25 to D38, screw clamp",0.02]
["LRD12S183","TEP. NADPRÚD. RELÉ",1,"ks",{"v":54.9045,"d":"54.905"},"3389118081253",{"v":9,"d":"9.00"},{"v":7.7,"d":"7.70"},{"v":7.7,"d":"7.70"},{"v":144,"d":"144.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LRD12S183","TEP.NADPRÚD.RELÉ",0]
["LRD063","OVERLOAD REL.1 A 1,6A RES",1,"ks",{"v":141.836625,"d":"141.837"},"3389110821994",{"v":10.4,"d":"10.40"},{"v":5.5,"d":"5.50"},{"v":8,"d":"8.00"},{"v":189,"d":"189.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LRD063","istiace nadprúdové relé - 1...1.6A - trieda 10A",0.02]
["LR9F7575","TEPELNÉ NADPRÚD. RELÉ",1,"ks",{"v":846.4443749999999,"d":"846.444"},"3389110640212",{"v":26,"d":"26.00"},{"v":17.2,"d":"17.20"},{"v":18,"d":"18.00"},{"v":1884,"d":"1,884.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LR9F7575","istiace nadprúdové relé pre motor - 200...330A - trieda 20",0.23]
["LR9F5563","TEPELNÉ NADPRÚD. RELÉ",1,"ks",{"v":498.715875,"d":"498.716"},"3389110640175",{"v":16,"d":"16.00"},{"v":13,"d":"13.00"},{"v":15.5,"d":"15.50"},{"v":880,"d":"880.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LR9F5563","TeSys LRF - electronic thermal overload relay - 48...80 A - class 20",0.11]
["LR9D32","Elektronické tepelné relé 6.4-32A",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3606485420950",{"v":9,"d":"9.00"},{"v":5.3,"d":"5.30"},{"v":7.4,"d":"7.40"},{"v":180,"d":"180.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LR9D32","elektronické tepelné relé 6.4-32A",0.02]
["LR97D38B","EL. NADPRÚD. RELÉ 20A-38A, 24V AC/DC",1,"ks",{"v":132.68587499999998,"d":"132.686"},"8809755436377",{"v":7.6,"d":"7.60"},{"v":5,"d":"5.00"},{"v":6.9,"d":"6.90"},{"v":172,"d":"172.00"},"KR","8536419089","https://www.se.com/sk/sk/product/LR97D38B","elektronické nadprúdové relé pre motor - 20...38A - 24V 50Hz/DC",0.02]
["LR3D340","TEP.NADPR.RELÉ 30-40A BEZ NESYMETRIE FÁZ",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389119215916",{"v":13.7,"d":"13.70"},{"v":6.5,"d":"6.50"},{"v":11,"d":"11.00"},{"v":392,"d":"392.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LR3D340","istiace nadprúdové relé - 30...40A - trieda 10A",0.05]
["LR3D318","TEP.NADPR.RELÉ 12-18A BEZ NESYMETRIE FÁZ",1,"ks",{"v":87.38966249999999,"d":"87.390"},"3389119215886",{"v":13.8,"d":"13.80"},{"v":7,"d":"7.00"},{"v":10.8,"d":"10.80"},{"v":375,"d":"375.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LR3D318","istiace nadprúdové relé - 12...18A - trieda 10A",0.05]
["LR3D06","TEPELNÉ RELÉ 1-1,6A BEZ NESYMETRIE FÁZ",1,"ks",{"v":48.498974999999994,"d":"48.499"},"3389110346923",{"v":8.8,"d":"8.80"},{"v":4.9,"d":"4.90"},{"v":7.6,"d":"7.60"},{"v":140,"d":"140.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LR3D06","istiace nadprúdové relé - 1...1.6A - trieda 10A",0.02]
["LR2D3559","TEPELNÉ RELÉ TRIEDA 20 48..65A",1,"ks",{"v":224.193375,"d":"224.193"},"3389110229110",{"v":11.8,"d":"11.80"},{"v":7.8,"d":"7.80"},{"v":8.5,"d":"8.50"},{"v":525,"d":"525.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LR2D3559","TeSys D istiace nadprúdové relé - 48...65 A - trieda 20",0.06]
["LP5K1201BW3","REV. STÝKAČ K 12A DC ZNÍŽ. SPOTR.",1,"ks",{"v":100.65825,"d":"100.658"},"3389110791228",{"v":6.2,"d":"6.20"},{"v":6.5,"d":"6.50"},{"v":9.2,"d":"9.20"},{"v":448,"d":"448.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP5K1201BW3","TeSys K reverzačný stýkač - 3P ( 3 NO ) - AC - 3 - <lt/> = 440 V 12 - 24 V DC cievka",0]
["LP4K09004BW3","STÝKAČ K 9A DC SO ZNÍŽ. SPOTR.",1,"ks",{"v":38.8906875,"d":"38.891"},"3389110498646",{"v":6.5,"d":"6.50"},{"v":5,"d":"5.00"},{"v":6.2,"d":"6.20"},{"v":220,"d":"220.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP4K09004BW3","ministýka? 4P (4Z) 20A AC-1 440V - cievka 24V DC",0.03]
["LP4K0601BW3","STÝKAČ K 6A DC SO ZNÍŽ. SPOTR.",1,"ks",{"v":35.687925,"d":"35.688"},"3389110428551",{"v":6.2,"d":"6.20"},{"v":6.6,"d":"6.60"},{"v":4.8,"d":"4.80"},{"v":221,"d":"221.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP4K0601BW3","ministýkač 3P (3Z) 6A AC-3 440V -pomocný kontakt 1V- cievka 24V DC",0.03]
["LP1K1210JD","STÝKAČ K 12A DC",1,"ks",{"v":43.008525,"d":"43.009"},"3389110790887",{"v":4.8,"d":"4.80"},{"v":6.5,"d":"6.50"},{"v":6.2,"d":"6.20"},{"v":217,"d":"217.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP1K1210JD","ministýkač 3P (3Z) 12A AC-3 440V -pomocný kontakt 1Z- cievka 12V DC",0.03]
["LP1K0910JD","STÝKAČ K 9A DC",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3389110496420",{"v":6.9,"d":"6.90"},{"v":4.8,"d":"4.80"},{"v":6.3,"d":"6.30"},{"v":217,"d":"217.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP1K0910JD","Contactor, TeSys K, 3P, AC-3/AC-3e, 440V, 9A, 1NO aux, 12V DC coil,screw clamps",0.03]
["LP1K0910ED","STÝKAČ K 9A DC",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3389110496352",{"v":6.5,"d":"6.50"},{"v":5,"d":"5.00"},{"v":6.2,"d":"6.20"},{"v":221,"d":"221.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP1K0910ED","ministýkač 3P (3Z) 9A AC-3 440V-pomocný kontakt 1Z-cievka 48V DC",0.03]
["LP1K09008ED","STÝKAČ K 9A DC",1,"ks",{"v":36.602999999999994,"d":"36.603"},"3389110495904",{"v":4.8,"d":"4.80"},{"v":6.5,"d":"6.50"},{"v":6.2,"d":"6.20"},{"v":219,"d":"219.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP1K09008ED","TeSys K stýkač - 4P (2Z + 2V) -AC-1 - <lt/>= 440 V 20 A - cievka 48 V DC",0.03]
["LP1K06105BD","STÝKAČ K 6A DC",1,"ks",{"v":40.2633,"d":"40.263"},"3389110494808",{"v":4.8,"d":"4.80"},{"v":6.8,"d":"6.80"},{"v":6.2,"d":"6.20"},{"v":249,"d":"249.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP1K06105BD","TeSys K stýkač - 3P ( 3Z ) - AC - 3 - <lt/> = 440 V 6 A - cievka 24 V DC",0.03]
["LP1K06013BD3","CONTACTOR",1,"ks",{"v":128.11049999999997,"d":"128.111"},"3389118020856",{"v":6.2,"d":"6.20"},{"v":4.8,"d":"4.80"},{"v":6.5,"d":"6.50"},{"v":224,"d":"224.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LP1K06013BD3","Contactor, TeSys K, 3P, AC-3/AC-3e, 440V, 6A, 1NC aux, 24V DC coil,spring terminal",0]
["LP1D40008ED","STÝKAČ 4P 60A 48V DC",1,"ks",{"v":306.550125,"d":"306.550"},"3389110200133",{"v":14,"d":"14.00"},{"v":19.5,"d":"19.50"},{"v":9.5,"d":"9.50"},{"v":2210,"d":"2,210.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LP1D40008ED","TeSys D stýkač - 4P(2Z+2V) - AC-1 - <lt/>= 440 V 60 A - 48 V DC cievka",0.27]
["LJ7K06Q705","SPÚŠŤAČ V SKRINI",1,"ks",{"v":431.0003249999999,"d":"431.000"},"3389110787306",{"v":25.5,"d":"25.50"},{"v":18,"d":"18.00"},{"v":22.5,"d":"22.50"},{"v":2270,"d":"2,270.00"},"FR","8537109899","https://www.se.com/sk/sk/product/LJ7K06Q705","spúšťač v skrinke - TeSys LJ7 - K - 0.63 ... 1 A - cievka 380 V AC",""]
["LGY412548","DISTRIBUČNÝ BLOK 4P 125A 48 BODOV",1,"ks",{"v":31.751999999999995,"d":"31.752"},"3606480542091",{"v":13,"d":"13.00"},{"v":5.5,"d":"5.50"},{"v":10.7,"d":"10.70"},{"v":457,"d":"457.00"},"FR","8536901000","https://www.se.com/sk/sk/product/LGY412548","skrutková prípojnica 4P 125A - 48 pozic",0]
["LG7K09Q714","SPÚŠŤAČ V SKRINI",1,"ks",{"v":512.4419999999999,"d":"512.442"},"3389110662061",{"v":29,"d":"29.00"},{"v":22.5,"d":"22.50"},{"v":23,"d":"23.00"},{"v":1740,"d":"1,740.00"},"FR","8537109899","https://www.se.com/sk/sk/product/LG7K09Q714","TeSys LG - spúšťač v skrinke - 6...10 A - 380/400 V AC cievka",0.21]
["LE2D09P7","REVERZAČNÝ SPÚŠŤAČ V SKRINI",1,"ks",{"v":288.24862499999995,"d":"288.249"},"3389110632231",{"v":20,"d":"20.00"},{"v":25.5,"d":"25.50"},{"v":16,"d":"16.00"},{"v":1586,"d":"1,586.00"},"FR","8537109899","https://www.se.com/sk/sk/product/LE2D09P7","TeSys LE - reverzačná spúšťač v skrinke - le2 - D - 9 A - cievka 230 V AC",0.19]
["LE1M35U721","SPÚŠŤAČ V SKRINI",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110781328",{"v":16.5,"d":"16.50"},{"v":8.2,"d":"8.20"},{"v":11.5,"d":"11.50"},{"v":591,"d":"591.00"},"CZ","8537109899","https://www.se.com/sk/sk/product/LE1M35U721","TeSys LE - spúšťač v skrinke - LE1-M - 10...14 A - cievka 240 V AC",0.07]
["LE1M35P710","Motorový spúštač",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110963069",{"v":16.5,"d":"16.50"},{"v":8.2,"d":"8.20"},{"v":11.6,"d":"11.60"},{"v":574,"d":"574.00"},"CZ","8537109899","https://www.se.com/sk/sk/product/LE1M35P710","TeSys LE - spúšťač v skrinke - 2.6 ... 3.7 A - 230 V AC cievka",0.07]
["LE1M35N712","SPÚŠŤAČ V SKRINI",1,"ks",{"v":118.95975,"d":"118.960"},"3389110781199",{"v":16.5,"d":"16.50"},{"v":8.5,"d":"8.50"},{"v":11.5,"d":"11.50"},{"v":589,"d":"589.00"},"CZ","8537109899","https://www.se.com/sk/sk/product/LE1M35N712","TeSys LE - spúšťač v skrinke - LE1 - M - 3.7 ... 5.5 A - cievka 415 V AC",0.07]
["LE1D09V7","SPÚŠŤAČ V SKRINI",1,"ks",109.809,"3389110573725",{"v":25.5,"d":"25.50"},{"v":19.5,"d":"19.50"},{"v":20,"d":"20.00"},{"v":874,"d":"874.00"},"FR","8536508090","https://www.se.com/sk/sk/product/LE1D09V7","Enclosed DOL starter,TeSys LE,9A,400V AC coil,including 1 LC1D,2 pushbuttons",0.1]
["LC3D80B7","Y/D - 75KW/400V BEZ MECH. BL., 24V AC",1,"ks",{"v":1098.09,"d":"1098.090"},"3389110094206",{"v":38,"d":"38.00"},{"v":27,"d":"27.00"},{"v":26,"d":"26.00"},{"v":6455,"d":"6,455.00"},"FR","85364190","https://www.se.com/sk/sk/product/LC3D80B7","Star delta starter, TeSys Deca, 3 x 3P (3NO), 80A, 24V AC coil",0.77]
["LC3D18AB7","Y/D - 18,5KW/400V S MECH. BL., 24V AC",1,"ks",{"v":535.3188749999999,"d":"535.319"},"3389110546064",{"v":24,"d":"24.00"},{"v":18,"d":"18.00"},{"v":17,"d":"17.00"},{"v":1728,"d":"1,728.00"},"FR","8537109899","https://www.se.com/sk/sk/product/LC3D18AB7","spúšťač Y-D- 3x 3P (3Z) 18A - cievka 24V 50Hz",0.21]
["LC2K1210P7","REVERZAČNÝ STÝKAČ 12A AC",1,"ks",{"v":79.15398749999999,"d":"79.154"},"3389110856934",{"v":9.1,"d":"9.10"},{"v":6,"d":"6.00"},{"v":6.4,"d":"6.40"},{"v":364,"d":"364.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2K1210P7","reverzačný ministýkač 3P 12A AC-3 440V-pomocný kontakt 1Z-cievka 230V 50Hz",0.04]
["LC2K0910P7","REVERZAČNÝ STÝKAČ 9A AC",1,"ks",{"v":65.4278625,"d":"65.428"},"3389110492514",{"v":6,"d":"6.00"},{"v":6.5,"d":"6.50"},{"v":9,"d":"9.00"},{"v":368,"d":"368.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2K0910P7","reverzačný ministýkač 3P 9A AC-3 440V-pomocný kontakt 1Z-cievka 230V 50Hz",0.05]
["LC2K0901B7","REVERZAČNÝ STÝKAČ 9A AC",1,"ks",{"v":65.4278625,"d":"65.428"},"3389110429398",{"v":6,"d":"6.00"},{"v":6.5,"d":"6.50"},{"v":9.3,"d":"9.30"},{"v":362,"d":"362.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2K0901B7","reverzačný ministýkač 3P 9A AC-3 440V-pomocný kontakt 1V-cievka 24V 50Hz",0.04]
["LC2F1854","REV. STÝKAČ 185A 4-PÓL BEZ CIEVOK",1,"ks",{"v":1875.90375,"d":"1875.904"},"3389110227413",{"v":50,"d":"50.00"},{"v":32,"d":"32.00"},{"v":31,"d":"31.00"},{"v":13240,"d":"13,240.00"},"CZ","85364900","https://www.se.com/sk/sk/product/LC2F1854","TeSys F changeover contactor - 4P(4 NO) AC-1 <lt/>= 440 V 275 A - without coil",1.59]
["LC2F1504","REV. STÝKAČ 150A 4-PÓL BEZ CIEVOK",1,"ks",{"v":1738.6424999999997,"d":"1738.643"},"3389110227390",{"v":53,"d":"53.00"},{"v":21.5,"d":"21.50"},{"v":35.5,"d":"35.50"},{"v":10540,"d":"10,540.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC2F1504","TeSys F changeover contactor - 4P(4 NO) AC-1 <lt/>= 440 V 250 A - without coil",1.34]
["LC2D65ABNE","TeSys D Green 3P reverzačný 65A 24 - 60V",1,"ks",{"v":814.4167499999999,"d":"814.417"},"3606480988141",{"v":19.8,"d":"19.80"},{"v":14.5,"d":"14.50"},{"v":16.2,"d":"16.20"},{"v":2360,"d":"2,360.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2D65ABNE","reverzačný stýkač 3P 65A AC-3 440V - cievka 24...60V 50Hz/DC",""]
["LC2D50ABBE","TeSys D Green 3P reverzačný 50A 24V DC",1,"ks",{"v":562.771125,"d":"562.771"},"3606480988189",{"v":19.4,"d":"19.40"},{"v":14.4,"d":"14.40"},{"v":16.2,"d":"16.20"},{"v":2371,"d":"2,371.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC2D50ABBE","reverzačný stýkač 3P 50A AC-3 440V -cievka 24V DC",0.28]
["LC2D38P7","REVERZ. STÝKAČ 38A 230V AC",1,"ks",{"v":306.550125,"d":"306.550"},"3389110391954",{"v":11.4,"d":"11.40"},{"v":13.5,"d":"13.50"},{"v":11.4,"d":"11.40"},{"v":943,"d":"943.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2D38P7","reverzačný stýkač 3P(3Z) 38A AC-3 440V-pomocné kontakty 1Z+1V-cievka 230V 50Hz",0.11]
["LC2D32P7","REVERZ. STÝKAČ 32A 230V AC",1,"ks",{"v":256.22099999999995,"d":"256.221"},"3389110391572",{"v":14.5,"d":"14.50"},{"v":11.2,"d":"11.20"},{"v":11.2,"d":"11.20"},{"v":944,"d":"944.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2D32P7","reverzačný stýkač 3P(3Z) 32A AC-3 440V-pomocné kontakty 1Z+1V-cievka 230V 50Hz",0.11]
["LC2D25D7","REVERZ. STÝKAČ 25A 42V AC",1,"ks",{"v":201.3165,"d":"201.317"},"3389110386752",{"v":11.8,"d":"11.80"},{"v":10.9,"d":"10.90"},{"v":11.4,"d":"11.40"},{"v":815,"d":"815.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2D25D7","reverzačný stýkač 3P(3Z) 25A AC-3 440V-pomocné kontakty 1Z+1V-cievka 42V 50Hz",0.1]
["LC2D12ED","REVERZ. STÝKAČ 12A 48V DC",1,"ks",{"v":187.59037499999997,"d":"187.590"},"3389110392289",{"v":11,"d":"11.00"},{"v":9.4,"d":"9.40"},{"v":11.4,"d":"11.40"},{"v":730,"d":"730.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2D12ED","Reversing Contactor, TeSys Deca, 3P(3NO),AC-3, <lt/>=440V 12A,48V DC coil, screw clamp terminals",0.09]
["LC2D09F7","REVERZ. STÝKAČ 9A 110V AC",1,"ks",{"v":100.65825,"d":"100.658"},"3389110383386",{"v":13.5,"d":"13.50"},{"v":11.3,"d":"11.30"},{"v":9.5,"d":"9.50"},{"v":810,"d":"810.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2D09F7","reverzačný stýkač 3P(3Z) 9A AC-3 440V-pomocné kontakty 1Z+1V-cievka 110V 50Hz",0.1]
["LC2D096BD","Reverzacný stýkac 9A oka",1,"ks",{"v":164.71349999999998,"d":"164.714"},"3389110706529",{"v":11,"d":"11.00"},{"v":9.4,"d":"9.40"},{"v":11.4,"d":"11.40"},{"v":1016.9999999999999,"d":"1,017.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC2D096BD","TeSys D reverzační stykač - 3P(3Z) - AC-3 - <lt/>= 440 V 9 A - 24 V DC cívka",0.13]
["LC1K1610U7","STÝKAČ K 16A AC",1,"ks",{"v":45.75375,"d":"45.754"},"3389118021709",{"v":6.4,"d":"6.40"},{"v":6.4,"d":"6.40"},{"v":4.9,"d":"4.90"},{"v":185,"d":"185.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1K1610U7","ministýkač 3P (3Z) 16A AC-3 440V-pomocný kontakt 1Z- cievka 230...240V 50Hz",0.02]
["LC1K1601M7","STÝKAČ K 16A AC",1,"ks",{"v":45.296212499999996,"d":"45.296"},"3389110124835",{"v":6.5,"d":"6.50"},{"v":5,"d":"5.00"},{"v":6,"d":"6.00"},{"v":177.5,"d":"177.50"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1K1601M7","ministýkač 3P (3Z) 16A AC-3 440V-pomocný kontakt 1V- cievka 220...230V 50Hz",0.02]
["LC1K1210F7","STÝKAČ K 12A AC",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110789751",{"v":6.2,"d":"6.20"},{"v":6.5,"d":"6.50"},{"v":4.8,"d":"4.80"},{"v":179,"d":"179.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1K1210F7","ministýkač 3P (3Z) 12A AC-3 440V-pomocný kontakt 1Z-cievka 110V 50Hz",0.02]
["LC1K1201F7","STÝKAČ K 12A AC",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110789638",{"v":6.5,"d":"6.50"},{"v":4.8,"d":"4.80"},{"v":6.2,"d":"6.20"},{"v":181,"d":"181.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1K1201F7","ministýkač 3P (3Z) 12A AC-3 440V-pomocný kontakt 1V-cievka 110V 50Hz",0.02]
["LC1K0910P7","STÝKAČ K 9A AC",1,"ks",{"v":28.824862499999995,"d":"28.825"},"3389110364521",{"v":6.5,"d":"6.50"},{"v":5,"d":"5.00"},{"v":6,"d":"6.00"},{"v":179.4,"d":"179.40"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1K0910P7","ministýkač 3P (3Z) 9A AC-3 440V-pomocný kontakt 1Z- cievka 230V 50Hz",0.02]
["LC1K09105E7","STÝKAČ K 9A AC",1,"ks",{"v":31.5700875,"d":"31.570"},"3389110490404",{"v":6.8,"d":"6.80"},{"v":4.8,"d":"4.80"},{"v":6.2,"d":"6.20"},{"v":202,"d":"202.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1K09105E7","ministýkač 3P (3Z) 9A AC-3 440V-pomocný kontakt 1Z- cievka 48V 50Hz",0.02]
["LC1K09008M7","STÝKAČ K 9A AC",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110488876",{"v":4.8,"d":"4.80"},{"v":6.5,"d":"6.50"},{"v":6.2,"d":"6.20"},{"v":177,"d":"177.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1K09008M7","TeSys K stýkač - 4P (2Z + 2V) -AC-1 - <lt/>= 440 V 20 A - cievka 220...230 V AC",0.02]
["LC1K09004E7","STÝKAČ K 9A AC",1,"ks",{"v":30.197474999999997,"d":"30.197"},"3389110488401",{"v":4.8,"d":"4.80"},{"v":6.5,"d":"6.50"},{"v":6.2,"d":"6.20"},{"v":180,"d":"180.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1K09004E7","TeSys K stýkač - 4P ( 4Z ) - AC - 1 - <lt/> = 440 V 20 A - cievka 48 V AC",0.02]
["LC1K0610FE7","STÝKAČ K 6A AC",1,"ks",{"v":31.5700875,"d":"31.570"},"3389110130461",{"v":6.6,"d":"6.60"},{"v":5,"d":"5.00"},{"v":6.3,"d":"6.30"},{"v":177,"d":"177.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1K0610FE7","Contactor, TeSys K, 3P, AC-3/AC-3e,440V 6A, aux. 1NO, 115V AC coil",0.02]
["LC1K0610B72","STÝKAČ K 6A AC",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110487558",{"v":4.9,"d":"4.90"},{"v":6.5,"d":"6.50"},{"v":6.3,"d":"6.30"},{"v":180,"d":"180.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1K0610B72","ministýkač 3P (3Z) 6A AC-3 440V-pomocný kontakt 1Z- cievka 24V 50Hz",0.02]
["LC1K06016BLS207","Stýkače TeSys K 3P AC3 440V 6A 24V DC",1,"ks",{"v":74.57861249999999,"d":"74.579"},"3606480920554",{"v":6.2,"d":"6.20"},{"v":5.7,"d":"5.70"},{"v":4.8,"d":"4.80"},{"v":215,"d":"215.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1K06016BLS207","Contactor, TeSys K, 3P, AC-3 <lt/>=440V 6A, 1NC aux., 24V DC low consumption coil",0.03]
["LC1G400BEEA","Stýkač 400A 3P 24-48V AC/DC pokročilý",1,"ks",{"v":1235.3512499999997,"d":"1235.351"},"3606481922281",{"v":37,"d":"37.00"},{"v":22.5,"d":"22.50"},{"v":31,"d":"31.00"},{"v":8944,"d":"8,944.00"},"CN","8536419089","https://www.se.com/sk/sk/product/LC1G400BEEA","High power contactor, TeSys Giga, 3 pole (3NO), AC-3 <lt/>=440V 400A, advanced version, 24…48V wide band AC/DC coil",1.07]
["LC1G3304KUEN","Stýkač 330A 4P 100-250V AC / DC štandard",1,"ks",{"v":1235.3512499999997,"d":"1235.351"},"3606481922175",{"v":32,"d":"32.00"},{"v":27.5,"d":"27.50"},{"v":31,"d":"31.00"},{"v":9074,"d":"9,074.00"},"CN","8536490099","https://www.se.com/sk/sk/product/LC1G3304KUEN","\"Stykač TeSys G 330A 4P AC3 cívka 100-250V AC/DC standard\"",1.07]
["LC1G2254KUEN","Stýkač 225A 4P 100-250V AC / DC štandard",1,"ks",{"v":960.8287499999999,"d":"960.829"},"3606481922151",{"v":38.5,"d":"38.50"},{"v":24.5,"d":"24.50"},{"v":27,"d":"27.00"},{"v":5687,"d":"5,687.00"},"CN","8536490099","https://www.se.com/sk/sk/product/LC1G2254KUEN","\"Stykač TeSys G 225A 4P AC3 cívka 100-250V AC/DC standard\"",0.68]
["LC1G1154LSEA","Stýkač 115A 4P 200-500V AC / DC pokročil",1,"ks",{"v":626.8263749999999,"d":"626.826"},"3606481922724",{"v":39,"d":"39.00"},{"v":25,"d":"25.00"},{"v":26.7,"d":"26.70"},{"v":6374,"d":"6,374.00"},"CN","8536490099","https://www.se.com/sk/sk/product/LC1G1154LSEA","\"Stykač TeSys G 115A 4P AC3 cívka 200-500V AC/DC pokročilý\"",0.73]
["LC1F800FW","STÝKAČ 800A",1,"ks",{"v":5902.233749999999,"d":"5902.234"},"3389110790597",{"v":33,"d":"33.00"},{"v":44,"d":"44.00"},{"v":33,"d":"33.00"},{"v":18750,"d":"18,750.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F800FW","TeSys F contactor - 3P (3 NO) - AC-3 - <lt/>= 440 V 800 A - coil 110...125 V DC",2.2800000000000002]
["LC1F500P7","STÝKAČ 500A 230V 50HZ",1,"ks",{"v":2013.1649999999997,"d":"2013.165"},"3389110788419",{"v":33,"d":"33.00"},{"v":26.5,"d":"26.50"},{"v":28.5,"d":"28.50"},{"v":11560,"d":"11,560.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F500P7","stýkač 3P (3Z) 500A AC-3 440V - cievka 230V 50Hz",1.4000000000000001]
["LC1F500","STÝKAČ 500A BEZ CIEVKY",1,"ks",{"v":1738.6424999999997,"d":"1738.643"},"3389110122169",{"v":30,"d":"30.00"},{"v":27.5,"d":"27.50"},{"v":30,"d":"30.00"},{"v":10398,"d":"10,398.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F500","stýkač 3P (3Z) 500A AC-3 440V - bez cievky",1.27]
["LC1F330Q7","STÝKAČ 330A",1,"ks",{"v":1464.12,"d":"1464.120"},"3389110460278",{"v":29.3,"d":"29.30"},{"v":25.5,"d":"25.50"},{"v":23.8,"d":"23.80"},{"v":8600,"d":"8,600.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F330Q7","TeSys F contactor - 3P (3 NO) - AC-3 - <lt/>= 440 V 330 A - coil 380 V AC",1.12]
["LC1F3304","STÝKAČ 330A 4-PÓL BEZ CIEVKY",1,"ks",{"v":1555.6274999999998,"d":"1555.628"},"3389110231144",{"v":31.5,"d":"31.50"},{"v":25,"d":"25.00"},{"v":24,"d":"24.00"},{"v":10059,"d":"10,059.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F3304","nevybavený stýkač LC1-F – F – 4 – 400 A – AC-1 – 440 V – bez cievky",1.22]
["LC1F2654M7","STÝKAČ 265A 4-PÓL",1,"ks",{"v":1601.3812499999997,"d":"1601.381"},"3389110432329",{"v":30,"d":"30.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":8540,"d":"8,540.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F2654M7","TeSys F contactor - 4P (4 NO) - AC-1 - <lt/>= 440 V 350 A - coil 220 V AC",0]
["LC1F225BD","STÝKAČ 225A",1,"ks",{"v":883.0473749999999,"d":"883.047"},"3389110788143",{"v":26,"d":"26.00"},{"v":21.5,"d":"21.50"},{"v":24,"d":"24.00"},{"v":4750,"d":"4,750.00"},"CZ","8536419089","https://www.se.com/sk/sk/product/LC1F225BD","TeSys F stýkač - 3P (3 Z) - AC-3 - <lt/>= 440 V 225 A - cievka 24 V DC",0.65]
["LC1F1854","STÝKAČ 185A 4-PÓL BEZ CIEVKY",1,"ks",{"v":773.238375,"d":"773.238"},"3389110122435",{"v":23.5,"d":"23.50"},{"v":21.6,"d":"21.60"},{"v":22,"d":"22.00"},{"v":5153,"d":"5,153.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F1854","nevybavený stýkač LC1-F – F – 4 – 275 A – AC-1 – 440 V – bez cievky",0.62]
["LC1F150F7","STÝKAČ 150A 110V 50HZ",1,"ks",{"v":567.3465,"d":"567.347"},"3389110350951",{"v":25,"d":"25.00"},{"v":21,"d":"21.00"},{"v":20,"d":"20.00"},{"v":3430,"d":"3,430.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F150F7","TeSys F stýkač - 3P (3Z) - AC-3 - <lt/>= 440 V 250 A - cievka 110 V AC",0.48]
["LC1F1154","STÝKAČ 115A 4-PÓL BEZ CIEVKY",1,"ks",{"v":576.4972499999999,"d":"576.497"},"3389110122237",{"v":26.5,"d":"26.50"},{"v":21.5,"d":"21.50"},{"v":20,"d":"20.00"},{"v":4208,"d":"4,208.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1F1154","nevybavený stýkač LC1-F – F – 4 – 200 A – AC-1 – 440 V – bez cievky",0.5]
["LC1E65F5","3P stykač TeSys E 30KW 400V AC 110V AC",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3606480339158",{"v":13.3,"d":"13.30"},{"v":8.5,"d":"8.50"},{"v":12.5,"d":"12.50"},{"v":979,"d":"979.00"},"CN","8536490099","https://www.se.com/sk/sk/product/LC1E65F5","Stýkač EasyPact TVS, 3P, AC-3, 65A, 110V AC cievka, 50Hz, 1Z+1V",0.12]
["LC1E50U5","3P stykač TeSys E 22KW 400V AC 240V AC",1,"ks",{"v":118.95975,"d":"118.960"},"3606480362040",{"v":13.2,"d":"13.20"},{"v":12.3,"d":"12.30"},{"v":8.6,"d":"8.60"},{"v":980,"d":"980.00"},"CN","8536490099","https://www.se.com/sk/sk/product/LC1E50U5","Stýkač EasyPact TVS, 3P, AC-3, 50A, 240V AC cievka, 50Hz, 1Z+1V",0.12]
["LC1E3810N5","3P stykač TeSys E 1Z 18,5KW 400V AC",1,"ks",{"v":88.762275,"d":"88.762"},"3606480361906",{"v":5.6,"d":"5.60"},{"v":8.6,"d":"8.60"},{"v":8.4,"d":"8.40"},{"v":449,"d":"449.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1E3810N5","Stýkač EasyPact TVS, 3P, AC-3, 38A, 415V AC cievka, 50Hz, 1Z",0.05]
["LC1E3201N5","3P stykač TeSys E 1V 15KW 415V AC",1,"ks",{"v":71.8333875,"d":"71.833"},"3606480361661",{"v":5.6,"d":"5.60"},{"v":8.6,"d":"8.60"},{"v":8.4,"d":"8.40"},{"v":449,"d":"449.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1E3201N5","Stýkač EasyPact TVS, 3P, AC-3, 32A, 415V AC cievka, 50Hz, 1V",0.05]
["LC1E300Q5","3P stykač TeSys E 160KW 380V",1,"ks",{"v":1326.8587499999999,"d":"1326.859"},"3606480324017",{"v":32.5,"d":"32.50"},{"v":26,"d":"26.00"},{"v":25,"d":"25.00"},{"v":5600,"d":"5,600.00"},"CN","8536490099","https://www.se.com/sk/sk/product/LC1E300Q5","Stýkač EasyPact TVS, 3P, AC-3, 300A, 380V AC cievka, 50Hz",0.67]
["LC1E250B5","3P stykač TeSys E 132KW 24V AC",1,"ks",{"v":791.5398749999999,"d":"791.540"},"3606480323881",{"v":26,"d":"26.00"},{"v":21.5,"d":"21.50"},{"v":24,"d":"24.00"},{"v":5400,"d":"5,400.00"},"CN","8536490099","https://www.se.com/sk/sk/product/LC1E250B5","Stýkač EasyPact TVS, 3P, AC-3, 250A, 24V AC cievka, 50Hz",0.65]
["LC1E2501Q5","3P stykač TeSys E 1V 11KW 380V AC",1,"ks",{"v":49.414049999999996,"d":"49.414"},"3606480328435",4.82,8.68,{"v":7.4,"d":"7.40"},{"v":359,"d":"359.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1E2501Q5","Stýkač EasyPact TVS, 3P, AC-3, 25A, 380V AC cievka, 50Hz, 1V",0.04]
["LC1E1810B5","3P stykač TeSys E 1Z 7,5KW 400V AC",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3606480328251",4.82,8.31,{"v":7.4,"d":"7.40"},{"v":349,"d":"349.00"},"IN","8536419089","https://www.se.com/sk/sk/product/LC1E1810B5","Stýkač EasyPact TVS, 3P, AC-3, 18A, 24V AC cievka, 50Hz, 1Z",0.04]
["LC1E1210Q5","3P stykač TeSys E 1Z 5,5KW 400V AC",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3606480328046",{"v":7.6,"d":"7.60"},{"v":8.8,"d":"8.80"},{"v":5,"d":"5.00"},{"v":344,"d":"344.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1E1210Q5","Stýkač EasyPact TVS, 3P, AC-3, 12A, 380V AC cievka, 50Hz, 1Z",0.04]
["LC1E120U5","3P stykač TeSys E 55KW 400V AC 240V",1,"ks",{"v":315.700875,"d":"315.701"},"3606480323683",{"v":21,"d":"21.00"},{"v":19,"d":"19.00"},{"v":17.5,"d":"17.50"},{"v":2300,"d":"2,300.00"},"CN","8536490099","https://www.se.com/sk/sk/product/LC1E120U5","Stýkač EasyPact TVS, 3P, AC-3, 120A, 240V AC cievka, 50Hz, 1Z+1V",0.28]
["LC1E0901Q5","3P stykač TeSys E 1V 4KW 380V AC",1,"ks",{"v":23.791949999999996,"d":"23.792"},"3606480327650",{"v":8.5,"d":"8.50"},{"v":5,"d":"5.00"},{"v":7.5,"d":"7.50"},{"v":348,"d":"348.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1E0901Q5","Stýkač EasyPact TVS, 3P, AC-3, 9A, 380V AC cievka, 50Hz, 1V",0.04]
["LC1E0610M5","3P stykač TeSys E 1Z 2,2KW 220V AC",1,"ks",{"v":21.5042625,"d":"21.504"},"3606480327506",4.82,8.31,{"v":7.4,"d":"7.40"},{"v":340,"d":"340.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1E0610M5","Stýkač EasyPact TVS, 3P, AC-3, 6A, 220V AC cievka, 50Hz, 1Z",0.04]
["LC1DT80AFD","STÝKAČ EVERLINK 80A 4P AC1 110V DC",1,"ks",{"v":466.68825,"d":"466.688"},"3389118330276",{"v":15,"d":"15.00"},{"v":7.5,"d":"7.50"},{"v":14,"d":"14.00"},{"v":1100,"d":"1,100.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1DT80AFD","stýka? 4P(4Z) 80A AC-1 440V - cievka 110V DC",0.13]
["LC1DT80A6MD","STÝKAČ EVERLINK 80A 4P AC1 220V DC, KAB.",1,"ks",{"v":526.1681249999999,"d":"526.168"},"3389118331136",{"v":15,"d":"15.00"},{"v":7.5,"d":"7.50"},{"v":14,"d":"14.00"},{"v":1100,"d":"1,100.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1DT80A6MD","TeSys D stýkač - 4P - AC-1 - <lt/>= 440V AC - 80A - cievka 220 VDC",0.13]
["LC1DT60AB7","STÝKAČ EVERLINK 60A 4P AC1 24V AC",1,"ks",{"v":215.042625,"d":"215.043"},"3389119409247",{"v":15,"d":"15.00"},{"v":7.8,"d":"7.80"},{"v":13.7,"d":"13.70"},{"v":1084,"d":"1,084.00"},"IN","8536419089","https://www.se.com/sk/sk/product/LC1DT60AB7","stýka? 4P(4Z) 60A AC-1 440V - cievka 24V 50Hz",0.13]
["LC1DT40D7","STÝKAČ 40A 4P AC1 42V AC",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110673722",9.95,9.08,{"v":4.5,"d":"4.50"},{"v":425,"d":"425.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1DT40D7","Contactor, TeSys Deca, 4P(4 NO), AC-1, <lt/>= 440V, 40A, 42V AC 50/60Hz coil, screw terminal",0]
["LC1DT32P7","STÝKAČ 32A 4P AC1 230V AC",1,"ks",{"v":58.56479999999999,"d":"58.565"},"3389110244625",{"v":12,"d":"12.00"},{"v":5.5,"d":"5.50"},{"v":9.5,"d":"9.50"},{"v":464,"d":"464.00"},"ID","8536490099","https://www.se.com/sk/sk/product/LC1DT32P7","stýka? 4P(4Z) 32A AC-1 440V-pomocné kontakty 1Z+1V- cievka 230V 50Hz",0.06]
["LC1DT25ED","STÝKAČ 25A 4P AC1 48V DC",1,"ks",{"v":86.01705,"d":"86.017"},"3389110247800",{"v":11.8,"d":"11.80"},{"v":5.5,"d":"5.50"},{"v":9.5,"d":"9.50"},{"v":558,"d":"558.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1DT25ED","stýka? 4P(4Z) 25A AC-1 440V-pomocné kontakty 1Z+1V- cievka 48V DC",0.07]
["LC1DT253BD","STÝKAČ 25A 4P AC1 24V DC PR. SVORKY",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389118007178",{"v":11.3,"d":"11.30"},{"v":5,"d":"5.00"},{"v":9.3,"d":"9.30"},{"v":545,"d":"545.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1DT253BD","Contactor, TeSys Deca, 4P(4 NO), AC-1, 0 to 440V, 25A, 24VDC standard coil, spring",0]
["LC1DT203B7","STÝKAČ 20A 4P AC1 24V AC PR. SVORKY",1,"ks",{"v":59.93741249999999,"d":"59.937"},"3389118008243",{"v":11.3,"d":"11.30"},{"v":5,"d":"5.00"},{"v":9.3,"d":"9.30"},{"v":380,"d":"380.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1DT203B7","TeSys D stýkač - 4P(4Z) - AC-1 - <lt/>= 440 V 20 A - 24 V AC cievka",0.05]
["LC1DMKB7","Kompenzačný stýkač 25kVAr 24V 50/60Hz",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3606480401565",{"v":23,"d":"23.00"},{"v":7,"d":"7.00"},{"v":20,"d":"20.00"},{"v":615,"d":"615.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1DMKB7","stýkač pre spínanie kondenzátorov 3P 25 kVAR 415V - cievka 24V 50Hz",0.07]
["LC1D95P5","Stýkač 95A 30-11 230V 50Hz",1,"ks",{"v":301.97475,"d":"301.975"},"3389110451726",{"v":14,"d":"14.00"},{"v":9.5,"d":"9.50"},{"v":13.5,"d":"13.50"},{"v":1569,"d":"1,569.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D95P5","stýkač 3P(3Z) 95A AC-3 440V - cievka 230V 50Hz",0.19]
["LC1D80U5","STÝKAČ 80A 1NO+1NC 240V AC",1,"ks",{"v":242.494875,"d":"242.495"},"3389110443073",{"v":13.5,"d":"13.50"},{"v":14,"d":"14.00"},{"v":9.5,"d":"9.50"},{"v":1554,"d":"1,554.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1D80U5","Contactor, TeSys Deca, 3P(3NO), AC-3/AC-3e, <lt/>=440V, 80A, 240V AC 50Hz coil, screw clamp terminals",0]
["LC1D80FE7","STÝKAČ 80A 1NO+1NC 115V AC",1,"ks",{"v":274.5225,"d":"274.523"},"3389110440591",{"v":14,"d":"14.00"},{"v":9.5,"d":"9.50"},{"v":13.5,"d":"13.50"},{"v":1559,"d":"1,559.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1D80FE7","stýkač 3P(3Z) 80A AC-3 440V-pomocné kontakty 1Z+1V- cievka 115V 50Hz",0.19]
["LC1D80AV7","Stykač 80A AC-3 3P 400V AC",1,"ks",{"v":253.47577499999997,"d":"253.476"},"3606481312235",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":13.5,"d":"13.50"},{"v":943,"d":"943.00"},"ID","8536490099","https://www.se.com/sk/sk/product/LC1D80AV7","stýkač 3P 80A AC-3 440V - cievka 400V 50/60Hz",""]
["LC1D806G7","STÝKAČ 80A 1NO+1NC 120V AC, KÁB. OKÁ",1,"ks",{"v":265.37174999999996,"d":"265.372"},"3389110298246",{"v":16.3,"d":"16.30"},{"v":11,"d":"11.00"},{"v":16,"d":"16.00"},{"v":1590,"d":"1,590.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1D806G7","Contactor, TeSys Deca, 3P(3NO), AC-3/AC-3e, <lt/>=440V 80A, 120V AC 50/60Hz coil, lugs-ring terminals",0.19]
["LC1D80004M7","STÝKAČ 4P 80A 220V AC",1,"ks",{"v":466.68825,"d":"466.688"},"3389110231854",{"v":15.5,"d":"15.50"},{"v":11,"d":"11.00"},{"v":13.5,"d":"13.50"},{"v":1701,"d":"1,701.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1D80004M7","stýka? 4P(4Z) 125A AC-1 440V - cievka 220V 50Hz",0.2]
["LC1D65AV7","STÝKAČ EVERLINK 65A 1NO+1NC 400V AC",1,"ks",{"v":205.891875,"d":"205.892"},"3389119409056",{"v":15.5,"d":"15.50"},{"v":6.4,"d":"6.40"},{"v":13.9,"d":"13.90"},{"v":906,"d":"906.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1D65AV7","stýkač 3P(3Z) 65A AC-3 440V - cievka 400V 50Hz",0.11]
["LC1D65AEHE","TeSys D Green 3P 65A 48 - 130V AC/DC",1,"ks",{"v":237.00442499999997,"d":"237.004"},"3606480988271",{"v":15.2,"d":"15.20"},{"v":6.2,"d":"6.20"},{"v":13.5,"d":"13.50"},{"v":1057,"d":"1,057.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D65AEHE","stýkač 3P 65A AC-3 440V - cievka 48...130V 50Hz/DC",""]
["LC1D65AB5","3P Stýkač AC3 440V 65A 24V 50Hz",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3606489602529",{"v":15.5,"d":"15.50"},{"v":6.5,"d":"6.50"},{"v":14,"d":"14.00"},{"v":929,"d":"929.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D65AB5","stýkač 3P 65A AC-3 440V-pomocné kontakty 1Z+1V - cievka 24V 50Hz",0.11]
["LC1D65A3BD","STÝKAČ EVERLINK 65A 1NO+1NC 24V DC, PR.",1,"ks",{"v":283.67325,"d":"283.673"},"3389119409193",{"v":15.2,"d":"15.20"},{"v":6.2,"d":"6.20"},{"v":13.7,"d":"13.70"},{"v":992,"d":"992.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D65A3BD","stýkač 3P(3Z) 65A AC-3 440V - cievka 24V DC",0.12]
["LC1D50AM7","STÝKAČ EVERLINK 50A 1NO+1NC 220V AC",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389119408691",{"v":15.2,"d":"15.20"},{"v":6.2,"d":"6.20"},{"v":13.5,"d":"13.50"},{"v":916,"d":"916.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1D50AM7","stýkač 3P(3Z) 50A AC-3 440V - cievka 220V 50Hz",0.11]
["LC1D50ABD","STÝKAČ EVERLINK 50A 1NO+1NC 24V DC",1,"ks",183.015,"3389119408783",{"v":15.2,"d":"15.20"},{"v":6.2,"d":"6.20"},{"v":13.7,"d":"13.70"},{"v":999,"d":"999.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D50ABD","stýkač 3P(3Z) 50A AC-3 440V - cievka 24V DC",0.12]
["LC1D50A3P7","STÝKAČ EVERLINK 50A 1NO+1NC 230V AC, PR.",1,"ks",{"v":141.836625,"d":"141.837"},"3389119408899",{"v":15.2,"d":"15.20"},{"v":6.2,"d":"6.20"},{"v":13.8,"d":"13.80"},{"v":921,"d":"921.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D50A3P7","stýkač 3P(3Z) 50A AC-3 440V - cievka 230V 50Hz",0.11]
["LC1D40AQ7","STÝKAČ EVERLINK 40A 1NO+1NC 380V AC",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3389119408424",{"v":15.2,"d":"15.20"},{"v":6.2,"d":"6.20"},{"v":13.7,"d":"13.70"},{"v":910,"d":"910.00"},"IN","8536490099","https://www.se.com/sk/sk/product/LC1D40AQ7","stýkač 3P(3Z) 40A AC-3 440V - cievka 380V 50Hz",0.11]
["LC1D40AJD","STÝKAČ EVERLINK 40A 1NO+1NC 12V DC",1,"ks",183.015,"3389118326675",{"v":15,"d":"15.00"},{"v":6,"d":"6.00"},{"v":14,"d":"14.00"},{"v":850,"d":"850.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D40AJD","stýkač 3P(3Z) 40A AC-3 440V - cievka 12V DC",0.1]
["LC1D40ABD","STÝKAČ EVERLINK 40A 1NO+1NC 24V DC",1,"ks",{"v":150.987375,"d":"150.987"},"3389119408486",{"v":15.2,"d":"15.20"},{"v":6.2,"d":"6.20"},{"v":13.7,"d":"13.70"},{"v":982,"d":"982.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D40ABD","stýkač 3P(3Z) 40A AC-3 440V - cievka 24V DC",0.12]
["LC1D40A3F7","STÝKAČ EVERLINK 40A 1NO+1NC 110V AC, PR.",1,"ks",{"v":137.26125,"d":"137.261"},"3389119408578",{"v":15.2,"d":"15.20"},{"v":6.2,"d":"6.20"},{"v":13.7,"d":"13.70"},{"v":944,"d":"944.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D40A3F7","stýkač 3P(3Z) 40A AC-3 440V - cievka 110V 50Hz",0.11]
["LC1D40004M7","STÝKAČ 4P 40A 220V AC",1,"ks",{"v":283.67325,"d":"283.673"},"3389110231564",{"v":15,"d":"15.00"},{"v":11,"d":"11.00"},{"v":13.2,"d":"13.20"},{"v":1470,"d":"1,470.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1D40004M7","TeSys Deca contactor,4P(4NO),AC-1 440V 60A,coil 220V AC",0.18]
["LC1D38EL","STÝKAČ 38A 1NO+1NC 48V LC",1,"ks",{"v":146.41199999999998,"d":"146.412"},"3389110361902",{"v":11.2,"d":"11.20"},{"v":5,"d":"5.00"},{"v":9.2,"d":"9.20"},{"v":587,"d":"587.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D38EL","stýkač 3P(3Z) 38A AC-3 440V-pomocné kontakty 1Z+1V- cievka 48V DC",0.07]
["LC1D32P7","STÝKAČ 32A 1NO+1NC 230V AC",1,"ks",{"v":83.7293625,"d":"83.729"},"3389110351125",{"v":11.2,"d":"11.20"},{"v":5,"d":"5.00"},{"v":9.2,"d":"9.20"},{"v":416,"d":"416.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D32P7","stýkač 3P(3Z) 32A AC-3 440V-pomocné kontakty 1Z+1V- cievka 230V 50Hz",0.05]
["LC1D32ED","STÝKAČ 32A 1NO+1NC 48V DC",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110357363",{"v":8.9,"d":"8.90"},{"v":4.9,"d":"4.90"},{"v":11.1,"d":"11.10"},{"v":583,"d":"583.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D32ED","stýkač 3P(3Z) 32A AC-3 440V-pomocné kontakty 1Z+1V- cievka 48V DC",0.07]
["LC1D32B5","Stýkač 32A 30-11 24V 50Hz",1,"ks",{"v":75.4936875,"d":"75.494"},"3606489602482",{"v":11,"d":"11.00"},{"v":5,"d":"5.00"},{"v":9.5,"d":"9.50"},{"v":415,"d":"415.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D32B5","stýkač 3P 32A AC-3 440V-pomocné kontakty 1Z + +1V- cievka 24V 50Hz",0.05]
["LC1D25U7","STÝKAČ 25A 1NO+1NC V AC",1,"ks",{"v":74.57861249999999,"d":"74.579"},"3389110350081",{"v":11.2,"d":"11.20"},{"v":5,"d":"5.00"},{"v":9.2,"d":"9.20"},{"v":414,"d":"414.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D25U7","stýkač 3P(3Z) 25A AC-3 440V-pomocné kontakty 1Z+1V- cievka 240V 50Hz",0.05]
["LC1D25N7","STÝKAČ 25A 1NO+1NC 415V AC",1,"ks",{"v":75.03614999999999,"d":"75.036"},"3389110349931",{"v":11.2,"d":"11.20"},{"v":5,"d":"5.00"},{"v":9.2,"d":"9.20"},{"v":414,"d":"414.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D25N7","TeSys D stýkač - 3P ( 3 NO ) - AC - 3 - <lt/> = 440 V 25 A - 415 V AC cievka",0.05]
["LC1D25D7","STÝKAČ 25A 1NO+1NC 42V AC",1,"ks",{"v":76.8663,"d":"76.866"},"3389110349672",{"v":11,"d":"11.00"},{"v":5,"d":"5.00"},{"v":9,"d":"9.00"},{"v":413,"d":"413.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D25D7","stýkač 3P(3Z) 25A AC-3 440V-pomocné kontakty 1Z+1V- cievka 42V 50Hz",0.05]
["LC1D25B5","Stýkač 25A 30-11 24V 50Hz",1,"ks",{"v":54.4469625,"d":"54.447"},"3606489602475",{"v":11.5,"d":"11.50"},{"v":5,"d":"5.00"},{"v":9.5,"d":"9.50"},{"v":418,"d":"418.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D25B5","stýkač 3P 25A AC-3 440V-pomocné kontakty 1Z + +1V- cievka 24V 50Hz",0.05]
["LC1D256B7","Stykač 25A 24V AC oka",1,"ks",{"v":68.20969050000001,"d":"68.210"},"3389110804454",11.68,5.59,{"v":9.4,"d":"9.40"},{"v":440,"d":"440.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D256B7","TeSys D stýkač - 3P ( 3 NO ) - AC - 3 - <lt/> = 440 V 25 - 24 V AC cievka",""]
["LC1D18MD","STÝKAČ18A 1NO+1NC 220V DC",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3389110355086",{"v":11.2,"d":"11.20"},{"v":5.1,"d":"5.10"},{"v":9.2,"d":"9.20"},{"v":500,"d":"500.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D18MD","stýkač 3P(3Z) 18A AC-3 440V-pomocné kontakty 1Z+1V- cievka 220V DC",0.06]
["LC1D18FE7","STÝKAČ 18A 1NO+1NC 115V AC",1,"ks",{"v":54.9045,"d":"54.905"},"3389110349443",{"v":9.5,"d":"9.50"},{"v":5.5,"d":"5.50"},{"v":8.1,"d":"8.10"},{"v":357,"d":"357.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D18FE7","stýkač 3P(3Z) 18A AC-3 440V-pomocné kontakty 1Z+1V- cievka 115V 50Hz",0.04]
["LC1D18B5","Stýkač 18A 30-11 24V 50Hz",1,"ks",{"v":39.80576249999999,"d":"39.806"},"3606489602468",{"v":11.5,"d":"11.50"},{"v":5,"d":"5.00"},{"v":9.5,"d":"9.50"},{"v":357.5,"d":"357.50"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D18B5","stýkač 3P 18A AC-3 440V-pomocné kontakty 1Z + 1V- cievka 24V 50Hz",0.04]
["LC1D188B7","STÝKAČ 18A 4P 24V AC",1,"ks",{"v":67.25801249999999,"d":"67.258"},"3389110334173",{"v":12,"d":"12.00"},{"v":5.5,"d":"5.50"},{"v":9.5,"d":"9.50"},{"v":465,"d":"465.00"},"ID","8536419089","https://www.se.com/sk/sk/product/LC1D188B7","stýka?-4P(2Z+ 2V) 32A AC-1 440V-pomocné kontakty 1Z+1V- cievka 24V 50Hz",0.06]
["LC1D183B7","STÝKAČ 18A 1NO+1NC 24V AC PR. SVORKY",1,"ks",{"v":50.329125,"d":"50.329"},"3389110803617",{"v":12.4,"d":"12.40"},{"v":5.6,"d":"5.60"},{"v":11,"d":"11.00"},{"v":438,"d":"438.00"},"ID","8536419089","https://www.se.com/sk/sk/product/LC1D183B7","stýkač 3P(3Z) 18A AC-3 440V-pomocné kontakty 1Z+1V- cievka 24V 50Hz",0.05]
["LC1D150FD","STÝKAČ 150A 1NO+1NC 110V DC",1,"ks",{"v":535.3188749999999,"d":"535.319"},"3389110476019",{"v":18.5,"d":"18.50"},{"v":16.8,"d":"16.80"},{"v":20.8,"d":"20.80"},{"v":2420,"d":"2,420.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1D150FD","stýkač 3P(3Z) 150A AC-3 440V-pomocné kontakty 1Z+1V- cievka 110V DC",0.29]
["LC1D12P7","STÝKAČ 12A 1NO+1NC 230V AC",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110349306",{"v":11.2,"d":"11.20"},{"v":5,"d":"5.00"},{"v":9.2,"d":"9.20"},{"v":353,"d":"353.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D12P7","stýkač 3P(3Z) 12A AC-3 440V-pomocné kontakty 1Z+1V- cievka 230V 50Hz",0.04]
["LC1D12F7","STÝKAČ 12A 1NO+1NC 110V AC",1,"ks",{"v":36.145462499999994,"d":"36.145"},"3389110349221",{"v":11.4,"d":"11.40"},{"v":5.3,"d":"5.30"},{"v":9.4,"d":"9.40"},{"v":353,"d":"353.00"},"ID","8536490099","https://www.se.com/sk/sk/product/LC1D12F7","stýkač 3P(3Z) 12A AC-3 440V-pomocné kontakty 1Z+1V- cievka 110V 50Hz",0.04]
["LC1D12B5","Stýkač 12A 30-11 24V 50Hz",1,"ks",{"v":30.197474999999997,"d":"30.197"},"3606489602451",{"v":11.5,"d":"11.50"},{"v":5,"d":"5.00"},{"v":9.5,"d":"9.50"},{"v":359.2,"d":"359.20"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D12B5","stýkač 3P 12A AC-3 440V-pomocné kontakty 1Z + +1V- cievka 24V 50Hz",0.04]
["LC1D123P7","STÝKAČ 12A 1NO+1NC 230V AC PR. SVORKY",1,"ks",{"v":37.518074999999996,"d":"37.518"},"3389110803013",{"v":12.2,"d":"12.20"},{"v":5.2,"d":"5.20"},{"v":10.8,"d":"10.80"},{"v":383,"d":"383.00"},"ID","8536490099","https://www.se.com/sk/sk/product/LC1D123P7","stýkač 3P(3Z) 12A AC-3 440V-pomocné kontakty 1Z+1V- cievka 230V 50Hz",0.05]
["LC1D115FD","STÝKAČ 115A 1NO+1NC 110V DC",1,"ks",{"v":443.81137499999994,"d":"443.811"},"3389110377033",{"v":20.5,"d":"20.50"},{"v":17,"d":"17.00"},{"v":19,"d":"19.00"},{"v":2497,"d":"2,497.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1D115FD","stýkač 3P(3Z) 115A AC-3 440V-pomocné kontakty 1Z+1V- cievka 110V DC",0.3]
["LC1D115B7","STÝKAČ 115A 1NO+1NC 24V AC",1,"ks",{"v":356.87924999999996,"d":"356.879"},"3389110376609",{"v":21,"d":"21.00"},{"v":19,"d":"19.00"},{"v":18,"d":"18.00"},{"v":2480,"d":"2,480.00"},"CZ","8536419089","https://www.se.com/sk/sk/product/LC1D115B7","stýkač 3P(3Z) 115A AC-3 440V-pomocné kontakty 1Z+1V- cievka 24V 50Hz",0.29]
["LC1D115004Q5","Stýkac TeSys 4P AC1 440V 200A 380V AC",1,"ks",{"v":791.5398749999999,"d":"791.540"},"3389110857306",{"v":18.5,"d":"18.50"},{"v":16.8,"d":"16.80"},{"v":21.2,"d":"21.20"},{"v":2750,"d":"2,750.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/LC1D115004Q5","contactor, TeSys Deca, 4P(4NO), AC-1, <lt/>=440V, 200A, 380V AC 50Hz coil",0.33]
["LC1D09MD","STÝKAČ 9A 1NO+1NC 220V DC",1,"ks",{"v":72.29092499999999,"d":"72.291"},"3389110353280",{"v":11.4,"d":"11.40"},{"v":5.2,"d":"5.20"},{"v":9.4,"d":"9.40"},{"v":494,"d":"494.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D09MD","stýkač 3P(3Z) 9A AC-3 440V-pomocné kontakty 1Z+1V- cievka 220V DC",0.06]
["LC1D09BD","STÝKAČ 9A 1NO+1NC 24V DC",1,"ks",{"v":60.394949999999994,"d":"60.395"},"3389110353075",{"v":11.1,"d":"11.10"},{"v":5,"d":"5.00"},{"v":9.2,"d":"9.20"},{"v":522,"d":"522.00"},"FR","8536419089","https://www.se.com/sk/sk/product/LC1D09BD","stýkač 3P(3Z) 9A AC-3 440V-pomocné kontakty 1Z+1V- cievka 24V DC",0.06]
["LC1D098MD","STÝKAČ 9A 4P 220V DC",1,"ks",{"v":88.30473749999999,"d":"88.305"},"3389110403381",{"v":11.8,"d":"11.80"},{"v":5.4,"d":"5.40"},{"v":9.5,"d":"9.50"},{"v":525,"d":"525.00"},"FR","8536490099","https://www.se.com/sk/sk/product/LC1D098MD","stýka? 4P(2Z+ 2V) 20A AC-1 440V-pomocné kontakty 1Z+1V- cievka 220V DC",0.07]
["LC1D093MD","STÝKAČ 9A 1NO+1NC 220V DC PR. SVORKY",1,"ks",{"v":81.89921249999999,"d":"81.899"},"3389110805857",{"v":12.2,"d":"12.20"},{"v":5.5,"d":"5.50"},{"v":11,"d":"11.00"},{"v":542,"d":"542.00"},"ID","8536490099","https://www.se.com/sk/sk/product/LC1D093MD","stýkač 3P(3Z) 9A AC-3 440V-pomocné kontakty 1Z+1V- cievka 220V DC",0.07]
["LAETSD","TEMPORISATION ETOILE TRIANGLE TeSys E",1,"ks",{"v":69.0881625,"d":"69.088"},"3606480311680",{"v":4.8,"d":"4.80"},{"v":6.5,"d":"6.50"},{"v":5.2,"d":"5.20"},{"v":60,"d":"60.00"},"FR","8536909500","https://www.se.com/sk/sk/product/LAETSD","Blokovanie časového oneskorenia, EasyPact TVS, oneskorenie zapnutia, 1 NO + 1 NC",0]
["LAEN22","Pomocné kontakty TeSys E 2V 2Z",1,"ks",{"v":10.5233625,"d":"10.523"},"3606480325281",{"v":7.2,"d":"7.20"},{"v":4.3,"d":"4.30"},{"v":6.9,"d":"6.90"},{"v":61,"d":"61.00"},"CN","8536508090","https://www.se.com/sk/sk/product/LAEN22","Blok pomocných kontaktov, EasyPact TVS, 2NO+2NC",0]
["LADT2","POM. KONTAKTY ONESK. 0,1-30S",1,"ks",{"v":66.34293749999999,"d":"66.343"},"3389110385892",{"v":5,"d":"5.00"},{"v":5.2,"d":"5.20"},{"v":6.5,"d":"6.50"},{"v":74,"d":"74.00"},"FR","8536508090","https://www.se.com/sk/sk/product/LADT2","blok pomocných kontaktov 1Z + 1V - skrutkové svorky",0]
["LADR03","POM. KONTAK. ONESK. 0,1-3S, PR. SVOR.",1,"ks",{"v":70.0032375,"d":"70.003"},"3389110821642",{"v":4.7,"d":"4.70"},{"v":5.2,"d":"5.20"},{"v":6.5,"d":"6.50"},{"v":79,"d":"79.00"},"FR","8536508090","https://www.se.com/sk/sk/product/LADR03","Time delay auxiliary contact block, TeSys Deca, 1NO+1NC, off delay 0.3-3s, front, spring terminals",0]
["LADN22","POM. KONTAKTY ČELNÉ 2NO+2NC",1,"ks",{"v":14.183662499999999,"d":"14.184"},"3389110384031",{"v":4.4,"d":"4.40"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":62,"d":"62.00"},"FR","8536508090","https://www.se.com/sk/sk/product/LADN22","blok pomocných kontaktov 2Z + 2V - skrutkové svorky",0]
["LADN046","CONTACTS BLOCK",1,"ks",{"v":24.707024999999998,"d":"24.707"},"3389110820836",{"v":4,"d":"4.00"},{"v":5,"d":"5.00"},{"v":4.7,"d":"4.70"},{"v":57,"d":"57.00"},"FR","8536508090","https://www.se.com/sk/sk/product/LADN046","Auxiliary contact block, TeSys Deca, 4NC, front mounting, lugs-ring terminals",0]
["LAD9R3","REVERZAČNÁ SADA, D40A-D65A",1,"ks",{"v":53.98942499999999,"d":"53.989"},"3389119410052",{"v":6,"d":"6.00"},{"v":4,"d":"4.00"},{"v":12,"d":"12.00"},{"v":163,"d":"163.00"},"CZ","8536909500","https://www.se.com/sk/sk/product/LAD9R3","reverzačná spínacia súprava - D40A až D65A",0]
["LAD91810","Súprava stop start reset",1,"ks",{"v":1.9674112499999996,"d":"1.967"},"3389110087239",{"v":5,"d":"5.00"},{"v":1,"d":"1.00"},{"v":4,"d":"4.00"},{"v":3,"d":"3.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LAD91810","TeSys LE - adaptation kit for head of start and stop/reset pushbutton",0]
["LAD7X3","ADAPTÉR MONTÁŽE D40A-D65A ZA D40-D65",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389119410113",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":18,"d":"18.00"},{"v":147,"d":"147.00"},"FR","7326909890","https://www.se.com/sk/sk/product/LAD7X3","TeSys GV2, TeSys GV3 & -doska retrofitu pre upevnenie skrutkami",0]
["LAD6K10M","MECHANICKÉ BLOKOVANIE 220/240V AC/DC",1,"ks",{"v":53.98942499999999,"d":"53.989"},"3389110842395",{"v":6.5,"d":"6.50"},{"v":4.5,"d":"4.50"},{"v":5,"d":"5.00"},{"v":98,"d":"98.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LAD6K10M","blok mechanického blokovania - 220...240V DC/50...60Hz",0]
["LAD4V3G","ODR. ČLEN VARISTOR 50-127V, D40A-D65A",1,"ks",{"v":12.81105,"d":"12.811"},"3389119410212",{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":17,"d":"17.00"},"CZ","8536301090","https://www.se.com/sk/sk/product/LAD4V3G","odrušovací člen varistor- 50...127V 50Hz/DC",0]
["LAD4RC3G","ODR. ČLEN RC 50-127V, D40A-D65A",1,"ks",{"v":15.528822749999996,"d":"15.529"},"3389119410175",{"v":10,"d":"10.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":19,"d":"19.00"},"CZ","8536301090","https://www.se.com/sk/sk/product/LAD4RC3G","Protective cover,TeSys Deca,for LC1D09…D80A and DT20…DT80A",""]
["LAD4BB3","ADAPTÉR PRIP. CIEVKY D40-D65 > D40A-D65A",1,"ks",{"v":20.589187499999998,"d":"20.589"},"3389119410144",{"v":6.5,"d":"6.50"},{"v":3.5,"d":"3.50"},{"v":5.5,"d":"5.50"},{"v":27,"d":"27.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/LAD4BB3","adaptér cievky pre stýkače D40A až D65A",0]
["LA9ZX01515","ZAKLADŇA 240X700 UL",2,"ks",{"v":116.35312499999999,"d":"116.353"},"3606480100130",{"v":70,"d":"70.00"},{"v":0.5,"d":"0.50"},{"v":24,"d":"24.00"},{"v":374,"d":"374.00"},"DE","85472000","https://www.se.com/sk/sk/product/LA9ZX01515","BASE PLATE 240X700 UL FOR 60 INTERAXIS 3P BUSBAR",0]
["LA9GRFB1","Retrofit pre TeSys G 115-225",1,"ks",{"v":24.249487499999997,"d":"24.249"},"3606481015990",{"v":21,"d":"21.00"},{"v":6.5,"d":"6.50"},{"v":12.5,"d":"12.50"},{"v":683,"d":"683.00"},"CN","7326199000","https://www.se.com/sk/sk/product/LA9GRFB1","Retrofit pre TeSys G 115-225",0]
["LA9G4751","Hrebene pre prepínanie 4P TeSys G 265-50",1,"ks",{"v":224.193375,"d":"224.193"},"3606481915900",{"v":46,"d":"46.00"},{"v":14.5,"d":"14.50"},{"v":16,"d":"16.00"},{"v":2766,"d":"2,766.00"},"CN","8536909500","https://www.se.com/sk/sk/product/LA9G4751","Hrebene pre prepínanie 4P sada pre TeSys G 265-500",0]
["LA9G4601","Priame pripojenie pre 4P TeSys G 115-225",1,"ks",{"v":43.92359999999999,"d":"43.924"},"3606481915672",{"v":14,"d":"14.00"},{"v":2.5,"d":"2.50"},{"v":12.5,"d":"12.50"},{"v":215,"d":"215.00"},"CN","8536909500","https://www.se.com/sk/sk/product/LA9G4601","Priame rozšírenie pripojenia pre 4P TeSys G 115-225",0]
["LA9G3751","Hrebene pre prepínanie 3P TeSys G 265-50",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3606481916662",{"v":46.5,"d":"46.50"},{"v":14.5,"d":"14.50"},{"v":15.5,"d":"15.50"},{"v":1933,"d":"1,933.00"},"CN","8536909500","https://www.se.com/sk/sk/product/LA9G3751","Hrebene pre prepínanie 3P sada pre TeSys G 265-500",0]
["LA9G3672","Pravouhlé veľké rozšírenie 3P G 265-500",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3606481015945",{"v":11.4,"d":"11.40"},{"v":6,"d":"6.00"},{"v":3.3,"d":"3.30"},{"v":752,"d":"752.00"},"CN","8536909500","https://www.se.com/sk/sk/product/LA9G3672","Pravouhlé veľké rozšírenie svoriek pre 3P TeSys G 265-500",0]
["LA9G3611","Pripojenie 3P TeSys G 115-225 35/45 mm",1,"ks",{"v":29.282399999999996,"d":"29.282"},"3606481916433",{"v":14,"d":"14.00"},{"v":3,"d":"3.00"},{"v":12.5,"d":"12.50"},{"v":264,"d":"264.00"},"CN","7326909890","https://www.se.com/sk/sk/product/LA9G3611","Sada pripojenie pre 3P TeSys G 115-225 35 mm - 45 mm",0]
["LA9FH601","KONEKTOR",1,"ks",{"v":43.008525,"d":"43.009"},"3389110168112",{"v":9,"d":"9.00"},{"v":10.5,"d":"10.50"},{"v":3.5,"d":"3.50"},{"v":109,"d":"109.00"},"CZ","7407100000","https://www.se.com/sk/sk/product/LA9FH601","vedenie pre pripojenie hviezdy- pro LC1F225...400",0]
["LA9F980","ODRUŠOVACÍ ČLEN",1,"ks",{"v":41.178374999999996,"d":"41.178"},"3389110120233",{"v":9,"d":"9.00"},{"v":4.7,"d":"4.70"},{"v":7.5,"d":"7.50"},{"v":42.9,"d":"42.90"},"FR","8538909999","https://www.se.com/sk/sk/product/LA9F980","odrušovací člen RC obvod- 220V 50Hz",0]
["LA9D80978","MECHANICKÉ BLOKOVANIE",1,"ks",{"v":59.0223375,"d":"59.022"},"3389110160505",{"v":17.2,"d":"17.20"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":170,"d":"170.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LA9D80978","mechanické blokovanie k stýkačom bez elektrického prepojenia",0]
["LA9D11567","SADA PRIPOJ. OVL. NAPÄTIA STRANA STÝK.",10,"ks",{"v":5.581957499999999,"d":"5.582"},"3389119409742",{"v":15,"d":"15.00"},{"v":8,"d":"8.00"},{"v":22,"d":"22.00"},{"v":190,"d":"190.00"},"CZ","85389099","https://www.se.com/sk/sk/product/LA9D11567","Control circuit take-off for LC1D115...150",0]
["LA7D903","Príslušenstvo pre popis prístrojov",100,"ks",{"v":0.27452249999999995,"d":"0.275"},"3389110055184",{"v":8,"d":"8.00"},{"v":5,"d":"5.00"},{"v":2,"d":"2.00"},{"v":20.324,"d":"20.32"},"FR","3926909790","https://www.se.com/sk/sk/product/LA7D903","nacvakávací držiak štítku - 8x18 mm - sada 100",0]
["LA7D03B","DIAĽKOVÁ SPÚŠŤ/RESET",1,"ks",{"v":91.5075,"d":"91.508"},"3389110055108",{"v":4.8,"d":"4.80"},{"v":5,"d":"5.00"},{"v":4.8,"d":"4.80"},{"v":109,"d":"109.00"},"FR","8538909999","https://www.se.com/sk/sk/product/LA7D03B","Thermal overload relays, TeSys Deca, remote electrical tripping, 24V DC/AC",0]
["LA5FF431","NÁHRADNÉ KONTAKTY PRE F115, F150",1,"ks",{"v":260.79637499999995,"d":"260.796"},"3389110128307",{"v":6,"d":"6.00"},{"v":10.5,"d":"10.50"},{"v":9,"d":"9.00"},{"v":270,"d":"270.00"},"CZ","8536909500","https://www.se.com/sk/sk/product/LA5FF431","súprava kontaktov 3P- pre LC1-F115",0]
["LA5D150803","SADA NÁHRADNÝCH KONTAKTOV",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110880489",{"v":10.6,"d":"10.60"},{"v":9,"d":"9.00"},{"v":6.2,"d":"6.20"},{"v":222,"d":"222.00"},"CZ","8536909500","https://www.se.com/sk/sk/product/LA5D150803","sada kontaktov LA5 - D - 3P - pre LC1 - D150",0]
["LA4KC1B","ODRUŠOVACÍ ČLEN",5,"ks",{"v":8.876227499999999,"d":"8.876"},"3389110230185",{"v":4.2,"d":"4.20"},{"v":0.8,"d":"0.80"},{"v":2.8,"d":"2.80"},{"v":5,"d":"5.00"},"ID","8536309090","https://www.se.com/sk/sk/product/LA4KC1B","odrušovací člen dióda- 12...24V DC",0]
["LA4DE1U","ODRUŠOVACÍ ČLEN",1,"ks",{"v":27.45225,"d":"27.452"},"3389110233094",{"v":5.1,"d":"5.10"},{"v":2.8,"d":"2.80"},{"v":4.2,"d":"4.20"},{"v":15,"d":"15.00"},"TN","8536301090","https://www.se.com/sk/sk/product/LA4DE1U","odrušovací člen varistor- 110...250V 50Hz/DC",0]
["LA4DA1G","ODRUŠOVACÍ ČLEN",1,"ks",{"v":29.282399999999996,"d":"29.282"},"3389110233018",{"v":5.1,"d":"5.10"},{"v":2.8,"d":"2.80"},{"v":4.2,"d":"4.20"},{"v":16,"d":"16.00"},"FR","8536301090","https://www.se.com/sk/sk/product/LA4DA1G","TeSys Deca, suppressor module, RC circuit, 50...127V AC",0]
["LA1KN31","POMOCNÉ KONTAKTY",1,"ks",{"v":11.895974999999998,"d":"11.896"},"3389110500097",{"v":4,"d":"4.00"},{"v":3.8,"d":"3.80"},{"v":3.6,"d":"3.60"},{"v":41,"d":"41.00"},"ID","8536909500","https://www.se.com/sk/sk/product/LA1KN31","blok pomocných kontaktov 3Z + 1V- skrutkové svorky",0]
["KZ66","VARIO SADA TESNENÍ",1,"ks",{"v":2.69947125,"d":"2.699"},"3389110552294",{"v":15,"d":"15.00"},{"v":1,"d":"1.00"},{"v":11,"d":"11.00"},{"v":4,"d":"4.00"},"CZ","4016930090","https://www.se.com/sk/sk/product/KZ66","tesn. IP 65 pre 60 x 60 mm čel. dosku a vačk. sp. s pred. montážou – súpr. 5 ks",0]
["KZ17X","NOSIČ ŠTÍTKOV 45X45",10,"ks",{"v":2.1961799999999996,"d":"2.196"},"3389110980837",{"v":4.6,"d":"4.60"},{"v":0.1,"d":"0.10"},{"v":4.6,"d":"4.60"},{"v":2,"d":"2.00"},"CZ","39269097","https://www.se.com/sk/sk/product/KZ17X","neoznačený štítok - pro vačkový spínač - 46x46 mm",0]
["KSC250EV4203","STUP. VED.250 A/ 2 M/ 3 VYV. CU",1,"ks",{"v":1346.6249999999998,"d":"1346.625"},"3606480677465",{"v":212,"d":"212.00"},{"v":6.5,"d":"6.50"},{"v":17,"d":"17.00"},{"v":13280,"d":"13,280.00"},"FR","85369001","https://www.se.com/sk/sk/product/KSC250EV4203","Vertical distribution length, Canalis KSC250, copper, 250A, fixed length 2m, 3 outlets, 3L+N+PE/3L+PE, white RAL9001",0]
["KSB400ZV1","PODPERA VEDENIA 250A",1,"ks",{"v":785.5312499999999,"d":"785.531"},"3606480005640",{"v":44,"d":"44.00"},{"v":11.5,"d":"11.50"},{"v":27.4,"d":"27.40"},{"v":5000,"d":"5,000.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSB400ZV1","Canalis – spodná podpora pre podstavec – 400 A",0]
["KSB400DC5","VÝV. SKR.COM NS-NSV./400A/3P+PEN/IP55",1,"ks",{"v":1627.1718749999995,"d":"1627.172"},"3606480005800",{"v":73.5,"d":"73.50"},{"v":35,"d":"35.00"},{"v":44,"d":"44.00"},{"v":21000,"d":"21,000.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KSB400DC5","Canalis - vývodná skriňa - 400 A pre Compact NSX - 3L + PEN",2.52]
["KSB250SM428","VÝV. SKRINKA/250A/25MOD/3P+N+PE",1,"ks",{"v":1963.8281249999995,"d":"1963.828"},"3606485137421",{"v":65,"d":"65.00"},{"v":44,"d":"44.00"},{"v":33,"d":"33.00"},{"v":14000,"d":"14,000.00"},"FR","85369001","https://www.se.com/sk/sk/product/KSB250SM428","Tap off unit, Canalis KS, vertical installation, Acti9 (2x14 modules 18mm), 250A, 3L+N+PE, rotary handle, RAL9001",1.68]
["KSB160SM424","VÝV. SKRINKA/160A/24MOD/3P+N+PE",1,"ks",{"v":1346.6249999999998,"d":"1346.625"},"3606485208619",{"v":52.5,"d":"52.50"},{"v":33,"d":"33.00"},{"v":34,"d":"34.00"},{"v":9000,"d":"9,000.00"},"SE","8536900100","https://www.se.com/sk/sk/product/KSB160SM424","Tap off unit, Canalis KS, for ComPact NG125 circuit breaker with rotary handle, 160A, 3L+N+PE, 24x18mm modules, RAL9001",1.48]
["KSB1000ZP1","PLOMBA NAPÁJECÍ SKŘÍNĚ",20,"ks",{"v":2.9289093749999995,"d":"2.929"},"3606485013015",{"v":5.7,"d":"5.70"},{"v":0.8,"d":"0.80"},{"v":2.6,"d":"2.60"},{"v":6.8,"d":"6.80"},"FR","8538909999","https://www.se.com/sk/sk/product/KSB1000ZP1","Canalis-plomba napájacej skrine",""]
["KSA630EV4203","STÚP.VED. 2M/3 VÝV. 630A",1,"ks",{"v":1683.2812499999995,"d":"1683.281"},"3606480005480",{"v":213.8,"d":"213.80"},{"v":12.2,"d":"12.20"},{"v":16.8,"d":"16.80"},{"v":30020,"d":"30,020.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA630EV4203","Canalis – distribučná dĺžka podstavca – 630 A – 2 m – 3 odbočovacie výstupy",3.6]
["KSA630ET450","NAP. VED. 5M / 630A",1,"ks",{"v":2412.7031249999995,"d":"2412.703"},"3606480005459",513.75,{"v":17,"d":"17.00"},{"v":12,"d":"12.00"},{"v":59200,"d":"59,200.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KSA630ET450","Canalis - rovné prenos. vedenie - 630 A - 5 m -",7.1000000000000005]
["KSA630DZE41A","Z - KOLENO 630 A NA MIERU",1,"ks",{"v":1851.6093749999995,"d":"1851.609"},"3606489511395",{"v":74.2,"d":"74.20"},{"v":12,"d":"12.00"},{"v":74.2,"d":"74.20"},{"v":18000,"d":"18,000.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA630DZE41A","Zed, Canalis KSA630, aluminium, 630A, side B made to measure, upward/downward, 3L+N+PE, white RAL9001",2.16]
["KSA630DMCK41A","3D KOLENO 630 A NA MIERU",1,"ks",{"v":2356.5937499999995,"d":"2356.594"},"3606489511951",{"v":86.6,"d":"86.60"},{"v":71.6,"d":"71.60"},{"v":84.5,"d":"84.50"},{"v":20000,"d":"20,000.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA630DMCK41A","Multiple, Canalis KSA630, aluminium, 630A, side B made to measure, downward then turns left, 3L+N+PE, white RAL9001",2.4]
["KSA630DLE41A","KOLENO 630A VERTIKLNE NA MIERU HORE",1,"ks",{"v":1571.0624999999998,"d":"1571.063"},"3606489510572",{"v":86.6,"d":"86.60"},{"v":12,"d":"12.00"},{"v":86.6,"d":"86.60"},{"v":19000,"d":"19,000.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA630DLE41A","Elbow, Canalis KSA630, aluminium, 630A, side B made to measure, to go upward, 3L+N+PE, white RAL9001",2.2800000000000002]
["KSA500ET430","NAP. VED. 500 A 3M",1,"ks",{"v":1851.6093749999995,"d":"1851.609"},"3606480004988",313.74,{"v":17,"d":"17.00"},{"v":12,"d":"12.00"},{"v":35900,"d":"35,900.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA500ET430","Canalis - rovné prenos. vedenie - 500 A - 3 m -",4.3100000000000005]
["KSA400FA4","ADAPTÉR 400 A",1,"ks",{"v":785.5312499999999,"d":"785.531"},"3606485014524",{"v":32.4,"d":"32.40"},{"v":10.6,"d":"10.60"},{"v":19,"d":"19.00"},{"v":4650,"d":"4,650.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA400FA4","Canalis - adaptér pre starý KS - 400 A",0.56]
["KSA400DZCG41A","Z - KOLENO 400 A NA MIERU",1,"ks",{"v":2468.8124999999995,"d":"2468.813"},"3606489511197",{"v":79,"d":"79.00"},{"v":16.7,"d":"16.70"},{"v":28.8,"d":"28.80"},{"v":21000,"d":"21,000.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA400DZCG41A","Zed, Canalis KSA400, aluminium, 400A, side B made to measure, turns left then right, 3L+N+PE, white RAL9001",2.52]
["KSA400DLF4CFM","KOLENO NA MIERU NADOL S PROTIPOŽIAR. UPC",1,"ks",{"v":1627.1718749999995,"d":"1627.172"},"3606489548162",{"v":98.3,"d":"98.30"},{"v":6.3,"d":"6.30"},{"v":82.8,"d":"82.80"},{"v":24000,"d":"24,000.00"},"FR","85369001","https://www.se.com/sk/sk/product/KSA400DLF4CFM","Elbow, missing link, Canalis KSA400, aluminium, 400A, sides A/B made to measure, 1 fire barrier, to go downward, RAL9001",2.88]
["KSA400ABGD4","KONCOVÁ NAPÁJECÍ SKŘÍŇ 400 A LEVÁ S JIŠT",1,"ks",{"v":4039.874999999999,"d":"4039.875"},"3606485015958",{"v":86.6,"d":"86.60"},{"v":21.8,"d":"21.80"},{"v":39.3,"d":"39.30"},{"v":22700,"d":"22,700.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KSA400ABGD4","Canalis-koncová napájacia skriňa 400 A ľavá s istením",2.72]
["KSA250EV4254","STUP. VED. 500-630 A / 0,8 M/ 1 VYV.",1,"ks",{"v":504.9843749999999,"d":"504.984"},"3606480004452",{"v":258.8,"d":"258.80"},{"v":6.4,"d":"6.40"},{"v":16.6,"d":"16.60"},{"v":18350,"d":"18,350.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA250EV4254","Canalis - rovná diaľka distribučná - 250 A - 2,5 m - 4 vývody",2.2]
["KSA250DTC40","T ODBOČKA STOJ 100/160/250A",1,"ks",{"v":1032.4124999999997,"d":"1032.413"},"3606480004254",{"v":44,"d":"44.00"},{"v":24.8,"d":"24.80"},{"v":21.6,"d":"21.60"},{"v":4782,"d":"4,782.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA250DTC40","Canalis – T-kus na zmenu smeru – 250 A – zvislá montáž",0.58]
["KSA250CM4AF","NAP.VED.S PROTIP.UPCH. VER. 250 A / 800-",1,"ks",{"v":931.4156249999997,"d":"931.416"},"3606489508494",{"v":195,"d":"195.00"},{"v":16.7,"d":"16.70"},{"v":6.4,"d":"6.40"},{"v":8200,"d":"8,200.00"},"FR","85369001","https://www.se.com/sk/sk/product/KSA250CM4AF","Vertical transport length, Canalis KSA250, aluminium, 250A, fire barrier, made to measure 0.8-1.9m, 3L+N+PE, RAL9001",0.98]
["KSA250AB4","KONC. NAP.SKR.100/160/250A/UNI",1,"ks",{"v":785.5312499999999,"d":"785.531"},"3606480004025",{"v":50.6,"d":"50.60"},{"v":18,"d":"18.00"},{"v":32,"d":"32.00"},{"v":9900,"d":"9,900.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA250AB4","Canalis – prívodná jednotka pre KSA – 250 A – ľavá alebo pravá montáž",1.19]
["KSA1000ET450","NAP.VED. 1000 A / 5 M",1,"ks",{"v":3254.343749999999,"d":"3254.344"},"3606480003844",513.75,{"v":17,"d":"17.00"},{"v":12,"d":"12.00"},{"v":90500,"d":"90,500.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KSA1000ET450","Canalis - rovné prenos. vedenie - 1000 A - 5 m -",10.86]
["KSA1000DLE4AM","KOLENO NA MIERU NAHOR 1000 A ML",1,"ks",{"v":2019.9374999999995,"d":"2019.938"},"3606489547974",{"v":86.6,"d":"86.60"},{"v":12,"d":"12.00"},{"v":86.6,"d":"86.60"},{"v":19500,"d":"19,500.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KSA1000DLE4AM","Elbow, missing link, Canalis KSA1000, aluminium, 1000A, sides A/B made to measure, to go upward, 3L+N+PE, white RAL9001",2.34]
["KSA1000ABG4","KONC. NAP.SKR.800/1000A/VLAVO",1,"ks",{"v":3198.2343749999995,"d":"3198.234"},"3606480003479",{"v":78,"d":"78.00"},{"v":40.5,"d":"40.50"},{"v":52.5,"d":"52.50"},{"v":29600,"d":"29,600.00"},"FR","8536909500","https://www.se.com/sk/sk/product/KSA1000ABG4","Canalis – prívodná jednotka pre KSA – 1000 A – ľavá montáž",3.5500000000000003]
["KNT100ED4306","DIST.VED. KNT 100 A / 3 M 6 VYV.",1,"ks",{"v":589.1484374999999,"d":"589.148"},"3606480003363",{"v":310,"d":"310.00"},{"v":3.5,"d":"3.50"},{"v":10,"d":"10.00"},{"v":5000,"d":"5,000.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KNT100ED4306","Canalis - ovná dĺžka - 100 A - 6 vývodov",0.6]
["KNB63SM412","VYVODOVÁ SKRINA",1,"ks",{"v":286.1578124999999,"d":"286.158"},"3606480006302",{"v":41.9,"d":"41.90"},{"v":13.7,"d":"13.70"},{"v":16.6,"d":"16.60"},{"v":1760,"d":"1,760.00"},"IT","8536900100","https://www.se.com/sk/sk/product/KNB63SM412","Canalis - vývodná modulárna skriňa 63A - 12x18 mm modul,",0.21]
["KNB160ZFPU","PRUZINOVY DRZIAK 40-160 A",1,"ks",{"v":28.054687499999993,"d":"28.055"},"3606480006401",{"v":6,"d":"6.00"},{"v":26.9,"d":"26.90"},{"v":3.3,"d":"3.30"},{"v":280,"d":"280.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KNB160ZFPU","Canalis-pružinový držiak KN",0]
["KNA63ED4204","ROVNÉ VEDENIE 2M 63A /4 VYVODY",1,"ks",{"v":230.04843749999995,"d":"230.048"},"3606480003219",{"v":210,"d":"210.00"},{"v":4,"d":"4.00"},{"v":10,"d":"10.00"},{"v":3000,"d":"3,000.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KNA63ED4204","Canalis – priama dĺžka – 63 A – 4 odbočovacie výstupy",0.36]
["KNA160DF410","PRUŽNÉ VED. 160 A / 1 M",1,"ks",{"v":650.8687499999999,"d":"650.869"},"3606480003097",{"v":101,"d":"101.00"},{"v":3.5,"d":"3.50"},{"v":9.2,"d":"9.20"},{"v":2200,"d":"2,200.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KNA160DF410","Canalis - flexibilný diel - 160 A - 1 m - montáž vľavo alebo vpravo",0.26]
["KNA100DL4","PRUZNE KOLENO 100 A /355 MM",1,"ks",{"v":454.4859374999999,"d":"454.486"},"3606480003028",{"v":54.5,"d":"54.50"},{"v":4,"d":"4.00"},{"v":11,"d":"11.00"},{"v":1037,"d":"1,037.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KNA100DL4","Canalis - flexibilné ohybné koleno - 100 A - vnútorný/vonkajší uhol 80 až 180°",0.12]
["KCE1YZ","OVLÁDAČ PRE NÚDZOVÝ VYPÍNAČ V02/V2",1,"ks",{"v":14.641199999999998,"d":"14.641"},"3389110424348",{"v":7.9,"d":"7.90"},{"v":6.5,"d":"6.50"},{"v":6.6,"d":"6.60"},{"v":40,"d":"40.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/KCE1YZ","pred. otočná rukoväť KCE – pre VN-12, VN-20, V02 - V2 – červená rukoväť",0]
["KBD1H","OVLÁDACIA HLAVICA PRE K1/K2",1,"ks",{"v":10.980899999999998,"d":"10.981"},"3389110980585",{"v":7,"d":"7.00"},{"v":8.5,"d":"8.50"},{"v":7,"d":"7.00"},{"v":66,"d":"66.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/KBD1H","operačná hlava 60 x 60 mm – kovová farba – čierna rukoväť – prázd. na vyrytie",0]
["KBC16ZL30","KaDOVACIE PÁSKY, CERVENÁ",1,"ks",{"v":4.3218,"d":"4.322"},"3606480002403",{"v":4.5,"d":"4.50"},{"v":0.5,"d":"0.50"},{"v":0.8,"d":"0.80"},{"v":2,"d":"2.00"},"FR","8538909999","https://www.se.com/sk/sk/product/KBC16ZL30","Canalis-zabezpečovacie zariadenie pre odbočné zás.a odbočné jednotky KDP-červená",0]
["KBC16DCB22","VÝV. KONEKTOR 16A",1,"ks",{"v":33.074999999999996,"d":"33.075"},"3606480002243",{"v":14,"d":"14.00"},{"v":5.5,"d":"5.50"},{"v":6.5,"d":"6.50"},{"v":110,"d":"110.00"},"FR","8536901000","https://www.se.com/sk/sk/product/KBC16DCB22","Connector, Canalis KB, 16A, polarity 2L+PE, phase selection, direct connection, not wired, compatible DALI/KNX protocol",0.01]
["KBC10DCS101","VYVOD 10A S KÁBLOM 0,8M",1,"ks",{"v":8.819999999999999,"d":"8.820"},"3606480002113",{"v":6,"d":"6.00"},{"v":3.3,"d":"3.30"},{"v":4,"d":"4.00"},{"v":66,"d":"66.00"},"FR","8536901000","https://www.se.com/sk/sk/product/KBC10DCS101","Canalis – odbočovacia jednotka – 10 A – pevná polarita – s pev. zapoj. – L1 + N",0]
["KBB40ZFC","HÁČIK NA REŤAZ",10,"ks",{"v":1.5876,"d":"1.588"},"3606480001888",{"v":15,"d":"15.00"},{"v":4,"d":"4.00"},{"v":15,"d":"15.00"},{"v":25,"d":"25.00"},"FR","8538909999","https://www.se.com/sk/sk/product/KBB40ZFC","Canalis – špirálový hák",0]
["KBB40ED22305W","ROV. VED. 40A 3M 5VÝV 2X P+N+PE BIELE",1,"ks",{"v":123.47999999999999,"d":"123.480"},"3606480001512",{"v":310,"d":"310.00"},{"v":5,"d":"5.00"},{"v":6,"d":"6.00"},{"v":5000,"d":"5,000.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KBB40ED22305W","Canalis - rovná dĺžka - 40 A - 3 m - 2 obvody - L+N+PE - biela",0.6]
["KBB40ED22203W","ROV.VED.40A/2M/3VÝV/3L+N+PE/L+N+PE BIELE",1,"ks",{"v":97.01999999999998,"d":"97.020"},"3606480001451",{"v":210,"d":"210.00"},{"v":5,"d":"5.00"},{"v":6,"d":"6.00"},{"v":4000,"d":"4,000.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KBB40ED22203W","Canalis - rovná dĺžka - 40 A - 2 m - 2 obvody - L+N+PE - biela",0.48]
["KBB40ABG4TW","KONCOVÁ NAPÁJACIA SKRIŇA 40A ĽAVÁ",1,"ks",{"v":77.61599999999999,"d":"77.616"},"3606480001093",{"v":27,"d":"27.00"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":550,"d":"550.00"},"PL","8536900100","https://www.se.com/sk/sk/product/KBB40ABG4TW","Canalis - napájacia jednotka pre KBB - 40A - montáž vľavo - vzd. ovl. - biela",0.07]
["KBA40ZFG2","PRÍSLUŠENSTVO K DRŽIAKOM",10,"ks",{"v":4.806899999999999,"d":"4.807"},"3606480000607",{"v":9.8,"d":"9.80"},{"v":2,"d":"2.00"},{"v":3.7,"d":"3.70"},{"v":26,"d":"26.00"},"FR","3926909790","https://www.se.com/sk/sk/product/KBA40ZFG2","Canalis - držiak káblového kanála a stredný držiak pre KBA",0]
["KBA40ED2303W","ROV. VED. 40A 3M 3VÝV L+N+PE BIELE",6,"ks",{"v":72.32399999999998,"d":"72.324"},"3606480000447",{"v":300,"d":"300.00"},{"v":4.6,"d":"4.60"},{"v":3,"d":"3.00"},{"v":3166,"d":"3,166.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KBA40ED2303W","Canalis - rovná dĺžka - 40 A - 3 m - L+N+PE -biela",0.38]
["KBA25ED4305TW","ROV. VED. 25A 3M 5VÝV. 3P+N+PE DIAL. OBV",1,"ks",{"v":167.57999999999998,"d":"167.580"},"3606480498787",{"v":300,"d":"300.00"},{"v":4.6,"d":"4.60"},{"v":3,"d":"3.00"},{"v":2666,"d":"2,666.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KBA25ED4305TW","Canalis-rovná dĺžka distribučná 25A 3m - 3L+N+PE",0.32]
["KBA25ED2302W","ROV. VED. 25A 3M 2VÝV. P+N+PE BIELE",1,"ks",{"v":46.745999999999995,"d":"46.746"},"3606480498718",{"v":314,"d":"314.00"},{"v":4,"d":"4.00"},{"v":3.2,"d":"3.20"},{"v":3000,"d":"3,000.00"},"FR","8536900100","https://www.se.com/sk/sk/product/KBA25ED2302W","Canalis-rovná dĺžka distribučná 25A 3m - L+N+PE",0.36]
["KAXZ1S141","OVL. HLAVICA PRE K1",1,"ks",{"v":21.5042625,"d":"21.504"},"3389110980806",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":64,"d":"64.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/KAXZ1S141","ovládateľná hlavica s rámčekom Ø 28.5 mm - kov - kľúč Ronis 455",0]
["KAC1H48","OVLÁDACIA HLAVICA PRE K1/K2",1,"ks",{"v":8.601705,"d":"8.602"},"3389110980523",{"v":8,"d":"8.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":58,"d":"58.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/KAC1H48","ovl. hlavica 45x45 mm - čierna farba - čierna rukoväť - 2 - 0 - 1",0]
["K63H001YP","VAČKOVÝ SPÍNAČ 63A",1,"ks",{"v":201.3165,"d":"201.317"},"3389110084641",{"v":7.2,"d":"7.20"},{"v":16,"d":"16.00"},{"v":7.2,"d":"7.20"},{"v":617,"d":"617.00"},"AT","8536508090","https://www.se.com/sk/sk/product/K63H001YP","Cam star-delta switch, Harmony K, front mounting, plastic, 3 poles, 60°, 63A, 64x64mm front plate, 3 marqued positions",0]
["K50H001YP","VAČKOVÝ SPÍNAČ 50A",1,"ks",{"v":169.288875,"d":"169.289"},"3389110084559",{"v":15.5,"d":"15.50"},{"v":7.2,"d":"7.20"},{"v":7.2,"d":"7.20"},{"v":465,"d":"465.00"},"AT","8536508090","https://www.se.com/sk/sk/product/K50H001YP","Cam star-delta switch, Harmony K, front mounting, plastic, 3 poles, 60°, 50A, 64x64mm front plate, 3 positions marked",0]
["K2M033N","BLOK KONTAKTOV K2",1,"ks",{"v":60.852487499999995,"d":"60.852"},"3389110479249",{"v":6.5,"d":"6.50"},{"v":11,"d":"11.00"},{"v":6.5,"d":"6.50"},{"v":217,"d":"217.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K2M033N","Body for stepping switch, Harmony K, Ø 22mm, plastic, 4 poles, 3 steps, 45°, 20A",0]
["K2H014U","BLOK KONTAKTOV K2",1,"ks",{"v":41.178374999999996,"d":"41.178"},"3389110478204",{"v":6.5,"d":"6.50"},{"v":10.9,"d":"10.90"},{"v":6.5,"d":"6.50"},{"v":165,"d":"165.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K2H014U","Body for changeover switch, Harmony K, Ø 22mm, plastic, 4 poles, 2 positions, 30°, 20A",0]
["K2D002ULH","VAČKOVÝ SPÍNAČ LP",1,"ks",{"v":33.857775,"d":"33.858"},"3389110979787",{"v":11,"d":"11.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":140,"d":"140.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K2D002ULH","vačkový prepínač - 2-pól.- 45° - 20 A - skrutkovacia montáž",0]
["K2B001UCH","VAČKOVÝ SPÍNAČ KOMPLET",1,"ks",{"v":30.197474999999997,"d":"30.197"},"3389110979756",{"v":11,"d":"11.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":135,"d":"135.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K2B001UCH","Cam changeover switch, Harmony K, Ø 22mm, plastic, 1 pole, position 0, 45°, 20A, 45x45mm, metallic legend, marked 2/0/1, 35mm black handle",0]
["K1Q034NZ4","Vačkový spínač, 4 polohy",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3389110726343",{"v":5,"d":"5.00"},{"v":15.5,"d":"15.50"},{"v":10,"d":"10.00"},{"v":528,"d":"528.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1Q034NZ4","vačkový krokový spínač - 4-pól - 60 ° - 12 A - čelná montáž - čierna rukoväť",0]
["K1H014NCH","VAČKOVÝ SPÍNAČ KOMPLET",1,"ks",{"v":51.70173749999999,"d":"51.702"},"3389110979046",{"v":16.5,"d":"16.50"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":225,"d":"225.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1H014NCH","vačkový krokový spínač - 2-pól.- 45° - 12 A - pre Ø 22 mm",0]
["K1F037MCH","VAČKOVÝ SPÍNAČ KOMPLET",1,"ks",{"v":43.92359999999999,"d":"43.924"},"3389110979435",{"v":5.6,"d":"5.60"},{"v":13.5,"d":"13.50"},{"v":5.2,"d":"5.20"},{"v":190,"d":"190.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1F037MCH","vačkový voltmetrový spínač - 3L a 3L-N - 60° - 12 A - pre Ø 22 mm",0]
["K1F006NX","BLOK KONTAKTOV S KOV. PRÍRUBOU",1,"ks",{"v":72.74846249999999,"d":"72.748"},"3389110794250",{"v":11,"d":"11.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":218,"d":"218.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1F006NX","telo pre krokový vačkový spínač - 1P - 45° - 12 A - pre Ø 22 mm",0]
["K1E005QLH","KOMPLET. VAČ. SPÍNAČ PRIEMERU 22",1,"ks",{"v":33.400237499999996,"d":"33.400"},"3389110978797",{"v":11,"d":"11.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":167,"d":"167.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1E005QLH","krokový vačkový spínač - 1P - 45° - 12 A - šróbová montáž",0]
["K1D004Q","BLOK KONTAKTOV K1",1,"ks",{"v":21.961799999999997,"d":"21.962"},"3389110442380",{"v":8,"d":"8.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":110,"d":"110.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1D004Q","teleso pre krokový volič – 1 pól – 45° – 12 A – pre Ø 22 mm",0]
["K1C003QCH","VAČKOVÝ SPÍNAČ KOMPLET",1,"ks",{"v":36.145462499999994,"d":"36.145"},"3389110978728",{"v":11,"d":"11.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":155,"d":"155.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1C003QCH","vačkový krokový volič – 1 pól – 45° – 12 A – pre Ø 22 mm",0]
["K1B1002HCH","VAČKOVÝ SPÍNAČ KOMPLET",1,"ks",{"v":26.994712499999995,"d":"26.995"},"3389110978377",{"v":11,"d":"11.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":157,"d":"157.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1B1002HCH","vačkový spínač – 2 póly – 90° – 12 A – pre Ø 22 mm",0]
["K1B002A","VAČKOVY SPÍNAČ",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110442946",{"v":8,"d":"8.00"},{"v":6.5,"d":"6.50"},{"v":6.5,"d":"6.50"},{"v":94,"d":"94.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/K1B002A","telo pre vačkový spínač - 2P - 45° - 12 A - pre Ø 22 mm",0]
["K150F003UP","VAČKOVÝ SPÍNAČ 150A",1,"ks",{"v":526.1681249999999,"d":"526.168"},"3389110083392",{"v":24,"d":"24.00"},{"v":9.8,"d":"9.80"},{"v":9.8,"d":"9.80"},{"v":760,"d":"760.00"},"AT","8536508090","https://www.se.com/sk/sk/product/K150F003UP","vačkový prepínač - 3-pól.- 60 ° - 150 A - skrutkovacia montáž",0]
["K10F003MCH","VAČKOVÝ AMPÉRMETROVÝ PREPÍNAČ",1,"ks",{"v":52.616812499999995,"d":"52.617"},"3389110076769",{"v":10.5,"d":"10.50"},{"v":4,"d":"4.00"},{"v":4.1,"d":"4.10"},{"v":55,"d":"55.00"},"AT","8536508090","https://www.se.com/sk/sk/product/K10F003MCH","vačkový prepínač ampérmetra – 3L-N – 90° – 10 A – pre Ø 16 alebo 22 mm",0]
["K10D002UCH","VAČKOVÝ SPÍNAČ 2-POLOHOVÝ 10A",1,"ks",{"v":69.0881625,"d":"69.088"},"3389110076653",{"v":4.1,"d":"4.10"},{"v":10.6,"d":"10.60"},{"v":4,"d":"4.00"},{"v":66,"d":"66.00"},"AT","8536508090","https://www.se.com/sk/sk/product/K10D002UCH","vačkový prepínač – 2 póly – 60° – 10 A – pre Ø 16 alebo 22 mm",0]
["ISM71501","KÁBLOVÁ VÝVODKA M12",20,"ks",{"v":0.8889299999999998,"d":"0.889"},"3606480077180",{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":5,"d":"5.00"},"TR","7326909890","https://www.se.com/sk/sk/product/ISM71501","káblové vývodky IP 68 – M12",0]
["ISM50524","Podlahová krabica, 4 jednoduché/2 dvojit",1,"ks",{"v":42.66863999999999,"d":"42.669"},"3606480030895",{"v":21.6,"d":"21.60"},{"v":8,"d":"8.00"},{"v":21.4,"d":"21.40"},{"v":1084,"d":"1,084.00"},"SE","7326909890","https://www.se.com/sk/sk/product/ISM50524","OptiLine 45 - Unica floor outlet box - 4 modules",0]
["ISM20821","doska pre upev. k podl. inšt.stĺpik,slot",1,"ks",{"v":51.55793999999999,"d":"51.558"},"3606480030710",{"v":15.6,"d":"15.60"},{"v":3.8,"d":"3.80"},{"v":12.1,"d":"12.10"},{"v":261,"d":"261.00"},"SE","7616999099","https://www.se.com/sk/sk/product/ISM20821","OptiLine 45 - floor fixing - grey",0]
["ISM20410","STOLNÝ BOX PRÁZDNY PRE 5+1 MOD",1,"ks",{"v":231.12179999999995,"d":"231.122"},"3606480317507",{"v":41,"d":"41.00"},{"v":16.5,"d":"16.50"},{"v":29,"d":"29.00"},{"v":1513,"d":"1,513.00"},"SE","7616999099","https://www.se.com/sk/sk/product/ISM20410","OptiLine 45 - výklopný zásuvkový box na 6 modulov 45x45",0]
["ISM20110","Inšt. stĺpik, obojstranný, pružne ukotve",1,"ks",{"v":542.2472999999999,"d":"542.247"},"3606480029660",{"v":366.5,"d":"366.50"},{"v":12.5,"d":"12.50"},{"v":16,"d":"16.00"},{"v":12000,"d":"12,000.00"},"SE","7616999099","https://www.se.com/sk/sk/product/ISM20110","OptiLine 45 - pole - tension-mounted - two-sided - natural - 3500-3900 mm",0]
["ISM20100","Inšt. stĺpik, pružne ukotvený 2.7-3.1m,",1,"ks",{"v":306.6808499999999,"d":"306.681"},"3606480029561",{"v":291.5,"d":"291.50"},{"v":12.5,"d":"12.50"},{"v":16.3,"d":"16.30"},{"v":7500,"d":"7,500.00"},"SE","7616999099","https://www.se.com/sk/sk/product/ISM20100","OptiLine 45 - pole - tension-mounted - one-sided - natural - 2700-3100 mm",0]
["ISM10904","Spojka kanála, vnútorná",1,"ks",{"v":2.0889854999999997,"d":"2.089"},"3606480028434",{"v":5.1,"d":"5.10"},{"v":0.5,"d":"0.50"},{"v":10,"d":"10.00"},{"v":12,"d":"12.00"},"SE","39269097","https://www.se.com/sk/sk/product/ISM10904","OptiLine 45 - internal jointing piece - PC/ABS - white",0]
["ISM10353","Koleno 90° 140x55, ALU",1,"ks",{"v":21.334319999999995,"d":"21.334"},"3606480028052",{"v":21.5,"d":"21.50"},{"v":21.5,"d":"21.50"},{"v":5.7,"d":"5.70"},{"v":183,"d":"183.00"},"SE","39259020","https://www.se.com/sk/sk/product/ISM10353","OptiLine 45 - bend 90° - PC/ABS - aluminium metallic",0]
["ISM10154","Záslepka 75x55, ALU",1,"ks",{"v":12.889484999999997,"d":"12.889"},"3606480027826",{"v":2.1,"d":"2.10"},{"v":7.9,"d":"7.90"},{"v":5.6,"d":"5.60"},{"v":25,"d":"25.00"},"SE","39259020","https://www.se.com/sk/sk/product/ISM10154","OptiLine 45 - stop end - PC/ABS - aluminium metallic",0]
["ISM10102P","Vonkajší roh 75x55, biely",1,"ks",{"v":8.5781745,"d":"8.578"},"3606480681516",{"v":13.5,"d":"13.50"},{"v":8.5,"d":"8.50"},{"v":8,"d":"8.00"},{"v":93,"d":"93.00"},"PL","39259020","https://www.se.com/sk/sk/product/ISM10102P","OptiLine 45 - Vonkajší roh 75x55, biely",0]
["INS52162","Káblový výstup pre krabice M-L, sada 2ks",1,"ks",{"v":3.5567909999999987,"d":"3.557"},"3606481457394",{"v":10,"d":"10.00"},{"v":3,"d":"3.00"},{"v":6,"d":"6.00"},{"v":24,"d":"24.00"},"ZZ","3925908000","https://www.se.com/sk/sk/product/INS52162","Unica System+ - Káblový výstup pre podlahovú krabicu M-L, (sada 2ks)",0]
["INS52158","Výplň veka linoleum L",1,"ks",{"v":12.734189999999998,"d":"12.734"},"3606489819101",{"v":24.4,"d":"24.40"},{"v":1,"d":"1.00"},{"v":12.5,"d":"12.50"},{"v":167,"d":"167.00"},"ZZ","59041000","https://www.se.com/sk/sk/product/INS52158","Unica System+ - Výplň veka linoleum L",0]
["INS52003","Krabica do betónu pre krabice XL, kovová",1,"ks",{"v":109.77749999999997,"d":"109.778"},"3606490150354",{"v":40,"d":"40.00"},{"v":16,"d":"16.00"},{"v":31,"d":"31.00"},{"v":3252,"d":"3,252.00"},"CZ","7326906000","https://www.se.com/sk/sk/product/INS52003","Unica System+ - Krabica do betónu pre podlahové krabice XL, kovová",0]
["INS44052","Stolný box S zásuvka + USB A 3.1A, Biela",1,"ks",{"v":68.06204999999999,"d":"68.062"},"3606489819293",{"v":12.2,"d":"12.20"},{"v":14,"d":"14.00"},{"v":13.3,"d":"13.30"},{"v":639,"d":"639.00"},"CN","8544429090","https://www.se.com/sk/sk/product/INS44052","Unica System+ - Stolní box S se zásuvkou 250V/16A + nabíječkou USB A 3.1A, Biela",0.08]
["INS44010","Stolný box XS bezdrôtová nabíjačka, Antr",1,"ks",{"v":37.76345999999999,"d":"37.763"},"3606489819262",{"v":11,"d":"11.00"},{"v":11,"d":"11.00"},{"v":11,"d":"11.00"},{"v":247,"d":"247.00"},"CN","8504406090","https://www.se.com/sk/sk/product/INS44010","Unica System+ - Stolní box XS s bezdrôtovou nabíjačkou, zápustný, Antracit",0]
["IMT47221","Mureva LED refl. PIR 50W/5000lm,6500K,IP",1,"ks",{"v":50.93675999999999,"d":"50.937"},"3606489903213",{"v":24.5,"d":"24.50"},{"v":24.5,"d":"24.50"},{"v":24.5,"d":"24.50"},{"v":1200,"d":"1,200.00"},"CN","9405423100","https://www.se.com/sk/sk/product/IMT47221","LED reflektor s pohybovým čidlom, Mureva, 50W/5000lm, 6500K, IP44, 230V",0.18]
["IMT46423","Viazacia páska 370x4.8, čierna,bal 100ks",1,"ks",{"v":4.918031999999998,"d":"4.918"},"3606486365663",{"v":40,"d":"40.00"},{"v":2.5,"d":"2.50"},{"v":13,"d":"13.00"},{"v":251,"d":"251.00"},"CN","3926909790","https://www.se.com/sk/sk/product/IMT46423","Viazacia páska, Thorsman, 370x4.8, čierna, balenie 100 ks",""]
["IMT46415","Viazacia páska 250x4.8, číra,bal 100ks",1,"ks",{"v":3.1615919999999997,"d":"3.162"},"3606486365588",{"v":33,"d":"33.00"},{"v":2,"d":"2.00"},{"v":13,"d":"13.00"},{"v":158,"d":"158.00"},"CN","3926909790","https://www.se.com/sk/sk/product/IMT46415","Viazacia páska, Thorsman, 250x4.8, číra, balenie 100 ks",""]
["IMT37314","KÁBLOVÝ VSTUP ISO M40",25,"ks",{"v":3.776345999999999,"d":"3.776"},"3606480398940",{"v":4.5,"d":"4.50"},{"v":3,"d":"3.00"},{"v":4.5,"d":"4.50"},{"v":23,"d":"23.00"},"IE","4016930090","https://www.se.com/sk/sk/product/IMT37314","Priechodka, Thorsman, EPDM, TET 20-26, 46/30mm, Ø38mm, sivá",0]
["IMT37304","PRIECHODKA IP67 M50 26-35MM 100s",50,"ks",{"v":0.7464869999999998,"d":"0.746"},"3606480398841",{"v":3,"d":"3.00"},{"v":2.5,"d":"2.50"},{"v":3,"d":"3.00"},{"v":5.3,"d":"5.30"},"SE","4016930090","https://www.se.com/sk/sk/product/IMT37304","Priechodka, Thorsman, CR, TET 7-10C, 24/20mm, Ø19mm, čierna",0]
["IMT36175","PRIECHODKA TET M26-35C 60/35 50 IP67 CR",25,"ks",{"v":5.244687,"d":"5.245"},"3606480163746",{"v":6,"d":"6.00"},{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":49,"d":"49.00"},"SE","40169300","https://www.se.com/sk/sk/product/IMT36175","Thorsman TET - priech.M26-35 - IP67 - čierna",0]
["IMT36161","PLASTOVÁ ZÁSLEPKA M12",40,"ks",{"v":0.6222509999999999,"d":"0.622"},"3606480163609",{"v":14,"d":"14.00"},{"v":3,"d":"3.00"},{"v":11,"d":"11.00"},{"v":2,"d":"2.00"},"DE","3926909790","https://www.se.com/sk/sk/product/IMT36161","záslepka pre M12 - káblová vývodka",0]
["IMT35944","Montážna krabica štvornásobná 40mm",1,"ks",{"v":6.1475399999999985,"d":"6.148"},"3606489550325",{"v":29,"d":"29.00"},{"v":4.1,"d":"4.10"},{"v":7.3,"d":"7.30"},{"v":102,"d":"102.00"},"PL","3925908000","https://www.se.com/sk/sk/product/IMT35944","montážna krabica štvornásobná, Multifix, 40mm",0]
["IMT33153","Predlž. gumový kábel 25m IP44 spojka",1,"ks",{"v":114.16859999999997,"d":"114.169"},"3606481375049",{"v":41.5,"d":"41.50"},{"v":34.5,"d":"34.50"},{"v":22.5,"d":"22.50"},{"v":9720,"d":"9,720.00"},"CN","8544429090","https://www.se.com/sk/sk/product/IMT33153","Predlžovací gumový kábel na bubne, Thorsman, 25m, 3G2.5, IP44, spojka",1.1500000000000001]
["ILS1F572PC1A0","Kompaktný pohon ILS krokový motor - 24",1,"ks",{"v":1001.3849999999999,"d":"1001.385"},"3389119227070",{"v":39,"d":"39.00"},{"v":10.5,"d":"10.50"},{"v":19,"d":"19.00"},{"v":2000,"d":"2,000.00"},"DE","8501510090","https://www.se.com/sk/sk/product/ILS1F572PC1A0","kompaktný pohon ILS krokový motor - 24..36 V - CANopen DS301 - 3.5A",0.24]
["ILA1F572PB1F0","LEXIUM ILA SERVOMOT 24 36V CANOP BRAKE",1,"ks",{"v":1464.3783,"d":"1464.378"},"3389119225519",{"v":18,"d":"18.00"},{"v":10.5,"d":"10.50"},{"v":38,"d":"38.00"},{"v":2583,"d":"2,583.00"},"DE","8501510090","https://www.se.com/sk/sk/product/ILA1F572PB1F0","kompaktný pohon ILA so servomotorom - 24..36 V - CANopen - PCB konektor",""]
["HMIZGPWS2","KONEKTORY PRE NAPÁJANIE UHL TYP",1,"ks",{"v":44.7678,"d":"44.768"},"3595864150352",17.78,2.54,10.16,{"v":40,"d":"40.00"},"JP","85369010","https://www.se.com/sk/sk/product/HMIZGPWS2","konektor pre napájanie DC - pravý",0]
["HMIWRT010","E. Operator Terminal Expert Web Viewer10",1,"ks",{"v":276.8535,"d":"276.854"},"3606481053985",24.89,0.51,17.53,54.43,"FR","4907009000","https://www.se.com/sk/sk/product/HMIWRT010","E. Operator Terminal Expert Web Viewer 10",0]
["HMISTU655W","DOTYK.OP 3,5\" FAREBNÝ, 1XSERIAL, TCP/IP,",1,"ks",{"v":658.35,"d":"658.350"},"3595864153308",{"v":18.5,"d":"18.50"},{"v":6.5,"d":"6.50"},{"v":13,"d":"13.00"},{"v":540,"d":"540.00"},"CN","85371091","https://www.se.com/sk/sk/product/HMISTU655W","graf. panel Magelis HMI STU 3.5\" bez popisu na paneli",0]
["HMIST6400","Magelis Basic HMI ST6, 7\"W",1,"ks",{"v":831.9150000000001,"d":"831.915"},"3606489523381",{"v":27,"d":"27.00"},{"v":9.2,"d":"9.20"},{"v":17.5,"d":"17.50"},{"v":800,"d":"800.00"},"CN","8537101090","https://www.se.com/sk/sk/product/HMIST6400","Dotykový panel, Harmony ST6, 7  palcový displej, 2COM, 2Ethernet, USB host&device, 24 VDC",0.15]
["HMIGTO6315","OP 12.1\" TFT IP66K NEREZ 2XSERIAL 2XUSB",1,"ks",{"v":3711.0149999999994,"d":"3711.015"},"3595864150314",{"v":53.5,"d":"53.50"},{"v":20.5,"d":"20.50"},{"v":42.5,"d":"42.50"},{"v":3000,"d":"3,000.00"},"CN","8537109199","https://www.se.com/sk/sk/product/HMIGTO6315","pokročilý dotykový panel HMIGTO 800 x 600 pixel SVGA- 12.1\" TFT - 96 MB - nerez.",0.75]
["HMIGK5310","Graf. panel Magelis GK 10,4\" color TFT",1,"ks",{"v":4064.4449999999997,"d":"4064.445"},"3606480992094",{"v":45.5,"d":"45.50"},{"v":22.4,"d":"22.40"},{"v":37.2,"d":"37.20"},{"v":2990,"d":"2,990.00"},"CN","8537101090","https://www.se.com/sk/sk/product/HMIGK5310","graf. panel Magelis GK 10,4\" color TFT,klávesy(30FK,NUM,JOY)2xserial (RS232,485)",0]
["GZ1E21","ISTENÝ MOTOROVÝ SPÚŠŤAČ GZ1 17-23A",1,"ks",{"v":52.159274999999994,"d":"52.159"},"3606480567896",{"v":9,"d":"9.00"},{"v":8.4,"d":"8.40"},{"v":4.7,"d":"4.70"},{"v":277,"d":"277.00"},"CN","8536201090","https://www.se.com/sk/sk/product/GZ1E21","motorový istič GZ1 - 3 pólový 3d - 17..23A - termomagnetická spúšť",0.03]
["GZ1E20","ISTENÝ MOTOROVÝ SPÚŠŤAČ GZ1 13-18A",1,"ks",{"v":48.956512499999995,"d":"48.957"},"3606480567889",{"v":9,"d":"9.00"},{"v":8.4,"d":"8.40"},{"v":4.8,"d":"4.80"},{"v":277,"d":"277.00"},"CN","8536201090","https://www.se.com/sk/sk/product/GZ1E20","motorový istič GZ1 - 3 pólový 3d - 13..18A - termomagnetická spúšť",0.03]
["GVAX385","PODPAŤOVÁ SPÚŠŤ 380V-50Hz (INRS)",1,"ks",{"v":55.81957499999999,"d":"55.820"},"3389110346312",{"v":9.5,"d":"9.50"},{"v":3.8,"d":"3.80"},{"v":8.5,"d":"8.50"},{"v":122,"d":"122.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/GVAX385","zníženie napätia TeSys GV-AX – 380 - 400 V AC 50 Hz",0]
["GVAU207","PODPAŤOVÁ SPÚŠŤ 200V",1,"ks",{"v":34.3153125,"d":"34.315"},"3389110345988",{"v":9.1,"d":"9.10"},{"v":8.3,"d":"8.30"},{"v":3.6,"d":"3.60"},{"v":105,"d":"105.00"},"CZ","8536309090","https://www.se.com/sk/sk/product/GVAU207","Undervoltage release (MN),TeSys Deca frame 2,200V AC 50Hz",0]
["GVAPL01","Zameriavací nástroj pre inštaláciu",1,"ks",{"v":96.08287499999999,"d":"96.083"},"3606480312663",{"v":30,"d":"30.00"},{"v":7,"d":"7.00"},{"v":8.5,"d":"8.50"},{"v":100,"d":"100.00"},"SG","8205598000","https://www.se.com/sk/sk/product/GVAPL01","TeSys GV2 & TeSys GV3 & TeSys U - nástroj pre mont. rukoväte",0]
["GVAE203","POM. KONTAKTY NO+NO PR. SVORKY",1,"ks",{"v":15.098737499999999,"d":"15.099"},"3389110346657",{"v":4.6,"d":"4.60"},{"v":1.4,"d":"1.40"},{"v":3.2,"d":"3.20"},{"v":16,"d":"16.00"},"CZ","8536508090","https://www.se.com/sk/sk/product/GVAE203","TeSys GV2 & GV3 -napätová spúšť - 2 Z",0]
["GV7AP01","OTOČNÝ OVLÁDAČ PREDL. RUK.",1,"ks",{"v":150.987375,"d":"150.987"},"3389110567328",{"v":49.2,"d":"49.20"},{"v":9.9,"d":"9.90"},{"v":10.6,"d":"10.60"},{"v":710,"d":"710.00"},"FR","8538909999","https://www.se.com/sk/sk/product/GV7AP01","pred. otočná rukoväť GV7AP GV7R – čierna rukoväť",0]
["GV6AP03","GV6 otočná ovládací rukojeť černá",1,"ks",{"v":70.1862525,"d":"70.186"},"3606489902124",{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":15,"d":"15.00"},{"v":504,"d":"504.00"},"IN","8538909999","https://www.se.com/sk/sk/product/GV6AP03","GV6 otočná ovládacia rukoväť čierna",""]
["GV4PEM12N6","Motorový istič multifunkčný 12.5A 50kA o",1,"ks",{"v":553.620375,"d":"553.620"},"3606481310903",{"v":22,"d":"22.00"},{"v":16.5,"d":"16.50"},{"v":11,"d":"11.00"},{"v":1422,"d":"1,422.00"},"PL","8536201090","https://www.se.com/sk/sk/product/GV4PEM12N6","motorový istič multifunkčný 12.5A 50kA oka",0.17]
["GV4PEM03N","Motorový istič multifunkčný 3.5A 50kA El",5,"ks",{"v":553.620375,"d":"553.620"},"3606481386274",{"v":22,"d":"22.00"},{"v":11,"d":"11.00"},{"v":17,"d":"17.00"},{"v":1450,"d":"1,450.00"},"PL","8536201090","https://www.se.com/sk/sk/product/GV4PEM03N","motorový istič multifunkčný 3.5A 50kA Elink",0.2]
["GV4PE25S","Motorový istič  termo-magnetická sp. 25A",5,"ks",{"v":462.1128749999999,"d":"462.113"},"3606481310590",{"v":22,"d":"22.00"},{"v":12.5,"d":"12.50"},{"v":9,"d":"9.00"},{"v":1450,"d":"1,450.00"},"PL","8536201090","https://www.se.com/sk/sk/product/GV4PE25S","motorový istič termo-magnetická spúšť 25A 100kA Elink",0.17]
["GV4PE03N6","Motorový istič  termo-magnetická sp. 3.5",1,"ks",{"v":544.469625,"d":"544.470"},"3606481310408",{"v":22,"d":"22.00"},{"v":16.5,"d":"16.50"},{"v":11,"d":"11.00"},{"v":1526,"d":"1,526.00"},"PL","8536201090","https://www.se.com/sk/sk/product/GV4PE03N6","motorový istič termo-magnetická spúšť 3.5A 50kA oka",0.18]
["GV4P12N","Motorový istič  termo-magnetická sp. 12.",3,"ks",{"v":416.35912499999995,"d":"416.359"},"3606481310347",{"v":22,"d":"22.00"},{"v":21,"d":"21.00"},{"v":10.7,"d":"10.70"},{"v":1820,"d":"1,820.00"},"PL","8536201090","https://www.se.com/sk/sk/product/GV4P12N","motorový istič termo-magnetická spúšť 12.5A 50kA Elink",0.22]
["GV4P07N6","Motorový istič  termo-magnetická sp. 7A ",1,"ks",{"v":576.4972499999999,"d":"576.497"},"3606481310491",{"v":22,"d":"22.00"},{"v":11,"d":"11.00"},{"v":21,"d":"21.00"},{"v":1695,"d":"1,695.00"},"PL","8536201090","https://www.se.com/sk/sk/product/GV4P07N6","motorový istič termo-magnetická spúšť 7A 50kA oka",0.2]
["GV4LE115N","Motorový istič magnetická sp. 115A 50kA",1,"ks",{"v":494.1404999999999,"d":"494.141"},"3606481309662",{"v":22,"d":"22.00"},{"v":16.6,"d":"16.60"},{"v":10.9,"d":"10.90"},{"v":1500,"d":"1,500.00"},"PL","8536209090","https://www.se.com/sk/sk/product/GV4LE115N","motorový istič magnetická spúšť 115A 50kA Elink",0.2]
["GV4LE02S6","Motorový istič  magnetická sp. 2A 100kA ",1,"ks",{"v":440.15107499999993,"d":"440.151"},"3606481309990",{"v":22,"d":"22.00"},{"v":16.5,"d":"16.50"},{"v":11,"d":"11.00"},{"v":1492,"d":"1,492.00"},"PL","8536201090","https://www.se.com/sk/sk/product/GV4LE02S6","motorový istič magnetická spúšť 2A 100kA oka",""]
["GV4L03N","Motorový istič  magnetická sp. 3.5A 50kA",1,"ks",{"v":397.14254999999997,"d":"397.143"},"3606481309686",{"v":22,"d":"22.00"},{"v":21,"d":"21.00"},{"v":10.7,"d":"10.70"},{"v":1900,"d":"1,900.00"},"PL","8536201090","https://www.se.com/sk/sk/product/GV4L03N","motorový istič magnetická spúšť 3.5A 50kA Elink",""]
["GV3PC01","KOVOVÁ SKRINKA PRE ISTIČ GV3P DO 30A",1,"ks",{"v":297.39937499999996,"d":"297.399"},"3389119409933",{"v":31.5,"d":"31.50"},{"v":19.5,"d":"19.50"},{"v":21.5,"d":"21.50"},{"v":3642,"d":"3,642.00"},"FR","8538100000","https://www.se.com/sk/sk/product/GV3PC01","TeSys GV3 - skriňa pre TeSys GV3P/L - čierna rukoväť - IP65",0.48]
["GV3P406","ISTENÝ MOT. SPÚŠŤAČ 30...40A KÁB. OKÁ",1,"ks",219.618,"3389118204119",{"v":14.5,"d":"14.50"},{"v":16,"d":"16.00"},{"v":6.5,"d":"6.50"},{"v":908,"d":"908.00"},"FR","8536209090","https://www.se.com/sk/sk/product/GV3P406","motor. istič GV3 póly – 30 - 40 A – 3 póly 3d – magnetická vypínacia jednotka",0.11]
["GV3L50","ISTENÝ MOT. SPÚŠŤAČ 50A, 50kA",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3389119405454",{"v":14.5,"d":"14.50"},{"v":6.5,"d":"6.50"},{"v":16,"d":"16.00"},{"v":997,"d":"997.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GV3L50","motor. istič GV3L – 50 A – 3 póly – magnetická vypínacia jednotka",0.12]
["GV2SN33","KONTR.SVETLO 400V ZE",1,"ks",{"v":20.13165,"d":"20.132"},"3389110476095",{"v":10,"d":"10.00"},{"v":6,"d":"6.00"},{"v":8,"d":"8.00"},{"v":6,"d":"6.00"},"FR","8531807000","https://www.se.com/sk/sk/product/GV2SN33","zelená kontrolka – TeSys GV2-SN – neónová – 380 - 440 V",0]
["GV2P21","ISTENÝ MOT. SPÚŠŤAČ 17-23A >50KA",1,"ks",{"v":155.56275,"d":"155.563"},"3389110213522",{"v":10,"d":"10.00"},{"v":9.3,"d":"9.30"},{"v":4.8,"d":"4.80"},{"v":338,"d":"338.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GV2P21","motor. istič GV2-P –17 - 23 A – 3 3d – termomagnetic. vypín. jedn.",0.04]
["GV2P05","ISTENÝ MOT. SPÚŠŤAČ 0,63-1A >50KA",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3389110213447",{"v":4.8,"d":"4.80"},{"v":9.3,"d":"9.30"},{"v":10,"d":"10.00"},{"v":264,"d":"264.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GV2P05","motor. istič GV2-P – 0,63 - 1 A – 3 3d – termomagnetic. vypín. jedn.",0.03]
["GV2ME22","ISTENÝ MOT. SPÚŠŤAČ 20-25A",1,"ks",{"v":85.5595125,"d":"85.560"},"3389110343250",{"v":9.5,"d":"9.50"},{"v":4.5,"d":"4.50"},{"v":8.5,"d":"8.50"},{"v":287,"d":"287.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GV2ME22","motor. istič GV2-ME – 3 póly 3d – 20 - 25 A – termomagnetic. vypín. jedn.",0.03]
["GV2ME10K1BW3","KOMBINÁCIA GV2ME + LP4K 6,3A 24VDC",1,"ks",{"v":100.65825,"d":"100.658"},"3389110948714",{"v":15.8,"d":"15.80"},{"v":5,"d":"5.00"},{"v":8.5,"d":"8.50"},{"v":518,"d":"518.00"},"FR","8537109899","https://www.se.com/sk/sk/product/GV2ME10K1BW3","DOL combination starter,TeSys Deca Frame 2,GV2ME10 and LC1K06,4-6.3A,110V AC",0.06]
["GV2ME08TQ","TeSys MOTOR CIRCUIT BREAKER",24,"ks",{"v":75.951225,"d":"75.951"},"3389110343106",{"v":40,"d":"40.00"},{"v":15,"d":"15.00"},{"v":30,"d":"30.00"},{"v":259,"d":"259.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GV2ME08TQ","Motor circuit breaker,TeSys Deca frame 2,3P,2.5-4A,thermal magnetic,push button,screw clamp terminals,bulk qty",0]
["GV2ME063","IST. MOT. SPÚŠŤAČ 1-1,6A PR. SVORKY",1,"ks",{"v":70.9183125,"d":"70.918"},"3389110346411",{"v":8.5,"d":"8.50"},{"v":5.5,"d":"5.50"},{"v":11,"d":"11.00"},{"v":284.9,"d":"284.90"},"FR","8536201090","https://www.se.com/sk/sk/product/GV2ME063","motor. istič GV2-ME – 3 póly 3d – 1 - 1,6 A – termomagnetic. vypín. jedn.",0.03]
["GV2ME05","ISTENÝ MOT. SPÚŠŤAČ 0,63-1A",1,"ks",{"v":67.71555,"d":"67.716"},"3389110343038",{"v":9.5,"d":"9.50"},{"v":4.5,"d":"4.50"},{"v":8.5,"d":"8.50"},{"v":231,"d":"231.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GV2ME05","motor. istič GV2-ME – 3 póly 3d – 0,63 - 1 A – termomagnetic. vypín. jedn.",0.03]
["GV2LE20","ISTENÝ MOT. SPÚŠŤAČ 18A",1,"ks",109.809,"3389110517019",{"v":4.6,"d":"4.60"},{"v":8.5,"d":"8.50"},{"v":9.3,"d":"9.30"},{"v":279,"d":"279.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GV2LE20","motor. istič GV2-LE – 18 A – 3 póly 3d – magnetická vypínacia jednotka",0.03]
["GV2LE05","ISTENÝ MOT. SPÚŠŤAČ 1A",1,"ks",{"v":82.35674999999999,"d":"82.357"},"3389110516890",{"v":5,"d":"5.00"},{"v":8.5,"d":"8.50"},{"v":9.2,"d":"9.20"},{"v":224,"d":"224.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GV2LE05","TeSys GV2 - motorový istič so skratovou ochranou. - 1 A - skrut. svorky",0.03]
["GV2K031","HLAVICA PRE GV2",1,"ks",{"v":36.602999999999994,"d":"36.603"},"3389110733471",{"v":9,"d":"9.00"},{"v":6.5,"d":"6.50"},{"v":8.5,"d":"8.50"},{"v":115,"d":"115.00"},"CZ","8538909999","https://www.se.com/sk/sk/product/GV2K031","hlava tlačidla Ø 40 mm – otočte pre uvoľnenie – Ø 22 – červená",0]
["GV2DM114BD","KOMBINÁCIA GV2ME+LC1D 6A 24V DC",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110817324",{"v":5.4,"d":"5.40"},{"v":10.5,"d":"10.50"},{"v":19.6,"d":"19.60"},{"v":600,"d":"600.00"},"FR","8537109899","https://www.se.com/sk/sk/product/GV2DM114BD","kombinovaný spúštač - TeSys GV2-DM - 6...10 A - 24 V AC",0.07]
["GV2AF4","PREP. BLOK PRE GV2M+LC1D09-38 S LAD31",1,"ks",{"v":5.17017375,"d":"5.170"},"3389110569100",{"v":7.5,"d":"7.50"},{"v":4,"d":"4.00"},{"v":4.5,"d":"4.50"},{"v":18,"d":"18.00"},"FR","8536909500","https://www.se.com/sk/sk/product/GV2AF4","pripojovacia svorka – GV2 namontovaná na LAD-311 so stýkačom LC1-D09 - D38",0]
["GS2V3","POISTKOVÝ ODPÍNAČ 3P 1250A",1,"ks",{"v":3157.0087499999995,"d":"3157.009"},"3389119410762",{"v":80,"d":"80.00"},{"v":51,"d":"51.00"},{"v":60,"d":"60.00"},{"v":40960,"d":"40,960.00"},"FR","8536508090","https://www.se.com/sk/sk/product/GS2V3","telo poistkového odpínača TeSys GS2V - 3P - 1250A - DIN 4",4.92]
["GS2LLG4","FUSE DISCONNECT SWITCH 4X 160A 00",1,"ks",{"v":645.1278749999999,"d":"645.128"},"3389119411042",{"v":21,"d":"21.00"},{"v":15.5,"d":"15.50"},{"v":17,"d":"17.00"},{"v":2300,"d":"2,300.00"},"FR","8536508090","https://www.se.com/sk/sk/product/GS2LLG4","telo poistkového odpínačaTeSys GS2L - 4P - 160A - DIN 00",0.28]
["GS2K3","ODPÍNAČ S POISTKAMI 3X125A 22X58",1,"ks",{"v":269.94712499999997,"d":"269.947"},"3389119410694",{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":21,"d":"21.00"},{"v":1500,"d":"1,500.00"},"FR","8536508090","https://www.se.com/sk/sk/product/GS2K3","telo poistkového odpínačaTeSys GS2K - 3P - 125A - DIN 22x58 mm",0.22]
["GS2AP64","TERMINAL SHROUDS 4X 630-800A",1,"ks",{"v":105.23362499999999,"d":"105.234"},"3389119412209",{"v":23.4,"d":"23.40"},{"v":19.6,"d":"19.60"},{"v":15.5,"d":"15.50"},{"v":718,"d":"718.00"},"FR","8547200090","https://www.se.com/sk/sk/product/GS2AP64","TeSys GS kryt svoriek pre odpínač 630 až 800 A",0]
["GS2AH340","OVLÁDACIA PÁKA IP65 ČERVENÁ",1,"ks",{"v":70.46077499999998,"d":"70.461"},"3389119411783",{"v":22.5,"d":"22.50"},{"v":6.3,"d":"6.30"},{"v":16.8,"d":"16.80"},{"v":395,"d":"395.00"},"FR","3926909790","https://www.se.com/sk/sk/product/GS2AH340","červená vonkajšia rukoväť TeSys GS2 - pre odpínač - 100...400 A",0]
["GS2AE8","PREDLŽOVACI HRIADEĽ 320MM",1,"ks",{"v":26.079637499999997,"d":"26.080"},"3389119412001",{"v":36.8,"d":"36.80"},{"v":3.5,"d":"3.50"},{"v":5.6,"d":"5.60"},{"v":116,"d":"116.00"},"FR","7326909890","https://www.se.com/sk/sk/product/GS2AE8","TeSys GS nástavba pre hriadeľ pre odpínač 30 - 32 A 5x5 mm",0]
["GS2AE21","PREDLŽOVACÍ HRIADEĽ 400MM",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389119412049",{"v":40.2,"d":"40.20"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":312,"d":"312.00"},"FR","8538909999","https://www.se.com/sk/sk/product/GS2AE21","TeSys GS nástavba pre hriadeľ pre odpínač 50 - 400 A 10x10 mm",0]
["GS1DD4","FUSE SWITCH 4X32A 10X38",1,"ks",{"v":196.74112499999998,"d":"196.741"},"3389110120110",{"v":11.5,"d":"11.50"},{"v":9,"d":"9.00"},{"v":10.5,"d":"10.50"},{"v":490,"d":"490.00"},"FR","8536508090","https://www.se.com/sk/sk/product/GS1DD4","Switch disconnector fuse, TeSys GS, 3P + N, 4NO, 32A, fuse type NFC, size 10x38mm",0.06]
["GS1AP44","KRYT SVORIEK",1,"ks",{"v":30.288982499999996,"d":"30.289"},"3389110561999",{"v":17.5,"d":"17.50"},{"v":15,"d":"15.00"},{"v":7,"d":"7.00"},{"v":216,"d":"216.00"},"FR","8538909999","https://www.se.com/sk/sk/product/GS1AP44","Terminal shrouds, TeSys GS, 4P, for switches 160 to 400A",""]
["GK1AP08","RUKOVÄŤ ODPOJOVAČA ĽAVÁ STRANA",1,"ks",{"v":46.2112875,"d":"46.211"},"3389110787818",{"v":15.7,"d":"15.70"},{"v":6.5,"d":"6.50"},{"v":7.6,"d":"7.60"},{"v":248,"d":"248.00"},"FR","8538909999","https://www.se.com/sk/sk/product/GK1AP08","TeSys držiak poistky - otočná rukoväť na ľavú stranu GK1 - pre 125 A",0]
["GC2540M5","INŠTAL. STÝKAČ 25A, 4ZAP, 220/240V",1,"ks",{"v":39.80576249999999,"d":"39.806"},"3389110641523",{"v":8,"d":"8.00"},{"v":9,"d":"9.00"},{"v":23,"d":"23.00"},{"v":203,"d":"203.00"},"FR","8536490099","https://www.se.com/sk/sk/product/GC2540M5","inštalačný stýkač 25A 4Z - cievka 220...240V 50Hz",0.03]
["GC2510M5","INŠTAL. STÝKAČ 25A, 1ZAP, 220/240V",1,"ks",{"v":35.23038749999999,"d":"35.230"},"3389110641394",{"v":23,"d":"23.00"},{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":109,"d":"109.00"},"FR","8536490099","https://www.se.com/sk/sk/product/GC2510M5","inštalačný stýkač 25A 1Z - cievka 220...240V 50Hz",0.01]
["GC10040M5","INŠTAL. STÝKAČ 100A, 4ZAP, 220/240V",1,"ks",{"v":544.469625,"d":"544.470"},"3389110707731",{"v":9,"d":"9.00"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},{"v":654,"d":"654.00"},"FR","8536490099","https://www.se.com/sk/sk/product/GC10040M5","inštalačný stýkač 100A 4Z - cievka 220...240V 50Hz",0.08]
["GBY080008K","UHLOVÁ PREVODOVKA 80MM, I=8",1,"ks",{"v":1237.0049999999999,"d":"1237.005"},"3606480388743",{"v":20.5,"d":"20.50"},{"v":10,"d":"10.00"},{"v":11,"d":"11.00"},{"v":3628,"d":"3,628.00"},"DE","8483405190","https://www.se.com/sk/sk/product/GBY080008K","angular gearbox straight teeth GBY, Lexium, 80mm, reduction 8:1, 13arc.min, 50N.m",0]
["GBX120040K","PRIAMA PREVODOVKA 120MM, i=40",1,"ks",{"v":1767.1499999999999,"d":"1767.150"},"3606480388545",{"v":13,"d":"13.00"},{"v":21,"d":"21.00"},{"v":13,"d":"13.00"},{"v":7207,"d":"7,207.00"},"DE","8483405190","https://www.se.com/sk/sk/product/GBX120040K","gearbox straight teeth GBX, Lexium, 120mm, reduction 40:1 , 9arc.min, 230N.m",0]
["GBX080005K","PRIAMA PREVODOVKA 80MM, i=5",1,"ks",{"v":783.4365,"d":"783.437"},"3606480388330",{"v":11,"d":"11.00"},{"v":16.2,"d":"16.20"},{"v":10.8,"d":"10.80"},{"v":1934,"d":"1,934.00"},"DE","8483405190","https://www.se.com/sk/sk/product/GBX080005K","gearbox straight teeth GBX, Lexium, 80mm, reduction 5:1 , 7arc.min, 110N.m",0]
["GBX080004K","PRIAMA PREVODOVKA 80MM, i=4",1,"ks",{"v":783.4365,"d":"783.437"},"3606480388323",{"v":17,"d":"17.00"},{"v":10.5,"d":"10.50"},{"v":11,"d":"11.00"},{"v":1930,"d":"1,930.00"},"DE","8483405190","https://www.se.com/sk/sk/product/GBX080004K","gearbox straight teeth GBX, Lexium, 80mm, reduction 4:1 , 7arc.min, 115N.m",0]
["GBX060004K","PRIAMA PREVODOVKA 60MM, i=4",1,"ks",612.612,"3606480388194",{"v":13.5,"d":"13.50"},{"v":6.8,"d":"6.80"},{"v":6.8,"d":"6.80"},{"v":825,"d":"825.00"},"DE","8483405190","https://www.se.com/sk/sk/product/GBX060004K","gearbox straight teeth GBX, Lexium, 60mm, reduction 4:1 , 10arc.min, 38N.m",0]
["GBK0400573S","ADAPTAČNÁ PRÍRUBA VEĽ. 40",1,"ks",{"v":359.3205,"d":"359.321"},"3606480397714",{"v":17.6,"d":"17.60"},{"v":7.7,"d":"7.70"},{"v":15.8,"d":"15.80"},{"v":208,"d":"208.00"},"DE","85030099","https://www.se.com/sk/sk/product/GBK0400573S","adaptation kit, Lexium SD3, size 40, 15mm, for assembly motor and gearbox",0]
["GB2DB05","ISTIČ 2P, 0,5A",1,"ks",{"v":67.71555,"d":"67.716"},"3389110865400",{"v":9.7,"d":"9.70"},{"v":8,"d":"8.00"},{"v":8.5,"d":"8.50"},{"v":103,"d":"103.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GB2DB05","TeSys GB2 termo-magnetický istič - 2P - 0.5 A - Id = 6.6 A",0]
["GB2CD06","ISTIČ 1P+N, 1A",1,"ks",{"v":58.10726249999999,"d":"58.107"},"3389110214727",{"v":7.5,"d":"7.50"},{"v":1.5,"d":"1.50"},{"v":7,"d":"7.00"},{"v":60,"d":"60.00"},"FR","8536201090","https://www.se.com/sk/sk/product/GB2CD06","TeSys GB2 termo-magnetický istič - 1P + N - 1 A - Id = 14 A",0.01]
["GB2CB06","ISTIČ 1P, 1A",1,"ks",{"v":31.112549999999995,"d":"31.113"},"3389110214666",{"v":7.4,"d":"7.40"},{"v":1.5,"d":"1.50"},{"v":6.9,"d":"6.90"},{"v":50.9,"d":"50.90"},"FR","8536201090","https://www.se.com/sk/sk/product/GB2CB06","TeSys GB2 termo-magnetický istič - 1P - 1 A - Id = 14 A",0.01]
["FAS-06","Kryt pre SE8000 drevo hnedé",1,"ks",{"v":43.115625,"d":"43.116"},"3606489420956",{"v":11,"d":"11.00"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":12,"d":"12.00"},"CA","9032900090","https://www.se.com/sk/sk/product/FAS-06","kryt pre SE8000 drevo hnedé",0]
["EZ9EUC108","EASY9 EU nástenná 8M dymové dvere",1,"ks",{"v":12.347999999999997,"d":"12.348"},"3606486370056",{"v":22,"d":"22.00"},{"v":10,"d":"10.00"},{"v":17,"d":"17.00"},{"v":690,"d":"690.00"},"IT","8538100000","https://www.se.com/sk/sk/product/EZ9EUC108","EASY9 EU nástenná rozvodnica 8M dymové dvere",0]
["EVP1CNL32122","príslušenstvo - nabíjací kabel EVlink 32",1,"ks",{"v":548.218125,"d":"548.218"},"3606481290595",{"v":35.5,"d":"35.50"},{"v":10,"d":"10.00"},{"v":31.5,"d":"31.50"},{"v":3058,"d":"3,058.00"},"DE","8544429090","https://www.se.com/sk/sk/product/EVP1CNL32122","EVlink príslušenstvo - nabíjecí kábel 7m - 32A 1fáz. T2-T2 IEC",0.37]
["EVH4S03NC","EVlink Home 1P integ. kábel 5m, 3.7kW 16",1,"ks",994.014,"3606482107335",{"v":49,"d":"49.00"},{"v":33.1,"d":"33.10"},{"v":39.5,"d":"39.50"},{"v":6913,"d":"6,913.00"},"CN","8537109899","https://www.se.com/sk/sk/product/EVH4S03NC","nabíjacia stanica EVlink Home 1P integrovaný kábel 5m, 3.7kW 16A filter na RCD-DD",0]
["EVB3S22N4A","nabíjacia stanica EVlink Pre AC/AC Metal",1,"ks",{"v":0,"d":"0.000"},"3606482213180",{"v":67,"d":"67.00"},{"v":29,"d":"29.00"},{"v":36,"d":"36.00"},{"v":8598,"d":"8,598.00"},"FR","8537109899","https://www.se.com/sk/sk/product/EVB3S22N4A","nabíjacia stanica EVlink Pro AC/AC Metal, 22kW, 32A, 3P+N, T2S, RDC-DD 6mA, RCD Asi 30mA, cievka MNx",1.05]
["EVB3S07N4A","nabíjacia stanica EVlink Pre AC/AC Metal",1,"ks",{"v":0,"d":"0.000"},"3606482213043",{"v":57.5,"d":"57.50"},{"v":28.5,"d":"28.50"},{"v":35.5,"d":"35.50"},{"v":8530,"d":"8,530.00"},"FR","8537109899","https://www.se.com/sk/sk/product/EVB3S07N4A","nabíjacia stanica EVlink Pro AC/AC Metal, 7.4kW, 32A, 1P+N, T2S, RDC-DD 6mA, RCD Asi 30mA, cievka MNx",1.02]
["EVA1PBS1","stĺpik pre samostatne stojacu montáž 1 E",1,"ks",{"v":0,"d":"0.000"},"3606482185517",{"v":135,"d":"135.00"},{"v":29,"d":"29.00"},{"v":32,"d":"32.00"},{"v":10300,"d":"10,300.00"},"SK","7616999099","https://www.se.com/sk/sk/product/EVA1PBS1","stĺpik EVlink Pro AC pre 1 nabíjaciu stanicu",0]
["ETK41925","1M/MINI KANÁL+KRYT 1K 40X25 2M LEP ULTRA",1,"M",{"v":1.7125289999999993,"d":"1.713"},"8690495072396",{"v":200,"d":"200.00"},{"v":2.6,"d":"2.60"},{"v":4,"d":"4.00"},{"v":275,"d":"275.00"},"TR","3925902000","https://www.se.com/sk/sk/product/ETK41925","Mini kanál, Ultra, 40x25, samolepiaci, PVC, biela, 2 m",0]
["ETK30330","1M/MINI KANÁL+KRYT 1K 30x30 2M ULTRA",88,"M",{"v":1.3612409999999997,"d":"1.361"},"8698150303304",{"v":200,"d":"200.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":249.5,"d":"249.50"},"TR","3925902000","https://www.se.com/sk/sk/product/ETK30330","Mini kanál, Ultra, 30x30, PVC, biela, 2 m",0]
["ETK25316","1M/MINI KANÁL+KRYT 1K 25x16 2M ULTRA",104,"M",{"v":0.8782199999999998,"d":"0.878"},"8698150253166",{"v":201,"d":"201.00"},{"v":1.5,"d":"1.50"},{"v":2.5,"d":"2.50"},{"v":320.933,"d":"320.93"},"TR","3925902000","https://www.se.com/sk/sk/product/ETK25316","Mini kanál, Ultra, 25x16, PVC, biela, 2 m",0]
["ETK16316","1M/MINI KANÁL+KRYT 1K 16x16 2M ULTRA",132,"M",{"v":0.7025759999999999,"d":"0.703"},"8698150163168",{"v":200,"d":"200.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":247.417,"d":"247.42"},"TR","3925902000","https://www.se.com/sk/sk/product/ETK16316","Mini kanál, Ultra, 16x16, PVC, biela, 2 m",0]
["ETK10151E","T-DIEL PRE IK 1K 101x34/50 ULTRA",5,"ks",{"v":2.2394609999999995,"d":"2.239"},"8690495055207",{"v":17,"d":"17.00"},{"v":5.5,"d":"5.50"},{"v":14,"d":"14.00"},{"v":70,"d":"70.00"},"TR","3925902000","https://www.se.com/sk/sk/product/ETK10151E","T Kus, Ultra, 101x34/50, biela",0]
["ETK10134E","1M/INŠT.KANÁL+KRYT 1K 101x34 2M ULTRA",24,"M",{"v":5.532785999999999,"d":"5.533"},"8690495056457",{"v":200,"d":"200.00"},{"v":4,"d":"4.00"},{"v":10,"d":"10.00"},{"v":941,"d":"941.00"},"TR","3925902000","https://www.se.com/sk/sk/product/ETK10134E","Instalačný kanál vrátane veka, Ultra, 101x34, biela, 2m",0]
["EPH9700121","ZÁSUVKA 2x2P BEZ UZEMN.16A ASFORA BIELA",1,"ks",{"v":4.171544999999998,"d":"4.172"},"3606480527616",{"v":12.5,"d":"12.50"},{"v":4.5,"d":"4.50"},{"v":8,"d":"8.00"},{"v":92.3,"d":"92.30"},"TR","8536699099","https://www.se.com/sk/sk/product/EPH9700121","Zásuvka 2x2P, Asfora, 16A, Biela",0]
["EPH5810361","KRYCÍ RÁMCEK 3-NÁS. VERT. ALU",1,"ks",{"v":3.337235999999999,"d":"3.337"},"3606480729010",{"v":26.5,"d":"26.50"},{"v":1,"d":"1.00"},{"v":11,"d":"11.00"},{"v":33,"d":"33.00"},"TR","3925901000","https://www.se.com/sk/sk/product/EPH5810361","Krycí rámček, Asfora, trojnásobný vertikálny, Aluminium",0]
["EPH5800661","KRYCÍ RÁMCEK 6-NÁS. ALU",1,"ks",{"v":7.113581999999997,"d":"7.114"},"3606480728990",{"v":44,"d":"44.00"},{"v":1,"d":"1.00"},{"v":8.5,"d":"8.50"},{"v":54,"d":"54.00"},"TR","3925901000","https://www.se.com/sk/sk/product/EPH5800661","Krycí rámček, Asfora, šestinásobný, Aluminium",0]
["EPH5800221","KRYCÍ RÁMČEK 2-NÁS. ASFORA BIELA",1,"ks",{"v":1.1416859999999998,"d":"1.142"},"3606480527180",{"v":15.5,"d":"15.50"},{"v":1,"d":"1.00"},{"v":8,"d":"8.00"},{"v":19,"d":"19.00"},"TR","3925901000","https://www.se.com/sk/sk/product/EPH5800221","Krycí rámček, Asfora, dvojnásobný, Biela",0]
["EPH5700171","ZÁSUVKA REPRODUKT. 2-NÁS. ANTRACIT",1,"ks",{"v":11.416859999999996,"d":"11.417"},"3606480729911",{"v":7,"d":"7.00"},{"v":4,"d":"4.00"},{"v":7,"d":"7.00"},{"v":57.4,"d":"57.40"},"TR","8536699099","https://www.se.com/sk/sk/product/EPH5700171","Zásuvka, Asfora, reproduktorová dvojitá, Antracit",0]
["EPH4800121","ZÁSUVKA DÁT. 2xRJ45 6 UTP ASFORA BIELA",1,"ks",{"v":11.416859999999996,"d":"11.417"},"3606480527036",{"v":8,"d":"8.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":70.5,"d":"70.50"},"TR","8536699099","https://www.se.com/sk/sk/product/EPH4800121","Zásuvka dátová 2xRJ45, Asfora, 6 UTP, Biela",0]
["EPH4400161","ZÁSUVKA DÁT. 2xRJ45 5E UTP ALU",1,"ks",{"v":10.099529999999996,"d":"10.100"},"3606480728891",{"v":7,"d":"7.00"},{"v":4,"d":"4.00"},{"v":7,"d":"7.00"},{"v":61.2,"d":"61.20"},"TR","8536699099","https://www.se.com/sk/sk/product/EPH4400161","Zásuvka dátová 2xRJ45, Asfora, 5e UTP, Aluminium",0]
["EPH3700161","ZÁSUVKA ANT. SAT KONC.1dB BIELA",1,"ks",{"v":6.059717999999998,"d":"6.060"},"3606480728723",{"v":7.2,"d":"7.20"},{"v":4.5,"d":"4.50"},{"v":7.2,"d":"7.20"},{"v":74,"d":"74.00"},"TR","8536699099","https://www.se.com/sk/sk/product/EPH3700161","Zásuvka SAT, Asfora, koncová, 1db, Aluminium",0]
["EPH3300271","ZÁSUVKA ANT. TV-R PRIE.4dB ANTRACIT",1,"ks",{"v":11.416859999999996,"d":"11.417"},"3606480729614",{"v":5,"d":"5.00"},{"v":16,"d":"16.00"},{"v":11,"d":"11.00"},{"v":105,"d":"105.00"},"TR","8536691000","https://www.se.com/sk/sk/product/EPH3300271","Zásuvka TV-R, Asfora, priebežná, 4db, Antracit",0]
["EPH3200223","ZÁSUVKA ANT. TV PRIE.4dB ASFORA KRÉMOVÁ",1,"ks",{"v":5.752340999999998,"d":"5.752"},"3606480611698",{"v":8,"d":"8.00"},{"v":4.5,"d":"4.50"},{"v":8,"d":"8.00"},{"v":80,"d":"80.00"},"TR","8536691000","https://www.se.com/sk/sk/product/EPH3200223","Zásuvka TV, Asfora, priebežná, 4db, Krémová",0]
["EPH2900121","ZÁSUVKA 1x2P+SE 16A ASFORA BIELA",1,"ks",{"v":3.337235999999999,"d":"3.337"},"3606480526084",{"v":8.5,"d":"8.50"},{"v":4,"d":"4.00"},{"v":8.5,"d":"8.50"},{"v":79.3,"d":"79.30"},"TR","8536699099","https://www.se.com/sk/sk/product/EPH2900121","Zásuvka SCHUKO 2P+SE, Asfora, 16A, Biela",0]
["EPH2800371","ZÁSUVKA 1x2P+PE 16A CL IP44 ANTRACIT",1,"ks",{"v":7.728335999999999,"d":"7.728"},"3606480729966",{"v":8,"d":"8.00"},{"v":4.5,"d":"4.50"},{"v":8,"d":"8.00"},{"v":107.3,"d":"107.30"},"TR","8536699099","https://www.se.com/sk/sk/product/EPH2800371","Zásuvka 2P+PE, Asfora, 16A, clonky, IP44, Antracit",0]
["EPH2700421","USB rychlonabíjačka A+C, 3A, 45W, Biela",1,"ks",{"v":45.667439999999985,"d":"45.667"},"3606482079069",{"v":13,"d":"13.00"},{"v":6,"d":"6.00"},{"v":8.5,"d":"8.50"},{"v":137,"d":"137.00"},"CN","8504408390","https://www.se.com/sk/sk/product/EPH2700421","Asfora, USB charger A+C, 3A, 45W, with frame, white",0.02]
["EPH2700223","2xUSB nabíjecí konektor 2.1A, krémová",1,"ks",{"v":32.933249999999994,"d":"32.933"},"3606481142351",{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},{"v":8.5,"d":"8.50"},{"v":125,"d":"125.00"},"TR","8504408390","https://www.se.com/sk/sk/product/EPH2700223","2xUSB nabíjecí konektor, Asfora, 2.1A, Krémová",0.01]
["EPH1500321","PREPÍNAČ STRIEDAVÝ (6So) 10A ASFORA BIEL",1,"ks",{"v":4.566743999999999,"d":"4.567"},"3606480525704",{"v":8,"d":"8.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":80,"d":"80.00"},"TR","8536508090","https://www.se.com/sk/sk/product/EPH1500321","Prepínač striedavý (6So), Asfora, 10A, Biela",0]
["EPH0900121","TLAČIDLO SVETLO (1/0) 10A ASFORA BIELA",1,"ks",{"v":2.898125999999999,"d":"2.898"},"3606480525452",{"v":8,"d":"8.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":72,"d":"72.00"},"TR","8536508090","https://www.se.com/sk/sk/product/EPH0900121","Tlačidlo svetlo (1/0), Asfora, 10A, Biela",0]
["EPH0800123","TLAČIDLO ZVONČEK (1/0) 10A ASFORA KRÉM.",1,"ks",{"v":2.898125999999999,"d":"2.898"},"3606480525384",{"v":8.5,"d":"8.50"},{"v":4,"d":"4.00"},{"v":8.5,"d":"8.50"},{"v":76.8,"d":"76.80"},"TR","8536508090","https://www.se.com/sk/sk/product/EPH0800123","Tlačidlo zvonček (1/0), Asfora, 10A, krémová",0]
["EPH0500121","PREPÍNAČ KRÍŽOVÝ (7) 10A ASFORA BIELA",1,"ks",{"v":4.083723,"d":"4.084"},"3606480525216",{"v":8,"d":"8.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":74.8,"d":"74.80"},"TR","8536508090","https://www.se.com/sk/sk/product/EPH0500121","Prepínač krížový (7), Asfora, 10A, Biela",0]
["EPH0400321","PREPÍNAČ STRIEDAVÝ (6) 10A ASFORA BIELA",10,"ks",{"v":2.7663929999999994,"d":"2.766"},"3606480525100",{"v":8.5,"d":"8.50"},{"v":4,"d":"4.00"},{"v":8.5,"d":"8.50"},{"v":77.2,"d":"77.20"},"TR","8536508090","https://www.se.com/sk/sk/product/EPH0400321","Prepínač striedavý (6), Asfora, 10A, Biela",0]
["EPH0200121","SPÍNAČ 2-PÓLOVÝ (2) 10A ASFORA BIELA",1,"ks",{"v":3.9959009999999986,"d":"3.996"},"3606480524967",{"v":8,"d":"8.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":73.5,"d":"73.50"},"TR","8536508090","https://www.se.com/sk/sk/product/EPH0200121","Spínač dvojpólový (2), Asfora, 10A, Biela",0]
["ENN47963","DRŽIAK POTRUBIÍ P40-63MM + HMOŽ. B / 100",100,"ks",{"v":38.20256999999999,"d":"38.203"},"3295150479630",{"v":15,"d":"15.00"},{"v":35,"d":"35.00"},{"v":15,"d":"15.00"},{"v":8,"d":"8.00"},"HU","3926909790","https://www.se.com/sk/sk/product/ENN47963","Držiak potrubií, Mureva Fix, ø40-63mm + hmoždinka, Biela, 100ks",0]
["ENN47935","DRŽIAK POTRUBIÍ P16-32MM ČIERNA / 100KS",100,"ks",{"v":11.416859999999996,"d":"11.417"},"3295150479357",{"v":15.5,"d":"15.50"},{"v":9,"d":"9.00"},{"v":22.5,"d":"22.50"},3.75,"HU","3926909790","https://www.se.com/sk/sk/product/ENN47935","Držiak potrubií, Mureva Fix, ø16-32mm, čierna, 100ks",0]
["ENN05084","ROZVODNÁ SKRINKA 80x80x45",1,"ks",{"v":2.0199059999999993,"d":"2.020"},"3295150050846",{"v":8,"d":"8.00"},{"v":4.5,"d":"4.50"},{"v":8,"d":"8.00"},{"v":67,"d":"67.00"},"FR","8536909500","https://www.se.com/sk/sk/product/ENN05084","Krabica rozbočná, Mureva, 80x80x45, IP55, šedá, odlamovacie otvory",0]
["ENN05007","ROZVODNÁ SKRINKA 150x105x80",1,"ks",{"v":6.411005999999999,"d":"6.411"},"3295150050075",{"v":12,"d":"12.00"},{"v":6.2,"d":"6.20"},{"v":8.3,"d":"8.30"},{"v":317,"d":"317.00"},"HU","8536909500","https://www.se.com/sk/sk/product/ENN05007","Krabica rozbočná, Mureva, 150x105x80, IP55, šedá, priechodky",0]
["DZ5ME9","MATICA M6 DIN",100,"ks",{"v":0.6405524999999999,"d":"0.641"},"3389110569001",{"v":2.5,"d":"2.50"},{"v":1,"d":"1.00"},{"v":2,"d":"2.00"},{"v":9,"d":"9.00"},"FR","7318169990","https://www.se.com/sk/sk/product/DZ5ME9","matica M6 DIN - sada 100",0]
["DZ5CE060","KÁBLOVÁ KONCOVKA",100,"ks",{"v":0.059062500000000004,"d":"0.059"},"3389110537048",{"v":1.4,"d":"1.40"},{"v":0.4,"d":"0.40"},{"v":0.4,"d":"0.40"},{"v":1,"d":"1.00"},"FR","8536901000","https://www.se.com/sk/sk/product/DZ5CE060","Cable ends, Linergy TR cable ends, single conductor, 6mm², for un-insulated cable, medium size, 10 sets of 100",0]
["DZ5CE010L6","KÁBLOVÁ KONCOVKA ČERV. 1MM2",1000,"ks",{"v":0.059062500000000004,"d":"0.059"},"3389110536874",{"v":1.4,"d":"1.40"},{"v":0.4,"d":"0.40"},{"v":0.4,"d":"0.40"},{"v":0.1,"d":"0.10"},"FR","8536901000","https://www.se.com/sk/sk/product/DZ5CE010L6","káblová koncovka - krátka - 1 mm² - červená",0]
["DZ5CA253","KÁBLOVÁ KONCOVKA",100,"ks",{"v":0.23625000000000002,"d":"0.236"},"3389110535716",{"v":3.2,"d":"3.20"},{"v":1.2,"d":"1.20"},{"v":1.4,"d":"1.40"},{"v":1.3,"d":"1.30"},"FR","8536901000","https://www.se.com/sk/sk/product/DZ5CA253","káblová koncovka - stredná - 25 mm² - čierna",0]
["DZ5CA042","CABLE ENDS",1000,"ks",{"v":0.059062500000000004,"d":"0.059"},"3389110535679",{"v":1.4,"d":"1.40"},{"v":0.4,"d":"0.40"},{"v":0.4,"d":"0.40"},{"v":0.3,"d":"0.30"},"FR","8536901000","https://www.se.com/sk/sk/product/DZ5CA042","káblová koncovka - stredná - 4 mm² - oranžová",0]
["DPER16","Tepelné nadprúdové relé 9...13A",1,"ks",{"v":36.602999999999994,"d":"36.603"},"3606485332468",{"v":9,"d":"9.00"},{"v":5,"d":"5.00"},{"v":7.8,"d":"7.80"},{"v":144,"d":"144.00"},"FR","8536490099","https://www.se.com/sk/sk/product/DPER16","Tepelné nadprúdové relé 9...13A",0.02]
["DPER08","Tepelné nadprúdové relé 2.5...4A",1,"ks",{"v":33.857775,"d":"33.858"},"3606485332499",{"v":8.9,"d":"8.90"},{"v":4.8,"d":"4.80"},{"v":7.8,"d":"7.80"},{"v":140.9,"d":"140.90"},"FR","8536490099","https://www.se.com/sk/sk/product/DPER08","Tepelné nadprúdové relé 2.5...4A",0.02]
["DPE25G7","Stýkač DPE25 3P cievka 120V AC",1,"ks",{"v":59.0223375,"d":"59.022"},"3606481063229",{"v":11.938,"d":"11.94"},{"v":5.588,"d":"5.59"},{"v":9.652,"d":"9.65"},{"v":353.806,"d":"353.81"},"ID","8536490099","https://www.se.com/sk/sk/product/DPE25G7","Stýkač DPE25 3P cievka 120V AC",0.04]
["DPE09BL","Stýkač DPE09 3P cievka 24V DC",1,"ks",{"v":32.942699999999995,"d":"32.943"},"3606481064257",{"v":7.7,"d":"7.70"},{"v":9.5,"d":"9.50"},{"v":4.5,"d":"4.50"},{"v":320,"d":"320.00"},"ID","8536419089","https://www.se.com/sk/sk/product/DPE09BL","Stýkač DPE09 3P cievka 24V DC",0.04]
["DL1CS7220","NEÓNKA",10,"ks",{"v":8.418689999999998,"d":"8.419"},"3389110300826",{"v":10.5,"d":"10.50"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":2,"d":"2.00"},"FR","8539398090","https://www.se.com/sk/sk/product/DL1CS7220","Neon bulb, Harmony XB4, BA9s, orange, 220…230V AC",0]
["DL1CE024NSP","ŽIAROVKA 24V PAK 100",10,"ks",{"v":9.6082875,"d":"9.608"},"3389110745566",{"v":18.1,"d":"18.10"},{"v":5,"d":"5.00"},{"v":17,"d":"17.00"},{"v":2,"d":"2.00"},"FR","8539299890","https://www.se.com/sk/sk/product/DL1CE024NSP","Incandescent bulb, Harmony XB4, BA9s, clear, 6W, 24V AC/DC",0]
["DL1BKG4","PÄTICA S ČERVENOU LED 120V",1,"ks",{"v":73.66353749999999,"d":"73.664"},"3389110967623",{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":12,"d":"12.00"},"ID","8539520000","https://www.se.com/sk/sk/product/DL1BKG4","LED bulb, Harmony XVB, BA15d, red, flashing signaling type, 120V AC",0]
["DL1BDG6","LED PÄTICA BA15D 120V",1,"ks",{"v":69.5457,"d":"69.546"},"3389110118155",{"v":6,"d":"6.00"},{"v":3.5,"d":"3.50"},{"v":4.5,"d":"4.50"},{"v":12,"d":"12.00"},"ID","8539520000","https://www.se.com/sk/sk/product/DL1BDG6","LED bulb, Harmony XVB, BA 15d, blue, steady light, 120V AC",0]
["DL1BA160","ŽIAROVKA",10,"ks",{"v":10.065825,"d":"10.066"},"3389110300161",{"v":13,"d":"13.00"},{"v":5,"d":"5.00"},{"v":6.5,"d":"6.50"},{"v":8,"d":"8.00"},"FR","8539299290","https://www.se.com/sk/sk/product/DL1BA160","Incandescent bulb, Harmony XB4, BA15d, clear, steady light, 6W, 110…160V AC",0]
["DF2HN1251","POISTKA",3,"ks",45.738,"3389110503364",{"v":14.3,"d":"14.30"},{"v":7,"d":"7.00"},{"v":12.5,"d":"12.50"},{"v":398,"d":"398.00"},"FR","8536109090","https://www.se.com/sk/sk/product/DF2HN1251","nožová poistka - gG vel.1 - 250A - 500V - bez signalizácie",0]
["DF2EA25","POISTKA",10,"ks",{"v":6.6528,"d":"6.653"},"3389110502404",{"v":10.5,"d":"10.50"},{"v":1.5,"d":"1.50"},{"v":7.5,"d":"7.50"},{"v":18,"d":"18.00"},"TN","8536105090","https://www.se.com/sk/sk/product/DF2EA25","TeSys držiak poistky - poistka 14 x 51 mm - aM 25 A - bez signalizácie",0]
["DF2CA25","POISTKA",10,"ks",{"v":3.5343000000000004,"d":"3.534"},"3389110573428",{"v":8,"d":"8.00"},{"v":1.4,"d":"1.40"},{"v":5.4,"d":"5.40"},{"v":7,"d":"7.00"},"FR","8536105090","https://www.se.com/sk/sk/product/DF2CA25","TeSys držiak poistky - poistka 10 x 38 mm - aM 25 A - bez signalizácie",0]
["DF2BN1600","KONZULTOVAŤ-POISTKA 16A",10,"ks",{"v":4.937625000000001,"d":"4.938"},"3389110499445",{"v":7,"d":"7.00"},{"v":1.1,"d":"1.10"},{"v":4.6,"d":"4.60"},{"v":4,"d":"4.00"},"FR","8536105090","https://www.se.com/sk/sk/product/DF2BN1600","TeSys držiak poistky - poistka 8.5 x 31.5 mm - gG 16 A - bez signalizácie",0]
["DF22AM2","2 mikrospínace pre poistkové odpojovace",1,"ks",{"v":13.726125,"d":"13.726"},"3389119407571",{"v":10.5,"d":"10.50"},{"v":2,"d":"2.00"},{"v":3.3,"d":"3.30"},{"v":28,"d":"28.00"},"TN","8536508090","https://www.se.com/sk/sk/product/DF22AM2","TeSys držiak poistky - sig.kontakt - 2V - 5A - moment.",0]
["DF143NC","POIST. ODPOJ. 3P+N, 50A, 14X51",1,"ks",109.809,"3389119407427",{"v":17.3,"d":"17.30"},{"v":8.1,"d":"8.10"},{"v":12,"d":"12.00"},{"v":551,"d":"551.00"},"TN","8536303099","https://www.se.com/sk/sk/product/DF143NC","TeSys poistkový odpojovač 3P N 50A - veľkosť poistky 14 x 51 mm",0.07]
["DF103","POIST. ODPOJ. 3P, 32A, 10X38",1,"ks",{"v":32.485162499999994,"d":"32.485"},"3389119407243",{"v":8,"d":"8.00"},{"v":5.3,"d":"5.30"},{"v":6.2,"d":"6.20"},{"v":133,"d":"133.00"},"FR","8536303099","https://www.se.com/sk/sk/product/DF103","TeSys poistkový odpojovač 3P 32A - veľkosť poistky 10 x 38 mm",0.02]
["DA1TT140","PTC INTEGROVANÁ SONDA TROJITÁ 140oC",1,"ks",{"v":36.145462499999994,"d":"36.145"},"3389110531879",{"v":13,"d":"13.00"},{"v":2,"d":"2.00"},{"v":9,"d":"9.00"},{"v":10,"d":"10.00"},"FR","8533401000","https://www.se.com/sk/sk/product/DA1TT140","termistorová sonda PTC DA1 - T - trojitá sonda 140°C",0]
["DA1TS080","PTC POVRCHOVÁ SONDA 80oC",1,"ks",{"v":25.1645625,"d":"25.165"},"3389110531930",{"v":15,"d":"15.00"},{"v":2,"d":"2.00"},{"v":10,"d":"10.00"},{"v":8,"d":"8.00"},"FR","85389099","https://www.se.com/sk/sk/product/DA1TS080","termistorová sonda PTC DA1 - T - povrchová sonda 80°C",0]
["CP-LI-DP-TR-0600","CP diferenciálny tlak: 0-6 bar - Max.Tol",1,"ks",{"v":366.1875,"d":"366.188"},"3606482179349",{"v":18,"d":"18.00"},{"v":13.7,"d":"13.70"},{"v":5.1,"d":"5.10"},{"v":420,"d":"420.00"},"CN","9026202000","https://www.se.com/sk/sk/product/CP-LI-DP-TR-0600","CP diferenciálny tlakový prevodník kvapalín: 0-6 bar - Max tolerancia na jednom konci: 2 bar",""]
["CCT551011","ARGUS det. prítomn. Dual Tech, 1 kanál",1,"ks",{"v":120.00554999999999,"d":"120.006"},"3606480995521",{"v":17.7,"d":"17.70"},{"v":13.2,"d":"13.20"},{"v":11.7,"d":"11.70"},{"v":346,"d":"346.00"},"CN","8537109899","https://www.se.com/sk/sk/product/CCT551011","ARGUS Detektor prítomnosti Dual-Tech, 1 kanál",0.06]
["CCT16364","SPÍNACIE HODINY IH 24H BEZ ZÁLOHY 1KAN.",1,"ks",{"v":66.14999999999999,"d":"66.150"},"3606480179570",{"v":10.6,"d":"10.60"},{"v":6.8,"d":"6.80"},{"v":8,"d":"8.00"},{"v":201,"d":"201.00"},"DE","9107000090","https://www.se.com/sk/sk/product/CCT16364","Acti 9 - IH - mechanický časový spínač - 24 h - bez pamäti",0.02]
["CCT15441","IHP 1C w (24h/7d)",1,"ks",{"v":158.75999999999996,"d":"158.760"},"3606489524456",{"v":10.3,"d":"10.30"},{"v":7.8,"d":"7.80"},{"v":6.5,"d":"6.50"},{"v":159,"d":"159.00"},"DE","8536508090","https://www.se.com/sk/sk/product/CCT15441","Acti9 IHP 1C w (24h/7d) programmable time switch",0.02]
["CCT15225","IC Astro 1C SMART",1,"ks",{"v":145.52999999999997,"d":"145.530"},"3606489524548",{"v":10.4,"d":"10.40"},{"v":8,"d":"8.00"},{"v":6.7,"d":"6.70"},{"v":159,"d":"159.00"},"DE","9107000090","https://www.se.com/sk/sk/product/CCT15225","Acti9 IC Astro 1C SMART programmable twilight switch",0.02]
["CAD50BL","POMOCNÝ STÝKAČ 5Z, 24V LC",1,"ks",{"v":51.70173749999999,"d":"51.702"},"3389110406962",{"v":10.6,"d":"10.60"},{"v":5.1,"d":"5.10"},{"v":8.6,"d":"8.60"},{"v":531,"d":"531.00"},"FR","8536419089","https://www.se.com/sk/sk/product/CAD50BL","pomocný stýkač 5Z 690V- cievka so zníženým príkonom 24V DC",0.06]
["CAD32P7","POMOCNÝ STÝKAČ 3Z 2V, 230V AC",1,"ks",{"v":36.602999999999994,"d":"36.603"},"3389110401448",{"v":11,"d":"11.00"},{"v":5,"d":"5.00"},{"v":9,"d":"9.00"},{"v":356,"d":"356.00"},"FR","8536490099","https://www.se.com/sk/sk/product/CAD32P7","pomocný stýkač 3Z + 2V 690V- cievka 230V 50Hz",0.04]
["CAD323F7","POMOCNÝ STÝKAČ 3Z 2V, 110V AC PR. SVORKY",1,"ks",{"v":40.2633,"d":"40.263"},"3389110819564",{"v":12,"d":"12.00"},{"v":5.5,"d":"5.50"},{"v":10.5,"d":"10.50"},{"v":380,"d":"380.00"},"ID","8536490099","https://www.se.com/sk/sk/product/CAD323F7","TeSys D ovl relé - 3Z +2 V - <lt/> = 690 V - 110 V AC štandard . cievka",0]
["CA3KN31MD3","POMOCNÝ STÝKAČ",1,"ks",{"v":33.857775,"d":"33.858"},"3389110484373",{"v":6.6,"d":"6.60"},{"v":4.8,"d":"4.80"},{"v":6.2,"d":"6.20"},{"v":225,"d":"225.00"},"FR","8536490099","https://www.se.com/sk/sk/product/CA3KN31MD3","pomocný ministýkač 3Z + 1V 10A 690V- cievka 220V DC",0.03]
["CA3KN22JD","POMOCNÝ STÝKAČ",1,"ks",{"v":32.02762499999999,"d":"32.028"},"3389110483918",{"v":4.8,"d":"4.80"},{"v":6.5,"d":"6.50"},{"v":6.1,"d":"6.10"},{"v":218,"d":"218.00"},"FR","8536419089","https://www.se.com/sk/sk/product/CA3KN22JD","control relay, TeSys K, 4P(2NO+2NC), <lt/>=690V, 12V DC standard coil",0.03]
["CA2SK20P7","POMOCNÝ STÝKAČ",1,"ks",{"v":41.635912499999996,"d":"41.636"},"3389110564198",{"v":6.5,"d":"6.50"},{"v":3.5,"d":"3.50"},{"v":6,"d":"6.00"},{"v":122,"d":"122.00"},"CZ","8536490099","https://www.se.com/sk/sk/product/CA2SK20P7","pomocný ministýkač 2Z 10A 690V- cievka 230 V 50Hz",0.02]
["CA2SK11P7","POMOCNÝ STÝKAČ",1,"ks",{"v":41.635912499999996,"d":"41.636"},"3389110564105",{"v":6.5,"d":"6.50"},{"v":3.5,"d":"3.50"},{"v":6,"d":"6.00"},{"v":123.5,"d":"123.50"},"CZ","8536490099","https://www.se.com/sk/sk/product/CA2SK11P7","pomocný ministýkač 1Z + 1V 10A 690V- cievka 230V 50Hz",0.01]
["CA2KN22U7","POMOCNÝ STÝKAČ",1,"ks",{"v":26.537175,"d":"26.537"},"3389110481372",{"v":4.8,"d":"4.80"},{"v":6.5,"d":"6.50"},{"v":6.2,"d":"6.20"},{"v":177,"d":"177.00"},"FR","8536490099","https://www.se.com/sk/sk/product/CA2KN22U7","pomocný ministýkač 2Z + 2V 10A 690V- cievka 230...240V 50Hz",0.02]
["C6PWM","Jednotka spúští Micrologic 6.0P výs. manual, NS630b-1600, ochrana LSIG",1,"ks",1480.248,"3606482098428",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536309090","https://www.se.com/sk/sk/product/C6PWM","Jednotka spúští Micrologic 6.0P výs. manual, NS630b-1600, ochrana LSIG",0]
["C63W45E630","NSX630HB2 100kA AC 4P 630A 5.3E",1,"ks",{"v":3792.599999999999,"d":"3792.600"},"3606481989338",{"v":29.2,"d":"29.20"},{"v":15.2,"d":"15.20"},{"v":20.3,"d":"20.30"},{"v":8080,"d":"8,080.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C63W45E630","NSX630HB2 100kA AC 4P 630A 5.3E",0.97]
["C63V32D630","NSX630HB1 75kA AC 3P 630A 2.3",1,"ks",{"v":2249.0999999999995,"d":"2249.100"},"3606481988980",{"v":29.2,"d":"29.20"},{"v":15.2,"d":"15.20"},{"v":15.2,"d":"15.20"},{"v":5700,"d":"5,700.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C63V32D630","NSX630HB1 75kA AC 3P 630A 2.3",0.68]
["C63R31M500","NSX630R 200kA AC 3P 500A 1.3M",1,"ks",{"v":2028.5999999999997,"d":"2028.600"},"3606481988843",{"v":29.2,"d":"29.20"},{"v":15.2,"d":"15.20"},{"v":15.2,"d":"15.20"},{"v":5782,"d":"5,782.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C63R31M500","NSX630R 200kA AC 3P 500A 1.3M",0.6900000000000001]
["C63N34V570","NSX630N 50kA AC 3P3D 570A 4.3",1,"ks",{"v":2734.1999999999994,"d":"2734.200"},"3606481994127",{"v":14,"d":"14.00"},{"v":16.8,"d":"16.80"},{"v":25.5,"d":"25.50"},{"v":7500,"d":"7,500.00"},"JP","8536209090","https://www.se.com/sk/sk/product/C63N34V570","NSX630N 50kA AC 3P3D 570A 4.3",0.9]
["C63F4TM600D","NSX630F 36kA DC 4P 600A TMD",1,"ks",{"v":1984.4999999999995,"d":"1984.500"},"3606482003415",{"v":29,"d":"29.00"},{"v":15,"d":"15.00"},{"v":20,"d":"20.00"},{"v":7197,"d":"7,197.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C63F4TM600D","NSX630F 36kA DC 4P 600A TMD",0.86]
["C63F37E570","NSX630F 36kA AC 3P3D 570A 7.3E",1,"ks",{"v":2645.9999999999995,"d":"2646.000"},"3606481994639",{"v":14,"d":"14.00"},{"v":16.8,"d":"16.80"},{"v":25.5,"d":"25.50"},{"v":7500,"d":"7,500.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C63F37E570","NSX630F 36kA AC 3P3D 570A 7.3E",0.9]
["C6344A570","Jednotka spúští NSX630 AC 4P4D 570A 4.3A",1,"ks",{"v":1896.2999999999995,"d":"1896.300"},"3606481994301",{"v":24.9,"d":"24.90"},{"v":17.2,"d":"17.20"},{"v":21.2,"d":"21.20"},{"v":2371,"d":"2,371.00"},"JP","8536303099","https://www.se.com/sk/sk/product/C6344A570","Jednotka spúští NSX630 AC 4P4D 570A 4.3AL",0]
["C633630DS","Odpínač NSX630NA DC 3P 630A",1,"ks",{"v":1411.1999999999998,"d":"1411.200"},"3606482003521",{"v":29.1,"d":"29.10"},{"v":14.7,"d":"14.70"},{"v":20,"d":"20.00"},{"v":5350,"d":"5,350.00"},"FR","8536508090","https://www.se.com/sk/sk/product/C633630DS","Odpínač NSX630NA DC 3P 630A",0.64]
["C50WM","Jednotka spúští Micrologic 5.0 výs. manual, NS630b-1600, ochrana LSI",1,"ks",{"v":670.4775000000001,"d":"670.478"},"3606482186071",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536309090","https://www.se.com/sk/sk/product/C50WM","Jednotka spúští Micrologic 5.0 výs. manual, NS630b-1600, ochrana LSI",0]
["C40W36E400","NSX400HB2 100kA AC 3P 400A 6.3E",1,"ks",{"v":2822.3999999999996,"d":"2822.400"},"3606481989215",{"v":29.2,"d":"29.20"},{"v":15.2,"d":"15.20"},{"v":15.2,"d":"15.20"},{"v":5882,"d":"5,882.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C40W36E400","NSX400HB2 100kA AC 3P 400A 6.3E",0.71]
["C40S4TM400D","NSX400S 100kA DC 4P 400A TMD",1,"ks",{"v":1719.8999999999999,"d":"1719.900"},"3606482003446",{"v":29.1,"d":"29.10"},{"v":14.7,"d":"14.70"},{"v":20,"d":"20.00"},{"v":7321,"d":"7,321.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C40S4TM400D","NSX400S 100kA DC 4P 400A TMD",0.88]
["C40R31M320","NSX400R 200kA AC 3P 320A 1.3M",1,"ks",{"v":1631.7,"d":"1631.700"},"3606481988836",{"v":29.5,"d":"29.50"},{"v":15.5,"d":"15.50"},{"v":16.2,"d":"16.20"},{"v":5776,"d":"5,776.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C40R31M320","NSX400R 200kA AC 3P 320A 1.3M",0.6900000000000001]
["C40N42D250","NSX400N 50kA AC 4P4D 250A 2.3",1,"ks",{"v":1499.3999999999999,"d":"1499.400"},"3606482002746",{"v":29.5,"d":"29.50"},{"v":15,"d":"15.00"},{"v":20.5,"d":"20.50"},{"v":7393,"d":"7,393.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C40N42D250","NSX400N 50kA AC 4P4D 250A 2.3",0.89]
["C40H4","Základný istič NSX400H 70kA AC 4P 400A",1,"ks",{"v":1102.4999999999998,"d":"1102.500"},"3606482003170",{"v":29.2,"d":"29.20"},{"v":15.2,"d":"15.20"},{"v":20.1,"d":"20.10"},{"v":5888,"d":"5,888.00"},"IT","8536209090","https://www.se.com/sk/sk/product/C40H4","Základný istič NSX400H 70kA AC 4P 400A",0]
["C40H32M320","NSX400H 70kA AC 3P3D 320A 2.3M",1,"ks",{"v":1367.0999999999997,"d":"1367.100"},"3606482002821",{"v":31,"d":"31.00"},{"v":23.8,"d":"23.80"},{"v":16.5,"d":"16.50"},{"v":5680,"d":"5,680.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C40H32M320","NSX400H 70kA AC 3P3D 320A 2.3M",0.68]
["C40F3TM400D","NSX400F 36kA DC 3P 400A TMD",1,"ks",{"v":970.1999999999998,"d":"970.200"},"3606481995018",{"v":29.1,"d":"29.10"},{"v":14.7,"d":"14.70"},{"v":20,"d":"20.00"},{"v":5518,"d":"5,518.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C40F3TM400D","NSX400F 36kA DC 3P 400A TMD",0.66]
["C4042D400","Jednotka spúští NSX400 AC 4P4D 400A 2.3",1,"ks",{"v":639.4499999999999,"d":"639.450"},"3606482003262",{"v":20.5,"d":"20.50"},{"v":14,"d":"14.00"},{"v":17.5,"d":"17.50"},{"v":1770,"d":"1,770.00"},"FR","8536309090","https://www.se.com/sk/sk/product/C4042D400","Jednotka spúští NSX400 AC 4P4D 400A 2.3",0]
["C4037A400","Jednotka spúští NSX400 AC 3P3D 400A 7.3E",1,"ks",{"v":1631.7,"d":"1631.700"},"3606481994318",{"v":25,"d":"25.00"},{"v":17.2,"d":"17.20"},{"v":21.3,"d":"21.30"},{"v":1886,"d":"1,886.00"},"JP","8536309090","https://www.se.com/sk/sk/product/C4037A400","Jednotka spúští NSX400 AC 3P3D 400A 7.3E-AL",0]
["C2AWM","Jednotka spúští Micrologic 2.0A výs. manual, NS630b-1600, ochrana LI",1,"ks",{"v":610.1865,"d":"610.187"},"3606482098350",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536309090","https://www.se.com/sk/sk/product/C2AWM","Jednotka spúští Micrologic 2.0A výs. manual, NS630b-1600, ochrana LI",0]
["C25W42D160","NSX250HB2 100kA AC 4P 160A 2.2",1,"ks",{"v":1675.8,"d":"1675.800"},"3606482002395",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2630,"d":"2,630.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25W42D160","NSX250HB2 100kA AC 4P 160A 2.2",0.32]
["C25W36M150","NSX250HB2 100kA AC 3P3D 150A 6.2EM",1,"ks",{"v":1896.2999999999995,"d":"1896.300"},"3606482013704",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":11,"d":"11.00"},{"v":2120,"d":"2,120.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C25W36M150","NSX250HB2 100kA AC 3P3D 150A 6.2EM",0.25]
["C25V4TM160","NSX250HB1 75kA AC 4P 160A TMD",1,"ks",{"v":1411.1999999999998,"d":"1411.200"},"3606482001787",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2700,"d":"2,700.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25V4TM160","NSX250HB1 75kA AC 4P 160A TMD",0.32]
["C25V42D250","NSX250HB1 75kA AC 4P 250A 2.2",1,"ks",{"v":1543.4999999999998,"d":"1543.500"},"3606482001855",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2731,"d":"2,731.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25V42D250","NSX250HB1 75kA AC 4P 250A 2.2",0.33]
["C25V36E250","NSX250HB1 75kA AC 3P 250A 6.2E",1,"ks",{"v":1984.4999999999995,"d":"1984.500"},"3606482001718",{"v":20,"d":"20.00"},{"v":11,"d":"11.00"},{"v":14,"d":"14.00"},{"v":2110,"d":"2,110.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C25V36E250","NSX250HB1 75kA AC 3P 250A 6.2E",0.25]
["C25S4D","Základný istič NSX250S 100kA DC 4P 250A",1,"ks",{"v":599.7599999999999,"d":"599.760"},"3606481994868",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2165,"d":"2,165.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25S4D","Základný istič NSX250S 100kA DC 4P 250A",0]
["C25R45E160","NSX250R 200kA AC 4P 160A 5.2E",1,"ks",{"v":1940.3999999999996,"d":"1940.400"},"3606482001251",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2650,"d":"2,650.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C25R45E160","NSX250R 200kA AC 4P 160A 5.2E",0.32]
["C25R36E160","NSX250R 200kA AC 3P 160A 6.2E",1,"ks",{"v":1808.0999999999997,"d":"1808.100"},"3606482001060",{"v":20,"d":"20.00"},{"v":11,"d":"11.00"},{"v":14,"d":"14.00"},{"v":2110,"d":"2,110.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C25R36E160","NSX250R 200kA AC 3P 160A 6.2E",0.25]
["C25N44V250","NSX250N 50kA AC 4P4D 250A 4.2",1,"ks",{"v":1411.1999999999998,"d":"1411.200"},"3606481993656",{"v":19.4,"d":"19.40"},{"v":14.2,"d":"14.20"},{"v":15,"d":"15.00"},{"v":2776,"d":"2,776.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25N44V250","NSX250N 50kA AC 4P4D 250A 4.2",0.34]
["C25N44V160","NSX250N 50kA AC 4P4D 160A 4.2",1,"ks",{"v":1411.1999999999998,"d":"1411.200"},"3606481993649",{"v":14,"d":"14.00"},{"v":12,"d":"12.00"},{"v":16,"d":"16.00"},{"v":2780,"d":"2,780.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25N44V160","NSX250N 50kA AC 4P4D 160A 4.2",0.33]
["C25N32D160","NSX250N 50kA AC 3P3D 160A 2.2",1,"ks",{"v":736.4699999999999,"d":"736.470"},"3606481998088",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2028,"d":"2,028.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C25N32D160","NSX250N 50kA AC 3P3D 160A 2.2",0.24]
["C25H47E250","NSX250H 70kA AC 4P4D 250A 7.2E",1,"ks",{"v":2557.7999999999997,"d":"2557.800"},"3606481994561",{"v":14,"d":"14.00"},{"v":12,"d":"12.00"},{"v":16,"d":"16.00"},{"v":3100,"d":"3,100.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C25H47E250","NSX250H 70kA AC 4P4D 250A 7.2E",0.37]
["C25H3TM250","NSX250H 70kA AC 3P3D 250A TMD",1,"ks",{"v":829.0799999999999,"d":"829.080"},"3606481998583",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":11,"d":"11.00"},{"v":2004,"d":"2,004.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25H3TM250","NSX250H 70kA AC 3P3D 250A TMD",0.24]
["C25H32D100","NSX250H 70kA AC 3P3D 100A 2.2",1,"ks",{"v":696.78,"d":"696.780"},"3606481998637",{"v":20,"d":"20.00"},{"v":12,"d":"12.00"},{"v":14,"d":"14.00"},{"v":2048,"d":"2,048.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C25H32D100","NSX250H 70kA AC 3P3D 100A 2.2",0.25]
["C25F4TM160","NSX250F 36kA AC 4P4D 160A TMD",1,"ks",{"v":740.88,"d":"740.880"},"3606481997586",{"v":19,"d":"19.00"},{"v":15,"d":"15.00"},{"v":18,"d":"18.00"},{"v":2631,"d":"2,631.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25F4TM160","NSX250F 36kA AC 4P4D 160A TMD",0.32]
["C25F3TM200","NSX250F 36kA AC 3P3D 200A TMD",1,"ks",{"v":661.4999999999999,"d":"661.500"},"3606481997135",{"v":19,"d":"19.00"},{"v":11.5,"d":"11.50"},{"v":14,"d":"14.00"},{"v":2003,"d":"2,003.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25F3TM200","NSX250F 36kA AC 3P3D 200A TMD",0.24]
["C25B47E160","NSX250B 25kA AC 4P4D 160A 7.2E",1,"ks",{"v":1940.3999999999996,"d":"1940.400"},"3606481994363",{"v":14,"d":"14.00"},{"v":12,"d":"12.00"},{"v":16,"d":"16.00"},{"v":3100,"d":"3,100.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C25B47E160","NSX250B 25kA AC 4P4D 160A 7.2E",0.37]
["C25B3TM200","NSX250B 25kA AC 3P3D 200A TMD",1,"ks",{"v":604.17,"d":"604.170"},"3606481996275",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":11,"d":"11.00"},{"v":1946,"d":"1,946.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C25B3TM200","NSX250B 25kA AC 3P3D 200A TMD",0.24]
["C256TM160","Jednotka spúští NSX250 AC 4P3D 160A TMD",1,"ks",{"v":194.03999999999996,"d":"194.040"},"3606482000025",{"v":15,"d":"15.00"},{"v":6.5,"d":"6.50"},{"v":9.5,"d":"9.50"},{"v":494,"d":"494.00"},"PL","8536309090","https://www.se.com/sk/sk/product/C256TM160","Jednotka spúští NSX250 AC 4P3D 160A TMD",0]
["C2547E250","Jednotka spúští NSX250 AC 4P4D 250A 7.2E",1,"ks",{"v":1808.0999999999997,"d":"1808.100"},"3606481993915",{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":11,"d":"11.00"},{"v":795,"d":"795.00"},"CN","8536309090","https://www.se.com/sk/sk/product/C2547E250","Jednotka spúští NSX250 AC 4P4D 250A 7.2E",0]
["C253MG250D","Jednotka spúští NSX250 DC 3P3D 250A TMG",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3606481055354",{"v":10.5,"d":"10.50"},{"v":9,"d":"9.00"},{"v":6,"d":"6.00"},{"v":350,"d":"350.00"},"CN","8536309090","https://www.se.com/sk/sk/product/C253MG250D","Jednotka spúští NSX250 DC 3P3D 250A TMG",0]
["C2535E250","Jednotka spúští NSX250 AC 3P3D 250A 5.2E",1,"ks",{"v":970.1999999999998,"d":"970.200"},"3606481999696",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":11,"d":"11.00"},{"v":556,"d":"556.00"},"FR","8536309090","https://www.se.com/sk/sk/product/C2535E250","Jednotka spúští NSX250 AC 3P3D 250A 5.2E",0]
["C16S4D","Základný istič NSX160S 100kA DC 4P 160A",1,"ks",{"v":374.84999999999997,"d":"374.850"},"3606481994851",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2023.0000000000002,"d":"2,023.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C16S4D","Základný istič NSX160S 100kA DC 4P 160A",0]
["C16N6TM080","NSX160N 50kA AC 4P3D 80A TMD",1,"ks",{"v":489.50999999999993,"d":"489.510"},"3606481997951",{"v":20,"d":"20.00"},{"v":15,"d":"15.00"},{"v":15,"d":"15.00"},{"v":2385,"d":"2,385.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C16N6TM080","NSX160N 50kA AC 4P3D 80A TMD",0.29]
["C16N3TM125","NSX160N 50kA AC 3P3D 125A TMD",1,"ks",{"v":401.30999999999995,"d":"401.310"},"3606481997814",{"v":19.6,"d":"19.60"},{"v":14.2,"d":"14.20"},{"v":11.5,"d":"11.50"},{"v":1838,"d":"1,838.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C16N3TM125","NSX160N 50kA AC 3P3D 125A TMD",0.22]
["C16H6TM160","NSX160H 70kA AC 4P3D 160A TMD",1,"ks",{"v":661.4999999999999,"d":"661.500"},"3606481998774",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":14.5,"d":"14.50"},{"v":2376,"d":"2,376.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C16H6TM160","NSX160H 70kA AC 4P3D 160A TMD",0.29]
["C16H4TM160","NSX160H 70kA AC 4P4D 160A TMD",1,"ks",{"v":701.1899999999998,"d":"701.190"},"3606481999009",{"v":19,"d":"19.00"},{"v":15,"d":"15.00"},{"v":17,"d":"17.00"},{"v":2429,"d":"2,429.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C16H4TM160","NSX160H 70kA AC 4P4D 160A TMD",0.29]
["C16H32M150","NSX160H 70kA AC 3P3D 150A 2.2M",1,"ks",{"v":621.81,"d":"621.810"},"3606481999191",{"v":19,"d":"19.00"},{"v":12,"d":"12.00"},{"v":18,"d":"18.00"},{"v":1943,"d":"1,943.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C16H32M150","NSX160H 70kA AC 3P3D 150A 2.2M",0.23]
["C16F6TM100","NSX160F 36kA AC 4P3D 100A TMD",1,"ks",{"v":432.17999999999995,"d":"432.180"},"3606481997319",{"v":19,"d":"19.00"},{"v":15,"d":"15.00"},{"v":17,"d":"17.00"},{"v":2456,"d":"2,456.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C16F6TM100","NSX160F 36kA AC 4P3D 100A TMD",0.29]
["C16F3TM160","NSX160F 36kA AC 3P3D 160A TMD",1,"ks",{"v":423.3599999999999,"d":"423.360"},"3606481997104",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":11.5,"d":"11.50"},{"v":1830,"d":"1,830.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C16F3TM160","NSX160F 36kA AC 3P3D 160A TMD",0.22]
["C16F32D100","NSX160F 36kA AC 3P3D 100A 2.2",1,"ks",{"v":392.48999999999995,"d":"392.490"},"3606481997173",{"v":20,"d":"20.00"},{"v":12,"d":"12.00"},{"v":18,"d":"18.00"},{"v":1880,"d":"1,880.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C16F32D100","NSX160F 36kA AC 3P3D 100A 2.2",0.23]
["C16B4TM100","NSX160B 25kA AC 4P4D 100A TMD",1,"ks",{"v":405.7199999999999,"d":"405.720"},"3606481996541",{"v":19,"d":"19.00"},{"v":13.5,"d":"13.50"},{"v":14.5,"d":"14.50"},{"v":2257,"d":"2,257.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C16B4TM100","NSX160B 25kA AC 4P4D 100A TMD",0.29]
["C164TM125D","Jednotka spúští NSX160 DC 4P 125A TMD",1,"ks",{"v":119.07,"d":"119.070"},"3606481994950",{"v":15,"d":"15.00"},{"v":6.6,"d":"6.60"},{"v":9.5,"d":"9.50"},{"v":505,"d":"505.00"},"PL","8536303099","https://www.se.com/sk/sk/product/C164TM125D","Jednotka spúští NSX160 DC 4P 125A TMD",0]
["C164MG160","Jednotka spúští NSX160 AC 4P4D 160A TMG",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3606482000742",{"v":15,"d":"15.00"},{"v":7,"d":"7.00"},{"v":9.5,"d":"9.50"},{"v":502,"d":"502.00"},"CN","8536309090","https://www.se.com/sk/sk/product/C164MG160","Jednotka spúští NSX160 AC 4P4D 160A TMG",0]
["C163MG125","Jednotka spúští NSX160 AC 3P3D 125A TMG",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3606482000544",{"v":12,"d":"12.00"},{"v":16,"d":"16.00"},{"v":10,"d":"10.00"},{"v":475,"d":"475.00"},"CN","8536303099","https://www.se.com/sk/sk/product/C163MG125","Jednotka spúští NSX160 AC 3P3D 125A TMG",0]
["C160S3NAFM","Odpínač ComPacT NS1600NA 3P 1600A pev. manual, NA ",1,"ks",{"v":1527.0255,"d":"1527.026"},"3606482100718",{"v":60,"d":"60.00"},{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":13862,"d":"13,862.00"},"IT","8536508090","https://www.se.com/sk/sk/product/C160S3NAFM","Odpínač ComPacT NS1600NA 3P 1600A pev. manual, NA",1.6600000000000001]
["C160N42EFM","Kompaktný istič ComPacT NS1600N 50kA 4P 1600A pev. manual, 2.0E ",1,"ks",3515.589,"3606482098060",{"v":30,"d":"30.00"},{"v":30,"d":"30.00"},{"v":38,"d":"38.00"},{"v":17035,"d":"17,035.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C160N42EFM","Kompaktný istič ComPacT NS1600N 50kA 4P 1600A pev. manual, 2.0E",2.04]
["C160H460FM","Kompaktný istič ComPacT NS1600H 70kA 4P 1600A pev. manual, 6.0 ",1,"ks",{"v":3920.9939999999997,"d":"3920.994"},"3606482100404",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":16961,"d":"16,961.00"},"IT","8536209090","https://www.se.com/sk/sk/product/C160H460FM","Kompaktný istič ComPacT NS1600H 70kA 4P 1600A pev. manual, 6.0",2.04]
["C160H42AFM","Kompaktný istič ComPacT NS1600H 70kA 4P 1600A pev. manual, 2.0A ",1,"ks",{"v":3660.0795000000003,"d":"3660.080"},"3606482100763",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":17035,"d":"17,035.00"},"IT","8536209090","https://www.se.com/sk/sk/product/C160H42AFM","Kompaktný istič ComPacT NS1600H 70kA 4P 1600A pev. manual, 2.0A",2.04]
["C12N4TM125L","NSXm160N 50kA AC 4P4D 125A TMD ELINK",1,"ks",{"v":538.02,"d":"538.020"},"3606481991447",{"v":21.4,"d":"21.40"},{"v":12.4,"d":"12.40"},{"v":11.6,"d":"11.60"},{"v":1544,"d":"1,544.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C12N4TM125L","NSXm160N 50kA AC 4P4D 125A TMD ELINK",0.19]
["C12H44V160L","NSXm160H 70kA AC 4P 160A 4.1 ELINK",1,"ks",{"v":1102.4999999999998,"d":"1102.500"},"3606481993076",{"v":19,"d":"19.00"},{"v":15,"d":"15.00"},{"v":13,"d":"13.00"},{"v":1814,"d":"1,814.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C12H44V160L","NSXm160H 70kA AC 4P 160A 4.1 ELINK",0.22]
["C12F6TM160L","NSXm160F 36kA AC 4P3D 160A TMD ELINK",1,"ks",{"v":564.4799999999999,"d":"564.480"},"3606481990754",{"v":22,"d":"22.00"},{"v":12,"d":"12.00"},{"v":13,"d":"13.00"},{"v":1600,"d":"1,600.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C12F6TM160L","NSXm160F 36kA AC 4P3D 160A TMD ELINK",0.19]
["C12F34V160B","NSXm160F 36kA AC 3P 160A 4.1",1,"ks",{"v":926.0999999999998,"d":"926.100"},"3606481992796",{"v":19,"d":"19.00"},{"v":15,"d":"15.00"},{"v":14,"d":"14.00"},{"v":1572,"d":"1,572.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C12F34V160B","NSXm160F 36kA AC 3P 160A 4.1",0.19]
["C12B4TM125L","NSXm160B 25kA AC 4P4D 125A TMD ELINK",1,"ks",{"v":436.59,"d":"436.590"},"3606481990242",{"v":21,"d":"21.00"},{"v":12,"d":"12.00"},{"v":11.5,"d":"11.50"},{"v":1550,"d":"1,550.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C12B4TM125L","NSXm160B 25kA AC 4P4D 125A TMD ELINK",0.19]
["C125N4FM","Kompaktný istič ComPacT NS základný istič NS1250N 4P 1250 pev. manual ",1,"ks",{"v":1872.1395,"d":"1872.140"},"3606482098206",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C125N4FM","Kompaktný istič ComPacT NS základný istič NS1250N 4P 1250 pev. manual",0]
["C125N42AFM","Kompaktný istič ComPacT NS1250N 50kA 4P 1250A pev. manual, 2.0A ",1,"ks",2885.652,"3606482097957",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":16440,"d":"16,440.00"},"IT","8536209090","https://www.se.com/sk/sk/product/C125N42AFM","Kompaktný istič ComPacT NS1250N 50kA 4P 1250A pev. manual, 2.0A",1.97]
["C125H460FM","Kompaktný istič ComPacT NS1250H 70kA 4P 1250A pev. manual, 6.0 ",1,"ks",{"v":3292.0965,"d":"3292.097"},"3606482100398",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":16366,"d":"16,366.00"},"IT","8536209090","https://www.se.com/sk/sk/product/C125H460FM","Kompaktný istič ComPacT NS1250H 70kA 4P 1250A pev. manual, 6.0",1.96]
["C11N6TM080L","NSXm100N 50kA AC 4P3D 80A TMD ELINK",1,"ks",{"v":321.92999999999995,"d":"321.930"},"3606481991324",{"v":22,"d":"22.00"},{"v":12,"d":"12.00"},{"v":13,"d":"13.00"},{"v":1600,"d":"1,600.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C11N6TM080L","NSXm100N 50kA AC 4P3D 80A TMD ELINK",0.19]
["C11N6TM016B","NSXm100N 50kA AC 4P3D 16A TMD",1,"ks",{"v":273.41999999999996,"d":"273.420"},"3606481991560",{"v":22,"d":"22.00"},{"v":13,"d":"13.00"},{"v":12,"d":"12.00"},{"v":1600,"d":"1,600.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11N6TM016B","NSXm100N 50kA AC 4P3D 16A TMD",0.19]
["C11N4TM040L","NSXm100N 50kA AC 4P4D 40A TMD ELINK",1,"ks",{"v":317.5199999999999,"d":"317.520"},"3606481991393",{"v":22,"d":"22.00"},{"v":12,"d":"12.00"},{"v":12,"d":"12.00"},{"v":1600,"d":"1,600.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11N4TM040L","NSXm100N 50kA AC 4P4D 40A TMD ELINK",0.19]
["C11N4TM016B","NSXm100N 50kA AC 4P4D 16A TMD",1,"ks",{"v":299.87999999999994,"d":"299.880"},"3606481991669",{"v":22,"d":"22.00"},{"v":13,"d":"13.00"},{"v":12,"d":"12.00"},{"v":1600,"d":"1,600.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11N4TM016B","NSXm100N 50kA AC 4P4D 16A TMD",0.19]
["C11N3TM032L","NSXm100N 50kA AC 3P 32A TMD ELINK",1,"ks",{"v":202.85999999999996,"d":"202.860"},"3606481991188",{"v":21,"d":"21.00"},{"v":12,"d":"12.00"},{"v":9,"d":"9.00"},{"v":1208,"d":"1,208.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11N3TM032L","NSXm100N 50kA AC 3P 32A TMD ELINK",0.15]
["C11H6TM050L","NSXm100H 70kA AC 4P3D 50A TMD ELINK",1,"ks",{"v":321.92999999999995,"d":"321.930"},"3606481991904",{"v":22,"d":"22.00"},{"v":13,"d":"13.00"},{"v":12,"d":"12.00"},{"v":1600,"d":"1,600.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11H6TM050L","NSXm100H 70kA AC 4P3D 50A TMD ELINK",0.19]
["C11H6TM032B","NSXm100H 70kA AC 4P3D 32A TMD",1,"ks",{"v":304.28999999999996,"d":"304.290"},"3606481992185",{"v":22,"d":"22.00"},{"v":12,"d":"12.00"},{"v":12,"d":"12.00"},{"v":1600,"d":"1,600.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11H6TM032B","NSXm100H 70kA AC 4P3D 32A TMD",0.19]
["C11H4TM080B","NSXm100H 70kA AC 4P4D 80A TMD",1,"ks",{"v":392.48999999999995,"d":"392.490"},"3606481992321",{"v":22,"d":"22.00"},{"v":13,"d":"13.00"},{"v":12,"d":"12.00"},{"v":1600,"d":"1,600.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C11H4TM080B","NSXm100H 70kA AC 4P4D 80A TMD",0.19]
["C11H44V050L","NSXm100H 70kA AC 4P 50A 4.1 ELINK",1,"ks",{"v":798.2099999999999,"d":"798.210"},"3606481993052",{"v":14,"d":"14.00"},{"v":10,"d":"10.00"},{"v":11,"d":"11.00"},{"v":1200,"d":"1,200.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11H44V050L","NSXm100H 70kA AC 4P 50A 4.1 ELINK",0.14]
["C11H34V100L","NSXm100H 70kA AC 3P 100A 4.1 ELINK",1,"ks",{"v":745.2899999999998,"d":"745.290"},"3606481993021",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":1708,"d":"1,708.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C11H34V100L","NSXm100H 70kA AC 3P 100A 4.1 ELINK",0.2]
["C11H34V050B","NSXm100H 70kA AC 3P 50A 4.1",1,"ks",{"v":705.5999999999999,"d":"705.600"},"3606481993090",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":1600,"d":"1,600.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11H34V050B","NSXm100H 70kA AC 3P 50A 4.1",0.19]
["C11F4TM100L","NSXm100F 36kA AC 4P4D 100A TMD ELINK",1,"ks",{"v":317.5199999999999,"d":"317.520"},"3606481990839",{"v":21.2,"d":"21.20"},{"v":12,"d":"12.00"},{"v":11.5,"d":"11.50"},{"v":1548,"d":"1,548.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C11F4TM100L","NSXm100F 36kA AC 4P4D 100A TMD ELINK",0.19]
["C11F4TM025L","NSXm100F 36kA AC 4P4D 25A TMD ELINK",1,"ks",{"v":269.01,"d":"269.010"},"3606481990778",{"v":21,"d":"21.00"},{"v":12,"d":"12.00"},{"v":11.5,"d":"11.50"},{"v":1550,"d":"1,550.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11F4TM025L","NSXm100F 36kA AC 4P4D 25A TMD ELINK",0.19]
["C11F3TM100L","NSXm100F 36kA AC 3P 100A TMD ELINK",1,"ks",{"v":211.67999999999995,"d":"211.680"},"3606481990631",{"v":21,"d":"21.00"},{"v":12,"d":"12.00"},{"v":9,"d":"9.00"},{"v":1204,"d":"1,204.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C11F3TM100L","NSXm100F 36kA AC 3P 100A TMD ELINK",0.14]
["C11F3TM025B","NSXm100F 36kA AC 3P 25A TMD",1,"ks",{"v":180.80999999999997,"d":"180.810"},"3606481990877",{"v":8,"d":"8.00"},{"v":8.1,"d":"8.10"},{"v":13.7,"d":"13.70"},{"v":1150,"d":"1,150.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11F3TM025B","NSXm100F 36kA AC 3P 25A TMD",0.14]
["C11B6TM063L","NSXm100B 25kA AC 4P3D 63A TMD ELINK",1,"ks",{"v":233.72999999999996,"d":"233.730"},"3606481990112",{"v":21,"d":"21.00"},{"v":12,"d":"12.00"},{"v":11.5,"d":"11.50"},{"v":1528,"d":"1,528.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11B6TM063L","NSXm100B 25kA AC 4P3D 63A TMD ELINK",0.18]
["C11B6TM016L","NSXm100B 25kA AC 4P3D 16A TMD ELINK",1,"ks",{"v":220.49999999999994,"d":"220.500"},"3606481990068",{"v":22,"d":"22.00"},{"v":12,"d":"12.00"},{"v":13,"d":"13.00"},{"v":1626,"d":"1,626.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11B6TM016L","NSXm100B 25kA AC 4P3D 16A TMD ELINK",0.2]
["C11B4TM032L","NSXm100B 25kA AC 4P4D 32A TMD ELINK",1,"ks",{"v":242.54999999999995,"d":"242.550"},"3606481990181",{"v":21,"d":"21.00"},{"v":12,"d":"12.00"},{"v":11.5,"d":"11.50"},{"v":1554,"d":"1,554.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11B4TM032L","NSXm100B 25kA AC 4P4D 32A TMD ELINK",0.19]
["C11B44V025B","NSXm100B 25kA AC 4P 25A 4.1",1,"ks",{"v":705.5999999999999,"d":"705.600"},"3606481992642",{"v":19,"d":"19.00"},{"v":13,"d":"13.00"},{"v":16,"d":"16.00"},{"v":1765,"d":"1,765.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C11B44V025B","NSXm100B 25kA AC 4P 25A 4.1",0.21]
["C114100BS","Odpínač NSXm100NA AC 4P 100A",1,"ks",{"v":220.49999999999994,"d":"220.500"},"3606481995148",{"v":22,"d":"22.00"},{"v":13,"d":"13.00"},{"v":12,"d":"12.00"},{"v":1600,"d":"1,600.00"},"PL","8536508090","https://www.se.com/sk/sk/product/C114100BS","Odpínač NSXm100NA AC 4P 100A",0.19]
["C10W4TM100","NSX100HB2 100kA AC 4P 100A TMD",1,"ks",{"v":798.2099999999999,"d":"798.210"},"3606482002319",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2390,"d":"2,390.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C10W4TM100","NSX100HB2 100kA AC 4P 100A TMD",0.29]
["C10W3MA013","NSX100HB2 100kA AC 3P 12.5A MA",1,"ks",{"v":577.7099999999999,"d":"577.710"},"3606482002463",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":11,"d":"11.00"},{"v":1810,"d":"1,810.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10W3MA013","NSX100HB2 100kA AC 3P 12.5A MA",0.22]
["C10W35E040","NSX100HB2 100kA AC 3P 40A 5.2E",1,"ks",{"v":1234.7999999999997,"d":"1234.800"},"3606482002241",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":11,"d":"11.00"},{"v":1948,"d":"1,948.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10W35E040","NSX100HB2 100kA AC 3P 40A 5.2E",0.23]
["C10V42D100","NSX100HB1 75kA AC 4P 100A 2.2",1,"ks",{"v":793.7999999999998,"d":"793.800"},"3606482001824",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2420,"d":"2,420.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C10V42D100","NSX100HB1 75kA AC 4P 100A 2.2",0.29]
["C10V3MA100","NSX100HB1 75kA AC 3P 100A MA",1,"ks",{"v":502.73999999999995,"d":"502.740"},"3606482001992",{"v":19,"d":"19.00"},{"v":11,"d":"11.00"},{"v":14,"d":"14.00"},{"v":1841,"d":"1,841.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C10V3MA100","NSX100HB1 75kA AC 3P 100A MA",0.22]
["C10S2TM040","NSX100S 70kA AC-DC 2P 40A TMD",1,"ks",{"v":185.22,"d":"185.220"},"3606482034341",{"v":18,"d":"18.00"},{"v":8,"d":"8.00"},{"v":13,"d":"13.00"},{"v":1281,"d":"1,281.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10S2TM040","NSX100S 70kA AC-DC 2P 40A TMD",0.15]
["C10R46E040","NSX100R 200kA AC 4P 40A 6.2E",1,"ks",{"v":1455.2999999999997,"d":"1455.300"},"3606482001275",{"v":20,"d":"20.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2590,"d":"2,590.00"},"FR","8536201090","https://www.se.com/sk/sk/product/C10R46E040","NSX100R 200kA AC 4P 40A 6.2E",0.31]
["C10R3MA025","NSX100R 200kA AC 3P 25A MA",1,"ks",{"v":471.86999999999995,"d":"471.870"},"3606482001336",{"v":19,"d":"19.00"},{"v":12,"d":"12.00"},{"v":14,"d":"14.00"},{"v":1805,"d":"1,805.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10R3MA025","NSX100R 200kA AC 3P 25A MA",0.22]
["C10N6TM100","NSX100N 50kA AC 4P3D 100A TMD",1,"ks",{"v":330.74999999999994,"d":"330.750"},"3606481997944",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":15,"d":"15.00"},{"v":2306,"d":"2,306.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C10N6TM100","NSX100N 50kA AC 4P3D 100A TMD",0.28]
["C10N4TM080","NSX100N 50kA AC 4P4D 80A TMD",1,"ks",{"v":339.56999999999994,"d":"339.570"},"3606481998163",{"v":19.2,"d":"19.20"},{"v":14,"d":"14.00"},{"v":14.6,"d":"14.60"},{"v":2319,"d":"2,319.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C10N4TM080","NSX100N 50kA AC 4P4D 80A TMD",0.28]
["C10N4","Základný istič NSX100N 50kA AC 4P 100A",1,"ks",{"v":229.32,"d":"229.320"},"3606481999764",{"v":19,"d":"19.00"},{"v":14,"d":"14.00"},{"v":14.5,"d":"14.50"},{"v":1892,"d":"1,892.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C10N4","Základný istič NSX100N 50kA AC 4P 100A",0]
["C10N3MA050","NSX100N 50kA AC 3P3D 50A MA",1,"ks",{"v":238.14,"d":"238.140"},"3606481998378",{"v":20,"d":"20.00"},{"v":12,"d":"12.00"},{"v":15,"d":"15.00"},{"v":1824,"d":"1,824.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10N3MA050","NSX100N 50kA AC 3P3D 50A MA",0.22]
["C10N1TM063","NSX100N 25kA AC-DC 1P 63A TMD",1,"ks",{"v":119.07,"d":"119.070"},"3606481995568",{"v":17.5,"d":"17.50"},{"v":4,"d":"4.00"},{"v":13,"d":"13.00"},{"v":724,"d":"724.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10N1TM063","NSX100N 25kA AC-DC 1P 63A TMD",0.09]
["C10M1TM050","NSX100M 40kA AC-DC 1P 50A TMD",1,"ks",{"v":158.75999999999996,"d":"158.760"},"3606481995773",{"v":18,"d":"18.00"},{"v":5,"d":"5.00"},{"v":13,"d":"13.00"},{"v":730,"d":"730.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10M1TM050","NSX100M 40kA AC-DC 1P 50A TMD",0.09]
["C10M1TM025","NSX100M 40kA AC-DC 1P 25A TMD",1,"ks",{"v":158.75999999999996,"d":"158.760"},"3606481995742",{"v":17.5,"d":"17.50"},{"v":4.5,"d":"4.50"},{"v":13,"d":"13.00"},{"v":738,"d":"738.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10M1TM025","NSX100M 40kA AC-DC 1P 25A TMD",0.09]
["C10H4TM016","NSX100H 70kA AC 4P4D 16A TMD",1,"ks",{"v":370.44,"d":"370.440"},"3606481998897",{"v":19,"d":"19.00"},{"v":15,"d":"15.00"},{"v":17,"d":"17.00"},{"v":2378,"d":"2,378.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10H4TM016","NSX100H 70kA AC 4P4D 16A TMD",0.29]
["C10H42D040","NSX100H 70kA AC 4P4D 40A 2.2",1,"ks",{"v":432.17999999999995,"d":"432.180"},"3606481998828",{"v":19,"d":"19.00"},{"v":15,"d":"15.00"},{"v":17,"d":"17.00"},{"v":2415,"d":"2,415.00"},"FR","8536201090","https://www.se.com/sk/sk/product/C10H42D040","NSX100H 70kA AC 4P4D 40A 2.2",0.29]
["C10H34V040","NSX100H 70kA AC 3P3D 40A 4.2",1,"ks",{"v":926.0999999999998,"d":"926.100"},"3606481993663",{"v":11,"d":"11.00"},{"v":13.5,"d":"13.50"},{"v":19,"d":"19.00"},{"v":1922,"d":"1,922.00"},"CN","8536201090","https://www.se.com/sk/sk/product/C10H34V040","NSX100H 70kA AC 3P3D 40A 4.2",0.25]
["C10H32D040","NSX100H 70kA AC 3P3D 40A 2.2",1,"ks",{"v":326.34,"d":"326.340"},"3606481998590",{"v":19,"d":"19.00"},{"v":12,"d":"12.00"},{"v":17,"d":"17.00"},{"v":1843,"d":"1,843.00"},"FR","8536201090","https://www.se.com/sk/sk/product/C10H32D040","NSX100H 70kA AC 3P3D 40A 2.2",0.22]
["C10F4TM016","NSX100F 36kA AC 4P4D 16A TMD",1,"ks",{"v":286.6499999999999,"d":"286.650"},"3606481997456",{"v":19,"d":"19.00"},{"v":15,"d":"15.00"},{"v":18,"d":"18.00"},{"v":2411,"d":"2,411.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10F4TM016","NSX100F 36kA AC 4P4D 16A TMD",0.29]
["C10F3MA100","NSX100F 36kA AC 3P3D 100A MA",1,"ks",{"v":207.26999999999998,"d":"207.270"},"3606481997661",{"v":19.4,"d":"19.40"},{"v":14.2,"d":"14.20"},{"v":11.3,"d":"11.30"},{"v":1812,"d":"1,812.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C10F3MA100","NSX100F 36kA AC 3P3D 100A MA",0.22]
["C10F2TM063","NSX100F 18kA AC-DC 2P 63A TMD",1,"ks",{"v":145.52999999999997,"d":"145.530"},"3606481995438",{"v":17.6,"d":"17.60"},{"v":7.9,"d":"7.90"},{"v":13.1,"d":"13.10"},{"v":1234,"d":"1,234.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10F2TM063","NSX100F 18kA AC-DC 2P 63A TMD",0.15]
["C10F1TM080","NSX100F 18kA AC-DC 1P 80A TMD",1,"ks",{"v":114.66,"d":"114.660"},"3606481995353",{"v":18,"d":"18.00"},{"v":5,"d":"5.00"},{"v":13,"d":"13.00"},{"v":750,"d":"750.00"},"PL","8536209090","https://www.se.com/sk/sk/product/C10F1TM080","NSX100F 18kA AC-DC 1P 80A TMD",0.09]
["C10F1TM016","NSX100F 18kA AC-DC 1P 16A TMD",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3606481995285",{"v":17.5,"d":"17.50"},{"v":4.3,"d":"4.30"},{"v":13,"d":"13.00"},{"v":732,"d":"732.00"},"PL","8536201090","https://www.se.com/sk/sk/product/C10F1TM016","NSX100F 18kA AC-DC 1P 16A TMD",0.09]
["C10B42D040","NSX100B 25kA AC 4P 40A 2.2",1,"ks",{"v":326.34,"d":"326.340"},"3606481996688",{"v":18,"d":"18.00"},{"v":15,"d":"15.00"},{"v":18,"d":"18.00"},{"v":2381,"d":"2,381.00"},"FR","8536201090","https://www.se.com/sk/sk/product/C10B42D040","NSX100B 25kA AC 4P 40A 2.2",0.29]
["C106TM040","Jednotka spúšte NSX100 AC 4P3D 40A TMD",1,"ks",{"v":88.19999999999999,"d":"88.200"},"3606481999955",{"v":15,"d":"15.00"},{"v":6.5,"d":"6.50"},{"v":9.5,"d":"9.50"},{"v":494,"d":"494.00"},"PL","8536303099","https://www.se.com/sk/sk/product/C106TM040","Jednotka spúští NSX100 AC 4P3D 40A TMD",0]
["C104TM100","Jednotka spúšte NSX100 AC 4P4D 100A TMD",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3606482000247",{"v":15,"d":"15.00"},{"v":7,"d":"7.00"},{"v":9.5,"d":"9.50"},{"v":548,"d":"548.00"},"PL","8536303099","https://www.se.com/sk/sk/product/C104TM100","Jednotka spúští NSX100 AC 4P4D 100A TMD",0]
["C1047E040","Jednotka spúšte NSX100 AC 4P4D 40A 7.2E",1,"ks",{"v":1367.0999999999997,"d":"1367.100"},"3606481993885",{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":11,"d":"11.00"},{"v":795,"d":"795.00"},"CN","8536303099","https://www.se.com/sk/sk/product/C1047E040","Jednotka spúští NSX100 AC 4P4D 40A 7.2E",0]
["C1044V100","Jednotka spúšte NSX100 AC 4P4D 100A 4.2",1,"ks",{"v":745.2899999999998,"d":"745.290"},"3606481993854",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":11,"d":"11.00"},{"v":774,"d":"774.00"},"CN","8536309090","https://www.se.com/sk/sk/product/C1044V100","Jednotka spúští NSX100 AC 4P4D 100A 4.2",0]
["C103MG100","Jednotka spúšte NSX100 AC 3P3D 100A TMG",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3606482000537",{"v":10,"d":"10.00"},{"v":16,"d":"16.00"},{"v":12,"d":"12.00"},{"v":457,"d":"457.00"},"CN","8536303099","https://www.se.com/sk/sk/product/C103MG100","Jednotka spúští NSX100 AC 3P3D 100A TMG",0]
["C103MG025","Jednotka spúšte NSX100 AC 3P3D 25A TMG",1,"ks",{"v":85.99499999999999,"d":"85.995"},"3606482000490",{"v":11.4,"d":"11.40"},{"v":6.8,"d":"6.80"},{"v":10,"d":"10.00"},{"v":438,"d":"438.00"},"PL","8536303099","https://www.se.com/sk/sk/product/C103MG025","Jednotka spúští NSX100 AC 3P3D 25A TMG",0]
["C1034A100","Jednotka spúšte NSX100 AC 3P3D 100A 4.2A",1,"ks",{"v":458.64,"d":"458.640"},"3606481993939",{"v":15,"d":"15.00"},{"v":9.5,"d":"9.50"},{"v":11,"d":"11.00"},{"v":602,"d":"602.00"},"JP","8536303099","https://www.se.com/sk/sk/product/C1034A100","Jednotka spúští NSX100 AC 3P3D 100A 4.2AL",0]
["C100N4FM","Kompaktný istič ComPacT NS základný istič NS1000N 4P 1000 pev. manual ",1,"ks",1694.385,"3606482098190",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C100N4FM","Kompaktný istič ComPacT NS základný istič NS1000N 4P 1000 pev. manual",0]
["C100N42EFM","Kompaktný istič ComPacT NS1000N 50kA 4P 1000A pev. manual, 2.0E ",1,"ks",{"v":2754.6749999999997,"d":"2754.675"},"3606482098046",{"v":60,"d":"60.00"},{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":15800,"d":"15,800.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C100N42EFM","Kompaktný istič ComPacT NS1000N 50kA 4P 1000A pev. manual, 2.0E",1.9000000000000001]
["C100L45AFM","Kompaktný istič ComPacT NS1000L 150kA 4P 1000A pev. manual, 5.0A ",1,"ks",{"v":3503.1150000000002,"d":"3503.115"},"3606482100879",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":17507,"d":"17,507.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C100L45AFM","Kompaktný istič ComPacT NS1000L 150kA 4P 1000A pev. manual, 5.0A",2.1]
["C100L32AFM","Kompaktný istič ComPacT NS1000L 150kA 3P 1000A pev. manual, 2.0A ",1,"ks",{"v":2689.1865000000003,"d":"2689.187"},"3606482100480",{"v":23,"d":"23.00"},{"v":37,"d":"37.00"},{"v":39,"d":"39.00"},{"v":13291,"d":"13,291.00"},"IT","8536209090","https://www.se.com/sk/sk/product/C100L32AFM","Kompaktný istič ComPacT NS1000L 150kA 3P 1000A pev. manual, 2.0A",1.59]
["C100H35AFM","Kompaktný istič ComPacT NS1000H 70kA 3P 1000A pev. manual, 5.0A ",1,"ks",{"v":2619.54,"d":"2619.540"},"3606482100510",{"v":23,"d":"23.00"},{"v":37,"d":"37.00"},{"v":39.5,"d":"39.50"},{"v":11892,"d":"11,892.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C100H35AFM","Kompaktný istič ComPacT NS1000H 70kA 3P 1000A pev. manual, 5.0A",1.43]
["C080N3FM","Kompaktný istič ComPacT NS základný istič NS800N 3P 800 pev. manual ",1,"ks",1191.267,"3606482098138",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C080N3FM","Kompaktný istič ComPacT NS základný istič NS800N 3P 800 pev. manual",0]
["C080N35AFM","Kompaktný istič ComPacT NS800N 50kA 3P 800A pev. manual, 5.0A ",1,"ks",{"v":2370.0600000000004,"d":"2370.060"},"3606482097780",{"v":23,"d":"23.00"},{"v":37,"d":"37.00"},{"v":39.5,"d":"39.50"},{"v":11892,"d":"11,892.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C080N35AFM","Kompaktný istič ComPacT NS800N 50kA 3P 800A pev. manual, 5.0A",1.43]
["C080H42EFM","Kompaktný istič ComPacT NS800H 70kA 4P 800A pev. manual, 2.0E ",1,"ks",2688.147,"3606482100893",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":15968,"d":"15,968.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C080H42EFM","Kompaktný istič ComPacT NS800H 70kA 4P 800A pev. manual, 2.0E",1.92]
["C080B4WM","Kompaktný istič ComPacT NS základný istič NS800LB 4P 800 výs. manual ",1,"ks",{"v":2855.5065,"d":"2855.507"},"3606482238305",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C080B4WM","Kompaktný istič ComPacT NS základný istič NS800LB 4P 800 výs. manual",0]
["C063N4FM","Kompaktný istič ComPacT NS základný istič NS630N 4P 630 pev. manual ",1,"ks",1357.587,"3606482098176",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C063N4FM","Kompaktný istič ComPacT NS základný istič NS630N 4P 630 pev. manual",0]
["C063N420FM","Kompaktný istič ComPacT NS630N 50kA 4P 630A pev. manual, 2.0 ",1,"ks",{"v":2230.7670000000003,"d":"2230.767"},"3606482097575",{"v":38,"d":"38.00"},{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":14873,"d":"14,873.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C063N420FM","Kompaktný istič ComPacT NS630N 50kA 4P 630A pev. manual, 2.0",1.78]
["C063L3WM","Kompaktný istič ComPacT NS základný istič NS630L 3P 630 výs. manual ",1,"ks",{"v":1688.1480000000001,"d":"1688.148"},"3606482238169",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":1,"d":"1.00"},{"v":10,"d":"10.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C063L3WM","Kompaktný istič ComPacT NS základný istič NS630L 3P 630 výs. manual",0]
["C063H35AFM","Kompaktný istič ComPacT NS630H 70kA 3P 630A pev. manual, 5.0A ",1,"ks",{"v":2333.6775,"d":"2333.678"},"3606482100497",{"v":23,"d":"23.00"},{"v":37,"d":"37.00"},{"v":39.5,"d":"39.50"},{"v":11892,"d":"11,892.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C063H35AFM","Kompaktný istič ComPacT NS630H 70kA 3P 630A pev. manual, 5.0A",1.43]
["C063H320FM","Kompaktný istič ComPacT NS630H 70kA 3P 630A pev. manual, 2.0 ",1,"ks",{"v":1931.3909999999998,"d":"1931.391"},"3606482099999",{"v":23,"d":"23.00"},{"v":37,"d":"37.00"},{"v":39.5,"d":"39.50"},{"v":12119,"d":"12,119.00"},"FR","8536209090","https://www.se.com/sk/sk/product/C063H320FM","Kompaktný istič ComPacT NS630H 70kA 3P 630A pev. manual, 2.0",1.45]
["BSH1403P22A2A","BSH MOTOR 140MM, 25,4NM, IP65",1,"ks",2768.535,"3389118142817",{"v":54.4,"d":"54.40"},{"v":27,"d":"27.00"},{"v":27,"d":"27.00"},{"v":15000,"d":"15,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1403P22A2A","servo motor BSH, Lexium 32, 22.2N.m, 1500rpm, 140mm, untapped shaft, Sincos multi turn, without brake, IP65",1.8]
["BSH1402P32F1A","BSH MOTOR 140MM, 19,2NM, IP65",1,"ks",{"v":2827.44,"d":"2827.440"},"3389118142022",{"v":48.2,"d":"48.20"},{"v":27,"d":"27.00"},{"v":27,"d":"27.00"},{"v":13290,"d":"13,290.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1402P32F1A","AC servomotor BSH - 14.9 N.m - 1500 rpm - hladká hriadeľ - s brzdou - IP50",1.59]
["BSH1402P22A2A","BSH MOTOR 140MM, 19,2NM, IP65",1,"ks",{"v":2365.6247999999996,"d":"2365.625"},"3389118141919",{"v":48.2,"d":"48.20"},{"v":27,"d":"27.00"},{"v":27,"d":"27.00"},{"v":11500,"d":"11,500.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1402P22A2A","AC servomotor BSH - 14.9 N.m - 1500 rpm - hladká hriadeľ - bez brzdy - IP50",0.08]
["BSH1401T32F2A","BSH MOTOR 140MM, 11,4NM, IP65",1,"ks",2532.915,"3389118141346",{"v":48.2,"d":"48.20"},{"v":27,"d":"27.00"},{"v":27,"d":"27.00"},{"v":9790,"d":"9,790.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1401T32F2A","AC servomotor BSH - 11.1 N.m - 2500 rpm - hriadeľ s perom - s brzdou - IP65",1.17]
["BSH1401T21F2A","BSH MOTOR 140MM, 11,4NM, IP65",1,"ks",{"v":2238.39,"d":"2238.390"},"3389118141148",{"v":48.2,"d":"48.20"},{"v":27,"d":"27.00"},{"v":27,"d":"27.00"},{"v":9790,"d":"9,790.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1401T21F2A","AC servomotor BSH - 11.1 N.m - 2500 rpm - hladká hriadeľ - s brzdou - IP65",1.17]
["BSH1401P31A1A","BSH MOTOR 140MM, 11,4NM, IP65",1,"ks",{"v":1767.1499999999999,"d":"1767.150"},"3389118140929",{"v":48.2,"d":"48.20"},{"v":27,"d":"27.00"},{"v":27,"d":"27.00"},{"v":8000,"d":"8,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1401P31A1A","AC servomotor BSH - 11.1 N.m - 1500 rpm - hriadeľ s perom - bez brzdy - IP65",0.96]
["BSH1401P11F1A","BSH MOTOR 140MM, 11,4NM, IP40",1,"ks",{"v":2179.4849999999997,"d":"2179.485"},"3389118140653",{"v":48.2,"d":"48.20"},{"v":27,"d":"27.00"},{"v":27,"d":"27.00"},{"v":9790,"d":"9,790.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1401P11F1A","AC servomotor BSH - 11.1 N.m - 1500 rpm - hriadeľ s perom - s brzdou - IP50",1.17]
["BSH1004P22A2A","BSH MOTOR 100MM, 9,3NM, IP65",1,"ks",{"v":2023.9758000000002,"d":"2023.976"},"3389118140486",{"v":49.2,"d":"49.20"},{"v":18.3,"d":"18.30"},{"v":16.3,"d":"16.30"},{"v":7500,"d":"7,500.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1004P22A2A","AC servomotor BSH - 9.31 N.m - 1500 rpm - hladká hriadeľ - bez brzdy - IP65",""]
["BSH1004P02A2A","BSH MOTOR 100MM, 9,3NM, IP40",1,"ks",{"v":2002.7699999999998,"d":"2002.770"},"3389118140394",{"v":49.2,"d":"49.20"},{"v":18.3,"d":"18.30"},{"v":16.3,"d":"16.30"},{"v":7500,"d":"7,500.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1004P02A2A","AC servomotor BSH - 9.31 N.m - 1500 rpm - hladká hriadeľ - bez brzdy - IP50",0.9]
["BSH1003P11A1A","BSH MOTOR 100MM, 7,8NM, IP40",1,"ks",1590.435,"3389118140219",{"v":57,"d":"57.00"},{"v":21,"d":"21.00"},{"v":18.3,"d":"18.30"},{"v":7400,"d":"7,400.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1003P11A1A","AC servomotor BSH - 7.8 N.m - 2500 rpm - hriadeľ s perom - bez brzdy - IP50",0.96]
["BSH1002T12F2A","BSH MOTOR 100MM, 5,5NM, IP40",1,"ks",{"v":2009.8385999999998,"d":"2009.839"},"3389118139619",{"v":40.7,"d":"40.70"},{"v":15.4,"d":"15.40"},{"v":16.3,"d":"16.30"},{"v":6450,"d":"6,450.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1002T12F2A","AC servomotor BSH - 5.5 N.m - 4000 rpm - hriadeľ s perom - s brzdou - IP50",""]
["BSH1002P32A2A","BSH MOTOR 100MM, 5,5NM, IP65",1,"ks",1708.245,"3389118139367",{"v":40.7,"d":"40.70"},{"v":15.4,"d":"15.40"},{"v":16.3,"d":"16.30"},{"v":5800,"d":"5,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1002P32A2A","AC servomotor BSH - 3.4 N.m - 2500 rpm - hriadeľ s perom - bez brzdy - IP65",0.7000000000000001]
["BSH1002P11F1A","BSH MOTOR 100MM, 5,5NM, IP40",1,"ks",1708.245,"3389118139213",{"v":40.7,"d":"40.70"},{"v":15.4,"d":"15.40"},{"v":16.3,"d":"16.30"},{"v":6450,"d":"6,450.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1002P11F1A","AC servomotor BSH - 3.4 N.m - 2500 rpm - hriadeľ s perom - s brzdou - IP50",0.77]
["BSH1001T32F2A","BSH MOTOR 100MM, 3,4NM, IP65",1,"ks",{"v":1884.9599999999998,"d":"1884.960"},"3389118138766",{"v":40.7,"d":"40.70"},{"v":15.4,"d":"15.40"},{"v":16.3,"d":"16.30"},{"v":4950,"d":"4,950.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1001T32F2A","AC servomotor BSH - 3.39 N.m - 4000 rpm - hriadeľ s perom - s brzdou - IP65",0.59]
["BSH1001P32F2A","BSH MOTOR 100MM, 3,4NM, IP65",1,"ks",{"v":1860.2199,"d":"1860.220"},"3389118138377",{"v":40.7,"d":"40.70"},{"v":15.4,"d":"15.40"},{"v":16.3,"d":"16.30"},{"v":4950,"d":"4,950.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1001P32F2A","AC servomotor BSH - 2.7 N.m - 3000 rpm - hriadeľ s perom - s brzdou - IP65",""]
["BSH1001P21A2A","BSH MOTOR 100MM, 3,4NM, IP65",1,"ks",{"v":1247.6079,"d":"1247.608"},"3389118138292",{"v":40.7,"d":"40.70"},{"v":15.4,"d":"15.40"},{"v":16.3,"d":"16.30"},{"v":4300,"d":"4,300.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH1001P21A2A","AC servomotor BSH - 2.7 N.m - 3000 rpm - hladká hriadeľ - bez brzdy - IP65",""]
["BSH0703T31F2A","BSH MOTOR 70MM, 2,8NM, IP65",1,"ks",{"v":1531.53,"d":"1531.530"},"3389118137714",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":4050,"d":"4,050.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH0703T31F2A","AC servomotor BSH - 2.83 N.m - 6000 rpm - hriadeľ s perom - s brzdou - IP65",0.49]
["BSH0703T12A2A","BSH MOTOR 70MM, 2,8NM, IP40",1,"ks",{"v":1505.6118,"d":"1505.612"},"3389118137578",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":3600,"d":"3,600.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH0703T12A2A","AC servomotor BSH - 2.83 N.m - 6000 rpm - hriadeľ s perom - bez brzdy - IP50",0.59]
["BSH0703P11A1A","BSH MOTOR 70MM, 2,8NM, IP40",1,"ks",1166.319,"3389118137202",{"v":46,"d":"46.00"},{"v":17.5,"d":"17.50"},{"v":16,"d":"16.00"},{"v":3620,"d":"3,620.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH0703P11A1A","AC servomotor BSH - 1.1 N.m - 3000 rpm - hriadeľ s perom - bez brzdy - IP50",0.47000000000000003]
["BSH0702T22A2A","BSH MOTOR 70MM, 2,1NM, IP65",1,"ks",{"v":1465.5564,"d":"1465.556"},"3389118136694",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":2800,"d":"2,800.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0702T22A2A","AC servomotor BSH - 2.12 N.m - 6000 rpm - hladká hriadeľ - bez brzdy - IP65",0.43]
["BSH0702P32A2A","BSH MOTOR 70MM, 2,1NM, IP65",1,"ks",1472.625,"3389118136472",{"v":48.5,"d":"48.50"},{"v":22,"d":"22.00"},{"v":19.5,"d":"19.50"},{"v":2890,"d":"2,890.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BSH0702P32A2A","AC servomotor BSH - 2.2 N.m - 3000 rpm - hriadeľ s perom - bez brzdy - IP65",0.41000000000000003]
["BSH0702P12A2A","BSH MOTOR 70MM, 2,1NM, IP40",1,"ks",{"v":1413.72,"d":"1413.720"},"3389118136311",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":2800,"d":"2,800.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0702P12A2A","AC servomotor BSH - 2.2 N.m - 3000 rpm - hriadeľ s perom - bez brzdy - IP50",0.34]
["BSH0702P02A1A","BSH MOTOR 70MM, 2,1NM, IP40",1,"ks",1354.815,"3389118136229",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":2800,"d":"2,800.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0702P02A1A","AC servomotor BSH - 2.2 N.m - 3000 rpm - hladká hriadeľ - bez brzdy - IP50",0.34]
["BSH0701T11A2A","BSH MOTOR 70MM, 1,4NM, IP40",1,"ks",{"v":1148.6474999999998,"d":"1148.648"},"3389118135956",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":2100,"d":"2,100.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0701T11A2A","AC servomotor BSH - 0.7 N.m - 8000 rpm - hriadeľ s perom - bez brzdy - IP50",0.25]
["BSH0701P31F2A","BSH MOTOR 70MM, 1,4NM, IP65",1,"ks",{"v":1367.7740999999999,"d":"1367.774"},"3389118135819",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":2550,"d":"2,550.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0701P31F2A","AC servomotor BSH - 1.4 N.m - 3000 rpm - hriadeľ s perom - s brzdou - IP65",""]
["BSH0701P11A1A","BSH MOTOR 70MM, 1,4NM, IP40",1,"ks",{"v":1066.1805000000002,"d":"1066.181"},"3389118135628",{"v":39.5,"d":"39.50"},{"v":11.5,"d":"11.50"},{"v":19,"d":"19.00"},{"v":2100,"d":"2,100.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0701P11A1A","AC servomotor BSH - 1.4 N.m - 3000 rpm - hriadeľ s perom - bez brzdy - IP50",0.25]
["BSH0553T11A1A","BSH MOTOR 55MM, 1,3NM, IP40",1,"ks",1107.414,"3389118159686",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":1400,"d":"1,400.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0553T11A1A","AC servomotor BSH - 1.3 N.m - 3000 rpm - hriadeľ s perom - bez brzdy - IP50",0.17]
["BSH0553T01F2A","BSH MOTOR 55MM, 1,3NM, IP40",1,"ks",{"v":1295.9099999999999,"d":"1295.910"},"3389118159648",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":1550,"d":"1,550.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0553T01F2A","AC servomotor BSH - 1.3 N.m - 3000 rpm - hladká hriadeľ - s brzdou - IP50",0.19]
["BSH0553P11F2A","BSH MOTOR 55MM, 1,3NM, IP40",1,"ks",{"v":1295.9099999999999,"d":"1295.910"},"3389118159327",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":1550,"d":"1,550.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0553P11F2A","AC servomotor BSH - 1.3 N.m - 3000 rpm - hriadeľ s perom - s brzdou - IP50",0.19]
["BSH0552T31A1A","BSH MOTOR 55MM, 0,9NM, IP65",1,"ks",{"v":1060.29,"d":"1060.290"},"3389118159174",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":1100,"d":"1,100.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0552T31A1A","AC servomotor BSH - 0.9 N.m - 6000 rpm - hriadeľ s perom - bez brzdy - IP65",0.13]
["BSH0552T22A1A","BSH MOTOR 55MM, 0,9NM, IP65",1,"ks",{"v":1315.9377,"d":"1315.938"},"3389118159143",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":1100,"d":"1,100.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0552T22A1A","AC servomotor BSH - 0.9 N.m - 6000 rpm - hladká hriadeľ - bez brzdy - IP65",""]
["BSH0552P32A2A","BSH MOTOR 55MM, 0,9NM, IP65",1,"ks",1354.815,"3389118158894",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":1100,"d":"1,100.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0552P32A2A","AC servomotor BSH - 0.9 N.m - 4000 rpm - hriadeľ s perom - bez brzdy - IP65",0.13]
["BSH0552P31A1A","BSH MOTOR 55MM, 0,9NM, IP65",1,"ks",1036.728,"3389118158870",{"v":37.7,"d":"37.70"},{"v":12.3,"d":"12.30"},{"v":12.8,"d":"12.80"},{"v":1100,"d":"1,100.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0552P31A1A","AC servomotor BSH - 0.9 N.m - 4000 rpm - hriadeľ s perom - bez brzdy - IP65",0.13]
["BSH0552P02A1A","BSH MOTOR 55MM, 0,9NM, IP40",1,"ks",{"v":1237.0049999999999,"d":"1237.005"},"3389118158719",{"v":39.5,"d":"39.50"},{"v":11.5,"d":"11.50"},{"v":19,"d":"19.00"},{"v":1757,"d":"1,757.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0552P02A1A","AC servomotor BSH - 0.9 N.m - 4000 rpm - hladká hriadeľ - bez brzdy - IP50",0.21]
["BSH0551T12F2A","BSH MOTOR 55MM, 0,5NM, IP40",1,"ks",1472.625,"3389118158351",{"v":39.5,"d":"39.50"},{"v":11.5,"d":"11.50"},{"v":19,"d":"19.00"},{"v":950,"d":"950.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0551T12F2A","AC servomotor BSH - 0.5 N.m - 8000 rpm - hriadeľ s perom - s brzdou - IP50",0.11]
["BSH0551T02A2A","BSH MOTOR 55MM, 0,5NM, IP40",1,"ks",{"v":1237.0049999999999,"d":"1237.005"},"3389118158313",{"v":39.5,"d":"39.50"},{"v":11.5,"d":"11.50"},{"v":19,"d":"19.00"},{"v":1646,"d":"1,646.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BSH0551T02A2A","AC servomotor BSH - 0.5 N.m - 8000 rpm - hladká hriadeľ - bez brzdy - IP50",0.2]
["BRS3ADW850ABA","KROKOVÝ MOTOR BRS 110MM,19.7 NM",1,"ks",{"v":1413.72,"d":"1413.720"},"3389119224239",{"v":22.5,"d":"22.50"},{"v":19,"d":"19.00"},{"v":40,"d":"40.00"},{"v":11200,"d":"11,200.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BRS3ADW850ABA","krokový 3-fáz. motor - 19.7 Nm - hriadeľ Ø19mm - L=230mm - bez brzdy -svork.",1.46]
["BRS39BW770ABA","KROKOVÝ MOTOR BRS 90MM, 6.78 NM",1,"ks",{"v":736.3125,"d":"736.313"},"3389119223997",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":19,"d":"19.00"},{"v":4300,"d":"4,300.00"},"DE","85015100","https://www.se.com/sk/sk/product/BRS39BW770ABA","krokový 3-fáz. motor-6.78 Nm-hriadeľ Ø 14mm-L=128mm-bez brzdy -svorkovnica",0.56]
["BRS39AW660FBA","KROKOVÝ MOTOR BRS 90MM, 4.52 NM",1,"ks",{"v":1148.6474999999998,"d":"1148.648"},"3389119223850",{"v":40,"d":"40.00"},{"v":22.5,"d":"22.50"},{"v":19,"d":"19.00"},{"v":5098,"d":"5,098.00"},"DE","85015100","https://www.se.com/sk/sk/product/BRS39AW660FBA","krokový 3-fáz. motor - 4.8 Nm - hriadeľ Ø 12mm - L=98mm - s brzdou-svork.",0.61]
["BRS39AW361ACB","KROKOVÝ MOTOR BRS 90MM,4.52 NM, ENKÓDER",1,"ks",{"v":1066.1805000000002,"d":"1066.181"},"3389119223928",{"v":40,"d":"40.00"},{"v":22.5,"d":"22.50"},{"v":19,"d":"19.00"},{"v":3924,"d":"3,924.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BRS39AW361ACB","krokový 3-fáz. motor - 4.52 Nm - hriadeľ Ø 12 mm - L=98 mm - bez brzdy - vodiče",0.47000000000000003]
["BRS397W360ABA","KROKOVÝ MOTOR BRS 90MM,2.26 NM, IP41",1,"ks",530.145,"3389119223584",{"v":40,"d":"40.00"},{"v":22.5,"d":"22.50"},{"v":19,"d":"19.00"},{"v":2520,"d":"2,520.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BRS397W360ABA","krokový 3-fáz. motor - 2.26 Nm - hriadeľ Ø 12 mm - L=68 mm - bez brzdy -svork.",0.3]
["BRS368W131ACA","KROKOVÝ MOTOR BRS 60 MM, 1.7 NM",1,"ks",1048.509,"3389119223553",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":19.5,"d":"19.50"},{"v":2000,"d":"2,000.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BRS368W131ACA","krokový 3-fáz. motor - 1.7 Nm - hriadeľ Ø8mm - L=79mm - bez brzdy -vodiče",0.28]
["BMXXSP0400","TIENIACI KIT PRE NOSNÚ LIŠTU 4 POZÍCIE",1,"ks",129.591,"3595863931716",{"v":26.2,"d":"26.20"},{"v":4.6,"d":"4.60"},{"v":9.3,"d":"9.30"},{"v":274,"d":"274.00"},"FR","8538100000","https://www.se.com/sk/sk/product/BMXXSP0400","sada pre spoločné uzemnenie vodičov - pre M340 rak - 4 sloty",0]
["BMXXBC030K","PREP.KÁBEL MEDZI NOSNÝMI LIŠTAMI 3M",1,"ks",188.496,"3595863992632",{"v":25,"d":"25.00"},{"v":2.5,"d":"2.50"},{"v":23,"d":"23.00"},{"v":423,"d":"423.00"},"TN","8544429090","https://www.se.com/sk/sk/product/BMXXBC030K","backplane predĺžený kábel M340 - 3m",0]
["BMXRMS008MPF","PAMÄŤOVÁ KARTA 8MB + 16MB PRE SÚBORY",1,"ks",{"v":500.69249999999994,"d":"500.693"},"3595863922257",{"v":14.5,"d":"14.50"},{"v":0.4,"d":"0.40"},{"v":12,"d":"12.00"},{"v":28,"d":"28.00"},"FR","8523519000","https://www.se.com/sk/sk/product/BMXRMS008MPF","SD flash pamäťová karta - 8 Mb - plus 8 Mb pre súbory - pre procesor M340",0]
["BMXMSP0200","MODUL PTO 2 MOTION KANÁLY",1,"ks",1354.815,"3595863998634",{"v":11.7,"d":"11.70"},{"v":5.4,"d":"5.40"},{"v":11.5,"d":"11.50"},{"v":147,"d":"147.00"},"FR","8538909999","https://www.se.com/sk/sk/product/BMXMSP0200","PTO module pre servopohony-2 kanály- 4 vstupy-24 V DC-4.3 mA-2 konektory 28 piny",0.02]
["BMXFCW501","FCN KON. (16 KANÁLOV) VOĽNÉ KONCE 5M",1,"ks",{"v":113.68665,"d":"113.687"},"3595863920130",{"v":25,"d":"25.00"},{"v":3.5,"d":"3.50"},{"v":24,"d":"24.00"},{"v":767,"d":"767.00"},"TN","8544429090","https://www.se.com/sk/sk/product/BMXFCW501","kábel s konektorom - 40-pin. svorka - jeden volný koniec - pro M340 I/O - 5 m",0]
["BMXFCW1003","FCN KON. (32 KANÁLOV) VOĽNÉ KONCE 10M",1,"ks",{"v":288.6345,"d":"288.635"},"3595863920192",{"v":25,"d":"25.00"},{"v":9.5,"d":"9.50"},{"v":25,"d":"25.00"},{"v":2837,"d":"2,837.00"},"TN","8544429090","https://www.se.com/sk/sk/product/BMXFCW1003","kábel s konektorom - 40-pin. svorka - dva volné konce - pro M340 I/O - 10 m",0]
["BMXFCC053","PREP.KÁBEL FCN KON.-TELEFAST 2XHE10 0,5M",1,"ks",{"v":107.79614999999998,"d":"107.796"},"3595863919752",{"v":25,"d":"25.00"},{"v":2,"d":"2.00"},{"v":20,"d":"20.00"},{"v":235,"d":"235.00"},"TN","8544429090","https://www.se.com/sk/sk/product/BMXFCC053","kábel s konektorom - 40-pin. svorka - 2 x HE10 konektor - pre M340 I/O - 0.5 m",0]
["BMXDDO6402K","MODUL 64DO TRANZ. 0,1A, FCN KON.",1,"ks",{"v":995.4944999999999,"d":"995.495"},"3595863910490",{"v":11.288,"d":"11.29"},5.45,{"v":10.793,"d":"10.79"},{"v":150,"d":"150.00"},"ID","8538909999","https://www.se.com/sk/sk/product/BMXDDO6402K","diskrétny výstupný modul M340 - 64 výst. - polovod. - 24 V DC poz. log.",0.02]
["BMXCPS3540T","VÝKONNÝ NAPÁJACÍ ZDROJ M340 125VDC 36W",1,"ks",{"v":1125.0855,"d":"1125.086"},"3595864082318",{"v":15.7,"d":"15.70"},{"v":13.7,"d":"13.70"},{"v":15.7,"d":"15.70"},{"v":360,"d":"360.00"},"FR","8504408390","https://www.se.com/sk/sk/product/BMXCPS3540T","napájací modul M340 - 125 V DC - pre rozširenú teplotu",0.06]
["BMXAMO0802","MODUL 8AO U/I NEIZOL. 15BIT+ZNAMIENKO",1,"ks",1095.633,"3595864081588",{"v":11.6,"d":"11.60"},{"v":5.3,"d":"5.30"},{"v":11,"d":"11.00"},{"v":169,"d":"169.00"},"FR","8538909999","https://www.se.com/sk/sk/product/BMXAMO0802","analog. výstupný modul M340-8 výstupov",0.02]
["BMP1002F3NA2A","Synchrónny motor 1,5 kW pre frekvenčné",1,"ks",{"v":736.3125,"d":"736.313"},"3606480564444",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":5980,"d":"5,980.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMP1002F3NA2A","Synchrónny motor PMSM 480 V AC 1,5 kW",0.72]
["BMI1002P31A","MOT 3P 70MM IP65 1,9KW CHV ENC SGT 128",1,"ks",{"v":2347.9532999999997,"d":"2347.953"},"3606485377162",{"v":55,"d":"55.00"},{"v":25,"d":"25.00"},{"v":18.6,"d":"18.60"},{"v":9500,"d":"9,500.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMI1002P31A","servomotor BMI 3-fáz.- s perom IP65 jedno ot. - 131072 p/t",""]
["BMI0703T27F","MOT 1P 70MM IP65 640W LIS ENC MLT 16 FR",1,"ks",{"v":2629.5192,"d":"2629.519"},"3606485376837",{"v":55,"d":"55.00"},{"v":25,"d":"25.00"},{"v":18.6,"d":"18.60"},{"v":6500,"d":"6,500.00"},"DE","8501402080","https://www.se.com/sk/sk/product/BMI0703T27F","servomotor BMI 1-fáz. - hladká IP65 viacot. - 32768 p/t x 4096 t -brzda",""]
["BMI0702T31F","MOT 1P 70MM IP65 640W CHV ENC SGT 128 FR",1,"ks",{"v":2505.8187000000003,"d":"2505.819"},"3606485376219",{"v":59,"d":"59.00"},{"v":26,"d":"26.00"},{"v":20,"d":"20.00"},{"v":5400,"d":"5,400.00"},"DE","8501402080","https://www.se.com/sk/sk/product/BMI0702T31F","servomotor BMI 1-fáz. - s perom IP65 jedno ot. - 131072 p/t -brzda",0.02]
["BMI0702P27A","MOT 3P 70MM IP65 790W LIS ENC MLT 16",1,"ks",{"v":2088.7713,"d":"2088.771"},"3606485375861",{"v":59,"d":"59.00"},{"v":26,"d":"26.00"},{"v":20,"d":"20.00"},{"v":5400,"d":"5,400.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMI0702P27A","servomotor BMI 3-fáz.- hladká IP65 viacot. - 32768 p/t x 4096 t",1.14]
["BMH2053P32F2A","MOTOR IEC 205MM 88NM IP65 HRIAD. S DRÁŽ.",1,"ks",9954.945,"3606485202235",{"v":79.5,"d":"79.50"},{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":71900,"d":"71,900.00"},"DE","8501523090","https://www.se.com/sk/sk/product/BMH2053P32F2A","servomotor BMH - 84 Nm - 3800 rpm - hriadeľ s perom - s brzdou - IP65/IP67",9.120000000000001]
["BMH2053P21F1A","MOTOR IEC 205MM 88NM IP65 HLADKÝ HRIAD.",1,"ks",9601.515,"3606485201986",{"v":73,"d":"73.00"},{"v":36,"d":"36.00"},{"v":31,"d":"31.00"},{"v":71000,"d":"71,000.00"},"DE","8501523090","https://www.se.com/sk/sk/product/BMH2053P21F1A","servomotor BMH - 84 Nm - 3800 rpm - hladká hriadeľ - s brzdou - IP65/IP67",8.52]
["BMH2052P36F2A","MOTOR IEC 205MM 62,5NM IP65 HR. S DRÁŽ.",1,"ks",{"v":7477.400699999999,"d":"7477.401"},"3606485203355",{"v":73,"d":"73.00"},{"v":36,"d":"36.00"},{"v":31,"d":"31.00"},{"v":58000,"d":"58,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH2052P36F2A","servomotor BMH - 62.5 Nm - 3800 rpm - hriadeľ s perom - s brzdou - IP65/IP67",0.65]
["BMH2052P26F1A","MOTOR IEC 205MM 62,5NM IP65 HLAD. HRIAD.",1,"ks",7363.125,"3606485203263",{"v":73,"d":"73.00"},{"v":36,"d":"36.00"},{"v":31,"d":"31.00"},{"v":54000,"d":"54,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH2052P26F1A","servomotor BMH - 62.5 Nm - 3800 rpm - hladká hriadeľ - s brzdou - IP65/IP67",6.48]
["BMH2052P12A2A","MOTOR IEC 205MM 62,5NM IP54 HR. S DRÁŽ.",1,"ks",{"v":7068.599999999999,"d":"7068.600"},"3606485203133",{"v":73,"d":"73.00"},{"v":36,"d":"36.00"},{"v":31,"d":"31.00"},{"v":44000,"d":"44,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH2052P12A2A","servomotor BMH - 62.5 Nm - 3800 rpm - hriadeľ s perom - bez brzdy - IP54",6]
["BMH2051P32F1A","MOTOR IEC 205MM 34,4NM IP65 HR. S DRÁŽ.",1,"ks",{"v":6008.31,"d":"6008.310"},"3606485202631",{"v":58,"d":"58.00"},{"v":36,"d":"36.00"},{"v":31,"d":"31.00"},{"v":39000,"d":"39,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH2051P32F1A","servomotor BMH - 34.4 Nm - 3800 rpm - hriadeľ s perom - s brzdou - IP65/IP67",4.68]
["BMH2051P22F2A","MOTOR IEC 205MM 34,4NM IP65 HLAD. HRIAD.",1,"ks",{"v":6005.9538,"d":"6005.954"},"3606485202709",{"v":58,"d":"58.00"},{"v":36,"d":"36.00"},{"v":31,"d":"31.00"},{"v":43000,"d":"43,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH2051P22F2A","servomotor BMH - 34.4 Nm - 3800 rpm - hladká hriadeľ - s brzdou - IP65/IP67",""]
["BMH2051P11A1A","MOTOR IEC 205MM 34,4NM IP54 HR. S DRÁŽ.",1,"ks",4771.305,"3606485201610",{"v":58,"d":"58.00"},{"v":36,"d":"36.00"},{"v":31,"d":"31.00"},{"v":33000,"d":"33,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH2051P11A1A","servomotor BMH - 34.4 Nm - 3800 rpm - hriadeľ s perom - bez brzdy - IP54",4.2]
["BMH1403P27F1A","Servomotor BMH - 24 Nm - 4 000 ot / min",1,"ks",{"v":2945.25,"d":"2945.250"},"3606485208367",{"v":60,"d":"60.00"},{"v":20.5,"d":"20.50"},{"v":26.5,"d":"26.50"},{"v":19260,"d":"19,260.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1403P27F1A","servomotor BMH - 24 Nm - 4000 rpm - hladká hriadel - s brzdou - IP65/IP67",2.31]
["BMH1402P06F2A","Servomotor PMSM, príruba 140 mm IEC 18,",1,"ks",{"v":2179.4849999999997,"d":"2179.485"},"3606485207780",{"v":60,"d":"60.00"},{"v":26,"d":"26.00"},{"v":20,"d":"20.00"},{"v":14300,"d":"14,300.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1402P06F2A","servomotor BMH - 18.5 Nm - 4000 rpm - hladká hriadel - s brzdou - IP54",1.72]
["BMH1401P32F2A","MOTOR IEC 140MM 10,3NM IP65 HR. S DRÁŽ.",1,"ks",2415.105,"3606485198392",{"v":60,"d":"60.00"},{"v":26,"d":"26.00"},{"v":20,"d":"20.00"},{"v":10300,"d":"10,300.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1401P32F2A","servomotor BMH - 10.3 Nm - 4000 rpm - hriadeľ s perom - s brzdou - IP65/IP67",1.24]
["BMH1401P26F1A","MOTOR IEC 140MM 10,3NM IP65 HLAD. HRIAD.",1,"ks",{"v":1816.6301999999998,"d":"1816.630"},"3606485198460",{"v":60,"d":"60.00"},{"v":26,"d":"26.00"},{"v":20,"d":"20.00"},{"v":10600,"d":"10,600.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1401P26F1A","servomotor BMH - 10.3 Nm - 4000 rpm - hladká hriadeľ - s brzdou - IP65/IP67",2.22]
["BMH1401P16A1A","MOTOR IEC 140MM 10,3NM IP54 HR. S DRÁŽ.",1,"ks",1472.625,"3606485198415",{"v":59,"d":"59.00"},{"v":20,"d":"20.00"},{"v":26,"d":"26.00"},{"v":9658,"d":"9,658.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1401P16A1A","servomotor BMH - 10.3 Nm - 4000 rpm - hriadeľ s perom - bez brzdy - IP54",1.16]
["BMH1401P11A1A","MOTOR IEC 140MM 10,3NM IP54 HR. S DRÁŽ.",1,"ks",1708.245,"3606485201139",{"v":60,"d":"60.00"},{"v":26,"d":"26.00"},{"v":20,"d":"20.00"},{"v":8000,"d":"8,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1401P11A1A","servomotor BMH - 10.3 Nm - 4000 rpm - hriadeľ s perom - bez brzdy - IP54",0.96]
["BMH1003T31F2A","MOTOR IEC 100MM 8,2NM IP65 HR. S DRÁŽ",1,"ks",{"v":1873.1789999999999,"d":"1873.179"},"3606485201115",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":8450,"d":"8,450.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1003T31F2A","servomotor BMH - 8.2 Nm - 6000 rpm - hriadeľ s perom - s brzdou - IP65/IP67",""]
["BMH1003T26F2A","MOTOR IEC 100MM 8,4NM IP65 HLADKÝ HRIAD.",1,"ks",{"v":1649.34,"d":"1649.340"},"3606485198064",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":8150,"d":"8,150.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1003T26F2A","servomotor BMH - 8.2 Nm - 6000 rpm - hladká hriadeľ - s brzdou - IP65/IP67",0.98]
["BMH1003T07F2A","MOTOR IEC 100MM 8,4NM IP54 HLADKÝ HRIAD.",1,"ks",{"v":1867.2884999999999,"d":"1867.289"},"3606485198200",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":8450,"d":"8,450.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1003T07F2A","servomotor BMH - 8.2 Nm - 6000 rpm - hladká hriadeľ - s brzdou - IP54",""]
["BMH1003P36A1A","MOTOR IEC 100MM 8,4NM IP65 HR. S DRÁŽ",1,"ks",1354.815,"3606485196534",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":6500,"d":"6,500.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1003P36A1A","servomotor BMH - 8.4 Nm - 6000 rpm - hriadeľ s perom - bez brzdy - IP65/IP67",0.78]
["BMH1003P32A1A","MOTOR IEC 100MM 8,4NM IP65 HR. S DRÁŽ",1,"ks",1826.055,"3606485196374",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":6500,"d":"6,500.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1003P32A1A","servomotor BMH - 8.4 Nm - 6000 rpm - hriadeľ s perom - bez brzdy - IP65/IP67",0.78]
["BMH1003P17A1A","MOTOR IEC 100MM 8,4NM IP54 HR. S DRÁŽ",1,"ks",1590.435,"3606485196671",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":6500,"d":"6,500.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1003P17A1A","servomotor BMH - 8.4 Nm - 6000 rpm - hriadeľ s perom - bez brzdy - IP54",0.78]
["BMH1003P11F1A","MOTOR IEC 100MM 8,4NM IP54 HR. S DRÁŽ",1,"ks",1826.055,"3606485200538",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":8150,"d":"8,150.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1003P11F1A","servomotor BMH - 8.4 Nm - 6000 rpm - hriadeľ s perom - s brzdou - IP54",0.98]
["BMH1003P02A2A","MOTOR IEC 100MM 8,4NM IP54 HLADKÝ HRIAD.",1,"ks",{"v":1767.1499999999999,"d":"1767.150"},"3606485196428",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":6500,"d":"6,500.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1003P02A2A","servomotor BMH - 8.4 Nm - 6000 rpm - hladká hriadeľ - bez brzdy - IP54",0.78]
["BMH1002T31A2A","MOTOR IEC 100MM 6NM IP65 HRIADEĽ S DRÁŽ.",1,"ks",{"v":1423.1447999999998,"d":"1423.145"},"3606485200910",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":5220,"d":"5,220.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1002T31A2A","servomotor BMH - 6 Nm - 6000 rpm - hriadeľ s perom - bez brzdy - IP65/IP67",""]
["BMH1002T16F2A","MOTOR IEC 100MM 6,2NM IP54 HR. S DRÁŽ",1,"ks",1472.625,"3606485197579",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":6380,"d":"6,380.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1002T16F2A","servomotor BMH - 6 Nm - 6000 rpm - hriadeľ s perom - s brzdou - IP54",0.77]
["BMH1002T11A1A","MOTOR IEC 100MM 6NM IP54 HRIADEĽ S DRÁŽ.",1,"ks",1354.815,"3606485200811",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":4920,"d":"4,920.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1002T11A1A","servomotor BMH - 6 Nm - 6000 rpm - hriadeľ s perom - bez brzdy - IP54",0.59]
["BMH1002P37F1A","MOTOR IEC 100MM 6,2NM IP65 HR. S DRÁŽ",1,"ks",{"v":1767.1499999999999,"d":"1767.150"},"3606485196251",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":6380,"d":"6,380.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1002P37F1A","servomotor BMH - 6.2 Nm - 6000 rpm - hriadeľ s perom - s brzdou - IP65/IP67",0.77]
["BMH1002P21F2A","MOTOR IEC 100MM 5,9NM IP65 HLADKÝ HRIAD.",1,"ks",{"v":1649.34,"d":"1649.340"},"3606485200460",{"v":39.5,"d":"39.50"},{"v":19.5,"d":"19.50"},{"v":22,"d":"22.00"},{"v":6880,"d":"6,880.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1002P21F2A","servomotor BMH - 6.2 Nm - 6000 rpm - hladká hriadeľ - s brzdou - IP65/IP67",0.8300000000000001]
["BMH1002P21A1A","MOTOR IEC 100MM 5,9NM IP65 HLADKÝ HRIAD.",1,"ks",{"v":1325.3625,"d":"1325.363"},"3606485200347",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":5220,"d":"5,220.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1002P21A1A","servomotor BMH - 6.2 Nm - 6000 rpm - hladká hriadeľ - bez brzdy - IP65/IP67",""]
["BMH1002P07F2A","MOTOR IEC 100MM 6,2NM IP54 HLADKÝ HRIAD.",1,"ks",1708.245,"3606485196305",{"v":40,"d":"40.00"},{"v":19.5,"d":"19.50"},{"v":22,"d":"22.00"},{"v":6900,"d":"6,900.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1002P07F2A","servomotor BMH - 6.2 Nm - 6000 rpm - hladká hriadeľ - s brzdou - IP54",0.8300000000000001]
["BMH1001T36F2A","MOTOR IEC 100MM 3,6NM IP65 HR. S DRÁŽ",1,"ks",1354.815,"3606485197128",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":4800,"d":"4,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001T36F2A","servomotor BMH - 3.4 Nm - 6000 rpm - hriadeľ s perom - s brzdou - IP65/IP67",0.58]
["BMH1001T31F2A","MOTOR IEC 100MM 3,4NM IP65 HR. S DRÁŽ",1,"ks",{"v":1529.1738,"d":"1529.174"},"3606485200798",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":5100,"d":"5,100.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001T31F2A","servomotor BMH - 3.4 Nm - 6000 rpm - hriadeľ s perom - s brzdou - IP65/IP67",""]
["BMH1001T16A1A","MOTOR IEC 100MM 3,6NM IP54 HR. S DRÁŽ",1,"ks",{"v":974.2887,"d":"974.289"},"3606485196992",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":3640,"d":"3,640.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001T16A1A","servomotor BMH - 3.4 Nm - 6000 rpm - hriadeľ s perom - bez brzdy - IP54",""]
["BMH1001T11A2A","MOTOR IEC 100MM 3,4NM IP54 HR. S DRÁŽ",1,"ks",{"v":1207.5525,"d":"1207.553"},"3606485200736",{"v":40,"d":"40.00"},{"v":20,"d":"20.00"},{"v":22,"d":"22.00"},{"v":3640,"d":"3,640.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001T11A2A","servomotor BMH - 3.4 Nm - 6000 rpm - hriadeľ s perom - bez brzdy - IP54",""]
["BMH1001P36A2A","MOTOR IEC 100MM 3,6NM IP65 HR. S DRÁŽ",1,"ks",1036.728,"3606485195667",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":3340,"d":"3,340.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001P36A2A","servomotor BMH - 3.3 Nm - 6000 rpm - hriadeľ s perom - bez brzdy - IP65/IP67",0.4]
["BMH1001P21F2A","MOTOR IEC 100MM 3,4NM IP65 HLADKÝ HRIAD.",1,"ks",1472.625,"3606485200309",{"v":40,"d":"40.00"},{"v":22,"d":"22.00"},{"v":20,"d":"20.00"},{"v":4800,"d":"4,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001P21F2A","servomotor BMH - 3.3 Nm - 6000 rpm - hladká hriadeľ - s brzdou - IP65/IP67",0.58]
["BMH1001P16F1A","MOTOR IEC 100MM 3,6NM IP54 HR. S DRÁŽ",1,"ks",{"v":1237.0049999999999,"d":"1237.005"},"3606485195612",{"v":40,"d":"40.00"},{"v":20,"d":"20.00"},{"v":22,"d":"22.00"},{"v":5100,"d":"5,100.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001P16F1A","servomotor BMH - 3.3 Nm - 6000 rpm - hriadeľ s perom - s brzdou - IP54",0.61]
["BMH1001P07A2A","MOTOR IEC 100MM 3,6NM IP54 HLADKÝ HRIAD.",1,"ks",{"v":1237.0049999999999,"d":"1237.005"},"3606485195797",{"v":40,"d":"40.00"},{"v":20,"d":"20.00"},{"v":22,"d":"22.00"},{"v":3340,"d":"3,340.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001P07A2A","servomotor BMH - 3.3 Nm - 6000 rpm - hladká hriadeľ - bez brzdy - IP54",0.4]
["BMH1001P01F2A","MOTOR IEC 100MM 3,4NM IP54 HLADKÝ HRIAD.",1,"ks",1472.625,"3606485200286",{"v":40,"d":"40.00"},{"v":20,"d":"20.00"},{"v":22,"d":"22.00"},{"v":4800,"d":"4,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH1001P01F2A","servomotor BMH - 3.3 Nm - 6000 rpm - hladká hriadeľ - s brzdou - IP54",0.58]
["BMH0703T27A2A","MOTOR IEC 70MM 3,4NM IP65 HLADKÝ HRIADEĽ",1,"ks",1354.815,"3606485195346",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":2000,"d":"2,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0703T27A2A","servomotor BMH - 3.4 Nm - 8000 rpm - hladká hriadeľ - bez brzdy - IP65/IP67",0.24]
["BMH0703T17A2A","MOTOR IEC 70MM 3,4NM IP54 HRIAD. S DRÁŽ.",1,"ks",{"v":1295.9099999999999,"d":"1295.910"},"3606485195339",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":2000,"d":"2,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0703T17A2A","servomotor BMH - 3.4 Nm - 8000 rpm - hriadeľ s perom - bez brzdy - IP54",0.24]
["BMH0703P32F2A","MOTOR IEC 70MM 3,4NM IP65 HRIAD. S DRÁŽ.",1,"ks",1708.245,"3606485199344",{"v":39,"d":"39.00"},{"v":11,"d":"11.00"},{"v":19,"d":"19.00"},{"v":4000,"d":"4,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0703P32F2A","servomotor BMH - 3.4 Nm - 8000 rpm - hriadeľ s perom - s brzdou - IP65/IP67",0.5]
["BMH0703P16F1A","MOTOR IEC 70MM 3,4NM IP54 HRIAD. S DRÁŽ.",1,"ks",{"v":1178.1,"d":"1178.100"},"3606485199405",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":3000,"d":"3,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0703P16F1A","servomotor BMH - 3.4 Nm - 8000 rpm - hriadeľ s perom - s brzdou - IP54",0.36]
["BMH0703P12A1A","MOTOR IEC 70MM 3,4NM IP54 HRIAD. S DRÁŽ.",1,"ks",1472.625,"3606485199207",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":2000,"d":"2,000.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0703P12A1A","servomotor BMH - 3.4 Nm - 8000 rpm - hriadeľ s perom - bez brzdy - IP54",0.24]
["BMH0702T36A2A","MOTOR IEC 70MM 2,5NM IP65 HRIAD. S DRÁŽ.",1,"ks",{"v":1007.2755,"d":"1007.276"},"3606485194721",{"v":39,"d":"39.00"},{"v":11,"d":"11.00"},{"v":18.5,"d":"18.50"},{"v":2946,"d":"2,946.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0702T36A2A","servomotor BMH - 2.5 Nm - 8000 rpm - hriadeľ s perom - bez brzdy - IP65/IP67",0.35000000000000003]
["BMH0702T26F2A","MOTOR IEC 70MM 2,5NM IP65 HLADKÝ HRIADEĽ",1,"ks",{"v":1191.0591,"d":"1191.059"},"3606485194752",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":2800,"d":"2,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0702T26F2A","servomotor BMH - 2.5 Nm - 8000 rpm - hladká hriadeľ - s brzdou - IP65/IP67",""]
["BMH0702T07F2A","MOTOR IEC 70MM 2,5NM IP54 HLADKÝ HRIADEĽ",1,"ks",1472.625,"3606485194899",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":2200,"d":"2,200.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0702T07F2A","servomotor BMH - 2.5 Nm - 8000 rpm - hladká hriadeľ - s brzdou - IP54",0.26]
["BMH0702T01A2A","MOTOR IEC 70MM 2,5NM IP54 HLADKÝ HRIADEĽ",1,"ks",{"v":1148.6474999999998,"d":"1148.648"},"3606485199917",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":1800,"d":"1,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0702T01A2A","servomotor BMH - 2.5 Nm - 8000 rpm - hladká hriadeľ - bez brzdy - IP54",0.35000000000000003]
["BMH0702P26F2A","MOTOR IEC 70MM 2,5NM IP65 HLADKÝ HRIADEĽ",1,"ks",{"v":1155.7161,"d":"1155.716"},"3606485193816",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":2800,"d":"2,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0702P26F2A","servomotor BMH - 2.5 Nm - 8000 rpm - hladká hriadeľ - s brzdou - IP65/IP67",""]
["BMH0702P11A1A","MOTOR IEC 70MM 2,5NM IP54 HRIAD. S DRÁŽ.",1,"ks",{"v":1142.7569999999998,"d":"1142.757"},"3606485198880",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":1800,"d":"1,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0702P11A1A","servomotor BMH - 2.5 Nm - 8000 rpm - hriadeľ s perom - bez brzdy - IP54",0.22]
["BMH0702P02A1A","MOTOR IEC 70MM 2,5NM IP54 HLADKÝ HRIADEĽ",1,"ks",{"v":1413.72,"d":"1413.720"},"3606485193526",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":1800,"d":"1,800.00"},"DE","8501522089","https://www.se.com/sk/sk/product/BMH0702P02A1A","servomotor BMH - 2.5 Nm - 8000 rpm - hladká hriadeľ - bez brzdy - IP54",0.22]
["BMH0701T31A1A","MOTOR IEC 70MM 1,4NM IP65 HRIAD. S DRÁŽ.",1,"ks",1130.976,"3606485199702",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":1600,"d":"1,600.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BMH0701T31A1A","servomotor BMH - 1.4 Nm - 8000 rpm - hriadeľ s perom - bez brzdy - IP65/IP67",0.19]
["BMH0701T16F1A","MOTOR IEC 70MM 1,4NM IP54 HRIAD. S DRÁŽ.",1,"ks",1095.633,"3606485194202",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":2600,"d":"2,600.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BMH0701T16F1A","servomotor BMH - 1.4 Nm - 8000 rpm - hriadeľ s perom - s brzdou - IP54",0.31]
["BMH0701T07A2A","MOTOR IEC 70MM 1,4NM IP54 HLADKÝ HRIADEĽ",1,"ks",{"v":1172.2095,"d":"1172.210"},"3606485194387",{"v":39.5,"d":"39.50"},{"v":11,"d":"11.00"},{"v":19,"d":"19.00"},{"v":1600,"d":"1,600.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BMH0701T07A2A","servomotor BMH - 1.4 Nm - 8000 rpm - hladká hriadeľ - bez brzdy - IP54",0.26]
["BMH0701P36F2A","MOTOR IEC 70MM 1,4NM IP65 HRIAD. S DRÁŽ.",1,"ks",{"v":1134.5103,"d":"1134.510"},"3606485193359",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":2800,"d":"2,800.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BMH0701P36F2A","servomotor BMH - 1.2 Nm - 8000 rpm - hriadeľ s perom - s brzdou - IP65/IP67",0.31]
["BMH0701P21A2A","MOTOR IEC 70MM 1,4NM IP65 HLADKÝ HRIADEĽ",1,"ks",{"v":1101.5235,"d":"1101.524"},"3606485198811",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":1600,"d":"1,600.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BMH0701P21A2A","servomotor BMH - 1.2 Nm - 8000 rpm - hladká hriadeľ - bez brzdy - IP65/IP67",0.19]
["BMH0701P12A2A","MOTOR IEC 70MM 1,4NM IP54 HRIAD. S DRÁŽ.",1,"ks",1354.815,"3606485193144",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":1600,"d":"1,600.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BMH0701P12A2A","servomotor BMH - 1.2 Nm - 8000 rpm - hriadeľ s perom - bez brzdy - IP54",0.19]
["BMH0701P06A1A","MOTOR IEC 70MM 1,4NM IP54 HLADKÝ HRIADEĽ",1,"ks",{"v":818.7795,"d":"818.780"},"3606485193212",{"v":40,"d":"40.00"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":1600,"d":"1,600.00"},"DE","8501510090","https://www.se.com/sk/sk/product/BMH0701P06A1A","servomotor BMH - 1.2 Nm - 8000 rpm - hladká hriadeľ - bez brzdy - IP54",0.24]
["BLRCH258A310B48","KONDENZÁTOR CAN HDUTY 25.8/31 KVAR 480V",1,"ks",{"v":189,"d":"189.000"},"3606485255958",{"v":31,"d":"31.00"},{"v":19,"d":"19.00"},{"v":19,"d":"19.00"},{"v":2500,"d":"2,500.00"},"IN","8532100000","https://www.se.com/sk/sk/product/BLRCH258A310B48","VarplusCan HDuty kondenzátor - 25.8/31 kVAr - 480 V - 50/60Hz",0.37]
["BLRCH200A240B44","KONDENZÁTOR VARPLUSCAN HDY 20 KVAR 440V",1,"ks",{"v":157.5,"d":"157.500"},"3606485255828",{"v":32,"d":"32.00"},{"v":19.5,"d":"19.50"},{"v":20,"d":"20.00"},{"v":2500,"d":"2,500.00"},"IN","8532100000","https://www.se.com/sk/sk/product/BLRCH200A240B44","VarplusCan HDuty kondenzátor - 20/24 kVAr - 440 V - 50/60Hz",0.37]
["BLRCH030A036B40","KONDENZÁTOR CAN HDUTY 3.0/3.6 KVAR 400V",1,"ks",{"v":69.1425,"d":"69.143"},"3606480547591",{"v":26,"d":"26.00"},{"v":28,"d":"28.00"},{"v":10,"d":"10.00"},{"v":1080,"d":"1,080.00"},"IN","8532100000","https://www.se.com/sk/sk/product/BLRCH030A036B40","Kondenzátor VarplusCan HDY 3/3.6 kvar - 400V - 50/60Hz",""]
["BLRCS104A125B40","KONDENZÁTOR CANSDUTY 10.4/12.5 KVAR 400V",1,"ks",{"v":85.83749999999999,"d":"85.838"},"3606485256139",{"v":11.8,"d":"11.80"},{"v":28.5,"d":"28.50"},{"v":11,"d":"11.00"},{"v":1100,"d":"1,100.00"},"IN","8532100000","https://www.se.com/sk/sk/product/BLRCS104A125B40","VarplusCan SDuty kondenzátor - 10.4/12.5 kvar - 400 V - 50/60Hz",0.17]
["BLRCS025A030B40","KONDENZÁTOR CAN SDUTY 2.5/3 KVAR 400V",3,"ks",{"v":44.887499999999996,"d":"44.888"},"3606485253251",{"v":28.5,"d":"28.50"},{"v":11,"d":"11.00"},{"v":26.5,"d":"26.50"},{"v":612,"d":"612.00"},"IN","8532100000","https://www.se.com/sk/sk/product/BLRCS025A030B40","VarplusCan SDuty kondenzátor - 2.5/3 kVAr - 400 V - 50/60Hz",0.07]
["BCH2MR2022CF6C","BCH2 motor 180mm 2000W with oil seal wo",1,"ks",{"v":2905.1946,"d":"2905.195"},"3606480734731",{"v":58.5,"d":"58.50"},{"v":24.5,"d":"24.50"},{"v":29,"d":"29.00"},{"v":19630,"d":"19,630.00"},"CN","8501522089","https://www.se.com/sk/sk/product/BCH2MR2022CF6C","BCH2 motor 180mm 2000W with oil seal wo key 20-bit enc. brake straight con.",""]
["BCH2MM0912CA6C","BCH2 motor 130mm 900W with oil seal wo k",1,"ks",{"v":1212.2649,"d":"1212.265"},"3606480734649",{"v":36,"d":"36.00"},{"v":18.1,"d":"18.10"},{"v":23,"d":"23.00"},{"v":8550,"d":"8,550.00"},"CN","8501522089","https://www.se.com/sk/sk/product/BCH2MM0912CA6C","BCH2 motor 130mm 900W with oil seal wo key 20-bit enc. straight con.",""]
["BCH2MBA532CF5C","BCH2 motor 40mm 50W with oil seal wo key",1,"ks",{"v":861.1911,"d":"861.191"},"3606480733376",{"v":24,"d":"24.00"},{"v":8,"d":"8.00"},{"v":13,"d":"13.00"},{"v":793,"d":"793.00"},"CN","8501510090","https://www.se.com/sk/sk/product/BCH2MBA532CF5C","BCH2 motor 40mm 50W with oil seal wo key 20-bit enc. brake leads con.",""]
["BCH2LD0232CA5C","BCH2 motor 60mm 200W with oil seal wo ke",1,"ks",{"v":610.2558,"d":"610.256"},"3606480733529",{"v":26.5,"d":"26.50"},{"v":11.1,"d":"11.10"},{"v":14.5,"d":"14.50"},{"v":1670,"d":"1,670.00"},"CN","8501510090","https://www.se.com/sk/sk/product/BCH2LD0232CA5C","BCH2 motor 60mm 200W with oil seal wo key 20-bit enc. leads con.",1.03]
["BCPMA042S","BCPM MONITOR VÝKONU A ENERGIE 42 OKRUHOV",1,"ks",{"v":2293.1999999999994,"d":"2293.200"},"3606480299490",{"v":794,"d":"794.00"},{"v":159,"d":"159.00"},{"v":248,"d":"248.00"},{"v":2977.27,"d":"2,977.27"},"US","9030337000","https://www.se.com/sk/sk/product/BCPMA042S","BCPM meranie výkonu a energie - 42 delené jadro 100 A - 19 mm CT rozstup",0.38]
["AZ5DE025D","KÁBLOVÁ DUTINKA 2X2,5MM2",250,"ks",{"v":0.17718749999999997,"d":"0.177"},"3389110518924",{"v":1.4,"d":"1.40"},{"v":0.4,"d":"0.40"},{"v":0.4,"d":"0.40"},{"v":0.3,"d":"0.30"},"DE","8536901000","https://www.se.com/sk/sk/product/AZ5DE025D","Cable end, Linergy TR cable ends, twin conductor, blue, 2.5mm², for insulated cable, medium size, 5 sets of 50",0]
["ATV950U75N4","Frekvenčný menič 7,5 kW, In = 16,5 A, 3",1,"ks",{"v":2453.85,"d":"2453.850"},"3606480883798",{"v":80,"d":"80.00"},{"v":75,"d":"75.00"},{"v":60,"d":"60.00"},{"v":33500,"d":"33,500.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV950U75N4","frekvenčný menič - ATV950 - 7,5kW - 400/480V- s brzdným modulom - IP55",2.52]
["ATV950D45N4E","Frekvenčný menič 45 kW, In = 88 A, 3 x 3",1,"ks",{"v":7766.1359999999995,"d":"7766.136"},"3606480884030",{"v":106,"d":"106.00"},{"v":43,"d":"43.00"},{"v":50.5,"d":"50.50"},{"v":61000,"d":"61,000.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV950D45N4E","frekvenčný menič - ATV950 - 45kW - 400/480V- s brzd. modulem/spínačem - IP55",""]
["ATV950D22N4E","Frekvenčný menič 22 kW, In = 46,3 A, 3 x",1,"ks",4643.163,"3606480884009",{"v":80,"d":"80.00"},{"v":54,"d":"54.00"},{"v":39,"d":"39.00"},{"v":29800,"d":"29,800.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV950D22N4E","frekvenčný menič - ATV950 - 22kW - 400/480V- s brzd. modulem/spínačem - IP55",""]
["ATV930U75N4","Frekvenčný menič 7,5 kW, In = 16,5 A, 3",1,"ks",{"v":2274.2999999999997,"d":"2274.300"},"3606480883316",{"v":58.5,"d":"58.50"},{"v":34.5,"d":"34.50"},{"v":21.5,"d":"21.50"},{"v":7700,"d":"7,700.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV930U75N4","frekvenčný menič - ATV930 - 7,5kW - 400/480V - s brzdným modulom - IP21",1.23]
["ATV930U30N4Z","Frekvenčný menič 3 kW, In = 7,2 A",1,"ks",{"v":1615.95,"d":"1615.950"},"3606489740047",{"v":40,"d":"40.00"},{"v":31.8,"d":"31.80"},{"v":19,"d":"19.00"},{"v":4957,"d":"4,957.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV930U30N4Z","variable speed drive, Altivar Process ATV900, ATV930, 3kW, 380 to 480V, cabinet Integration, IP20",0.48]
["ATV930D75N4Z","Frekvenčný menič 75 kW, In = 145 A",1,"ks",{"v":9815.4,"d":"9815.400"},"3606489740160",{"v":111,"d":"111.00"},{"v":60,"d":"60.00"},{"v":43,"d":"43.00"},{"v":68000,"d":"68,000.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV930D75N4Z","variable speed drive, Altivar Process ATV900, ATV930, 75kW, 380 to 480V, cabinet Integration, IP20",8.290000000000001]
["ATV930D30M3C","Frekven.menič 30kW,In=123A,3x 200-240V",1,"ks",{"v":5506.2,"d":"5506.200"},"3606480883682",{"v":114.5,"d":"114.50"},{"v":46,"d":"46.00"},{"v":59,"d":"59.00"},{"v":60000,"d":"60,000.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV930D30M3C","frekvenčný menič - ATV930 - 30kW - 200/240V- bez brzdného modulu - IP21",7.2]
["ATV930D18Y6","Frekvenčný menič 18 kW, 500 - 690 V",1,"ks",{"v":4189.5,"d":"4189.500"},"3606481325310",{"v":80,"d":"80.00"},{"v":48,"d":"48.00"},{"v":40,"d":"40.00"},{"v":32000,"d":"32,000.00"},"IN","8504409590","https://www.se.com/sk/sk/product/ATV930D18Y6","variable speed drive, Altivar Process ATV900, ATV930, 18.5kW, 25hp, 500 to 690V, IP00",3.6]
["ATV930C16N4C","Frekvenčný menič 160 kW, In=302 A, 3x",1,"ks",{"v":18505.62,"d":"18505.620"},"3606480883477",{"v":103,"d":"103.00"},{"v":66,"d":"66.00"},{"v":48,"d":"48.00"},{"v":89800,"d":"89,800.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV930C16N4C","frekvenčný menič - ATV930 - 160kW - 400/480V - bez brzdného modulu - IP00",10.78]
["ATV930C11N4","FM 110 kW s integrovanou brzdnou jednot.",1,"ks",16677.801,"3606487109495",{"v":144.5,"d":"144.50"},{"v":68,"d":"68.00"},{"v":48.5,"d":"48.50"},{"v":128000,"d":"128,000.00"},"","","https://www.se.com/sk/sk/product/ATV930C11N4","variable speed drive, Altivar Process ATV900, ATV930, 110kW, 380 to 480V, with braking unit, IP20",14.16]
["ATV650D75N4","Frekvenční měnič 75kW, In=145A, 3 x 380",1,"ks",{"v":9216.9,"d":"9216.900"},"3606480701634",{"v":145,"d":"145.00"},{"v":70,"d":"70.00"},{"v":50,"d":"50.00"},{"v":95000,"d":"95,000.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV650D75N4","frekvenčný menič ATV650 - 75kW/100HP - 380...480V - IP55",10.92]
["ATV650C31N4F","Frekvenčný menič 315 kW, In=590A, IP54",1,"ks",{"v":42470.1585,"d":"42470.159"},"3606485410869",{"v":110.5,"d":"110.50"},{"v":214.5,"d":"214.50"},{"v":120,"d":"120.00"},{"v":475000,"d":"475,000.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV650C31N4F","frekvenčný menič ATV650 - 315kW - 380...440V - IP54 - odpojovač",57]
["ATV630U75M3","Frekvenční měnič 7,5kW, In=32,7A, 3 x 20",1,"ks",{"v":1915.2,"d":"1915.200"},"3606485406930",{"v":34,"d":"34.00"},{"v":27,"d":"27.00"},{"v":74,"d":"74.00"},{"v":17375,"d":"17,375.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV630U75M3","frekvenčný menič ATV630 - 7.5kW/10HP - 200...240V - IP21/UL typ 1",2.09]
["ATV630U22M3","Frekvenční měnič 2,2kW, In=11,2A, 3 x 20",1,"ks",{"v":1197,"d":"1197.000"},"3606480761638",{"v":40.5,"d":"40.50"},{"v":31.5,"d":"31.50"},{"v":19,"d":"19.00"},{"v":4500,"d":"4,500.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV630U22M3","frekvenčný menič ATV630 - 2.2kW/3HP - 200...240V - IP21/UL typ 1",0.73]
["ATV630D45M3","Frekvenční měnič 45kW, In=176A, 3 x 200",1,"ks",{"v":6344.099999999999,"d":"6344.100"},"3606480701535",{"v":112,"d":"112.00"},{"v":60,"d":"60.00"},{"v":43.5,"d":"43.50"},{"v":72500,"d":"72,500.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV630D45M3","frekvenčný menič ATV630 - 45kW/60HP - 200...240V - IP21/UL typ 1",6.6000000000000005]
["ATV630C25N4F","Frekvenčný menič 250 kW, In = 477A, IP21",1,"ks",35900.424,"3606485410791",{"v":110.5,"d":"110.50"},{"v":204.5,"d":"204.50"},{"v":120,"d":"120.00"},{"v":535000,"d":"535,000.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV630C25N4F","frekvenčný menič ATV630 - 250kW - 380...440V - IP21",64.2]
["ATV630C16N4F","Frekvenčný menič 160 kW, In=302 A",1,"ks",23074.569,"3606485410388",{"v":75,"d":"75.00"},{"v":258,"d":"258.00"},{"v":85,"d":"85.00"},{"v":362000,"d":"362,000.00"},"CN","8504409590","https://www.se.com/sk/sk/product/ATV630C16N4F","frekvenčný menič ATV630 - 160kW - 380...440V - IP21",43.44]
["ATV340U15N4S","Frekvenčný menič 1,5 kW, In = 4 A, 3 x 3",1,"ks",807.975,"3606489497828",{"v":35.3,"d":"35.30"},{"v":10.7,"d":"10.70"},{"v":28.8,"d":"28.80"},{"v":1700,"d":"1,700.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV340U15N4S","variable speed drive, Altivar Machine ATV340, 1.5kW, heavy duty, 400V, 3 phases, Sercos",0.27]
["ATV340D15N4E","Frekvenčný menič 15 kW, In = 32 A, 3 x 3",1,"ks",{"v":2513.7,"d":"2513.700"},"3606480967061",{"v":56,"d":"56.00"},{"v":34,"d":"34.00"},{"v":30.5,"d":"30.50"},{"v":9500,"d":"9,500.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV340D15N4E","frek.menič ATV340-15kW-380...400V-3f-EMC filter-IP20-trieda 3C3 a 3S3-Ethernet",1.36]
["ATV320U75N4B","Frekvenčný menič 7,5 kW, In = 17 A, 3 x",1,"ks",{"v":1436.3999999999999,"d":"1436.400"},"3606480931307",{"v":32.8,"d":"32.80"},{"v":20.5,"d":"20.50"},{"v":27.2,"d":"27.20"},{"v":4400,"d":"4,400.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV320U75N4B","frekvenčný menič ATV320-7,5kW-380...500V-3f-EMC filter-IP20-3C3 a 3S2-Book",0.67]
["ATV320U22N4C","Frekvenčný menič 2,2 kW, In = 5,5 A, 3 x",1,"ks",736.155,"3606480966767",{"v":26.7,"d":"26.70"},{"v":24.5,"d":"24.50"},{"v":19.5,"d":"19.50"},{"v":2100,"d":"2,100.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV320U22N4C","frekvenčný menič ATV320-2,2kW-380...500V-3f -EMC filter-IP20-3C3 a 3S2-Compact",0.32]
["ATV320U22M2W","Frekvenčný menič 2,2 kW, In = 11 A, 1 x",1,"ks",784.035,"3606489548452",{"v":45,"d":"45.00"},{"v":29.3,"d":"29.30"},{"v":30.5,"d":"30.50"},{"v":9918,"d":"9,918.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV320U22M2W","variable speed drive, Altivar Machine ATV320, 2.2kW, 200 to 240V, 1 phase, enclosed",0.89]
["ATV320U07N4C","Frekvenčný menič 0,75 kW, In = 2,3 A, 3",1,"ks",{"v":502.73999999999995,"d":"502.740"},"3606480966736",{"v":18.5,"d":"18.50"},{"v":18,"d":"18.00"},{"v":19,"d":"19.00"},{"v":1664,"d":"1,664.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV320U07N4C","frekvenčný menič ATV320-0,75kW-380...500V-3f -EMC filter-IP20-3C3 a 3S2-Compact",0.2]
["ATV320U04N4C","Frekvenčný menič 0,37 kW, In = 1,5 A, 3",1,"ks",{"v":395.01,"d":"395.010"},"3606480966712",{"v":19,"d":"19.00"},{"v":18,"d":"18.00"},{"v":18.6,"d":"18.60"},{"v":1637,"d":"1,637.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV320U04N4C","frekvenčný menič ATV320-0,37kW-380...500V-3f-EMC filter-IP20-3C3 a 3S2-Compact",0.2]
["ATV320D15N4B","Frekvenčný menič 15 kW, In = 33 A, 3 x 3",1,"ks",{"v":2214.45,"d":"2214.450"},"3606480931321",{"v":27.1,"d":"27.10"},{"v":23,"d":"23.00"},{"v":42,"d":"42.00"},{"v":8777,"d":"8,777.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV320D15N4B","frekvenčný menič ATV320-15 kW-380 ...500V -3f-EMC filter-IP20-3C3 a 3S2-Book",1.04]
["ATV12HU40M3","ATV12 3F 4KW 240V",1,"ks",{"v":562.771125,"d":"562.771"},"3606480071201",{"v":26.8,"d":"26.80"},{"v":25,"d":"25.00"},{"v":19.5,"d":"19.50"},{"v":2000,"d":"2,000.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV12HU40M3","variable speed drive, Altivar 12, 4kW, 5hp, 200 to 240V, 3 phases, with heat sink",0.29]
["ATV12H075F1","ATV12 1F 0,75KW 120V",1,"ks",{"v":311.1255,"d":"311.126"},"3606480071034",{"v":19,"d":"19.00"},{"v":17,"d":"17.00"},{"v":19.5,"d":"19.50"},{"v":1587,"d":"1,587.00"},"ID","8504409590","https://www.se.com/sk/sk/product/ATV12H075F1","variable speed drive, Altivar 12, 0.75kW, 1hp, 100 to 120V, 1 phase, with heat sink",0.19]
["ATS480D88Y","Softštartér 45kW, 88A, 208 až 690 V",1,"ks",{"v":2453.85,"d":"2453.850"},"3606481089069",{"v":39,"d":"39.00"},{"v":37,"d":"37.00"},{"v":31,"d":"31.00"},{"v":9785,"d":"9,785.00"},"ID","8537109899","https://www.se.com/sk/sk/product/ATS480D88Y","Altivar Softštartér 45kW, 88A, 208 až 690 V",1.17]
["ATS480C48Y","Softštartér 250kW, 480A, 208 až 690 V",1,"ks",{"v":8857.8,"d":"8857.800"},"3606481089144",{"v":81,"d":"81.00"},{"v":55,"d":"55.00"},{"v":53,"d":"53.00"},{"v":61000,"d":"61,000.00"},"CN","8537109899","https://www.se.com/sk/sk/product/ATS480C48Y","Altivar Softštartér 250kW, 480A, 208 až 690 V",7.32]
["ATS22D62S6","SOFŠTARTÉR 30kW, 62A, 208 - 600 V",1,"ks",{"v":1436.3999999999999,"d":"1436.400"},"3606480167300",{"v":36,"d":"36.00"},{"v":30,"d":"30.00"},{"v":25,"d":"25.00"},{"v":8350,"d":"8,350.00"},"CN","8537109899","https://www.se.com/sk/sk/product/ATS22D62S6","softštartér- ATS22 - ovl. 220V - výkon 230V(15kW)/400...440V(30kW)/500V(37kW)",1.02]
["ATS22C48S6","SOFŠTARTÉR 250kW, 480A, 208 - 600 V",1,"ks",{"v":6523.65,"d":"6523.650"},"3606480211355",{"v":60,"d":"60.00"},{"v":53,"d":"53.00"},{"v":40,"d":"40.00"},{"v":40000,"d":"40,000.00"},"CN","8537109899","https://www.se.com/sk/sk/product/ATS22C48S6","softštartér-ATS22-ovl. 220V-výkon 230V(132kW)/400...440V(250kW)/500V(315kW)",4.8]
["ATS22C11S6","SOFŠTARTÉR 55kW, 110A, 208 - 600 V",1,"ks",{"v":2214.45,"d":"2214.450"},"3606480167331",{"v":41,"d":"41.00"},{"v":26,"d":"26.00"},{"v":33,"d":"33.00"},{"v":12900,"d":"12,900.00"},"CN","8537109899","https://www.se.com/sk/sk/product/ATS22C11S6","softštartér- ATS22 - ovl. 220V - výkon 230V(30kW)/400...440V(55kW)/500V(75kW)",1.55]
["ATS01N109FT","ATS01 1F/3F 9A (400V=4kW) LEN ROZBEH",1,"ks",{"v":192.16574999999997,"d":"192.166"},"3389110667158",{"v":15.5,"d":"15.50"},{"v":5.5,"d":"5.50"},{"v":17,"d":"17.00"},{"v":344,"d":"344.00"},"DE","8537109899","https://www.se.com/sk/sk/product/ATS01N109FT","softštartér pre asynchrónny motor – ATS01 – 9 A – 110 - 480 V – 1,1 - 4 kW",0.04]
["ASILUFC51","TESYS U - MODUL ASI",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389110745092",{"v":3.3,"d":"3.30"},{"v":4.8,"d":"4.80"},{"v":9.4,"d":"9.40"},{"v":59,"d":"59.00"},"FR","8536201090","https://www.se.com/sk/sk/product/ASILUFC51","komunikačný modul - pre TeSys U",0.01]
["AR1MB01P","ŠTÍTOK P",200,"ks",{"v":0.0118125,"d":"0.012"},"3389110574265",{"v":0.5,"d":"0.50"},{"v":0.3,"d":"0.30"},{"v":0.3,"d":"0.30"},{"v":0.035,"d":"0.04"},"FR","3926909790","https://www.se.com/sk/sk/product/AR1MB01P","žltá nacvakávacia značka-symbol P - sada 200",0]
["AR1MB01G","ŠTÍTOK G",200,"ks",{"v":0.0118125,"d":"0.012"},"3389110574180",{"v":0.5,"d":"0.50"},{"v":0.3,"d":"0.30"},{"v":0.3,"d":"0.30"},0.04,"FR","3926909790","https://www.se.com/sk/sk/product/AR1MB01G","Marker, Linergy TR cable ends, yellow, clipin type, character G, symbolic, set of 200",0]
["AR1MA016","ŠTÍTOK 6",200,"ks",{"v":0.0118125,"d":"0.012"},"3389110574081",{"v":0.5,"d":"0.50"},{"v":0.3,"d":"0.30"},{"v":0.3,"d":"0.30"},{"v":0.035,"d":"0.04"},"FR","3926909790","https://www.se.com/sk/sk/product/AR1MA016","žltá nacvakávacia značka-číselný znak 6 - sada 200",0]
["AK5JB144","BUSBAR TETRA 160A LG 452",1,"ks",{"v":171.28125,"d":"171.281"},"3389110576795",{"v":52.5,"d":"52.50"},{"v":11,"d":"11.00"},{"v":11,"d":"11.00"},{"v":900,"d":"900.00"},"FR","8536909500","https://www.se.com/sk/sk/product/AK5JB144","zbernica 160A - dĺžka 452 mm - pre AK5",0]
["AK2GA69","KÁBLOVY KANÁL",8,"ks",{"v":20.13165,"d":"20.132"},"3389110570564",{"v":215,"d":"215.00"},{"v":18.5,"d":"18.50"},{"v":14.5,"d":"14.50"},{"v":916,"d":"916.00"},"FR","3926909790","https://www.se.com/sk/sk/product/AK2GA69","káblový žlab 2m - 60x90mm - modrý - 2m",0]
["AK2CD125","KRYT PRE KANÁL Š=125MM SIVÝ",8,"ks",{"v":13.2685875,"d":"13.269"},"3389110570618",{"v":200,"d":"200.00"},{"v":3.5,"d":"3.50"},{"v":12.5,"d":"12.50"},{"v":600,"d":"600.00"},"FR","3925908000","https://www.se.com/sk/sk/product/AK2CD125","kryt pre káblový žlab - 125mm - šedý - 2m",0]
["AF1VA416","SKRUT.PRIEMER 4MM",100,"ks",{"v":0.18301499999999998,"d":"0.183"},"3389110568561",{"v":2,"d":"2.00"},{"v":0.5,"d":"0.50"},{"v":0.5,"d":"0.50"},{"v":2,"d":"2.00"},"IT","7318155890","https://www.se.com/sk/sk/product/AF1VA416","šesťhranný šrób M4x16 - obj. množstvo 100 ks",0]
["ABT7ESM025B","OPT. TRANSFORMÁTOR 24V 250VA",1,"ks",{"v":210.46724999999998,"d":"210.467"},"3389119400800",{"v":14.8,"d":"14.80"},{"v":25.5,"d":"25.50"},{"v":18.5,"d":"18.50"},{"v":3540,"d":"3,540.00"},"CZ","8504318090","https://www.se.com/sk/sk/product/ABT7ESM025B","menič napätia – 230 V – 1 x 24 V – 250 VA",0.47000000000000003]
["ABS7EA3M5","VÝMENNÉ RELÉ VSTUPNÉ 230-240VST, 12MM",4,"ks",{"v":54.1926,"d":"54.193"},"3389110720853",{"v":6.5,"d":"6.50"},{"v":5,"d":"5.00"},{"v":5.2,"d":"5.20"},{"v":13,"d":"13.00"},"FR","8536490099","https://www.se.com/sk/sk/product/ABS7EA3M5","výmenné vstupné tranzistorové relé- 12.5 mm - vstup - 230..240 V AC 50HZ",0]
["ABLS1A24038","Rad Modicon Opti, 24V, 3.8A 1f.",1,"ks",{"v":114.38437499999999,"d":"114.384"},"3606481500212",{"v":11.9,"d":"11.90"},5.25,{"v":8.6,"d":"8.60"},{"v":374,"d":"374.00"},"TH","8504408390","https://www.se.com/sk/sk/product/ABLS1A24038","Regulated Power Supply, 100...240V AC, 24V, 3.8A, single phase, Optimized",0.04]
["ABLM1A12042","Modulární řada Modicon, 12V, 4,2A",1,"ks",{"v":123.53512499999998,"d":"123.535"},"3606481500168",{"v":11,"d":"11.00"},{"v":6.1,"d":"6.10"},{"v":6.1,"d":"6.10"},{"v":221,"d":"221.00"},"TH","8504408390","https://www.se.com/sk/sk/product/ABLM1A12042","Regulated Power Supply, 100...240V AC, 12V, 4.2A, single phase, Modular",0.03]
["ABL8RED24400","REDUNDANTNÝ MODUL 40A",1,"ks",{"v":178.43962499999998,"d":"178.440"},"3389119406871",{"v":16,"d":"16.00"},{"v":6.5,"d":"6.50"},{"v":16.5,"d":"16.50"},{"v":575,"d":"575.00"},"CN","8536909500","https://www.se.com/sk/sk/product/ABL8RED24400","záložný modul – 40 A – pre regulovaný spínaný zdroj",0.07]
["ABL6TS100U","TRF 230-400/230 1KVA",1,"ks",622.251,"3389110880311",{"v":30,"d":"30.00"},{"v":24,"d":"24.00"},{"v":28,"d":"28.00"},{"v":14300,"d":"14,300.00"},"CZ","8504318090","https://www.se.com/sk/sk/product/ABL6TS100U","menič napätia – 230 - 400 V – 1 x 230 V – 1000 VA",1.8900000000000001]
["ABL6TS06B","TRANSFORMÁTOR 230-400/24V 63VA",1,"ks",{"v":132.68587499999998,"d":"132.686"},"3389110585780",{"v":15,"d":"15.00"},{"v":18.6,"d":"18.60"},{"v":12.6,"d":"12.60"},{"v":1655,"d":"1,655.00"},"CZ","8504318090","https://www.se.com/sk/sk/product/ABL6TS06B","menič napätia – 230 - 400 V – 1 x 24 V – 63 VA",0.2]
["ABFH20H300","PREPOJOVACÍ KÁBEL HE20 3M",1,"ks",{"v":80.69985,"d":"80.700"},"3389110588514",{"v":22.5,"d":"22.50"},{"v":3.5,"d":"3.50"},{"v":18.5,"d":"18.50"},{"v":191,"d":"191.00"},"CN","8544429090","https://www.se.com/sk/sk/product/ABFH20H300","rolled ribbon cable - 3 m - for Modicon Premium",0]
["ABFC08R02R","KÁBLOVÁ PREPOJKA 8 PÓL /1MM2 ČERVENÁ 2CM",1,"ks",{"v":14.726249999999999,"d":"14.726"},"3389110474770",{"v":7.5,"d":"7.50"},{"v":0.5,"d":"0.50"},{"v":3,"d":"3.00"},{"v":7,"d":"7.00"},"FR","8536901000","https://www.se.com/sk/sk/product/ABFC08R02R","commoning link for connection sub-base - for common AC - red - 2 cm",0]
["ABE7R08S210","INTERFACE TELEFASTII-VYST.RELE",1,"ks",{"v":265.0725,"d":"265.073"},"3389110545265",{"v":13.7,"d":"13.70"},{"v":7.2,"d":"7.20"},{"v":8.2,"d":"8.20"},{"v":355,"d":"355.00"},"FR","8536909500","https://www.se.com/sk/sk/product/ABE7R08S210","sokl - výstupná relé svorkovnica ABE7 - 8 kanálov - relé 10 mm",0]
["ABE7H16S43","SVORKOVNICA 16K/2S VSTUPY TYP 2",1,"ks",{"v":276.8535,"d":"276.854"},"3389110644524",{"v":21,"d":"21.00"},{"v":7,"d":"7.00"},{"v":8.2,"d":"8.20"},{"v":624,"d":"624.00"},"FR","8536909500","https://www.se.com/sk/sk/product/ABE7H16S43","pasívne pripojenie zákl. ABE7 - 16 vstupov - fuses - LED - izol.",0]
["ABE7H16R31","TELEFAST SYSTEM PREPOJENIA",1,"ks",176.715,"3389110544985",{"v":14,"d":"14.00"},{"v":6.8,"d":"6.80"},{"v":9,"d":"9.00"},{"v":355,"d":"355.00"},"FR","8536909500","https://www.se.com/sk/sk/product/ABE7H16R31","pasívne pripojenie zákl. ABE7 - 16 vstupy alebo výstupy - LED",0]
["ABE7FU100","RÝCHLA POISTKA 5X20 250V 1A",10,"ks",{"v":1.7671499999999998,"d":"1.767"},"3389110602838",{"v":7,"d":"7.00"},{"v":1,"d":"1.00"},{"v":2.5,"d":"2.50"},{"v":1.1,"d":"1.10"},"CH","8536101090","https://www.se.com/sk/sk/product/ABE7FU100","poistková vložka 5 x 20 – tavná poistka 1 A – bez indikácie",0]
["ABE7ACC21","PREPOJOVACÍ BLOK 12MM",1,"ks",{"v":159.0435,"d":"159.044"},"3389110715941",{"v":6.5,"d":"6.50"},{"v":5,"d":"5.00"},{"v":5.2,"d":"5.20"},{"v":10,"d":"10.00"},"FR","8538909999","https://www.se.com/sk/sk/product/ABE7ACC21","príslušenstvo pre pripoj.soklu - pripojovací blok šírka 12,5 mm",0]
["A9Z83463","PR. CHRÁNIČ IID 4P 63A 100MA-S A THV",1,"ks",{"v":149.93999999999997,"d":"149.940"},"3606480442902",{"v":10,"d":"10.00"},{"v":7.5,"d":"7.50"},{"v":8.3,"d":"8.30"},{"v":382,"d":"382.00"},"ES","8536303099","https://www.se.com/sk/sk/product/A9Z83463","Acti 9 - prúdový chránič iID - 4P - 63A - 100mA - typ S A THV",0.05]
["A9Z61225","Prúdový chránič iID 2P 25A 30mA typ B-SI",1,"ks",{"v":533.6099999999999,"d":"533.610"},"3606489502744",{"v":9.9,"d":"9.90"},{"v":7.5,"d":"7.50"},{"v":8.5,"d":"8.50"},{"v":363,"d":"363.00"},"ES","8536303099","https://www.se.com/sk/sk/product/A9Z61225","prúdový chránič iID 2P 25A 30mA typ B-SI 230V",0.04]
["A9Z35463","PR. CHRÁN. ACTI9 IID 4P 63A 300MA-S A-SI",1,"ks",{"v":224.90999999999997,"d":"224.910"},"3606480442780",{"v":10,"d":"10.00"},{"v":7.5,"d":"7.50"},{"v":8.5,"d":"8.50"},{"v":378,"d":"378.00"},"ES","8536303099","https://www.se.com/sk/sk/product/A9Z35463","prúdový chránič iID - 4P - 63A - 300mA - typ S ASI",0.05]
["A9Z25480","PR. CHRÁNIČ ACTI9 IID 4P 80A 300MA-S A",1,"ks",{"v":176.39999999999998,"d":"176.400"},"3606480443343",{"v":9.8,"d":"9.80"},{"v":7.5,"d":"7.50"},{"v":8.2,"d":"8.20"},{"v":370,"d":"370.00"},"ES","85363030","https://www.se.com/sk/sk/product/A9Z25480","prúdový chránič iID - 4P - 80A - 300mA - typ S A",0.04]
["A9Z24425","PR. CHRÁNIČ ACTI9 IID 4P 25A 300MA A",1,"ks",69.237,"3606480443183",{"v":10,"d":"10.00"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":377.4,"d":"377.40"},"ES","8536303099","https://www.se.com/sk/sk/product/A9Z24425","prúdový chránič iID - 4P - 25A - 300mA - typ A",0.05]
["A9Z21425","PR. CHRÁNIČ ACTI9 IID 4P 25A 30MA A",1,"ks",57.771,"3606480443176",{"v":10,"d":"10.00"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":377.5,"d":"377.50"},"ES","8536303099","https://www.se.com/sk/sk/product/A9Z21425","prúdový chránič iID - 4P - 25A - 30mA - typ A",0.05]
["A9Z14463","PR. CHRÁNIČ ACTI9 IID 4P 63A 300MA AC",1,"ks",{"v":92.61,"d":"92.610"},"3606480442445",{"v":10,"d":"10.00"},{"v":7.5,"d":"7.50"},{"v":8.5,"d":"8.50"},{"v":375,"d":"375.00"},"ES","85363030","https://www.se.com/sk/sk/product/A9Z14463","prúdový chránič iID - 4P - 63A - 300mA - typ AC",0.05]
["A9Z06463","PR. CHRÁNIČ ID K 4P 63A 300 MA AC",1,"ks",{"v":92.61,"d":"92.610"},"3606480500510",{"v":9.2,"d":"9.20"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":344,"d":"344.00"},"ES","85363030","https://www.se.com/sk/sk/product/A9Z06463","prúdový chránič iIDK - 4P - 63A - 300mA - typ AC",0.04]
["A9Z05240","PR. CHRÁNIČ ID K 2P 40A 30 MA AC",1,"ks",{"v":48.95099999999999,"d":"48.951"},"3606480473890",{"v":9,"d":"9.00"},{"v":4,"d":"4.00"},{"v":8.5,"d":"8.50"},{"v":181,"d":"181.00"},"ES","85363030","https://www.se.com/sk/sk/product/A9Z05240","prúdový chránič iIDK - 2P - 40A - 30mA - typ AC",0.02]
["A9XPH724","COMB BUSBAR BOTTOM 3PN 24 MODULES",5,"ks",{"v":53.80199999999999,"d":"53.802"},"3606480794162",{"v":43.8,"d":"43.80"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":331,"d":"331.00"},"DE","8536909500","https://www.se.com/sk/sk/product/A9XPH724","comb busbar bottom, Acti9, 3P+N balanced, 9 mm pitch, 24 modules, 80 A",0]
["A9XPH157","HREBEŇ. PREPOJ. LIŠTA 1P 100A 57MOD.",1,"ks",{"v":18.521999999999995,"d":"18.522"},"3606480485114",{"v":106,"d":"106.00"},0.52,{"v":0.9,"d":"0.90"},{"v":234,"d":"234.00"},"DE","8536909500","https://www.se.com/sk/sk/product/A9XPH157","prepojovacia lišta - deliteľná Acti 9- 1P - 57 mod. - 100A",0.03]
["A9XPH106","HREBEŇ. PREPOJ. LIŠTA 1P 100A 6MOD.",1,"ks",{"v":4.9392,"d":"4.939"},"3606480484995",{"v":24.7,"d":"24.70"},{"v":6,"d":"6.00"},{"v":8.6,"d":"8.60"},{"v":25,"d":"25.00"},"DE","8536909500","https://www.se.com/sk/sk/product/A9XPH106","prepojovacia lišta - deliteľná Acti 9- 1P - 6 mod. - 100A",0]
["A9XMSB11","SMART MODBUS RS485 I/O MOD",1,"ks",{"v":448.8749999999999,"d":"448.875"},"3606480430602",{"v":36.4,"d":"36.40"},{"v":3.4,"d":"3.40"},{"v":6.4,"d":"6.40"},{"v":271,"d":"271.00"},"FR","8517620000","https://www.se.com/sk/sk/product/A9XMSB11","Acti9 Smartlink Modbus RS485 smart komunikačný modul I/O",0]
["A9XAH157","HREBEŇ. PREPOJ. LIŠTA AUX1P 100A 57MOD.",1,"ks",{"v":24.695999999999994,"d":"24.696"},"3606480485121",{"v":107,"d":"107.00"},{"v":5.5,"d":"5.50"},{"v":9,"d":"9.00"},{"v":160,"d":"160.00"},"DE","8536909500","https://www.se.com/sk/sk/product/A9XAH157","prepojovacia lišta - deliteľná Acti 91P + AUX 57 mod. 100A",0.02]
["A9W35463","ACTI9 VIGI IC60 4P 63A 300MA-S ASI",1,"ks",{"v":260.19,"d":"260.190"},"3606480443732",{"v":14,"d":"14.00"},{"v":8.5,"d":"8.50"},{"v":11.5,"d":"11.50"},{"v":249,"d":"249.00"},"FR","8536303099","https://www.se.com/sk/sk/product/A9W35463","chr. spúšť Vigi iC60 4P 63A 300mA-S A-SI pre istič iC60N, iC60H",0.03]
["A9W21225","ACTI9 VIGI IC60 2P 25A 30MA A",1,"ks",{"v":119.07,"d":"119.070"},"3606480443404",{"v":11.2,"d":"11.20"},{"v":8.6,"d":"8.60"},{"v":7.2,"d":"7.20"},{"v":145,"d":"145.00"},"FR","8536303099","https://www.se.com/sk/sk/product/A9W21225","chr. spúšť Vigi iC60 2P 25A 30mA A pre istič iC60N, iC60H",0.02]
["A9V65463","ACTI9 VIGI IC60 4P 63A 300MA-S ASI",1,"ks",{"v":273.41999999999996,"d":"273.420"},"3606480087820",{"v":14.7,"d":"14.70"},{"v":8.7,"d":"8.70"},{"v":12,"d":"12.00"},{"v":252,"d":"252.00"},"CN","8536303099","https://www.se.com/sk/sk/product/A9V65463","Vigi iC60 - earth leakage add-on block - 4P - 63A - 300mA - SI type - selective",0.03]
["A9V51225","ACTI9 VIGI IC60 2P 25A 30MA A",1,"ks",{"v":88.19999999999999,"d":"88.200"},"3606480090653",{"v":14.6,"d":"14.60"},{"v":8.8,"d":"8.80"},{"v":13.4,"d":"13.40"},{"v":145,"d":"145.00"},"FR","8536303099","https://www.se.com/sk/sk/product/A9V51225","chráničová spúšť Vigi iC60 2P 25A pre istič iC60L",0.02]
["A9V41325","ACTI9 VIGI IC60 3P 25A 30MA AC-TYP",1,"ks",{"v":114.66,"d":"114.660"},"3606480087349",{"v":14,"d":"14.00"},{"v":8.5,"d":"8.50"},{"v":11.5,"d":"11.50"},{"v":200,"d":"200.00"},"FR","8536303099","https://www.se.com/sk/sk/product/A9V41325","chráničová spúšť Vigi iC60 3P 25A 30mA AC pre istič iC60L",0.02]
["A9V22225","ACTI9 VIGI IC60 2P 25A 100MA A",1,"ks",{"v":58.71473999999998,"d":"58.715"},"3606480090950",{"v":11.5,"d":"11.50"},{"v":8.5,"d":"8.50"},{"v":7.7,"d":"7.70"},{"v":140.9,"d":"140.90"},"FR","8536303099","https://www.se.com/sk/sk/product/A9V22225","Vigi iC60 - earth leakage add-on block - 2P - 25A - 100mA - A type",""]
["A9S70790","ACTI9 ISW-NA VYPÍNAČ 3P+N 100A 415VAC",1,"ks",{"v":198.44999999999996,"d":"198.450"},"3606480098970",{"v":10,"d":"10.00"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":330.2,"d":"330.20"},"ES","8536508090","https://www.se.com/sk/sk/product/A9S70790","vypínač iSW-NA - 3P + N - 100 A",0.04]
["A9S65291","ACTI9 ISW VYPÍNAČ 2P 100A 415VAC",1,"ks",44.541,"3606480531132",{"v":9.5,"d":"9.50"},{"v":3.6,"d":"3.60"},{"v":7.5,"d":"7.50"},{"v":167,"d":"167.00"},"HU","8536508090","https://www.se.com/sk/sk/product/A9S65291","odpínač iSW - 2P - 100 A - 240 V",0.02]
["A9S60232","ACTI9 ISW VYPÍNAČ 2P 32A 415V",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3606480088728",7.55,{"v":7.7,"d":"7.70"},{"v":1.8,"d":"1.80"},{"v":65,"d":"65.00"},"BE","8536508090","https://www.se.com/sk/sk/product/A9S60232","vypínač Acti9 iSW - 2P - 32 A - 415V",0.01]
["A9R44225","PR.CHRÁNIČ ACTI9 IID 2P 25A 300MA AC exp",1,"ks",{"v":75.41099999999999,"d":"75.411"},"3606480089015",{"v":10,"d":"10.00"},{"v":8.5,"d":"8.50"},{"v":4,"d":"4.00"},{"v":188.9,"d":"188.90"},"ES","8536201090","https://www.se.com/sk/sk/product/A9R44225","prúdový chránič iID - 2P - 25A - 300mA - typ AC",0.02]
["A9R35440","PR.CHRÁNIČ ACTI9 IID 4P 40A 300MA-S A-SI",1,"ks",{"v":264.59999999999997,"d":"264.600"},"3606480089671",{"v":10,"d":"10.00"},{"v":7.5,"d":"7.50"},{"v":8.5,"d":"8.50"},{"v":351,"d":"351.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9R35440","prúdový chránič iID - 4P - 40A - 300mA - typ SI",0.04]
["A9R24240","PR.CHRÁNIČ ACTI9 IID 2P 40A 300MA A expo",1,"ks",{"v":101.42999999999998,"d":"101.430"},"3606480374692",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8.3,"d":"8.30"},{"v":193,"d":"193.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9R24240","prúdový chránič iID - 2P - 40A - 300mA - typ A",0.02]
["A9R21425","ACTI9 IID 4P 25A 30MA A-TYP",1,"ks",{"v":136.70999999999998,"d":"136.710"},"3606480090851",{"v":10,"d":"10.00"},{"v":7.6,"d":"7.60"},{"v":8.2,"d":"8.20"},{"v":360.8,"d":"360.80"},"ES","85363030","https://www.se.com/sk/sk/product/A9R21425","prúdový chránič iID - 4P - 25A - 30mA - typ A",0.04]
["A9P64725","Istič Acti9 iC40N 3P+N 25A D 6kA",1,"ks",{"v":35.72099999999999,"d":"35.721"},"3606481326249",{"v":9.4,"d":"9.40"},{"v":5.4,"d":"5.40"},{"v":7.4,"d":"7.40"},{"v":341,"d":"341.00"},"HU","8536201090","https://www.se.com/sk/sk/product/A9P64725","Miniature circuit breaker (MCB), Acti9 iC40N, 3P+N, 25A, D curve, 6000A (IEC/EN 60898-1), 10kA (IEC/EN 60947-2)",0.04]
["A9P64616","Istič Acti9 iC40N 1P+N 16A D 6kA",1,"ks",16.758,"3606481324719",{"v":9.4,"d":"9.40"},{"v":1.8,"d":"1.80"},{"v":7.4,"d":"7.40"},{"v":115,"d":"115.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9P64616","Miniature circuit breaker (MCB), Acti9 iC40N, 1P+N, 16A, D curve, 6000A (IEC/EN 60898-1), 10kA (IEC/EN 60947-2)",0.01]
["A9P54713","Istič Acti9 iC40N 3P+N 13A C 6kA",1,"ks",{"v":30.869999999999997,"d":"30.870"},"3606481326133",{"v":9.4,"d":"9.40"},{"v":5.4,"d":"5.40"},{"v":7.4,"d":"7.40"},{"v":322,"d":"322.00"},"HU","8536201090","https://www.se.com/sk/sk/product/A9P54713","Miniature circuit breaker (MCB), Acti9 iC40N, 3P+N, 13A, C curve, 6000A (IEC/EN 60898-1), 10kA (IEC/EN 60947-2)",0.04]
["A9P54610","Istič Acti9 iC40N 1P+N 10A C 6kA",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3606481324603",{"v":9.4,"d":"9.40"},{"v":1.8,"d":"1.80"},{"v":7.4,"d":"7.40"},{"v":113,"d":"113.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9P54610","Miniature circuit breaker (MCB), Acti9 iC40N, 1P+N, 10A, C curve, 6000A (IEC/EN 60898-1), 10kA (IEC/EN 60947-2)",0.01]
["A9P44725","Istič Acti9 iC40N 3P+N 25A B 6kA",1,"ks",{"v":31.751999999999995,"d":"31.752"},"3606481326089",{"v":9.4,"d":"9.40"},{"v":7.4,"d":"7.40"},{"v":5.4,"d":"5.40"},{"v":348.9,"d":"348.90"},"HU","8536201090","https://www.se.com/sk/sk/product/A9P44725","Miniature circuit breaker (MCB), Acti9 iC40N, 3P+N, 25A, B curve, 6000A (IEC/EN 60898-1), 10kA (IEC/EN 60947-2)",0.04]
["A9N61650","C60PV-DC 800VDC 10A 2P",1,"ks",{"v":63.50399999999999,"d":"63.504"},"3606480504068",{"v":13.6,"d":"13.60"},{"v":8,"d":"8.00"},{"v":7.5,"d":"7.50"},{"v":534,"d":"534.00"},"CH","8536201090","https://www.se.com/sk/sk/product/A9N61650","C60PV-DC - 2P - 10A - 800 V - char. C",0.06]
["A9N61529","ISTIČ C60H-DC 500VDC 13A 2P C",1,"ks",{"v":31.751999999999995,"d":"31.752"},"3606480424281",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":225,"d":"225.00"},"CN","8536201090","https://www.se.com/sk/sk/product/A9N61529","modulárny istič C60H - 2P - 13 A - char. C",0.03]
["A9N61515","ISTIČ C60H-DC 250VDC 32A 1P C",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3606480424168",{"v":7.5,"d":"7.50"},{"v":7,"d":"7.00"},{"v":1.8,"d":"1.80"},{"v":121,"d":"121.00"},"CN","8536201090","https://www.se.com/sk/sk/product/A9N61515","modulárny istič C60H - 1P - 32 A - char. C",0.01]
["A9N61503","ISTIČ C60H-DC 250VDC 3A 1P C",1,"ks",14.994,"3606480424052",{"v":7.5,"d":"7.50"},{"v":7,"d":"7.00"},{"v":1.8,"d":"1.80"},{"v":117,"d":"117.00"},"CN","8536201090","https://www.se.com/sk/sk/product/A9N61503","modulárny istič C60H - 1P - 3 A - char. C",0.01]
["A9N26914","Pomocný kontakt C60 C120 OF 2-100mA",1,"ks",{"v":18.521999999999995,"d":"18.522"},"3606482129184",{"v":9.3,"d":"9.30"},{"v":1.8,"d":"1.80"},{"v":7.6,"d":"7.60"},{"v":39,"d":"39.00"},"CN","8536508090","https://www.se.com/sk/sk/product/A9N26914","Signalizační kontakt C60 C120, OF, 2-100 mA, svorky zdola",0]
["A9N26904","1 OF Signalizačný kontakt 0,1-6A",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3606486351789",{"v":9.4,"d":"9.40"},{"v":2,"d":"2.00"},{"v":7.8,"d":"7.80"},{"v":36.7,"d":"36.70"},"BE","8536508090","https://www.se.com/sk/sk/product/A9N26904","1 OF signalizační kontakt",0]
["A9N18592","VIGI C120 125A 2P 300MA SI",1,"ks",{"v":354.56399999999996,"d":"354.564"},"3606480376665",{"v":13.5,"d":"13.50"},{"v":9.5,"d":"9.50"},{"v":13.5,"d":"13.50"},{"v":389,"d":"389.00"},"FR","8536303099","https://www.se.com/sk/sk/product/A9N18592","chráničová spúšť Vigi iC120 - 2P - 300 mA - typ A si",""]
["A9N18558","VIGI C120 125A 3P 300MA S SI",1,"ks",{"v":436.59,"d":"436.590"},"3606480376610",{"v":25.5,"d":"25.50"},{"v":9.2,"d":"9.20"},{"v":13.7,"d":"13.70"},{"v":587,"d":"587.00"},"FR","8536303099","https://www.se.com/sk/sk/product/A9N18558","chráničová spúšť Vigi iC120 - 3P - 300 mA - typ A si",""]
["A9N18554","VIGI C120 125A 4P 30MA SI",1,"ks",{"v":342.21599999999995,"d":"342.216"},"3606480376573",{"v":25.6,"d":"25.60"},{"v":9.6,"d":"9.60"},{"v":13.7,"d":"13.70"},{"v":812.9,"d":"812.90"},"FR","8536303099","https://www.se.com/sk/sk/product/A9N18554","chráničová spúšť Vigi iC120 - 4P - 30 mA - typ A si",""]
["A9N18489","ISTIČ C120H 1P 63A D 15KA 240/415V",1,"ks",{"v":71.88299999999998,"d":"71.883"},"3606480380600",{"v":8.5,"d":"8.50"},{"v":2.7,"d":"2.70"},{"v":7.5,"d":"7.50"},{"v":189,"d":"189.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9N18489","modulárny istič C120H - 1P - 63A - char. D",0.02]
["A9N18456","ISTIČ C120H 2P 63A C 15KA 415V",1,"ks",{"v":101.42999999999998,"d":"101.430"},"3606480380273",{"v":8.5,"d":"8.50"},{"v":5.3,"d":"5.30"},{"v":6.8,"d":"6.80"},{"v":376,"d":"376.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9N18456","modulárny istič C120H - 2P - 63A - char. C",0.05]
["A9N18425","ISTIČ C120H 3P 100A B 15KA 415V",1,"ks",{"v":171.98999999999998,"d":"171.990"},"3606480379963",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":578,"d":"578.00"},"FR","8536209090","https://www.se.com/sk/sk/product/A9N18425","modulárny istič C120H - 3P - 100A - char. B",0.07]
["A9N18391","ISTIČ C120N 4P 80A D 10KA 415V",1,"ks",{"v":216.08999999999997,"d":"216.090"},"3606480379628",{"v":10.7,"d":"10.70"},{"v":7.5,"d":"7.50"},{"v":8.7,"d":"8.70"},{"v":776,"d":"776.00"},"FR","8536209090","https://www.se.com/sk/sk/product/A9N18391","modulárny istič C120N - 4P - 80A - char. D",0.09]
["A9N18382","ISTIČ C120N 2P 63A D 10KA 415V",1,"ks",{"v":97.01999999999998,"d":"97.020"},"3606480379536",{"v":8.5,"d":"8.50"},{"v":5.3,"d":"5.30"},{"v":6.8,"d":"6.80"},{"v":375,"d":"375.00"},"FR","8536209090","https://www.se.com/sk/sk/product/A9N18382","modulárny istič C120N - 2P - 63A - char. D",0.05]
["A9N18364","ISTIČ C120N 3P 63A C 10KA 415V",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3606480379383",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":566,"d":"566.00"},"FR","8536209090","https://www.se.com/sk/sk/product/A9N18364","modulárny istič C120N - 3P - 63A - char. C",0.07]
["A9N18352","ISTIČ C120N 4P 63A B 10KA 415V",1,"ks",{"v":238.14,"d":"238.140"},"3606480379260",{"v":10.8,"d":"10.80"},{"v":7.5,"d":"7.50"},{"v":8.8,"d":"8.80"},{"v":753,"d":"753.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9N18352","modulárny istič C120N - 4P - 63A - char. B",0.09]
["A9N18341","ISTIČ C120N 1P 80A B 10KA 240/415V",1,"ks",{"v":37.04399999999999,"d":"37.044"},"3606480379154",{"v":8.4,"d":"8.40"},{"v":2.7,"d":"2.70"},{"v":6.8,"d":"6.80"},{"v":192,"d":"192.00"},"FR","8536209090","https://www.se.com/sk/sk/product/A9N18341","modulárny istič C120N - 1P - 80A - char. B",0.02]
["A9MEM3375","3F ELEKTROMER PRIAM. MER. 125A LON MID",1,"ks",{"v":432.17999999999995,"d":"432.180"},"3606480696442",{"v":13,"d":"13.00"},{"v":8.5,"d":"8.50"},{"v":11,"d":"11.00"},{"v":580,"d":"580.00"},"CN","9028309000","https://www.se.com/sk/sk/product/A9MEM3375","iEM3175 elektromer - 125 A - LON - 1 digital I - multi-tariff",0.07]
["A9MEM3115","3F ELEKTROMER PRIAM.MER.63A MULTITAR.MID",1,"ks",{"v":202.85999999999996,"d":"202.860"},"3606480481505",{"v":10.4,"d":"10.40"},{"v":8.5,"d":"8.50"},{"v":9.6,"d":"9.60"},{"v":447,"d":"447.00"},"CN","9028309000","https://www.se.com/sk/sk/product/A9MEM3115","iEM3110 elektromer - 63 A - 2 digit. I - multi-tariff",0.05]
["A9MEM3100","3F ELEKTROMER PRIAM. MERANIE 63A",1,"ks",{"v":185.22,"d":"185.220"},"3606480481482",{"v":10.2,"d":"10.20"},{"v":8.5,"d":"8.50"},{"v":9.5,"d":"9.50"},{"v":428,"d":"428.00"},"CN","9028309000","https://www.se.com/sk/sk/product/A9MEM3100","iEM3000 elektromer - 63 A",0.05]
["A9MEM1520","PowerTag sensor 1P max 63A",1,"ks",{"v":110.24999999999997,"d":"110.250"},"3606480909122",{"v":8.5,"d":"8.50"},{"v":5,"d":"5.00"},{"v":6.2,"d":"6.20"},{"v":45,"d":"45.00"},"FR","9030337000","https://www.se.com/sk/sk/product/A9MEM1520","Acti 9 - PowerTag - 1P - horné a dolné umiestnenie - max. 63A - Energy Sensor",0.01]
["A9L40321","Zvodič prepätia iPRD 40r 40 KA 460V 3P",1,"ks",{"v":158.75999999999996,"d":"158.760"},"3606480801655",8.48,{"v":6.915,"d":"6.92"},{"v":5.4,"d":"5.40"},{"v":340,"d":"340.00"},"CN","8536303099","https://www.se.com/sk/sk/product/A9L40321","zvodič prepätia iPRD 40r 40 KA 460V 3P IT",0.05]
["A9L40201","ZVODIČ IPRD 40R 40 KA 340V",1,"ks",{"v":110.24999999999997,"d":"110.250"},"3606480506369",{"v":9.2,"d":"9.20"},{"v":4.2,"d":"4.20"},{"v":7.2,"d":"7.20"},{"v":250,"d":"250.00"},"CN","8536303099","https://www.se.com/sk/sk/product/A9L40201","iPRD40r modulárny zvodič prepätia - 2P - 350V - s diaľkovým prenosom",0.03]
["A9L20100","ZVODIČ IPRD 20 20 KA 340V 1P",1,"ks",{"v":33.956999999999994,"d":"33.957"},"3606480506505",{"v":9.2,"d":"9.20"},{"v":7.2,"d":"7.20"},{"v":2.2,"d":"2.20"},{"v":128,"d":"128.00"},"CN","8536303099","https://www.se.com/sk/sk/product/A9L20100","iPRD20 modulárny zvodič prepätia - 1P - 350V",0.02]
["A9L16311","ZVODIČ MODUL C 20-350",1,"ks",{"v":92.61,"d":"92.610"},"3606480387142",{"v":9.5,"d":"9.50"},{"v":2,"d":"2.00"},{"v":6.7,"d":"6.70"},{"v":60,"d":"60.00"},"DE","8536309090","https://www.se.com/sk/sk/product/A9L16311","cartridge C20-350 for surge arrester iQuick PRD",0.01]
["A9L15586","ZVODIČ IPF 65 65 KA 340V 3P N",1,"ks",{"v":171.98999999999998,"d":"171.990"},"3606480089800",{"v":8.1,"d":"8.10"},{"v":7,"d":"7.00"},{"v":7.2,"d":"7.20"},{"v":335,"d":"335.00"},"CN","8536303099","https://www.se.com/sk/sk/product/A9L15586","iPF65 modulárny zvodič prepätia - 3 póly + N - 340V",0.06]
["A9K02332","ISTIČ ACTI9 K60N 3P 32A C",1,"ks",{"v":14.552999999999997,"d":"14.553"},"3606480478437",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":340,"d":"340.00"},"IN","8536201090","https://www.se.com/sk/sk/product/A9K02332","Acti 9 - istič K60N - 3P - 32 A - char. C - 6000 A",0.04]
["A9K02125","ISTIČ ACTI9 K60N 1P 25A C",1,"ks",{"v":4.057199999999999,"d":"4.057"},"3606480478345",{"v":8.5,"d":"8.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":111,"d":"111.00"},"IN","8536201090","https://www.se.com/sk/sk/product/A9K02125","Acti 9 - istič K60N - 1P - 25 A - char. C - 6000 A",0]
["A9K01316","ISTIČ ACTI9 K60N 3P 16A B",1,"ks",{"v":11.906999999999998,"d":"11.907"},"3606480478222",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":5.5,"d":"5.50"},{"v":321,"d":"321.00"},"IN","8536201090","https://www.se.com/sk/sk/product/A9K01316","Acti 9 - istič K60N - 3P - 16 A - char. B - 6000 A",0.04]
["A9K01110","ISTIČ ACTI9 K60N 1P 10A B",1,"ks",{"v":3.4397999999999995,"d":"3.440"},"3606480478130",{"v":8.6,"d":"8.60"},{"v":2,"d":"2.00"},{"v":6.8,"d":"6.80"},{"v":103,"d":"103.00"},"IN","8536201090","https://www.se.com/sk/sk/product/A9K01110","Acti 9 - istič K60N - 1P - 10 A - char. B - 6000 A",0]
["A9FDB7613","Oblúková ochrana s ističom 13A B 6kA",1,"ks",{"v":185.22,"d":"185.220"},"3606489508296",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8.5,"d":"8.50"},{"v":220,"d":"220.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9FDB7613","Acti 9 - iDPN N Arc - 1P+N 13A B 6000A - Istič s oblúkovou ochranou",0.03]
["A9F95472","ISTIČ ACTI9 IC60L 4P 1,6A K",1,"ks",{"v":255.77999999999994,"d":"255.780"},"3606480085130",{"v":9.5,"d":"9.50"},{"v":7.3,"d":"7.30"},{"v":7.5,"d":"7.50"},{"v":452,"d":"452.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F95472","modulárny istič iC60L - 4P - 1.6A - char. K",0.05]
["A9F95370","Istič ACTI9 IC60L 3P 0,5A K",1,"ks",{"v":141.11999999999998,"d":"141.120"},"3606480084935",{"v":9.4,"d":"9.40"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":371,"d":"371.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F95370","modulárny istič iC60L - 3P - 0.5A - char. K",0.04]
["A9F95310","ISTIČ ACTI9 IC60L 3P 10A K",1,"ks",{"v":101.42999999999998,"d":"101.430"},"3606480085062",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":5.3,"d":"5.30"},{"v":329,"d":"329.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F95310","modulárny istič iC60L - 3P - 10A - char. K",0.04]
["A9F95216","ISTIČ ACTI9 IC60L 2P 16A K",1,"ks",{"v":72.32399999999998,"d":"72.324"},"3606480084720",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":230,"d":"230.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F95216","modulárny istič iC60L - 2P - 16A - char. K",0.03]
["A9F95106","ISTIČ ACTI9 IC60L 1P 6A K",1,"ks",32.193,"3606480084768",{"v":9.2,"d":"9.20"},{"v":1.7,"d":"1.70"},{"v":7.1,"d":"7.10"},{"v":108,"d":"108.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F95106","modulárny istič iC60L - 1P - 6A - char. K",0.01]
["A9F94470","ISTIČ ACTI9 IC60L 4P 0,5A C",1,"ks",{"v":202.85999999999996,"d":"202.860"},"3606480084119",{"v":9.4,"d":"9.40"},{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":444,"d":"444.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F94470","modulárny istič iC60L - 4P - 0.5A - char. C",0.05]
["A9F94332","ISTIČ ACTI9 IC60L 3P 32A C",1,"ks",{"v":110.24999999999997,"d":"110.250"},"3606480084416",{"v":8.5,"d":"8.50"},{"v":7.3,"d":"7.30"},{"v":5.4,"d":"5.40"},{"v":375,"d":"375.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F94332","modulárny istič iC60L - 3P - 32A - char. C",0.05]
["A9F94302","ISTIČ ACTI9 IC60L 3P 2A C",1,"ks",{"v":136.70999999999998,"d":"136.710"},"3606480084485",{"v":9,"d":"9.00"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":333,"d":"333.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F94302","modulárny istič iC60L - 3P - 2A - char. C",0.04]
["A9F94201","ISTIČ ACTI9 IC60L 2P 1A C",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3606480084270",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":3.5,"d":"3.50"},{"v":225,"d":"225.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F94201","modulárny istič iC60L - 2P - 1A - char. C",0.03]
["A9F93420","ISTIČ ACTI9 IC60L 4P 20A B",1,"ks",{"v":163.17,"d":"163.170"},"3606480083822",{"v":9.5,"d":"9.50"},{"v":7.2,"d":"7.20"},{"v":7.5,"d":"7.50"},{"v":452,"d":"452.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F93420","modulárny istič iC60L - 4P - 20A - char. B",0.05]
["A9F93406","ISTIČ ACTI9 IC60L 4P 6A B",1,"ks",{"v":141.11999999999998,"d":"141.120"},"3606480083785",{"v":9.5,"d":"9.50"},{"v":7,"d":"7.00"},{"v":7,"d":"7.00"},{"v":430,"d":"430.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F93406","modulárny istič iC60L - 4P - 6A - char. B",0.05]
["A9F93263","ISTIČ ACTI9 IC60L 2P 63A B",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3606480084010",{"v":9.1,"d":"9.10"},{"v":3.5,"d":"3.50"},{"v":7.1,"d":"7.10"},{"v":268,"d":"268.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F93263","modulárny istič iC60L - 2P - 63A - char. B",0.03]
["A9F93201","ISTIČ ACTI9 IC60L 2P 1A B",1,"ks",{"v":78.05699999999999,"d":"78.057"},"3606480083549",{"v":9.4,"d":"9.40"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":234.357,"d":"234.36"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F93201","modulárny istič iC60L - 2P - 1A - char. B",0.03]
["A9F93106","ISTIČ ACTI9 IC60L 1P 6A B",1,"ks",{"v":26.900999999999996,"d":"26.901"},"3606480083914",{"v":9.5,"d":"9.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":108,"d":"108.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F93106","modulárny istič iC60L - 1P - 6A - char. B",0.01]
["A9F92350","ISTIČ ACTI9 IC60L 3P 50A Z",1,"ks",{"v":242.54999999999995,"d":"242.550"},"3606480085529",{"v":9.4,"d":"9.40"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":418.611,"d":"418.61"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F92350","modulárny istič iC60L - 3P - 50A - char. Z",0.04]
["A9F92306","ISTIČ ACTI9 IC60L 3P 6A Z",1,"ks",{"v":185.22,"d":"185.220"},"3606480085437",{"v":9.4,"d":"9.40"},{"v":7.1,"d":"7.10"},{"v":5.3,"d":"5.30"},{"v":326,"d":"326.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F92306","modulárny istič iC60L - 3P - 6A - char. Z",0.04]
["A9F92203","ISTIČ ACTI9 IC60L 2P 3A Z",1,"ks",{"v":101.42999999999998,"d":"101.430"},"3606480085376",{"v":9.3,"d":"9.30"},{"v":3.5,"d":"3.50"},{"v":6.8,"d":"6.80"},{"v":224,"d":"224.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F92203","modulárny istič iC60L - 2P - 3A - char. Z",0.03]
["A9F92170","ACTI9 IC60L 1P Z 0,5A MCB",1,"ks",{"v":40.7484,"d":"40.748"},"3606480085277",{"v":9.4,"d":"9.40"},{"v":7.5,"d":"7.50"},{"v":1.8,"d":"1.80"},{"v":116.199,"d":"116.20"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F92170","modulárny istič iC60L - 1P - 0.5A - char. Z",""]
["A9F90340","ACTI9 IC60LMA 3P 40A MA",1,"ks",{"v":149.93999999999997,"d":"149.940"},"3606480085970",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":5.5,"d":"5.50"},{"v":373,"d":"373.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F90340","modulárny istič iC60L - 3P - 40A - char. MA",0.05]
["A9F85432","ACTI9 IC60H 4P 32A D",1,"ks",{"v":88.19999999999999,"d":"88.200"},"3606480083488",{"v":8.5,"d":"8.50"},{"v":7.3,"d":"7.30"},{"v":7.1,"d":"7.10"},{"v":498,"d":"498.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F85432","modulárny istič iC60H - 4P - 32A - char. D",0.06]
["A9F85332","ACTI9 IC60H 3P 32A D",1,"ks",65.268,"3606480083105",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":5.5,"d":"5.50"},{"v":369,"d":"369.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F85332","modulárny istič iC60H - 3P - 32A - char. D",0.05]
["A9F85232","ACTI9 IC60H 2P 32A D",1,"ks",{"v":42.776999999999994,"d":"42.777"},"3606480083198",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":244,"d":"244.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F85232","modulárny istič iC60H - 2P - 32A - char. D",0.03]
["A9F85202","ACTI9 IC60H 2P 2A D",1,"ks",{"v":48.50999999999999,"d":"48.510"},"3606480082764",{"v":9.5,"d":"9.50"},{"v":3.6,"d":"3.60"},{"v":7.5,"d":"7.50"},{"v":222,"d":"222.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F85202","modulárny istič iC60H - 2P - 2A - char. D",0.03]
["A9F84610","ACTI9 IC60H 1P-N 10A C",1,"ks",{"v":21.167999999999996,"d":"21.168"},"3606480082016",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":7.5,"d":"7.50"},{"v":220.3,"d":"220.30"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F84610","modulárny istič iC60H - 1P + N - 10A - char. C",0.03]
["A9F84463","ACTI9 IC60H 4P 63A C",1,"ks",{"v":145.52999999999997,"d":"145.530"},"3606480082030",{"v":9.5,"d":"9.50"},{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":527,"d":"527.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F84463","modulárny istič iC60H - 4P - 63A - char. C",0.06]
["A9F84402","ACTI9 IC60H 4P 2A C",1,"ks",{"v":87.75899999999999,"d":"87.759"},"3606480082696",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":7.2,"d":"7.20"},{"v":442,"d":"442.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F84402","modulárny istič iC60H - 4P - 2A - char. C",0.06]
["A9F84216","ACTI9 IC60H 2P 16A C",1,"ks",{"v":22.049999999999997,"d":"22.050"},"3606480081729",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":3.5,"d":"3.50"},{"v":221,"d":"221.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F84216","modulárny istič iC60H - 2P - 16A - char. C",0.03]
["A9F84132","ACTI9 IC60H 1P 32A C",1,"ks",11.466,"3606480081804",{"v":9.5,"d":"9.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":120,"d":"120.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F84132","modulárny istič iC60H - 1P - 32A - char. C",0]
["A9F83420","ACTI9 IC60H 4P 20A B",1,"ks",{"v":63.944999999999986,"d":"63.945"},"3606480081651",{"v":9.4,"d":"9.40"},{"v":7.5,"d":"7.50"},{"v":7.2,"d":"7.20"},{"v":468.588,"d":"468.59"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F83420","modulárny istič iC60H - 4P - 20A - char. B",0.06]
["A9F83320","ACTI9 IC60H 3P 20A B",1,"ks",{"v":36.602999999999994,"d":"36.603"},"3606480081293",{"v":9.5,"d":"9.50"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":286,"d":"286.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F83320","modulárny istič iC60H - 3P - 20A - char. B",0.04]
["A9F83204","Istič iC60H 2P 4A B",1,"ks",{"v":40.13099999999999,"d":"40.131"},"3606480082245",{"v":9.5,"d":"9.50"},{"v":3.5,"d":"3.50"},{"v":7.5,"d":"7.50"},{"v":221.3,"d":"221.30"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F83204","Miniature circuit breaker (MCB), Acti9 iC60H, 2P, 4A, B curve, 10000A (IEC/EN 60898-1), 70kA (IEC/EN 60947-2)",0.03]
["A9F83102","ACTI9 IC60H 1P 2A B",1,"ks",{"v":36.16199999999999,"d":"36.162"},"3606480082177",{"v":9.5,"d":"9.50"},{"v":2,"d":"2.00"},{"v":7.5,"d":"7.50"},{"v":113,"d":"113.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F83102","modulárny istič iC60H - 1P - 2A - char.B",0.01]
["A9F75420","ACTI9 IC60N 4P 20A D",1,"ks",64.386,"3606480081118",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":7.2,"d":"7.20"},{"v":452,"d":"452.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F75420","modulárny istič iC60N - 4P - 20A - char. D",0.05]
["A9F75401","ACTI9 IC60N 4P 1A D",1,"ks",{"v":154.34999999999997,"d":"154.350"},"3606480080715",{"v":9.3,"d":"9.30"},{"v":7.1,"d":"7.10"},{"v":7.1,"d":"7.10"},{"v":452,"d":"452.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F75401","modulárny istič iC60N - 4P - 1A - char. D",0.05]
["A9F75301","ACTI9 IC60N 3P 1A D",1,"ks",44.982,"3606480080661",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":5.2,"d":"5.20"},{"v":340,"d":"340.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F75301","modulárny istič iC60N - 3P - 1A - char. D",0.04]
["A9F75116","ACTI9 IC60N 1P 16A D",1,"ks",{"v":12.347999999999997,"d":"12.348"},"3606480080913",{"v":9.5,"d":"9.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":109,"d":"109.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F75116","modulárny istič iC60N - 1P - 16A - char. D",0]
["A9F74604","ACTI9 IC60N 1P-N 4A C",1,"ks",28.665,"3606480080401",{"v":8.5,"d":"8.50"},{"v":7.3,"d":"7.30"},{"v":3.6,"d":"3.60"},{"v":220,"d":"220.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F74604","modulárny istič iC60N - 1P + N - 4A - char. C",0.03]
["A9F74432","ACTI9 IC60N 4P 32A C",1,"ks",{"v":62.18099999999999,"d":"62.181"},"3606480079771",{"v":9.4,"d":"9.40"},{"v":7.2,"d":"7.20"},{"v":7.5,"d":"7.50"},{"v":494,"d":"494.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F74432","modulárny istič iC60N - 4P - 32A - char. C",0.06]
["A9F74363","ACTI9 IC60N 3P 63A C",1,"ks",{"v":88.19999999999999,"d":"88.200"},"3606480079719",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":5.4,"d":"5.40"},{"v":381,"d":"381.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F74363","modulárny istič iC60N - 3P - 63A - char. C",0.05]
["A9F74303","ACTI9 IC60N 3P 3A C",1,"ks",{"v":51.596999999999994,"d":"51.597"},"3606480080272",{"v":9.5,"d":"9.50"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":339.3,"d":"339.30"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F74303","modulárny istič iC60N - 3P - 3A - char. C",0.04]
["A9F74210","ISTIČ ACTI9 IC60N 2P 10A C export",1,"ks",{"v":18.080999999999996,"d":"18.081"},"3606480079559",{"v":9.3,"d":"9.30"},{"v":3.5,"d":"3.50"},{"v":7.2,"d":"7.20"},{"v":212,"d":"212.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F74210","modulárny istič iC60N - 2P - 10A - char. C",0.03]
["A9F74113","ACTI9 IC60N 1P 13A C",1,"ks",11.466,"3606480080302",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":1.8,"d":"1.80"},{"v":108,"d":"108.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F74113","modulárny istič iC60N - 1P - 13A - char. C",0]
["A9F73450","ACTI9 IC60N 4P 50A B",1,"ks",{"v":88.19999999999999,"d":"88.200"},"3606480079344",{"v":9.5,"d":"9.50"},{"v":7.2,"d":"7.20"},{"v":7.5,"d":"7.50"},{"v":494,"d":"494.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F73450","modulárny istič iC60N - 4P - 50A - char. B",0.06]
["A9F73340","ACTI9 IC60N 3P 40A B",1,"ks",{"v":38.80799999999999,"d":"38.808"},"3606480079245",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":5.5,"d":"5.50"},{"v":373.641,"d":"373.64"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F73340","modulárny istič iC60N - 3P - 40A - char. B",0.04]
["A9F73203","ACTI9 IC60N 2P 3A B",1,"ks",{"v":35.279999999999994,"d":"35.280"},"3606480080029",{"v":9.5,"d":"9.50"},{"v":3.5,"d":"3.50"},{"v":7.5,"d":"7.50"},{"v":224,"d":"224.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F73203","modulárny istič iC60N - 2P - 3A - char.B",0.03]
["A9F73102","ACTI9 IC60N 1P 2A B",1,"ks",14.994,"3606480080005",{"v":9.5,"d":"9.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":112,"d":"112.00"},"FR","8536201090","https://www.se.com/sk/sk/product/A9F73102","modulárny istič iC60N - 1P - 2A - char. B",0]
["A9F54216","ISTIČ ACTI9 IC60H 2P 16A C",1,"ks",{"v":22.049999999999997,"d":"22.050"},"3606480514852",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":222,"d":"222.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F54216","Miniature circuit breaker (MCB), Acti9 iC60H Disbo, 2P, 16A, C curve, 10000A (IEC/EN 60898-1), 15kA (IEC/EN 60947-2)",0.03]
["A9F08403","ISTIČ ACTI9 IC60H 4P 3A D",1,"ks",{"v":101.42999999999998,"d":"101.430"},"3606480439506",{"v":8.8,"d":"8.80"},{"v":7.1,"d":"7.10"},{"v":7.3,"d":"7.30"},{"v":467.7,"d":"467.70"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F08403","modulárny istič iC60H - 4P - 3A - char. D",0.06]
["A9F08316","ISTIČ ACTI9 IC60H 3P 16A D",1,"ks",32.193,"3606480439407",{"v":9,"d":"9.00"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":352.6,"d":"352.60"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F08316","modulárny istič iC60H - 3P - 16A - char. D",0.04]
["A9F08204","ISTIČ ACTI9 IC60H 2P 4A D",1,"ks",{"v":25.136999999999997,"d":"25.137"},"3606480439216",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":7.5,"d":"7.50"},{"v":229,"d":"229.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F08204","modulárny istič iC60H - 2P - 4A - char. D",0.03]
["A9F08170","ISTIČ ACTI9 IC60H 1P 0,5A D",1,"ks",26.019,"3606480439179",{"v":8.8,"d":"8.80"},{"v":1.8,"d":"1.80"},{"v":7.3,"d":"7.30"},{"v":117,"d":"117.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F08170","modulárny istič iC60H - 1P - 0.5A - char. D",0.01]
["A9F07632","ISTIČ ACTI9 IC60H 1P+N 32A C",1,"ks",{"v":56.44799999999999,"d":"56.448"},"3606480438981",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":7,"d":"7.00"},{"v":246,"d":"246.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F07632","modulárny istič iC60H - 1P + N - 32A - char. C",0.03]
["A9F07420","ISTIČ ACTI9 IC60H 4P 20A C",1,"ks",{"v":41.01299999999999,"d":"41.013"},"3606480438813",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":474,"d":"474.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F07420","modulárny istič iC60H - 4P - 20A - char. C",0.06]
["A9F07404","ISTIČ ACTI9 IC60H 4P 4A C",1,"ks",45.864,"3606480438769",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":7.2,"d":"7.20"},{"v":460,"d":"460.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F07404","modulárny istič iC60H - 4P - 4A - char. C",0.06]
["A9F07263","ISTIČ ACTI9 IC60H 2P 63A C",1,"ks",{"v":35.72099999999999,"d":"35.721"},"3606480438561",{"v":9.5,"d":"9.50"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":277,"d":"277.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F07263","modulárny istič iC60H - 2P - 63A - char. C",0.03]
["A9F07210","ISTIČ ACTI9 IC60H 2P 10A C",1,"ks",{"v":19.844999999999995,"d":"19.845"},"3606480438486",{"v":9,"d":"9.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":227,"d":"227.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F07210","modulárny istič iC60H - 2P - 10A - char. C",0.03]
["A9F07113","ISTIČ ACTI9 IC60H 1P 13A C",1,"ks",{"v":8.4231,"d":"8.423"},"3606480438349",{"v":9,"d":"9.00"},{"v":2,"d":"2.00"},{"v":7.5,"d":"7.50"},{"v":116.8,"d":"116.80"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F07113","modulárny istič iC60H - 1P - 13A - char. C",0]
["A9F06640","ISTIČ ACTI9 IC60H 1P+N 40A B",1,"ks",43.659,"3606480438257",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":3.5,"d":"3.50"},{"v":253,"d":"253.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F06640","modulárny istič iC60H - 1P + N - 40A - char. B",0.03]
["A9F06420","ISTIČ ACTI9 IC60H 4P 20A B",1,"ks",{"v":42.776999999999994,"d":"42.777"},"3606480438127",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":473,"d":"473.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F06420","modulárny istič iC60H - 4P - 20A - char. B",0.06]
["A9F06232","ISTIČ ACTI9 IC60H 2P 32A B",1,"ks",22.491,"3606480437946",{"v":9.5,"d":"9.50"},{"v":3.6,"d":"3.60"},{"v":7.5,"d":"7.50"},{"v":246,"d":"246.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F06232","modulárny istič iC60H - 2P - 32A - char. B",0.03]
["A9F06213","ISTIČ ACTI9 IC60H 2P 13A B",1,"ks",{"v":20.726999999999997,"d":"20.727"},"3606480437908",{"v":9.5,"d":"9.50"},{"v":3.6,"d":"3.60"},{"v":7.5,"d":"7.50"},{"v":228,"d":"228.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F06213","modulárny istič iC60H - 2P - 13A - char. B",0.03]
["A9F05416","ISTIČ ACTI9 IC60N 4P 16A D",1,"ks",29.988,"3606480441714",{"v":8.7,"d":"8.70"},{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":449,"d":"449.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F05416","modulárny istič iC60N - 4P - 16A - char. D",0.05]
["A9F05340","ISTIČ ACTI9 IC60N 3P 40A D",1,"ks",{"v":29.105999999999995,"d":"29.106"},"3606480441608",{"v":9.1,"d":"9.10"},{"v":5.3,"d":"5.30"},{"v":7.4,"d":"7.40"},{"v":394,"d":"394.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F05340","modulárny istič iC60N - 3P - 40A - char. D",0.05]
["A9F05232","ISTIČ ACTI9 IC60N 2P 32A D",1,"ks",{"v":19.844999999999995,"d":"19.845"},"3606480441448",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":7,"d":"7.00"},{"v":256,"d":"256.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F05232","modulárny istič iC60N - 2P - 32A - char. D",0.03]
["A9F05206","ISTIČ ACTI9 IC60N 2P 6A D",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3606480441387",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":7.5,"d":"7.50"},{"v":226,"d":"226.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F05206","modulárny istič iC60N - 2P - 6A - char. D",0.03]
["A9F05103","ISTIČ ACTI9 IC60N 1P 3A D",1,"ks",{"v":20.285999999999998,"d":"20.286"},"3606480441219",{"v":9,"d":"9.00"},{"v":2,"d":"2.00"},{"v":7.5,"d":"7.50"},{"v":119.5,"d":"119.50"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F05103","modulárny istič iC60N - 1P - 3A - char. D",0.01]
["A9F04670","ISTIČ ACTI9 IC60N 1P+N 0,5A C",1,"ks",{"v":50.71499999999999,"d":"50.715"},"3606480441035",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":7,"d":"7.00"},{"v":230,"d":"230.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F04670","modulárny istič iC60N - 1P + N - 0.5A - char. C",0.03]
["A9F04602","ISTIČ ACTI9 IC60N 1P+N 2A C",1,"ks",16.317,"3606480440908",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":7.5,"d":"7.50"},{"v":230.8,"d":"230.80"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F04602","modulárny istič iC60N - 1P + N - 2A - char. C",0.03]
["A9F04416","ISTIČ ACTI9 IC60N 4P 16A C",1,"ks",27.342,"3606480440816",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":7.5,"d":"7.50"},{"v":455.2,"d":"455.20"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F04416","modulárny istič iC60N - 4P - 16A - char. C",0.05]
["A9F04320","ISTIČ ACTI9 IC60N 3P 20A C",1,"ks",{"v":19.844999999999995,"d":"19.845"},"3606480440670",{"v":8.7,"d":"8.70"},{"v":7.3,"d":"7.30"},{"v":5.3,"d":"5.30"},{"v":355,"d":"355.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F04320","modulárny istič iC60N - 3P - 20A - char. C",0.04]
["A9F04301","ISTIČ ACTI9 IC60N 3P 1A C",1,"ks",{"v":26.459999999999994,"d":"26.460"},"3606480440595",{"v":9,"d":"9.00"},{"v":5.5,"d":"5.50"},{"v":7.5,"d":"7.50"},{"v":352.1,"d":"352.10"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F04301","modulárny istič iC60N - 3P - 1A - char. C",0.04]
["A9F04201","ISTIČ ACTI9 IC60N 2P 1A C",1,"ks",{"v":17.198999999999998,"d":"17.199"},"3606480440441",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":7.5,"d":"7.50"},{"v":234.3,"d":"234.30"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F04201","modulárny istič iC60N - 2P - 1A - char. C",0.03]
["A9F04106","ISTIČ ACTI9 IC60N 1P 6A C",1,"ks",{"v":6.306299999999999,"d":"6.306"},"3606480440335",{"v":8.7,"d":"8.70"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":114,"d":"114.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F04106","modulárny istič iC60N - 1P - 6A - char. C",0]
["A9F03650","ISTIČ ACTI9 IC60N 1P+N 50A B",1,"ks",{"v":41.894999999999996,"d":"41.895"},"3606480440175",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":3.6,"d":"3.60"},{"v":254,"d":"254.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F03650","modulárny istič iC60N - 1P + N - 50A - char. B",0.03]
["A9F03613","ISTIČ ACTI9 IC60N 1P+N 13A B",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3606480440113",{"v":9.1,"d":"9.10"},{"v":3.5,"d":"3.50"},{"v":7.4,"d":"7.40"},{"v":224,"d":"224.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F03613","modulárny istič iC60N - 1P + N - 13A - char. B",0.03]
["A9F03313","ISTIČ ACTI9 IC60N 3P 13A B",1,"ks",16.317,"3606480439919",{"v":9.1,"d":"9.10"},{"v":5.3,"d":"5.30"},{"v":7.4,"d":"7.40"},{"v":336,"d":"336.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F03313","modulárny istič iC60N - 3P - 13A - char. B",0.04]
["A9F03202","ISTIČ ACTI9 IC60N 2P 2A B",1,"ks",16.758,"3606480439766",{"v":9,"d":"9.00"},{"v":3.5,"d":"3.50"},{"v":7.5,"d":"7.50"},{"v":231,"d":"231.00"},"BG","8536201090","https://www.se.com/sk/sk/product/A9F03202","modulárny istič iC60N - 2P - 2A - char. B",0.03]
["A9F03116SK","AKCIA 5 S5 A9F03116 - 12 KS",1,"ks",{"v":26.900999999999996,"d":"26.901"},"",{"v":9,"d":"9.00"},{"v":15,"d":"15.00"},{"v":8,"d":"8.00"},{"v":114,"d":"114.00"},"IN","85362010","https://www.se.com/sk/sk/product/A9F03116SK","",0]
["A9E18333","SIGNÁLKA IIL MODRÁ 12/24/48 V AC/DC",1,"ks",{"v":14.552999999999997,"d":"14.553"},"3606480088445",{"v":6.8,"d":"6.80"},{"v":9,"d":"9.00"},{"v":1.7,"d":"1.70"},{"v":39,"d":"39.00"},"BE","8531807000","https://www.se.com/sk/sk/product/A9E18333","Acti9 iIL signálka - modrá - 12-48 V AC/DC",0]
["A9E18326","SIGNÁLKA IIL ČERVENÁ BLIKACIA 110-230 V",1,"ks",{"v":52.478999999999985,"d":"52.479"},"3606480088384",{"v":9,"d":"9.00"},{"v":6.8,"d":"6.80"},{"v":1.7,"d":"1.70"},{"v":44,"d":"44.00"},"BE","8531807000","https://www.se.com/sk/sk/product/A9E18326","Acti9 iIL blikacia signálka - červená - 110-230 V AC",0.01]
["A9E18038","TLAČ. IBP 1ZAP+ ZEL SIGNÁLKA 12-48 V",1,"ks",{"v":25.577999999999996,"d":"25.578"},"3606480088308",{"v":8.2,"d":"8.20"},{"v":6.6,"d":"6.60"},{"v":1.8,"d":"1.80"},{"v":46,"d":"46.00"},"BE","8536508090","https://www.se.com/sk/sk/product/A9E18038","Acti9 iPB 1Z tlačítko šedé - signálka zelená 12-48Vac/dc",0.01]
["A9E16070","RELÉ IRTMF 2P 24-240 VCA/24VCC",1,"ks",{"v":114.66,"d":"114.660"},"3606480377464",{"v":10.2,"d":"10.20"},{"v":2.2,"d":"2.20"},{"v":7.4,"d":"7.40"},{"v":82,"d":"82.00"},"FR","8536490099","https://www.se.com/sk/sk/product/A9E16070","iRTMF multifunkčné časovo zmeškané relé - 1 prep. - 12-240 VAC/DC",0.01]
["A9E15123","OTOČNÝ PREPÍNAČ ICMC",1,"ks",{"v":149.93999999999997,"d":"149.940"},"3606480377013",{"v":8.4,"d":"8.40"},{"v":4.3,"d":"4.30"},{"v":7.6,"d":"7.60"},{"v":89,"d":"89.00"},"AT","85365080","https://www.se.com/sk/sk/product/A9E15123","2-polohový otočný prepínač s kľúčom iCMC 10A 2P U 415V CA",0]
["A9DF3732","Chránič-istič Acti9 iCV40N 3P+N 32A C 6k",1,"ks",{"v":158.75999999999996,"d":"158.760"},"3606481328885",{"v":12.5,"d":"12.50"},{"v":8.5,"d":"8.50"},{"v":11.2,"d":"11.20"},{"v":615,"d":"615.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9DF3732","Residual current breaker with overcurrent protection (RCBO), Acti9 iCV40N, 3P+N, 32A, C curve, 6000A, A-SI type, 30mA",0.07]
["A9DC3725","Chránič-istič Acti9 iCV40N 3P+N 25A C 6k",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3606481328663",{"v":11.2,"d":"11.20"},{"v":8.6,"d":"8.60"},{"v":12.5,"d":"12.50"},{"v":581,"d":"581.00"},"ZZ","8536201090","https://www.se.com/sk/sk/product/A9DC3725","Residual current breaker with overcurrent protection (RCBO), Acti9 iCV40N, 3P+N, 25A, C curve, 6000A, A type, 30mA",0.07]
["A9D77432","Acti 9 chránič-istič 4P 32A 30mA C 6kA S",1,"ks",{"v":238.14,"d":"238.140"},"3606481157911",{"v":10,"d":"10.00"},{"v":8.8,"d":"8.80"},{"v":8,"d":"8.00"},{"v":450,"d":"450.00"},"PT","8536201090","https://www.se.com/sk/sk/product/A9D77432","Acti 9 - chránič-istič 4P 32A 30mA C 6kA SI",0.06]
["A9D69604","IDPN N VIGI 4A B 300MA A",1,"ks",{"v":59.093999999999994,"d":"59.094"},"3606480472978",{"v":7.8,"d":"7.80"},{"v":9.5,"d":"9.50"},{"v":3.6,"d":"3.60"},{"v":215,"d":"215.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D69604","chránič s nadprúdovou ochranou iDPN N Vigi - 1P + N - 4A - 300mA trieda A",0.02]
["A9D60616","IDPN N VIGI 16A B 100MA A",1,"ks",52.038,"3606480472800",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8.3,"d":"8.30"},{"v":125,"d":"125.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D60616","chránič s nadprúdovou ochranou iDPN N Vigi - 1P + N - 16A - 100mA trieda A",0.03]
["A9D57416","Acti 9 chránič-istič 4P 16A 30mA C 6kA A",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3606481157713",{"v":10.3,"d":"10.30"},{"v":8.5,"d":"8.50"},{"v":8,"d":"8.00"},{"v":435,"d":"435.00"},"PT","8536201090","https://www.se.com/sk/sk/product/A9D57416","Acti 9 - chránič-istič 4P 16A 30mA C 6kA AC",0.05]
["A9D55620","IDPN N VIGI 20A B 30MA AC",1,"ks",52.038,"3606480472633",{"v":9.8,"d":"9.80"},{"v":8,"d":"8.00"},{"v":4,"d":"4.00"},{"v":196,"d":"196.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D55620","chránič s nadprúdovou ochranou iDPN N Vigi - 1P + N - 20A - 30mA trieda AC",0.03]
["A9D55410","Acti 9 chránič-istič 4P 10A 300mA C 6kA",1,"ks",{"v":136.70999999999998,"d":"136.710"},"3606481157751",{"v":9.8,"d":"9.80"},{"v":8.8,"d":"8.80"},{"v":8,"d":"8.00"},{"v":436,"d":"436.00"},"PT","8536201090","https://www.se.com/sk/sk/product/A9D55410","Acti 9 - chránič-istič 4P 10A 300mA C 6kA AC",0.05]
["A9D52613","IDPN N VIGI 13A C 100MA A",1,"ks",{"v":77.61599999999999,"d":"77.616"},"3606480472459",{"v":7.8,"d":"7.80"},{"v":9.5,"d":"9.50"},{"v":3.6,"d":"3.60"},{"v":215,"d":"215.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D52613","chránič s nadprúdovou ochranou iDPN N Vigi - 1P + N - 13A - 100mA trieda A",0.02]
["A9D43616","IDPN N VIGI 16A C 300MA ASI",1,"ks",{"v":67.91399999999999,"d":"67.914"},"3606480472381",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":190,"d":"190.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D43616","chránič s nadprúdovou ochranou iDPN N Vigi - 1P + N - 16A - 300mA trieda SI",0.02]
["A9D42640","IDPN N VIGI 40A C 300MA A",1,"ks",84.231,"3606480472343",{"v":7.8,"d":"7.80"},{"v":9.5,"d":"9.50"},{"v":3.6,"d":"3.60"},{"v":215,"d":"215.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D42640","chránič s nadprúdovou ochranou iDPN N Vigi - 1P + N - 40A - 300mA trieda A",0.02]
["A9D38625","IDPN H VIGI 25A C 30MA ASI",1,"ks",{"v":123.47999999999999,"d":"123.480"},"3606480484445",{"v":7.8,"d":"7.80"},{"v":9.5,"d":"9.50"},{"v":3.6,"d":"3.60"},{"v":215,"d":"215.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D38625","chránič s nadprúdovou ochranou iDPN H Vigi - 1P + N - 25A - 30mA trieda SI",0.02]
["A9D34616","IDPNA VIGI 16A C 30MA AC-TYP",1,"ks",{"v":40.13099999999999,"d":"40.131"},"3606480471582",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},193.25,"ES","8536201090","https://www.se.com/sk/sk/product/A9D34616","Residual current breaker with overcurrent protection (RCBO), Acti9 iDPNa Vigi, 1P+N, 16A, C curve, 4500A, AC type, 30mA",0]
["A9D32616","IDPN N VIGI 16A C 30MA A",1,"ks",52.038,"3606480472077",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8.5,"d":"8.50"},{"v":203,"d":"203.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D32616","chránič s nadprúdovou ochranou iDPN N Vigi - 1P + N - 16A - 30mA trieda A",0.03]
["A9D31606","IDPN N VIGI 6A C 30MA AC",1,"ks",52.038,"3606480471971",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8.5,"d":"8.50"},{"v":193,"d":"193.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D31606","chránič s nadprúdovou ochranou iDPN N Vigi - 1P + N - 6A - 30mA trieda AC",0.02]
["A9D20616","Chránič-istič K60N 1PN 16A C 30mA 6kA AC",1,"ks",{"v":37.925999999999995,"d":"37.926"},"3606480551970",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":201,"d":"201.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9D20616","Acti 9 - chránič-istič K60N 1PN 16A C 30mA 6kA AC",0.03]
["A9D07225","Acti9 IC60 RCBO 2P 25A 30mA C 10kA AC",1,"ks",{"v":101.42999999999998,"d":"101.430"},"3606481157348",{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":234,"d":"234.00"},"PT","8536201090","https://www.se.com/sk/sk/product/A9D07225","Residual current breaker with overcurrent protection (RCBO), Acti9 iC60, 2P, 25A, C curve, 10000A/15kA, AC type, 30mA",0.03]
["A9CR4225","Acti9 RED 2P 63A 30mA typ A",1,"ks",{"v":269.01,"d":"269.010"},"3606481489432",{"v":11.2,"d":"11.20"},{"v":10.5,"d":"10.50"},{"v":13.3,"d":"13.30"},{"v":384,"d":"384.00"},"PT","8536201090","https://www.se.com/sk/sk/product/A9CR4225","Residual current circuit breaker (RCCB), Acti9 REDs, 2P, 25A, A type, 30mA",0.05]
["A9C66225","ACTI 9 REFLEX IC60H TI24 25 A 2P D",1,"ks",{"v":326.34,"d":"326.340"},"3606480455216",{"v":16.8,"d":"16.80"},{"v":9,"d":"9.00"},{"v":11,"d":"11.00"},{"v":569.9,"d":"569.90"},"ES","8536201090","https://www.se.com/sk/sk/product/A9C66225","istič Reflex iC60H Ti24 25 A 2P char. D",0.07]
["A9C64325","ACTI 9 REFLEX IC60H TI24 25 A 3P B",1,"ks",{"v":635.0399999999998,"d":"635.040"},"3606480455018",{"v":16.7,"d":"16.70"},{"v":9,"d":"9.00"},{"v":11.2,"d":"11.20"},{"v":692.9,"d":"692.90"},"ES","8536201090","https://www.se.com/sk/sk/product/A9C64325","istič Reflex iC60H Ti24 25 A 3P char. B",0.08]
["A9C63216","ACTI 9 REFLEX IC60N TI24 16 A 2P D",1,"ks",{"v":361.61999999999995,"d":"361.620"},"3606480455742",{"v":16.5,"d":"16.50"},{"v":9,"d":"9.00"},{"v":11,"d":"11.00"},{"v":569.9,"d":"569.90"},"ES","8536201090","https://www.se.com/sk/sk/product/A9C63216","istič Reflex iC60N Ti24 16 A 2P char. D",0.07]
["A9C61440","ACTI 9 REFLEX IC60N TI24 40 A 4P B",1,"ks",{"v":802.6199999999999,"d":"802.620"},"3606480455568",{"v":16.5,"d":"16.50"},{"v":9,"d":"9.00"},{"v":11,"d":"11.00"},{"v":900,"d":"900.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9C61440","istič Reflex iC60N Ti24 40 A 4P char. B",0.11]
["A9C61325","ACTI 9 REFLEX IC60N TI24 25 A 3P B",1,"ks",{"v":555.66,"d":"555.660"},"3606480455506",{"v":16.5,"d":"16.50"},{"v":9.2,"d":"9.20"},{"v":11.2,"d":"11.20"},{"v":699,"d":"699.00"},"ES","8536201090","https://www.se.com/sk/sk/product/A9C61325","istič Reflex iC60N Ti24 25 A 3P char. B",0.08]
["A9C34811","IMP. RELÉ ITLM 16A 1ZAP 230-240VAC",1,"ks",{"v":40.13099999999999,"d":"40.131"},"3606480092107",{"v":8.4,"d":"8.40"},{"v":1.8,"d":"1.80"},{"v":7.2,"d":"7.20"},{"v":111,"d":"111.00"},"BE","8536490099","https://www.se.com/sk/sk/product/A9C34811","impulzné relé iTLm - 1P - 1Z - 16A - cievka 230...240 VAC 50/60Hz",0.01]
["A9C32811","IMP. RELÉ ITLS16A 1ZAP 230/240VAC 110",1,"ks",{"v":40.13099999999999,"d":"40.131"},"3606480092046",{"v":9.5,"d":"9.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":113,"d":"113.00"},"BE","8536490099","https://www.se.com/sk/sk/product/A9C32811","impulzné relé iTLs - 1P - 1Z - 16A - cievka 110 VDC - 230...240 VAC 50/60Hz",0.01]
["A9C30212","IMP. RELÉ ITL16A 2ZAP 48VAC 24VDC",1,"ks",46.305,"3606480091872",{"v":8.5,"d":"8.50"},{"v":7.5,"d":"7.50"},{"v":1.8,"d":"1.80"},{"v":110,"d":"110.00"},"BE","8536419089","https://www.se.com/sk/sk/product/A9C30212","impulzné relé iTL - 2P - 2 Z - 16A - cievka 24 VDC - 48 VAC 50/60Hz",0.01]
["A9C22818","STÝKAČ ICT16A 2ZAP 2VYP 220-240VAC 50HZ",1,"ks",52.038,"3606480097102",{"v":12.1,"d":"12.10"},{"v":4,"d":"4.00"},{"v":11.1,"d":"11.10"},{"v":238,"d":"238.00"},"FR","8536490099","https://www.se.com/sk/sk/product/A9C22818","iCT 16A 2Z 2V 220/240V 50Hz stýkač",0.03]
["A9C22711","ICT16A 1NO 230/240V AC 50HZ",1,"ks",{"v":22.049999999999997,"d":"22.050"},"3606480088643",{"v":8.5,"d":"8.50"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":110,"d":"110.00"},"FR","8536490099","https://www.se.com/sk/sk/product/A9C22711","iCT 16A 1Z 230/240V 50Hz stýkač",0.01]
["A9C21843","STÝKAČ ICT40A 3ZAP 220-240VAC 50HZ",1,"ks",{"v":57.33,"d":"57.330"},"3606480096860",{"v":12,"d":"12.00"},{"v":6,"d":"6.00"},{"v":11,"d":"11.00"},{"v":339,"d":"339.00"},"FR","8536490099","https://www.se.com/sk/sk/product/A9C21843","iCT 40A 3Z 220/240V 50Hz MO stýkač",0.04]
["A9C21532","STÝKAČ ICT25A 2ZAP 220VAC 50HZ RUČ. OVL.",1,"ks",{"v":27.782999999999994,"d":"27.783"},"3606480375316",{"v":8.5,"d":"8.50"},{"v":1.8,"d":"1.80"},{"v":7.5,"d":"7.50"},{"v":118,"d":"118.00"},"FR","8536490099","https://www.se.com/sk/sk/product/A9C21532","iCT 25A 2Z 220V 50Hz MO stýkač",0.01]
["A9C20837","STÝKAČ ICT25A 4VYP 220-240VAC 50HZ",1,"ks",{"v":46.745999999999995,"d":"46.746"},"3606480375101",{"v":12.2,"d":"12.20"},{"v":4.2,"d":"4.20"},{"v":11.2,"d":"11.20"},{"v":236,"d":"236.00"},"FR","8536490099","https://www.se.com/sk/sk/product/A9C20837","iCT 25A 4V 220/240V 50Hz stýkač",0.03]
["A9C20636","STÝKAČ ICT25A 2VYP 220-240VAC 60HZ",1,"ks",{"v":30.428999999999995,"d":"30.429"},"3606480375057",{"v":8.4,"d":"8.40"},{"v":1.9,"d":"1.90"},{"v":6.8,"d":"6.80"},{"v":123,"d":"123.00"},"FR","8536490099","https://www.se.com/sk/sk/product/A9C20636","iCT 25A 2NC 220...240V 60Hz contactor",0.01]
["A9C18195","MODUL IMDU",1,"ks",{"v":211.67999999999995,"d":"211.680"},"3606480393402",{"v":9.2,"d":"9.20"},{"v":2,"d":"2.00"},{"v":7.9,"d":"7.90"},{"v":47,"d":"47.00"},"BE","8538909999","https://www.se.com/sk/sk/product/A9C18195","iMDU 24-48V DC napätový modul",0.01]
["A9C15405","MODUL. SIGNAL IATLS 24-240VAC/DC",1,"ks",{"v":37.925999999999995,"d":"37.926"},"3606480374845",{"v":7.7,"d":"7.70"},{"v":2.1,"d":"2.10"},{"v":9.3,"d":"9.30"},{"v":40,"d":"40.00"},"BE","8536508090","https://www.se.com/sk/sk/product/A9C15405","vzdialená signalizácia iATLs",0]
["A9A27062","ACTI9 5X DIŠTANČNÝ DIEL 9MM IC60 IID ICT",1,"ks",{"v":26.459999999999994,"d":"26.460"},"3606480088155",{"v":8.5,"d":"8.50"},{"v":7,"d":"7.00"},{"v":4.5,"d":"4.50"},{"v":81,"d":"81.00"},"HU","3926909790","https://www.se.com/sk/sk/product/A9A27062","Acti 9 - dištančná vložka - 9 mm biela",0]
["A9A26948","ACTI9 NAPÄŤ. SPÚŠŤ IMX-OF 12-24VAC/DC",1,"ks",{"v":60.85799999999999,"d":"60.858"},"3606480087912",{"v":9.5,"d":"9.50"},{"v":7.7,"d":"7.70"},{"v":8,"d":"8.00"},{"v":82,"d":"82.00"},"BE","8536301090","https://www.se.com/sk/sk/product/A9A26948","napäťová spúšť - iMX+OF - vypínacia jednotka - 12..24 VAC",0.01]
["A9A26916","Signalizačný kont. iSD 2-100mA sv. dole",1,"ks",{"v":17.198999999999998,"d":"17.199"},"3606482129177",9.25,{"v":7.7,"d":"7.70"},{"v":2,"d":"2.00"},{"v":34,"d":"34.00"},"IN","8536508090","https://www.se.com/sk/sk/product/A9A26916","Poruchový kontakt Acti9 iSD, 2-100 mA, svorky shora",0]
["A9A19801","RCBO pomocný kontakt OF",1,"ks",{"v":17.198999999999998,"d":"17.199"},"3606481158048",{"v":9.8,"d":"9.80"},{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":50,"d":"50.00"},"PT","8536909500","https://www.se.com/sk/sk/product/A9A19801","Acti 9 - RCBO pomocný kontakt OF",0.01]
["A9A15212","ZVONČ. TRANSFORMÁTOR TR 16VA 230V/12-18V",1,"ks",{"v":56.00699999999999,"d":"56.007"},"3606480097843",{"v":9.5,"d":"9.50"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":414,"d":"414.00"},"DE","8504312190","https://www.se.com/sk/sk/product/A9A15212","modulárny zvonkový transformátor iTR - 230 V 50..60 Hz - výstup 8..12 V - 16 VA",0.04]
["A9A15151","DRŽIAK TLAČIDIEL PRIEMER 22MM",1,"ks",{"v":10.583999999999998,"d":"10.584"},"3606480377020",{"v":6,"d":"6.00"},{"v":6.6,"d":"6.60"},{"v":5.4,"d":"5.40"},{"v":28,"d":"28.00"},"FR","3926909790","https://www.se.com/sk/sk/product/A9A15151","DIN montážna lišta - Ø 22 mm jednotky - pre ovládacie a signalizačné jednotky",0]
["9141046000","Montážny kit ZG-MDSR-MD10/20SR",1,"ks",{"v":135.84375,"d":"135.844"},"3606481819888",{"v":25,"d":"25.00"},{"v":3.5,"d":"3.50"},{"v":19.5,"d":"19.50"},{"v":400,"d":"400.00"},"CH","8481900090","https://www.se.com/sk/sk/product/9141046000","Mounting kit (ZG-MDSR): for flat and side installations",0]
["9121043000","Mosadzné puzdro pre snímač STP 200 mm",1,"ks",{"v":23.034375,"d":"23.034"},"7332552012938",{"v":21.6,"d":"21.60"},{"v":2.7,"d":"2.70"},{"v":2.7,"d":"2.70"},{"v":130,"d":"130.00"},"DE","9025900090","https://www.se.com/sk/sk/product/9121043000","Pocket STP 200 mm (7.87 in) Brass",0]
["9112105050","Šrúbenie špec. pre zváranie DN 50",1,"ks",{"v":124.03125,"d":"124.031"},"7332552005435",{"v":12.8,"d":"12.80"},{"v":7.2,"d":"7.20"},{"v":9.5,"d":"9.50"},{"v":910.2,"d":"910.20"},"SE","7419809099","https://www.se.com/sk/sk/product/9112105050","Welded Connection, DN50, For V241/V341 Valve.",0]
["9112103020","Šrúbenie špec. s vnútorným závitom DN 20",1,"ks",{"v":46.06875,"d":"46.069"},"7332552005275",{"v":5.5,"d":"5.50"},{"v":4.8,"d":"4.80"},{"v":2.8,"d":"2.80"},{"v":175.8,"d":"175.80"},"SE","7419809099","https://www.se.com/sk/sk/product/9112103020","Internal Thread Connection, DN20: V241/V341 Valve, Special High Pressure/Temp. for Primary Circuit in District Heating.",0]
["9112100032","Spoj. diel s vnútorným závitom DN 32",1,"ks",{"v":44.887499999999996,"d":"44.888"},"7332552005114",{"v":7.4,"d":"7.40"},{"v":3.3,"d":"3.30"},{"v":6.8,"d":"6.80"},{"v":402,"d":"402.00"},"DE","84819000","https://www.se.com/sk/sk/product/9112100032","skrutkovanie s vnútorným závitom DN 32",0]
["9001KR1UH5","Ovládacia hlavica stískacia",1,"ks",{"v":55.3620375,"d":"55.362"},"785901033417",{"v":9.5,"d":"9.50"},{"v":5.8,"d":"5.80"},{"v":5.4,"d":"5.40"},{"v":127,"d":"127.00"},"FR","8536508090","https://www.se.com/sk/sk/product/9001KR1UH5","Push button, Harmony 9001K, metal, flush, 7 colours choice, 30mm, spring return, 1NO",0]
["8800500000","Pohon M 3000",1,"ks",{"v":2598.75,"d":"2598.750"},"3606489659448",{"v":31,"d":"31.00"},{"v":22,"d":"22.00"},{"v":22.5,"d":"22.50"},{"v":3650,"d":"3,650.00"},"SE","85011091","https://www.se.com/sk/sk/product/8800500000","pohon TAC Forta M3000 pre guľový ventil",0.44]
["8800311030","POHON M 800 S2",1,"ks",826.875,"7332552013201",{"v":25.5,"d":"25.50"},{"v":17.8,"d":"17.80"},{"v":13.1,"d":"13.10"},{"v":1800,"d":"1,800.00"},"SE","8501109990","https://www.se.com/sk/sk/product/8800311030","pohon TAC Forta M 800 S2 pre guľový ventil",0.23]
["8800126000","MONTÁŽNA SADA L7SV",1,"ks",{"v":567,"d":"567.000"},"3606489659356",{"v":13,"d":"13.00"},{"v":4,"d":"4.00"},{"v":13,"d":"13.00"},{"v":998,"d":"998.00"},"SE","84811099","https://www.se.com/sk/sk/product/8800126000","Linkage kit L7SV: connecting M700 / M3000 / MV15B actuators with Satchwell valves",0]
["8740003000","Klap. pohon s pruž. TAC M-LF24 (4 Nm)",1,"ks",{"v":366.1875,"d":"366.188"},"3606489659165",{"v":28.2,"d":"28.20"},{"v":10.1,"d":"10.10"},{"v":12.4,"d":"12.40"},{"v":1508,"d":"1,508.00"},"CH","8501109190","https://www.se.com/sk/sk/product/8740003000","pohon on/off TAC M-LF24 (4Nm) - pružina vratná 24V AC",0.18]
["8455051000","Pohon MZ 20A",1,"ks",259.875,"3606489659042",{"v":12,"d":"12.00"},{"v":8,"d":"8.00"},{"v":9.5,"d":"9.50"},{"v":259,"d":"259.00"},"IT","8501109190","https://www.se.com/sk/sk/product/8455051000","MZ20A Electric Zone Valve Actuator, Modulating, Non-Spring Return, 24Vac, 200N, Linear, IP43",0.03]
["83920","NÁSTENNÁ KRABICA PRE ZÁS. UNIKA 103X255",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3303430839200",{"v":24.6,"d":"24.60"},{"v":10.9,"d":"10.90"},{"v":10,"d":"10.00"},{"v":400,"d":"400.00"},"IT","3926909790","https://www.se.com/sk/sk/product/83920","Mounting box, Mureva PK, 103x255",0]
["83566","PRÍVODKA NÁST.B.SC IP67 32A 250V 2P+E",1,"ks",{"v":17.657639999999997,"d":"17.658"},"3303430835660",{"v":11,"d":"11.00"},{"v":15,"d":"15.00"},{"v":19.5,"d":"19.50"},{"v":422,"d":"422.00"},"IT","8536699099","https://www.se.com/sk/sk/product/83566","PratiKa-priem.prívodka nást.s boxom-2P+E-32 A 250 VAC-IP67-skrut. svorky",""]
["83159","ZÁSUVKA NÁST.B. SC IP67 16A 415V 3P+N+E",1,"ks",{"v":18.962999999999997,"d":"18.963"},"3303430831594",{"v":13,"d":"13.00"},{"v":15,"d":"15.00"},{"v":10.7,"d":"10.70"},{"v":428,"d":"428.00"},"IT","8536699099","https://www.se.com/sk/sk/product/83159","PratiKa-priem. zás. nást.s boxom-3P+N+E-16 A 415 VAC-IP67-skrut. svorky",0]
["82076","ZÁSUVKA UNIKA INTERLOCK 16A 2P 400-240V",1,"ks",{"v":216.08999999999997,"d":"216.090"},"3303430820765",{"v":26.1,"d":"26.10"},{"v":10.6,"d":"10.60"},{"v":17.3,"d":"17.30"},{"v":2320,"d":"2,320.00"},"IT","8536699099","https://www.se.com/sk/sk/product/82076","Interlocked socket, Mureva PK, 16A, 2P, 230V, IP65",0]
["81709","VIDLICA UHL.90° SC IP44 16A 415V 3P+N+E",1,"ks",{"v":18.080999999999996,"d":"18.081"},"3303430817093",{"v":10.5,"d":"10.50"},{"v":12,"d":"12.00"},{"v":6.5,"d":"6.50"},{"v":160,"d":"160.00"},"IT","8536699099","https://www.se.com/sk/sk/product/81709","PratiKa-priem.vidlica uhlová 90°-3P+N+E-16 A 415 VAC-IP44-skrut. svorky",0]
["81583","PRÍVODKA NÁST.B.SC IP67 63A 415V 3P+N+E",1,"ks",{"v":42.33599999999999,"d":"42.336"},"3303430815839",{"v":27.5,"d":"27.50"},{"v":18,"d":"18.00"},{"v":10.5,"d":"10.50"},{"v":1109,"d":"1,109.00"},"IT","8536699099","https://www.se.com/sk/sk/product/81583","PratiKa-priem.prívodka nást.s boxom-3P+N+E-63 A 415 VAC-IP67-skrut. svorky",0]
["81391","VIDLICA SPOJOV. SC IP67 125A 250V 3P+E",1,"ks",{"v":127.00799999999998,"d":"127.008"},"3303430813910",{"v":30.6,"d":"30.60"},{"v":12.9,"d":"12.90"},{"v":12.9,"d":"12.90"},{"v":1514,"d":"1,514.00"},"IT","8536699099","https://www.se.com/sk/sk/product/81391","PratiKa-priem.vidlica spojovacia-3P+E-125 A 250 VAC-IP67-skrut. svorky",0]
["81144","ZÁSUVKA 65 BC IP65 16A 250V 2P+E UK GREY",1,"ks",16.317,"3303430811442",{"v":8.5,"d":"8.50"},{"v":4.5,"d":"4.50"},{"v":6.5,"d":"6.50"},{"v":312,"d":"312.00"},"IT","8536699099","https://www.se.com/sk/sk/product/81144","PratiKa-zás.1x2P+E -10/16A 250VAC-65x85mm-IP65-skrut.sv.-sivá-povrchová montáž",0]
["7311725000","Reg. ventil závit. 3-cestný V311T/15/4",1,"ks",212.625,"3606489658700",{"v":18.5,"d":"18.50"},{"v":4.5,"d":"4.50"},{"v":8.5,"d":"8.50"},{"v":909,"d":"909.00"},"SE","8481807100","https://www.se.com/sk/sk/product/7311725000","Venta V311T Globe Valve, 3-Way, PN16, Rp 1/2 Internal Thread, DN15, 4.0 Kvs, Nodular Iron, Brass plug.",0]
["7219262010","Ventil reg. 2-cestný, prírubový V292/100",1,"ks",{"v":5374.6875,"d":"5374.688"},"3606481076953",{"v":23.5,"d":"23.50"},{"v":34.5,"d":"34.50"},{"v":41,"d":"41.00"},{"v":39600,"d":"39,600.00"},"DE","8538909999","https://www.se.com/sk/sk/product/7219262010","V292 Globe Valve, 2-Way, PN25, Flanged, DN100, 130 Kvs, Nodular Iron Body and Stainless Steel Trim, Stem Down Closed.",0]
["7214110000","Regulačný ventil závitový V241/15/0,4",1,"ks",{"v":295.3125,"d":"295.313"},"3606489658458",{"v":16.5,"d":"16.50"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":966,"d":"966.00"},"SE","84811099","https://www.se.com/sk/sk/product/7214110000","Venta V241 Globe Valve, 2-Way, PN16, G 1 External Thread, DN15, Kvs 0.40, Bronze Body, Stainless Trim, Stem Up Closed.",0]
["7213134000","Regulačný ventil prírubový V231/20/6.3",1,"ks",{"v":584.71875,"d":"584.719"},"3606481819758",{"v":23,"d":"23.00"},{"v":10.5,"d":"10.50"},{"v":15.5,"d":"15.50"},{"v":4378,"d":"4,378.00"},"SE","8481807100","https://www.se.com/sk/sk/product/7213134000","Venta V231 Globe Valve, 2-Way, PN25, Flanged, DN20, Kvs 6.3, Nodular Iron, Stainless Plug and Seat, Stem Up Closed.",0]
["7212254010","Ventil reg. 2-cestný, prírubový V222/65/",1,"ks",{"v":1240.3125,"d":"1240.313"},"3606481076908",{"v":35,"d":"35.00"},{"v":18.5,"d":"18.50"},{"v":29.5,"d":"29.50"},{"v":17,"d":"17.00"},"DE","8481807100","https://www.se.com/sk/sk/product/7212254010","V222 Globe Valve, 2-Way, PN16, Flanged, Balanced plug, DN65, Kvs 63, Cast Iron Body, Stainless plug and seat",0]
["7211720000","Regulačný ventil závitový V211/T15/2,5",1,"ks",259.875,"3606481819680",{"v":16.5,"d":"16.50"},{"v":5,"d":"5.00"},{"v":8.5,"d":"8.50"},{"v":851,"d":"851.00"},"SE","84811099","https://www.se.com/sk/sk/product/7211720000","Venta V211T Globe Valve, 2-Way, PN16, Rp 1/2 Internal thread, DN15, 2.5 Kvs, Nodular Iron, Brass Plug, Stem Up Closed.",0]
["65316","Sada ENVT pre Micrologic E a P",1,"ks",{"v":18.711000000000002,"d":"18.711"},"3303432448912",{"v":20,"d":"20.00"},{"v":30,"d":"30.00"},{"v":10,"d":"10.00"},{"v":1,"d":"1.00"},"","","https://www.se.com/sk/sk/product/65316","external neutral voltage tap, drawout ComPact NS630b to NS1600 with MicroLogic P",0]
["64906","1 CLUSTER PRE ŠASI",1,"ks",{"v":36.3825,"d":"36.383"},"3303430649069",{"v":5.3,"d":"5.30"},{"v":2.4,"d":"2.40"},{"v":4.2,"d":"4.20"},{"v":219,"d":"219.00"},"FR","8538909999","https://www.se.com/sk/sk/product/64906","Disconnecting contact cluster for chassis, MasterPact NT/NW drawout, spare part",0]
["56226","VIGIREX RH10P 110/130V AC 50/60HZ 0,5 A",1,"ks",{"v":401.30999999999995,"d":"401.310"},"3303430562269",{"v":11,"d":"11.00"},{"v":0.1,"d":"0.10"},{"v":7,"d":"7.00"},{"v":2001.9999999999998,"d":"2,002.00"},"FR","85364900","https://www.se.com/sk/sk/product/56226","ochranné relé na reziduálny prúd RH10P - 500 mA - 130 V",0.24]
["56145","VIGIREX RH10M 380/415V AC 50/60HZ 0,3 A",1,"ks",{"v":299.87999999999994,"d":"299.880"},"3303430561453",{"v":9.2,"d":"9.20"},{"v":8.8,"d":"8.80"},{"v":8.1,"d":"8.10"},{"v":368,"d":"368.00"},"FR","85364900","https://www.se.com/sk/sk/product/56145","ochranné relé na reziduálny prúd RH10M - 300 mA - 415 V",0.04]
["54443","EXTERNÝ NAPÁJACÍ MODUL AD 110/130 VAC",1,"ks",{"v":249.48,"d":"249.480"},"3303430544432",{"v":12.3,"d":"12.30"},{"v":7,"d":"7.00"},{"v":9.7,"d":"9.70"},{"v":349,"d":"349.00"},"FR","85389099","https://www.se.com/sk/sk/product/54443","externí napájecí modul 110 V AC - pro NS630b..3200/NT/NW",0]
["515504","Dvojzásuvka 230V, s výst. kan. od rozv.",1,"ks",{"v":13.612409999999995,"d":"13.612"},"4013984123043",{"v":17,"d":"17.00"},{"v":4.5,"d":"4.50"},{"v":8,"d":"8.00"},{"v":190,"d":"190.00"},"DE","8536699099","https://www.se.com/sk/sk/product/515504","Dvojzásuvka, Elso Renova, 230V, s výstupným kanálom od rozvádzača",0]
["5141104010","PRIESTOROVÝ SNÍMAČ TEPLOTY",1,"ks",{"v":76.190625,"d":"76.191"},"7332552012730",{"v":16.4,"d":"16.40"},{"v":5.7,"d":"5.70"},{"v":15.3,"d":"15.30"},{"v":220,"d":"220.00"},"SE","9025190090","https://www.se.com/sk/sk/product/5141104010","Temp Sensor: STO500, Outdoor, Andover Continuum",0.03]
["5127010000","STT901 protimrazový termostat A 1,8m",1,"ks",{"v":194.90625,"d":"194.906"},"7332552012631",{"v":20,"d":"20.00"},{"v":13.5,"d":"13.50"},{"v":9,"d":"9.00"},{"v":572,"d":"572.00"},"SE","9032108090","https://www.se.com/sk/sk/product/5127010000","Frost Thermostat: STT901, 1.8 m (5.9 ft) Capillary, Automatic, Water",0.07]
["5123134010","Ponorný snímač teploty STP 200-150",1,"ks",{"v":53.15625,"d":"53.156"},"7332552012150",{"v":28.1,"d":"28.10"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":107,"d":"107.00"},"SE","9025190090","https://www.se.com/sk/sk/product/5123134010","Temp Sensor: STP200-150, Pipe, 150 mm (5.9 in), TAC I/NET",0.02]
["5123132010","Snímač teploty ponorný STP200-100",1,"ks",{"v":53.15625,"d":"53.156"},"7332552012143",{"v":20.2,"d":"20.20"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":104,"d":"104.00"},"SE","9025190090","https://www.se.com/sk/sk/product/5123132010","STP Series temperature sensor, STP200-100, pipe, 100 mm, TAC I/NET compatible",0.02]
["5123004010","Kanálový snímač teploty STD 100-100",1,"ks",{"v":47.840624999999996,"d":"47.841"},"7332552011856",{"v":28.2,"d":"28.20"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":117,"d":"117.00"},"SE","90329000","https://www.se.com/sk/sk/product/5123004010","STD Series STD100-100 Model, temperature sensor, duct, 100mm, TAC Vista And TAC Xenta compatible",0.02]
["50172","OBMEDZOVAČ CARDEW 660V AC",1,"ks",{"v":369.1996874999999,"d":"369.200"},"3303430501725",{"v":17,"d":"17.00"},{"v":9.9,"d":"9.90"},{"v":11.7,"d":"11.70"},{"v":683,"d":"683.00"},"FR","8536309090","https://www.se.com/sk/sk/product/50172","cartridge Cardew - typ C - 660 V",""]
["490NTW00080","KÁBEL ETHERNET TIENENÝ SFTP, 80M",1,"ks",259.182,"3595862002226",{"v":39.5,"d":"39.50"},{"v":9,"d":"9.00"},{"v":38,"d":"38.00"},{"v":3475,"d":"3,475.00"},"FR","8544421000","https://www.se.com/sk/sk/product/490NTW00080","Ethernet ConneXium cable - shielded twisted pair straight cord - 80 m - 2 x RJ45",0]
["489460","Rámček M-Elegance 4násobný Diamond Silv",1,"ks",{"v":90.67085999999998,"d":"90.671"},"4042811050412",{"v":30.8,"d":"30.80"},{"v":2.6,"d":"2.60"},{"v":9.4,"d":"9.40"},{"v":260,"d":"260.00"},"DE","7016907000","https://www.se.com/sk/sk/product/489460","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["489219","M-PLAN SKLO DVOJRÁMČEK BRILLIANT WHITE",1,"ks",{"v":51.34459679999999,"d":"51.345"},"4042811081423",{"v":16.5,"d":"16.50"},{"v":2.7,"d":"2.70"},{"v":9.2,"d":"9.20"},{"v":144,"d":"144.00"},"DE","7016907000","https://www.se.com/sk/sk/product/489219","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["486514","Rámček M-Plan 5násobný Antracit",1,"ks",{"v":23.245519499999993,"d":"23.246"},"4011281895427",{"v":37.5,"d":"37.50"},{"v":1.7,"d":"1.70"},{"v":9.4,"d":"9.40"},{"v":114,"d":"114.00"},"DE","3925901000","https://www.se.com/sk/sk/product/486514","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["48605","ESCUTCHEON BLANKING PLATE",1,"ks",{"v":109.1475,"d":"109.148"},"3303430486053",{"v":35.5,"d":"35.50"},{"v":1,"d":"1.00"},{"v":30.5,"d":"30.50"},{"v":1887,"d":"1,887.00"},"FR","3926909790","https://www.se.com/sk/sk/product/48605","zaslepovací panel - pre Masterpact NW/NW DC",0]
["48598","KRYT SVORIEK POM. OBVODOV PRE NW4000B",1,"ks",135.135,"3303430485988",{"v":102.6,"d":"102.60"},{"v":11.3,"d":"11.30"},{"v":14.3,"d":"14.30"},{"v":2660,"d":"2,660.00"},"FR","8547200090","https://www.se.com/sk/sk/product/48598","pomocný kryt svoriek - pre 4P Masterpact NW",0]
["48565","UZAMYKANIE POLOHY ODPOJ. KIRK",1,"ks",{"v":187.11,"d":"187.110"},"3303430485650",{"v":9.5,"d":"9.50"},{"v":1.5,"d":"1.50"},{"v":6.5,"d":"6.50"},{"v":28,"d":"28.00"},"FR","8301409000","https://www.se.com/sk/sk/product/48565","Kirk adaptačná sada bez zámkov - pre Masterpact NW podvozok",0]
["48550","RONIS - 2 ZÁMKY S ROVNAK. KĽÚČOM",1,"ks",{"v":188.14950000000002,"d":"188.150"},"3303430485506",{"v":12.4,"d":"12.40"},{"v":7,"d":"7.00"},{"v":9,"d":"9.00"},{"v":351,"d":"351.00"},"FR","8538909999","https://www.se.com/sk/sk/product/48550","Ronis zámok - adaptačná sada - pre NW - OFF uzamknuté v polohe - 2 rovnaké kľúče",""]
["48523","MOT. POHON S PREVODOM 100/130VDC",1,"ks",{"v":1143.45,"d":"1143.450"},"3303430485230",{"v":22.9,"d":"22.90"},{"v":12.7,"d":"12.70"},{"v":13.1,"d":"13.10"},{"v":1746,"d":"1,746.00"},"FR","8501310099","https://www.se.com/sk/sk/product/48523","motorový pohon - MCH - 100..130 V DC - výsuvný istič",0.21]
["48511","2. MX 24/30VAC/DC PRE VÝSUV. ISTIČ",1,"ks",218.295,"3303430485117",{"v":8.3,"d":"8.30"},{"v":3.4,"d":"3.40"},{"v":6.1,"d":"6.10"},{"v":1166,"d":"1,166.00"},"FR","8538909999","https://www.se.com/sk/sk/product/48511","vypínacia napäťová špúšť MX - 24 V DC/AC 50/60Hz",0.14]
["48485","XF 277VAC PRE VÝSUV. ISTIČ",1,"ks",{"v":223.4925,"d":"223.493"},"3303430484851",{"v":6,"d":"6.00"},{"v":3,"d":"3.00"},{"v":9,"d":"9.00"},{"v":1170,"d":"1,170.00"},"FR","85389099","https://www.se.com/sk/sk/product/48485","zapínacia napäťová špúšť XF - 277 V AC 50/60Hz",0.14]
["48476","NÍZKOÚROVŇ. KONTAKT SDE PRE VÝSUV. ISTIČ",1,"ks",{"v":73.80449999999999,"d":"73.805"},"3303430484769",{"v":11,"d":"11.00"},{"v":5,"d":"5.00"},{"v":11,"d":"11.00"},{"v":68,"d":"68.00"},"FR","85389099","https://www.se.com/sk/sk/product/48476","pomocný kontakt - 1 SDE nízkoúrovňový",0.01]
["48434","SKRAT. SÚPRAVA PRE ŠASI 4P NW08 AŽ NW40",1,"ks",{"v":2286.9,"d":"2286.900"},"3303430484349",{"v":61,"d":"61.00"},{"v":6,"d":"6.00"},{"v":15.5,"d":"15.50"},{"v":3450,"d":"3,450.00"},"FR","85389099","https://www.se.com/sk/sk/product/48434","Chassis earthing kit, MasterPact NW drawout, 4P, spare part",0]
["48413","HOR. 3P PRED. PRÍVODY 2000A PRE ŠASI",1,"ks",{"v":337.8375,"d":"337.838"},"3303430484134",{"v":8,"d":"8.00"},{"v":2,"d":"2.00"},{"v":18,"d":"18.00"},{"v":6924,"d":"6,924.00"},"FR","8538909999","https://www.se.com/sk/sk/product/48413","predné pripojenie horná montáž - 3P - pre NW 20 šasi",0.8300000000000001]
["48403","NW 4P 800/1250A ŠASI N1 N1 H1HA",1,"ks",{"v":2079,"d":"2079.000"},"3303430484035",{"v":60,"d":"60.00"},{"v":65,"d":"65.00"},{"v":70,"d":"70.00"},{"v":46736,"d":"46,736.00"},"FR","85389099","https://www.se.com/sk/sk/product/48403","šasi - na NW800..1250N1 - 4P - 1250 A",5.61]
["48352","NW 63 H2 4P ZÁKLADNÝ MODUL, VÝSUVNÝ",1,"ks",{"v":52508.2635,"d":"52508.264"},"3303430483526",{"v":120,"d":"120.00"},{"v":60,"d":"60.00"},{"v":50,"d":"50.00"},{"v":61322,"d":"61,322.00"},"FR","8536209090","https://www.se.com/sk/sk/product/48352","istič Masterpact NW63H2 - 6300 A - 4P - výsuvný - bez jednotky spúšte",7.36]
["48349","NW 63 H2 3P ZÁKLADNÝ MODUL, VÝSUVNÝ",1,"ks",{"v":41431.351500000004,"d":"41431.352"},"3303430483496",{"v":120,"d":"120.00"},{"v":75,"d":"75.00"},{"v":75,"d":"75.00"},{"v":132286,"d":"132,286.00"},"FR","8536209090","https://www.se.com/sk/sk/product/48349","istič Masterpact NW63H2 - 6300 A - 3P - výsuvný - bez jednotky spúšte",15.870000000000001]
["48326","NW 40 HF 3P ZÁKLADNÝ MODUL, VÝSUVNÝ",1,"ks",{"v":16169.4225,"d":"16169.423"},"3303430483267",{"v":37.5,"d":"37.50"},{"v":29.5,"d":"29.50"},{"v":30.5,"d":"30.50"},{"v":52035,"d":"52,035.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48326","odpínač Masterpact NW40HF - 4000 A - 690 V - 3P - výsuvný",6.24]
["48304","NW 25 HA 3P VÝSUVNÝ",1,"ks",9615.375,"3303430483045",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":48434,"d":"48,434.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48304","odpínač Masterpact NW25HA - 2500 A - 690 V - 3P - výsuvný",5.8100000000000005]
["48298","NW 20 HA 4P VÝSUVNÝ",1,"ks",7536.375,"3303430482987",{"v":49.5,"d":"49.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":49514,"d":"49,514.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48298","odpínač Masterpact NW20HA - 2000 A - 690 V - 4P - výsuvný",5.94]
["48278","NW 16 HF 3P ZÁKLADNÝ MODUL, VÝSUVNÝ",1,"ks",6392.925,"3303430482789",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47175,"d":"47,175.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48278","odpínač Masterpact NW16HF - 1600 A - 690 V - 3P - výsuvný",5.66]
["48273","NW 16 H1 3P ZÁKLADNÝ MODUL, VÝSUVNÝ",1,"ks",{"v":5197.5,"d":"5197.500"},"3303430482734",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47035,"d":"47,035.00"},"FR","8536209090","https://www.se.com/sk/sk/product/48273","istič Masterpact NW16H1 - 1600 A - 3P - výsuvný - bez jednotky spúšte",5.64]
["48249","NW 10 HA 3P VÝSUVNÝ",1,"ks",4521.825,"3303430482499",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47048,"d":"47,048.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48249","odpínač Masterpact NW10HA - 1000 A - 690 V - 3P - výsuvný",5.65]
["48233","NW 08 L1 3P ZÁKLADNÝ MODUL, VÝSUVNÝ",1,"ks",{"v":4989.599999999999,"d":"4989.600"},"3303430482338",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":49682,"d":"49,682.00"},"FR","8536209090","https://www.se.com/sk/sk/product/48233","istič Masterpact NW08L1 - 800 A - 3P - výsuvný - bez jednotky spúšte",5.96]
["48208","MOT. POHON S PREVODOM 100/130VDC",1,"ks",1195.425,"3303430482086",{"v":22.9,"d":"22.90"},{"v":12.7,"d":"12.70"},{"v":13.1,"d":"13.10"},{"v":1740,"d":"1,740.00"},"FR","8501200090","https://www.se.com/sk/sk/product/48208","motorový pohon - MCH - 100..130 V DC - pevný istič",0.21]
["48174","DOL. 4P ZADNÉ HORIZ.PRÍVODY 3200A PEVNÉ",1,"ks",{"v":472.9725,"d":"472.973"},"3303430481744",{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},{"v":8,"d":"8.00"},{"v":4156,"d":"4,156.00"},"FR","8538909999","https://www.se.com/sk/sk/product/48174","pevný istič zadné horizontální pripojenie 2500/3200 A spodné 4P - pre NW 25..32",0.5]
["48161","HOR. 4P VERTIK. ZAD. PRÍV. 4000B/6300A",1,"ks",{"v":940.7475000000001,"d":"940.748"},"3303430481614",{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},{"v":8,"d":"8.00"},{"v":7312,"d":"7,312.00"},"FR","85389099","https://www.se.com/sk/sk/product/48161","pevný istič zadné vertikálne pripojenie 4000b/5000 A horné 4P - pre NW 40..50",0.88]
["48146","HOR. 3P HORIZ. ZAD. PRÍVODY NW 40B/63",1,"ks",{"v":706.86,"d":"706.860"},"3303430481461",{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},{"v":8,"d":"8.00"},{"v":5734,"d":"5,734.00"},"FR","85389099","https://www.se.com/sk/sk/product/48146","pevný istič zadné horizontální pripojenie 4000b/5000 A horné 3P - pre NW 40..50",0.6900000000000001]
["48136","HOR. 3P VERT. ZAD. PRÍV.Y NW 40B/63",1,"ks",{"v":706.86,"d":"706.860"},"3303430481362",{"v":7,"d":"7.00"},{"v":5,"d":"5.00"},{"v":8,"d":"8.00"},{"v":5734,"d":"5,734.00"},"FR","85389099","https://www.se.com/sk/sk/product/48136","výsuvný odpínač zadné pripojenie pre šasi vert.4000b/5000 A-horné 3P",0.6900000000000001]
["48122","NW 63 H2 4P ZÁKLADNÝ MODUL, PEVNÝ",1,"ks",{"v":52799.323500000006,"d":"52799.324"},"3303430481225",{"v":120,"d":"120.00"},{"v":60,"d":"60.00"},{"v":50,"d":"50.00"},{"v":62128,"d":"62,128.00"},"FR","8536209090","https://www.se.com/sk/sk/product/48122","istič Masterpact NW63H2 - 6300 A - 4P - pevný - bez jednotky spúšte",7.46]
["48108","NW 40B HA 3P PEVNÝ",1,"ks",{"v":20874.199500000002,"d":"20874.200"},"3303430481089",{"v":120,"d":"120.00"},{"v":57,"d":"57.00"},{"v":64,"d":"64.00"},{"v":118430,"d":"118,430.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48108","odpínač Masterpact NW40bHA - 4000 A - 690 V - 3P - pevný",14.21]
["48071","NW 25 H2 3P ZÁKLADNÝ MODUL, PEVNÝ",1,"ks",{"v":9459.449999999999,"d":"9459.450"},"3303430480716",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47251,"d":"47,251.00"},"FR","8536209090","https://www.se.com/sk/sk/product/48071","istič Masterpact NW25H2 - 2500 A - 3P - pevný - bez jednotky spúšte",5.67]
["48048","NW 16 HF 3P ZÁKLADNÝ MODUL, PEVNÝ",1,"ks",5457.375,"3303430480488",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47391,"d":"47,391.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48048","odpínač Masterpact NW16HF - 1600 A - 690 V - 3P - pevný",5.69]
["48037","NW 12 H2 4P ZÁKLADNÝ MODUL, PEVNÝ",1,"ks",5665.275,"3303430480372",{"v":49.5,"d":"49.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47252,"d":"47,252.00"},"FR","8536209090","https://www.se.com/sk/sk/product/48037","istič Masterpact NW12H2 - 1250 A - 4P - pevný - bez jednotky spúšte",5.67]
["48020","NW 10 HF 3P ZÁKLADNÝ MODUL, PEVNÝ",1,"ks",4625.775,"3303430480204",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47392,"d":"47,392.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48020","odpínač Masterpact NW10HF - 1000 A - 690 V - 3P - pevný",5.69]
["48006","NW 08 HF 3P ZÁKLADNÝ MODUL, PEVNÝ",1,"ks",3690.225,"3303430480068",{"v":37.5,"d":"37.50"},{"v":30.5,"d":"30.50"},{"v":29.5,"d":"29.50"},{"v":47390,"d":"47,390.00"},"FR","8536508090","https://www.se.com/sk/sk/product/48006","odpínač Masterpact NW08HF - 800 A - 690 V - 3P - pevný",5.69]
["47940","Náhradná páka akumulátora – NW",1,"ks",{"v":109.1475,"d":"109.148"},"3303430479406",{"v":17.5,"d":"17.50"},{"v":6,"d":"6.00"},{"v":27,"d":"27.00"},{"v":296,"d":"296.00"},"FR","85389099","https://www.se.com/sk/sk/product/47940","Spring charging handle, MasterPact NW, spare part",0]
["478325","Rámček M-Smart 3násobný Active",1,"ks",{"v":5.982498899999999,"d":"5.982"},"4042811043766",{"v":23.8,"d":"23.80"},{"v":2,"d":"2.00"},{"v":8.6,"d":"8.60"},{"v":34,"d":"34.00"},"DE","3925901000","https://www.se.com/sk/sk/product/478325","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["475560","KRYCÍ RÁMČEK 5-NÁS. EL/M PLATINUM SILVER",1,"ks",{"v":116.44982999999998,"d":"116.450"},"4042811101749",{"v":37.1,"d":"37.10"},{"v":1.1,"d":"1.10"},{"v":8.6,"d":"8.60"},{"v":480,"d":"480.00"},"DE","7326909890","https://www.se.com/sk/sk/product/475560","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["475214","Rámček M-Elegance 2násobný Rhodium Grey",1,"ks",{"v":46.15324559999999,"d":"46.153"},"4042811101404",{"v":9.2,"d":"9.20"},{"v":16.3,"d":"16.30"},{"v":2.6,"d":"2.60"},{"v":218,"d":"218.00"},"DE","7326909890","https://www.se.com/sk/sk/product/475214","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",0]
["47512","TLAČIDLO ELEKTRICKÉHO ZAPNUTIA BPFE",1,"ks",{"v":129.9375,"d":"129.938"},"3303430475125",{"v":6,"d":"6.00"},{"v":4,"d":"4.00"},{"v":6,"d":"6.00"},{"v":63,"d":"63.00"},"FR","8538909999","https://www.se.com/sk/sk/product/47512","tlač. el. zapnutia BPFE - 1 NO - pre Masterpact NT",0.01]
["47462","MOT. POHON S PREVODOM 100-130 VDC",1,"ks",{"v":1143.45,"d":"1143.450"},"3303430474623",{"v":12.5,"d":"12.50"},{"v":6,"d":"6.00"},{"v":18,"d":"18.00"},{"v":787,"d":"787.00"},"FR","8501200090","https://www.se.com/sk/sk/product/47462","motorový pohon - MCH - 100..130 V DC - výsuvný istič",0.09]
["47442","ZAP. CIEVKA XF 100-130 VAC-DC",1,"ks",{"v":223.4925,"d":"223.493"},"3303430474425",{"v":8.1,"d":"8.10"},{"v":3.5,"d":"3.50"},{"v":6.3,"d":"6.30"},{"v":1167,"d":"1,167.00"},"FR","8538909999","https://www.se.com/sk/sk/product/47442","zapínacia napäťová špúšť XF - 100..130 V DC/AC 50/60 Hz",0.14]
["47412","XF COM 24/30 VAC/VDC PRE VÝSUV. ISTIČ",1,"ks",{"v":223.4925,"d":"223.493"},"3303430474128",{"v":4,"d":"4.00"},{"v":9,"d":"9.00"},{"v":6,"d":"6.00"},{"v":1167,"d":"1,167.00"},"FR","8536301090","https://www.se.com/sk/sk/product/47412","zapínacia napäťová špúšť XF com - 24 V DC/AC 50/60Hz",0]
["47392","MOT. POHON S PREVODOM 100-130VDC",1,"ks",{"v":1143.45,"d":"1143.450"},"3303430473923",{"v":12.5,"d":"12.50"},{"v":6,"d":"6.00"},{"v":18,"d":"18.00"},{"v":782,"d":"782.00"},"FR","8501109190","https://www.se.com/sk/sk/product/47392","motorový pohon - MCH - 100..130 V DC - pevný istič",0.09]
["47370","2. MX 24/30VAC/DC PRE PEVNÝ ISTIČ",1,"ks",{"v":223.4925,"d":"223.493"},"3303430473701",{"v":8.3,"d":"8.30"},{"v":3.4,"d":"3.40"},{"v":6.1,"d":"6.10"},{"v":1160,"d":"1,160.00"},"FR","8538909999","https://www.se.com/sk/sk/product/47370","vypínacia napäťová špúšť MX - 24 V DC/AC 50/60Hz",0]
["47340","STANDARD SDE CONTACT FOR FIXED B",1,"ks",72.765,"3303430473404",{"v":5,"d":"5.00"},{"v":2,"d":"2.00"},{"v":18,"d":"18.00"},{"v":38,"d":"38.00"},"FR","8538909999","https://www.se.com/sk/sk/product/47340","pomocný kontakt - 1 SDE",0]
["47331","DOL. 4P PRED. PRÍVODY 630/1600A",1,"ks",{"v":291.06,"d":"291.060"},"3303430473312",{"v":28,"d":"28.00"},{"v":2,"d":"2.00"},{"v":8.7,"d":"8.70"},{"v":3506,"d":"3,506.00"},"FR","8538909999","https://www.se.com/sk/sk/product/47331","predné pripojenie spodná montáž - pre NT 06..16 - 4P",0.42]
["47299","MICROLOGIC 7.0 P PRE VÝSUVNÝ ISTIČ",1,"ks",{"v":3534.2999999999997,"d":"3534.300"},"3303430472995",{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},{"v":22,"d":"22.00"},{"v":1112,"d":"1,112.00"},"FR","90303900","https://www.se.com/sk/sk/product/47299","Micrologic 7.0 P jednotka spúští - LSIG - pre NT - výsuvný",0.13]
["47282","MICROLOGIC 2.0 A FOR FIXED",1,"ks",{"v":1871.1,"d":"1871.100"},"3303430472827",{"v":21.5,"d":"21.50"},{"v":6.8,"d":"6.80"},{"v":8,"d":"8.00"},{"v":297,"d":"297.00"},"FR","90303200","https://www.se.com/sk/sk/product/47282","Control unit MicroLogic 2.0A, MasterPact NT/NW fixed, basic protections (LI), ammeter",0.04]
["47253","NT 10 HA 4P VÝSUVNÝ",1,"ks",{"v":5197.5,"d":"5197.500"},"3303430472537",{"v":30,"d":"30.00"},{"v":41,"d":"41.00"},{"v":39,"d":"39.00"},{"v":4645,"d":"4,645.00"},"FR","8536508090","https://www.se.com/sk/sk/product/47253","odpínač Masterpact NT10HA - 1000 A - 690 V - 4P - výsuvný",0.56]
["47217","NT 08 L1 4P ZÁKLADNÝ MODUL, VÝSUVNÝ",1,"ks",{"v":4885.65,"d":"4885.650"},"3303430472179",{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":30,"d":"30.00"},{"v":5118,"d":"5,118.00"},"FR","8536209090","https://www.se.com/sk/sk/product/47217","istič Masterpact NT08L1 - 800 A - 4P - výsuvný - bez jednotky spúští",0.61]
["47210","NT 08 H1 3P ZÁKLADNÝ MODUL, VÝSUVNÝ",1,"ks",{"v":3274.4249999999997,"d":"3274.425"},"3303430472100",{"v":40,"d":"40.00"},{"v":25,"d":"25.00"},{"v":40,"d":"40.00"},{"v":23062,"d":"23,062.00"},"FR","8536209090","https://www.se.com/sk/sk/product/47210","istič Masterpact NT08H1 - 800 A - 3P - výsuvný - bez jednotky spúští",2.77]
["47145","NT 12 H1 4P ZÁKLADNÝ MODUL PEVNÝ",1,"ks",{"v":4261.95,"d":"4261.950"},"3303430471455",{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":15690,"d":"15,690.00"},"FR","8536209090","https://www.se.com/sk/sk/product/47145","istič Masterpact NT12H1 - 1250 A - 4P - pevný - bez jednotky spúští",1.8800000000000001]
["471219","Rámček M-Smart 2násobný popis pole Polar",1,"ks",{"v":9.573776099999998,"d":"9.574"},"4042811033200",{"v":16.2,"d":"16.20"},{"v":2.2,"d":"2.20"},{"v":8.5,"d":"8.50"},{"v":36,"d":"36.00"},"DE","3926909790","https://www.se.com/sk/sk/product/471219","Rámček, Merten M-Smart, trojnásobný s popisovým poľom, Polar",""]
["47077","1 ks nízkoúrovňový pom. kontakt OF (1 ks",1,"ks",81.081,"3303430470779",{"v":14,"d":"14.00"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":22,"d":"22.00"},"TH","8536508090","https://www.se.com/sk/sk/product/47077","ON/OFF (OF) indication contact, MasterPact NT, 1 changeover contact, low level, 5A/240VAC, spare part",0]
["47067","NÁHRADNÝ DIEL",1,"ks",{"v":8.9397,"d":"8.940"},"3303430470670",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":6.3,"d":"6.30"},{"v":18,"d":"18.00"},"","","https://www.se.com/sk/sk/product/47067","Transparent cover, MicroLogic P and H control units, lead sealed, spare part",0]
["34431","NS1000H ML5. 0E 4P KOMPL. ISTIČ PRED. PR",1,"ks",{"v":6237,"d":"6237.000"},"3606480345135",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":15970,"d":"15,970.00"},"IT","8536209090","https://www.se.com/sk/sk/product/34431","istič Compact NS1000H - Micrologic 5.0 E - 1000 A - 4P 4t",1.92]
["34401","NS630H ML2. 0E 3P KOMPL. ISTIČ PRED. PRI",1,"ks",2858.625,"3606480344848",{"v":23,"d":"23.00"},{"v":37,"d":"37.00"},{"v":39.5,"d":"39.50"},{"v":11890,"d":"11,890.00"},"IT","85362090","https://www.se.com/sk/sk/product/34401","Circuit breaker, ComPact NS630bH, 70kA/415VAC, Micrologic 2.0E trip unit, 630A, fixed, 3 poles 3d",1.43]
["33929","KRYCÍ RÁMIK NS3200",1,"ks",{"v":30.1455,"d":"30.146"},"785901623649",{"v":42,"d":"42.00"},{"v":2,"d":"2.00"},{"v":28,"d":"28.00"},{"v":290,"d":"290.00"},"US","3926909790","https://www.se.com/sk/sk/product/33929","escutcheon for toggle,fixed ComPact NS1600b to NS3200, manually operated, IP40",0]
["33884","2 RÝCHLOROZPÍNACIE KONTAKTY",1,"ks",176.715,"3303430338840",{"v":18,"d":"18.00"},{"v":5,"d":"5.00"},{"v":11,"d":"11.00"},{"v":94,"d":"94.00"},"FR","85389099","https://www.se.com/sk/sk/product/33884","standard early make contact, ComPact NS630b to NS1600, fixed, rotary handle position CAF, 1 changeover contact type",0]
["33872","UZAMYKANIE ZAP. POLOHA PRE OTOČ. RUKOVÄŤ",1,"ks",{"v":59.25150000000001,"d":"59.252"},"3303430338727",{"v":6.5,"d":"6.50"},{"v":2.3,"d":"2.30"},{"v":3.5,"d":"3.50"},{"v":160,"d":"160.00"},"FR","8538909999","https://www.se.com/sk/sk/product/33872","Ronis zámok - pre otočnú rukoväť - NS630b..1600 - ON - OFF poloha uzamknutia",0]
["33838","DIAĽK. ZAP./VYP. COM 048/060 VDC/VAC",1,"ks",1091.475,"3303430338383",{"v":18,"d":"18.00"},{"v":7,"d":"7.00"},{"v":13,"d":"13.00"},{"v":1404,"d":"1,404.00"},"FR","8501109990","https://www.se.com/sk/sk/product/33838","motorový pohon - MCH - 48 V AC - výsuvný istič",0.17]
["33813","MX 200/250 VAC/VDC PRE VÝSUV. ISTIČ",1,"ks",{"v":150.7275,"d":"150.728"},"3303430338130",{"v":8.5,"d":"8.50"},{"v":4,"d":"4.00"},{"v":6,"d":"6.00"},{"v":180.3,"d":"180.30"},"FR","8536309090","https://www.se.com/sk/sk/product/33813","vypínacia napäťová spúšť MX - 200..250 V DC/AC 50/60 Hz",0]
["33802","NÍZKOÚROVŇ. KONTAKT SDE PRE RUČNÉ. OVL.",1,"ks",31.185,"3303430338024",{"v":20,"d":"20.00"},{"v":2,"d":"2.00"},{"v":5,"d":"5.00"},{"v":37,"d":"37.00"},"FR","85389099","https://www.se.com/sk/sk/product/33802","pomocný kontakt - 1 SDE nízkoúrovňový",0]
["33775","PROFALUX - 2 ZÁMKY S RÔZNYMI KĽÚČMI",1,"ks",218.295,"3303430337751",{"v":6.6,"d":"6.60"},{"v":14.8,"d":"14.80"},{"v":4.9,"d":"4.90"},{"v":260,"d":"260.00"},"FR","8538909999","https://www.se.com/sk/sk/product/33775","zámok Profalux - adaptačná sada - pre NT šasi - poloha odpojená - 2 rôzne kľúče",0]
["33769","SADA PROFALUX UZAMYKANIA POLOHY OPOJENE",1,"ks",{"v":37.422000000000004,"d":"37.422"},"3303430337690",{"v":6.1,"d":"6.10"},{"v":1.6,"d":"1.60"},{"v":2.3,"d":"2.30"},{"v":16,"d":"16.00"},"IT","8538909999","https://www.se.com/sk/sk/product/33769","Profalux adaptačná sada bez zámku - pre NS630b..1600 NT/NT UL 489 šasi",0]
["33738","DOL. HORIZ. ZAD. PRÍVODY PRE 4P ŠASI 630",1,"ks",{"v":181.9125,"d":"181.913"},"3303430337386",{"v":6,"d":"6.00"},{"v":1.5,"d":"1.50"},{"v":4.5,"d":"4.50"},{"v":2384,"d":"2,384.00"},"FR","8536909500","https://www.se.com/sk/sk/product/33738","zadné pripojenie spodná montáž - 4P- pre NS 630b..1600 šasi",0.29]
["33703","ECO MODBUS PRE RUČNÉ AL. ELEK. OVLÁDANIE",1,"ks",{"v":275.46750000000003,"d":"275.468"},"3303430337034",{"v":9.3,"d":"9.30"},{"v":3,"d":"3.00"},{"v":7.6,"d":"7.60"},{"v":1056,"d":"1,056.00"},"FR","85389099","https://www.se.com/sk/sk/product/33703","ECO Modbus COM modul - pre manuálne ovládanie - pevný NS630b..1600",0.13]
["33702","MODBUS MODUL PRE RUČNÉ OVLÁDANIE",1,"ks",{"v":493.7625,"d":"493.763"},"3303430337027",{"v":9.3,"d":"9.30"},{"v":3,"d":"3.00"},{"v":7.6,"d":"7.60"},{"v":221,"d":"221.00"},"FR","8538909999","https://www.se.com/sk/sk/product/33702","Modbus COM modul - pre manuálne ovládanie - pevný NS630b..1600",0.03]
["33673","MN 380/480 VAC PRE PEVNÝ ISTIČ",1,"ks",{"v":192.3075,"d":"192.308"},"3303430336730",{"v":8.2,"d":"8.20"},{"v":3.5,"d":"3.50"},{"v":6.2,"d":"6.20"},{"v":152,"d":"152.00"},"FR","8536301090","https://www.se.com/sk/sk/product/33673","zníženie napätia MN – 380 - 480 V AC 50/60 Hz",0]
["33645","1 CABLE LUG ADAPTER 4P",1,"ks",{"v":332.64000000000004,"d":"332.640"},"3303430336457",{"v":27.2,"d":"27.20"},{"v":6.6,"d":"6.60"},{"v":21,"d":"21.00"},{"v":5576,"d":"5,576.00"},"FR","7419809099","https://www.se.com/sk/sk/product/33645","rozšířenie svoriek pre káble s oky-sada 4-4P-pre Masterpact NT-INS/INV630b..1600",0]
["33615","DOLNÉ 4P VERTIK. ZAD. PRÍVODY",1,"ks",239.085,"3303430336150",{"v":28,"d":"28.00"},{"v":2,"d":"2.00"},{"v":8.7,"d":"8.70"},{"v":2684,"d":"2,684.00"},"FR","8538909999","https://www.se.com/sk/sk/product/33615","zadné pripojenie spodná vert. montáž - 4P- pre NS 630b..1600",0.32]
["33612","HORNÉ 4PPREDNÉ PRÍVODY, PEVNÝ 1600A",1,"ks",{"v":202.70250000000001,"d":"202.703"},"3303430336129",{"v":27.9,"d":"27.90"},{"v":5.3,"d":"5.30"},{"v":12,"d":"12.00"},{"v":2080,"d":"2,080.00"},"FR","8538909999","https://www.se.com/sk/sk/product/33612","predné pripojenie horná montáž - 4P - pre NS 1600",0.25]
["33579","OBDĹŽNIK. PRÚD. TRAFO ZEM. SPOJENIA",1,"ks",{"v":602.91,"d":"602.910"},"785901335795",{"v":22.5,"d":"22.50"},{"v":5,"d":"5.00"},{"v":15.5,"d":"15.50"},{"v":2786,"d":"2,786.00"},"FR","8504318090","https://www.se.com/sk/sk/product/33579","CT externý senzor pre zemnú ochranu - pre NS/NT/NW",0]
["33545","MODUL BEZ OCHRANY PROTI PREŤAŽENIU",1,"ks",{"v":50.935500000000005,"d":"50.936"},"3303430335450",{"v":8.5,"d":"8.50"},{"v":3.5,"d":"3.50"},{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},"CN","8538909999","https://www.se.com/sk/sk/product/33545","IEC modul rozsahu nastavenia spúšte LT OFF - pre pevný istič Masterpact NT/NW",0]
["33536","MICROLOGIC 2. 0 E PRE VÝSUVNÝ ISTIČ",1,"ks",654.885,"3606480344688",{"v":38,"d":"38.00"},{"v":13.5,"d":"13.50"},{"v":14,"d":"14.00"},{"v":452,"d":"452.00"},"","","https://www.se.com/sk/sk/product/33536","Micrologic 2.0 E jednotka spúšte - pre Compact NS630b až 1600 výsuvný",0.04]
["33483","NS1600H ML2.0 - KOMPLETNÝ ISTIČ S PREDNÝ",1,"ks",{"v":3430.35,"d":"3430.350"},"3303430334835",{"v":60,"d":"60.00"},{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":13192,"d":"13,192.00"},"FR","8536209090","https://www.se.com/sk/sk/product/33483","istič Compact NS1600H - Micrologic 2.0 - 1600 A - 3 p 3t",1.79]
["33476","NS1000H ML2.0 4P - KOMPLETNÝ ISTIČ S PRE",1,"ks",4313.925,"3303430334767",{"v":60,"d":"60.00"},{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":16460,"d":"16,460.00"},"FR","85362090","https://www.se.com/sk/sk/product/33476","istič Compact NS1000H - Micrologic 2.0 - 1000 A - 4 p 4t",1.98]
["33444","NS1000 NA 3P ELEKTRICKY OVLÁDANÁ VERZIA",1,"ks",{"v":1351.35,"d":"1351.350"},"3303430334446",{"v":39,"d":"39.00"},{"v":36,"d":"36.00"},{"v":23,"d":"23.00"},{"v":11738,"d":"11,738.00"},"FR","8536508090","https://www.se.com/sk/sk/product/33444","odpínač Compact NS1000 NA - 1000 A - 3P",1.41]
["33428","NS1600 NA 3P",1,"ks",{"v":1975.05,"d":"1975.050"},"3303430334286",{"v":33,"d":"33.00"},{"v":35,"d":"35.00"},{"v":20,"d":"20.00"},{"v":9521,"d":"9,521.00"},"FR","8536508090","https://www.se.com/sk/sk/product/33428","odpínač Compact NS1600 NA - 1600 A - 3P",1.1400000000000001]
["33401","NS1250 H 3P ZAKLADNÝ ISTIČ VÝSUVNÝ ELEKT",1,"ks",{"v":2598.75,"d":"2598.750"},"3303430334019",{"v":40,"d":"40.00"},{"v":25,"d":"25.00"},{"v":40,"d":"40.00"},{"v":23024,"d":"23,024.00"},"FR","8536209090","https://www.se.com/sk/sk/product/33401","istič Compact NS1250H - 1250 A - 3P - výsuvný - bez jednotky spúšte",2.7600000000000002]
["33363","NS1600NFM5 A + PP 3P kompletná zostava",1,"ks",{"v":3742.2,"d":"3742.200"},"3303430333630",{"v":23,"d":"23.00"},{"v":37,"d":"37.00"},{"v":39.5,"d":"39.50"},{"v":12705,"d":"12,705.00"},"IT","8536209090","https://www.se.com/sk/sk/product/33363","Circuit breaker, ComPact NS1600N, 50kA/415VAC, Micrologic 5.0A trip unit, 1600A, fixed, 3 poles 3d",0]
["33341","NS1000 H 3P ZÁKLADNÝ ISTIČ VÝSUVNÝ",1,"ks",1819.125,"3303430333418",{"v":23,"d":"23.00"},{"v":37,"d":"37.00"},{"v":39.5,"d":"39.50"},{"v":12949,"d":"12,949.00"},"FR","8536209090","https://www.se.com/sk/sk/product/33341","istič Compact NS1000H - 1000 A - 3P - výsuvný - bez jednotky spúšte",1.55]
["33305","NS1250 H 4p ZáKLAD. ISTIČ ELEKTR. OVLÁD.",1,"ks",{"v":3014.5499999999997,"d":"3014.550"},"3303430333050",{"v":30,"d":"30.00"},{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":15060,"d":"15,060.00"},"FR","85362090","https://www.se.com/sk/sk/product/33305","istič Compact NS1250H - 1250 A - 4P - pevný - bez jednotky spúšte",1.81]
["33255","NS1250 H 4P ZÁKLADNÝ ISTIČ",1,"ks",{"v":3638.25,"d":"3638.250"},"3303430332558",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":13578,"d":"13,578.00"},"FR","8536209090","https://www.se.com/sk/sk/product/33255","istič Compact NS1250H - 4P - 1250 A - pevný - bez jednotky spúšte",1.6300000000000001]
["33225","NS630H 4P ZÁKLADNÝ ISTIČ",1,"ks",{"v":2027.0249999999999,"d":"2027.025"},"3303430332251",{"v":30,"d":"30.00"},{"v":37,"d":"37.00"},{"v":38,"d":"38.00"},{"v":13578,"d":"13,578.00"},"FR","8536209090","https://www.se.com/sk/sk/product/33225","istič Compact NS630bH - 630 A - 4P - pevný - bez jednotky spúšte",1.6300000000000001]
["33188","Motorový pohon 200/250 V DC",1,"ks",{"v":1455.3,"d":"1455.300"},"3303430331889",{"v":17.5,"d":"17.50"},{"v":6.5,"d":"6.50"},{"v":12.5,"d":"12.50"},{"v":783.5,"d":"783.50"},"FR","8501200090","https://www.se.com/sk/sk/product/33188","Gear motor MCH, fixed MasterPact NT, 200/250VDC, spare part",0.09]
["32556","ŠTÍTNAČELNÝPANEL PREPÁKU",1,"ks",{"v":18.711000000000002,"d":"18.711"},"3303430325567",{"v":15,"d":"15.00"},{"v":1,"d":"1.00"},{"v":10.2,"d":"10.20"},{"v":57,"d":"57.00"},"PL","3926909790","https://www.se.com/sk/sk/product/32556","štít. panel pre pevnú montáž-páčka-pre NS400..630",0]
["31369","INTERPACT INV2500 4P, PP",1,"ks",{"v":6923.7,"d":"6923.700"},"3303430313694",{"v":40,"d":"40.00"},{"v":5,"d":"5.00"},{"v":37,"d":"37.00"},{"v":55000,"d":"55,000.00"},"FR","8536508090","https://www.se.com/sk/sk/product/31369","odpínač Compact INV2500 - 2500 A - 4P",6.6000000000000005]
["31361","INTERPACT INV1000 4P,PP",1,"ks",{"v":1896.2999999999995,"d":"1896.300"},"3303430313618",{"v":43,"d":"43.00"},{"v":21,"d":"21.00"},{"v":33.5,"d":"33.50"},{"v":18630,"d":"18,630.00"},"FR","8536508090","https://www.se.com/sk/sk/product/31361","odpínač Compact INV1000 - 1000 A - 4P",2.24]
["31341","INTERPACT INS2500 4P,PP",1,"ks",{"v":6615,"d":"6615.000"},"3303430313410",{"v":59.7,"d":"59.70"},{"v":34.5,"d":"34.50"},{"v":61.4,"d":"61.40"},{"v":45000,"d":"45,000.00"},"FR","8536508090","https://www.se.com/sk/sk/product/31341","odpínač Compact INS2500 - 2500 A - 4P",7.46]
["31332","INTERPACT INS1000 3P,PP",1,"ks",{"v":1543.4999999999998,"d":"1543.500"},"3303430313328",{"v":35.5,"d":"35.50"},{"v":20,"d":"20.00"},{"v":33,"d":"33.00"},{"v":14000,"d":"14,000.00"},"FR","8536508090","https://www.se.com/sk/sk/product/31332","odpínač Compact INS1000 - 1000 A - 3P",1.81]
["31208","Metal enclosure IP55for front+black rota",1,"ks",1195.425,"3303430312086",{"v":37,"d":"37.00"},{"v":11,"d":"11.00"},{"v":84,"d":"84.00"},{"v":17948,"d":"17,948.00"},"FR","8538100000","https://www.se.com/sk/sk/product/31208","kovová skriňa - čierna rukoväť - oceľ - pre Interpact INS40 .. 160",0]
["31169","INV320 4P",1,"ks",{"v":696.78,"d":"696.780"},"3303430311690",{"v":22.9,"d":"22.90"},{"v":19.3,"d":"19.30"},{"v":19.8,"d":"19.80"},{"v":5477,"d":"5,477.00"},"PL","8536508090","https://www.se.com/sk/sk/product/31169","switch disconnector, Compact INV320, visible break, 320A, standard version with black rotary handle, 4 poles",0.66]
["31153","ZÁSKOK ZDROJOV S INTERPACT INS500 4-PÓL.",1,"ks",{"v":2775.9375,"d":"2775.938"},"3303430311539",{"v":23,"d":"23.00"},{"v":23,"d":"23.00"},{"v":50,"d":"50.00"},{"v":14930,"d":"14,930.00"},"FR","8536508090","https://www.se.com/sk/sk/product/31153","Manuálny prepínač napájania, TransferPacT FXM500, odpínač, 500A, 4P",1.79]
["31143","ZÁSKOK ZDROJOV S INTERPACT INS250-200A 4",1,"ks",{"v":1358.4375,"d":"1358.438"},"3303430311430",{"v":40,"d":"40.00"},{"v":15,"d":"15.00"},{"v":17,"d":"17.00"},{"v":6752,"d":"6,752.00"},"FR","8536508090","https://www.se.com/sk/sk/product/31143","ručný prepínač zdrojov Interpact INS250 - 4 póly - 200",0.81]
["31125","INS250 160A 4P ČERV. RUKOVÄŤ-ŽLTÉ ČELO",1,"ks",{"v":273.41999999999996,"d":"273.420"},"3303430311256",{"v":16.8,"d":"16.80"},{"v":13.8,"d":"13.80"},{"v":16.1,"d":"16.10"},{"v":2495,"d":"2,495.00"},"PL","8536508090","https://www.se.com/sk/sk/product/31125","switch disconnector, Compact INS250-160, 160A, with red rotary handle and yellow front, 4 poles",0.3]
["31107","INS250 4P",1,"ks",{"v":269.01,"d":"269.010"},"3303430311072",{"v":16.3,"d":"16.30"},{"v":17,"d":"17.00"},{"v":13.7,"d":"13.70"},{"v":2420,"d":"2,420.00"},"PL","8536508090","https://www.se.com/sk/sk/product/31107","odpínač Compact INS250 - 250 A - 4 p",0.29]
["31087","UZAMYK. ZARIADENIE NA ZÁMKU RONIS/PROFAL",1,"ks",{"v":29.546999999999997,"d":"29.547"},"3303430310877",{"v":15,"d":"15.00"},{"v":0.4,"d":"0.40"},{"v":10.5,"d":"10.50"},{"v":19,"d":"19.00"},"PL","3926909790","https://www.se.com/sk/sk/product/31087","sada uzamykanie pre zámok Profalux alebo Ronis - pre INS40 .. 250",0]
["31054","ADAPTÉR PRIAMEJ RUKOVÄTE (INS250)",1,"ks",27.342,"3303430310549",{"v":12,"d":"12.00"},{"v":2.5,"d":"2.50"},{"v":10,"d":"10.00"},{"v":169,"d":"169.00"},"PL","85389099","https://www.se.com/sk/sk/product/31054","otočná bočná kľučka INS/INV 250 - konverzné príslušenstvo",0]
["29452","1 POMOCNÝ KONTAKT OF/SD/SDE/SDV",1,"ks",{"v":35.279999999999994,"d":"35.280"},"3303430294528",{"v":6,"d":"6.00"},{"v":1.4,"d":"1.40"},{"v":7.8,"d":"7.80"},{"v":24,"d":"24.00"},"FR","8538909999","https://www.se.com/sk/sk/product/29452","pomocný kontakt - 1 OC alebo 1 SD alebo SDE 1 alebo 1 SDV nízka hladina",0]
["29349","ZÁKLADNÁ DOSKA + MECHANIKA",1,"ks",{"v":251.36999999999998,"d":"251.370"},"3303430293491",{"v":38,"d":"38.00"},{"v":31,"d":"31.00"},{"v":11,"d":"11.00"},{"v":4075.9999999999995,"d":"4,076.00"},"PL","8538909999","https://www.se.com/sk/sk/product/29349","mechanical interlocking, TransferPacT interlock accessory for ComPacT NSX100…250",0.49]
["28929","INS160 4P ČERVENÁ RUKOVÄŤ ŽLTÉ ČELO",1,"ks",{"v":189.62999999999997,"d":"189.630"},"3303430289296",{"v":15.3,"d":"15.30"},{"v":13.6,"d":"13.60"},{"v":11.9,"d":"11.90"},{"v":900,"d":"900.00"},"PL","8536508090","https://www.se.com/sk/sk/product/28929","odpínač Compact INS160 - 4P - 160 A",0.14]
["28927","INS125 4P ČERVENÁ RUKOVÄŤ ŽLTÉ ČELO",1,"ks",{"v":180.80999999999997,"d":"180.810"},"3303430289272",{"v":15.5,"d":"15.50"},{"v":11.5,"d":"11.50"},{"v":13.5,"d":"13.50"},{"v":1125,"d":"1,125.00"},"PL","8536508090","https://www.se.com/sk/sk/product/28927","odpínač Compact INS125 - 4P - 125 A",0.14]
["28900","ODPÍNAČ INS40",1,"ks",{"v":114.66,"d":"114.660"},"3303430289005",{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":9.5,"d":"9.50"},{"v":600,"d":"600.00"},"PL","8536508090","https://www.se.com/sk/sk/product/28900","odpínač Compact INS40 - 3P - 40 A",0.07]
["27048","PEVNÝ DIEL OTOČ RUKOVÄŤE NA KRYT ROZV",1,"ks",{"v":29.105999999999995,"d":"29.106"},"3303430270485",{"v":15,"d":"15.00"},{"v":4,"d":"4.00"},{"v":10.5,"d":"10.50"},{"v":103,"d":"103.00"},"ES","8538909999","https://www.se.com/sk/sk/product/27048","pred., bočná otočná rukoväť C60/120 a NC45/100/125 – čierna rukoväť",0.01]
["21119","POM KONTAKTY PRE P25M O+SD.F 1VYP",1,"ks",{"v":20.285999999999998,"d":"20.286"},"3303430211198",{"v":9,"d":"9.00"},{"v":1.2,"d":"1.20"},{"v":6.6,"d":"6.60"},{"v":45,"d":"45.00"},"CZ","85389099","https://www.se.com/sk/sk/product/21119","pomocný kontakt - 1 NC + 1 NO SD - pre P25M - 415 V - 2.2",0.01]
["21101","ISTENÝ MOTOR SPÚŠŤAČ P25M 3P 0.25A",1,"ks",{"v":97.01999999999998,"d":"97.020"},"3303430211013",{"v":9.5,"d":"9.50"},{"v":4.7,"d":"4.70"},{"v":8.5,"d":"8.50"},{"v":232,"d":"232.00"},"FR","8536201090","https://www.se.com/sk/sk/product/21101","motorový istič P25M - 0.25 A - 3P - termomagnetická spúšť",0.03]
["19106","CHR.SPÚŠŤ VIGING125 3P 125A 300-3000MA",1,"ks",{"v":1102.4999999999998,"d":"1102.500"},"3303430191063",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":13.8,"d":"13.80"},{"v":758,"d":"758.00"},"FR","3926909790","https://www.se.com/sk/sk/product/19106","NG125 - chráničová spúšť - Vigi NG125 - 3P - 125A - 300mA",0.09]
["19084","PLOMBOVATEĽNÉ KRYTY SKRUTIEK 1P 2KS",1,"ks",{"v":41.01299999999999,"d":"41.013"},"3303430190844",{"v":10,"d":"10.00"},{"v":3,"d":"3.00"},{"v":4,"d":"4.00"},{"v":50.9,"d":"50.90"},"FR","85389099","https://www.se.com/sk/sk/product/19084","kryt svoriek - 1 tyč - pre NG125",0.01]
["19061","NAPÄŤ SPÚŠŤ MNX 230V AC",1,"ks",{"v":357.21,"d":"357.210"},"3303430190615",{"v":10.9,"d":"10.90"},{"v":7.8,"d":"7.80"},{"v":5.5,"d":"5.50"},{"v":199,"d":"199.00"},"BE","85365080","https://www.se.com/sk/sk/product/19061","napäťová spúšť MNx - 220..240 V AC",0.02]
["19046","CHR.SPÚŠŤ VIGING125 4P 125A 0,3-0,5-1A",1,"ks",{"v":771.7499999999999,"d":"771.750"},"3303430190462",{"v":25,"d":"25.00"},{"v":9.1,"d":"9.10"},{"v":13.5,"d":"13.50"},{"v":849,"d":"849.00"},"FR","85363030","https://www.se.com/sk/sk/product/19046","NG125 - chráničová spúšť - Vigi NG125 - 4P - 125A - 300mA",0.1]
["19012","BLOK VIGI NG125 2P 63A 300MA A",1,"ks",{"v":180.80999999999997,"d":"180.810"},"3303430190127",{"v":15,"d":"15.00"},{"v":9.4,"d":"9.40"},{"v":15.5,"d":"15.50"},{"v":305,"d":"305.00"},"FR","85363030","https://www.se.com/sk/sk/product/19012","NG125 - chráničová spúšť - Vigi NG125 - 2P - 63A - 300mA",0.04]
["19011","BLOK VIGI NG125 2P 63A 30MA A",1,"ks",{"v":1014.2999999999998,"d":"1014.300"},"3303430190110",{"v":16,"d":"16.00"},{"v":9.5,"d":"9.50"},{"v":14,"d":"14.00"},{"v":340,"d":"340.00"},"FR","85363030","https://www.se.com/sk/sk/product/19011","NG125 - chráničová spúšť - Vigi NG125 - 2P - 63A - 30mA",0.04]
["19010","BLOK VIGI NG125 2P 63A 30MA A",1,"ks",{"v":220.49999999999994,"d":"220.500"},"3303430190103",{"v":14.5,"d":"14.50"},{"v":10,"d":"10.00"},{"v":15.5,"d":"15.50"},{"v":331,"d":"331.00"},"FR","8536209090","https://www.se.com/sk/sk/product/19010","NG125 - chráničová spúšť - Vigi NG125 - 2P - 63A - 30mA",0.04]
["19009","CHRÁN SPÚŠŤ VIGING125 2P 63A 300MA",1,"ks",{"v":299.87999999999994,"d":"299.880"},"3303430190097",{"v":15,"d":"15.00"},{"v":9,"d":"9.00"},{"v":14.5,"d":"14.50"},{"v":327,"d":"327.00"},"FR","85363030","https://www.se.com/sk/sk/product/19009","NG125 - chráničová spúšť - Vigi NG125 - 2P - 63A - 300mA",0.04]
["19008","CHRÁN SPÚŠŤ VIGING125 2P 63A 30MA",1,"ks",{"v":317.5199999999999,"d":"317.520"},"3303430190080",{"v":16,"d":"16.00"},{"v":9.5,"d":"9.50"},{"v":14.5,"d":"14.50"},{"v":330,"d":"330.00"},"FR","8536209090","https://www.se.com/sk/sk/product/19008","NG125 - chráničová spúšť - Vigi NG125 - 2P - 63A - 30mA",0]
["19005","BLOK VIGI NG125 3P 63A 300MA",1,"ks",{"v":282.23999999999995,"d":"282.240"},"3303430190059",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":13.5,"d":"13.50"},{"v":519,"d":"519.00"},"FR","8536209090","https://www.se.com/sk/sk/product/19005","NG125 - chráničová spúšť- Vigi NG125 - 4P - 63A - 300mA",0.06]
["19004","BLOK VIGI NG125 4P 63A 30MA",1,"ks",{"v":313.10999999999996,"d":"313.110"},"3303430190042",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":13.5,"d":"13.50"},{"v":541,"d":"541.00"},"FR","8536303099","https://www.se.com/sk/sk/product/19004","NG125 - chráničová spúšť - Vigi NG125 - 4P - 63A - 30mA",0.07]
["19003","BLOK VIGI NG125 3P 63A 300MA",1,"ks",{"v":255.77999999999994,"d":"255.780"},"3303430190035",{"v":25.3,"d":"25.30"},{"v":9.5,"d":"9.50"},{"v":13.5,"d":"13.50"},{"v":480,"d":"480.00"},"FR","85363030","https://www.se.com/sk/sk/product/19003","NG125 - chráničová spúšť- Vigi NG125 - 3P - 63A - 300mA",0.06]
["19002","VIGI NG125 3P 63A 30MA AC",1,"ks",{"v":282.23999999999995,"d":"282.240"},"3303430190028",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":13.5,"d":"13.50"},{"v":502,"d":"502.00"},"FR","85363030","https://www.se.com/sk/sk/product/19002","NG125 - chráničová spúšť - Vigi NG125 - 3P - 63A - 30mA",0.06]
["19001","BLOK VIGI NG125 2P 63A 300MA",1,"ks",{"v":180.80999999999997,"d":"180.810"},"3303430190011",{"v":14,"d":"14.00"},{"v":9.6,"d":"9.60"},{"v":13.6,"d":"13.60"},{"v":308,"d":"308.00"},"FR","85363030","https://www.se.com/sk/sk/product/19001","NG125 - chráničová spúšť - Vigi NG125 - 2P - 63A - 300mA",0.04]
["19000","BLOK VIGI NG125 2P 63A 30MA",1,"ks",{"v":202.85999999999996,"d":"202.860"},"3303430190004",{"v":13.8,"d":"13.80"},{"v":9.4,"d":"9.40"},{"v":13.8,"d":"13.80"},{"v":316,"d":"316.00"},"FR","85363030","https://www.se.com/sk/sk/product/19000","NG125 - chráničová spúšť - Vigi NG125 - 2P - 63A - 30mA",0.04]
["18891","ODPÍNAČ NG125NA 3P 100A",1,"ks",{"v":493.91999999999996,"d":"493.920"},"3303430188919",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":779,"d":"779.00"},"FR","8536508090","https://www.se.com/sk/sk/product/18891","odpínač NG125NA - 3P - 100 A",0.09]
["18887","ISTIČ NG125L 3P 80A MA",1,"ks",{"v":926.0999999999998,"d":"926.100"},"3303430188872",{"v":13,"d":"13.00"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":788,"d":"788.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18887","NG125 - istič - NG125LMA - 3P - 80A - char. MA",0.1]
["18886","ISTIČ NG125LMA 63 A 3P",1,"ks",{"v":829.0799999999999,"d":"829.080"},"3303430188865",{"v":12.5,"d":"12.50"},{"v":8.5,"d":"8.50"},{"v":12,"d":"12.00"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18886","Miniature circuit breaker (MCB), Acti9 NG125LMA, 3P, 63A, MA curve, 50kA (IEC/EN 60947-2)",0.09]
["18884","ISTIČ NG125LMA 25 A 3P",1,"ks",{"v":926.0999999999998,"d":"926.100"},"3303430188841",{"v":13,"d":"13.00"},{"v":8.5,"d":"8.50"},{"v":12,"d":"12.00"},{"v":737,"d":"737.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18884","NG125 - istič - NG125LMA - 3P - 25A - char. MA",0.09]
["18883","ISTIČ NG125LMA 16 A 3P",1,"ks",{"v":970.1999999999998,"d":"970.200"},"3303430188834",{"v":12.9,"d":"12.90"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":750,"d":"750.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18883","Miniature circuit breaker (MCB), Acti9 NG125LMA, 3P, 16A, MA curve, 50kA (IEC/EN 60947-2)",0.09]
["18880","ISTIČ NG125LMA 6.3A 3P",1,"ks",{"v":1058.3999999999999,"d":"1058.400"},"3303430188803",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":738,"d":"738.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18880","Miniature circuit breaker (MCB), Acti9 NG125LMA, 3P, 6.3A, MA curve, 50kA (IEC/EN 60947-2)",0.09]
["18870","ISTIČ NG125LMA 2P 10A",1,"ks",{"v":1014.2999999999998,"d":"1014.300"},"3303430188704",{"v":11,"d":"11.00"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":485,"d":"485.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18870","Miniature circuit breaker (MCB), Acti9 NG125LMA, 2P, 10A, MA curve, 50kA (IEC/EN 60947-2)",0.06]
["18865","ISTIČ NG125L 4P 80A D",1,"ks",{"v":842.31,"d":"842.310"},"3303430188650",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1053,"d":"1,053.00"},"FR","85362090","https://www.se.com/sk/sk/product/18865","NG125 - istič - NG125L - 4P - 80A - char. D",0.13]
["18864","ISTIČ NG125L 4P 63A D",1,"ks",{"v":762.93,"d":"762.930"},"3303430188643",{"v":15.5,"d":"15.50"},{"v":8.2,"d":"8.20"},{"v":12,"d":"12.00"},{"v":986,"d":"986.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18864","NG125 - istič - NG125L - 4P - 63A - char. D",0.12]
["18863","ISTIČ NG125L 4P 50A D",1,"ks",{"v":789.3899999999999,"d":"789.390"},"3303430188636",{"v":15.2,"d":"15.20"},{"v":8.5,"d":"8.50"},{"v":12.4,"d":"12.40"},{"v":999,"d":"999.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18863","NG125 - istič - NG125L - 4P - 50A - char. D",0.12]
["18862","ISTIČ NG125L 4P 40A D",1,"ks",{"v":807.03,"d":"807.030"},"3303430188629",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":997,"d":"997.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18862","NG125 - istič - NG125L - 4P - 40A - char. D",0.12]
["18861","ISTIČ NG125L 4P 32A D",1,"ks",{"v":824.6699999999998,"d":"824.670"},"3303430188612",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":976,"d":"976.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18861","NG125 - istič - NG125L - 4P - 32A - char. D",0.12]
["18860","ISTIČ NG125L 4P 25A D",1,"ks",{"v":842.31,"d":"842.310"},"3303430188605",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":991,"d":"991.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18860","NG125 - istič - NG125L - 4P - 25A - char. D",0.12]
["18859","ISTIČ NG125L 4P 20A D",1,"ks",{"v":868.7699999999999,"d":"868.770"},"3303430188599",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":999.9,"d":"999.90"},"FR","8536201090","https://www.se.com/sk/sk/product/18859","NG125 - istič - NG125L - 4P - 20A - char. D",0.12]
["18858","ISTIČ NG125L 4P 16A D",1,"ks",{"v":926.0999999999998,"d":"926.100"},"3303430188582",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":981,"d":"981.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18858","NG125 - istič - NG125L - 4P - 16A - char. D",0.12]
["18857","ISTIČ NG125L 4P 10A D",1,"ks",{"v":970.1999999999998,"d":"970.200"},"3303430188575",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":986,"d":"986.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18857","NG125 - istič - NG125L - 4P - 10A - char. D",0.12]
["18856","ISTIČ NG125L 3P 80A D",1,"ks",{"v":617.3999999999999,"d":"617.400"},"3303430188568",{"v":12.9,"d":"12.90"},{"v":8.8,"d":"8.80"},{"v":12.4,"d":"12.40"},{"v":800,"d":"800.00"},"FR","85362090","https://www.se.com/sk/sk/product/18856","NG125 - istič - NG125L - 3P - 80A - char. D",0.1]
["18855","ISTIČ NG125L 3P 63A D",1,"ks",{"v":560.0699999999999,"d":"560.070"},"3303430188551",{"v":12.9,"d":"12.90"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18855","NG125 - istič - NG125L - 3P - 63A - char. D",0.09]
["18854","ISTIČ NG125L 3P 50A D",1,"ks",{"v":582.1199999999999,"d":"582.120"},"3303430188544",{"v":12.9,"d":"12.90"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":747,"d":"747.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18854","NG125 - istič - NG125L - 3P - 50A - char. D",0.09]
["18853","ISTIČ NG125L 3P 40A D",1,"ks",{"v":590.9399999999999,"d":"590.940"},"3303430188537",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18853","NG125 - istič - NG125L - 3P - 40A - char. D",0.09]
["18852","ISTIČ NG125L 3P 32A D",1,"ks",{"v":604.17,"d":"604.170"},"3303430188520",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":744,"d":"744.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18852","NG125 - istič - NG125L - 3P - 32A - char. D",0.09]
["18851","ISTIČ NG125L 3P 25A D",1,"ks",{"v":617.3999999999999,"d":"617.400"},"3303430188513",{"v":12.9,"d":"12.90"},{"v":8.8,"d":"8.80"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18851","NG125 - istič - NG125L - 3P - 25A - char. D",0.09]
["18850","ISTIČ NG125L 3P 20A D",1,"ks",{"v":639.4499999999999,"d":"639.450"},"3303430188506",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":743,"d":"743.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18850","NG125 - istič - NG125L - 3P - 20A - char. D",0.09]
["18849","ISTIČ NG125L 3P 16A D",1,"ks",{"v":665.9099999999999,"d":"665.910"},"3303430188490",{"v":13,"d":"13.00"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":753,"d":"753.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18849","NG125 - istič - NG125L - 3P - 16A - char. D",0.09]
["18848","ISTIČ NG125L 3P 10A D",1,"ks",{"v":696.78,"d":"696.780"},"3303430188483",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":752,"d":"752.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18848","NG125 - istič - NG125L - 3P - 10A - char. D",0.09]
["18847","ISTIČ NG125L 2P 80A D",1,"ks",{"v":524.79,"d":"524.790"},"3303430188476",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":501,"d":"501.00"},"FR","85362090","https://www.se.com/sk/sk/product/18847","NG125 - istič - NG125L - 2P - 80A - char. D",0.06]
["18846","ISTIČ NG125L 2P 63A D",1,"ks",{"v":485.0999999999999,"d":"485.100"},"3303430188469",{"v":10.9,"d":"10.90"},{"v":5.5,"d":"5.50"},{"v":8,"d":"8.00"},{"v":484,"d":"484.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18846","NG125 - istič - NG125L - 2P - 63A - char. D",0.06]
["18845","ISTIČ NG125L 2P 50A D",1,"ks",{"v":498.3299999999999,"d":"498.330"},"3303430188452",{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},{"v":5.6,"d":"5.60"},{"v":480,"d":"480.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18845","NG125 - istič - NG125L - 2P - 50A - char. D",0.06]
["18844","ISTIČ NG125L 2P 40A D",1,"ks",{"v":511.5599999999999,"d":"511.560"},"3303430188445",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":478,"d":"478.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18844","NG125 - istič - NG125L - 2P - 40A - char. D",0.06]
["18843","ISTIČ NG125L 2P 32A D",1,"ks",{"v":524.79,"d":"524.790"},"3303430188438",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":478,"d":"478.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18843","NG125 - istič - NG125L - 2P - 32A - char. D",0.06]
["18842","ISTIČ NG125L 2P 25A D",1,"ks",{"v":401.30999999999995,"d":"401.310"},"3303430188421",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":477,"d":"477.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18842","NG125 - istič - NG125L - 2P - 25A - char. D",0.06]
["18841","ISTIČ NG125L 2P 20A D",1,"ks",{"v":555.66,"d":"555.660"},"3303430188414",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":478,"d":"478.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18841","NG125 - istič - NG125L - 2P - 20A - char. D",0.06]
["18840","ISTIČ NG125L 2P 16A D",1,"ks",{"v":432.17999999999995,"d":"432.180"},"3303430188407",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":478,"d":"478.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18840","NG125 - istič - NG125L - 2P - 16A - char. D",0.06]
["18839","ISTIČ NG125L 2P 10A D",1,"ks",{"v":454.22999999999996,"d":"454.230"},"3303430188391",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":471,"d":"471.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18839","NG125 - istič - NG125L - 2P - 10A - char. D",0.06]
["18835","ISTIČ NG125L 1P 40A D",1,"ks",{"v":246.95999999999998,"d":"246.960"},"3303430188353",{"v":10.9,"d":"10.90"},{"v":3.2,"d":"3.20"},{"v":8.3,"d":"8.30"},{"v":244,"d":"244.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18835","NG125 - istič - NG125L - 1P - 40A - char. D",0.03]
["18831","ISTIČ NG125L 1P 16A D",1,"ks",{"v":246.95999999999998,"d":"246.960"},"3303430188315",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":246,"d":"246.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18831","NG125 - istič - NG125L - 1P - 16A - char. D",0.03]
["18829","ISTIČ NG125L 4P 80A C",1,"ks",{"v":732.06,"d":"732.060"},"3303430188292",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1044,"d":"1,044.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18829","Miniature circuit breaker (MCB), Acti9 NG125L, 4P, 80A, C curve, 50kA (IEC/EN 60947-2)",0.13]
["18828","ISTIČ NG125L 4P 63A C",1,"ks",{"v":661.4999999999999,"d":"661.500"},"3303430188285",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},0.96,"FR","8536209090","https://www.se.com/sk/sk/product/18828","Miniature circuit breaker (MCB), Acti9 NG125L, 4P, 63A, C curve, 50kA (IEC/EN 60947-2)",0.12]
["18827","ISTIČ NG125L 4P 50A C",1,"ks",{"v":687.9599999999999,"d":"687.960"},"3303430188278",{"v":15.6,"d":"15.60"},{"v":8.3,"d":"8.30"},{"v":12,"d":"12.00"},{"v":986,"d":"986.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18827","Miniature circuit breaker (MCB), Acti9 NG125L, 4P, 50A, C curve, 50kA (IEC/EN 60947-2)",0.12]
["18826","ISTIČ NG125L 4P 40A C",1,"ks",{"v":701.1899999999998,"d":"701.190"},"3303430188261",{"v":15.8,"d":"15.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":985,"d":"985.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18826","Miniature circuit breaker (MCB), Acti9 NG125L, 4P, 40A, C curve, 50kA (IEC/EN 60947-2)",0.12]
["18825","ISTIČ NG125L 4P 32A C",1,"ks",{"v":718.8299999999999,"d":"718.830"},"3303430188254",{"v":15.7,"d":"15.70"},{"v":8.3,"d":"8.30"},{"v":12.3,"d":"12.30"},{"v":994,"d":"994.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18825","Miniature circuit breaker (MCB), Acti9 NG125L, 4P, 32A, C curve, 50kA (IEC/EN 60947-2)",0.12]
["18823","ISTIČ NG125L 4P 20A C",1,"ks",{"v":859.9499999999999,"d":"859.950"},"3303430188230",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":994,"d":"994.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18823","Miniature circuit breaker (MCB), Acti9 NG125L, 4P, 20A, C curve, 50kA (IEC/EN 60947-2)",0]
["18821","ISTIČ NG125L 4P 10A C",1,"ks",{"v":824.6699999999998,"d":"824.670"},"3303430188216",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":967,"d":"967.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18821","Miniature circuit breaker (MCB), Acti9 NG125L, 4P, 10A, C curve, 50kA (IEC/EN 60947-2)",0.12]
["18818","ISTIČ NG125L 4P 80A C",1,"ks",{"v":732.06,"d":"732.060"},"3303430188186",{"v":16.8,"d":"16.80"},{"v":8.4,"d":"8.40"},{"v":13.4,"d":"13.40"},{"v":1028,"d":"1,028.00"},"FR","85362090","https://www.se.com/sk/sk/product/18818","NG125 - istič - NG125L - 4P - 80A - char. C",0.12]
["18817","ISTIČ NG125L 4P 63A C",1,"ks",{"v":661.4999999999999,"d":"661.500"},"3303430188179",{"v":15.4,"d":"15.40"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":987,"d":"987.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18817","NG125 - istič - NG125L - 4P - 63A - char. C",0.12]
["18816","ISTIČ NG125L 4P 50A C",1,"ks",{"v":687.9599999999999,"d":"687.960"},"3303430188162",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":997,"d":"997.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18816","NG125 - istič - NG125L - 4P - 50A - char. C",0.12]
["18815","ISTIČ NG125L 4P 40A C",1,"ks",{"v":701.1899999999998,"d":"701.190"},"3303430188155",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.6,"d":"12.60"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18815","NG125 - istič - NG125L - 4P - 40A - char. C",0.12]
["18814","ISTIČ NG125L 4P 32A C",1,"ks",{"v":718.8299999999999,"d":"718.830"},"3303430188148",{"v":15.7,"d":"15.70"},{"v":8.2,"d":"8.20"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18814","NG125 - istič - NG125L - 4P - 32A - char. C",0.12]
["18813","ISTIČ NG125L 4P 25A C",1,"ks",{"v":732.06,"d":"732.060"},"3303430188131",{"v":15.5,"d":"15.50"},{"v":8.4,"d":"8.40"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18813","NG125 - istič - NG125L - 4P - 25A - char. C",0.12]
["18812","ISTIČ NG125L 4P 20A C",1,"ks",{"v":754.1099999999999,"d":"754.110"},"3303430188124",{"v":15.4,"d":"15.40"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1002,"d":"1,002.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18812","NG125 - istič - NG125L - 4P - 20A - char. C",0.12]
["18811","ISTIČ NG125L 4P 16A C",1,"ks",{"v":784.9799999999999,"d":"784.980"},"3303430188117",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":990,"d":"990.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18811","NG125 - istič - NG125L - 4P - 16A - char. C",0.12]
["18810","ISTIČ NG125L 4P 10A C",1,"ks",{"v":824.6699999999998,"d":"824.670"},"3303430188100",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18810","NG125 - istič - NG125L - 4P - 10A - char. C",0.12]
["18807","ISTIČ NG125L 3P 80A C",1,"ks",{"v":538.02,"d":"538.020"},"3303430188070",{"v":12.7,"d":"12.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18807","NG125 - istič - NG125L - 3P - 80A - char. C",0.09]
["18806","ISTIČ NG125L 3P 63A C",1,"ks",{"v":489.50999999999993,"d":"489.510"},"3303430188063",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":761,"d":"761.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18806","NG125 - istič - NG125L - 3P - 63A - char. C",0.09]
["18805","ISTIČ NG125L 3P 50A C",1,"ks",{"v":502.73999999999995,"d":"502.740"},"3303430188056",{"v":12.5,"d":"12.50"},{"v":8.3,"d":"8.30"},{"v":12,"d":"12.00"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18805","NG125 - istič - NG125L - 3P - 50A - char. C",0.09]
["18804","ISTIČ NG125L 3P 40A C",1,"ks",{"v":515.9699999999999,"d":"515.970"},"3303430188049",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":761,"d":"761.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18804","NG125 - istič - NG125L - 3P - 40A - char. C",0.09]
["18803","ISTIČ NG125L 3P 32A C",1,"ks",{"v":529.1999999999999,"d":"529.200"},"3303430188032",{"v":12.7,"d":"12.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18803","NG125 - istič - NG125L - 3P - 32A - char. C",0.09]
["18802","ISTIČ NG125L 3P 25A C",1,"ks",{"v":538.02,"d":"538.020"},"3303430188025",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":741,"d":"741.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18802","NG125 - istič - NG125L - 3P - 25A - char. C",0.09]
["18801","ISTIČ NG125L 3P 20A C",1,"ks",{"v":555.66,"d":"555.660"},"3303430188018",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":762,"d":"762.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18801","NG125 - istič - NG125L - 3P - 20A - char. C",0.09]
["18800","ISTIČ NG125L 3P 16A C",1,"ks",{"v":577.7099999999999,"d":"577.710"},"3303430188001",{"v":12.9,"d":"12.90"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":756,"d":"756.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18800","NG125 - istič - NG125L - 3P - 16A - char. C",0.09]
["18799","ISTIČ NG125L 3P 10A C",1,"ks",{"v":608.5799999999999,"d":"608.580"},"3303430187998",{"v":12.9,"d":"12.90"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":734,"d":"734.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18799","NG125 - istič - NG125L - 3P - 10A - char. C",0.09]
["18796","ISTIČ NG125L 2P 80A C",1,"ks",{"v":476.28,"d":"476.280"},"3303430187967",{"v":11.1,"d":"11.10"},{"v":5.8,"d":"5.80"},{"v":8.6,"d":"8.60"},{"v":502,"d":"502.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18796","NG125 - istič - NG125L - 2P - 80A - char. C",0.06]
["18795","ISTIČ NG125L 2P 63A C",1,"ks",{"v":440.9999999999999,"d":"441.000"},"3303430187950",{"v":10.9,"d":"10.90"},{"v":5.8,"d":"5.80"},{"v":8.3,"d":"8.30"},{"v":480,"d":"480.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18795","NG125 - istič - NG125L - 2P - 63A - char. C",0.06]
["18794","ISTIČ NG125L 2P 50A C",1,"ks",{"v":326.34,"d":"326.340"},"3303430187943",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":480,"d":"480.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18794","NG125 - istič - NG125L - 2P - 50A - char. C",0.06]
["18793","ISTIČ NG125L 2P 40A C",1,"ks",{"v":335.15999999999997,"d":"335.160"},"3303430187936",{"v":10.8,"d":"10.80"},{"v":8.3,"d":"8.30"},{"v":5.5,"d":"5.50"},{"v":476,"d":"476.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18793","NG125 - istič - NG125L - 2P - 40A - char. C",0.06]
["18792","ISTIČ NG125L 2P 32A C",1,"ks",{"v":343.97999999999996,"d":"343.980"},"3303430187929",{"v":10.7,"d":"10.70"},{"v":5.6,"d":"5.60"},{"v":8,"d":"8.00"},{"v":471,"d":"471.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18792","NG125 - istič - NG125L - 2P - 32A - char. C",0.06]
["18791","ISTIČ NG125L 2P 25A C",1,"ks",{"v":348.39,"d":"348.390"},"3303430187912",{"v":11.1,"d":"11.10"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":477,"d":"477.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18791","NG125 - istič - NG125L - 2P - 25A - char. C",0.06]
["18790","ISTIČ NG125L 2P 20A C",1,"ks",{"v":361.61999999999995,"d":"361.620"},"3303430187905",{"v":10.8,"d":"10.80"},{"v":5.8,"d":"5.80"},{"v":8.3,"d":"8.30"},{"v":475,"d":"475.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18790","NG125 - istič - NG125L - 2P - 20A - char. C",0.06]
["18789","ISTIČ NG125L 2P 16A C",1,"ks",{"v":374.84999999999997,"d":"374.850"},"3303430187899",{"v":11,"d":"11.00"},{"v":5.8,"d":"5.80"},{"v":8.3,"d":"8.30"},{"v":478,"d":"478.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18789","NG125 - istič - NG125L - 2P - 16A - char. C",0.06]
["18788","ISTIČ NG125L 2P 10A C",1,"ks",{"v":392.48999999999995,"d":"392.490"},"3303430187882",{"v":11.2,"d":"11.20"},{"v":5.6,"d":"5.60"},{"v":7.8,"d":"7.80"},{"v":466,"d":"466.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18788","NG125 - istič - NG125L - 2P - 10A - char. C",0.06]
["18785","ISTIČ NG125L 1P 80A C",1,"ks",{"v":202.85999999999996,"d":"202.860"},"3303430187851",{"v":10.8,"d":"10.80"},{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":257,"d":"257.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18785","NG125 - istič - NG125L - 1P - 80A - char. C",0.03]
["18784","ISTIČ NG125L 1P 63A C",1,"ks",{"v":189.62999999999997,"d":"189.630"},"3303430187844",{"v":11,"d":"11.00"},{"v":8.2,"d":"8.20"},{"v":3,"d":"3.00"},{"v":248,"d":"248.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18784","NG125 - istič - NG125L - 1P - 63A - char. C",0.03]
["18783","ISTIČ NG125L 1P 50A C",1,"ks",{"v":194.03999999999996,"d":"194.040"},"3303430187837",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.2,"d":"8.20"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18783","NG125 - istič - NG125L - 1P - 50A - char. C",0.03]
["18782","ISTIČ NG125L 1P 40A C",1,"ks",{"v":145.52999999999997,"d":"145.530"},"3303430187820",{"v":10.7,"d":"10.70"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":247,"d":"247.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18782","NG125 - istič - NG125L - 1P - 40A - char. C",0.03]
["18781","ISTIČ NG125L 1P 32A C",1,"ks",{"v":145.52999999999997,"d":"145.530"},"3303430187813",{"v":10.8,"d":"10.80"},{"v":2.8,"d":"2.80"},{"v":8,"d":"8.00"},{"v":242,"d":"242.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18781","NG125 - istič - NG125L - 1P - 32A - char. C",0.03]
["18780","ISTIČ NG125L 1P 25A C",1,"ks",{"v":207.26999999999998,"d":"207.270"},"3303430187806",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.3,"d":"8.30"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18780","NG125 - istič - NG125L - 1P - 25A - char. C",0.03]
["18779","ISTIČ NG125L 1P 20A C",1,"ks",{"v":211.67999999999995,"d":"211.680"},"3303430187790",{"v":11,"d":"11.00"},{"v":3.2,"d":"3.20"},{"v":8.1,"d":"8.10"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18779","NG125 - istič - NG125L - 1P - 20A - char. C",0.03]
["18778","ISTIČ NG125L 1P 16A C",1,"ks",{"v":163.17,"d":"163.170"},"3303430187783",{"v":10.8,"d":"10.80"},{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18778","NG125 - istič - NG125L - 1P - 16A - char. C",0.03]
["18777","ISTIČ NG125L 1P 10A C",1,"ks",{"v":171.98999999999998,"d":"171.990"},"3303430187776",{"v":10.8,"d":"10.80"},{"v":2.8,"d":"2.80"},{"v":8,"d":"8.00"},{"v":239,"d":"239.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18777","NG125 - istič - NG125L - 1P - 10A - char. C",0.03]
["18776","ISTIČ NG125L 4P 80A B",1,"ks",{"v":970.1999999999998,"d":"970.200"},"3303430187769",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1056,"d":"1,056.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18776","NG125 - istič - NG125L - 4P - 80A - char. B",0.13]
["18775","ISTIČ NG125L 4P 63A B",1,"ks",{"v":696.78,"d":"696.780"},"3303430187752",{"v":15.4,"d":"15.40"},{"v":8.3,"d":"8.30"},{"v":12.2,"d":"12.20"},{"v":1008.9999999999999,"d":"1,009.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18775","NG125 - istič - NG125L - 4P - 63A - char. B",0.12]
["18774","ISTIČ NG125L 4P 50A B",1,"ks",{"v":718.8299999999999,"d":"718.830"},"3303430187745",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":1040,"d":"1,040.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18774","NG125 - istič - NG125L - 4P - 50A - char. B",0.12]
["18773","ISTIČ NG125L 4P 40A B",1,"ks",{"v":736.4699999999999,"d":"736.470"},"3303430187738",{"v":15.8,"d":"15.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1000.9999999999999,"d":"1,001.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18773","NG125 - istič - NG125L - 4P - 40A - char. B",0.12]
["18772","ISTIČ NG125L 4P 32A B",1,"ks",{"v":754.1099999999999,"d":"754.110"},"3303430187721",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":999,"d":"999.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18772","NG125 - istič - NG125L - 4P - 32A - char. B",0.12]
["18771","ISTIČ NG125L 4P 25A B",1,"ks",{"v":767.3399999999999,"d":"767.340"},"3303430187714",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1000.9999999999999,"d":"1,001.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18771","NG125 - istič - NG125L - 4P - 25A - char. B",0.12]
["18770","ISTIČ NG125L 4P 20A B",1,"ks",{"v":1014.2999999999998,"d":"1014.300"},"3303430187707",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":999,"d":"999.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18770","NG125 - istič - NG125L - 4P - 20A - char. B",0.12]
["18769","ISTIČ NG125L 4P 16A B",1,"ks",{"v":824.6699999999998,"d":"824.670"},"3303430187691",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":998,"d":"998.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18769","NG125 - istič - NG125L - 4P - 16A - char. B",0.12]
["18768","ISTIČ NG125L 4P 10A B",1,"ks",{"v":864.3599999999999,"d":"864.360"},"3303430187684",{"v":15.8,"d":"15.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":986,"d":"986.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18768","NG125 - istič - NG125L - 4P - 10A - char. B",0.12]
["18767","ISTIČ NG125L 3P 80A B",1,"ks",{"v":564.4799999999999,"d":"564.480"},"3303430187677",{"v":13,"d":"13.00"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":801,"d":"801.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18767","NG125 - istič - NG125L - 3P - 80A - char. B",0.1]
["18766","ISTIČ NG125L 3P 63A B",1,"ks",{"v":511.5599999999999,"d":"511.560"},"3303430187660",{"v":12.5,"d":"12.50"},{"v":8.2,"d":"8.20"},{"v":12,"d":"12.00"},{"v":749,"d":"749.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18766","NG125 - istič - NG125L - 3P - 63A - char. B",0.09]
["18765","ISTIČ NG125L 3P 50A B",1,"ks",{"v":529.1999999999999,"d":"529.200"},"3303430187653",{"v":12.7,"d":"12.70"},{"v":8.3,"d":"8.30"},{"v":12,"d":"12.00"},{"v":759,"d":"759.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18765","NG125 - istič - NG125L - 3P - 50A - char. B",0.09]
["18764","ISTIČ NG125L 3P 40A B",1,"ks",{"v":542.43,"d":"542.430"},"3303430187646",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":757,"d":"757.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18764","NG125 - istič - NG125L - 3P - 40A - char. B",0.09]
["18763","ISTIČ NG125L 3P 32A B",1,"ks",{"v":551.2499999999999,"d":"551.250"},"3303430187639",{"v":13.1,"d":"13.10"},{"v":8.1,"d":"8.10"},{"v":12.1,"d":"12.10"},{"v":756,"d":"756.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18763","NG125 - istič - NG125L - 3P - 32A - char. B",0.09]
["18762","ISTIČ NG125L 3P 25A B",1,"ks",{"v":564.4799999999999,"d":"564.480"},"3303430187622",{"v":13.2,"d":"13.20"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":758,"d":"758.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18762","NG125 - istič - NG125L - 3P - 25A - char. B",0.09]
["18761","ISTIČ NG125L 3P 20A B",1,"ks",{"v":582.1199999999999,"d":"582.120"},"3303430187615",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":758,"d":"758.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18761","NG125 - istič - NG125L - 3P - 20A - char. B",0.09]
["18760","ISTIČ NG125L 3P 16A B",1,"ks",{"v":608.5799999999999,"d":"608.580"},"3303430187608",{"v":12.5,"d":"12.50"},{"v":8.3,"d":"8.30"},{"v":12.1,"d":"12.10"},{"v":761,"d":"761.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18760","NG125 - istič - NG125L - 3P - 16A - char. B",0.09]
["18759","ISTIČ NG125L 3P 10A B",1,"ks",{"v":635.0399999999998,"d":"635.040"},"3303430187592",{"v":13,"d":"13.00"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":734,"d":"734.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18759","NG125 - istič - NG125L - 3P - 10A - char. B",0.09]
["18758","ISTIČ NG125L 2P 80A B",1,"ks",{"v":551.2499999999999,"d":"551.250"},"3303430187585",{"v":10.8,"d":"10.80"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":500,"d":"500.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18758","NG125 - istič - NG125L - 2P - 80A - char. B",0.06]
["18757","ISTIČ NG125L 2P 63A B",1,"ks",{"v":498.3299999999999,"d":"498.330"},"3303430187578",{"v":11,"d":"11.00"},{"v":5.6,"d":"5.60"},{"v":8,"d":"8.00"},{"v":479,"d":"479.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18757","NG125 - istič - NG125L - 2P - 63A - char. B",0.06]
["18756","ISTIČ NG125L 2P 50A B",1,"ks",{"v":432.17999999999995,"d":"432.180"},"3303430187561",{"v":11,"d":"11.00"},{"v":5.5,"d":"5.50"},{"v":8,"d":"8.00"},{"v":479,"d":"479.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18756","NG125 - istič - NG125L - 2P - 50A - char. B",0.06]
["18755","ISTIČ NG125L 2P 40A B",1,"ks",{"v":529.1999999999999,"d":"529.200"},"3303430187554",{"v":11.1,"d":"11.10"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":480,"d":"480.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18755","NG125 - istič - NG125L - 2P - 40A - char. B",0.06]
["18754","ISTIČ NG125L 2P 32A B",1,"ks",{"v":458.64,"d":"458.640"},"3303430187547",{"v":10.8,"d":"10.80"},{"v":5.8,"d":"5.80"},{"v":8.3,"d":"8.30"},{"v":476,"d":"476.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18754","NG125 - istič - NG125L - 2P - 32A - char. B",0.06]
["18753","ISTIČ NG125L 2P 25A B",1,"ks",{"v":467.4599999999999,"d":"467.460"},"3303430187530",{"v":11,"d":"11.00"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":476,"d":"476.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18753","NG125 - istič - NG125L - 2P - 25A - char. B",0.06]
["18752","ISTIČ NG125L 2P 20A B",1,"ks",{"v":507.1499999999999,"d":"507.150"},"3303430187523",{"v":10.8,"d":"10.80"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":477,"d":"477.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18752","NG125 - istič - NG125L - 2P - 20A - char. B",0.06]
["18751","ISTIČ NG125L 2P 16A B",1,"ks",{"v":392.48999999999995,"d":"392.490"},"3303430187516",{"v":10.8,"d":"10.80"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":477,"d":"477.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18751","NG125 - istič - NG125L - 2P - 16A - char. B",0.06]
["18750","ISTIČ NG125L 2P 10A B",1,"ks",{"v":414.53999999999996,"d":"414.540"},"3303430187509",{"v":10.8,"d":"10.80"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":471,"d":"471.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18750","NG125 -istič - NG125L - 2P - 10A - char. B",0.06]
["18749","ISTIČ NG125L 1P 80A B",1,"ks",{"v":238.14,"d":"238.140"},"3303430187493",{"v":10.8,"d":"10.80"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":257,"d":"257.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18749","NG125 - istič - NG125L - 1P - 80A - char. B",0.03]
["18748","ISTIČ NG125L 1P 63A B",1,"ks",{"v":216.08999999999997,"d":"216.090"},"3303430187486",{"v":10.8,"d":"10.80"},{"v":3.2,"d":"3.20"},{"v":8.1,"d":"8.10"},{"v":248,"d":"248.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18748","NG125 - istič - NG125L - 1P - 63A - char. B",0.03]
["18747","ISTIČ NG125L 1P 50A B",1,"ks",{"v":202.85999999999996,"d":"202.860"},"3303430187479",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":246,"d":"246.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18747","NG125 - istič - NG125L - 1P - 50A - char. B",0.03]
["18746","ISTIČ NG125L 1P 40A B",1,"ks",{"v":189.62999999999997,"d":"189.630"},"3303430187462",{"v":11.1,"d":"11.10"},{"v":3,"d":"3.00"},{"v":8.3,"d":"8.30"},{"v":232,"d":"232.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18746","NG125 - istič - NG125L - 1P - 40A - char. B",0.03]
["18745","ISTIČ NG125L 1P 32A B",1,"ks",{"v":194.03999999999996,"d":"194.040"},"3303430187455",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":244,"d":"244.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18745","NG125 - istič - NG125L - 1P - 32A - char. B",0.03]
["18744","ISTIČ NG125L 1P 25A B",1,"ks",{"v":238.14,"d":"238.140"},"3303430187448",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":245,"d":"245.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18744","NG125 - istič - NG125L - 1P - 25A - char. B",0.03]
["18743","ISTIČ NG125L 1P 20A B",1,"ks",{"v":246.95999999999998,"d":"246.960"},"3303430187431",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":244,"d":"244.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18743","NG125 - istič - NG125L - 1P - 20A - char. B",0.03]
["18742","ISTIČ NG125L 1P 16A B",1,"ks",{"v":171.98999999999998,"d":"171.990"},"3303430187424",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":246,"d":"246.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18742","NG125 - istič - NG125L - 1P - 16A - char. B",0.03]
["18741","ISTIČ NG125L 1P 10A B",1,"ks",{"v":176.39999999999998,"d":"176.400"},"3303430187417",{"v":10.9,"d":"10.90"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":244,"d":"244.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18741","NG125 - istič - NG125L - 1P - 10A - char. B",0.03]
["18740","ISTIČ NG125H 4P 80A C",1,"ks",{"v":604.17,"d":"604.170"},"3303430187400",{"v":16,"d":"16.00"},{"v":8,"d":"8.00"},{"v":12,"d":"12.00"},{"v":1044,"d":"1,044.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18740","NG125 - istič - NG125H - 4P - 80A - char. C",0.13]
["18739","NG125H 4P 63A C",1,"ks",{"v":546.8399999999999,"d":"546.840"},"3303430187394",{"v":15.4,"d":"15.40"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":990,"d":"990.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18739","NG125 - istič - NG125H - 4P - 63A - char. C",0.12]
["18738","ISTIČ NG125H 4P 50A C",1,"ks",{"v":568.89,"d":"568.890"},"3303430187387",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1000,"d":"1,000.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18738","NG125 - istič - NG125H - 4P - 50A - char. C",0.12]
["18737","ISTIČ NG125H 4P 40A C",1,"ks",{"v":582.1199999999999,"d":"582.120"},"3303430187370",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":737,"d":"737.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18737","NG125 - istič - NG125H - 4P - 40A - char. C",0.12]
["18736","ISTIČ NG125H 4P 32A C",1,"ks",{"v":595.3499999999999,"d":"595.350"},"3303430187363",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":979,"d":"979.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18736","NG125 - istič - NG125H - 4P - 32A - char. C",0.12]
["18735","ISTIČ NG125H 4P 25A C",1,"ks",{"v":604.17,"d":"604.170"},"3303430187356",{"v":15.4,"d":"15.40"},{"v":8.4,"d":"8.40"},{"v":12.2,"d":"12.20"},{"v":991,"d":"991.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18735","Miniature circuit breaker (MCB), Acti9 NG125H, 4P, 25A, C curve, 36kA (IEC/EN 60947-2)",0.12]
["18734","NG125H 4P 20A C 4P 20A C 380/415V 3600",1,"ks",{"v":626.2199999999999,"d":"626.220"},"3303430187349",{"v":15.2,"d":"15.20"},{"v":8.5,"d":"8.50"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18734","Miniature circuit breaker (MCB), Acti9 NG125H, 4P, 20A, C curve, 36kA (IEC/EN 60947-2)",0.12]
["18733","ISTIČ NG125H 4P 16A C",1,"ks",{"v":652.68,"d":"652.680"},"3303430187332",{"v":15.6,"d":"15.60"},{"v":8.4,"d":"8.40"},{"v":12.2,"d":"12.20"},{"v":978,"d":"978.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18733","NG125 - istič - NG125H - 4P - 16A - char. C",0.12]
["18732","ISTIČ NG125H 4P 10A C",1,"ks",{"v":683.5499999999998,"d":"683.550"},"3303430187325",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18732","Miniature circuit breaker (MCB), Acti9 NG125H, 4P, 10A, C curve, 36kA (IEC/EN 60947-2)",0.12]
["18731","ISTIČ NG125H 3P 80A C",1,"ks",{"v":445.4099999999999,"d":"445.410"},"3303430187318",{"v":12.7,"d":"12.70"},{"v":8.4,"d":"8.40"},{"v":12.2,"d":"12.20"},{"v":785,"d":"785.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18731","NG125 - istič - NG125H - 3P - 80A - char. C",0.1]
["18730","ISTIČ NG125H 3P 63A C",1,"ks",{"v":401.30999999999995,"d":"401.310"},"3303430187301",{"v":12.9,"d":"12.90"},{"v":8.8,"d":"8.80"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18730","NG125 - istič - NG125H - 3P - 63A - char. C",0.09]
["18729","ISTIČ NG125H 3P 50A C",1,"ks",{"v":418.95,"d":"418.950"},"3303430187295",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":750,"d":"750.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18729","NG125 - istič - NG125H - 3P - 50A - char. C",0.09]
["18728","NG125H 3P 40A C",1,"ks",{"v":427.7699999999999,"d":"427.770"},"3303430187288",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":747,"d":"747.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18728","NG125 - istič - NG125H - 3P - 40A - char. C",0.09]
["18727","ISTIČ NG125H 3P 32A C",1,"ks",{"v":436.59,"d":"436.590"},"3303430187271",{"v":12.7,"d":"12.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":753,"d":"753.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18727","NG125 - istič - NG125H - 3P - 32A - char. C",0.09]
["18726","ISTIČ NG125H 3P 25A C",1,"ks",{"v":445.4099999999999,"d":"445.410"},"3303430187264",{"v":12.8,"d":"12.80"},{"v":8.8,"d":"8.80"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18726","NG125 - istič - NG125H - 3P - 25A - char. C",0.09]
["18725","ISTIČ NG125H 3P 20A C",1,"ks",{"v":458.64,"d":"458.640"},"3303430187257",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18725","NG125 - istič - NG125H - 3P - 20A - char. C",0.09]
["18724","ISTIČ NG125H 3P 16A C",1,"ks",{"v":476.28,"d":"476.280"},"3303430187240",{"v":12.9,"d":"12.90"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":756,"d":"756.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18724","NG125 - istič - NG125H - 3P - 16A - char. C",0.09]
["18723","ISTIČ NG125H 3P 10A C",1,"ks",{"v":502.73999999999995,"d":"502.740"},"3303430187233",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":737,"d":"737.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18723","NG125 - istič - NG125H - 3P - 10A - char. C",0.09]
["18721","ISTIČ NG125H 2P 63A C",1,"ks",{"v":260.19,"d":"260.190"},"3303430187219",{"v":11.1,"d":"11.10"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":480,"d":"480.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18721","Miniature circuit breaker (MCB), Acti9 NG125H, 2P, 63A, C curve, 36kA (IEC/EN 60947-2)",0.06]
["18720","ISTIČ NG125H 2P 50A C",1,"ks",{"v":374.84999999999997,"d":"374.850"},"3303430187202",{"v":10.8,"d":"10.80"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":475,"d":"475.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18720","Miniature circuit breaker (MCB), Acti9 NG125H, 2P, 50A, C curve, 36kA (IEC/EN 60947-2)",0.06]
["18719","ISTIČ NG125H 2P 40A C",1,"ks",{"v":277.83,"d":"277.830"},"3303430187196",{"v":10.8,"d":"10.80"},{"v":5.5,"d":"5.50"},{"v":8.1,"d":"8.10"},{"v":475,"d":"475.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18719","Miniature circuit breaker (MCB), Acti9 NG125H, 2P, 40A, C curve, 36kA (IEC/EN 60947-2)",0.06]
["18718","ISTIČ NG125H 2P 32A C",1,"ks",{"v":282.23999999999995,"d":"282.240"},"3303430187189",{"v":11,"d":"11.00"},{"v":5.8,"d":"5.80"},{"v":8.3,"d":"8.30"},{"v":478,"d":"478.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18718","NG125 - istič - NG125H - 2P - 32A - char. C",0.06]
["18717","ISTIČ NG125H 2P 25A C",1,"ks",{"v":291.05999999999995,"d":"291.060"},"3303430187172",{"v":10.8,"d":"10.80"},{"v":5.5,"d":"5.50"},{"v":8.1,"d":"8.10"},{"v":475,"d":"475.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18717","NG125 - istič - NG125H - 2P - 25A - char. C",0.06]
["18716","ISTIČ NG125H 2P 20A C",1,"ks",{"v":299.87999999999994,"d":"299.880"},"3303430187165",{"v":10.9,"d":"10.90"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":478,"d":"478.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18716","NG125 - istič - NG125H - 2P - 20A - char. C",0.06]
["18715","ISTIČ NG125H 2P 16A C",1,"ks",{"v":313.10999999999996,"d":"313.110"},"3303430187158",{"v":10.8,"d":"10.80"},{"v":8,"d":"8.00"},{"v":5.5,"d":"5.50"},{"v":476,"d":"476.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18715","NG125 - istič - NG125H - 2P - 16A - char. C",0.06]
["18714","NG125H 2P 10A C",1,"ks",{"v":326.34,"d":"326.340"},"3303430187141",{"v":11,"d":"11.00"},{"v":5.5,"d":"5.50"},{"v":8.1,"d":"8.10"},{"v":469,"d":"469.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18714","NG125 - istič - NG125H - 2P - 10A - char. C",0.06]
["18713","ISTIČ NG125H 1P 80A C",1,"ks",{"v":167.57999999999998,"d":"167.580"},"3303430187134",{"v":11,"d":"11.00"},{"v":3.2,"d":"3.20"},{"v":8.1,"d":"8.10"},{"v":240,"d":"240.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18713","Miniature circuit breaker (MCB), Acti9 NG125H, 1P, 80A, C curve, 36kA (IEC/EN 60947-2)",0.03]
["18712","ISTIČ NG125H 1P 63A C",1,"ks",{"v":114.66,"d":"114.660"},"3303430187127",{"v":11,"d":"11.00"},{"v":3.2,"d":"3.20"},{"v":8.1,"d":"8.10"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18712","Miniature circuit breaker (MCB), Acti9 NG125H, 1P, 63A, C curve, 36kA (IEC/EN 60947-2)",0.03]
["18711","ISTIČ NG125H 1P 50A C",1,"ks",{"v":158.75999999999996,"d":"158.760"},"3303430187110",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18711","Miniature circuit breaker (MCB), Acti9 NG125H, 1P, 50A, C curve, 36kA (IEC/EN 60947-2)",0.03]
["18710","ISTIČ NG125H 1P 40A C",1,"ks",{"v":180.80999999999997,"d":"180.810"},"3303430187103",{"v":10.9,"d":"10.90"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18710","NG125 - istič - NG125H - 1P - 40A - char. C",0.03]
["18709","ISTIČ NG125H 1P 32A C",1,"ks",{"v":123.47999999999999,"d":"123.480"},"3303430187097",{"v":10.8,"d":"10.80"},{"v":3.2,"d":"3.20"},{"v":8.3,"d":"8.30"},{"v":242,"d":"242.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18709","NG125 - istič - NG125H - 1P - 32A - char. C",0.03]
["18708","ISTIČ NG125H 1P 25A C",1,"ks",{"v":123.47999999999999,"d":"123.480"},"3303430187080",{"v":10.8,"d":"10.80"},{"v":3.2,"d":"3.20"},{"v":8.3,"d":"8.30"},{"v":237,"d":"237.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18708","Miniature circuit breaker (MCB), Acti9 NG125H, 1P, 25A, C curve, 36kA (IEC/EN 60947-2)",0.03]
["18707","ISTIČ NG125H 1P 20A C",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3303430187073",{"v":10.7,"d":"10.70"},{"v":3.2,"d":"3.20"},{"v":8.1,"d":"8.10"},{"v":243,"d":"243.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18707","Miniature circuit breaker (MCB), Acti9 NG125H, 1P, 20A, C curve, 36kA (IEC/EN 60947-2)",0.03]
["18706","ISTIČ NG125H 1P 16A C",1,"ks",{"v":132.29999999999998,"d":"132.300"},"3303430187066",{"v":11.1,"d":"11.10"},{"v":3.2,"d":"3.20"},{"v":8.3,"d":"8.30"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18706","Miniature circuit breaker (MCB), Acti9 NG125H, 1P, 16A, C curve, 36kA (IEC/EN 60947-2)",0.03]
["18705","ISTIČ NG125H 1P 10A C",1,"ks",{"v":141.11999999999998,"d":"141.120"},"3303430187059",{"v":10.9,"d":"10.90"},{"v":3.2,"d":"3.20"},{"v":8.1,"d":"8.10"},{"v":242,"d":"242.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18705","NG125 - istič - NG125H - 1P - 10A - char. C",0.03]
["18674","ISTIČ NG125N 4P 125A D",1,"ks",{"v":701.1899999999998,"d":"701.190"},"3303430186748",{"v":15.6,"d":"15.60"},{"v":8.4,"d":"8.40"},{"v":12.2,"d":"12.20"},{"v":1038,"d":"1,038.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18674","NG125 - istič - NG125N - 4P - 125A - char. D",0.12]
["18673","ISTIČ NG125N 4P 100A D",1,"ks",{"v":612.9899999999999,"d":"612.990"},"3303430186731",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18673","NG125 - istič - NG125N - 4P - 100A - char. D",0.13]
["18672","ISTIČ NG125N 4P 80A D",1,"ks",{"v":582.1199999999999,"d":"582.120"},"3303430186724",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1054,"d":"1,054.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18672","NG125 - istič - NG125N - 4P - 80A - char. D",0.13]
["18671","ISTIČ NG125N 3P 125A D",1,"ks",{"v":515.9699999999999,"d":"515.970"},"3303430186717",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":788,"d":"788.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18671","NG125 - istič - NG125N - 3P - 125A - char. D",0.1]
["18670","ISTIČ NG125N 3P 100A D",1,"ks",{"v":449.81999999999994,"d":"449.820"},"3303430186700",{"v":13,"d":"13.00"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":793,"d":"793.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18670","NG125 - istič - NG125N - 3P - 100A - char. D",0.1]
["18669","ISTIČ NG125N 3P 80A D",1,"ks",{"v":427.7699999999999,"d":"427.770"},"3303430186694",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":782,"d":"782.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18669","NG125 - istič - NG125N - 3P - 80A - char. D",0.1]
["18668","ISTIČ NG125N 4P 125A B",1,"ks",{"v":643.8599999999999,"d":"643.860"},"3303430186687",{"v":15.7,"d":"15.70"},{"v":8.8,"d":"8.80"},{"v":12.1,"d":"12.10"},{"v":1060,"d":"1,060.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18668","NG125 - istič - NG125N - 4P - 125A - char. B",0.13]
["18667","ISTIČ NG125N 4P 100A B",1,"ks",{"v":560.0699999999999,"d":"560.070"},"3303430186670",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1047,"d":"1,047.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18667","NG125 - istič - NG125N - 4P - 100A - char. B",0.13]
["18666","ISTIČ NG125N 4P 80A B",1,"ks",{"v":529.1999999999999,"d":"529.200"},"3303430186663",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1057,"d":"1,057.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18666","NG125 - istič - NG125N - 4P - 80A - char. B",0.13]
["18665","ISTIČ NG125N 3P 125A B",1,"ks",{"v":471.86999999999995,"d":"471.870"},"3303430186656",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":720,"d":"720.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18665","NG125 - istič - NG125N - 3P - 125A - char. B",0.1]
["18664","ISTIČ NG125N 3P 100A B",1,"ks",{"v":410.12999999999994,"d":"410.130"},"3303430186649",{"v":13,"d":"13.00"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":796,"d":"796.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18664","NG125 - istič - NG125N - 3P - 100A - char. B",0.1]
["18663","ISTIČ NG125N 3P 80A B",1,"ks",{"v":388.0799999999999,"d":"388.080"},"3303430186632",{"v":13,"d":"13.00"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":797,"d":"797.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18663","NG125 - istič - NG125N - 3P - 80A - char. B",0.1]
["18662","ISTIČ NG125N 4P 125A C",1,"ks",{"v":612.9899999999999,"d":"612.990"},"3303430186625",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1053,"d":"1,053.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18662","miniatúrny istič – NG125N – 4 póly – 125 A – krivka C",0.13]
["18661","ISTIČ NG125N 4P 125A C",1,"ks",{"v":612.9899999999999,"d":"612.990"},"3303430186618",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1035,"d":"1,035.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18661","Miniature circuit breaker (MCB), Acti9 NG125N, 4P, 125A, C curve, 25kA (IEC/EN 60947-2)",0]
["18660","ISTIČ NG125N 4P 100A C",1,"ks",{"v":573.2999999999998,"d":"573.300"},"3303430186601",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18660","miniatúrny istič – NG125N – 4 póly – 100 A – krivka C",0.13]
["18658","ISTIČ NG125N 4P 80A C",1,"ks",{"v":507.1499999999999,"d":"507.150"},"3303430186588",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1050,"d":"1,050.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18658","miniatúrny istič – NG125N – 4 póly – 80 A – krivka C",0]
["18656","ISTIČ NG125N 4P 63A C",1,"ks",{"v":458.64,"d":"458.640"},"3303430186564",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":1004.9999999999999,"d":"1,005.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18656","NG125 - istič - NG125N - 4P - 63A - char. C",0.12]
["18655","ISTIČ NG125N 4P 50A C",1,"ks",{"v":471.86999999999995,"d":"471.870"},"3303430186557",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18655","NG125 - istič - NG125N - 4P - 50A - char. C",0.12]
["18654","ISTIČ NG125N 4P 40A C",1,"ks",{"v":485.0999999999999,"d":"485.100"},"3303430186540",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18654","NG125 - istič - NG125N - 4P - 40A - char. C",0.12]
["18653","ISTIČ NG125N 4P 32A C",1,"ks",{"v":493.91999999999996,"d":"493.920"},"3303430186533",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":960,"d":"960.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18653","NG125 - istič - NG125N - 4P - 32A - char. C",0.12]
["18652","ISTIČ NG125N 4P 25A C",1,"ks",{"v":507.1499999999999,"d":"507.150"},"3303430186526",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":993,"d":"993.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18652","NG125 - istič - NG125N - 4P - 25A - char. C",0.12]
["18651","ISTIČ NG125N 4P 20A C",1,"ks",{"v":520.38,"d":"520.380"},"3303430186519",{"v":15.6,"d":"15.60"},{"v":8.2,"d":"8.20"},{"v":12.4,"d":"12.40"},{"v":980,"d":"980.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18651","NG125 - istič - NG125N - 4P - 20A - char. C",0.12]
["18650","ISTIČ NG125N 4P 16A C",1,"ks",{"v":542.43,"d":"542.430"},"3303430186502",{"v":15.5,"d":"15.50"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":997,"d":"997.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18650","NG125 - istič - NG125N - 4P - 16A - char. C",0.12]
["18649","ISTIČ NG125N 4P 10A C",1,"ks",{"v":568.89,"d":"568.890"},"3303430186496",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":971,"d":"971.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18649","NG125 - istič - NG125N - 4P - 10A - char. C",0.12]
["18648","ISTIČ NG125N 3P+N 125A C",1,"ks",{"v":560.0699999999999,"d":"560.070"},"3303430186489",{"v":15.8,"d":"15.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1052,"d":"1,052.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18648","Miniature circuit breaker (MCB), Acti9 NG125N, 3P+N, 125A, C curve, 25kA (IEC/EN 60947-2)",0.13]
["18647","ISTIČ NG125N 3P+N 100A C",1,"ks",{"v":489.50999999999993,"d":"489.510"},"3303430186472",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1046,"d":"1,046.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18647","Miniature circuit breaker (MCB), Acti9 NG125N, 3P+N, 100A, C curve, 25kA (IEC/EN 60947-2)",0.13]
["18646","ISTIČ NG125N 3P+N 80A C",1,"ks",{"v":463.0499999999999,"d":"463.050"},"3303430186465",{"v":15.6,"d":"15.60"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1055,"d":"1,055.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18646","Miniature circuit breaker (MCB), Acti9 NG125N, 3P+N, 80A, C curve, 25kA (IEC/EN 60947-2)",0.13]
["18644","ISTIČ NG125N 3P 125A C",1,"ks",{"v":449.81999999999994,"d":"449.820"},"3303430186441",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":799,"d":"799.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18644","miniatúrny istič – NG125N – 3póly – 125 A – krivka C",0.1]
["18642","ISTIČ NG125N 3P 100A C",1,"ks",{"v":392.48999999999995,"d":"392.490"},"3303430186427",{"v":12.8,"d":"12.80"},{"v":8.8,"d":"8.80"},{"v":12.1,"d":"12.10"},{"v":780,"d":"780.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18642","miniatúrny istič – NG125N – 3 póly – 100 A – krivka C",0.1]
["18640","ISTIČ NG125N 3P 80A C",1,"ks",{"v":370.44,"d":"370.440"},"3303430186403",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":783,"d":"783.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18640","miniatúrny istič – NG125N – 3 póly – 80 A – krivka C",0.1]
["18639","ISTIČ NG125N 3P 63A C",1,"ks",{"v":335.15999999999997,"d":"335.160"},"3303430186397",{"v":12.9,"d":"12.90"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":758,"d":"758.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18639","NG125 - istič - NG125N - 3P - 63A - char. C",0.09]
["18638","ISTIČ NG125N 3P 50A C",1,"ks",{"v":348.39,"d":"348.390"},"3303430186380",{"v":12.7,"d":"12.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":758,"d":"758.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18638","NG125 - istič - NG125N - 3P - 50A - char. C",0.09]
["18637","ISTIČ NG125N 3P 40A C",1,"ks",{"v":357.21,"d":"357.210"},"3303430186373",{"v":12.5,"d":"12.50"},{"v":8.3,"d":"8.30"},{"v":12,"d":"12.00"},{"v":746,"d":"746.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18637","NG125 - istič - NG125N - 3P - 40A - char. C",0.09]
["18636","ISTIČ NG125N 3P 32A C",1,"ks",{"v":361.61999999999995,"d":"361.620"},"3303430186366",{"v":12.8,"d":"12.80"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":742,"d":"742.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18636","NG125 - istič - NG125N - 3P - 32A - char. C",0.09]
["18635","ISTIČ NG125N 3P 25A C",1,"ks",{"v":370.44,"d":"370.440"},"3303430186359",{"v":13,"d":"13.00"},{"v":8.6,"d":"8.60"},{"v":12.1,"d":"12.10"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18635","NG125 - istič - NG125N - 3P - 25A - char. C",0.09]
["18634","ISTIČ NG125N 3P 20A C",1,"ks",{"v":383.66999999999996,"d":"383.670"},"3303430186342",{"v":13.2,"d":"13.20"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":720,"d":"720.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18634","NG125 - istič - NG125N - 3P - 20A - char. C",0.09]
["18633","ISTIČ NG125N 3P 16A C",1,"ks",{"v":401.30999999999995,"d":"401.310"},"3303430186335",{"v":12.9,"d":"12.90"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":743,"d":"743.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18633","NG125 - istič - NG125N - 3P - 16A - char. C",0.09]
["18632","ISTIČ NG125N 3P 10A C",1,"ks",{"v":418.95,"d":"418.950"},"3303430186328",{"v":12.9,"d":"12.90"},{"v":8.8,"d":"8.80"},{"v":12.4,"d":"12.40"},{"v":745,"d":"745.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18632","NG125 - istič - NG125N - 3P - 10A - char. C",0.09]
["18629","ISTIČ NG125N 2P 80A C",1,"ks",{"v":242.54999999999995,"d":"242.550"},"3303430186298",{"v":11,"d":"11.00"},{"v":5.8,"d":"5.80"},{"v":8,"d":"8.00"},{"v":497,"d":"497.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18629","NG125 -istič - NG125N - 2P - 80A - char. C",0.06]
["18628","ISTIČ NG125N 2P 63A C",1,"ks",{"v":220.49999999999994,"d":"220.500"},"3303430186281",{"v":11.1,"d":"11.10"},{"v":5.5,"d":"5.50"},{"v":8.3,"d":"8.30"},{"v":480,"d":"480.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18628","NG125 - istič - NG125N - 2P - 63A - char. C",0.06]
["18627","ISTIČ NG125N 2P 50A C",1,"ks",{"v":313.10999999999996,"d":"313.110"},"3303430186274",{"v":11,"d":"11.00"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":480,"d":"480.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18627","NG125 - istič - NG125N - 2P - 50A - char. C",0.06]
["18626","ISTIČ NG125N 2P 40A C",1,"ks",{"v":229.32,"d":"229.320"},"3303430186267",{"v":11.1,"d":"11.10"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":480,"d":"480.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18626","NG125 - istič - NG125N - 2P - 40A - char. C",0.06]
["18625","ISTIČ NG125N 2P 32A C",1,"ks",{"v":238.14,"d":"238.140"},"3303430186250",{"v":10.9,"d":"10.90"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":477,"d":"477.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18625","NG125 - istič - NG125N - 2P - 32A - char. C",0.06]
["18624","ISTIČ NG125N 2P 25A C",1,"ks",{"v":242.54999999999995,"d":"242.550"},"3303430186243",{"v":10.8,"d":"10.80"},{"v":5.5,"d":"5.50"},{"v":8,"d":"8.00"},{"v":477,"d":"477.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18624","NG125 - istič - NG125N - 2P - 25A - char. C",0.06]
["18623","ISTIČ NG125N 2P 20A C",1,"ks",{"v":246.95999999999998,"d":"246.960"},"3303430186236",{"v":11,"d":"11.00"},{"v":5.8,"d":"5.80"},{"v":8.1,"d":"8.10"},{"v":477,"d":"477.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18623","NG125 - istič - NG125N - 2P - 20A - char. C",0.06]
["18622","ISTIČ NG125N 2P 16A C",1,"ks",{"v":260.19,"d":"260.190"},"3303430186229",{"v":10.2,"d":"10.20"},{"v":5.6,"d":"5.60"},{"v":8,"d":"8.00"},{"v":477,"d":"477.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18622","NG125 - istič - NG125N - 2P - 16A - char. C",0.06]
["18621","ISTIČ NG125N 2P 10A C",1,"ks",{"v":273.41999999999996,"d":"273.420"},"3303430186212",{"v":11.2,"d":"11.20"},{"v":5.4,"d":"5.40"},{"v":7.8,"d":"7.80"},{"v":468,"d":"468.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18621","NG125 - istič - NG125N - 2P - 10A - char. C",0.06]
["18617","ISTIČ NG125N 1P 63A C",1,"ks",{"v":132.29999999999998,"d":"132.300"},"3303430186175",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.3,"d":"8.30"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18617","NG125 - istič - NG125N - 1P - 63A - char. C",0.03]
["18616","ISTIČ NG125N 1P 50A C",1,"ks",{"v":136.70999999999998,"d":"136.710"},"3303430186168",{"v":10.8,"d":"10.80"},{"v":3.2,"d":"3.20"},{"v":8.3,"d":"8.30"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18616","NG125 - istič - NG125N - 1P - 50A - char. C",0.03]
["18615","ISTIČ NG125N 1P 40A C",1,"ks",{"v":101.42999999999998,"d":"101.430"},"3303430186151",{"v":10.8,"d":"10.80"},{"v":2.9,"d":"2.90"},{"v":8,"d":"8.00"},{"v":246,"d":"246.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18615","NG125 - istič - NG125N - 1P - 40A - char. C",0.03]
["18614","ISTIČ NG125N 1P 32A C",1,"ks",{"v":101.42999999999998,"d":"101.430"},"3303430186144",{"v":10.9,"d":"10.90"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":243,"d":"243.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18614","NG125 - istič - NG125N - 1P - 32A - char. C",0.03]
["18613","ISTIČ NG125N 1P 25A C",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3303430186137",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18613","NG125 - istič - NG125N - 1P - 25A - char. C",0.03]
["18612","ISTIČ NG125N 1P 20A C",1,"ks",{"v":105.83999999999997,"d":"105.840"},"3303430186120",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8,"d":"8.00"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18612","NG125 - istič - NG125N - 1P - 20A - char. C",0.03]
["18611","ISTIČ NG125N 1P 16A C",1,"ks",{"v":110.24999999999997,"d":"110.250"},"3303430186113",{"v":10.8,"d":"10.80"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":244,"d":"244.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18611","NG125 - istič - NG125N - 1P - 16A - char. C",0.03]
["18610","ISTIČ NG125N 1P 10A C",1,"ks",{"v":119.07,"d":"119.070"},"3303430186106",{"v":11,"d":"11.00"},{"v":3,"d":"3.00"},{"v":8.1,"d":"8.10"},{"v":240,"d":"240.00"},"FR","8536201090","https://www.se.com/sk/sk/product/18610","NG125 - istič - NG125N - 1P - 10A - char. C",0.03]
["18607","ISTIČ NG125A 4P 80A C",1,"ks",{"v":454.22999999999996,"d":"454.230"},"3303430186076",{"v":15.7,"d":"15.70"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":1051,"d":"1,051.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18607","Miniature circuit breaker (MCB), Acti9 NG125a, 4P, 80A, C curve, 16kA (IEC/EN 60947-2)",0.12]
["18603","Istic NG125A 3P 80A B",1,"ks",{"v":370.44,"d":"370.440"},"3303430186038",{"v":13.1,"d":"13.10"},{"v":8.6,"d":"8.60"},{"v":12.4,"d":"12.40"},{"v":798,"d":"798.00"},"FR","8536209090","https://www.se.com/sk/sk/product/18603","Miniature circuit breaker (MCB), Acti9 NG125a, 3P, 80A, C curve, 16kA (IEC/EN 60947-2)",0.1]
["18528","SADA PRE ZADNÝ PRÍVOD C120 2 KS",1,"ks",66.591,"3303430185284",{"v":7.5,"d":"7.50"},{"v":2.8,"d":"2.80"},{"v":7.5,"d":"7.50"},{"v":106,"d":"106.00"},"FR","85369010","https://www.se.com/sk/sk/product/18528","kryt svoriek - zadné pripojenie - 1 tyč - pre C120 - sada 2 ks",0.01]
["18527","KRYT SKRUTIEK NA SVORKÁCH C120 2KS",1,"ks",{"v":39.248999999999995,"d":"39.249"},"3303430185277",{"v":11.5,"d":"11.50"},{"v":1.8,"d":"1.80"},{"v":4,"d":"4.00"},{"v":26,"d":"26.00"},"FR","85362010","https://www.se.com/sk/sk/product/18527","kryt skrutiek - pre C120 - sada 8",0]
["18526","KRYT SVORIEK C120, SADA 2KS",1,"ks",{"v":26.459999999999994,"d":"26.460"},"3303430185260",{"v":7,"d":"7.00"},{"v":3,"d":"3.00"},{"v":5.5,"d":"5.50"},{"v":36,"d":"36.00"},"FR","85362010","https://www.se.com/sk/sk/product/18526","kryt svoriek- 1 pól - pre C120",0]
["18281","RED TEST 2P 40A 30MA A",1,"ks",{"v":397.7819999999999,"d":"397.782"},"3303430182818",{"v":17.5,"d":"17.50"},{"v":12.3,"d":"12.30"},{"v":15,"d":"15.00"},{"v":728,"d":"728.00"},"IT","8536303099","https://www.se.com/sk/sk/product/18281","Residual current circuit breaker (RCCB), Acti9 REDtest, 2P, 40A, A type, 30mA",""]
["18268","PR. CHRÁNIČ REDS 4P 63A 30MA A",1,"ks",{"v":718.8299999999999,"d":"718.830"},"3303430182689",{"v":17,"d":"17.00"},{"v":11.6,"d":"11.60"},{"v":14,"d":"14.00"},{"v":770,"d":"770.00"},"IT","73044999","https://www.se.com/sk/sk/product/18268","prúdový chránič s opätovným zapnutím REDS 4P 63A 30MA A",0.1]
["18267","PR. CHRÁNIČ REDS 4P 40A 300MA A",1,"ks",{"v":405.7199999999999,"d":"405.720"},"3303430182672",{"v":17,"d":"17.00"},{"v":11.6,"d":"11.60"},{"v":13.8,"d":"13.80"},{"v":707,"d":"707.00"},"IT","73044999","https://www.se.com/sk/sk/product/18267","prúdový chránič s opätovným zapnutím REDS 4P 40A 300MA A",0.1]
["18266","PR. CHRÁNIČ REDS 4P 40A 30MA A",1,"ks",{"v":449.81999999999994,"d":"449.820"},"3303430182665",{"v":16.8,"d":"16.80"},{"v":11.6,"d":"11.60"},{"v":13.8,"d":"13.80"},{"v":737,"d":"737.00"},"IT","8536303099","https://www.se.com/sk/sk/product/18266","prúdový chránič s opätovným zapnutím REDS 4P 40A 30MA A",0.1]
["18264","PR. CHRÁNIČ REDS 4P 25A 30MA A",1,"ks",{"v":427.7699999999999,"d":"427.770"},"3303430182641",{"v":17,"d":"17.00"},{"v":12,"d":"12.00"},{"v":14,"d":"14.00"},{"v":731,"d":"731.00"},"IT","73044999","https://www.se.com/sk/sk/product/18264","prúdový chránič s opätovným zapnutím REDS 4P 25A 30MA A",0.08]
["171CBU78090","MOMENTUM UNITY M1 SERIAL 232/485, SERIAL",1,"ks",{"v":1006.0974,"d":"1006.097"},"3595864171388",{"v":20.5,"d":"20.50"},{"v":7.5,"d":"7.50"},{"v":11.1,"d":"11.10"},{"v":236,"d":"236.00"},"FR","8537109199","https://www.se.com/sk/sk/product/171CBU78090","Momentum Unity M1 Serial 232/485, Serial 485, USB, IO Bus, RTC, 3584K RAM",""]
["170XTS00200","BLOK BEZSKRUTKOVÝCH SVORIEK 3ks",1,"ks",{"v":88.3575,"d":"88.358"},"3389110886771",{"v":9,"d":"9.00"},{"v":2,"d":"2.00"},{"v":1.6,"d":"1.60"},{"v":31,"d":"31.00"},"CN","8536901000","https://www.se.com/sk/sk/product/170XTS00200","spring terminal block - Modicon Momentum, Modicon Quantum",0]
["170XTS00100","BLOK SKRUTKOVÝCH SVORIEK 3 ks",1,"ks",{"v":64.20644999999999,"d":"64.206"},"3389110886764",{"v":10,"d":"10.00"},{"v":1.8,"d":"1.80"},{"v":8,"d":"8.00"},{"v":103,"d":"103.00"},"DE","85366990","https://www.se.com/sk/sk/product/170XTS00100","screw terminal block - Modicon Momentum, Modicon Quantum",0]
["170MCI10001","INTERBUS S CABLE - 100CM LONG",1,"ks",{"v":90.12465,"d":"90.125"},"3595860027139",{"v":16,"d":"16.00"},{"v":1.5,"d":"1.50"},{"v":13,"d":"13.00"},{"v":74,"d":"74.00"},"PT","8544429090","https://www.se.com/sk/sk/product/170MCI10001","interbus preconnected cable - Modicon Quantum - 1 m",0]
["170MCI00700","INTERBUS/S hlavný kábel, 11CM",1,"ks",{"v":62.439299999999996,"d":"62.439"},"3595861148031",{"v":20,"d":"20.00"},{"v":2,"d":"2.00"},{"v":5,"d":"5.00"},{"v":46,"d":"46.00"},"CN","8544429090","https://www.se.com/sk/sk/product/170MCI00700","interbus preconnected cable - Modicon Quantum, Modicon Premium - 0.11 m",0]
["170INT11003","ADAPTÉR INTERBUS-S GENERATION4 SUPI3",1,"ks",223.839,"3595862060721",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18.1,"d":"18.10"},{"v":198,"d":"198.00"},"FR","8517620000","https://www.se.com/sk/sk/product/170INT11003","Modicon Momentum - Interbus communication adaptor - twisted pair",0.02]
["170INT11000","KOM. ADAPTÉR INTERBUS/S (I/O BUS), METAL",1,"ks",223.839,"3595861000360",{"v":26,"d":"26.00"},{"v":5.6,"d":"5.60"},{"v":17.8,"d":"17.80"},{"v":183,"d":"183.00"},"FR","8517620000","https://www.se.com/sk/sk/product/170INT11000","Modicon Momentum - Interbus communication adaptor - twisted pair",0.02]
["170ENT11002","KOM.ADAPTÉR ETHERNET 10BASE-T + MODBUS",1,"ks",329.868,"3595862065054",{"v":26,"d":"26.00"},{"v":5.8,"d":"5.80"},{"v":17.8,"d":"17.80"},{"v":219,"d":"219.00"},"FR","8517620000","https://www.se.com/sk/sk/product/170ENT11002","Modicon Momentum - Ethernet communication adaptor - 10 Mbit/s",0.03]
["170ENT11001","Kom.adaptér Ethernet,WEBserver,Modbus",1,"ks",{"v":783.4365,"d":"783.437"},"3595862034302",{"v":26.1,"d":"26.10"},{"v":6,"d":"6.00"},{"v":18.3,"d":"18.30"},{"v":233,"d":"233.00"},"FR","8517620000","https://www.se.com/sk/sk/product/170ENT11001","Modicon Momentum - Ethernet communication adaptor - 10/100 Mbit/s",0.03]
["170ANR12091","ZÁKLADŇA 6AI/4AO 10VDC, 8DI/8DO 24VDC",1,"ks",1590.435,"3595862053402",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":240,"d":"240.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ANR12091","distributed analog/discrete I/O - 4 I / 8 O discrete - 6 I / 4 O analog",0.05]
["170ANR12090","ZÁKLADŇA 6AI, 4AO, 8DI 24VJS",1,"ks",1590.435,"3595860019523",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":240,"d":"240.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ANR12090","distributed analog/discrete I/O Modicon Momentum",0.05]
["170AMM09000","ZÁKLADŇA 4 AI, 2 AO, 4KDI 24VJS",1,"ks",{"v":1237.0049999999999,"d":"1237.005"},"3595861000292",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":240,"d":"240.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170AMM09000","distributed analog/discrete I/O Modicon Momentum",0.05]
["170AEC92000","ZÁKLADŇA 2K RÝCHLY ČÍTAČ",1,"ks",{"v":1237.0049999999999,"d":"1237.005"},"3595861147744",{"v":26.2,"d":"26.20"},{"v":5.8,"d":"5.80"},{"v":18,"d":"18.00"},{"v":356,"d":"356.00"},"FR","9029100090","https://www.se.com/sk/sk/product/170AEC92000","Modicon Momentum - high speed counter module base - 6 I / 4 O",0.04]
["170ADO74050","ZÁKLADŇA 16K DISKR. VÝSTUP 230VST 0.5A",1,"ks",{"v":883.5749999999999,"d":"883.575"},"3595861147584",{"v":26,"d":"26.00"},{"v":9.5,"d":"9.50"},{"v":18,"d":"18.00"},{"v":284,"d":"284.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADO74050","discrete output module Modicon Momentum - 16 O solid state",0.06]
["170ADO54050","ZÁKLADŇA 16K DISKR. VÝSTUP 120VST 0.5A",1,"ks",612.612,"3595861147560",{"v":25.5,"d":"25.50"},{"v":9,"d":"9.00"},{"v":18,"d":"18.00"},{"v":284,"d":"284.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADO54050","discrete output module Modicon Momentum - 16 O solid state",0.06]
["170ADO53050","ZÁKLADŇA 8K DISKR. VÝSTUP 120VST 2.0A",1,"ks",{"v":677.4075,"d":"677.408"},"3595861147553",{"v":26,"d":"26.00"},{"v":9,"d":"9.00"},{"v":18,"d":"18.00"},{"v":320,"d":"320.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADO53050","discrete output module Modicon Momentum - 8 O solid state",0.06]
["170ADO35000","ZÁKLADŇA 32K DISKR. VÝSTUP 24VJS 0.5A",1,"ks",494.802,"3595861147676",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":210,"d":"210.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADO35000","discrete output module Modicon Momentum - 32 O solid state",0.05]
["170ADO34000","ZÁKLADŇA 16K DISKR. VÝSTUP 24VJS 0.5A",1,"ks",{"v":347.5395,"d":"347.540"},"3595861147669",{"v":26,"d":"26.00"},{"v":5.7,"d":"5.70"},{"v":18.2,"d":"18.20"},{"v":210,"d":"210.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADO34000","discrete output module Modicon Momentum - 16 O solid state",0.05]
["170ADM85010","ZÁKLADŇA 16DI/16DO 10-60VDC",1,"ks",836.451,"3595862070133",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":380,"d":"380.00"},"US","8538909999","https://www.se.com/sk/sk/product/170ADM85010","discrete I/O module Modicon Momentum - 16 I/O relay",0.05]
["170ADM69051","ZÁKLADŇA 10 DI 120VST, 8 DO 120VST 0.5",1,"ks",695.079,"3595860019271",{"v":25.5,"d":"25.50"},{"v":9,"d":"9.00"},{"v":18.5,"d":"18.50"},{"v":484,"d":"484.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADM69051","discrete I/O module Modicon Momentum - 10I / 8O solid state",0.06]
["170ADM54080","ZÁKLADŇA 6 DI 120VST, 3 DO 120VST 0.5",1,"ks",{"v":860.0129999999999,"d":"860.013"},"3595860009326",{"v":21,"d":"21.00"},{"v":6.7,"d":"6.70"},{"v":17,"d":"17.00"},{"v":240,"d":"240.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADM54080","Modicon Momentum - Modbus I/O module base - 6 I / 3 O",0]
["170ADM39030","ZÁKLADŇA 10 DI 24VJS, 8 DO RELÉ",1,"ks",{"v":371.1015,"d":"371.102"},"3595861147652",{"v":26,"d":"26.00"},{"v":9,"d":"9.00"},{"v":18,"d":"18.00"},{"v":260,"d":"260.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADM39030","discrete I/O module Modicon Momentum - 10I / 8O relay",0.06]
["170ADM37010","ZÁKLADŇA 16 DI 24VJS, 8 DO 24VJS 2.0A",1,"ks",483.021,"3595861147638",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":220,"d":"220.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADM37010","discrete I/O module Modicon Momentum - 16I / 8O solid state",0.05]
["170ADM35011","ZÁKLADŇA 16K DI 24VJS, 16K DO 24VJS 0.5A",1,"ks",435.897,"3595861147621",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":200,"d":"200.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADM35011","discrete I/O module Modicon Momentum - 16 I/O solid state",0.05]
["170ADM35010","ZÁKLADŇA 16 DI 24VJS, 16 DO 24VJS 0.5",1,"ks",435.897,"3595861000261",{"v":25.8,"d":"25.80"},{"v":5.8,"d":"5.80"},{"v":18,"d":"18.00"},{"v":200,"d":"200.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADM35010","discrete I/O module Modicon Momentum - 16 I/O solid state",0.05]
["170ADI54050","ZÁKLADŇA 16K DISKR. VSTUP 120VST",1,"ks",{"v":606.7215,"d":"606.722"},"3595861147522",{"v":26,"d":"26.00"},{"v":9,"d":"9.00"},{"v":18,"d":"18.00"},{"v":284,"d":"284.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADI54050","discrete input module Modicon Momentum - 16 Input 100..120 V AC",0.06]
["170ADI35000","ZÁKLADŇA 32K DISKR. VSTUP 24VJS",1,"ks",{"v":365.21099999999996,"d":"365.211"},"3595861000254",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":200,"d":"200.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADI35000","discrete input module Modicon Momentum - 32 Input 24 V DC",0.05]
["170ADI34000","ZÁKLADŇA 16K DISKR. VSTUP 24VJS",1,"ks",306.306,"3595861000247",{"v":26,"d":"26.00"},{"v":5.7,"d":"5.70"},{"v":18.2,"d":"18.20"},{"v":190,"d":"190.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170ADI34000","discrete input module Modicon Momentum - 16 Input 24 V DC",0.05]
["170AAO92100","ZÁKLADŇA 4 ANAL. VÝSTUP 4-20MA",1,"ks",{"v":1042.6185,"d":"1042.619"},"3595861147720",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":215,"d":"215.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170AAO92100","distributed analog output Modicon Momentum - 4 Output - 4..20 mA",0.05]
["170AAO12000","ZÁKLADŇA 4 ANAL. VÝSTUP 0-20MA/ 10V",1,"ks",{"v":1042.6185,"d":"1042.619"},"3595861147713",{"v":25.5,"d":"25.50"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":210,"d":"210.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170AAO12000","distributed analog output Modicon Momentum - 4 Output - 0..20 mA",0.03]
["170AAI52040","ZÁKLADŇA 4 ANAL. VSTUP MULTIFUNKČNÝ",1,"ks",{"v":1237.0049999999999,"d":"1237.005"},"3389110886498",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":215,"d":"215.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170AAI52040","distributed analog input Modicon Momentum - 4 Input",0.05]
["170AAI03000","ZÁKLADŇA 8 ANAL. VSTUP 0-20MA/ 10V",1,"ks",{"v":1042.6185,"d":"1042.619"},"3595861147683",{"v":26,"d":"26.00"},{"v":5.5,"d":"5.50"},{"v":18,"d":"18.00"},{"v":215,"d":"215.00"},"FR","8538909999","https://www.se.com/sk/sk/product/170AAI03000","distributed analog input Modicon Momentum - 8 Input",0.05]
["16966","PRÚDOVÝ CHRÁNIČ 2P 125A 30MA A",1,"ks",{"v":471.86999999999995,"d":"471.870"},"3303430169666",{"v":9,"d":"9.00"},{"v":4,"d":"4.00"},{"v":8.2,"d":"8.20"},{"v":259,"d":"259.00"},"DE","85363030","https://www.se.com/sk/sk/product/16966","prúdový chránič ID Fi - 2P - 125 A - trieda AC 30mA",0.03]
["16940","POMOCNÝ KONTAKT PRE PRÚD CHRÁNIČ OFSP",1,"ks",{"v":23.813999999999997,"d":"23.814"},"3303430169406",{"v":9.5,"d":"9.50"},{"v":2.7,"d":"2.70"},{"v":8.1,"d":"8.10"},{"v":52,"d":"52.00"},"DE","85365080","https://www.se.com/sk/sk/product/16940","pomocný kontakt - 1 NC + 1 OC - 380 .. 415 V - 6 - pre RCCB",0]
["16939","KRYT SVORIEK 4MOD., SADA 10KS",1,"ks",14.994,"3303430169390",{"v":9.5,"d":"9.50"},{"v":2.5,"d":"2.50"},{"v":8,"d":"8.00"},{"v":48,"d":"48.00"},"DE","39269097","https://www.se.com/sk/sk/product/16939","kryt svoriek - 4 pól - pre ID RCCB - sada 10",0.01]
["16927","PRÚD CHRÁNIČ 4P 125A 500MA A",1,"ks",{"v":630.63,"d":"630.630"},"3303430169277",{"v":9,"d":"9.00"},{"v":8,"d":"8.00"},{"v":7.5,"d":"7.50"},{"v":413,"d":"413.00"},"DE","85363030","https://www.se.com/sk/sk/product/16927","prúdový chránič ID - 4 póly - 125 A - trieda 500 mA",0.05]
["16926","PRÚD CHRÁNIČ 4P 125A 300MA A",1,"ks",{"v":515.9699999999999,"d":"515.970"},"3303430169260",{"v":11.4,"d":"11.40"},{"v":7.6,"d":"7.60"},{"v":9.2,"d":"9.20"},{"v":418,"d":"418.00"},"DE","85363030","https://www.se.com/sk/sk/product/16926","prúdový chránič ID - 4 póly - 125 A - trieda 300 mA",0.05]
["16925","PRÚD CHRÁNIČ 4P 125A 300MA S A",1,"ks",{"v":723.2399999999999,"d":"723.240"},"3303430169253",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":436,"d":"436.00"},"DE","85363030","https://www.se.com/sk/sk/product/16925","prúdový chránič ID - 4 póly - 125 A - trieda 300 mA S",0.05]
["16924","PRÚD CHRÁNIČ 4P 125A 30MA S A",1,"ks",{"v":573.2999999999998,"d":"573.300"},"3303430169246",{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},{"v":8,"d":"8.00"},{"v":420,"d":"420.00"},"DE","85363030","https://www.se.com/sk/sk/product/16924","prúdový chránič ID - 4 póly - 125 A - trieda 30 mA",0.05]
["16921","PRÚD CHRÁNIČ 4P 125A 300MA ASI",1,"ks",{"v":573.2999999999998,"d":"573.300"},"3303430169215",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":414,"d":"414.00"},"DE","85363030","https://www.se.com/sk/sk/product/16921","prúdový chránič ID si - 4 póly - 125 A - trieda A 300mA",0.05]
["16920","PRÚD CHRÁNIČ 4P 125A 30MA ASI",1,"ks",{"v":582.1199999999999,"d":"582.120"},"3303430169208",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":432,"d":"432.00"},"DE","85363030","https://www.se.com/sk/sk/product/16920","prúdový chránič ID si - 4 póly - 125 A - trieda 30 mA",0.05]
["16908","PRÚD CHRÁNIČ 4P 125A 500MA",1,"ks",{"v":573.2999999999998,"d":"573.300"},"3303430169086",{"v":10,"d":"10.00"},{"v":9,"d":"9.00"},{"v":9,"d":"9.00"},{"v":416,"d":"416.00"},"DE","85363030","https://www.se.com/sk/sk/product/16908","prúdový chránič ID Fi - 4 póly - 125 A - trieda AC 500 mA",0.05]
["16907","PRÚD CHRÁNIČ 4P 125A 300MA",1,"ks",{"v":471.86999999999995,"d":"471.870"},"3303430169079",{"v":9.8,"d":"9.80"},{"v":7.2,"d":"7.20"},{"v":7.8,"d":"7.80"},{"v":417,"d":"417.00"},"DE","85363030","https://www.se.com/sk/sk/product/16907","prúdový chránič ID Fi - 4 póly - 125 A - trieda AC 300 mA",0.05]
["16906","PRÚD CHRÁNIČ 4P 125A 100MA",1,"ks",{"v":493.91999999999996,"d":"493.920"},"3303430169062",{"v":9.1,"d":"9.10"},{"v":8,"d":"8.00"},{"v":7.7,"d":"7.70"},{"v":448,"d":"448.00"},"DE","85363030","https://www.se.com/sk/sk/product/16906","prúdový chránič ID Fi - 4 póly - 125 A - trieda AC 100 mA",0.05]
["16905","PRÚD CHRÁNIČ 4P 125A 30MA",1,"ks",{"v":520.38,"d":"520.380"},"3303430169055",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":8,"d":"8.00"},{"v":450,"d":"450.00"},"DE","85363030","https://www.se.com/sk/sk/product/16905","prúdový chránič ID Fi - 4 póly - 125 A - 30 mA - trieda AC",0.05]
["16766","RCCB 4P 125A 500MA B",1,"ks",{"v":2998.7999999999997,"d":"2998.800"},"3303430167662",{"v":9,"d":"9.00"},{"v":7.5,"d":"7.50"},{"v":7.5,"d":"7.50"},{"v":495,"d":"495.00"},"DE","85363030","https://www.se.com/sk/sk/product/16766","prúdový chránič ID - 4P - 125 A - trieda B 500 mA",0.06]
["16765","RCCB 4P 125A 300MA S B",1,"ks",{"v":2866.4999999999995,"d":"2866.500"},"3303430167655",{"v":9,"d":"9.00"},{"v":8,"d":"8.00"},{"v":7.5,"d":"7.50"},{"v":498,"d":"498.00"},"DE","85363030","https://www.se.com/sk/sk/product/16765","prúdový chránič ID - 4P - 125 A - trieda B 300 mA S",0.06]
["16764","RCCB 4P 125A 300MA B",1,"ks",{"v":2866.4999999999995,"d":"2866.500"},"3303430167648",{"v":9,"d":"9.00"},{"v":8,"d":"8.00"},{"v":7.5,"d":"7.50"},{"v":495,"d":"495.00"},"DE","85363030","https://www.se.com/sk/sk/product/16764","prúdový chránič ID - 4P - 125 A - trieda B 300 mA",0.06]
["16763","RCCB 4P 125A 30MA B",1,"ks",{"v":2690.0999999999995,"d":"2690.100"},"3303430167631",{"v":9,"d":"9.00"},{"v":8,"d":"8.00"},{"v":7.5,"d":"7.50"},{"v":450,"d":"450.00"},"DE","85363030","https://www.se.com/sk/sk/product/16763","prúdový chránič ID - 4P - 125 A - trieda B 30 mA",0.06]
["16655","MINCLIC SCHOD.AUTOMAT MIN 1-7 240V",1,"ks",{"v":49.83299999999999,"d":"49.833"},"3303430166559",{"v":9.9,"d":"9.90"},{"v":2,"d":"2.00"},{"v":6.9,"d":"6.90"},{"v":82,"d":"82.00"},"DE","9107000090","https://www.se.com/sk/sk/product/16655","DuoLine - MIN'clic - electromechanical timer - adjustable from 1 to 7 minutes",0]
["16649","PRF1 MASTER 1P",1,"ks",{"v":392.48999999999995,"d":"392.490"},"3606480943256",{"v":11,"d":"11.00"},{"v":8.2,"d":"8.20"},{"v":4.5,"d":"4.50"},{"v":428,"d":"428.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16649","PRD135r zvodič prepätia - 1 pól - 440V - s diaľkovou signalizáciou",0.05]
["16363","ZVODIČ PRD1 MASTER 3P+N 350V SO SIGN",1,"ks",{"v":1543.4999999999998,"d":"1543.500"},"3606480060465",{"v":17.5,"d":"17.50"},{"v":9.5,"d":"9.50"},{"v":14,"d":"14.00"},{"v":1563,"d":"1,563.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16363","PRD1 Master modulárny zvodič prepätia - 3 póly+N - 350V - s diaľkovým prenosom",0.19]
["16362","ZVODIČ PRD1 MASTER 3P 350V SO SIGN",1,"ks",{"v":970.1999999999998,"d":"970.200"},"3606480060458",{"v":17.8,"d":"17.80"},{"v":9.8,"d":"9.80"},{"v":14,"d":"14.00"},{"v":1252,"d":"1,252.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16362","PRD1 Master modulárny zvodič prepätia - 3 póly - 350V - s diaľkovým prenosom",0.15]
["16361","ZVODIČ PRD1 MASTER 1P+N 350V SO SIGN",1,"ks",{"v":837.9,"d":"837.900"},"3606480060441",{"v":11,"d":"11.00"},{"v":8.1,"d":"8.10"},{"v":7.6,"d":"7.60"},{"v":769,"d":"769.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16361","PRD1 Master modulárny zvodič prepätia - 1 pól + N - 350V - s diaľkovým prenosom",0.09]
["16360","ZVODIČ PRD1 MASTER 1P 350V SO SIGN",1,"ks",{"v":379.25999999999993,"d":"379.260"},"3606480060434",{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},{"v":4.5,"d":"4.50"},{"v":418,"d":"418.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16360","PRD1 Master modulárny zvodič prepätia - 1 pól.- 350V - s diaľkovým prenosom",0.05]
["16332","ZVODIČ PRD1 25R 3P+N TYP I+II (B+C) 350V",1,"ks",{"v":970.1999999999998,"d":"970.200"},"3606480060427",{"v":17.5,"d":"17.50"},{"v":9.5,"d":"9.50"},{"v":14,"d":"14.00"},{"v":1370,"d":"1,370.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16332","PRD1 25r modulárny zvodič prepätia - 3 póly + N - 350V - s diaľkovým prenosom",0.16]
["16331","ZVODIČ PRD1 25R 3P TYP I+II 50V SIGNAL",1,"ks",{"v":784.9799999999999,"d":"784.980"},"3606480060410",{"v":18,"d":"18.00"},{"v":10,"d":"10.00"},{"v":14,"d":"14.00"},{"v":1049,"d":"1,049.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16331","PRD1 25r modulárny zvodič prepätia - 3 póly - 350V - s diaľkovým prenosom",0.13]
["16330","ZVODIČ PRD1 25R 1P+N TYP I+II N 350 SIGN",1,"ks",{"v":524.79,"d":"524.790"},"3606480060403",{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},{"v":7.5,"d":"7.50"},{"v":668,"d":"668.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16330","PRD1 25r modulárny zvodič prepätia - 1 pól + N - 350V - s diaľkovým prenosom",0.09]
["16329","ZVODIČ PRD1 25R 1P TYP I+II 350V SIGN",1,"ks",{"v":260.19,"d":"260.190"},"3606480060397",{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},{"v":4.5,"d":"4.50"},{"v":334,"d":"334.00"},"DE","8536303099","https://www.se.com/sk/sk/product/16329","PRD1 25r modulárny zvodič prepätia - 1 pól.- 350V - s diaľkovým prenosom",0.04]
["16317","ZVODIČ VÝMENNÝ MODUL C1 NEUTRAL - 35",1,"ks",{"v":185.22,"d":"185.220"},"3606480060380",{"v":11,"d":"11.00"},{"v":4.5,"d":"4.50"},{"v":8.3,"d":"8.30"},{"v":215,"d":"215.00"},"DE","85363090","https://www.se.com/sk/sk/product/16317","modul C1 Neutral-350 pre zvodiče prepätia PRD1 25R a PRD1 majstra",0.03]
["16315","ZVODIČ VÝMENNÝ MODUL C1 25 - 350V",1,"ks",{"v":185.22,"d":"185.220"},"3606480060366",{"v":11,"d":"11.00"},{"v":8,"d":"8.00"},{"v":4.4,"d":"4.40"},{"v":152,"d":"152.00"},"DE","85363090","https://www.se.com/sk/sk/product/16315","modul C1 25-350 pre zvodiče prepätia PRD1",0.02]
["16314","ZVODIČ VÝMENNÝ MODUL C1 MASTER - 350",1,"ks",{"v":299.87999999999994,"d":"299.880"},"3606480060359",{"v":10.8,"d":"10.80"},{"v":8.2,"d":"8.20"},{"v":4.4,"d":"4.40"},{"v":262,"d":"262.00"},"DE","85363090","https://www.se.com/sk/sk/product/16314","modul C1 Master-350 pre zvodiče prepätia PRD1 majstra",0.03]
["16092","STUP. PRE AMPÉRMETER AMP 96x96 6000 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160922",{"v":11,"d":"11.00"},{"v":7.5,"d":"7.50"},{"v":11,"d":"11.00"},{"v":12,"d":"12.00"},"IT","90309000","https://www.se.com/sk/sk/product/16092","ampérmeter dial PowerLogic - 1,3 V -prevod 6000 / 5 A",0]
["16091","STUP. PRE AMPÉRMETER AMP 96x96 5000 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160915",{"v":11,"d":"11.00"},{"v":7.5,"d":"7.50"},{"v":11,"d":"11.00"},{"v":200,"d":"200.00"},"IT","90309000","https://www.se.com/sk/sk/product/16091","ampérmeter dial PowerLogic - 1,3 V -prevod 5000 / 5 A",0]
["16090","STUP. PRE AMPÉRMETER AMP 96x96 4000 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160908",{"v":8.7,"d":"8.70"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":12,"d":"12.00"},"IT","90309000","https://www.se.com/sk/sk/product/16090","ampérmeter dial PowerLogic - 1,3 V - prevod 4000 / 5 A",0]
["16089","STUP. PRE AMPÉRMETER AMP 96x96 3000 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160892",{"v":11,"d":"11.00"},{"v":7.5,"d":"7.50"},{"v":11,"d":"11.00"},{"v":12,"d":"12.00"},"IT","90309000","https://www.se.com/sk/sk/product/16089","ampérmeter dial PowerLogic - 1,3 V - prevod 3000 / 5 A",0]
["16088","STUP. PRE AMPÉRMETER AMP 96x96 2500 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160885",{"v":11,"d":"11.00"},{"v":7.5,"d":"7.50"},{"v":11,"d":"11.00"},{"v":200,"d":"200.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16088","ampérmeter dial PowerLogic - 1,3 V - prevod 2500 / 5 A",0]
["16087","STUP. PRE AMPÉRMETER AMP 96x96 2000 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160878",{"v":11,"d":"11.00"},{"v":7.5,"d":"7.50"},{"v":11,"d":"11.00"},{"v":12,"d":"12.00"},"IT","90309000","https://www.se.com/sk/sk/product/16087","ampérmeter dial PowerLogic - 1,3 V -prevod 2000 / 5 A",0]
["16086","STUP. PRE AMPÉRMETER AMP 96x96 1500 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160861",{"v":11,"d":"11.00"},{"v":7.5,"d":"7.50"},{"v":11,"d":"11.00"},{"v":200,"d":"200.00"},"IT","90309000","https://www.se.com/sk/sk/product/16086","ampérmeter dial PowerLogic - 1,3 V - prevod 1500 / 5 A",0]
["16085","STUP. PRE AMPÉRMETER AMP 96x96 1250 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160854",{"v":8.6,"d":"8.60"},{"v":0.1,"d":"0.10"},{"v":8.6,"d":"8.60"},{"v":12,"d":"12.00"},"IT","9030900000","https://www.se.com/sk/sk/product/16085","ampérmeter dial PowerLogic - 1,3 V - prevod 1250 / 5 A",0]
["16084","STUP. PRE AMPÉRMETER AMP 96x96 1000 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160847",{"v":8.4,"d":"8.40"},{"v":0.1,"d":"0.10"},{"v":8.4,"d":"8.40"},{"v":13,"d":"13.00"},"IT","90309000","https://www.se.com/sk/sk/product/16084","ampérmeter dial PowerLogic - 1,3 V - prevod 1000 / 5 A",0]
["16083","STUPNICA PRE AMPÉRMETER AMP 96x96 600 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160830",{"v":8.5,"d":"8.50"},{"v":0.1,"d":"0.10"},{"v":8.3,"d":"8.30"},{"v":12,"d":"12.00"},"IT","90309000","https://www.se.com/sk/sk/product/16083","ampérmeter dial PowerLogic - 1,3 V - prevod 600 / 5 A",0]
["16082","STUP. PRE AMPÉRMETER AMP 96x96 400 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160823",{"v":8.5,"d":"8.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":13,"d":"13.00"},"IT","90309000","https://www.se.com/sk/sk/product/16082","ampérmeter dial PowerLogic - 1,3 V - prevod 400 / 5 A",0]
["16081","STUPNICA PRE AMPÉRMETER AMP 96x96 200 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160816",{"v":8.5,"d":"8.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":12,"d":"12.00"},"IT","9030900000","https://www.se.com/sk/sk/product/16081","ampérmeter dial PowerLogic - 1,3 V - prevod 200 / 5 A",0]
["16080","STUPNICA PRE AMPÉRMETER AMP 96x96 100 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160809",{"v":8,"d":"8.00"},{"v":0.1,"d":"0.10"},{"v":8,"d":"8.00"},{"v":12,"d":"12.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16080","ampérmeter dial PowerLogic - 1,3 V - prevod 100 / 5 A",0]
["16079","STUPNICA PRE AMPÉRMETER AMP 96x96 50 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160793",{"v":8,"d":"8.00"},{"v":0.1,"d":"0.10"},{"v":8,"d":"8.00"},{"v":15,"d":"15.00"},"IT","9030900000","https://www.se.com/sk/sk/product/16079","ampérmeter dial PowerLogic - 1,3 V - prevodr 50 / 5 A",0]
["16078","STUPNICA PRE MOTOR VÝV AMP 96x96 200 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160786",{"v":8.7,"d":"8.70"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":12,"d":"12.00"},"IT","9030900000","https://www.se.com/sk/sk/product/16078","ampérmeter dial PowerLogic - 3 V -prevod 200 / 5 A",0]
["16077","STUPNICA PRE MOTOR VÝV AMP 96x96 75 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160779",{"v":11,"d":"11.00"},{"v":7.5,"d":"7.50"},{"v":11,"d":"11.00"},{"v":200,"d":"200.00"},"IT","9030900000","https://www.se.com/sk/sk/product/16077","ampérmeter dial PowerLogic - 3 V - prevod 75 / 5 A",0]
["16076","STUPNICA PRE MOTOR VÝV AMP 96x96 30 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160762",{"v":10,"d":"10.00"},{"v":0.1,"d":"0.10"},{"v":10,"d":"10.00"},{"v":13,"d":"13.00"},"IT","9030900000","https://www.se.com/sk/sk/product/16076","ampérmeter vytočiť PowerLogic - 3 V - prevod 30 / 5 A",0]
["16075","VOLTMETER VLT 96x96 DO 500 V",1,"ks",{"v":50.273999999999994,"d":"50.274"},"3303430160755",{"v":11.5,"d":"11.50"},{"v":10.5,"d":"10.50"},{"v":11,"d":"11.00"},{"v":282,"d":"282.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16075","voltmeter VLT PowerLogic - 96 x 96 - feromagnetické - 0 .. 500 V",0.03]
["16074","AMPÉRMETER TELO PRÍSTR AMP 96x96 50 A",1,"ks",{"v":47.62799999999999,"d":"47.628"},"3303430160748",{"v":11.6,"d":"11.60"},{"v":11.4,"d":"11.40"},{"v":11.5,"d":"11.50"},{"v":256,"d":"256.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16074","ampérmeter AMP PowerLogic - 96 x 96 - feromagnetické - štandard. Nap.",0.03]
["16073","AMPÉRMETER PRE MOTOR VÝV AMP 96x96 30 A",1,"ks",{"v":71.88299999999998,"d":"71.883"},"3303430160731",{"v":13,"d":"13.00"},{"v":12,"d":"12.00"},{"v":12,"d":"12.00"},{"v":268,"d":"268.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16073","ampérmeter AMP PowerLogic - 96 x 96 - feromagnetické - pre motor. nap.",0.03]
["16061","VOLTMETER VLT 0-500 V",1,"ks",{"v":50.273999999999994,"d":"50.274"},"3303430160618",{"v":9.3,"d":"9.30"},{"v":7.8,"d":"7.80"},{"v":7.5,"d":"7.50"},{"v":163,"d":"163.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16061","modulárny analógový voltmeter IVLT - 0 .. 500 V",0.02]
["16060","VOLTMETER VLT 0-300 V",1,"ks",{"v":75.41099999999999,"d":"75.411"},"3303430160601",{"v":9.3,"d":"9.30"},{"v":7.8,"d":"7.80"},{"v":7.7,"d":"7.70"},{"v":165,"d":"165.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16060","modular analog voltmeter iVLT - 0..300 V",0.02]
["16045","STUPNICA PRE AMPÉRMETER AMP 0-2000A c",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160458",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16045","analógový ampérmeter stupnica - 0 .. 2000",0]
["16044","STUPNICA PRE AMPÉRMETER AMP 0-1500A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160441",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16044","analógový ampérmeter stupnica - 0 .. 1500",0]
["16043","STUPNICA PRE AMPÉRMETER AMP 0-1000A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160434",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16043","analógový ampérmeter stupnica - 0 .. 1000",0]
["16042","STUPNICA PRE AMPÉRMETER AMP 0-800A",5,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160427",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16042","analógový ampérmeter stupnica - 0 .. 800",0]
["16041","STUPNICA PRE AMPÉRMETER AMP 0-600A",5,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160410",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16041","analógový ampérmeter stupnica - 0 .. 600",0]
["16040","STUPNICA PRE AMPÉRMETER AMP 0-500A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160403",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16040","analógový ampérmeter stupnica - 0 .. 500",0]
["16039","STUPNICA PRE AMPÉRMETER AMP 0-400A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160397",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16039","analógový ampérmeter stupnica - 0 .. 400",0]
["16038","STUPNICA PRE AMPÉRMETER AMP 0-300A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160380",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16038","analógový ampérmeter stupnica - 0 .. 300",0]
["16037","STUPNICA PRE AMPÉRMETER AMP 0-250A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160373",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16037","analógový ampérmeter stupnica - 0 .. 250",0]
["16036","STUPNICA PRE AMPÉRMETER AMP 0-200A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160366",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16036","analógový ampérmeter stupnica - 0 .. 200",0]
["16035","STUPNICA PRE AMPÉRMETER AMP 0-150A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160359",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16035","analógový ampérmeter stupnica - 0 .. 150",0]
["16034","STUPNICA PRE AMPÉRMETER AMP 0-100A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160342",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16034","analógový ampérmeter stupnica - 0 .. 100",0]
["16033","STUPNICA PRE AMPÉRMETER AMP 0-75A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160335",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16033","analógový ampérmeter stupnica - 0 .. 75",0]
["16032","STUPNICA PRE AMPÉRMETER AMP 0-50A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160328",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16032","analógový ampérmeter stupnica - 0 .. 50",0]
["16031","STUPNICA PRE AMPÉRMETER AMP 0-5A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160311",{"v":13.5,"d":"13.50"},{"v":0.1,"d":"0.10"},{"v":8.5,"d":"8.50"},{"v":6,"d":"6.00"},"IT","85389099","https://www.se.com/sk/sk/product/16031","analógový ampérmeter stupnica - 0 .. 5",0]
["16030","AMPÉRMETER TELO PRÍSTROJA AMP 5A",1,"ks",{"v":47.62799999999999,"d":"47.628"},"3303430160304",{"v":9.3,"d":"9.30"},{"v":7.5,"d":"7.50"},{"v":7.7,"d":"7.70"},{"v":154,"d":"154.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16030","modulárny analógový ampérmeter bez stupnice iAMP - 0. .. 2000 A",0.02]
["16029","AMPÉRMETER AMP 0-30A",1,"ks",{"v":50.273999999999994,"d":"50.274"},"3303430160298",{"v":9.2,"d":"9.20"},{"v":7.8,"d":"7.80"},{"v":7.5,"d":"7.50"},{"v":163,"d":"163.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16029","modulárny analógový ampérmeter iAMP - 0 .. 30",0.02]
["16019","STUPNICA PRE AMPÉRMETER AMP 72x72 2000A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160199",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16019","ampérmeter dial PowerLogic - 1,5 V - CT pomere 2000/5 A",0]
["16018","OTOČNÝ PREPÍNAČ CMV ( 7 POZ ) 48x48",1,"ks",64.827,"3303430160182",{"v":7.3,"d":"7.30"},{"v":10.3,"d":"10.30"},{"v":7.3,"d":"7.30"},{"v":122,"d":"122.00"},"AT","8536508090","https://www.se.com/sk/sk/product/16018","cam voltmeter prepínač CMV - 3L a 3L - N - 45 ° - pre Ø 22,3 mm",0]
["16017","OTOČNÝ PREPÍNAČ CMA ( 4 POZ ) 48x48",1,"ks",64.827,"3303430160175",{"v":5.5,"d":"5.50"},{"v":10.5,"d":"10.50"},{"v":5.5,"d":"5.50"},{"v":122,"d":"122.00"},"AT","85365080","https://www.se.com/sk/sk/product/16017","cam ampérmeter Prepínač CMA - 3L - N - 90 ° - 20 A - pre Ø 22,3 mm",0]
["16016","STUP. PRE AMPÉRMETER AMP 72x72 1500 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160168",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"IT","85389099","https://www.se.com/sk/sk/product/16016","analógový ampérmeter stupnica - 0 .. 1500",0]
["16015","STUP. PRE AMPÉRMETER AMP 72x72 1250 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160151",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"IT","85389099","https://www.se.com/sk/sk/product/16015","analógový ampérmeter stupnica - 0 .. 1250",0]
["16014","STUP. PRE AMPÉRMETER AMP 72x72 1000 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160144",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"IT","85389099","https://www.se.com/sk/sk/product/16014","analógový ampérmeter stupnica - 0 .. 1000",0]
["16013","STUPNICA PRE AMPÉRMETER AMP 72x72 600 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160137",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"IT","85389099","https://www.se.com/sk/sk/product/16013","analógový ampérmeter stupnica - 0 .. 600",0]
["16012","STUP. PRE AMPÉRMETER AMP 72x72 400 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160120",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16012","analógový ampérmeter stupnica - 0 .. 400",0]
["16011","STUPNICA PRE AMPÉRMETER AMP 72x72 200 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160113",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16011","analógový ampérmeter stupnica - 0 .. 200",0]
["16010","STUPNICA PRE AMPÉRMETER AMP 72x72 100 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160106",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},"IT","85389099","https://www.se.com/sk/sk/product/16010","analógový ampérmeter stupnica - 0 .. 100",0]
["16009","STUPNICA PRE AMPÉRMETER AMP 72x72 50 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160090",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":7,"d":"7.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16009","analógový ampérmeter stupnica - 0 .. 50",0]
["16008","STUPNICA PRE MOTOR VÝV AMP 72x72 200 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160083",{"v":8,"d":"8.00"},{"v":0.1,"d":"0.10"},{"v":6.2,"d":"6.20"},{"v":8,"d":"8.00"},"IT","85389099","https://www.se.com/sk/sk/product/16008","analógový ampérmeter stupnica - 0 .. 200",0]
["16007","STUPNICA PRE MOTOR VÝV AMP 72x72 75 A",10,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160076",{"v":8,"d":"8.00"},{"v":0.1,"d":"0.10"},{"v":6.2,"d":"6.20"},{"v":8,"d":"8.00"},"IT","85389099","https://www.se.com/sk/sk/product/16007","analógový ampérmeter stupnica - 0 .. 75",0]
["16006","STUPNICA PRE MOTOR VÝV AMP 72x72 30 A",1,"ks",{"v":3.5720999999999994,"d":"3.572"},"3303430160069",{"v":7.5,"d":"7.50"},{"v":0.2,"d":"0.20"},{"v":8,"d":"8.00"},{"v":8,"d":"8.00"},"IT","85389099","https://www.se.com/sk/sk/product/16006","analógový ampérmeter stupnica - 0 .. 30",0]
["16005","VOLTMETER VLT DO 500 V",1,"ks",{"v":50.273999999999994,"d":"50.274"},"3303430160052",{"v":10,"d":"10.00"},{"v":8.5,"d":"8.50"},{"v":9,"d":"9.00"},{"v":215,"d":"215.00"},"IT","9030337000","https://www.se.com/sk/sk/product/16005","analógový voltmeter VLT - 72 x 72 mm - 0 .. 500 V",0.03]
["16004","AMPÉRMETER TELO PRÍSTR AMP 72x72 50 A",1,"ks",{"v":47.62799999999999,"d":"47.628"},"3303430160045",{"v":9.5,"d":"9.50"},{"v":10,"d":"10.00"},{"v":8.5,"d":"8.50"},{"v":193,"d":"193.00"},"IT","9030332090","https://www.se.com/sk/sk/product/16004","analógový ampérmeter AMP - 1,3 V bez ciferníku - 72 x 72 mm",0.02]
["16003","AMPÉRMETER PRE MOTOR VÝV AMP 72x72 30 A",1,"ks",{"v":47.62799999999999,"d":"47.628"},"3303430160038",{"v":9,"d":"9.00"},{"v":10,"d":"10.00"},{"v":8.5,"d":"8.50"},{"v":191,"d":"191.00"},"IT","9030332090","https://www.se.com/sk/sk/product/16003","analógový ampérmeter AMP - 3 V bez ciferníku - 72 x 72 mm",0.02]
["15870","TERMOSTAT TH",1,"ks",{"v":25.136999999999997,"d":"25.137"},"3303430158707",{"v":8,"d":"8.00"},{"v":3.5,"d":"3.50"},{"v":8,"d":"8.00"},{"v":86,"d":"86.00"},"DE","90321020","https://www.se.com/sk/sk/product/15870","Multi9 - TH - wall mounted thermostat",0]
["15835","NENASTAVITEĽNÝ SNÍMAČ",1,"ks",{"v":30.869999999999997,"d":"30.870"},"3303430158356",{"v":9.5,"d":"9.50"},{"v":4.3,"d":"4.30"},{"v":7.5,"d":"7.50"},{"v":67,"d":"67.00"},"DE","90259000","https://www.se.com/sk/sk/product/15835","Acti 9 - teplotný snímač pre THP1 a THP2 - nást.montáž - vnútorná",0.01]
["15669","ZAISŤ.DIEL VISIAC.ZÁMKU PRE STI 2KS",1,"ks",{"v":15.434999999999999,"d":"15.435"},"3303430156697",{"v":9.5,"d":"9.50"},{"v":1.5,"d":"1.50"},{"v":9,"d":"9.00"},{"v":7,"d":"7.00"},"BE","85389099","https://www.se.com/sk/sk/product/15669","padlocking device STI - set of 2",0]
["15668","FUSE INDICATOR SFT/STI",1,"ks",{"v":5.2479,"d":"5.248"},"3303430156680",{"v":6.5,"d":"6.50"},{"v":2,"d":"2.00"},{"v":4.5,"d":"4.50"},{"v":5,"d":"5.00"},"BE","8536508090","https://www.se.com/sk/sk/product/15668","signálka pre SFT/STI - 230 V AC 50/60 Hz",0]
["15608","ČÍTAČ PREVÁDZ. HODÍN 48x48 230VAC/50HZ",1,"ks",26.019,"3303430156086",{"v":6.3,"d":"6.30"},{"v":5.6,"d":"5.60"},{"v":6.3,"d":"6.30"},{"v":60,"d":"60.00"},"DE","9029100090","https://www.se.com/sk/sk/product/15608","počítadlo prevádz. hodín - mech. 7 digit. displej - 230 V AC 50 Hz",0.01]
["15443","ČÍTAČ IMPULZOV CI",1,"ks",{"v":51.596999999999994,"d":"51.597"},"3303430154433",{"v":9,"d":"9.00"},{"v":4,"d":"4.00"},{"v":7.4,"d":"7.40"},{"v":93,"d":"93.00"},"DE","90291000","https://www.se.com/sk/sk/product/15443","počítadlo modulárny impulzný tu - 230",0.01]
["15440","ČÍTAČ PREVÁDZ HODÍN CH 220V/240V 50HZ",1,"ks",{"v":51.596999999999994,"d":"51.597"},"3303430154402",{"v":9,"d":"9.00"},{"v":7.6,"d":"7.60"},{"v":4,"d":"4.00"},{"v":94,"d":"94.00"},"DE","9029100090","https://www.se.com/sk/sk/product/15440","Modulárne počítadlo hodín Ich - 230",0.01]
["15363","SCHODISKOVÝ AUTOMAT MIN 1-7 MIN 240V",1,"ks",45.864,"3303430153634",{"v":9.9,"d":"9.90"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":82,"d":"82.00"},"DE","9107000090","https://www.se.com/sk/sk/product/15363","Acti 9 - MIN - elektromechanický časovač - nastaviteľný 1-7 minút",0.01]
["15336","SPÍN HODINY IH 24H ZÁLOHA 1KAN 16A 18MM",1,"ks",{"v":45.422999999999995,"d":"45.423"},"3303430153368",{"v":10,"d":"10.00"},{"v":2.4,"d":"2.40"},{"v":6.8,"d":"6.80"},{"v":87,"d":"87.00"},"DE","91070000","https://www.se.com/sk/sk/product/15336","Acti 9 - IH - mechanický časový spínač - 24 h - 100 h Pamäť",0.01]
["15335","SPÍN HODINY IH 24H BEZ ZÁL 1KAN 16A",1,"ks",{"v":45.422999999999995,"d":"45.423"},"3303430153351",{"v":9.9,"d":"9.90"},{"v":2.1,"d":"2.10"},{"v":7.1,"d":"7.10"},{"v":82,"d":"82.00"},"DE","9107000090","https://www.se.com/sk/sk/product/15335","Acti 9 - IH - mechanický časový spínač - 24 h - bez pamäti",0.01]
["15331","SPÍN HODINY IH PROGRAM 7D 1KAN 18MM",1,"ks",{"v":63.944999999999986,"d":"63.945"},"3303430153313",{"v":10,"d":"10.00"},{"v":2,"d":"2.00"},{"v":7,"d":"7.00"},{"v":89,"d":"89.00"},"DE","91070000","https://www.se.com/sk/sk/product/15331","Acti 9 - IHH - mechanický časový spínač - 7 dní - 100 h Pamäť",0.01]
["15324","ZÁSUVKA PC 2P S KOLÍKOM ŽLTÁ",1,"ks",27.342,"3303430153245",{"v":22.7,"d":"22.70"},{"v":6.9,"d":"6.90"},{"v":8.5,"d":"8.50"},{"v":101,"d":"101.00"},"BE","8536699099","https://www.se.com/sk/sk/product/15324","zás.PC 2P s kolíkom žltá - 16A - 250VAC - NFC 61314",0]
["15209","DIGITÁLNY AMPÉRMETER AMP 50-6000/5A TI",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3303430152095",{"v":9.2,"d":"9.20"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":180,"d":"180.00"},"IT","9030337000","https://www.se.com/sk/sk/product/15209","modulárny digitálny ampérmeter iAMP - 230 - 5. .. 5000A",0.02]
["15202","DIGITÁLNY AMPÉRMETER AMP 0/10A",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3303430152026",{"v":9.2,"d":"9.20"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":187,"d":"187.00"},"IT","9030337000","https://www.se.com/sk/sk/product/15202","modulárny digitálny ampérmeter iAMP - 230 - 0 .. 10A",0.02]
["15201","DIGITÁLNY VOLTMETER VLT 0/600V",1,"ks",{"v":127.88999999999997,"d":"127.890"},"3303430152019",{"v":9.2,"d":"9.20"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":178,"d":"178.00"},"IT","9030337000","https://www.se.com/sk/sk/product/15201","modulárny digitálny voltmeter IVLT - 230 - 0 .. 600V",0.02]
["15126","OTOČNÝ PREPÍNAČ CMA",1,"ks",{"v":74.96999999999998,"d":"74.970"},"3303430151265",{"v":7.5,"d":"7.50"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":77,"d":"77.00"},"AT","85365080","https://www.se.com/sk/sk/product/15126","prepínač ampérmetra ICMA - 10",0]
["15125","OTOČNÝ PREPÍNAČ CMV",1,"ks",{"v":74.96999999999998,"d":"74.970"},"3303430151258",{"v":8,"d":"8.00"},{"v":4,"d":"4.00"},{"v":7.5,"d":"7.50"},{"v":76,"d":"76.00"},"AT","8536508090","https://www.se.com/sk/sk/product/15125","prepínač voltmetra iCMV - 10",0]
["14979","ZBERNICA 125A 14 OTVOROV",5,"ks",{"v":8.334899999999998,"d":"8.335"},"3303430149798",{"v":13,"d":"13.00"},{"v":3.5,"d":"3.50"},{"v":11.5,"d":"11.50"},{"v":64,"d":"64.00"},"FR","8536901000","https://www.se.com/sk/sk/product/14979","svorkovnica 125A 14 otvorov",0]
["14977","ZBERNICA 125A 10 OTVOROV",5,"ks",{"v":7.0119,"d":"7.012"},"3303430149774",{"v":12,"d":"12.00"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":50,"d":"50.00"},"FR","85369010","https://www.se.com/sk/sk/product/14977","svorkovnica 80A 10 otvorov",0]
["14976","ZBERNICA 125A 6 OTVOROV",5,"ks",5.733,"3303430149767",{"v":7,"d":"7.00"},{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":35,"d":"35.00"},"FR","8536901000","https://www.se.com/sk/sk/product/14976","svorkovnica 80A 6 otvorov",0]
["14965","ZBERNICA 125A 14 OTVOROV",20,"ks",{"v":5.512499999999999,"d":"5.513"},"3303430149651",{"v":10,"d":"10.00"},{"v":1.5,"d":"1.50"},{"v":0.7,"d":"0.70"},{"v":53,"d":"53.00"},"FR","8536901000","https://www.se.com/sk/sk/product/14965","SVORKOVNICA 125A 14 OTVOROV",0]
["14964","ZBERNICA 80A 11 OTVOROV",20,"ks",{"v":3.4397999999999995,"d":"3.440"},"3303430149644",{"v":7.4,"d":"7.40"},{"v":0.6,"d":"0.60"},{"v":1.5,"d":"1.50"},{"v":10,"d":"10.00"},"FR","8536901000","https://www.se.com/sk/sk/product/14964","SVORKOVNICA 125A 10 OTVOROV",0]
["14818","KRYT VOĽNÝCH VÝVODOV LIŠTY 40KS",1,"ks",{"v":7.2323999999999975,"d":"7.232"},"3303430148180",{"v":8,"d":"8.00"},{"v":3,"d":"3.00"},{"v":11.5,"d":"11.50"},{"v":30,"d":"30.00"},"DE","85472000","https://www.se.com/sk/sk/product/14818","kryty vývodov pre hrebeňovú lištu C120, NG125",0]
["14814","HREB.PREP.LIŠTA 4P 54 VÝV C120,NG125",1,"ks",{"v":55.124999999999986,"d":"55.125"},"3303430148142",{"v":37,"d":"37.00"},{"v":2.5,"d":"2.50"},{"v":3.5,"d":"3.50"},{"v":281.9,"d":"281.90"},"DE","85369010","https://www.se.com/sk/sk/product/14814","hrebeňová lišta - 4P - 63 A - L = 432 mm, 16 x 27 mm",0.03]
["14813","HREB.PREP.LIŠTA 3P 54 VÝV C120,NG125",1,"ks",44.541,"3303430148135",{"v":42,"d":"42.00"},{"v":1.7,"d":"1.70"},{"v":5,"d":"5.00"},{"v":218,"d":"218.00"},"DE","85369010","https://www.se.com/sk/sk/product/14813","hrebeňová lišta Domae - 3P - 63 A - L = 405 mm, 15x27 mm",0.03]
["14812","HREB.PREP.LIŠTA 2P 54 VÝV C120,NG125",1,"ks",{"v":41.01299999999999,"d":"41.013"},"3303430148128",{"v":44,"d":"44.00"},{"v":1.7,"d":"1.70"},{"v":4,"d":"4.00"},{"v":194,"d":"194.00"},"DE","85369010","https://www.se.com/sk/sk/product/14812","hrebeňová lišta - 2P - 63 A - L = 432 mm, 16 x 27 mm",0.02]
["14811","HREB.PREP.LIŠTA 1P 54 VÝV C120,NG125",1,"ks",{"v":20.285999999999998,"d":"20.286"},"3303430148111",{"v":48,"d":"48.00"},{"v":2,"d":"2.00"},{"v":6,"d":"6.00"},{"v":105,"d":"105.00"},"DE","8536909500","https://www.se.com/sk/sk/product/14811","hrebeňová lišta - 1P - 63 A - L = 432 mm, 16 x 27 mm",0.01]
["14211","DRŽIAK SYMETRICKEJ LIŠTY",1,"ks",{"v":26.459999999999994,"d":"26.460"},"3303430142119",{"v":18.5,"d":"18.50"},{"v":1.7,"d":"1.70"},{"v":10.5,"d":"10.50"},{"v":240,"d":"240.00"},"FR","8538909999","https://www.se.com/sk/sk/product/14211","DIN rail with support - through door mounting - 10 modules",0]
["14210","ZÁVESNÝ PRIEHĽADNÝ KRYT",1,"ks",{"v":68.79599999999999,"d":"68.796"},"3303430142102",{"v":25.5,"d":"25.50"},{"v":6,"d":"6.00"},{"v":14,"d":"14.00"},{"v":391,"d":"391.00"},"FR","8538909999","https://www.se.com/sk/sk/product/14210","Multi9 HINGED TRANSPARENT COVER",0]
["13994","ROZVODNICA 4 ROZŠ. ROZHRANIA IP65 KAEDRA",1,"ks",44.982,"3303430139942",{"v":62,"d":"62.00"},{"v":13.5,"d":"13.50"},{"v":15.8,"d":"15.80"},{"v":1595,"d":"1,595.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13994","Kaedra - rozhranní - 138x610 mm - 4 otvory",0]
["13993","ROZVODNICA 3 ROZŠ. ROZHRANIA IP65 KAEDRA",1,"ks",{"v":27.915299999999995,"d":"27.915"},"3303430139935",{"v":47,"d":"47.00"},{"v":15.5,"d":"15.50"},{"v":17,"d":"17.00"},{"v":1310,"d":"1,310.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13993","Kaedra - rozhranní - 138x460 mm - 3 otvory",""]
["13992","ROZVODNICA 3X12 MOD. 4 ROZŠ. IP65 KAEDRA",1,"ks",{"v":110.24999999999997,"d":"110.250"},"3303430139928",{"v":62,"d":"62.00"},{"v":16.5,"d":"16.50"},{"v":46.5,"d":"46.50"},{"v":5390,"d":"5,390.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13992","Enclosure for modular device with interface, Mureva Enclosure, 3x12 mod, 5 open., (W)448mm x(H)460mm, earth term block",0]
["13991","Mureva Encl. w/int. IP65 2x12M+3op ETB",1,"ks",{"v":81.5409,"d":"81.541"},"3303430139911",{"v":47,"d":"47.00"},{"v":17.5,"d":"17.50"},{"v":46.8,"d":"46.80"},{"v":3975,"d":"3,975.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13991","Mureva Encl. w/int. IP65 2x12M+3op ETB",""]
["13987","ROZVODNICA 4X18 MODULOV IP65 KAEDRA",1,"ks",{"v":198.44999999999996,"d":"198.450"},"3303430139874",{"v":85,"d":"85.00"},{"v":17,"d":"17.00"},{"v":47,"d":"47.00"},{"v":7530,"d":"7,530.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13987","Enclosure for modular device, Mureva Enclosure, 4x18 modules, earth terminal blocks",0]
["13986","ROZVODNICA 3X18 MODULOV IP65 KAEDRA",1,"ks",{"v":145.52999999999997,"d":"145.530"},"3303430139867",{"v":62,"d":"62.00"},{"v":17,"d":"17.00"},{"v":46.5,"d":"46.50"},{"v":5705,"d":"5,705.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13986","Enclosure for modular device, Mureva Enclosure, 3x18 modules, earth terminal blocks",0]
["13985","ROZVODNICA 3X12 MODULOV IP65 KAEDRA",1,"ks",{"v":110.24999999999997,"d":"110.250"},"3303430139850",{"v":62,"d":"62.00"},{"v":16.8,"d":"16.80"},{"v":35.5,"d":"35.50"},{"v":4375,"d":"4,375.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13985","Enclosure for modular device, Mureva Enclosure, 3x12 modules, earth terminal block",0]
["13984","ROZVODNICA 2X18 MODULOV IP65 KAEDRA",1,"ks",{"v":97.01999999999998,"d":"97.020"},"3303430139843",{"v":47,"d":"47.00"},{"v":17,"d":"17.00"},{"v":46.8,"d":"46.80"},{"v":4190,"d":"4,190.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13984","Kaedra rozvodnica pre povrch. montáž-IP 65-2x18 mod.-priehledné dvere",0]
["13983","ROZVODNICA 2X12 MODULOV IP65 KAEDRA",1,"ks",{"v":78.05699999999999,"d":"78.057"},"3303430139836",{"v":47.5,"d":"47.50"},{"v":17,"d":"17.00"},{"v":36,"d":"36.00"},{"v":3316,"d":"3,316.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13983","modulárna Kaedra - 2 x 12 modulov - 1+1 svorkovnice",0]
["13982","ROZVODNICA 1X18 MODULOV IP65 KAEDRA",1,"ks",{"v":70.11899999999999,"d":"70.119"},"3303430139829",{"v":46.8,"d":"46.80"},{"v":17,"d":"17.00"},{"v":29.5,"d":"29.50"},{"v":2510,"d":"2,510.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13982","Mureva rozvodnice IP65 1x18M ETB",0]
["13981","ROZVODNICA 1X12 MODULOV IP65 KAEDRA",1,"ks",{"v":52.91999999999999,"d":"52.920"},"3303430139812",{"v":28.5,"d":"28.50"},{"v":16.5,"d":"16.50"},{"v":36,"d":"36.00"},{"v":2025,"d":"2,025.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13981","Enclosure for modular device, Mureva Enclosure, 1x12 modules, earth terminal block",0]
["13979","MINI ROZVODNICA 12 MODULOV IP65 KAEDRA",1,"ks",{"v":39.68999999999999,"d":"39.690"},"3303430139799",{"v":26.6,"d":"26.60"},{"v":11.4,"d":"11.40"},{"v":20,"d":"20.00"},{"v":810,"d":"810.00"},"IT","9403700000","https://www.se.com/sk/sk/product/13979","Mureva Mini rozvodnice IP65 12M",0]
["13978","MINI ROZVODNICA 8 MODULOV IP65 KAEDRA",1,"ks",{"v":24.254999999999995,"d":"24.255"},"3303430139782",{"v":19.6,"d":"19.60"},{"v":11,"d":"11.00"},{"v":19.4,"d":"19.40"},{"v":630,"d":"630.00"},"IT","9403700000","https://www.se.com/sk/sk/product/13978","Mureva Mini rozvodnice IP65 8M",0]
["13977","MINI ROZVODNICA 6 MODULOV IP65 KAEDRA",1,"ks",{"v":24.254999999999995,"d":"24.255"},"3303430139775",{"v":20,"d":"20.00"},11.15,{"v":16,"d":"16.00"},{"v":515,"d":"515.00"},"IT","9403700000","https://www.se.com/sk/sk/product/13977","Mini enclosure for modular device, Mureva Enclosure, 1x6 modules, without terminal block",0]
["13976","MINI ROZVODNICA 4 MODULY IP65 KAEDRA",1,"ks",{"v":20.726999999999997,"d":"20.727"},"3303430139768",{"v":12.2,"d":"12.20"},{"v":11.2,"d":"11.20"},{"v":20,"d":"20.00"},{"v":445,"d":"445.00"},"IT","9403700000","https://www.se.com/sk/sk/product/13976","Mureva Mini rozvodnice IP65 4M",0]
["13975","MINI ROZVODNICA 2/3 MODULY IP65 KAEDRA",1,"ks",{"v":17.639999999999997,"d":"17.640"},"3303430139751",{"v":10,"d":"10.00"},{"v":8,"d":"8.00"},{"v":15,"d":"15.00"},{"v":255,"d":"255.00"},"IT","9403700000","https://www.se.com/sk/sk/product/13975","Mureva Mini rozvodnice IP65 3M",0]
["13950","ZÁMOK S ŠTVORCOVOU VLOŽKOU",1,"ks",{"v":20.285999999999998,"d":"20.286"},"3303430139508",{"v":11,"d":"11.00"},{"v":4,"d":"4.00"},{"v":8,"d":"8.00"},{"v":35,"d":"35.00"},"IT","8301600090","https://www.se.com/sk/sk/product/13950","zámok - štvorcový kľúč",0]
["13948","ZÁMOK S KĽÚČOM KAEDRA",1,"ks",{"v":19.403999999999996,"d":"19.404"},"3303430139485",{"v":10.3,"d":"10.30"},{"v":4,"d":"4.00"},{"v":6.9,"d":"6.90"},{"v":48,"d":"48.00"},"IT","8301300000","https://www.se.com/sk/sk/product/13948","kľúč so zámkom - Eurolocks n° 850",0]
["13945","Krycia doska 18 modulov",1,"ks",{"v":6.394499999999999,"d":"6.395"},"3303430139454",{"v":35,"d":"35.00"},{"v":0.5,"d":"0.50"},{"v":15,"d":"15.00"},{"v":214,"d":"214.00"},"IT","39269097","https://www.se.com/sk/sk/product/13945","plný čelní panel - 18 mod.",0]
["13941","Perforovaná montážna doska 150mm Kaedra",1,"ks",{"v":23.813999999999997,"d":"23.814"},"3303430139416",{"v":24.5,"d":"24.50"},{"v":0.2,"d":"0.20"},{"v":14,"d":"14.00"},{"v":225,"d":"225.00"},"IT","85389099","https://www.se.com/sk/sk/product/13941","perforovaná doska 100x250mm",0]
["13940","ZÁSLEPKA, SADA 10KS X 5MOD.",1,"ks",{"v":4.2776999999999985,"d":"4.278"},"3303430139409",{"v":6,"d":"6.00"},{"v":4.6,"d":"4.60"},{"v":9,"d":"9.00"},{"v":85,"d":"85.00"},"IT","85389099","https://www.se.com/sk/sk/product/13940","záslepka - sada 10x5mod.",0]
["13935","FIXAČNÉ OKÁ NA STENU (SADA 4KS)",1,"ks",{"v":4.586399999999999,"d":"4.586"},"3303430139355",{"v":9,"d":"9.00"},{"v":1,"d":"1.00"},{"v":10.5,"d":"10.50"},{"v":39,"d":"39.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13935","patky na stenu - sada 4",0]
["13934","PREPOJOVACIA SADA, 2 PRIECH., 4 MATICE",1,"ks",{"v":10.142999999999999,"d":"10.143"},"3303430139348",{"v":5,"d":"5.00"},{"v":6,"d":"6.00"},{"v":10,"d":"10.00"},{"v":36,"d":"36.00"},"IT","7326909890","https://www.se.com/sk/sk/product/13934","spojovacia sada - 2 púzdra s maticami a spojmi",0]
["13599","KAEDRA DRŽIAK SVORKOVNICE 12M",1,"ks",{"v":5.194979999999999,"d":"5.195"},"3303430135999",{"v":24,"d":"24.00"},{"v":1,"d":"1.00"},{"v":8,"d":"8.00"},{"v":50,"d":"50.00"},"IT","7326909890","https://www.se.com/sk/sk/product/13599","Kaedra držiak svorkovnice - 12 mod.",""]
["13598","KAEDRA DRŽIAK SVORKOVNICE 18 M",1,"ks",{"v":4.903919999999999,"d":"4.904"},"3303430135982",{"v":41,"d":"41.00"},{"v":2,"d":"2.00"},{"v":1.5,"d":"1.50"},{"v":90,"d":"90.00"},"IT","8538909999","https://www.se.com/sk/sk/product/13598","Kaedra držiakk svorkovnice - 18 mod.",""]
["13597","KAEDRA DRŽIAK SVORKOVNICE 12 M",1,"ks",{"v":4.057199999999999,"d":"4.057"},"3303430135975",{"v":30,"d":"30.00"},{"v":3,"d":"3.00"},{"v":2,"d":"2.00"},{"v":68,"d":"68.00"},"IT","7326909890","https://www.se.com/sk/sk/product/13597","Kaedra držiak svorkovnice - 12 mod.",""]
["13595","Terminal block supp. for mini enclosure",1,"ks",{"v":5.5565999999999995,"d":"5.557"},"3303430135951",{"v":35,"d":"35.00"},{"v":0.2,"d":"0.20"},{"v":1.1,"d":"1.10"},{"v":75,"d":"75.00"},"IT","85389099","https://www.se.com/sk/sk/product/13595","Kaedra držiak svorkovnice - 18 mod.",0]
["13587","PRAGMA C,MINI,D KRYT SVORK MODRÝ 202MM",5,"ks",{"v":4.895099999999999,"d":"4.895"},"3303430135876",{"v":2,"d":"2.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":12,"d":"12.00"},"IT","85472000","https://www.se.com/sk/sk/product/13587","IP2 kryt pre 16 - 22 a 32 otvorov svorkovnice - modrá",0]
["13586","PRAGMA C,MINI,D KRYT SVORK MODRÝ 85MM",5,"ks",{"v":1.2348,"d":"1.235"},"3303430135869",{"v":5.9,"d":"5.90"},{"v":1.4,"d":"1.40"},{"v":2,"d":"2.00"},{"v":49,"d":"49.00"},"IT","85472000","https://www.se.com/sk/sk/product/13586","IP2 kryt pre 8 otvorov svorkovnice - modrá",0]
["13585","PRAGMA C,D KRYT SVORK ČERVENÝ 202MM",5,"ks",{"v":8.4231,"d":"8.423"},"3303430135852",{"v":1,"d":"1.00"},{"v":2,"d":"2.00"},{"v":20,"d":"20.00"},{"v":10,"d":"10.00"},"IT","85472000","https://www.se.com/sk/sk/product/13585","IP2 kryt pre 16 - 22 a 32 otvorov svorkovnice - červená",0]
["13583","PRAGMA C,MINI,D KRYT SVORK ZELENÝ 202MM",5,"ks",{"v":3.7043999999999997,"d":"3.704"},"3303430135838",{"v":19.8,"d":"19.80"},{"v":1.7,"d":"1.70"},{"v":1.8,"d":"1.80"},{"v":13,"d":"13.00"},"IT","85472000","https://www.se.com/sk/sk/product/13583","IP2 kryt pre 16 - 22 a 32 otvorov svorkovnice - zelená",0]
["13582","PRAGMA C,MINI,D KRYT SVORK ZELENÝ 85MM",5,"ks",{"v":1.2348,"d":"1.235"},"3303430135821",{"v":2,"d":"2.00"},{"v":3,"d":"3.00"},{"v":10,"d":"10.00"},{"v":4,"d":"4.00"},"IT","8547200090","https://www.se.com/sk/sk/product/13582","IP2 kryt pre 8 otvorov svorkovnice - zelená",0]
["13579","PRAGMA C,MINI,D SVORKOVNICA 32 OTVOROV",1,"ks",{"v":14.552999999999997,"d":"14.553"},"3303430135791",{"v":24,"d":"24.00"},{"v":3,"d":"3.00"},{"v":3,"d":"3.00"},{"v":97,"d":"97.00"},"IT","85369010","https://www.se.com/sk/sk/product/13579","distribution terminal block - 80 A - 32 holes",0]
["13577","PRAGMA C,MINI,D SVORKOVNICA 16 OTVOROV",1,"ks",{"v":9.260999999999997,"d":"9.261"},"3303430135777",{"v":2,"d":"2.00"},{"v":1.5,"d":"1.50"},{"v":21,"d":"21.00"},{"v":58,"d":"58.00"},"IT","85369010","https://www.se.com/sk/sk/product/13577","distribution terminal block - 80 A - 16 holes",0]
["13576","PRAGMA C,MINI,D SVORKOVNICA 8 OTVOROV",5,"ks",{"v":5.203799999999999,"d":"5.204"},"3303430135760",{"v":10.5,"d":"10.50"},{"v":2.5,"d":"2.50"},{"v":10.5,"d":"10.50"},{"v":28,"d":"28.00"},"IT","85369010","https://www.se.com/sk/sk/product/13576","distrib. svorkovnica - 80 A - 8 otvorov",0]
["13575","PRAGMA C,MINI,D SVORKOVNICA 4 OTVORY",1,"ks",{"v":4.674599999999999,"d":"4.675"},"3303430135753",{"v":8,"d":"8.00"},{"v":1,"d":"1.00"},{"v":7,"d":"7.00"},{"v":16,"d":"16.00"},"IT","85369010","https://www.se.com/sk/sk/product/13575","distribution terminal block - 80 A - 4 holes",0]
["13444","MINIKAEDRA IP65 PRIEHĽ DVERE POVRCH 12M",1,"ks",{"v":37.925999999999995,"d":"37.926"},"3303430134442",{"v":26.5,"d":"26.50"},{"v":11,"d":"11.00"},{"v":20,"d":"20.00"},{"v":935,"d":"935.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13444","Mureva Mini rozvodnice IP65 12M E/N TB",0]
["13443","MINI KAEDRA IP65 PRIEHĽ DVERE POVRCH 8M",1,"ks",{"v":28.223999999999997,"d":"28.224"},"3303430134435",{"v":26,"d":"26.00"},{"v":6,"d":"6.00"},{"v":24.5,"d":"24.50"},{"v":740,"d":"740.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13443","Mureva Mini rozvodnice IP65 8M E/N TB",0]
["13442","MINI KAEDRA IP65 PRIEHĽ DVERE POVRCH 6M",1,"ks",22.932,"3303430134428",{"v":20,"d":"20.00"},{"v":11,"d":"11.00"},{"v":16,"d":"16.00"},{"v":590,"d":"590.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13442","mini Kaedra - pre modulárne prístroje - 6 mod. - svorkovnice",0]
["13441","MINI KAEDRA IP65 PRIEHĽ DVERE POVRCH 4M",1,"ks",{"v":19.844999999999995,"d":"19.845"},"3303430134411",{"v":20,"d":"20.00"},{"v":12,"d":"12.00"},{"v":12,"d":"12.00"},{"v":515,"d":"515.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13441","Mureva Mini rozvodnice IP65 4M E/N TB",0]
["13440","KAEDRA ROZVODNICA IP65 36MOD. 4 ZÁS.",1,"ks",{"v":114.66,"d":"114.660"},"3303430134404",{"v":17,"d":"17.00"},{"v":62,"d":"62.00"},{"v":47,"d":"47.00"},{"v":5635,"d":"5,635.00"},"","8538100000","https://www.se.com/sk/sk/product/13440","Kaedra skrina rozhranná - 3x12 mod.",0]
["13439","KAEDRA ROZVODNICA IP65 24MOD. 3 ZÁS.",1,"ks",{"v":145.52999999999997,"d":"145.530"},"3303430134398",{"v":47.5,"d":"47.50"},{"v":18,"d":"18.00"},{"v":47,"d":"47.00"},{"v":4250,"d":"4,250.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13439","Mureva rozv. w/int IP65 2x12M+3op E/N TB",0]
["13438","KAEDRA ROZVODNICA IP65 12MOD. 1 ZÁS",1,"ks",{"v":92.61,"d":"92.610"},"3303430134381",{"v":46.5,"d":"46.50"},{"v":17,"d":"17.00"},{"v":29,"d":"29.00"},{"v":2625,"d":"2,625.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13438","Kaedra skrina rozhranná- 12 mod.",0]
["13437","KAEDRA ROZVODNICA IP65 72 MOD. 4 RAD",1,"ks",{"v":189.62999999999997,"d":"189.630"},"3303430134374",{"v":85,"d":"85.00"},{"v":17,"d":"17.00"},{"v":47,"d":"47.00"},{"v":8010,"d":"8,010.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13437","Kaedra - pre modulárne prístroje - 4x18 mod. - priehladné",0]
["13436","KAEDRA ROZVODNICA IP65 54 MOD. 3 RAD",1,"ks",{"v":141.11999999999998,"d":"141.120"},"3303430134367",{"v":62,"d":"62.00"},{"v":17,"d":"17.00"},{"v":46,"d":"46.00"},{"v":5853,"d":"5,853.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13436","Kaedra - pre modulárne prístroje - 3x18 mod. - priehladné",0]
["13435","KAEDRA ROZVODNICA IP65 36 MOD. 3 RAD",1,"ks",{"v":110.24999999999997,"d":"110.250"},"3303430134350",{"v":62.5,"d":"62.50"},{"v":17.2,"d":"17.20"},{"v":36,"d":"36.00"},{"v":4550,"d":"4,550.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13435","Kaedra - pre modulárne prístroje - 3x12 mod. - priehladné",0]
["13434","KAEDRA ROZVODNICA IP65 36 MOD. 2 RAD",1,"ks",{"v":92.61,"d":"92.610"},"3303430134343",{"v":47,"d":"47.00"},{"v":17.5,"d":"17.50"},{"v":47,"d":"47.00"},{"v":4425,"d":"4,425.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13434","Kaedra - pre modulárne prístroje - 2x18 mod. - priehladné",0]
["13433","KAEDRA ROZVODNICA IP65 24 MOD. 2 RAD",1,"ks",{"v":83.34899999999999,"d":"83.349"},"3303430134336",{"v":47.2,"d":"47.20"},{"v":17,"d":"17.00"},{"v":35.5,"d":"35.50"},{"v":3495,"d":"3,495.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13433","Kaedra - pre modulárne prístroje - 2x12 mod. - priehladné",0]
["13432","KAEDRA ROZVODNICA IP65 18 MOD. 1 RAD",1,"ks",67.032,"3303430134329",{"v":46.5,"d":"46.50"},{"v":17.5,"d":"17.50"},{"v":29,"d":"29.00"},{"v":2679,"d":"2,679.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13432","Mureva rozvodnice IP65 1x18M E/N TB",0]
["13431","KAEDRA ROZVODNICA IP65 12 MOD. 1 RAD",1,"ks",{"v":56.888999999999996,"d":"56.889"},"3303430134312",{"v":36,"d":"36.00"},{"v":16,"d":"16.00"},{"v":29,"d":"29.00"},{"v":1978,"d":"1,978.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13431","Kaedra - pre modulárne prístroje - 1x12 mod. - priehladné",0]
["13398","MINI OPALE KRYT NA PRÍSTROJE 1R 8M",1,"ks",{"v":11.906999999999998,"d":"11.907"},"3303430133988",{"v":16,"d":"16.00"},{"v":6,"d":"6.00"},{"v":15.5,"d":"15.50"},{"v":220,"d":"220.00"},"IT","85381000","https://www.se.com/sk/sk/product/13398","mini Opale rozvodnice pre povrch. montáž - IP 30 - 1x8 mod. - bez dverí",0]
["13396","MINI OPALE KRYT NA PRÍSTROJE 1R 6M",1,"ks",{"v":10.583999999999998,"d":"10.584"},"3303430133964",{"v":16,"d":"16.00"},{"v":6.5,"d":"6.50"},{"v":12,"d":"12.00"},{"v":190,"d":"190.00"},"IT","85381000","https://www.se.com/sk/sk/product/13396","mini Opale rozvodnice pre povrch. montáž - IP 30 - 1x6 mod. - bez dverí",0]
["13394","MINI OPALE KRYT NA PRÍSTROJE 1R 4M",1,"ks",{"v":4.409999999999999,"d":"4.410"},"3303430133940",{"v":5.7,"d":"5.70"},{"v":13,"d":"13.00"},{"v":8,"d":"8.00"},{"v":90,"d":"90.00"},"IT","85381000","https://www.se.com/sk/sk/product/13394","mini Opale rozvodnice pre povrch. montáž - IP 30 - 1x4 mod. - bez dverí",0]
["13392","MINI OPALE KRYT NA PRÍSTROJE 1R 2M",1,"ks",{"v":4.1013,"d":"4.101"},"3303430133926",{"v":13.1,"d":"13.10"},{"v":5.3,"d":"5.30"},{"v":4.4,"d":"4.40"},{"v":70,"d":"70.00"},"IT","85381000","https://www.se.com/sk/sk/product/13392","mini Opale rozvodnice pre povrch. montáž - IP 30 - 1x2 mod. - bez dverí",0]
["13229","MOD.ZÁSLEPKY RAL9003-SADA50 MOD(18MM)",1,"ks",{"v":8.819999999999999,"d":"8.820"},"3303430132295",{"v":10.5,"d":"10.50"},{"v":5,"d":"5.00"},{"v":7,"d":"7.00"},{"v":98,"d":"98.00"},"IT","39269097","https://www.se.com/sk/sk/product/13229","záslepky - sada 10 - biela RAL9003",0]
["13198","UNIVERZ.ROZVODNICA 448X610MM IP65 KAEDRA",1,"ks",{"v":167.57999999999998,"d":"167.580"},"3303430131984",{"v":62,"d":"62.00"},{"v":16.8,"d":"16.80"},{"v":46.8,"d":"46.80"},{"v":3110,"d":"3,110.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13198","Mureva rozvodnice IP65 Poly-Door 448x610",0]
["13197","UNIVERZ.ROZVODNICA 448x460mm IP65",1,"ks",{"v":132.29999999999998,"d":"132.300"},"3303430131977",{"v":16.8,"d":"16.80"},{"v":47,"d":"47.00"},{"v":46.8,"d":"46.80"},{"v":3110,"d":"3,110.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13197","Mureva rozvodnice IP65 Poly-Door 448x460",0]
["13196","UNIVERZ.ROZVODNICA 448X460MM IP65 KAEDRA",1,"ks",{"v":163.17,"d":"163.170"},"3303430131960",{"v":16.8,"d":"16.80"},{"v":62,"d":"62.00"},{"v":36,"d":"36.00"},{"v":2687,"d":"2,687.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13196","Kaedra - viacúčelová - 340 x 610 mm - 17 vylam. otvorov",0]
["13195","UNIVERZ.ROZVODNICA 340X460MM IP65 KAEDRA",1,"ks",{"v":97.01999999999998,"d":"97.020"},"3303430131953",{"v":47,"d":"47.00"},{"v":16.8,"d":"16.80"},{"v":36.2,"d":"36.20"},{"v":2687,"d":"2,687.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13195","Mureva rozvodnice IP65 Poly-Door 340x460",0]
["13193","UNIV.ROZVODNICA 1X18 MODULOV IP65 KAEDRA",1,"ks",{"v":97.01999999999998,"d":"97.020"},"3303430131939",{"v":47,"d":"47.00"},{"v":10,"d":"10.00"},{"v":47,"d":"47.00"},{"v":3741,"d":"3,741.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13193","Mureva rozvodnice IP65 Poly-Smooth 18M-46",0]
["13192","Mureva rozvodnice IP65 Poly-Smooth 12M-4",1,"ks",{"v":55.98935999999999,"d":"55.989"},"3303430131922",{"v":47,"d":"47.00"},{"v":17,"d":"17.00"},{"v":36,"d":"36.00"},{"v":2869,"d":"2,869.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13192","Mureva rozvodnice IP65 Poly-Smooth 12M-46",""]
["13191","Mureva rozvodnice IP65 Poly-Smooth 12M-3",1,"ks",{"v":49.55957999999999,"d":"49.560"},"3303430131915",{"v":36,"d":"36.00"},{"v":16.8,"d":"16.80"},{"v":34.5,"d":"34.50"},{"v":2122,"d":"2,122.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13191","Mureva rozvodnice IP65 Poly-Smooth 12M-34",""]
["13190","Mureva rozvodnice IP65 Poly-Smooth 8M-h4",1,"ks",{"v":43.129799999999996,"d":"43.130"},"3303430131908",{"v":47,"d":"47.00"},{"v":17,"d":"17.00"},{"v":26,"d":"26.00"},{"v":1910,"d":"1,910.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13190","Mureva rozvodnice IP65 Poly-Smooth 8M-h46",""]
["13189","Mureva rozvodnice IP65 Poly-Smooth 5M-h4",1,"ks",{"v":411.01199999999994,"d":"411.012"},"3303430131892",{"v":16.8,"d":"16.80"},{"v":47,"d":"47.00"},{"v":15.8,"d":"15.80"},{"v":1356,"d":"1,356.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13189","Mureva rozvodnice IP65 Poly-Smooth 5M-h46",""]
["13188","ROZVODNICA 1X18 MOD. 4 ROZŠ. IP65 KAEDRA",1,"ks",{"v":119.07,"d":"119.070"},"3303430131885",{"v":16.8,"d":"16.80"},{"v":47,"d":"47.00"},{"v":46.8,"d":"46.80"},{"v":3110,"d":"3,110.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13188","Mureva rozvodnice IP65 for Int.sock 18Mx4",0]
["13186","Mureva rozvodnice IP65 for Int.sock 8Mx2",1,"ks",{"v":48.077819999999996,"d":"48.078"},"3303430131861",{"v":16.8,"d":"16.80"},{"v":47,"d":"47.00"},{"v":25.6,"d":"25.60"},{"v":1867,"d":"1,867.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13186","Mureva rozvodnice IP65 for Int.sock 8Mx2",0]
["13185","Mureva rozvodnice IP65 for Int. sock 5Mx",1,"ks",{"v":47.61035999999999,"d":"47.610"},"3303430131854",{"v":16.8,"d":"16.80"},{"v":47,"d":"47.00"},{"v":15.8,"d":"15.80"},{"v":1377,"d":"1,377.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13185","Mureva rozvodnice IP65 for Int. sock 5Mx1",0]
["13182","Mureva rozvodnice IP65 for IEC sock 18Mx",1,"ks",{"v":90.84599999999999,"d":"90.846"},"3303430131823",{"v":16.8,"d":"16.80"},{"v":47,"d":"47.00"},{"v":46.8,"d":"46.80"},{"v":3350,"d":"3,350.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13182","Mureva rozvodnice IP65 for IEC sock 18Mx8",0]
["13181","ROZVODNICA 1X12 MOD. 6 ROZŠ. IP65 KAEDRA",1,"ks",{"v":88.19999999999999,"d":"88.200"},"3303430131816",{"v":47,"d":"47.00"},{"v":16.8,"d":"16.80"},{"v":36,"d":"36.00"},{"v":2848,"d":"2,848.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13181","Mureva rozvodnice IP65 for IEC sock 12Mx6",0]
["13180","ROZVODNICA 1X12 MOD. 3 ROZŠ. IP65 KAEDRA",1,"ks",67.473,"3303430131809",{"v":35,"d":"35.00"},{"v":17.2,"d":"17.20"},{"v":35.7,"d":"35.70"},{"v":2100,"d":"2,100.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13180","Mureva rozvodnice IP65 for IEC sock 12Mx3",0]
["13179","ROZVODNICA 1X8 MOD. 4 ROZŠ. IP65 KAEDRA",1,"ks",46.305,"3303430131793",{"v":47.3,"d":"47.30"},{"v":17.4,"d":"17.40"},{"v":26.3,"d":"26.30"},{"v":1960,"d":"1,960.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13179","Mureva rozvodnice IP65 for IEC sock 8Mx4",0]
["13178","Mureva rozvodnice IP65 for IEC sock 5Mx2",1,"ks",{"v":38.41992,"d":"38.420"},"3303430131786",{"v":17,"d":"17.00"},{"v":47,"d":"47.00"},{"v":16,"d":"16.00"},{"v":1416,"d":"1,416.00"},"IT","8538100000","https://www.se.com/sk/sk/product/13178","Mureva rozvodnice IP65 for IEC sock 5Mx2",""]
["13177","MINI ROZVODNICA 4 MOD 3 ROZŠ IP65 KAEDRA",1,"ks",33.516,"3303430131779",{"v":39,"d":"39.00"},{"v":10,"d":"10.00"},{"v":10.4,"d":"10.40"},{"v":557,"d":"557.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13177","Mureva rozvodnice IP65 for sock mini 4Mx3",0]
["13176","Mureva rozvodnice IP65 for sock mini 4Mx",1,"ks",{"v":22.199939999999998,"d":"22.200"},"3303430131762",{"v":31,"d":"31.00"},{"v":9.7,"d":"9.70"},{"v":9.7,"d":"9.70"},{"v":490,"d":"490.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13176","Mureva rozvodnice IP65 for sock mini 4Mx2",""]
["13175","Mureva rozvodnice IP65 for sock mini 4Mx",1,"ks",{"v":18.275039999999997,"d":"18.275"},"3303430131755",{"v":24.5,"d":"24.50"},{"v":9.7,"d":"9.70"},{"v":9.8,"d":"9.80"},{"v":395,"d":"395.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13175","Mureva rozvodnice IP65 for sock mini 4Mx1",""]
["13144","FUNKČNÁ DOSKA 103X225, 100X107",100,"ks",{"v":6.614999999999998,"d":"6.615"},"3303430131441",{"v":10.2,"d":"10.20"},{"v":2.4,"d":"2.40"},{"v":22.4,"d":"22.40"},{"v":132,"d":"132.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13144","Kaedra funkčná doska 103 x 225 mm - otvor pre zásuvku 100x107mm",0]
["13143","FUNKČNÁ DOSKA 103X225, 65X65-75X75",1,"ks",{"v":9.701999999999998,"d":"9.702"},"3303430131434",{"v":24.2,"d":"24.20"},{"v":3.6,"d":"3.60"},{"v":12.3,"d":"12.30"},{"v":148,"d":"148.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13143","Kaedra funkčná doska 103 x 225 mm - otvor pre zásuvku 65x65 - 75x75mm",0]
["13142","FUNKČNÁ DOSKA 103X225, 65x85-90X100",100,"ks",{"v":7.055999999999999,"d":"7.056"},"3303430131427",{"v":22.5,"d":"22.50"},{"v":2.4,"d":"2.40"},{"v":10.2,"d":"10.20"},{"v":144,"d":"144.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13142","Kaedra funkčná doska 103 x 225 mm - 2 otvory - 65x85 - 90x100mm",0]
["13138","DOSKA PLNÁ 90X100 PRE TLAČ./SIGN. KAEDRA",1,"ks",{"v":4.3659,"d":"4.366"},"3303430131380",{"v":10,"d":"10.00"},{"v":1.3,"d":"1.30"},{"v":9,"d":"9.00"},{"v":34,"d":"34.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13138","Kaedra funkčná doska 90x100 - pre ovl. 3 x 22mm",0]
["13137","DOSKA PLNÁ 90x100 PRE ZÁS. 65x65 KAEDRA",1,"ks",{"v":4.498199999999999,"d":"4.498"},"3303430131373",{"v":11.9,"d":"11.90"},{"v":1.9,"d":"1.90"},{"v":9.7,"d":"9.70"},{"v":44,"d":"44.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13137","Kaedra funkčná doska 90x100 - pre zásuvku 65 x 65 alebo 75 x 75 mm",0]
["13136","DOSKA PRECH 90x100 PRE ZÁS. 65x85 KAEDRA",1,"ks",{"v":4.3659,"d":"4.366"},"3303430131366",{"v":11.7,"d":"11.70"},{"v":2,"d":"2.00"},{"v":10.5,"d":"10.50"},{"v":30,"d":"30.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13136","Kaedra funkčná doska 90x100 - pre zásuvku 65x85mm",0]
["13135","DOSKA PLNÁ 65X85 PRE ZÁS. 50X50 KAEDRA",1,"ks",{"v":4.718699999999999,"d":"4.719"},"3303430131359",{"v":9.5,"d":"9.50"},{"v":2,"d":"2.00"},{"v":8.5,"d":"8.50"},{"v":33,"d":"33.00"},"IT","3926909790","https://www.se.com/sk/sk/product/13135","Kaedra funkčná doska 85x65 pre vývod 50x50mm",0]
["123251","VIDLICA SCHUKO GUMOVÁ 3X2,5MM²",1,"ks",{"v":7.684424999999997,"d":"7.684"},"4011281129652",{"v":11.3,"d":"11.30"},{"v":4.1,"d":"4.10"},{"v":4.2,"d":"4.20"},{"v":78,"d":"78.00"},"DE","85369010","https://www.se.com/sk/sk/product/123251","Vidlica 2P+PE/SE, MERTEN, 16A, 250VAC, IP44",0]
["121700","PREPÍNAČ KRÍŽOVÝ (7) 10A ELSO BIELA",1,"ks",{"v":10.977749999999999,"d":"10.978"},"4013984106442",{"v":7,"d":"7.00"},{"v":3,"d":"3.00"},{"v":7,"d":"7.00"},{"v":54.7,"d":"54.70"},"DE","85365080","https://www.se.com/sk/sk/product/121700","ELSO Inserts - vypínač - krížový - zapustený - 10 A - skrutkové sv.",0]
["111600","PREPÍNAČ STRIEDAVÝ (6) 10A ELSO",1,"ks",{"v":6.3231839999999995,"d":"6.323"},"4013984106497",{"v":7,"d":"7.00"},{"v":3,"d":"3.00"},{"v":7,"d":"7.00"},{"v":52,"d":"52.00"},"DE","85365080","https://www.se.com/sk/sk/product/111600","Prepínač striedavý (6), ELSO mechanizmus, 10A",0]
["111500","PREPÍNAČ SÉRIOVÝ (5) 10A ELSO",1,"ks",{"v":8.782199999999998,"d":"8.782"},"4013984106473",{"v":7,"d":"7.00"},{"v":3,"d":"3.00"},{"v":7,"d":"7.00"},{"v":54,"d":"54.00"},"DE","85365080","https://www.se.com/sk/sk/product/111500","Prepínač sériový (5), ELSO mechanizmus, 10A",0]
["10502","STOJAN PRE KAEDRU 18M",1,"ks",{"v":90.84599999999999,"d":"90.846"},"3303430105022",{"v":75,"d":"75.00"},{"v":26,"d":"26.00"},{"v":47,"d":"47.00"},{"v":2160,"d":"2,160.00"},"IT","7326909890","https://www.se.com/sk/sk/product/10502","stojan pre Kaedru 18 modulov",""]
["10501","STOJAN PRE KAEDRU 12M",1,"ks",89.964,"3303430105015",{"v":69,"d":"69.00"},{"v":15,"d":"15.00"},{"v":44.8,"d":"44.80"},{"v":2091,"d":"2,091.00"},"IT","7326909890","https://www.se.com/sk/sk/product/10501","stojan pre Kaedru 12 modulov",""]
["10287","UL1077 prepojovací hrebeň 3x18mm 12 MOD",1,"ks",{"v":11.906999999999998,"d":"11.907"},"3303430102878",{"v":22,"d":"22.00"},{"v":1.3,"d":"1.30"},{"v":5.5,"d":"5.50"},{"v":108,"d":"108.00"},"DE","8536901000","https://www.se.com/sk/sk/product/10287","UL1077 prepájací hrebeň 3x18mm 12 MOD",0]
["10286","HREB.PREP.LIŠTA 2X18MM 12 MOD. UL1077",1,"ks",{"v":9.260999999999997,"d":"9.261"},"3303430102861",{"v":21.5,"d":"21.50"},{"v":1.3,"d":"1.30"},{"v":5.5,"d":"5.50"},{"v":94,"d":"94.00"},"US","85369010","https://www.se.com/sk/sk/product/10286","HREBEŇOVÁ LIŠTA C60N UL1077 2-POLÓVÁ 63A 12X18MM",0]
["10285","HREB.PREP.LIŠTA 1X18MM 12 MOD. UL1077",1,"ks",{"v":10.142999999999999,"d":"10.143"},"3303430102854",{"v":21.5,"d":"21.50"},{"v":2,"d":"2.00"},{"v":5.5,"d":"5.50"},{"v":79,"d":"79.00"},"US","85369010","https://www.se.com/sk/sk/product/10285","HREBEŇOVÁ LIŠTA C60N UL1077 1-POLÓVÁ 63A 12X18MM",0]
["10209","KRYCIA DOSKA 18 MODULOV",1,"ks",{"v":8.819999999999999,"d":"8.820"},"3303430102090",{"v":35,"d":"35.00"},{"v":2,"d":"2.00"},{"v":15,"d":"15.00"},{"v":105,"d":"105.00"},"IT","39269097","https://www.se.com/sk/sk/product/10209","čelný panel - 18 mod. - preKaedra",0]
["1005016","TP 2B PRÍCHYTKA",100,"ks",{"v":4.215455999999999,"d":"4.215"},"7315881005017",{"v":3.9,"d":"3.90"},{"v":0.9,"d":"0.90"},{"v":0.9,"d":"0.90"},{"v":10,"d":"10.00"},"SE","39259080","https://www.se.com/sk/sk/product/1005016","TP 2B príchytka",0]
["100108110","Ucpavka sada pre VG211",1,"ks",{"v":105.721875,"d":"105.722"},"3606489656577",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":149,"d":"149.00"},"IT","84811099","https://www.se.com/sk/sk/product/100108110","Replacement Packing Gland / Stuffing box for the VGS211F (VG211) Steam Valve.",0]
["100108000","TESNENIE NA VENTIL VENTA",1,"ks",{"v":96.271875,"d":"96.272"},"3606480935510",{"v":3.2,"d":"3.20"},{"v":6.2,"d":"6.20"},{"v":3.2,"d":"3.20"},{"v":124,"d":"124.00"},"SE","90329000","https://www.se.com/sk/sk/product/100108000","Replacement Stuffing Box / Packing Gland Kit - (Type S) 20mm Venta Valves.",0]
["006920640","Exteriérový prevodník osvetlenia SLO 320",1,"ks",{"v":442.96875,"d":"442.969"},"7332552011702",{"v":11.4,"d":"11.40"},{"v":6.5,"d":"6.50"},{"v":9.6,"d":"9.60"},{"v":149,"d":"149.00"},"DE","9027808000","https://www.se.com/sk/sk/product/006920640","SLO Series outdoor light transmitter, SLO320, selectable outputs, 0-20,000 Lux",0.02]
["006920630","Interiérový prevodník osvetlenia SLR 320",1,"ks",{"v":442.96875,"d":"442.969"},"7332552011696",{"v":12.4,"d":"12.40"},{"v":4.1,"d":"4.10"},{"v":9.6,"d":"9.60"},{"v":75,"d":"75.00"},"DE","90329000","https://www.se.com/sk/sk/product/006920630","Light transmitter, SLR320, room, wall mounting",0.01]
["006920501","Exteriérový prevodník teploty STO300",1,"ks",{"v":242.15625,"d":"242.156"},"7332552011689",{"v":16.5,"d":"16.50"},{"v":5.8,"d":"5.80"},{"v":15.4,"d":"15.40"},{"v":237,"d":"237.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006920501","STO Series outdoor temperature sensor, STO300-50/50, output 4-20 mA, -50-50 °C",0.03]
["006920301","Ponor. prevodník tepl. STP300-200 0/100",1,"ks",{"v":224.4375,"d":"224.438"},"7332552011603",{"v":28.3,"d":"28.30"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":195,"d":"195.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006920301","STP Series immersion temperature sensor, STP300-200 0/100, pipe, 200 mm probe, 2-Wire, 0-100 °C, accuracy 0.4%",0.02]
["006920281","PONOR. PREVODNÍK TEPL. STP300-200 -50/50",1,"ks",{"v":224.4375,"d":"224.438"},"7332552011597",{"v":28.3,"d":"28.30"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":195,"d":"195.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006920281","Temp Sensor: Immer, Pipe, Probe: 200mm, 2-Wire, 50/+50 C, Acc: 0.4 %, STP300-200 -50/50",0.02]
["006920261","PONOR. PREVODNÍK TEPL. STP300-100 0/160",1,"ks",{"v":218.53125,"d":"218.531"},"7332552011580",{"v":20.5,"d":"20.50"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":171,"d":"171.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006920261","Temp Sensor: Immer, Pipe, Probe: 100mm, 2-Wire, 0-160 C, Acc: 0.4 %, STP300-100 0/160",0.02]
["006920241","PONOR. PREVODNÍK TEPL. STP300-100 0/100",1,"ks",{"v":218.53125,"d":"218.531"},"7332552011573",{"v":20.5,"d":"20.50"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":171,"d":"171.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006920241","STP Series immersion temperature sensor, STP300-100 0/100, pipe, 100 mm probe, 2-Wire, 0-100 °C",0.02]
["006920221","PONOR. PREVODNÍK TEPL. STP300-100 -50/50",1,"ks",{"v":218.53125,"d":"218.531"},"7332552011566",{"v":20.5,"d":"20.50"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":171,"d":"171.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006920221","STP Series immersion temperature sensor, STP300-100, pipe, 100 mm probe, 2-Wire, -50-50 °C, accuracy 0.4 %",0.02]
["006920141","KANÁLOVÝ PREVODNÍK TEPLOTY STD300-300 0/",1,"ks",{"v":236.25,"d":"236.250"},"7332552011559",{"v":38.3,"d":"38.30"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":237,"d":"237.00"},"DE","9025190090","https://www.se.com/sk/sk/product/006920141","STD Series temperature sensor, STD300-300, duct, 0-100 °C",0.03]
["006920121","Kanálový převodník teploty STD300-300 -5",1,"ks",{"v":236.25,"d":"236.250"},"7332552011542",{"v":38.3,"d":"38.30"},{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":237,"d":"237.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006920121","STD Series temperature sensor, STD300-300, duct, -50-50 °C",0.03]
["006920041","Príložný prevodník teploty STC300 0/100",1,"ks",{"v":200.8125,"d":"200.813"},"7332552011528",{"v":9.6,"d":"9.60"},{"v":7.2,"d":"7.20"},{"v":20.2,"d":"20.20"},{"v":250,"d":"250.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006920041","STC Series contact temperature transmitter, STC300, 2-Wire, 0-100 °C, accuracy 0.3 °C at 25 °C",0.03]
["006902510","Kondenzačný snímač SCC110",1,"ks",{"v":313.03125,"d":"313.031"},"7332552011504",{"v":9.6,"d":"9.60"},{"v":7.2,"d":"7.20"},{"v":20.2,"d":"20.20"},{"v":268,"d":"268.00"},"SE","9025808090","https://www.se.com/sk/sk/product/006902510","SCC Series SCC110 Model, Contact Condensation Switch, Supply 24 VAC, Remote Sensor With A 2 m Wire",0.03]
["006902500","Kondenzačný snímač SCP110",1,"ks",259.875,"7332552011498",{"v":9.6,"d":"9.60"},{"v":6.5,"d":"6.50"},{"v":12,"d":"12.00"},{"v":194,"d":"194.00"},"SE","9025808090","https://www.se.com/sk/sk/product/006902500","SCP Series SCP110 Model, Pipe Condensation Switch, Supply 24 VAC",0.02]
["006902401","EXT. PREVODNÍK REL. VLHKOSTI SHO 101-T5",1,"ks",{"v":378,"d":"378.000"},"7332552011474",{"v":11.5,"d":"11.50"},{"v":6.5,"d":"6.50"},{"v":9.6,"d":"9.60"},{"v":163,"d":"163.00"},"SE","9025804089","https://www.se.com/sk/sk/product/006902401","RH and Temp Sensor: Outdoor, 24 VAC, Systems: Continuum, Vista, Xenta, Selectable Outputs, 0-95% RH, 2% Acc, SH0100-T5",0.02]
["006902381","KANÁL. PREVODNÍK R. VLHKOSTI SHD 101-T5",1,"ks",{"v":313.03125,"d":"313.031"},"7332552011467",{"v":9.6,"d":"9.60"},{"v":7.2,"d":"7.20"},{"v":38.3,"d":"38.30"},{"v":251,"d":"251.00"},"SE","9025190090","https://www.se.com/sk/sk/product/006902381","SHD Series SHD100-T5 Model, Duct Humidity And Temperature Sensor, Supply 24 VAC, Selectable Outputs, 0-95% RH, Continuum/Vista/Xenta Compatible",0.03]
["006902371","Exter. prevodník rel. vlhkosti SHO 100-T",1,"ks",{"v":454.78125,"d":"454.781"},"7332552011450",{"v":11.4,"d":"11.40"},{"v":6.5,"d":"6.50"},{"v":9.6,"d":"9.60"},{"v":164,"d":"164.00"},"SE","9025804089","https://www.se.com/sk/sk/product/006902371","SHO Series SHO100-T Model, Outdoor Humidity & Temperature Sensor, Supply 24 VAC, Selectable Outputs, 0-95% RH, I/NET/Vista/Xenta Compatible",0.02]
["006902361","Čidlo rel.vlhkosti venkovní SHO100",1,"ks",401.625,"7332552011443",{"v":11.4,"d":"11.40"},{"v":6.5,"d":"6.50"},{"v":9.6,"d":"9.60"},{"v":163,"d":"163.00"},"SE","9025804089","https://www.se.com/sk/sk/product/006902361","RH Sensor: Outdoor, 24 VAC, Systems: All (%RH only), Selectable Outputs, 0-95% RH, 2% Acc, SH0100",0.02]
["006902331","Kanál. prevodník rel. vlhkosti SHD 100-T",1,"ks",{"v":289.40625,"d":"289.406"},"7332552011436",{"v":9.6,"d":"9.60"},{"v":7.2,"d":"7.20"},{"v":38.3,"d":"38.30"},{"v":250,"d":"250.00"},"SE","9025804089","https://www.se.com/sk/sk/product/006902331","SHD Series SHD100-T Model, Duct Humidity & Temperature Sensor, Supply 24 VAC, Selectable Outputs, 0-95% RH, I/NET/Vista/Xenta Compatible",0.03]
["006902321","Kanálový prevodník rel. vlhkosti SHD 100",1,"ks",{"v":330.75,"d":"330.750"},"7332552011429",{"v":9.6,"d":"9.60"},{"v":7.2,"d":"7.20"},{"v":38.3,"d":"38.30"},{"v":246,"d":"246.00"},"SE","9025804089","https://www.se.com/sk/sk/product/006902321","SHD Series SHD100 Model, Duct Humidity & Temperature Sensor, Selectable Outputs, 0-95% RH,Continuum/I/NET/Vista/Xenta/Satchwell Compatible",0.03]
["004702140","TLAKOVÝ PREVODNÍK SPP110-4000KPA",1,"ks",{"v":318.9375,"d":"318.938"},"7332552011405",{"v":11.3,"d":"11.30"},{"v":6.5,"d":"6.50"},{"v":9.9,"d":"9.90"},{"v":222,"d":"222.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004702140","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004702120","Tlakový prevodník SPP110-2500kPa",1,"ks",{"v":289.40625,"d":"289.406"},"7332552011399",{"v":9.6,"d":"9.60"},{"v":6.5,"d":"6.50"},{"v":11.4,"d":"11.40"},{"v":222,"d":"222.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004702120","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004702100","TLAKOVÝ PREVODNÍK SPP110-1600KPA",1,"ks",{"v":289.40625,"d":"289.406"},"7332552011382",{"v":11.3,"d":"11.30"},{"v":6.5,"d":"6.50"},{"v":9.9,"d":"9.90"},{"v":222,"d":"222.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004702100","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004702080","Tlakový prevodník SPP110-1000kPa",1,"ks",{"v":289.40625,"d":"289.406"},"7332552011375",{"v":11.3,"d":"11.30"},{"v":6.5,"d":"6.50"},{"v":9.9,"d":"9.90"},{"v":222,"d":"222.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004702080","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004702060","Tlakový prevodník SPP110-600kPa",1,"ks",{"v":289.40625,"d":"289.406"},"7332552011368",{"v":11.3,"d":"11.30"},{"v":6.5,"d":"6.50"},{"v":9.9,"d":"9.90"},{"v":222,"d":"222.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004702060","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004702040","Tlakový prevodník SPP110-250kPa",1,"ks",307.125,"7332552011351",{"v":11.3,"d":"11.30"},{"v":6.5,"d":"6.50"},{"v":9.9,"d":"9.90"},{"v":222,"d":"222.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004702040","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004702020","TLAKOVÝ PREVODNÍK SPP110-100KPA",1,"ks",{"v":330.75,"d":"330.750"},"7332552011344",{"v":11.3,"d":"11.30"},{"v":6.5,"d":"6.50"},{"v":9.9,"d":"9.90"},{"v":222,"d":"222.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004702020","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004701170","Přetlakový snímač SPP930-6000, 1000-6000",1,"ks",{"v":330.75,"d":"330.750"},"7332552011337",{"v":8.7,"d":"8.70"},{"v":9,"d":"9.00"},{"v":8.6,"d":"8.60"},{"v":298,"d":"298.00"},"SE","9025190090","https://www.se.com/sk/sk/product/004701170","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.04]
["004701110","Rozdiel.tlak.spínač SPD920-060,15-60mbar",1,"ks",{"v":378,"d":"378.000"},"7332552011276",{"v":11.9,"d":"11.90"},{"v":8.5,"d":"8.50"},{"v":12.4,"d":"12.40"},{"v":1844,"d":"1,844.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004701110","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.22]
["004701100","Spínač diferenčního tlaku SPD920-020, 6-",1,"ks",{"v":378,"d":"378.000"},"7332552011269",{"v":11.9,"d":"11.90"},{"v":8.5,"d":"8.50"},{"v":12.4,"d":"12.40"},{"v":1051,"d":"1,051.00"},"CH","9026202000","https://www.se.com/sk/sk/product/004701100","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.13]
["004701090","Rozdiel. tlakový spínač SPD 910-2000 Pa",1,"ks",{"v":55.51875,"d":"55.519"},"7332552011252",{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":20.2,"d":"20.20"},{"v":274,"d":"274.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004701090","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004701080","Rozdielový tlakový spínač SPD 910-1000Pa",1,"ks",{"v":55.51875,"d":"55.519"},"7332552011245",{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":20.2,"d":"20.20"},{"v":274,"d":"274.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004701080","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.03]
["004701070","Rozdielový tlakový spínač SPD 910-500 Pa",1,"ks",{"v":55.51875,"d":"55.519"},"7332552011238",{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":20.2,"d":"20.20"},{"v":208,"d":"208.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004701070","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.02]
["004701060","Rozdielový tlakový spínač SPD 910-300 Pa",1,"ks",{"v":55.51875,"d":"55.519"},"7332552011221",{"v":7.2,"d":"7.20"},{"v":9.6,"d":"9.60"},{"v":20.2,"d":"20.20"},{"v":208,"d":"208.00"},"SE","9026202000","https://www.se.com/sk/sk/product/004701060","Differential Air Pressure Trans: For the monitoring of air ducts, filters and fans, SPD310-100/300/500/1000Pa",0.02]